(footprint "5557_connector" (version 20201116) (generator pcbnew) (layer "F.Cu")
  (tedit 5FEB16B3)
  (fp_text reference "REF**" (at -25.6 0 90) (layer "F.SilkS"))
  (fp_text value "5557_connector" (at 0 0) (layer "F.Fab"))
  (pad "1" thru_hole circle (at -23.1 2.1) (size 2 2) (drill 1.15) (layers *.Cu *.Mask))
  (pad "2" thru_hole circle (at -18.9 2.1) (size 2 2) (drill 1.15) (layers *.Cu *.Mask))
  (pad "3" thru_hole circle (at -14.7 2.1) (size 2 2) (drill 1.15) (layers *.Cu *.Mask))
  (pad "4" thru_hole circle (at -10.5 2.1) (size 2 2) (drill 1.15) (layers *.Cu *.Mask))
  (pad "5" thru_hole circle (at -6.3 2.1) (size 2 2) (drill 1.15) (layers *.Cu *.Mask))
  (pad "6" thru_hole circle (at -2.1 2.1) (size 2 2) (drill 1.15) (layers *.Cu *.Mask))
  (pad "7" thru_hole circle (at 2.1 2.1) (size 2 2) (drill 1.15) (layers *.Cu *.Mask))
  (pad "8" thru_hole circle (at 6.3 2.1) (size 2 2) (drill 1.15) (layers *.Cu *.Mask))
  (pad "9" thru_hole circle (at 10.5 2.1) (size 2 2) (drill 1.15) (layers *.Cu *.Mask))
  (pad "10" thru_hole circle (at 14.7 2.1) (size 2 2) (drill 1.15) (layers *.Cu *.Mask))
  (pad "11" thru_hole circle (at 18.9 2.1) (size 2 2) (drill 1.15) (layers *.Cu *.Mask))
  (pad "12" thru_hole circle (at 23.1 2.1) (size 2 2) (drill 1.15) (layers *.Cu *.Mask))
  (pad "13" thru_hole circle (at -23.1 -2.1) (size 2 2) (drill 1.15) (layers *.Cu *.Mask))
  (pad "14" thru_hole circle (at -18.9 -2.1) (size 2 2) (drill 1.15) (layers *.Cu *.Mask))
  (pad "15" thru_hole circle (at -14.7 -2.1) (size 2 2) (drill 1.15) (layers *.Cu *.Mask))
  (pad "16" thru_hole circle (at -10.5 -2.1) (size 2 2) (drill 1.15) (layers *.Cu *.Mask))
  (pad "17" thru_hole circle (at -6.3 -2.1) (size 2 2) (drill 1.15) (layers *.Cu *.Mask))
  (pad "18" thru_hole circle (at -2.1 -2.1) (size 2 2) (drill 1.15) (layers *.Cu *.Mask))
  (pad "19" thru_hole circle (at 2.1 -2.1 90) (size 2 2) (drill 1.15) (layers *.Cu *.Mask))
  (pad "20" thru_hole circle (at 6.3 -2.1) (size 2 2) (drill 1.15) (layers *.Cu *.Mask))
  (pad "21" thru_hole circle (at 10.5 -2.1) (size 2 2) (drill 1.15) (layers *.Cu *.Mask))
  (pad "22" thru_hole circle (at 14.7 -2.1) (size 2 2) (drill 1.15) (layers *.Cu *.Mask))
  (pad "23" thru_hole circle (at 18.9 -2.1) (size 2 2) (drill 1.15) (layers *.Cu *.Mask))
  (pad "24" thru_hole circle (at 23.1 -2.1) (size 2 2) (drill 1.15) (layers *.Cu *.Mask))
)
