(kicad_symbol_lib (version 20200827) (generator kicad_symbol_editor)
  (symbol "CM4IO:1-1734248-5"
    (property "Reference" "J" (id 0) (at -5.08 20.955 0))
    (property "Value" "1-1734248-5" (id 1) (at -5.08 -22.86 0))
    (property "Footprint" "TE_1-1734248-5" (id 2) (at 0 0 0))
    (property "Datasheet" "https://www.te.com/usa-en/product-1-1734248-5.html?te_bu=Cor&te_type=disp&te_campaign=seda_glo_cor-seda-global-disp-prtnr-fy19-seda-model-bom-cta_sma-317_1&elqCampaignId=32493" (id 3) (at 0 0 0))
    (property "Field4" "Manufacturer Recommendations" (id 4) (at 0 0 0))
    (property "Field5" "TE Connectivity" (id 5) (at 0 0 0))
    (property "Field6" "1-1734248-5" (id 6) (at 0 0 0))
    (property "Field7" "Conn FPC Connector SKT 15 POS 1mm Solder ST SMD T/R" (id 7) (at 0 0 0))
    (property "Field8" "None" (id 8) (at 0 0 0))
    (property "Field9" "Unavailable" (id 9) (at 0 0 0))
    (property "Field10" "E1" (id 10) (at 0 0 0))
    (property "Field11" "Compliant" (id 11) (at 0 0 0))
    (property "Field12" "None" (id 12) (at 0 0 0))
    (property "Field13" "1-1734248-5" (id 13) (at 0 0 0))
    (property "ki_locked" "" (id 14) (at 0 0 0))
    (symbol "1-1734248-5_0_0"
      (pin passive line (at -7.62 17.78 0) (length 2.54)
        (name "1")
        (number "1")
      )
      (pin passive line (at -7.62 -5.08 0) (length 2.54)
        (name "10")
        (number "10")
      )
      (pin passive line (at 7.62 -5.08 180) (length 2.54)
        (name "10")
        (number "10_1")
      )
      (pin passive line (at -7.62 -7.62 0) (length 2.54)
        (name "11")
        (number "11")
      )
      (pin passive line (at 7.62 -7.62 180) (length 2.54)
        (name "11")
        (number "11_1")
      )
      (pin passive line (at -7.62 -10.16 0) (length 2.54)
        (name "12")
        (number "12")
      )
      (pin passive line (at 7.62 -10.16 180) (length 2.54)
        (name "12")
        (number "12_1")
      )
      (pin passive line (at -7.62 -12.7 0) (length 2.54)
        (name "13")
        (number "13")
      )
      (pin passive line (at 7.62 -12.7 180) (length 2.54)
        (name "13")
        (number "13_1")
      )
      (pin passive line (at -7.62 -15.24 0) (length 2.54)
        (name "14")
        (number "14")
      )
      (pin passive line (at 7.62 -15.24 180) (length 2.54)
        (name "14")
        (number "14_1")
      )
      (pin passive line (at -7.62 -17.78 0) (length 2.54)
        (name "15")
        (number "15")
      )
      (pin passive line (at 7.62 -17.78 180) (length 2.54)
        (name "15")
        (number "15_1")
      )
      (pin passive line (at 7.62 17.78 180) (length 2.54)
        (name "1")
        (number "1_1")
      )
      (pin passive line (at -7.62 15.24 0) (length 2.54)
        (name "2")
        (number "2")
      )
      (pin passive line (at 7.62 15.24 180) (length 2.54)
        (name "2")
        (number "2_1")
      )
      (pin passive line (at -7.62 12.7 0) (length 2.54)
        (name "3")
        (number "3")
      )
      (pin passive line (at 7.62 12.7 180) (length 2.54)
        (name "3")
        (number "3_1")
      )
      (pin passive line (at -7.62 10.16 0) (length 2.54)
        (name "4")
        (number "4")
      )
      (pin passive line (at 7.62 10.16 180) (length 2.54)
        (name "4")
        (number "4_1")
      )
      (pin passive line (at -7.62 7.62 0) (length 2.54)
        (name "5")
        (number "5")
      )
      (pin passive line (at 7.62 7.62 180) (length 2.54)
        (name "5")
        (number "5_1")
      )
      (pin passive line (at -7.62 5.08 0) (length 2.54)
        (name "6")
        (number "6")
      )
      (pin passive line (at 7.62 5.08 180) (length 2.54)
        (name "6")
        (number "6_1")
      )
      (pin passive line (at -7.62 2.54 0) (length 2.54)
        (name "7")
        (number "7")
      )
      (pin passive line (at 7.62 2.54 180) (length 2.54)
        (name "7")
        (number "7_1")
      )
      (pin passive line (at -7.62 0 0) (length 2.54)
        (name "8")
        (number "8")
      )
      (pin passive line (at 7.62 0 180) (length 2.54)
        (name "8")
        (number "8_1")
      )
      (pin passive line (at -7.62 -2.54 0) (length 2.54)
        (name "9")
        (number "9")
      )
      (pin passive line (at 7.62 -2.54 180) (length 2.54)
        (name "9")
        (number "9_1")
      )
    )
  )
  (symbol "CM4IO:74LVC1G07_copy"
    (property "Reference" "U" (id 0) (at -2.54 3.81 0))
    (property "Value" "74LVC1G07_copy" (id 1) (at 0 -3.81 0))
    (property "Footprint" "Package_TO_SOT_SMD:SOT-353_SC-70-5" (id 2) (at 0 0 0))
    (property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf" (id 3) (at 0 0 0))
    (property "ki_keywords" "Single Gate Buff LVC CMOS Open Drain" (id 4) (at 0 0 0))
    (property "ki_description" "Single Buffer Gate w/ Open Drain, Low-Voltage CMOS" (id 5) (at 0 0 0))
    (property "ki_fp_filters" "SOT*\nSG-*" (id 6) (at 0 0 0))
    (symbol "74LVC1G07_copy_0_1")
    (symbol "74LVC1G07_copy_1_1"
      (pin input line (at -7.62 0 0) (length 3.81)
        (name "~")
        (number "2")
      )
      (pin power_in line (at 0 -2.54 270) (length 0)
        (name "GND")
        (number "3")
      )
      (pin open_collector line (at 6.35 0 180) (length 3.81)
        (name "~")
        (number "4")
      )
      (pin power_in line (at 0 2.54 90) (length 0)
        (name "VCC")
        (number "5")
      )
    )
  )
  (symbol "CM4IO:74AUC1G07_copy" (extends "74LVC1G07_copy")
    (property "Reference" "U" (id 0) (at -2.54 3.81 0))
    (property "Value" "74AUC1G07_copy" (id 1) (at 0 -3.81 0))
    (property "Footprint" "Package_TO_SOT_SMD:SOT-353_SC-70-5" (id 2) (at 0 0 0))
    (property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf" (id 3) (at 0 0 0))
    (property "ki_keywords" "Single Gate Buff LVC CMOS Open Drain" (id 4) (at 0 0 0))
    (property "ki_description" "Single Buffer Gate w/ Open Drain, Low-Voltage CMOS" (id 5) (at 0 0 0))
  )
  (symbol "CM4IO:74AUP1G07_copy" (extends "74LVC1G07_copy")
    (property "Reference" "U" (id 0) (at -2.54 3.81 0))
    (property "Value" "74AUP1G07_copy" (id 1) (at 0 -3.81 0))
    (property "Footprint" "Package_TO_SOT_SMD:SOT-353_SC-70-5" (id 2) (at 0 0 0))
    (property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf" (id 3) (at 0 0 0))
    (property "ki_keywords" "Single Gate Buff LVC CMOS Open Drain" (id 4) (at 0 0 0))
    (property "ki_description" "Single Buffer Gate w/ Open Drain, Low-Voltage CMOS" (id 5) (at 0 0 0))
  )
  (symbol "CM4IO:AP2553W6"
    (property "Reference" "U" (id 0) (at 3.81 -6.35 0))
    (property "Value" "AP2553W6" (id 1) (at -3.81 -6.35 0))
    (property "Footprint" "Package_TO_SOT_SMD:SOT-23-6" (id 2) (at 3.81 -6.35 0))
    (property "Datasheet" "https://www.diodes.com/assets/Datasheets/AP255x.pdf" (id 3) (at 3.81 -6.35 0))
    (property "Field4" "Digikey" (id 4) (at 0 0 0))
    (property "Field5" "AP2553W6-7DICT-ND" (id 5) (at 0 0 0))
    (symbol "AP2553W6_0_1")
    (symbol "AP2553W6_0_0"
      (pin power_in line (at -8.89 2.54 0) (length 2.54)
        (name "IN")
        (number "1")
      )
      (pin power_out line (at -8.89 0 0) (length 2.54)
        (name "GND")
        (number "2")
      )
      (pin input line (at -8.89 -2.54 0) (length 2.54)
        (name "EN")
        (number "3")
      )
      (pin open_collector line (at 7.62 -2.54 180) (length 2.54)
        (name "nFault")
        (number "4")
      )
      (pin passive line (at 7.62 0 180) (length 2.54)
        (name "ILIM")
        (number "5")
      )
      (pin power_out line (at 7.62 2.54 180) (length 2.54)
        (name "OUT")
        (number "6")
      )
    )
  )
  (symbol "CM4IO:AP64351"
    (property "Reference" "U" (id 0) (at 0 8.89 0))
    (property "Value" "AP64351" (id 1) (at 1.27 6.35 0))
    (property "Footprint" "Package_SO:SOIC-8-1EP_3.9x4.9mm_P1.27mm_EP2.95x4.9mm_Mask2.71x3.4mm_ThermalVias" (id 2) (at 0 0 0))
    (property "Datasheet" "" (id 3) (at 0 0 0))
    (symbol "AP64351_0_1")
    (symbol "AP64351_1_1"
      (pin passive line (at -7.62 2.54 0) (length 2.54)
        (name "BST")
        (number "1")
      )
      (pin power_in line (at -7.62 0 0) (length 2.54)
        (name "VIN")
        (number "2")
      )
      (pin input line (at -7.62 -2.54 0) (length 2.54)
        (name "EN")
        (number "3")
      )
      (pin input line (at -7.62 -5.08 0) (length 2.54)
        (name "SS")
        (number "4")
      )
      (pin input line (at 8.89 -5.08 180) (length 2.54)
        (name "FB")
        (number "5")
      )
      (pin input line (at 8.89 -2.54 180) (length 2.54)
        (name "COMP")
        (number "6")
      )
      (pin power_in line (at 8.89 0 180) (length 2.54)
        (name "GND")
        (number "7")
      )
      (pin output line (at 8.89 2.54 180) (length 2.54)
        (name "SW")
        (number "8")
      )
      (pin passive line (at 0 -10.16 90) (length 2.54)
        (name "EP")
        (number "9")
      )
    )
  )
  (symbol "CM4IO:Barrel_Jack"
    (property "Reference" "J" (id 0) (at 0 5.334 0))
    (property "Value" "Barrel_Jack" (id 1) (at 0 -5.08 0))
    (property "Footprint" "" (id 2) (at 1.27 -1.016 0))
    (property "Datasheet" "" (id 3) (at 1.27 -1.016 0))
    (property "ki_fp_filters" "BarrelJack*" (id 4) (at 0 0 0))
    (symbol "Barrel_Jack_0_1")
    (symbol "Barrel_Jack_1_1"
      (pin passive line (at 7.62 2.54 180) (length 2.54)
        (name "~")
        (number "1")
      )
      (pin passive line (at 7.62 -2.54 180) (length 2.54)
        (name "~")
        (number "2")
      )
      (pin passive line (at 7.62 -5.08 180) (length 2.54)
        (name "~")
        (number "3")
      )
    )
  )
  (symbol "CM4IO:ComputeModule4-CM4"
    (property "Reference" "Module" (id 0) (at 113.03 -68.58 0))
    (property "Value" "ComputeModule4-CM4" (id 1) (at 140.97 2.54 0))
    (property "Footprint" "CM4IO:Raspberry-Pi-4-Compute-Module" (id 2) (at 142.24 -26.67 0))
    (property "Datasheet" "" (id 3) (at 142.24 -26.67 0))
    (property "Field4" "Hirose" (id 4) (at 0 0 0))
    (property "Field5" "2x DF40C-100DS-0.4V" (id 5) (at 0 -2.54 0))
    (symbol "ComputeModule4-CM4_1_0"
      (text "GPIO" (at 0 6.35 0))
    )
    (symbol "ComputeModule4-CM4_1_1"
      (text "600mA Max" (at -8.89 -53.34 0))
      (text "600mA Max" (at -8.89 -48.26 0))
      (text "NB SD signals are only available" (at -1.27 -27.94 0))
      (text "on modules without eMMC" (at -1.27 -30.48 0))
      (pin power_in line (at 27.94 55.88 180) (length 2.54)
        (name "GND")
        (number "1")
      )
      (pin passive line (at -33.02 45.72 0) (length 2.54)
        (name "Ethernet_Pair0_N")
        (number "10")
      )
      (pin output line (at -33.02 -68.58 0) (length 2.54)
        (name "nEXTRST")
        (number "100")
      )
      (pin passive line (at 27.94 43.18 180) (length 2.54)
        (name "Ethernet_Pair2_P")
        (number "11")
      )
      (pin passive line (at -33.02 43.18 0) (length 2.54)
        (name "Ethernet_Pair0_P")
        (number "12")
      )
      (pin power_in line (at 27.94 40.64 180) (length 2.54)
        (name "GND")
        (number "13")
      )
      (pin power_in line (at -33.02 40.64 0) (length 2.54)
        (name "GND")
        (number "14")
      )
      (pin output line (at 27.94 38.1 180) (length 2.54)
        (name "Ethernet_nLED3(3.3v)")
        (number "15")
      )
      (pin input line (at -33.02 38.1 0) (length 2.54)
        (name "Ethernet_SYNC_IN(1.8v)")
        (number "16")
      )
      (pin output line (at 27.94 35.56 180) (length 2.54)
        (name "Ethernet_nLED2(3.3v)")
        (number "17")
      )
      (pin input line (at -33.02 35.56 0) (length 2.54)
        (name "Ethernet_SYNC_OUT(1.8v)")
        (number "18")
      )
      (pin output line (at 27.94 33.02 180) (length 2.54)
        (name "Ethernet_nLED1(3.3v)")
        (number "19")
      )
      (pin power_in line (at -33.02 55.88 0) (length 2.54)
        (name "GND")
        (number "2")
      )
      (pin passive line (at -33.02 33.02 0) (length 2.54)
        (name "EEPROM_nWP")
        (number "20")
      )
      (pin open_collector line (at 27.94 30.48 180) (length 2.54)
        (name "PI_nLED_Activity")
        (number "21")
      )
      (pin power_in line (at -33.02 30.48 0) (length 2.54)
        (name "GND")
        (number "22")
      )
      (pin power_in line (at 27.94 27.94 180) (length 2.54)
        (name "GND")
        (number "23")
      )
      (pin passive line (at -33.02 27.94 0) (length 2.54)
        (name "GPIO26")
        (number "24")
      )
      (pin passive line (at 27.94 25.4 180) (length 2.54)
        (name "GPIO21")
        (number "25")
      )
      (pin passive line (at -33.02 25.4 0) (length 2.54)
        (name "GPIO19")
        (number "26")
      )
      (pin passive line (at 27.94 22.86 180) (length 2.54)
        (name "GPIO20")
        (number "27")
      )
      (pin passive line (at -33.02 22.86 0) (length 2.54)
        (name "GPIO13")
        (number "28")
      )
      (pin passive line (at 27.94 20.32 180) (length 2.54)
        (name "GPIO16")
        (number "29")
      )
      (pin passive line (at 27.94 53.34 180) (length 2.54)
        (name "Ethernet_Pair3_P")
        (number "3")
      )
      (pin passive line (at -33.02 20.32 0) (length 2.54)
        (name "GPIO6")
        (number "30")
      )
      (pin passive line (at 27.94 17.78 180) (length 2.54)
        (name "GPIO12")
        (number "31")
      )
      (pin power_in line (at -33.02 17.78 0) (length 2.54)
        (name "GND")
        (number "32")
      )
      (pin power_in line (at 27.94 15.24 180) (length 2.54)
        (name "GND")
        (number "33")
      )
      (pin passive line (at -33.02 15.24 0) (length 2.54)
        (name "GPIO5")
        (number "34")
      )
      (pin passive line (at 27.94 12.7 180) (length 2.54)
        (name "ID_SC")
        (number "35")
      )
      (pin passive line (at -33.02 12.7 0) (length 2.54)
        (name "ID_SD")
        (number "36")
      )
      (pin passive line (at 27.94 10.16 180) (length 2.54)
        (name "GPIO7")
        (number "37")
      )
      (pin passive line (at -33.02 10.16 0) (length 2.54)
        (name "GPIO11")
        (number "38")
      )
      (pin passive line (at 27.94 7.62 180) (length 2.54)
        (name "GPIO8")
        (number "39")
      )
      (pin passive line (at -33.02 53.34 0) (length 2.54)
        (name "Ethernet_Pair1_P")
        (number "4")
      )
      (pin passive line (at -33.02 7.62 0) (length 2.54)
        (name "GPIO9")
        (number "40")
      )
      (pin passive line (at 27.94 5.08 180) (length 2.54)
        (name "GPIO25")
        (number "41")
      )
      (pin power_in line (at -33.02 5.08 0) (length 2.54)
        (name "GND")
        (number "42")
      )
      (pin power_in line (at 27.94 2.54 180) (length 2.54)
        (name "GND")
        (number "43")
      )
      (pin passive line (at -33.02 2.54 0) (length 2.54)
        (name "GPIO10")
        (number "44")
      )
      (pin passive line (at 27.94 0 180) (length 2.54)
        (name "GPIO24")
        (number "45")
      )
      (pin passive line (at -33.02 0 0) (length 2.54)
        (name "GPIO22")
        (number "46")
      )
      (pin passive line (at 27.94 -2.54 180) (length 2.54)
        (name "GPIO23")
        (number "47")
      )
      (pin passive line (at -33.02 -2.54 0) (length 2.54)
        (name "GPIO27")
        (number "48")
      )
      (pin passive line (at 27.94 -5.08 180) (length 2.54)
        (name "GPIO18")
        (number "49")
      )
      (pin passive line (at 27.94 50.8 180) (length 2.54)
        (name "Ethernet_Pair3_N")
        (number "5")
      )
      (pin passive line (at -33.02 -5.08 0) (length 2.54)
        (name "GPIO17")
        (number "50")
      )
      (pin passive line (at 27.94 -7.62 180) (length 2.54)
        (name "GPIO15")
        (number "51")
      )
      (pin power_in line (at -33.02 -7.62 0) (length 2.54)
        (name "GND")
        (number "52")
      )
      (pin power_in line (at 27.94 -10.16 180) (length 2.54)
        (name "GND")
        (number "53")
      )
      (pin passive line (at -33.02 -10.16 0) (length 2.54)
        (name "GPIO4")
        (number "54")
      )
      (pin passive line (at 27.94 -12.7 180) (length 2.54)
        (name "GPIO14")
        (number "55")
      )
      (pin passive line (at -33.02 -12.7 0) (length 2.54)
        (name "GPIO3")
        (number "56")
      )
      (pin passive line (at 27.94 -15.24 180) (length 2.54)
        (name "SD_CLK")
        (number "57")
      )
      (pin passive line (at -33.02 -15.24 0) (length 2.54)
        (name "GPIO2")
        (number "58")
      )
      (pin power_in line (at 27.94 -17.78 180) (length 2.54)
        (name "GND")
        (number "59")
      )
      (pin passive line (at -33.02 50.8 0) (length 2.54)
        (name "Ethernet_Pair1_N")
        (number "6")
      )
      (pin power_in line (at -33.02 -17.78 0) (length 2.54)
        (name "GND")
        (number "60")
      )
      (pin passive line (at 27.94 -20.32 180) (length 2.54)
        (name "SD_DAT3")
        (number "61")
      )
      (pin passive line (at -33.02 -20.32 0) (length 2.54)
        (name "SD_CMD")
        (number "62")
      )
      (pin passive line (at 27.94 -22.86 180) (length 2.54)
        (name "SD_DAT0")
        (number "63")
      )
      (pin passive line (at -33.02 -22.86 0) (length 2.54)
        (name "SD_DAT5")
        (number "64")
      )
      (pin power_in line (at 27.94 -25.4 180) (length 2.54)
        (name "GND")
        (number "65")
      )
      (pin power_in line (at -33.02 -25.4 0) (length 2.54)
        (name "GND")
        (number "66")
      )
      (pin passive line (at 27.94 -27.94 180) (length 2.54)
        (name "SD_DAT1")
        (number "67")
      )
      (pin passive line (at -33.02 -27.94 0) (length 2.54)
        (name "SD_DAT4")
        (number "68")
      )
      (pin passive line (at 27.94 -30.48 180) (length 2.54)
        (name "SD_DAT2")
        (number "69")
      )
      (pin power_in line (at 27.94 48.26 180) (length 2.54)
        (name "GND")
        (number "7")
      )
      (pin passive line (at -33.02 -30.48 0) (length 2.54)
        (name "SD_DAT7")
        (number "70")
      )
      (pin power_in line (at 27.94 -33.02 180) (length 2.54)
        (name "GND")
        (number "71")
      )
      (pin passive line (at -33.02 -33.02 0) (length 2.54)
        (name "SD_DAT6")
        (number "72")
      )
      (pin input line (at 27.94 -35.56 180) (length 2.54)
        (name "SD_VDD_Override")
        (number "73")
      )
      (pin power_in line (at -33.02 -35.56 0) (length 2.54)
        (name "GND")
        (number "74")
      )
      (pin output line (at 27.94 -38.1 180) (length 2.54)
        (name "SD_PWR_ON")
        (number "75")
      )
      (pin passive line (at -33.02 -38.1 0) (length 2.54)
        (name "Reserved")
        (number "76")
      )
      (pin power_in line (at 27.94 -40.64 180) (length 2.54)
        (name "+5v_(Input)")
        (number "77")
      )
      (pin power_in line (at -33.02 -40.64 0) (length 2.54)
        (name "GPIO_VREF(1.8v/3.3v_Input)")
        (number "78")
      )
      (pin power_in line (at 27.94 -43.18 180) (length 2.54)
        (name "+5v_(Input)")
        (number "79")
      )
      (pin power_in line (at -33.02 48.26 0) (length 2.54)
        (name "GND")
        (number "8")
      )
      (pin passive line (at -33.02 -43.18 0) (length 2.54)
        (name "SCL0")
        (number "80")
      )
      (pin power_in line (at 27.94 -45.72 180) (length 2.54)
        (name "+5v_(Input)")
        (number "81")
      )
      (pin passive line (at -33.02 -45.72 0) (length 2.54)
        (name "SDA0")
        (number "82")
      )
      (pin power_in line (at 27.94 -48.26 180) (length 2.54)
        (name "+5v_(Input)")
        (number "83")
      )
      (pin power_out line (at -33.02 -48.26 0) (length 2.54)
        (name "+3.3v_(Output)")
        (number "84")
      )
      (pin power_in line (at 27.94 -50.8 180) (length 2.54)
        (name "+5v_(Input)")
        (number "85")
      )
      (pin power_out line (at -33.02 -50.8 0) (length 2.54)
        (name "+3.3v_(Output)")
        (number "86")
      )
      (pin power_in line (at 27.94 -53.34 180) (length 2.54)
        (name "+5v_(Input)")
        (number "87")
      )
      (pin power_out line (at -33.02 -53.34 0) (length 2.54)
        (name "+1.8v_(Output)")
        (number "88")
      )
      (pin power_in line (at 27.94 -55.88 180) (length 2.54)
        (name "WiFi_nDisable")
        (number "89")
      )
      (pin passive line (at 27.94 45.72 180) (length 2.54)
        (name "Ethernet_Pair2_N")
        (number "9")
      )
      (pin power_out line (at -33.02 -55.88 0) (length 2.54)
        (name "+1.8v_(Output)")
        (number "90")
      )
      (pin power_in line (at 27.94 -58.42 180) (length 2.54)
        (name "BT_nDisable")
        (number "91")
      )
      (pin passive line (at -33.02 -58.42 0) (length 2.54)
        (name "RUN_PG")
        (number "92")
      )
      (pin input line (at 27.94 -60.96 180) (length 2.54)
        (name "nRPIBOOT")
        (number "93")
      )
      (pin passive line (at -33.02 -60.96 0) (length 2.54)
        (name "AnalogIP0")
        (number "94")
      )
      (pin output line (at 27.94 -63.5 180) (length 2.54)
        (name "nPI_LED_PWR")
        (number "95")
      )
      (pin passive line (at -33.02 -63.5 0) (length 2.54)
        (name "AnalogIP1")
        (number "96")
      )
      (pin passive line (at 27.94 -66.04 180) (length 2.54)
        (name "Camera_GPIO")
        (number "97")
      )
      (pin power_in line (at -33.02 -66.04 0) (length 2.54)
        (name "GND")
        (number "98")
      )
      (pin input line (at 27.94 -68.58 180) (length 2.54)
        (name "Global_EN")
        (number "99")
      )
    )
    (symbol "ComputeModule4-CM4_2_1"
      (text "High Speed Serial" (at 140.97 0 0))
      (pin input line (at 170.18 60.96 180) (length 5.08)
        (name "USB_OTG_ID")
        (number "101")
      )
      (pin input line (at 109.22 60.96 0) (length 5.08)
        (name "PCIe_CLK_nREQ")
        (number "102")
      )
      (pin passive line (at 170.18 58.42 180) (length 5.08)
        (name "USB2_N")
        (number "103")
      )
      (pin passive line (at 109.22 58.42 0) (length 5.08)
        (name "Reserved")
        (number "104")
      )
      (pin passive line (at 170.18 55.88 180) (length 5.08)
        (name "USB2_P")
        (number "105")
      )
      (pin passive line (at 109.22 55.88 0) (length 5.08)
        (name "Reserved")
        (number "106")
      )
      (pin power_in line (at 170.18 53.34 180) (length 5.08)
        (name "GND")
        (number "107")
      )
      (pin power_in line (at 109.22 53.34 0) (length 5.08)
        (name "GND")
        (number "108")
      )
      (pin bidirectional line (at 170.18 50.8 180) (length 5.08)
        (name "PCIe_nRST")
        (number "109")
      )
      (pin output line (at 109.22 50.8 0) (length 5.08)
        (name "PCIe_CLK_P")
        (number "110")
      )
      (pin passive line (at 170.18 48.26 180) (length 5.08)
        (name "VDAC_COMP")
        (number "111")
      )
      (pin output line (at 109.22 48.26 0) (length 5.08)
        (name "PCIe_CLK_N")
        (number "112")
      )
      (pin power_in line (at 170.18 45.72 180) (length 5.08)
        (name "GND")
        (number "113")
      )
      (pin power_in line (at 109.22 45.72 0) (length 5.08)
        (name "GND")
        (number "114")
      )
      (pin input line (at 170.18 43.18 180) (length 5.08)
        (name "CAM1_D0_N")
        (number "115")
      )
      (pin input line (at 109.22 43.18 0) (length 5.08)
        (name "PCIe_RX_P")
        (number "116")
      )
      (pin input line (at 170.18 40.64 180) (length 5.08)
        (name "CAM1_D0_P")
        (number "117")
      )
      (pin input line (at 109.22 40.64 0) (length 5.08)
        (name "PCIe_RX_N")
        (number "118")
      )
      (pin power_in line (at 170.18 38.1 180) (length 5.08)
        (name "GND")
        (number "119")
      )
      (pin power_in line (at 109.22 38.1 0) (length 5.08)
        (name "GND")
        (number "120")
      )
      (pin input line (at 170.18 35.56 180) (length 5.08)
        (name "CAM1_D1_N")
        (number "121")
      )
      (pin output line (at 109.22 35.56 0) (length 5.08)
        (name "PCIe_TX_P")
        (number "122")
      )
      (pin input line (at 170.18 33.02 180) (length 5.08)
        (name "CAM1_D1_P")
        (number "123")
      )
      (pin output line (at 109.22 33.02 0) (length 5.08)
        (name "PCIe_TX_N")
        (number "124")
      )
      (pin power_in line (at 170.18 30.48 180) (length 5.08)
        (name "GND")
        (number "125")
      )
      (pin power_in line (at 109.22 30.48 0) (length 5.08)
        (name "GND")
        (number "126")
      )
      (pin input line (at 170.18 27.94 180) (length 5.08)
        (name "CAM1_C_N")
        (number "127")
      )
      (pin input line (at 109.22 27.94 0) (length 5.08)
        (name "CAM0_D0_N")
        (number "128")
      )
      (pin input line (at 170.18 25.4 180) (length 5.08)
        (name "CAM1_C_P")
        (number "129")
      )
      (pin input line (at 109.22 25.4 0) (length 5.08)
        (name "CAM0_D0_P")
        (number "130")
      )
      (pin power_in line (at 170.18 22.86 180) (length 5.08)
        (name "GND")
        (number "131")
      )
      (pin power_in line (at 109.22 22.86 0) (length 5.08)
        (name "GND")
        (number "132")
      )
      (pin input line (at 170.18 20.32 180) (length 5.08)
        (name "CAM1_D2_N")
        (number "133")
      )
      (pin input line (at 109.22 20.32 0) (length 5.08)
        (name "CAM0_D1_N")
        (number "134")
      )
      (pin input line (at 170.18 17.78 180) (length 5.08)
        (name "CAM1_D2_P")
        (number "135")
      )
      (pin input line (at 109.22 17.78 0) (length 5.08)
        (name "CAM0_D1_P")
        (number "136")
      )
      (pin power_in line (at 170.18 15.24 180) (length 5.08)
        (name "GND")
        (number "137")
      )
      (pin power_in line (at 109.22 15.24 0) (length 5.08)
        (name "GND")
        (number "138")
      )
      (pin input line (at 170.18 12.7 180) (length 5.08)
        (name "CAM1_D3_N")
        (number "139")
      )
      (pin input line (at 109.22 12.7 0) (length 5.08)
        (name "CAM0_C_N")
        (number "140")
      )
      (pin input line (at 170.18 10.16 180) (length 5.08)
        (name "CAM1_D3_P")
        (number "141")
      )
      (pin input line (at 109.22 10.16 0) (length 5.08)
        (name "CAM0_C_P")
        (number "142")
      )
      (pin input line (at 170.18 7.62 180) (length 5.08)
        (name "HDMI1_HOTPLUG")
        (number "143")
      )
      (pin power_in line (at 109.22 7.62 0) (length 5.08)
        (name "GND")
        (number "144")
      )
      (pin bidirectional line (at 170.18 5.08 180) (length 5.08)
        (name "HDMI1_SDA")
        (number "145")
      )
      (pin output line (at 109.22 5.08 0) (length 5.08)
        (name "HDMI1_TX2_P")
        (number "146")
      )
      (pin open_collector line (at 170.18 2.54 180) (length 5.08)
        (name "HDMI1_SCL")
        (number "147")
      )
      (pin output line (at 109.22 2.54 0) (length 5.08)
        (name "HDMI1_TX2_N")
        (number "148")
      )
      (pin open_collector line (at 170.18 0 180) (length 5.08)
        (name "HDMI1_CEC")
        (number "149")
      )
      (pin power_in line (at 109.22 0 0) (length 5.08)
        (name "GND")
        (number "150")
      )
      (pin open_collector line (at 170.18 -2.54 180) (length 5.08)
        (name "HDMI0_CEC")
        (number "151")
      )
      (pin output line (at 109.22 -2.54 0) (length 5.08)
        (name "HDMI1_TX1_P")
        (number "152")
      )
      (pin input line (at 170.18 -5.08 180) (length 5.08)
        (name "HDMI0_HOTPLUG")
        (number "153")
      )
      (pin output line (at 109.22 -5.08 0) (length 5.08)
        (name "HDMI1_TX1_N")
        (number "154")
      )
      (pin power_in line (at 170.18 -7.62 180) (length 5.08)
        (name "GND")
        (number "155")
      )
      (pin power_in line (at 109.22 -7.62 0) (length 5.08)
        (name "GND")
        (number "156")
      )
      (pin output line (at 170.18 -10.16 180) (length 5.08)
        (name "DSI0_D0_N")
        (number "157")
      )
      (pin output line (at 109.22 -10.16 0) (length 5.08)
        (name "HDMI1_TX0_P")
        (number "158")
      )
      (pin output line (at 170.18 -12.7 180) (length 5.08)
        (name "DSI0_D0_P")
        (number "159")
      )
      (pin output line (at 109.22 -12.7 0) (length 5.08)
        (name "HDMI1_TX0_N")
        (number "160")
      )
      (pin power_in line (at 170.18 -15.24 180) (length 5.08)
        (name "GND")
        (number "161")
      )
      (pin power_in line (at 109.22 -15.24 0) (length 5.08)
        (name "GND")
        (number "162")
      )
      (pin output line (at 170.18 -17.78 180) (length 5.08)
        (name "DSI0_D1_N")
        (number "163")
      )
      (pin output line (at 109.22 -17.78 0) (length 5.08)
        (name "HDMI1_CLK_P")
        (number "164")
      )
      (pin output line (at 170.18 -20.32 180) (length 5.08)
        (name "DSI0_D1_P")
        (number "165")
      )
      (pin output line (at 109.22 -20.32 0) (length 5.08)
        (name "HDMI1_CLK_N")
        (number "166")
      )
      (pin power_in line (at 170.18 -22.86 180) (length 5.08)
        (name "GND")
        (number "167")
      )
      (pin power_in line (at 109.22 -22.86 0) (length 5.08)
        (name "GND")
        (number "168")
      )
      (pin output line (at 170.18 -25.4 180) (length 5.08)
        (name "DSI0_C_N")
        (number "169")
      )
      (pin output line (at 109.22 -25.4 0) (length 5.08)
        (name "HDMI0_TX2_P")
        (number "170")
      )
      (pin output line (at 170.18 -27.94 180) (length 5.08)
        (name "DSI0_C_P")
        (number "171")
      )
      (pin output line (at 109.22 -27.94 0) (length 5.08)
        (name "HDMI0_TX2_N")
        (number "172")
      )
      (pin power_in line (at 170.18 -30.48 180) (length 5.08)
        (name "GND")
        (number "173")
      )
      (pin power_in line (at 109.22 -30.48 0) (length 5.08)
        (name "GND")
        (number "174")
      )
      (pin output line (at 170.18 -33.02 180) (length 5.08)
        (name "DSI1_D0_N")
        (number "175")
      )
      (pin output line (at 109.22 -33.02 0) (length 5.08)
        (name "HDMI0_TX1_P")
        (number "176")
      )
      (pin output line (at 170.18 -35.56 180) (length 5.08)
        (name "DSI1_D0_P")
        (number "177")
      )
      (pin output line (at 109.22 -35.56 0) (length 5.08)
        (name "HDMI0_TX1_N")
        (number "178")
      )
      (pin power_in line (at 170.18 -38.1 180) (length 5.08)
        (name "GND")
        (number "179")
      )
      (pin power_in line (at 109.22 -38.1 0) (length 5.08)
        (name "GND")
        (number "180")
      )
      (pin output line (at 170.18 -40.64 180) (length 5.08)
        (name "DSI1_D1_N")
        (number "181")
      )
      (pin output line (at 109.22 -40.64 0) (length 5.08)
        (name "HDMI0_TX0_P")
        (number "182")
      )
      (pin output line (at 170.18 -43.18 180) (length 5.08)
        (name "DSI1_D1_P")
        (number "183")
      )
      (pin output line (at 109.22 -43.18 0) (length 5.08)
        (name "HDMI0_TX0_N")
        (number "184")
      )
      (pin power_in line (at 170.18 -45.72 180) (length 5.08)
        (name "GND")
        (number "185")
      )
      (pin power_in line (at 109.22 -45.72 0) (length 5.08)
        (name "GND")
        (number "186")
      )
      (pin output line (at 170.18 -48.26 180) (length 5.08)
        (name "DSI1_C_N")
        (number "187")
      )
      (pin output line (at 109.22 -48.26 0) (length 5.08)
        (name "HDMI0_CLK_P")
        (number "188")
      )
      (pin output line (at 170.18 -50.8 180) (length 5.08)
        (name "DSI1_C_P")
        (number "189")
      )
      (pin output line (at 109.22 -50.8 0) (length 5.08)
        (name "HDMI0_CLK_N")
        (number "190")
      )
      (pin power_in line (at 170.18 -53.34 180) (length 5.08)
        (name "GND")
        (number "191")
      )
      (pin power_in line (at 109.22 -53.34 0) (length 5.08)
        (name "GND")
        (number "192")
      )
      (pin output line (at 170.18 -55.88 180) (length 5.08)
        (name "DSI1_D2_N")
        (number "193")
      )
      (pin output line (at 109.22 -55.88 0) (length 5.08)
        (name "DSI1_D3_N")
        (number "194")
      )
      (pin output line (at 170.18 -58.42 180) (length 5.08)
        (name "DSI1_D2_P")
        (number "195")
      )
      (pin output line (at 109.22 -58.42 0) (length 5.08)
        (name "DSI1_D3_P")
        (number "196")
      )
      (pin power_in line (at 170.18 -60.96 180) (length 5.08)
        (name "GND")
        (number "197")
      )
      (pin power_in line (at 109.22 -60.96 0) (length 5.08)
        (name "GND")
        (number "198")
      )
      (pin bidirectional line (at 170.18 -63.5 180) (length 5.08)
        (name "HDMI0_SDA")
        (number "199")
      )
      (pin open_collector line (at 109.22 -63.5 0) (length 5.08)
        (name "HDMI0_SCL")
        (number "200")
      )
    )
  )
  (symbol "CM4IO:EMC2301"
    (property "Reference" "U" (id 0) (at -7.62 13.97 0))
    (property "Value" "EMC2301" (id 1) (at -1.27 -1.27 0))
    (property "Footprint" "" (id 2) (at 0 0 0))
    (property "Datasheet" "" (id 3) (at 0 0 0))
    (symbol "EMC2301_0_1")
    (symbol "EMC2301_0_0"
      (pin open_collector line (at -11.43 10.16 0) (length 2.54)
        (name "SDA")
        (number "1")
      )
      (pin open_collector line (at -11.43 7.62 0) (length 2.54)
        (name "SCL")
        (number "2")
      )
      (pin power_in line (at -11.43 5.08 0) (length 2.54)
        (name "VDD")
        (number "3")
      )
      (pin power_in line (at -11.43 2.54 0) (length 2.54)
        (name "GND")
        (number "4")
      )
      (pin output line (at 7.62 2.54 180) (length 2.54)
        (name "PWM")
        (number "5")
      )
      (pin input line (at 7.62 5.08 180) (length 2.54)
        (name "TACH")
        (number "6")
      )
      (pin input line (at 7.62 7.62 180) (length 2.54)
        (name "CLK")
        (number "7")
      )
      (pin open_collector line (at 7.62 10.16 180) (length 2.54)
        (name "nALERT")
        (number "8")
      )
    )
  )
  (symbol "CM4IO:FSUSB42MX"
    (property "Reference" "U" (id 0) (at -7.62 20.32 0))
    (property "Value" "FSUSB42MX" (id 1) (at -2.54 -2.54 0))
    (property "Footprint" "" (id 2) (at 0 0 0))
    (property "Datasheet" "" (id 3) (at 0 0 0))
    (symbol "FSUSB42MX_0_1")
    (symbol "FSUSB42MX_0_0"
      (pin power_in line (at 8.89 16.51 180) (length 2.54)
        (name "VCC")
        (number "1")
      )
      (pin input line (at 8.89 3.81 180) (length 2.54)
        (name "nOE")
        (number "10")
      )
      (pin input line (at 8.89 13.97 180) (length 2.54)
        (name "SEL")
        (number "2")
      )
      (pin bidirectional line (at 8.89 10.16 180) (length 2.54)
        (name "D_P")
        (number "3")
      )
      (pin bidirectional line (at 8.89 7.62 180) (length 2.54)
        (name "D_N")
        (number "4")
      )
      (pin power_in line (at 8.89 1.27 180) (length 2.54)
        (name "GND")
        (number "5")
      )
      (pin bidirectional line (at -11.43 13.97 0) (length 2.54)
        (name "HSD0_M")
        (number "6")
      )
      (pin bidirectional line (at -11.43 16.51 0) (length 2.54)
        (name "HSD0_P")
        (number "7")
      )
      (pin bidirectional line (at -11.43 1.27 0) (length 2.54)
        (name "HSD1_M")
        (number "8")
      )
      (pin bidirectional line (at -11.43 3.81 0) (length 2.54)
        (name "HSD1_P")
        (number "9")
      )
    )
  )
  (symbol "CM4IO:HDMI_A_1.4"
    (property "Reference" "J" (id 0) (at -6.35 26.67 0))
    (property "Value" "HDMI_A_1.4" (id 1) (at 10.16 26.67 0))
    (property "Footprint" "" (id 2) (at 0.635 0 0))
    (property "Datasheet" "https://en.wikipedia.org/wiki/HDMI" (id 3) (at 0.635 0 0))
    (property "ki_keywords" "hdmi conn" (id 4) (at 0 0 0))
    (property "ki_description" "HDMI 1.4+ type A connector" (id 5) (at 0 0 0))
    (property "ki_fp_filters" "HDMI*A*" (id 6) (at 0 0 0))
    (symbol "HDMI_A_1.4_0_1")
    (symbol "HDMI_A_1.4_0_0"
      (pin passive line (at 7.62 -27.94 90) (length 2.54)
        (name "SH")
        (number "SH2")
      )
      (pin passive line (at 7.62 -27.94 90) (length 2.54)
        (name "SH")
        (number "SH3")
      )
      (pin passive line (at 7.62 -27.94 90) (length 2.54)
        (name "SH")
        (number "SH4")
      )
    )
    (symbol "HDMI_A_1.4_1_1"
      (pin passive line (at -10.16 20.32 0) (length 2.54)
        (name "D2+")
        (number "1")
      )
      (pin passive line (at -10.16 5.08 0) (length 2.54)
        (name "CK+")
        (number "10")
      )
      (pin power_in line (at 2.54 -27.94 90) (length 2.54)
        (name "CKS")
        (number "11")
      )
      (pin passive line (at -10.16 2.54 0) (length 2.54)
        (name "CK-")
        (number "12")
      )
      (pin bidirectional line (at -10.16 -2.54 0) (length 2.54)
        (name "CEC")
        (number "13")
      )
      (pin passive line (at -10.16 -15.24 0) (length 2.54)
        (name "UTILITY/HEAC+")
        (number "14")
      )
      (pin passive line (at -10.16 -7.62 0) (length 2.54)
        (name "SCL")
        (number "15")
      )
      (pin bidirectional line (at -10.16 -10.16 0) (length 2.54)
        (name "SDA")
        (number "16")
      )
      (pin power_in line (at 5.08 -27.94 90) (length 2.54)
        (name "GND")
        (number "17")
      )
      (pin power_in line (at 0 27.94 270) (length 2.54)
        (name "+5V")
        (number "18")
      )
      (pin passive line (at -10.16 -17.78 0) (length 2.54)
        (name "HPD/HEAC-")
        (number "19")
      )
      (pin power_in line (at -5.08 -27.94 90) (length 2.54)
        (name "D2S")
        (number "2")
      )
      (pin passive line (at -10.16 17.78 0) (length 2.54)
        (name "D2-")
        (number "3")
      )
      (pin passive line (at -10.16 15.24 0) (length 2.54)
        (name "D1+")
        (number "4")
      )
      (pin power_in line (at -2.54 -27.94 90) (length 2.54)
        (name "D1S")
        (number "5")
      )
      (pin passive line (at -10.16 12.7 0) (length 2.54)
        (name "D1-")
        (number "6")
      )
      (pin passive line (at -10.16 10.16 0) (length 2.54)
        (name "D0+")
        (number "7")
      )
      (pin power_in line (at 0 -27.94 90) (length 2.54)
        (name "D0S")
        (number "8")
      )
      (pin passive line (at -10.16 7.62 0) (length 2.54)
        (name "D0-")
        (number "9")
      )
      (pin passive line (at 7.62 -27.94 90) (length 2.54)
        (name "SH")
        (number "SH1")
      )
    )
  )
  (symbol "CM4IO:MagJack-A70-112-331N126"
    (property "Reference" "U" (id 0) (at 0 0 0))
    (property "Value" "MagJack-A70-112-331N126" (id 1) (at 0 0 0))
    (property "Footprint" "" (id 2) (at 0 0 0))
    (property "Datasheet" "" (id 3) (at 0 0 0))
    (symbol "MagJack-A70-112-331N126_1_1"
      (text "1000pF" (at 6.35 17.399 0))
      (text "75" (at 8.89 13.335 900))
      (text "C1" (at 6.985 71.755 0))
      (text "C2" (at 6.985 66.675 0))
      (text "C3" (at 6.985 64.135 0))
      (text "C4" (at 6.985 51.435 0))
      (text "C5" (at 6.985 46.355 0))
      (text "C6" (at 6.985 59.055 0))
      (text "C7" (at 6.985 43.815 0))
      (text "C8" (at 6.985 38.735 0))
      (text "GREEN" (at -4.445 12.7 0))
      (text "YELLOW" (at -4.445 17.78 0))
      (pin passive line (at -21.59 71.12 0) (length 3.81)
        (name "TRD0+")
        (number "1")
      )
      (pin passive line (at -21.59 38.1 0) (length 3.81)
        (name "TRD3-")
        (number "10")
      )
      (pin passive line (at -21.59 33.02 0) (length 3.81)
        (name "VC1")
        (number "11")
      )
      (pin passive line (at -21.59 30.48 0) (length 3.81)
        (name "VC2")
        (number "12")
      )
      (pin passive line (at -21.59 27.94 0) (length 3.81)
        (name "VC3")
        (number "13")
      )
      (pin passive line (at -21.59 25.4 0) (length 3.81)
        (name "VC4")
        (number "14")
      )
      (pin passive line (at -21.59 20.32 0) (length 3.81)
        (name "LEDY_A")
        (number "15")
      )
      (pin passive line (at -21.59 17.78 0) (length 3.81)
        (name "LEDY_K")
        (number "16")
      )
      (pin passive line (at -21.59 15.24 0) (length 3.81)
        (name "LEDG_A")
        (number "17")
      )
      (pin passive line (at -21.59 12.7 0) (length 3.81)
        (name "LEDG_K")
        (number "18")
      )
      (pin passive line (at -21.59 7.62 0) (length 3.81)
        (name "SHIELD")
        (number "19")
      )
      (pin passive line (at -21.59 66.04 0) (length 3.81)
        (name "TRD0-")
        (number "2")
      )
      (pin passive line (at -21.59 5.08 0) (length 3.81)
        (name "SHIELD")
        (number "20")
      )
      (pin passive line (at -21.59 63.5 0) (length 3.81)
        (name "TRD1+")
        (number "3")
      )
      (pin passive line (at -21.59 55.88 0) (length 3.81)
        (name "CT")
        (number "4")
      )
      (pin passive line (at -21.59 53.34 0) (length 3.81)
        (name "CT")
        (number "5")
      )
      (pin passive line (at -21.59 58.42 0) (length 3.81)
        (name "TRD1-")
        (number "6")
      )
      (pin passive line (at -21.59 50.8 0) (length 3.81)
        (name "TRD2+")
        (number "7")
      )
      (pin passive line (at -21.59 45.72 0) (length 3.81)
        (name "TRD2-")
        (number "8")
      )
      (pin passive line (at -21.59 43.18 0) (length 3.81)
        (name "TRD3+")
        (number "9")
      )
    )
    (symbol "MagJack-A70-112-331N126_0_1")
  )
  (symbol "CM4IO:PCIe-x1"
    (property "Reference" "J" (id 0) (at -13.97 36.83 0))
    (property "Value" "PCIe-x1" (id 1) (at -5.08 -13.97 0))
    (property "Footprint" "" (id 2) (at 0 0 0))
    (property "Datasheet" "" (id 3) (at 0 0 0))
    (symbol "PCIe-x1_0_1")
    (symbol "PCIe-x1_0_0"
      (pin passive line (at 10.16 33.02 180) (length 5.08)
        (name "nPRSNT1")
        (number "A1")
      )
      (pin power_in line (at 10.16 10.16 180) (length 5.08)
        (name "+3.3V")
        (number "A10")
      )
      (pin input line (at 10.16 7.62 180) (length 5.08)
        (name "nPERST")
        (number "A11")
      )
      (pin power_in line (at 10.16 5.08 180) (length 5.08)
        (name "GND")
        (number "A12")
      )
      (pin input line (at 10.16 2.54 180) (length 5.08)
        (name "REFCLK+")
        (number "A13")
      )
      (pin input line (at 10.16 0 180) (length 5.08)
        (name "REFCLK-")
        (number "A14")
      )
      (pin power_in line (at 10.16 -2.54 180) (length 5.08)
        (name "GND")
        (number "A15")
      )
      (pin output line (at 10.16 -5.08 180) (length 5.08)
        (name "PERP0")
        (number "A16")
      )
      (pin output line (at 10.16 -7.62 180) (length 5.08)
        (name "PERN0")
        (number "A17")
      )
      (pin power_in line (at 10.16 -10.16 180) (length 5.08)
        (name "GND")
        (number "A18")
      )
      (pin power_in line (at 10.16 30.48 180) (length 5.08)
        (name "+12V")
        (number "A2")
      )
      (pin power_in line (at 10.16 27.94 180) (length 5.08)
        (name "+12V")
        (number "A3")
      )
      (pin power_in line (at 10.16 25.4 180) (length 5.08)
        (name "GND")
        (number "A4")
      )
      (pin input line (at 10.16 22.86 180) (length 5.08)
        (name "TCK")
        (number "A5")
      )
      (pin input line (at 10.16 20.32 180) (length 5.08)
        (name "TDI")
        (number "A6")
      )
      (pin output line (at 10.16 17.78 180) (length 5.08)
        (name "TD0")
        (number "A7")
      )
      (pin input line (at 10.16 15.24 180) (length 5.08)
        (name "TMS")
        (number "A8")
      )
      (pin power_in line (at 10.16 12.7 180) (length 5.08)
        (name "+3.3V")
        (number "A9")
      )
      (pin power_in line (at -19.05 33.02 0) (length 5.08)
        (name "+12v")
        (number "B1")
      )
      (pin power_in line (at -19.05 10.16 0) (length 5.08)
        (name "+3.3vAUX")
        (number "B10")
      )
      (pin open_collector line (at -19.05 7.62 0) (length 5.08)
        (name "nWAKE")
        (number "B11")
      )
      (pin open_collector line (at -19.05 5.08 0) (length 5.08)
        (name "nCLKREQ")
        (number "B12")
      )
      (pin power_in line (at -19.05 2.54 0) (length 5.08)
        (name "GND")
        (number "B13")
      )
      (pin input line (at -19.05 0 0) (length 5.08)
        (name "PETP0")
        (number "B14")
      )
      (pin input line (at -19.05 -2.54 0) (length 5.08)
        (name "PETN0")
        (number "B15")
      )
      (pin power_in line (at -19.05 -5.08 0) (length 5.08)
        (name "GND")
        (number "B16")
      )
      (pin passive line (at -19.05 -7.62 0) (length 5.08)
        (name "nPRSNT2")
        (number "B17")
      )
      (pin power_in line (at -19.05 -10.16 0) (length 5.08)
        (name "GND")
        (number "B18")
      )
      (pin power_in line (at -19.05 30.48 0) (length 5.08)
        (name "+12v")
        (number "B2")
      )
      (pin power_in line (at -19.05 27.94 0) (length 5.08)
        (name "+12v")
        (number "B3")
      )
      (pin power_in line (at -19.05 25.4 0) (length 5.08)
        (name "GND")
        (number "B4")
      )
      (pin passive line (at -19.05 22.86 0) (length 5.08)
        (name "SMCLK")
        (number "B5")
      )
      (pin passive line (at -19.05 20.32 0) (length 5.08)
        (name "SMDAT")
        (number "B6")
      )
      (pin power_in line (at -19.05 17.78 0) (length 5.08)
        (name "GND")
        (number "B7")
      )
      (pin power_in line (at -19.05 15.24 0) (length 5.08)
        (name "+3.3v")
        (number "B8")
      )
      (pin input line (at -19.05 12.7 0) (length 5.08)
        (name "nTRST")
        (number "B9")
      )
    )
  )
  (symbol "CM4IO:RT9742SNGV"
    (property "Reference" "U" (id 0) (at -2.54 7.62 0))
    (property "Value" "RT9742SNGV" (id 1) (at 3.81 -5.08 0))
    (property "Footprint" "" (id 2) (at 0 0 0))
    (property "Datasheet" "" (id 3) (at 0 0 0))
    (symbol "RT9742SNGV_0_1")
    (symbol "RT9742SNGV_1_1"
      (pin power_in line (at -5.08 3.81 0) (length 2.54)
        (name "IN")
        (number "1")
      )
      (pin power_in line (at 10.16 3.81 180) (length 2.54)
        (name "OUT")
        (number "2")
      )
      (pin power_in line (at -5.08 -2.54 0) (length 2.54)
        (name "GND")
        (number "3")
      )
    )
  )
  (symbol "CM4IO:TPD4EUSB30" (pin_names (offset 0))
    (property "Reference" "U" (id 0) (at -0.635 8.89 0))
    (property "Value" "TPD4EUSB30" (id 1) (at 8.89 -10.16 0))
    (property "Footprint" "Package_SON:USON-10_2.5x1.0mm_P0.5mm" (id 2) (at -24.13 -10.16 0))
    (property "Datasheet" "http://www.ti.com/lit/ds/symlink/tpd2eusb30a.pdf" (id 3) (at 0 0 0))
    (property "ki_keywords" "ESD protection USB 3.0" (id 4) (at 0 0 0))
    (property "ki_description" "4-Channel ESD Protection for Super-Speed USB 3.0 Interface, USON-10" (id 5) (at 0 0 0))
    (property "ki_fp_filters" "USON*2.5x1.0mm*P0.5mm*" (id 6) (at 0 0 0))
    (symbol "TPD4EUSB30_0_1")
    (symbol "TPD4EUSB30_0_0")
    (symbol "TPD4EUSB30_1_1"
      (pin passive line (at -12.7 2.54 0) (length 5.08)
        (name "D1+")
        (number "1")
      )
      (pin passive line (at -12.7 2.54 0) (length 5.08) hide
        (name "~")
        (number "10")
      )
      (pin passive line (at -12.7 -2.54 0) (length 5.08)
        (name "D1-")
        (number "2")
      )
      (pin power_in line (at 0 -12.7 90) (length 5.08)
        (name "GND")
        (number "3")
      )
      (pin passive line (at 12.7 2.54 180) (length 5.08)
        (name "D2+")
        (number "4")
      )
      (pin passive line (at 12.7 -2.54 180) (length 5.08)
        (name "D2-")
        (number "5")
      )
      (pin passive line (at 12.7 -2.54 180) (length 5.08) hide
        (name "~")
        (number "6")
      )
      (pin passive line (at 12.7 2.54 180) (length 5.08) hide
        (name "~")
        (number "7")
      )
      (pin passive line (at 0 -12.7 90) (length 5.08) hide
        (name "GND")
        (number "8")
      )
      (pin passive line (at -12.7 -2.54 0) (length 5.08) hide
        (name "~")
        (number "9")
      )
    )
  )
  (symbol "CM4IO:USB3_A"
    (property "Reference" "J" (id 0) (at -10.16 33.02 0))
    (property "Value" "USB3_A" (id 1) (at 10.16 33.02 0))
    (property "Footprint" "" (id 2) (at 3.81 20.32 0))
    (property "Datasheet" "~" (id 3) (at 3.81 20.32 0))
    (property "ki_keywords" "usb universal serial bus" (id 4) (at 0 0 0))
    (property "ki_description" "USB 3.0 A connector" (id 5) (at 0 0 0))
    (symbol "USB3_A_1_1"
      (text "SS" (at 4.572 3.175 900))
      (pin passive line (at 13.97 -36.83 180) (length 2.54)
        (name "SHIELD")
        (number "10")
      )
      (pin power_in line (at -11.43 26.67 0) (length 2.54)
        (name "VBUS")
        (number "A1")
      )
      (pin bidirectional line (at -11.43 19.05 0) (length 2.54)
        (name "D-")
        (number "A2")
      )
      (pin bidirectional line (at -11.43 21.59 0) (length 2.54)
        (name "D+")
        (number "A3")
      )
      (pin power_in line (at -11.43 0 0) (length 2.54)
        (name "GND")
        (number "A4")
      )
      (pin bidirectional line (at -11.43 11.43 0) (length 2.54)
        (name "SSRX-")
        (number "A5")
      )
      (pin bidirectional line (at -11.43 13.97 0) (length 2.54)
        (name "SSRX+")
        (number "A6")
      )
      (pin power_in line (at -11.43 -2.54 0) (length 2.54)
        (name "DRAIN")
        (number "A7")
      )
      (pin bidirectional line (at -11.43 3.81 0) (length 2.54)
        (name "SSTX-")
        (number "A8")
      )
      (pin bidirectional line (at -11.43 6.35 0) (length 2.54)
        (name "SSTX+")
        (number "A9")
      )
      (pin power_in line (at -11.43 -7.62 0) (length 2.54)
        (name "VBUS")
        (number "B1")
      )
      (pin bidirectional line (at -11.43 -15.24 0) (length 2.54)
        (name "D-")
        (number "B2")
      )
      (pin bidirectional line (at -11.43 -12.7 0) (length 2.54)
        (name "D+")
        (number "B3")
      )
      (pin power_in line (at -11.43 -34.29 0) (length 2.54)
        (name "GND")
        (number "B4")
      )
      (pin bidirectional line (at -11.43 -22.86 0) (length 2.54)
        (name "SSRX-")
        (number "B5")
      )
      (pin bidirectional line (at -11.43 -20.32 0) (length 2.54)
        (name "SSRX+")
        (number "B6")
      )
      (pin power_in line (at -11.43 -36.83 0) (length 2.54)
        (name "DRAIN")
        (number "B7")
      )
      (pin bidirectional line (at -11.43 -30.48 0) (length 2.54)
        (name "SSTX-")
        (number "B8")
      )
      (pin bidirectional line (at -11.43 -27.94 0) (length 2.54)
        (name "SSTX+")
        (number "B9")
      )
    )
  )
  (symbol "CM4IO:USB_67298-4090" (pin_numbers hide)
    (property "Reference" "J" (id 0) (at -5.08 21.6408 0))
    (property "Value" "USB_67298-4090" (id 1) (at -5.08 -17.8054 0))
    (property "Footprint" "CM4IO:MOLEX_USB_67298-4090" (id 2) (at 0 0 0))
    (property "Datasheet" "Conn USB Type A RCP 4/4 POS Solder RA Thru-Hole 8 Terminal 2 Port Tray" (id 3) (at 0 0 0))
    (property "Field4" "Farnell" (id 4) (at 0 0 0))
    (property "Field5" "2751688" (id 5) (at 0 0 0))
    (property "Field6" "None" (id 6) (at 0 0 0))
    (property "Field7" "Molex" (id 7) (at 0 0 0))
    (property "Field8" "None" (id 8) (at 0 0 0))
    (symbol "USB_67298-4090_0_0"
      (pin power_in line (at -7.62 -2.54 0) (length 7.62)
        (name "VBUS`")
        (number "1")
      )
      (pin passive line (at -7.62 -5.08 0) (length 7.62)
        (name "D-`")
        (number "2")
      )
      (pin passive line (at -7.62 -7.62 0) (length 7.62)
        (name "D+`")
        (number "3")
      )
      (pin power_in line (at -7.62 -10.16 0) (length 7.62)
        (name "GND`")
        (number "4")
      )
      (pin power_in line (at -7.62 15.24 0) (length 7.62)
        (name "VBUS")
        (number "5")
      )
      (pin passive line (at -7.62 12.7 0) (length 7.62)
        (name "D-")
        (number "6")
      )
      (pin passive line (at -7.62 10.16 0) (length 7.62)
        (name "D+")
        (number "7")
      )
      (pin power_in line (at -7.62 7.62 0) (length 7.62)
        (name "GND")
        (number "8")
      )
      (pin passive line (at 12.7 -12.7 180) (length 2.54)
        (name "MT1")
        (number "MT1")
      )
      (pin passive line (at 12.7 -10.16 180) (length 2.54)
        (name "MT2")
        (number "MT2")
      )
      (pin passive line (at 12.7 -7.62 180) (length 2.54)
        (name "MT3")
        (number "MT3")
      )
      (pin passive line (at 12.7 -5.08 180) (length 2.54)
        (name "MT4")
        (number "MT4")
      )
    )
  )
)
