(kicad_pcb (version 20201116) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (color "Green") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (color "Green") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "GND")
  (net 2 "/+12v")
  (net 3 "/+5v")
  (net 4 "/pcie+3.3v")
  (net 5 "Net-(C5-Pad1)")
  (net 6 "Net-(C6-Pad1)")
  (net 7 "Net-(C7-Pad1)")
  (net 8 "/+3.3v")
  (net 9 "Net-(D2-Pad1)")
  (net 10 "Net-(D16-Pad1)")
  (net 11 "Net-(D17-Pad1)")
  (net 12 "Net-(D18-Pad1)")
  (net 13 "Net-(D20-Pad1)")
  (net 14 "/SDA0")
  (net 15 "/SCL0")
  (net 16 "no_connect_183")
  (net 17 "no_connect_182")
  (net 18 "/DSI1_D3_P")
  (net 19 "/DSI1_D3_N")
  (net 20 "/DSI1_D2_P")
  (net 21 "/DSI1_D2_N")
  (net 22 "/DSI1_C_P")
  (net 23 "/DSI1_C_N")
  (net 24 "/DSI1_D1_P")
  (net 25 "/DSI1_D1_N")
  (net 26 "/DSI1_D0_P")
  (net 27 "/DSI1_D0_N")
  (net 28 "/TRD2_P")
  (net 29 "/TRD2_N")
  (net 30 "/TRD3_N")
  (net 31 "/TRD3_P")
  (net 32 "/TRD1_P")
  (net 33 "/TRD1_N")
  (net 34 "/TRD0_N")
  (net 35 "/TRD0_P")
  (net 36 "/HDMI1_D2_P")
  (net 37 "/HDMI1_D2_N")
  (net 38 "/HDMI1_D1_P")
  (net 39 "/HDMI1_D1_N")
  (net 40 "/HDMI1_D0_P")
  (net 41 "/HDMI1_D0_N")
  (net 42 "/HDMI1_CK_P")
  (net 43 "/HDMI1_CK_N")
  (net 44 "/HDMI1_CEC")
  (net 45 "no_connect_192")
  (net 46 "/HDMI1_SCL")
  (net 47 "/HDMI1_SDA")
  (net 48 "/HDMI1_HOTPLUG")
  (net 49 "/HD3_N")
  (net 50 "/HD3_P")
  (net 51 "/HD4_N")
  (net 52 "/HD4_P")
  (net 53 "/HD2_N")
  (net 54 "/HD2_P")
  (net 55 "/GPIO21")
  (net 56 "/GPIO20")
  (net 57 "/GPIO26")
  (net 58 "/GPIO16")
  (net 59 "/GPIO19")
  (net 60 "/GPIO13")
  (net 61 "/GPIO12")
  (net 62 "/GPIO6")
  (net 63 "/GPIO5")
  (net 64 "/ID_SC")
  (net 65 "/ID_SD")
  (net 66 "/GPIO7")
  (net 67 "/GPIO8")
  (net 68 "/GPIO11")
  (net 69 "/GPIO25")
  (net 70 "/GPIO9")
  (net 71 "/GPIO10")
  (net 72 "/GPIO24")
  (net 73 "/GPIO23")
  (net 74 "/GPIO22")
  (net 75 "/GPIO27")
  (net 76 "/GPIO18")
  (net 77 "/GPIO17")
  (net 78 "/GPIO15")
  (net 79 "/GPIO14")
  (net 80 "/GPIO4")
  (net 81 "/GPIO3")
  (net 82 "/GPIO2")
  (net 83 "/HD1_N")
  (net 84 "/HD1_P")
  (net 85 "Net-(J13-Pad9)")
  (net 86 "/SD_DAT1")
  (net 87 "/SD_DAT0")
  (net 88 "/SD_CLK")
  (net 89 "/SD_CMD")
  (net 90 "/SD_DAT3")
  (net 91 "/SD_DAT2")
  (net 92 "/GLOBAL_EN")
  (net 93 "Net-(J14-Pad13)")
  (net 94 "/TV_OUT")
  (net 95 "/SYNC_OUT")
  (net 96 "/SYNC_IN")
  (net 97 "/AIN1")
  (net 98 "/AIN0")
  (net 99 "/EEPROM_nWP")
  (net 100 "/nRPIBOOT")
  (net 101 "no_connect_181")
  (net 102 "/CAM_GPIO")
  (net 103 "/CAM1_D3_P")
  (net 104 "/CAM1_D3_N")
  (net 105 "/CAM1_D2_P")
  (net 106 "/CAM1_D2_N")
  (net 107 "/CAM1_C_P")
  (net 108 "/CAM1_C_N")
  (net 109 "/CAM1_D1_P")
  (net 110 "/CAM1_D1_N")
  (net 111 "/CAM1_D0_P")
  (net 112 "/CAM1_D0_N")
  (net 113 "no_connect_187")
  (net 114 "/PCIE_TX_P")
  (net 115 "/PCIE_TX_N")
  (net 116 "/PCIE_CLK_nREQ")
  (net 117 "no_connect_186")
  (net 118 "no_connect_189")
  (net 119 "no_connect_188")
  (net 120 "/PCIE_RX_P")
  (net 121 "/PCIE_RX_N")
  (net 122 "/PCIE_CLK_N")
  (net 123 "/PCIE_CLK_P")
  (net 124 "/PCIE_nRST")
  (net 125 "no_connect_185")
  (net 126 "no_connect_184")
  (net 127 "/USBD_P")
  (net 128 "/USBD_N")
  (net 129 "/VBUS_OTG")
  (net 130 "/HDMI0_D2_P")
  (net 131 "/HDMI0_D2_N")
  (net 132 "/HDMI0_D1_P")
  (net 133 "/HDMI0_D1_N")
  (net 134 "/HDMI0_D0_P")
  (net 135 "/HDMI0_D0_N")
  (net 136 "/HDMI0_CK_P")
  (net 137 "/HDMI0_CK_N")
  (net 138 "/HDMI0_CEC")
  (net 139 "no_connect_191")
  (net 140 "/HDMI0_SCL")
  (net 141 "/HDMI0_SDA")
  (net 142 "/HDMI0_HOTPLUG")
  (net 143 "/DSI0_C_P")
  (net 144 "/DSI0_C_N")
  (net 145 "/DSI0_D1_P")
  (net 146 "/DSI0_D1_N")
  (net 147 "/DSI0_D0_P")
  (net 148 "/DSI0_D0_N")
  (net 149 "/CAM0_C_P")
  (net 150 "/CAM0_C_N")
  (net 151 "/CAM0_D1_P")
  (net 152 "/CAM0_D1_N")
  (net 153 "/CAM0_D0_P")
  (net 154 "/CAM0_D0_N")
  (net 155 "no_connect_194")
  (net 156 "/USB2_P")
  (net 157 "no_connect_193")
  (net 158 "/USB2_N")
  (net 159 "/USBOTG")
  (net 160 "/nEXTRST")
  (net 161 "Net-(Module2-Pad97)")
  (net 162 "/nPWR_LED")
  (net 163 "/RUN_PG")
  (net 164 "/BT_nDis")
  (net 165 "/+1.8v")
  (net 166 "/WL_nDis")
  (net 167 "/SD_DET")
  (net 168 "/SD_PWR_ON")
  (net 169 "no_connect_200")
  (net 170 "no_connect_199")
  (net 171 "no_connect_198")
  (net 172 "no_connect_197")
  (net 173 "no_connect_196")
  (net 174 "Net-(Module2-Pad21)")
  (net 175 "no_connect_195")
  (net 176 "/ETH_LEDY")
  (net 177 "/ETH_LEDG")
  (net 178 "Net-(R1-Pad2)")
  (net 179 "Net-(R3-Pad1)")
  (net 180 "Net-(R4-Pad2)")
  (net 181 "Net-(R5-Pad1)")
  (net 182 "Net-(R6-Pad1)")
  (net 183 "Net-(R7-Pad1)")
  (net 184 "Net-(R48-Pad2)")
  (net 185 "no_connect_206")
  (net 186 "no_connect_205")
  (net 187 "no_connect_204")
  (net 188 "no_connect_208")
  (net 189 "/USBH_P")
  (net 190 "/USBH_N")
  (net 191 "Net-(U3-Pad21)")
  (net 192 "Net-(U3-Pad20)")
  (net 193 "Net-(U3-Pad19)")
  (net 194 "Net-(U3-Pad18)")
  (net 195 "Net-(U3-Pad17)")
  (net 196 "Net-(U3-Pad16)")
  (net 197 "no_connect_207")
  (net 198 "Net-(U3-Pad13)")
  (net 199 "/PWR1")
  (net 200 "Net-(U3-Pad11)")
  (footprint "Connector_USB:USB_A_Wuerth_614004134726_Horizontal" (layer "F.Cu")
    (tedit 600EF072)
    (at 149.06 118.15 90)
    (descr "USB A connector https://www.we-online.com/catalog/datasheet/614004134726.pdf")
    (tags "USB_A Female Connector receptacle")
    (property "Sheet file" "CM4_1.kicad_sch")
    (property "Sheet name" "")
    (attr through_hole)
    (fp_text reference "J9" (at -4.92 0.11 90) (layer "F.SilkS"))
    (fp_text value "USB_A" (at 0 5.08 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at -2.855 0 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.6 1.6) (drill 0.92) (layers *.Cu *.Mask)
      (net 3 "/+5v") (pinfunction "VBUS"))
    (pad "2" thru_hole circle (at 2 0 90) (size 1.6 1.6) (drill 0.92) (layers *.Cu *.Mask)
      (net 83 "/HD1_N") (pinfunction "D-"))
    (pad "3" thru_hole circle (at 4 0 90) (size 1.6 1.6) (drill 0.92) (layers *.Cu *.Mask)
      (net 84 "/HD1_P") (pinfunction "D+"))
    (pad "4" thru_hole circle (at 6 0 90) (size 1.6 1.6) (drill 0.92) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "GND"))
    (pad "5" thru_hole circle (at 6.27 2.72 90) (size 2.15 2.15) (drill 1.5) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Shield"))
    (pad "5" thru_hole circle (at -0.73 2.72 90) (size 2.15 2.15) (drill 1.5) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Shield"))
    (pad "5" thru_hole circle (at 6.27 -2.72 90) (size 2.15 2.15) (drill 1.5) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Shield"))
    (pad "5" thru_hole circle (at -0.73 -2.72 90) (size 2.15 2.15) (drill 1.5) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Shield"))
    (model "${KISYS3DMOD}/Connector_USB.3dshapes/USB_A_Wuerth_614004134726_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEF1)
    (at 108.87 129.24 -90)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "LED")
    (property "Sheet file" "CM4_1.kicad_sch")
    (property "Sheet name" "")
    (attr smd)
    (fp_text reference "D17" (at -3.06 0.73 90) (layer "F.SilkS"))
    (fp_text value "LED yellow" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 11 "Net-(D17-Pad1)") (pinfunction "K"))
    (pad "2" smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 8 "/+3.3v") (pinfunction "A"))
    (model "${KISYS3DMOD}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_2x07_P2.54mm_Vertical_SMD" (layer "F.Cu")
    (tedit 59FED5CC)
    (at 118.55 56.97 90)
    (descr "surface-mounted straight pin header, 2x07, 2.54mm pitch, double rows")
    (tags "Surface mounted pin header SMD 2x07 2.54mm double row")
    (property "Field4" "Toby")
    (property "Field5" "THD-07-R")
    (property "Field6" "THD-07-R")
    (property "Field7" "Toby")
    (property "Part Description" "PinHeader_2x07_P2.54mm_Vertical")
    (property "Sheet file" "CM4_1.kicad_sch")
    (property "Sheet name" "")
    (attr smd)
    (fp_text reference "J14" (at 0.21 1.3 90) (layer "F.SilkS"))
    (fp_text value "Conn_02x07_Odd_Even" (at 0 9.95 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 180) (layer "F.Fab"))
    (pad "1" smd rect (at -2.525 -7.62 90) (size 3.15 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "Pin_1"))
    (pad "2" smd rect (at 2.525 -7.62 90) (size 3.15 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 100 "/nRPIBOOT") (pinfunction "Pin_2"))
    (pad "3" smd rect (at -2.525 -5.08 90) (size 3.15 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "Pin_3"))
    (pad "4" smd rect (at 2.525 -5.08 90) (size 3.15 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 99 "/EEPROM_nWP") (pinfunction "Pin_4"))
    (pad "5" smd rect (at -2.525 -2.54 90) (size 3.15 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 98 "/AIN0") (pinfunction "Pin_5"))
    (pad "6" smd rect (at 2.525 -2.54 90) (size 3.15 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 97 "/AIN1") (pinfunction "Pin_6"))
    (pad "7" smd rect (at -2.525 0 90) (size 3.15 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "Pin_7"))
    (pad "8" smd rect (at 2.525 0 90) (size 3.15 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 96 "/SYNC_IN") (pinfunction "Pin_8"))
    (pad "9" smd rect (at -2.525 2.54 90) (size 3.15 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 95 "/SYNC_OUT") (pinfunction "Pin_9"))
    (pad "10" smd rect (at 2.525 2.54 90) (size 3.15 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "Pin_10"))
    (pad "11" smd rect (at -2.525 5.08 90) (size 3.15 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 94 "/TV_OUT") (pinfunction "Pin_11"))
    (pad "12" smd rect (at 2.525 5.08 90) (size 3.15 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "Pin_12"))
    (pad "13" smd rect (at -2.525 7.62 90) (size 3.15 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 93 "Net-(J14-Pad13)") (pinfunction "Pin_13"))
    (pad "14" smd rect (at 2.525 7.62 90) (size 3.15 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 92 "/GLOBAL_EN") (pinfunction "Pin_14"))
    (model "${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x07_P2.54mm_Vertical_SMD.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0402_1005Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 109.03 126.13 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Field4" "Farnell")
    (property "Field5" "9239197")
    (property "Field6" "RK73G1ETQTP4700D         ")
    (property "Field7" "KOA EUROPE GMBH")
    (property "Field8" "120887981")
    (property "Part Description" "Resistor 470R M1005 1% 63mW")
    (property "Sheet file" "CM4_1.kicad_sch")
    (property "Sheet name" "")
    (attr smd)
    (fp_text reference "R46" (at 2.71 0.29 90) (layer "F.SilkS"))
    (fp_text value "470R" (at 0 1.17 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.51 0 90) (size 0.54 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 11 "Net-(D17-Pad1)"))
    (pad "2" smd roundrect (at 0.51 0 90) (size 0.54 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 176 "/ETH_LEDY"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0402_1005Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 110.6 126.08 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Field4" "Farnell")
    (property "Field5" "9239197")
    (property "Field6" "RK73G1ETQTP4700D         ")
    (property "Field7" "KOA EUROPE GMBH")
    (property "Field8" "120887981")
    (property "Part Description" "Resistor 470R M1005 1% 63mW")
    (property "Sheet file" "CM4_1.kicad_sch")
    (property "Sheet name" "")
    (attr smd)
    (fp_text reference "R47" (at 3.03 -0.12 90) (layer "F.SilkS"))
    (fp_text value "470R" (at 0 1.17 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.51 0 90) (size 0.54 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 12 "Net-(D18-Pad1)"))
    (pad "2" smd roundrect (at 0.51 0 90) (size 0.54 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 177 "/ETH_LEDG"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEF1)
    (at 105.36 129.23 -90)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "LED")
    (property "Field4" "Digikey ")
    (property "Field5" "LTST-S270KGKT")
    (property "Field6" "SML-A12M8TT86N")
    (property "Field7" "Rohm")
    (property "Field8" "650263301")
    (property "Part Description" "	Green 572nm LED Indication - Discrete 2.2V 2-SMD, No Lead")
    (property "Sheet file" "CM4_1.kicad_sch")
    (property "Sheet name" "")
    (attr smd)
    (fp_text reference "D16" (at 0.9 2.07 180) (layer "F.SilkS"))
    (fp_text value "LED Green" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 10 "Net-(D16-Pad1)") (pinfunction "K"))
    (pad "2" smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 8 "/+3.3v") (pinfunction "A"))
    (model "${KISYS3DMOD}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "CM4IO:PCIex1-36" (layer "F.Cu")
    (tedit 5EBC0A65)
    (at 150.23 58.42 180)
    (property "Field4" "Mouser")
    (property "Field5" "649-10018783-1200TLF")
    (property "Field6" "10018783-11200TLF")
    (property "Field7" "Amphenol FCI")
    (property "Part Description" "PCI Express/PCI Connectors PCIE THROUGH HOLE 36P")
    (property "Sheet file" "CM4_1.kicad_sch")
    (property "Sheet name" "")
    (fp_text reference "J20" (at -1.24 4) (layer "F.SilkS"))
    (fp_text value "10018783-11200TLF" (at -1 -6) (layer "F.Fab"))
    (pad "19" thru_hole circle (at 11.65 1.25 180) (size 2.35 2.35) (drill 2.35) (layers *.Cu *.Mask))
    (pad "19" thru_hole circle (at 20.8 1.25 180) (size 2.35 2.35) (drill 2.35) (layers *.Cu *.Mask))
    (pad "A1" thru_hole rect (at 0 0 180) (size 1.3 1.3) (drill 0.7) (layers *.Cu *.Mask)
      (net 126 "no_connect_184") (pinfunction "nPRSNT1"))
    (pad "A2" thru_hole circle (at 1 -2 180) (size 1.3 1.3) (drill 0.7) (layers *.Cu *.Mask)
      (net 2 "/+12v") (pinfunction "+12V"))
    (pad "A3" thru_hole circle (at 2 0 180) (size 1.3 1.3) (drill 0.7) (layers *.Cu *.Mask)
      (net 2 "/+12v") (pinfunction "+12V"))
    (pad "A4" thru_hole circle (at 3 -2 180) (size 1.3 1.3) (drill 0.7) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "GND"))
    (pad "A5" thru_hole circle (at 4 0 180) (size 1.3 1.3) (drill 0.7) (layers *.Cu *.Mask)
      (net 4 "/pcie+3.3v") (pinfunction "TCK"))
    (pad "A6" thru_hole circle (at 5 -2 180) (size 1.3 1.3) (drill 0.7) (layers *.Cu *.Mask)
      (net 4 "/pcie+3.3v") (pinfunction "TDI"))
    (pad "A7" thru_hole circle (at 6 0 180) (size 1.3 1.3) (drill 0.7) (layers *.Cu *.Mask)
      (net 125 "no_connect_185") (pinfunction "TD0"))
    (pad "A8" thru_hole circle (at 7 -2 180) (size 1.3 1.3) (drill 0.7) (layers *.Cu *.Mask)
      (net 4 "/pcie+3.3v") (pinfunction "TMS"))
    (pad "A9" thru_hole circle (at 8 0 180) (size 1.3 1.3) (drill 0.7) (layers *.Cu *.Mask)
      (net 4 "/pcie+3.3v") (pinfunction "+3.3V"))
    (pad "A10" thru_hole circle (at 9 -2 180) (size 1.3 1.3) (drill 0.7) (layers *.Cu *.Mask)
      (net 4 "/pcie+3.3v") (pinfunction "+3.3V"))
    (pad "A11" thru_hole circle (at 10 0 180) (size 1.3 1.3) (drill 0.7) (layers *.Cu *.Mask)
      (net 124 "/PCIE_nRST") (pinfunction "nPERST"))
    (pad "A12" thru_hole circle (at 13 -2 180) (size 1.3 1.3) (drill 0.7) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "GND"))
    (pad "A13" thru_hole circle (at 14 0 180) (size 1.3 1.3) (drill 0.7) (layers *.Cu *.Mask)
      (net 123 "/PCIE_CLK_P") (pinfunction "REFCLK+"))
    (pad "A14" thru_hole circle (at 15 -2 180) (size 1.3 1.3) (drill 0.7) (layers *.Cu *.Mask)
      (net 122 "/PCIE_CLK_N") (pinfunction "REFCLK-"))
    (pad "A15" thru_hole circle (at 16 0 180) (size 1.3 1.3) (drill 0.7) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "GND"))
    (pad "A16" thru_hole circle (at 17 -2 180) (size 1.3 1.3) (drill 0.7) (layers *.Cu *.Mask)
      (net 121 "/PCIE_RX_N") (pinfunction "PERP0"))
    (pad "A17" thru_hole circle (at 18 0 180) (size 1.3 1.3) (drill 0.7) (layers *.Cu *.Mask)
      (net 120 "/PCIE_RX_P") (pinfunction "PERN0"))
    (pad "A18" thru_hole circle (at 19 -2 180) (size 1.3 1.3) (drill 0.7) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "GND"))
    (pad "B1" thru_hole circle (at 0 2.5 180) (size 1.3 1.3) (drill 0.7) (layers *.Cu *.Mask)
      (net 2 "/+12v") (pinfunction "+12v"))
    (pad "B2" thru_hole circle (at 1 4.5 180) (size 1.3 1.3) (drill 0.7) (layers *.Cu *.Mask)
      (net 2 "/+12v") (pinfunction "+12v"))
    (pad "B3" thru_hole circle (at 2 2.5 180) (size 1.3 1.3) (drill 0.7) (layers *.Cu *.Mask)
      (net 2 "/+12v") (pinfunction "+12v"))
    (pad "B4" thru_hole circle (at 3 4.5 180) (size 1.3 1.3) (drill 0.7) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "GND"))
    (pad "B5" thru_hole circle (at 4 2.5 180) (size 1.3 1.3) (drill 0.7) (layers *.Cu *.Mask)
      (net 119 "no_connect_188") (pinfunction "SMCLK"))
    (pad "B6" thru_hole circle (at 5 4.5 180) (size 1.3 1.3) (drill 0.7) (layers *.Cu *.Mask)
      (net 118 "no_connect_189") (pinfunction "SMDAT"))
    (pad "B7" thru_hole circle (at 6 2.5 180) (size 1.3 1.3) (drill 0.7) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "GND"))
    (pad "B8" thru_hole circle (at 7 4.5 180) (size 1.3 1.3) (drill 0.7) (layers *.Cu *.Mask)
      (net 4 "/pcie+3.3v") (pinfunction "+3.3v"))
    (pad "B9" thru_hole circle (at 8 2.5 180) (size 1.3 1.3) (drill 0.7) (layers *.Cu *.Mask)
      (net 4 "/pcie+3.3v") (pinfunction "nTRST"))
    (pad "B10" thru_hole circle (at 9 4.5 180) (size 1.3 1.3) (drill 0.7) (layers *.Cu *.Mask)
      (net 4 "/pcie+3.3v") (pinfunction "+3.3vAUX"))
    (pad "B11" thru_hole circle (at 10 2.5 180) (size 1.3 1.3) (drill 0.7) (layers *.Cu *.Mask)
      (net 117 "no_connect_186") (pinfunction "nWAKE"))
    (pad "B12" thru_hole circle (at 13 4.5 180) (size 1.3 1.3) (drill 0.7) (layers *.Cu *.Mask)
      (net 116 "/PCIE_CLK_nREQ") (pinfunction "nCLKREQ"))
    (pad "B13" thru_hole circle (at 14 2.5 180) (size 1.3 1.3) (drill 0.7) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "GND"))
    (pad "B14" thru_hole circle (at 15 4.5 180) (size 1.3 1.3) (drill 0.7) (layers *.Cu *.Mask)
      (net 115 "/PCIE_TX_N") (pinfunction "PETP0"))
    (pad "B15" thru_hole circle (at 16 2.5 180) (size 1.3 1.3) (drill 0.7) (layers *.Cu *.Mask)
      (net 114 "/PCIE_TX_P") (pinfunction "PETN0"))
    (pad "B16" thru_hole circle (at 17 4.5 180) (size 1.3 1.3) (drill 0.7) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "GND"))
    (pad "B17" thru_hole circle (at 18 2.5 180) (size 1.3 1.3) (drill 0.7) (layers *.Cu *.Mask)
      (net 113 "no_connect_187") (pinfunction "nPRSNT2"))
    (pad "B18" thru_hole circle (at 19 4.5 180) (size 1.3 1.3) (drill 0.7) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "GND"))
    (model "./CM4IO.3dshapes/PCIe-x1-36.step"
      (offset (xyz 11.5 -1.25 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric" (layer "F.Cu")
    (tedit 60127B49)
    (at 134.93 108.6)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (attr smd)
    (fp_text reference "R0" (at 0 -1.82) (layer "F.SilkS"))
    (fp_text value "0R" (at 0 1.82) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.4625 0) (size 1.125 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.222)
      (net 1 "GND"))
    (pad "2" smd roundrect (at 1.4625 0) (size 1.125 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.222)
      (net 1 "GND"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_USB:USB_A_Wuerth_614004134726_Horizontal" (layer "F.Cu")
    (tedit 60112577)
    (at 130.28 118.16 90)
    (descr "USB A connector https://www.we-online.com/catalog/datasheet/614004134726.pdf")
    (tags "USB_A Female Connector receptacle")
    (property "Sheet file" "CM4_1.kicad_sch")
    (property "Sheet name" "")
    (attr through_hole)
    (fp_text reference "J5" (at -5.58 0.04 90) (layer "F.SilkS"))
    (fp_text value "USB_A" (at 0 5.08 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at -2.855 0 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.6 1.6) (drill 0.92) (layers *.Cu *.Mask)
      (net 3 "/+5v") (pinfunction "VBUS"))
    (pad "2" thru_hole circle (at 2 0 90) (size 1.6 1.6) (drill 0.92) (layers *.Cu *.Mask)
      (net 49 "/HD3_N") (pinfunction "D-"))
    (pad "3" thru_hole circle (at 4 0 90) (size 1.6 1.6) (drill 0.92) (layers *.Cu *.Mask)
      (net 50 "/HD3_P") (pinfunction "D+"))
    (pad "4" thru_hole circle (at 6 0 90) (size 1.6 1.6) (drill 0.92) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "GND"))
    (pad "5" thru_hole circle (at 6.27 -2.72 90) (size 2.15 2.15) (drill 1.5) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Shield"))
    (pad "5" thru_hole circle (at -0.73 -2.72 90) (size 2.15 2.15) (drill 1.5) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Shield"))
    (pad "5" thru_hole circle (at 6.27 2.72 90) (size 2.15 2.15) (drill 1.5) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Shield"))
    (pad "5" thru_hole circle (at -0.73 2.72 90) (size 2.15 2.15) (drill 1.5) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Shield"))
    (model "${KISYS3DMOD}/Connector_USB.3dshapes/USB_A_Wuerth_614004134726_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEF1)
    (at 107.03 129.24 -90)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "LED")
    (property "Field4" "Digikey ")
    (property "Field5" "	LTST-S270KRKT")
    (property "Field6" "SML-A12U8TT86Q")
    (property "Field7" "Rohm")
    (property "Field8" "650295101")
    (property "Part Description" "	Red 620nm LED Indication - Discrete 2.2V 2-SMD, No Lead")
    (property "Sheet file" "CM4_1.kicad_sch")
    (property "Sheet name" "")
    (attr smd)
    (fp_text reference "D20" (at -0.11 -0.09 90) (layer "User.1"))
    (fp_text value "LED Red" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 13 "Net-(D20-Pad1)") (pinfunction "K"))
    (pad "2" smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 8 "/+3.3v") (pinfunction "A"))
    (model "${KISYS3DMOD}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0402_1005Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 105.61 126.58 -90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Field4" "Farnell")
    (property "Field5" "9239235")
    (property "Field6" "RK73H1ETTP1001F")
    (property "Field7" "KOA EUROPE GMBH")
    (property "Field8" "125049511")
    (property "Part Description" "Resistor 1K M1005 1% 63mW")
    (property "Sheet file" "CM4_1.kicad_sch")
    (property "Sheet name" "")
    (attr smd)
    (fp_text reference "R45" (at -2.71 -0.01 90) (layer "F.SilkS"))
    (fp_text value "1k" (at 0 1.17 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.51 0 270) (size 0.54 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 174 "Net-(Module2-Pad21)"))
    (pad "2" smd roundrect (at 0.51 0 270) (size 0.54 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 10 "Net-(D16-Pad1)"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_USB:USB_A_Wuerth_614004134726_Horizontal" (layer "F.Cu")
    (tedit 600EF078)
    (at 120.58 118.15 90)
    (descr "USB A connector https://www.we-online.com/catalog/datasheet/614004134726.pdf")
    (tags "USB_A Female Connector receptacle")
    (property "Sheet file" "CM4_1.kicad_sch")
    (property "Sheet name" "")
    (attr through_hole)
    (fp_text reference "J6" (at -5.69 -0.34 90) (layer "F.SilkS"))
    (fp_text value "USB_A" (at 0 5.08 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at -2.855 0 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.6 1.6) (drill 0.92) (layers *.Cu *.Mask)
      (net 3 "/+5v") (pinfunction "VBUS"))
    (pad "2" thru_hole circle (at 2 0 90) (size 1.6 1.6) (drill 0.92) (layers *.Cu *.Mask)
      (net 51 "/HD4_N") (pinfunction "D-"))
    (pad "3" thru_hole circle (at 4 0 90) (size 1.6 1.6) (drill 0.92) (layers *.Cu *.Mask)
      (net 52 "/HD4_P") (pinfunction "D+"))
    (pad "4" thru_hole circle (at 6 0 90) (size 1.6 1.6) (drill 0.92) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "GND"))
    (pad "5" thru_hole circle (at 6.27 -2.72 90) (size 2.15 2.15) (drill 1.5) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Shield"))
    (pad "5" thru_hole circle (at 6.27 2.72 90) (size 2.15 2.15) (drill 1.5) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Shield"))
    (pad "5" thru_hole circle (at -0.73 2.72 90) (size 2.15 2.15) (drill 1.5) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Shield"))
    (pad "5" thru_hole circle (at -0.73 -2.72 90) (size 2.15 2.15) (drill 1.5) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Shield"))
    (model "${KISYS3DMOD}/Connector_USB.3dshapes/USB_A_Wuerth_614004134726_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_2x06_P2.54mm_Horizontal" (layer "F.Cu")
    (tedit 6012470C)
    (at 108.09 68.4 180)
    (descr "Through hole angled pin header, 2x06, 2.54mm pitch, 6mm pin length, double rows")
    (tags "Through hole angled pin header THT 2x06 2.54mm double row")
    (property "Sheet file" "CM4_1.kicad_sch")
    (property "Sheet name" "")
    (attr through_hole)
    (fp_text reference "J3" (at 1.17 14.43) (layer "F.SilkS"))
    (fp_text value "Conn_01x10_Female" (at 5.655 14.97) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 5.31 6.35 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "/+12v") (pinfunction "Pin_1"))
    (pad "2" thru_hole oval (at 2.54 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "/+5v") (pinfunction "Pin_2"))
    (pad "3" thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_3"))
    (pad "4" thru_hole oval (at 2.54 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 35 "/TRD0_P") (pinfunction "Pin_4"))
    (pad "5" thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 "/TRD0_N") (pinfunction "Pin_5"))
    (pad "6" thru_hole oval (at 2.54 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 33 "/TRD1_N") (pinfunction "Pin_6"))
    (pad "7" thru_hole oval (at 0 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 "/TRD1_P") (pinfunction "Pin_7"))
    (pad "8" thru_hole oval (at 2.54 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 "/TRD3_P") (pinfunction "Pin_8"))
    (pad "9" thru_hole oval (at 0 10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 "/TRD3_N") (pinfunction "Pin_9"))
    (pad "10" thru_hole oval (at 2.54 10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 "/TRD2_N") (pinfunction "Pin_10"))
    (pad "11" thru_hole oval (at 0 12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 "/TRD2_P") (pinfunction "Pin_11"))
    (pad "12" thru_hole oval (at 2.54 12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "GND"))
    (model "${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x06_P2.54mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_2x17_P2.54mm_Vertical_SMD" (layer "F.Cu")
    (tedit 59FED5CC)
    (at 131.24 65.9 90)
    (descr "surface-mounted straight pin header, 2x17, 2.54mm pitch, double rows")
    (tags "Surface mounted pin header SMD 2x17 2.54mm double row")
    (property "Sheet file" "CM4_1.kicad_sch")
    (property "Sheet name" "")
    (attr smd)
    (fp_text reference "J8" (at -0.01 -0.24 90) (layer "F.SilkS"))
    (fp_text value "THD-20-R" (at 0 22.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 180) (layer "F.Fab"))
    (pad "1" smd rect (at -2.525 -20.32 90) (size 3.15 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 8 "/+3.3v") (pinfunction "Pin_1"))
    (pad "2" smd rect (at 2.525 -20.32 90) (size 3.15 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "/+5v") (pinfunction "Pin_2"))
    (pad "3" smd rect (at -2.525 -17.78 90) (size 3.15 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 82 "/GPIO2") (pinfunction "Pin_3"))
    (pad "4" smd rect (at 2.525 -17.78 90) (size 3.15 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "/+5v") (pinfunction "Pin_4"))
    (pad "5" smd rect (at -2.525 -15.24 90) (size 3.15 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 81 "/GPIO3") (pinfunction "Pin_5"))
    (pad "6" smd rect (at 2.525 -15.24 90) (size 3.15 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "Pin_6"))
    (pad "7" smd rect (at -2.525 -12.7 90) (size 3.15 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 80 "/GPIO4") (pinfunction "Pin_7"))
    (pad "8" smd rect (at 2.525 -12.7 90) (size 3.15 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 79 "/GPIO14") (pinfunction "Pin_8"))
    (pad "9" smd rect (at -2.525 -10.16 90) (size 3.15 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "Pin_9"))
    (pad "10" smd rect (at 2.525 -10.16 90) (size 3.15 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 78 "/GPIO15") (pinfunction "Pin_10"))
    (pad "11" smd rect (at -2.525 -7.62 90) (size 3.15 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 77 "/GPIO17") (pinfunction "Pin_11"))
    (pad "12" smd rect (at 2.525 -7.62 90) (size 3.15 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 76 "/GPIO18") (pinfunction "Pin_12"))
    (pad "13" smd rect (at -2.525 -5.08 90) (size 3.15 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 75 "/GPIO27") (pinfunction "Pin_13"))
    (pad "14" smd rect (at 2.525 -5.08 90) (size 3.15 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "Pin_14"))
    (pad "15" smd rect (at -2.525 -2.54 90) (size 3.15 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 74 "/GPIO22") (pinfunction "Pin_15"))
    (pad "16" smd rect (at 2.525 -2.54 90) (size 3.15 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 73 "/GPIO23") (pinfunction "Pin_16"))
    (pad "17" smd rect (at -2.525 0 90) (size 3.15 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 8 "/+3.3v") (pinfunction "Pin_17"))
    (pad "18" smd rect (at 2.525 0 90) (size 3.15 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 72 "/GPIO24") (pinfunction "Pin_18"))
    (pad "19" smd rect (at -2.525 2.54 90) (size 3.15 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 71 "/GPIO10") (pinfunction "Pin_19"))
    (pad "20" smd rect (at 2.525 2.54 90) (size 3.15 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "Pin_20"))
    (pad "21" smd rect (at -2.525 5.08 90) (size 3.15 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 70 "/GPIO9") (pinfunction "Pin_21"))
    (pad "22" smd rect (at 2.525 5.08 90) (size 3.15 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 69 "/GPIO25") (pinfunction "Pin_22"))
    (pad "23" smd rect (at -2.525 7.62 90) (size 3.15 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 68 "/GPIO11") (pinfunction "Pin_23"))
    (pad "24" smd rect (at 2.525 7.62 90) (size 3.15 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 67 "/GPIO8") (pinfunction "Pin_24"))
    (pad "25" smd rect (at -2.525 10.16 90) (size 3.15 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "Pin_25"))
    (pad "26" smd rect (at 2.525 10.16 90) (size 3.15 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 66 "/GPIO7") (pinfunction "Pin_26"))
    (pad "27" smd rect (at -2.525 12.7 90) (size 3.15 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 65 "/ID_SD") (pinfunction "Pin_27"))
    (pad "28" smd rect (at 2.525 12.7 90) (size 3.15 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 64 "/ID_SC") (pinfunction "Pin_28"))
    (pad "29" smd rect (at -2.525 15.24 90) (size 3.15 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 63 "/GPIO5") (pinfunction "Pin_29"))
    (pad "30" smd rect (at 2.525 15.24 90) (size 3.15 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "Pin_30"))
    (pad "31" smd rect (at -2.525 17.78 90) (size 3.15 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 62 "/GPIO6") (pinfunction "Pin_31"))
    (pad "32" smd rect (at 2.525 17.78 90) (size 3.15 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 61 "/GPIO12") (pinfunction "Pin_32"))
    (pad "33" smd rect (at -2.525 20.32 90) (size 3.15 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 60 "/GPIO13") (pinfunction "Pin_33"))
    (pad "34" smd rect (at 2.525 20.32 90) (size 3.15 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "Pin_34"))
    (model "${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x17_P2.54mm_Vertical_SMD.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0402_1005Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 107.12 126.58 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Field4" "Farnell")
    (property "Field5" "9239235")
    (property "Field6" "RK73H1ETTP1001F")
    (property "Field7" "KOA EUROPE GMBH")
    (property "Field8" "125049511")
    (property "Part Description" "Resistor 1K M1005 1% 63mW")
    (property "Sheet file" "CM4_1.kicad_sch")
    (property "Sheet name" "")
    (attr smd)
    (fp_text reference "R48" (at 2.62 -0.16 90) (layer "F.SilkS"))
    (fp_text value "1k" (at 0 1.17 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.51 0 90) (size 0.54 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 13 "Net-(D20-Pad1)"))
    (pad "2" smd roundrect (at 0.51 0 90) (size 0.54 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 184 "Net-(R48-Pad2)"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEF1)
    (at 110.7 129.27 -90)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "LED")
    (property "Sheet file" "CM4_1.kicad_sch")
    (property "Sheet name" "")
    (attr smd)
    (fp_text reference "D18" (at -2.96 -1 90) (layer "F.SilkS"))
    (fp_text value "LED green" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 12 "Net-(D18-Pad1)") (pinfunction "K"))
    (pad "2" smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 8 "/+3.3v") (pinfunction "A"))
    (model "${KISYS3DMOD}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_HDMI:HDMI_Micro-D_Molex_46765-1x01" (layer "F.Cu")
    (tedit 6011299D)
    (at 100.55 128.25)
    (descr "HDMI, Micro, Type D, THT, 0.4mm pitch, 19 ckt, right angle (http://www.molex.com/pdm_docs/sd/467651301_sd.pdf)")
    (tags "hdmi micro type d right angle tht")
    (property "Field4" "Farnell")
    (property "Field5" "2614936")
    (property "Field6" "690-019-298-412")
    (property "Field7" "EDAC")
    (property "Field8" "UCON00802")
    (property "Part Description" "HDMI Connector, Right Angle, 19 Contacts, Receptacle, Surface Mount, Surface Mount Right Angle")
    (property "Sheet file" "CM4_1.kicad_sch")
    (property "Sheet name" "")
    (attr smd)
    (fp_text reference "J4" (at 1.06 -6.1) (layer "F.SilkS"))
    (fp_text value "690-019-298-412" (at 0 3.6) (layer "F.Fab"))
    (fp_text user "KEEPOUT" (at 0 -0.47) (layer "Cmts.User"))
    (fp_text user "${REFERENCE}" (at 0 -3.3) (layer "F.Fab"))
    (pad "1" smd rect (at 1.8 -4.775) (size 0.23 0.85) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 36 "/HDMI1_D2_P") (pinfunction "D2+"))
    (pad "2" smd rect (at 1.6 -3.55) (size 0.23 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "D2S"))
    (pad "3" smd rect (at 1.4 -4.775) (size 0.23 0.85) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 37 "/HDMI1_D2_N") (pinfunction "D2-"))
    (pad "4" smd rect (at 1.2 -3.55) (size 0.23 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 38 "/HDMI1_D1_P") (pinfunction "D1+"))
    (pad "5" smd rect (at 1 -4.775) (size 0.23 0.85) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "D1S"))
    (pad "6" smd rect (at 0.8 -3.55) (size 0.23 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 39 "/HDMI1_D1_N") (pinfunction "D1-"))
    (pad "7" smd rect (at 0.6 -4.775) (size 0.23 0.85) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 40 "/HDMI1_D0_P") (pinfunction "D0+"))
    (pad "8" smd rect (at 0.4 -3.55) (size 0.23 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "D0S"))
    (pad "9" smd rect (at 0.2 -4.775) (size 0.23 0.85) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 41 "/HDMI1_D0_N") (pinfunction "D0-"))
    (pad "10" smd rect (at 0 -3.55) (size 0.23 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 42 "/HDMI1_CK_P") (pinfunction "CK+"))
    (pad "11" smd rect (at -0.2 -4.775) (size 0.23 0.85) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "CKS"))
    (pad "12" smd rect (at -0.4 -3.55) (size 0.23 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 43 "/HDMI1_CK_N") (pinfunction "CK-"))
    (pad "13" smd rect (at -0.6 -4.775) (size 0.23 0.85) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 44 "/HDMI1_CEC") (pinfunction "CEC"))
    (pad "14" smd rect (at -0.8 -3.55) (size 0.23 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 45 "no_connect_192") (pinfunction "UTILITY/HEAC+"))
    (pad "15" smd rect (at -1 -4.775) (size 0.23 0.85) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 46 "/HDMI1_SCL") (pinfunction "SCL"))
    (pad "16" smd rect (at -1.2 -3.55) (size 0.23 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 47 "/HDMI1_SDA") (pinfunction "SDA"))
    (pad "17" smd rect (at -1.4 -4.775) (size 0.23 0.85) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "GND"))
    (pad "18" smd rect (at -1.6 -3.55) (size 0.23 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "/+5v") (pinfunction "+5V"))
    (pad "19" smd rect (at -1.8 -4.775) (size 0.23 0.85) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 48 "/HDMI1_HOTPLUG") (pinfunction "HPD/HEAC-"))
    (pad "SH" thru_hole oval (at 3.1 -3.36) (size 1.5 2.55) (drill oval 0.65 1.7) (layers *.Cu *.Mask)
      (net 1 "GND"))
    (pad "SH" thru_hole oval (at -3.1 0) (size 1.5 2.55) (drill oval 0.65 1.7) (layers *.Cu *.Mask)
      (net 1 "GND"))
    (pad "SH" thru_hole oval (at -3.1 -3.36) (size 1.5 2.55) (drill oval 0.65 1.7) (layers *.Cu *.Mask)
      (net 1 "GND"))
    (pad "SH" thru_hole oval (at 3.1 0) (size 1.5 2.55) (drill oval 0.65 1.7) (layers *.Cu *.Mask)
      (net 1 "GND"))
    (model "${KISYS3DMOD}/Connector_HDMI.3dshapes/HDMI_Micro-D_Molex_46765-1x01.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "CM4IO:Raspberry-Pi-4-Compute-Module" (layer "F.Cu")
    (tedit 5EF08346)
    (at 98.81 73.64 -90)
    (descr "Raspberry Pi 4 Compute Module")
    (tags "Raspberry Pi 4 Compute Module")
    (property "Field4" "Hirose")
    (property "Field5" "2off DF40C-100DS-0.4V")
    (property "Field6" "2off DF40C-100DS-0.4V")
    (property "Field7" "Hirose")
    (property "Part Description" "	100 Position Connector Receptacle, Center Strip Contacts Surface Mount Gold")
    (property "Sheet file" "CM4_1.kicad_sch")
    (property "Sheet name" "")
    (attr smd)
    (fp_text reference "Module2" (at 18.38 -5.08 180) (layer "F.SilkS"))
    (fp_text value "ComputeModule4" (at 16.52 0.19 90) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 33 0 270) (size 2.7 2.7) (drill 2.7) (layers *.Cu *.Mask)
      (solder_mask_margin 1.7) (clearance 1.7))
    (pad "" np_thru_hole circle (at 0 -48 270) (size 2.7 2.7) (drill 2.7) (layers *.Cu *.Mask)
      (solder_mask_margin 1.7) (clearance 1.7))
    (pad "" np_thru_hole circle (at 0 0 270) (size 2.7 2.7) (drill 2.7) (layers *.Cu *.Mask)
      (solder_mask_margin 1.7) (clearance 1.7))
    (pad "" np_thru_hole circle (at 33 -48 270) (size 2.7 2.7) (drill 2.7) (layers *.Cu *.Mask)
      (solder_mask_margin 1.7) (clearance 1.7))
    (pad "1" smd rect (at -2 -31.3 180) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "GND"))
    (pad "2" smd rect (at 1.08 -31.3 180) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "GND"))
    (pad "3" smd rect (at -2 -30.9 180) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 31 "/TRD3_P") (pinfunction "Ethernet_Pair3_P"))
    (pad "4" smd rect (at 1.08 -30.9 180) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 32 "/TRD1_P") (pinfunction "Ethernet_Pair1_P"))
    (pad "5" smd rect (at -2 -30.5 180) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 30 "/TRD3_N") (pinfunction "Ethernet_Pair3_N"))
    (pad "6" smd rect (at 1.08 -30.5 180) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 33 "/TRD1_N") (pinfunction "Ethernet_Pair1_N"))
    (pad "7" smd rect (at -2 -30.1 180) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "GND"))
    (pad "8" smd rect (at 1.08 -30.1 180) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "GND"))
    (pad "9" smd rect (at -2 -29.7 180) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 29 "/TRD2_N") (pinfunction "Ethernet_Pair2_N"))
    (pad "10" smd rect (at 1.08 -29.7 180) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 34 "/TRD0_N") (pinfunction "Ethernet_Pair0_N"))
    (pad "11" smd rect (at -2 -29.3 180) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 28 "/TRD2_P") (pinfunction "Ethernet_Pair2_P"))
    (pad "12" smd rect (at 1.08 -29.3 180) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "/TRD0_P") (pinfunction "Ethernet_Pair0_P"))
    (pad "13" smd rect (at -2 -28.9 180) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "GND"))
    (pad "14" smd rect (at 1.08 -28.9 180) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "GND"))
    (pad "15" smd rect (at -2 -28.5 180) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 177 "/ETH_LEDG") (pinfunction "Ethernet_nLED3(3.3v)"))
    (pad "16" smd rect (at 1.08 -28.5 180) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 96 "/SYNC_IN") (pinfunction "Ethernet_SYNC_IN(1.8v)"))
    (pad "17" smd rect (at -2 -28.1 180) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 176 "/ETH_LEDY") (pinfunction "Ethernet_nLED2(3.3v)"))
    (pad "18" smd rect (at 1.08 -28.1 180) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 95 "/SYNC_OUT") (pinfunction "Ethernet_SYNC_OUT(1.8v)"))
    (pad "19" smd rect (at -2 -27.7 180) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 175 "no_connect_195") (pinfunction "Ethernet_nLED1(3.3v)"))
    (pad "20" smd rect (at 1.08 -27.7 180) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 99 "/EEPROM_nWP") (pinfunction "EEPROM_nWP"))
    (pad "21" smd rect (at -2 -27.3 180) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 174 "Net-(Module2-Pad21)") (pinfunction "PI_nLED_Activity"))
    (pad "22" smd rect (at 1.08 -27.3 180) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "GND"))
    (pad "23" smd rect (at -2 -26.9 180) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "GND"))
    (pad "24" smd rect (at 1.08 -26.9 180) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 57 "/GPIO26") (pinfunction "GPIO26"))
    (pad "25" smd rect (at -2 -26.5 180) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 55 "/GPIO21") (pinfunction "GPIO21"))
    (pad "26" smd rect (at 1.08 -26.5 180) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 59 "/GPIO19") (pinfunction "GPIO19"))
    (pad "27" smd rect (at -2 -26.1 180) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 56 "/GPIO20") (pinfunction "GPIO20"))
    (pad "28" smd rect (at 1.08 -26.1 180) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 60 "/GPIO13") (pinfunction "GPIO13"))
    (pad "29" smd rect (at -2 -25.7 180) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 58 "/GPIO16") (pinfunction "GPIO16"))
    (pad "30" smd rect (at 1.08 -25.7 180) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 62 "/GPIO6") (pinfunction "GPIO6"))
    (pad "31" smd rect (at -2 -25.3 180) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 61 "/GPIO12") (pinfunction "GPIO12"))
    (pad "32" smd rect (at 1.08 -25.3 180) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "GND"))
    (pad "33" smd rect (at -2 -24.9 180) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "GND"))
    (pad "34" smd rect (at 1.08 -24.9 180) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 63 "/GPIO5") (pinfunction "GPIO5"))
    (pad "35" smd rect (at -2 -24.5 180) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 64 "/ID_SC") (pinfunction "ID_SC"))
    (pad "36" smd rect (at 1.08 -24.5 180) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 65 "/ID_SD") (pinfunction "ID_SD"))
    (pad "37" smd rect (at -2 -24.1 180) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 66 "/GPIO7") (pinfunction "GPIO7"))
    (pad "38" smd rect (at 1.08 -24.1 180) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 68 "/GPIO11") (pinfunction "GPIO11"))
    (pad "39" smd rect (at -2 -23.7 180) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 67 "/GPIO8") (pinfunction "GPIO8"))
    (pad "40" smd rect (at 1.08 -23.7 180) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 70 "/GPIO9") (pinfunction "GPIO9"))
    (pad "41" smd rect (at -2 -23.3 180) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 69 "/GPIO25") (pinfunction "GPIO25"))
    (pad "42" smd rect (at 1.08 -23.3 180) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "GND"))
    (pad "43" smd rect (at -2 -22.9 180) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "GND"))
    (pad "44" smd rect (at 1.08 -22.9 180) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 71 "/GPIO10") (pinfunction "GPIO10"))
    (pad "45" smd rect (at -2 -22.5 180) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 72 "/GPIO24") (pinfunction "GPIO24"))
    (pad "46" smd rect (at 1.08 -22.5 180) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 74 "/GPIO22") (pinfunction "GPIO22"))
    (pad "47" smd rect (at -2 -22.1 180) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 73 "/GPIO23") (pinfunction "GPIO23"))
    (pad "48" smd rect (at 1.08 -22.1 180) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 75 "/GPIO27") (pinfunction "GPIO27"))
    (pad "49" smd rect (at -2 -21.7 180) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 76 "/GPIO18") (pinfunction "GPIO18"))
    (pad "50" smd rect (at 1.08 -21.7 180) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 77 "/GPIO17") (pinfunction "GPIO17"))
    (pad "51" smd rect (at -2 -21.3 180) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 78 "/GPIO15") (pinfunction "GPIO15"))
    (pad "52" smd rect (at 1.08 -21.3 180) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "GND"))
    (pad "53" smd rect (at -2 -20.9 180) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "GND"))
    (pad "54" smd rect (at 1.08 -20.9 180) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 80 "/GPIO4") (pinfunction "GPIO4"))
    (pad "55" smd rect (at -2 -20.5 180) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 79 "/GPIO14") (pinfunction "GPIO14"))
    (pad "56" smd rect (at 1.08 -20.5 180) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 81 "/GPIO3") (pinfunction "GPIO3"))
    (pad "57" smd rect (at -2 -20.1 180) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 88 "/SD_CLK") (pinfunction "SD_CLK"))
    (pad "58" smd rect (at 1.08 -20.1 180) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 82 "/GPIO2") (pinfunction "GPIO2"))
    (pad "59" smd rect (at -2 -19.7 180) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "GND"))
    (pad "60" smd rect (at 1.08 -19.7 180) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "GND"))
    (pad "61" smd rect (at -2 -19.3 180) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 90 "/SD_DAT3") (pinfunction "SD_DAT3"))
    (pad "62" smd rect (at 1.08 -19.3 180) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 89 "/SD_CMD") (pinfunction "SD_CMD"))
    (pad "63" smd rect (at -2 -18.9 180) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 87 "/SD_DAT0") (pinfunction "SD_DAT0"))
    (pad "64" smd rect (at 1.08 -18.9 180) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 173 "no_connect_196") (pinfunction "SD_DAT5"))
    (pad "65" smd rect (at -2 -18.5 180) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "GND"))
    (pad "66" smd rect (at 1.08 -18.5 180) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "GND"))
    (pad "67" smd rect (at -2 -18.1 180) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 86 "/SD_DAT1") (pinfunction "SD_DAT1"))
    (pad "68" smd rect (at 1.08 -18.1 180) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 172 "no_connect_197") (pinfunction "SD_DAT4"))
    (pad "69" smd rect (at -2 -17.7 180) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 91 "/SD_DAT2") (pinfunction "SD_DAT2"))
    (pad "70" smd rect (at 1.08 -17.7 180) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 171 "no_connect_198") (pinfunction "SD_DAT7"))
    (pad "71" smd rect (at -2 -17.3 180) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "GND"))
    (pad "72" smd rect (at 1.08 -17.3 180) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 170 "no_connect_199") (pinfunction "SD_DAT6"))
    (pad "73" smd rect (at -2 -16.9 180) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 169 "no_connect_200") (pinfunction "SD_VDD_Override"))
    (pad "74" smd rect (at 1.08 -16.9 180) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "GND"))
    (pad "75" smd rect (at -2 -16.5 180) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 168 "/SD_PWR_ON") (pinfunction "SD_PWR_ON"))
    (pad "76" smd rect (at 1.08 -16.5 180) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 167 "/SD_DET") (pinfunction "Reserved"))
    (pad "77" smd rect (at -2 -16.1 180) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "/+5v") (pinfunction "+5v_(Input)"))
    (pad "78" smd rect (at 1.08 -16.1 180) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 8 "/+3.3v") (pinfunction "GPIO_VREF(1.8v/3.3v_Input)"))
    (pad "79" smd rect (at -2 -15.7 180) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "/+5v") (pinfunction "+5v_(Input)"))
    (pad "80" smd rect (at 1.08 -15.7 180) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "/SCL0") (pinfunction "SCL0"))
    (pad "81" smd rect (at -2 -15.3 180) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "/+5v") (pinfunction "+5v_(Input)"))
    (pad "82" smd rect (at 1.08 -15.3 180) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 14 "/SDA0") (pinfunction "SDA0"))
    (pad "83" smd rect (at -2 -14.9 180) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "/+5v") (pinfunction "+5v_(Input)"))
    (pad "84" smd rect (at 1.08 -14.9 180) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 8 "/+3.3v") (pinfunction "+3.3v_(Output)"))
    (pad "85" smd rect (at -2 -14.5 180) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "/+5v") (pinfunction "+5v_(Input)"))
    (pad "86" smd rect (at 1.08 -14.5 180) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 8 "/+3.3v") (pinfunction "+3.3v_(Output)"))
    (pad "87" smd rect (at -2 -14.1 180) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "/+5v") (pinfunction "+5v_(Input)"))
    (pad "88" smd rect (at 1.08 -14.1 180) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 165 "/+1.8v") (pinfunction "+1.8v_(Output)"))
    (pad "89" smd rect (at -2 -13.7 180) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 166 "/WL_nDis") (pinfunction "WL_nDisable"))
    (pad "90" smd rect (at 1.08 -13.7 180) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 165 "/+1.8v") (pinfunction "+1.8v_(Output)"))
    (pad "91" smd rect (at -2 -13.3 180) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 164 "/BT_nDis") (pinfunction "BT_nDisable"))
    (pad "92" smd rect (at 1.08 -13.3 180) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 163 "/RUN_PG") (pinfunction "RUN_PG"))
    (pad "93" smd rect (at -2 -12.9 180) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 100 "/nRPIBOOT") (pinfunction "nRPIBOOT"))
    (pad "94" smd rect (at 1.08 -12.9 180) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 97 "/AIN1") (pinfunction "AnalogIP1"))
    (pad "95" smd rect (at -2 -12.5 180) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 162 "/nPWR_LED") (pinfunction "nPI_LED_PWR"))
    (pad "96" smd rect (at 1.08 -12.5 180) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 98 "/AIN0") (pinfunction "AnalogIP0"))
    (pad "97" smd rect (at -2 -12.1 180) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 161 "Net-(Module2-Pad97)") (pinfunction "Camera_GPIO"))
    (pad "98" smd rect (at 1.08 -12.1 180) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "GND"))
    (pad "99" smd rect (at -2 -11.7 180) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 92 "/GLOBAL_EN") (pinfunction "Global_EN"))
    (pad "100" smd rect (at 1.08 -11.7 180) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 160 "/nEXTRST") (pinfunction "nEXTRST"))
    (pad "101" smd rect (at 31.92 -31.3 180) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 159 "/USBOTG") (pinfunction "USB_OTG_ID"))
    (pad "102" smd rect (at 35 -31.3 180) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 116 "/PCIE_CLK_nREQ") (pinfunction "PCIe_CLK_nREQ"))
    (pad "103" smd rect (at 31.92 -30.9 180) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 158 "/USB2_N") (pinfunction "USB2_N"))
    (pad "104" smd rect (at 35 -30.9 180) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 157 "no_connect_193") (pinfunction "Reserved"))
    (pad "105" smd rect (at 31.92 -30.5 180) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 156 "/USB2_P") (pinfunction "USB2_P"))
    (pad "106" smd rect (at 35 -30.5 180) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 155 "no_connect_194") (pinfunction "Reserved"))
    (pad "107" smd rect (at 31.92 -30.1 180) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "GND"))
    (pad "108" smd rect (at 35 -30.1 180) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "GND"))
    (pad "109" smd rect (at 31.92 -29.7 180) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 124 "/PCIE_nRST") (pinfunction "PCIe_nRST"))
    (pad "110" smd rect (at 35 -29.7 180) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 123 "/PCIE_CLK_P") (pinfunction "PCIe_CLK_P"))
    (pad "111" smd rect (at 31.92 -29.3 180) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 94 "/TV_OUT") (pinfunction "VDAC_COMP"))
    (pad "112" smd rect (at 35 -29.3 180) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 122 "/PCIE_CLK_N") (pinfunction "PCIe_CLK_N"))
    (pad "113" smd rect (at 31.92 -28.9 180) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "GND"))
    (pad "114" smd rect (at 35 -28.9 180) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "GND"))
    (pad "115" smd rect (at 31.92 -28.5 180) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 112 "/CAM1_D0_N") (pinfunction "CAM1_D0_N") (die_length 0.02))
    (pad "116" smd rect (at 35 -28.5 180) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 120 "/PCIE_RX_P") (pinfunction "PCIe_RX_P"))
    (pad "117" smd rect (at 31.92 -28.1 180) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 111 "/CAM1_D0_P") (pinfunction "CAM1_D0_P") (die_length 0.01))
    (pad "118" smd rect (at 35 -28.1 180) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 121 "/PCIE_RX_N") (pinfunction "PCIe_RX_N"))
    (pad "119" smd rect (at 31.92 -27.7 180) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "GND"))
    (pad "120" smd rect (at 35 -27.7 180) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "GND"))
    (pad "121" smd rect (at 31.92 -27.3 180) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 110 "/CAM1_D1_N") (pinfunction "CAM1_D1_N") (die_length 0.4))
    (pad "122" smd rect (at 35 -27.3 180) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 114 "/PCIE_TX_P") (pinfunction "PCIe_TX_P"))
    (pad "123" smd rect (at 31.92 -26.9 180) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 109 "/CAM1_D1_P") (pinfunction "CAM1_D1_P") (die_length 0.4))
    (pad "124" smd rect (at 35 -26.9 180) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 115 "/PCIE_TX_N") (pinfunction "PCIe_TX_N"))
    (pad "125" smd rect (at 31.92 -26.5 180) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "GND"))
    (pad "126" smd rect (at 35 -26.5 180) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "GND"))
    (pad "127" smd rect (at 31.92 -26.1 180) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 108 "/CAM1_C_N") (pinfunction "CAM1_C_N") (die_length 0.78))
    (pad "128" smd rect (at 35 -26.1 180) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 154 "/CAM0_D0_N") (pinfunction "CAM0_D0_N") (die_length 0.06))
    (pad "129" smd rect (at 31.92 -25.7 180) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 107 "/CAM1_C_P") (pinfunction "CAM1_C_P") (die_length 0.78))
    (pad "130" smd rect (at 35 -25.7 180) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 153 "/CAM0_D0_P") (pinfunction "CAM0_D0_P") (die_length 0.07))
    (pad "131" smd rect (at 31.92 -25.3 180) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "GND"))
    (pad "132" smd rect (at 35 -25.3 180) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "GND"))
    (pad "133" smd rect (at 31.92 -24.9 180) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 106 "/CAM1_D2_N") (pinfunction "CAM1_D2_N") (die_length 0.05))
    (pad "134" smd rect (at 35 -24.9 180) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 152 "/CAM0_D1_N") (pinfunction "CAM0_D1_N"))
    (pad "135" smd rect (at 31.92 -24.5 180) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 105 "/CAM1_D2_P") (pinfunction "CAM1_D2_P") (die_length 0.04))
    (pad "136" smd rect (at 35 -24.5 180) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 151 "/CAM0_D1_P") (pinfunction "CAM0_D1_P"))
    (pad "137" smd rect (at 31.92 -24.1 180) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "GND"))
    (pad "138" smd rect (at 35 -24.1 180) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "GND"))
    (pad "139" smd rect (at 31.92 -23.7 180) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 104 "/CAM1_D3_N") (pinfunction "CAM1_D3_N"))
    (pad "140" smd rect (at 35 -23.7 180) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 150 "/CAM0_C_N") (pinfunction "CAM0_C_N") (die_length 0.02))
    (pad "141" smd rect (at 31.92 -23.3 180) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 103 "/CAM1_D3_P") (pinfunction "CAM1_D3_P"))
    (pad "142" smd rect (at 35 -23.3 180) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 149 "/CAM0_C_P") (pinfunction "CAM0_C_P") (die_length 0.02))
    (pad "143" smd rect (at 31.92 -22.9 180) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 48 "/HDMI1_HOTPLUG") (pinfunction "HDMI1_HOTPLUG"))
    (pad "144" smd rect (at 35 -22.9 180) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "GND"))
    (pad "145" smd rect (at 31.92 -22.5 180) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 47 "/HDMI1_SDA") (pinfunction "HDMI1_SDA"))
    (pad "146" smd rect (at 35 -22.5 180) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 36 "/HDMI1_D2_P") (pinfunction "HDMI1_TX2_P"))
    (pad "147" smd rect (at 31.92 -22.1 180) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 46 "/HDMI1_SCL") (pinfunction "HDMI1_SCL"))
    (pad "148" smd rect (at 35 -22.1 180) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 37 "/HDMI1_D2_N") (pinfunction "HDMI1_TX2_N"))
    (pad "149" smd rect (at 31.92 -21.7 180) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 44 "/HDMI1_CEC") (pinfunction "HDMI1_CEC"))
    (pad "150" smd rect (at 35 -21.7 180) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "GND"))
    (pad "151" smd rect (at 31.92 -21.3 180) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 138 "/HDMI0_CEC") (pinfunction "HDMI0_CEC"))
    (pad "152" smd rect (at 35 -21.3 180) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 38 "/HDMI1_D1_P") (pinfunction "HDMI1_TX1_P") (die_length 1))
    (pad "153" smd rect (at 31.92 -20.9 180) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 142 "/HDMI0_HOTPLUG") (pinfunction "HDMI0_HOTPLUG"))
    (pad "154" smd rect (at 35 -20.9 180) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 39 "/HDMI1_D1_N") (pinfunction "HDMI1_TX1_N") (die_length 1))
    (pad "155" smd rect (at 31.92 -20.5 180) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "GND"))
    (pad "156" smd rect (at 35 -20.5 180) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "GND"))
    (pad "157" smd rect (at 31.92 -20.1 180) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 148 "/DSI0_D0_N") (pinfunction "DSI0_D0_N"))
    (pad "158" smd rect (at 35 -20.1 180) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 40 "/HDMI1_D0_P") (pinfunction "HDMI1_TX0_P") (die_length 1.51))
    (pad "159" smd rect (at 31.92 -19.7 180) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 147 "/DSI0_D0_P") (pinfunction "DSI0_D0_P"))
    (pad "160" smd rect (at 35 -19.7 180) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 41 "/HDMI1_D0_N") (pinfunction "HDMI1_TX0_N") (die_length 1.51))
    (pad "161" smd rect (at 31.92 -19.3 180) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "GND"))
    (pad "162" smd rect (at 35 -19.3 180) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "GND"))
    (pad "163" smd rect (at 31.92 -18.9 180) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 146 "/DSI0_D1_N") (pinfunction "DSI0_D1_N"))
    (pad "164" smd rect (at 35 -18.9 180) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 42 "/HDMI1_CK_P") (pinfunction "HDMI1_CLK_P") (die_length 2.47))
    (pad "165" smd rect (at 31.92 -18.5 180) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 145 "/DSI0_D1_P") (pinfunction "DSI0_D1_P"))
    (pad "166" smd rect (at 35 -18.5 180) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 43 "/HDMI1_CK_N") (pinfunction "HDMI1_CLK_N") (die_length 2.47))
    (pad "167" smd rect (at 31.92 -18.1 180) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "GND"))
    (pad "168" smd rect (at 35 -18.1 180) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "GND"))
    (pad "169" smd rect (at 31.92 -17.7 180) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 144 "/DSI0_C_N") (pinfunction "DSI0_C_N"))
    (pad "170" smd rect (at 35 -17.7 180) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 130 "/HDMI0_D2_P") (pinfunction "HDMI0_TX2_P"))
    (pad "171" smd rect (at 31.92 -17.3 180) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 143 "/DSI0_C_P") (pinfunction "DSI0_C_P"))
    (pad "172" smd rect (at 35 -17.3 180) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 131 "/HDMI0_D2_N") (pinfunction "HDMI0_TX2_N"))
    (pad "173" smd rect (at 31.92 -16.9 180) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "GND"))
    (pad "174" smd rect (at 35 -16.9 180) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "GND"))
    (pad "175" smd rect (at 31.92 -16.5 180) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 27 "/DSI1_D0_N") (pinfunction "DSI1_D0_N"))
    (pad "176" smd rect (at 35 -16.5 180) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 132 "/HDMI0_D1_P") (pinfunction "HDMI0_TX1_P") (die_length 0.62))
    (pad "177" smd rect (at 31.92 -16.1 180) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 26 "/DSI1_D0_P") (pinfunction "DSI1_D0_P") (die_length 0.01))
    (pad "178" smd rect (at 35 -16.1 180) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 133 "/HDMI0_D1_N") (pinfunction "HDMI0_TX1_N") (die_length 0.62))
    (pad "179" smd rect (at 31.92 -15.7 180) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "GND"))
    (pad "180" smd rect (at 35 -15.7 180) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "GND"))
    (pad "181" smd rect (at 31.92 -15.3 180) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 25 "/DSI1_D1_N") (pinfunction "DSI1_D1_N") (die_length 1.06))
    (pad "182" smd rect (at 35 -15.3 180) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 134 "/HDMI0_D0_P") (pinfunction "HDMI0_TX0_P") (die_length 1.76))
    (pad "183" smd rect (at 31.92 -14.9 180) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 24 "/DSI1_D1_P") (pinfunction "DSI1_D1_P") (die_length 1.06))
    (pad "184" smd rect (at 35 -14.9 180) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 135 "/HDMI0_D0_N") (pinfunction "HDMI0_TX0_N") (die_length 1.76))
    (pad "185" smd rect (at 31.92 -14.5 180) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "GND"))
    (pad "186" smd rect (at 35 -14.5 180) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "GND"))
    (pad "187" smd rect (at 31.92 -14.1 180) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 23 "/DSI1_C_N") (pinfunction "DSI1_C_N"))
    (pad "188" smd rect (at 35 -14.1 180) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 136 "/HDMI0_CK_P") (pinfunction "HDMI0_CLK_P") (die_length 3.24))
    (pad "189" smd rect (at 31.92 -13.7 180) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 22 "/DSI1_C_P") (pinfunction "DSI1_C_P") (die_length 1.28))
    (pad "190" smd rect (at 35 -13.7 180) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 137 "/HDMI0_CK_N") (pinfunction "HDMI0_CLK_N") (die_length 3.25))
    (pad "191" smd rect (at 31.92 -13.3 180) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "GND") (die_length 1.28))
    (pad "192" smd rect (at 35 -13.3 180) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "GND"))
    (pad "193" smd rect (at 31.92 -12.9 180) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 21 "/DSI1_D2_N") (pinfunction "DSI1_D2_N") (die_length 0.83))
    (pad "194" smd rect (at 35 -12.9 180) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 19 "/DSI1_D3_N") (pinfunction "DSI1_D3_N") (die_length 3.78))
    (pad "195" smd rect (at 31.92 -12.5 180) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 20 "/DSI1_D2_P") (pinfunction "DSI1_D2_P") (die_length 0.84))
    (pad "196" smd rect (at 35 -12.5 180) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 18 "/DSI1_D3_P") (pinfunction "DSI1_D3_P") (die_length 3.78))
    (pad "197" smd rect (at 31.92 -12.1 180) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "GND"))
    (pad "198" smd rect (at 35 -12.1 180) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "GND"))
    (pad "199" smd rect (at 31.92 -11.7 180) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 141 "/HDMI0_SDA") (pinfunction "HDMI0_SDA"))
    (pad "200" smd rect (at 35 -11.7 180) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 140 "/HDMI0_SCL") (pinfunction "HDMI0_SCL"))
    (model "./CM4.3dshapes/DF40C-100DS.stp"
      (offset (xyz -0.46 15.38 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
    (model "./CM4IO.3dshapes/DF40C-100DS.stp"
      (offset (xyz 33.46 15.38 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (footprint "Connector_USB:USB_A_Wuerth_614004134726_Horizontal" (layer "F.Cu")
    (tedit 600EF080)
    (at 139.58 118.15 90)
    (descr "USB A connector https://www.we-online.com/catalog/datasheet/614004134726.pdf")
    (tags "USB_A Female Connector receptacle")
    (property "Sheet file" "CM4_1.kicad_sch")
    (property "Sheet name" "")
    (attr through_hole)
    (fp_text reference "J7" (at -4.36 0.06 90) (layer "F.SilkS"))
    (fp_text value "USB_A" (at 0 5.08 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at -2.855 0 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.6 1.6) (drill 0.92) (layers *.Cu *.Mask)
      (net 3 "/+5v") (pinfunction "VBUS"))
    (pad "2" thru_hole circle (at 2 0 90) (size 1.6 1.6) (drill 0.92) (layers *.Cu *.Mask)
      (net 53 "/HD2_N") (pinfunction "D-"))
    (pad "3" thru_hole circle (at 4 0 90) (size 1.6 1.6) (drill 0.92) (layers *.Cu *.Mask)
      (net 54 "/HD2_P") (pinfunction "D+"))
    (pad "4" thru_hole circle (at 6 0 90) (size 1.6 1.6) (drill 0.92) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "GND"))
    (pad "5" thru_hole circle (at 6.27 2.72 90) (size 2.15 2.15) (drill 1.5) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Shield"))
    (pad "5" thru_hole circle (at -0.73 -2.72 90) (size 2.15 2.15) (drill 1.5) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Shield"))
    (pad "5" thru_hole circle (at 6.27 -2.72 90) (size 2.15 2.15) (drill 1.5) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Shield"))
    (pad "5" thru_hole circle (at -0.73 2.72 90) (size 2.15 2.15) (drill 1.5) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Shield"))
    (model "${KISYS3DMOD}/Connector_USB.3dshapes/USB_A_Wuerth_614004134726_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "CM4IO:type-c_90degree_14pin" (layer "F.Cu")
    (tedit 600FC9F8)
    (at 112.95 120.215 -90)
    (fp_text reference "REF**" (at -0.125 -3.02 90) (layer "F.SilkS"))
    (fp_text value "type-c_90degree_14pin" (at 0 2.19 90) (layer "F.Fab"))
    (pad "1" thru_hole oval (at -2.925 0.39 270) (size 0.6 0.6) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 "GND"))
    (pad "2" thru_hole oval (at -2.475 -0.39 270) (size 0.6 0.6) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 "GND"))
    (pad "3" thru_hole oval (at -2.025 0.39 270) (size 0.6 0.6) (drill 0.4) (layers *.Cu *.Mask)
      (net 129 "/VBUS_OTG"))
    (pad "4" thru_hole oval (at -1.575 -0.39 270) (size 0.6 0.6) (drill 0.4) (layers *.Cu *.Mask)
      (net 129 "/VBUS_OTG"))
    (pad "5" thru_hole oval (at -1.125 0.39 270) (size 0.6 0.6) (drill 0.4) (layers *.Cu *.Mask)
      (net 128 "/USBD_N"))
    (pad "6" thru_hole oval (at -0.675 -0.39 270) (size 0.6 0.6) (drill 0.4) (layers *.Cu *.Mask))
    (pad "7" thru_hole oval (at -0.225 0.39 270) (size 0.6 0.6) (drill 0.4) (layers *.Cu *.Mask)
      (net 127 "/USBD_P"))
    (pad "8" thru_hole oval (at 0.225 -0.39 270) (size 0.6 0.6) (drill 0.4) (layers *.Cu *.Mask)
      (net 127 "/USBD_P"))
    (pad "9" thru_hole oval (at 0.675 0.39 270) (size 0.6 0.6) (drill 0.4) (layers *.Cu *.Mask))
    (pad "10" thru_hole oval (at 1.125 -0.39 270) (size 0.6 0.6) (drill 0.4) (layers *.Cu *.Mask)
      (net 128 "/USBD_N"))
    (pad "11" thru_hole oval (at 1.575 0.39 270) (size 0.6 0.6) (drill 0.4) (layers *.Cu *.Mask)
      (net 129 "/VBUS_OTG"))
    (pad "12" thru_hole oval (at 2.025 -0.39 270) (size 0.6 0.6) (drill 0.4) (layers *.Cu *.Mask)
      (net 129 "/VBUS_OTG"))
    (pad "13" thru_hole oval (at 2.475 0.39 270) (size 0.6 0.6) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 "GND"))
    (pad "14" thru_hole oval (at 2.925 -0.39 270) (size 0.6 0.6) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 "GND"))
    (pad "15" thru_hole oval (at 2.425 -1.43 270) (size 1.9 0.9) (drill oval 1.6 0.6) (layers *.Cu *.Mask)
      (net 1 "GND"))
    (pad "15" thru_hole oval (at -2.42 1.43 270) (size 1.9 0.9) (drill oval 1.6 0.6) (layers *.Cu *.Mask)
      (net 1 "GND"))
    (pad "15" thru_hole oval (at -2.42 -1.43 270) (size 1.9 0.9) (drill oval 1.6 0.6) (layers *.Cu *.Mask)
      (net 1 "GND"))
    (pad "15" thru_hole oval (at 2.43 1.43 270) (size 1.9 0.9) (drill oval 1.6 0.6) (layers *.Cu *.Mask)
      (net 1 "GND"))
  )
  (footprint "Connector_HDMI:HDMI_Micro-D_Molex_46765-1x01" (layer "F.Cu")
    (tedit 601129B6)
    (at 97.58 114.69 -90)
    (descr "HDMI, Micro, Type D, THT, 0.4mm pitch, 19 ckt, right angle (http://www.molex.com/pdm_docs/sd/467651301_sd.pdf)")
    (tags "hdmi micro type d right angle tht")
    (property "Field4" "Farnell")
    (property "Field5" "2614936")
    (property "Field6" "690-019-298-412")
    (property "Field7" "EDAC")
    (property "Field8" "UCON00802")
    (property "Part Description" "HDMI Connector, Right Angle, 19 Contacts, Receptacle, Surface Mount, Surface Mount Right Angle")
    (property "Sheet file" "CM4_1.kicad_sch")
    (property "Sheet name" "")
    (attr smd)
    (fp_text reference "J25" (at 0 -6.3 90) (layer "F.SilkS"))
    (fp_text value "690-019-298-412" (at 0 3.6 90) (layer "F.Fab"))
    (fp_text user "KEEPOUT" (at 0 -0.47 90) (layer "Cmts.User"))
    (fp_text user "${REFERENCE}" (at 0 -3.3 90) (layer "F.Fab"))
    (pad "1" smd rect (at 1.8 -4.775 270) (size 0.23 0.85) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 130 "/HDMI0_D2_P") (pinfunction "D2+"))
    (pad "2" smd rect (at 1.6 -3.55 270) (size 0.23 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "D2S"))
    (pad "3" smd rect (at 1.4 -4.775 270) (size 0.23 0.85) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 131 "/HDMI0_D2_N") (pinfunction "D2-"))
    (pad "4" smd rect (at 1.2 -3.55 270) (size 0.23 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 132 "/HDMI0_D1_P") (pinfunction "D1+"))
    (pad "5" smd rect (at 1 -4.775 270) (size 0.23 0.85) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "D1S"))
    (pad "6" smd rect (at 0.8 -3.55 270) (size 0.23 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 133 "/HDMI0_D1_N") (pinfunction "D1-"))
    (pad "7" smd rect (at 0.6 -4.775 270) (size 0.23 0.85) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 134 "/HDMI0_D0_P") (pinfunction "D0+"))
    (pad "8" smd rect (at 0.4 -3.55 270) (size 0.23 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "D0S"))
    (pad "9" smd rect (at 0.2 -4.775 270) (size 0.23 0.85) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 135 "/HDMI0_D0_N") (pinfunction "D0-"))
    (pad "10" smd rect (at 0 -3.55 270) (size 0.23 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 136 "/HDMI0_CK_P") (pinfunction "CK+"))
    (pad "11" smd rect (at -0.2 -4.775 270) (size 0.23 0.85) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "CKS"))
    (pad "12" smd rect (at -0.4 -3.55 270) (size 0.23 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 137 "/HDMI0_CK_N") (pinfunction "CK-"))
    (pad "13" smd rect (at -0.6 -4.775 270) (size 0.23 0.85) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 138 "/HDMI0_CEC") (pinfunction "CEC"))
    (pad "14" smd rect (at -0.8 -3.55 270) (size 0.23 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 139 "no_connect_191") (pinfunction "UTILITY/HEAC+"))
    (pad "15" smd rect (at -1 -4.775 270) (size 0.23 0.85) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 140 "/HDMI0_SCL") (pinfunction "SCL"))
    (pad "16" smd rect (at -1.2 -3.55 270) (size 0.23 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 141 "/HDMI0_SDA") (pinfunction "SDA"))
    (pad "17" smd rect (at -1.4 -4.775 270) (size 0.23 0.85) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "GND"))
    (pad "18" smd rect (at -1.6 -3.55 270) (size 0.23 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "/+5v") (pinfunction "+5V"))
    (pad "19" smd rect (at -1.8 -4.775 270) (size 0.23 0.85) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 142 "/HDMI0_HOTPLUG") (pinfunction "HPD/HEAC-"))
    (pad "SH" thru_hole oval (at 3.1 -3.36 270) (size 1.5 2.55) (drill oval 0.65 1.7) (layers *.Cu *.Mask)
      (net 1 "GND"))
    (pad "SH" thru_hole oval (at -3.1 -3.36 270) (size 1.5 2.55) (drill oval 0.65 1.7) (layers *.Cu *.Mask)
      (net 1 "GND"))
    (pad "SH" thru_hole oval (at -3.1 0 270) (size 1.5 2.55) (drill oval 0.65 1.7) (layers *.Cu *.Mask)
      (net 1 "GND"))
    (pad "SH" thru_hole oval (at 3.1 0 270) (size 1.5 2.55) (drill oval 0.65 1.7) (layers *.Cu *.Mask)
      (net 1 "GND"))
    (model "${KISYS3DMOD}/Connector_HDMI.3dshapes/HDMI_Micro-D_Molex_46765-1x01.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 137.8 121.64 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheet file" "CM4_1.kicad_sch")
    (property "Sheet name" "")
    (attr smd)
    (fp_text reference "C62" (at -2.97 -0.03) (layer "B.SilkS"))
    (fp_text value "22uf" (at 0 -1.68) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.95 0 180) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 3 "/+5v"))
    (pad "2" smd roundrect (at 0.95 0 180) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 1 "GND"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Crystal:Crystal_SMD_EuroQuartz_MT-4Pin_3.2x2.5mm" (layer "B.Cu")
    (tedit 600F9BA4)
    (at 149.34 97.53 180)
    (descr "SMD Crystal EuroQuartz MT series http://cdn-reichelt.de/documents/datenblatt/B400/MT.pdf, 3.2x2.5mm^2 package")
    (tags "SMD SMT crystal")
    (property "Field4" "Farnell")
    (property "Field5" "2508493")
    (property "Field6" "X24M000000S128")
    (property "Field7" "AEL")
    (property "Part Description" "24MHz Crystal 18pf 30ppm 30ppm")
    (property "Sheet file" "CM4_1.kicad_sch")
    (property "Sheet name" "")
    (attr smd)
    (fp_text reference "Y1" (at -1.62 2.32) (layer "B.SilkS"))
    (fp_text value "24MHz" (at 0 -2.45) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd rect (at -1.1 -0.9 180) (size 1.3 1) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 6 "Net-(C6-Pad1)") (pinfunction "1"))
    (pad "2" smd rect (at 1.1 -0.9 180) (size 1.3 1) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
    (pad "3" smd rect (at 1.1 0.9 180) (size 1.3 1) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 7 "Net-(C7-Pad1)") (pinfunction "2"))
    (pad "4" smd rect (at -1.1 0.9 180) (size 1.3 1) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND"))
    (model "${KISYS3DMOD}/Crystal.3dshapes/Crystal_SMD_EuroQuartz_MT-4Pin_3.2x2.5mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "B.Cu")
    (tedit 600FD01F)
    (at 147.35 124.11)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Field4" "Digikey")
    (property "Field5" "490-14381-1-ND")
    (property "Field6" "GRM21BR71A106KA73L")
    (property "Field7" "Murata")
    (property "Field8" "111893011")
    (property "Part Description" "	10uF 10% 10V Ceramic Capacitor X7R 0805 (2012 Metric)")
    (property "Sheet file" "CM4_1.kicad_sch")
    (property "Sheet name" "")
    (attr smd)
    (fp_text reference "C58" (at 3.45 0.03) (layer "B.SilkS"))
    (fp_text value "10u" (at 0 -1.68) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.95 0) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 1 "GND"))
    (pad "2" smd roundrect (at 0.95 0) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 3 "/+5v"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0402_1005Metric" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 142.13 92.35 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Field4" "Farnell")
    (property "Field5" "1458788")
    (property "Field6" "MCR01MZPF3602")
    (property "Field7" "Rohm")
    (property "Part Description" "Resistor 36K M1005 1% 63mW")
    (property "Sheet file" "CM4_1.kicad_sch")
    (property "Sheet name" "")
    (attr smd)
    (fp_text reference "R6" (at 1.82 -0.04 90) (layer "B.SilkS"))
    (fp_text value "36K 1%" (at 0 -1.17 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.51 0 90) (size 0.54 0.64) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 182 "Net-(R6-Pad1)"))
    (pad "2" smd roundrect (at 0.51 0 90) (size 0.54 0.64) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 1 "GND"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "B.Cu")
    (tedit 600FD01F)
    (at 137.79 124.02)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Field4" "Digikey")
    (property "Field5" "490-14381-1-ND")
    (property "Field6" "GRM21BR71A106KA73L")
    (property "Field7" "Murata")
    (property "Field8" "111893011")
    (property "Part Description" "	10uF 10% 10V Ceramic Capacitor X7R 0805 (2012 Metric)")
    (property "Sheet file" "CM4_1.kicad_sch")
    (property "Sheet name" "")
    (attr smd)
    (fp_text reference "C61" (at 3.17 -0.04) (layer "B.SilkS"))
    (fp_text value "10u" (at 0 -1.68) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.95 0) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 1 "GND"))
    (pad "2" smd roundrect (at 0.95 0) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 3 "/+5v"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 147.76 79.5 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheet file" "CM4_1.kicad_sch")
    (property "Sheet name" "")
    (attr smd)
    (fp_text reference "C5" (at 0 1.16 90) (layer "B.SilkS"))
    (fp_text value "10nf" (at 0 -1.16 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.48 0 90) (size 0.56 0.62) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 5 "Net-(C5-Pad1)"))
    (pad "2" smd roundrect (at 0.48 0 90) (size 0.56 0.62) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 4 "/pcie+3.3v"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_FFC-FPC:Hirose_FH12-22S-0.5SH_1x22-1MP_P0.50mm_Horizontal" (layer "B.Cu")
    (tedit 5D24667B)
    (at 121.81 98.33 180)
    (descr "Hirose FH12, FFC/FPC connector, FH12-22S-0.5SH, 22 Pins per row (https://www.hirose.com/product/en/products/FH12/FH12-24S-0.5SH(55)/), generated with kicad-footprint-generator")
    (tags "connector Hirose FH12 horizontal")
    (property "Field4" "Mouser")
    (property "Field5" "798-FH12-22S-0.5SH55")
    (property "Field6" "FH12-22S-0.5SH55")
    (property "Field7" "Hirose")
    (property "Part Description" "22 Position FFC, FPC Connector Contacts, Bottom 0.020\" (0.50mm) Surface Mount, Right Angle")
    (property "Sheet file" "CM4_1.kicad_sch")
    (property "Sheet name" "")
    (attr smd)
    (fp_text reference "J16" (at 0 3.7) (layer "B.SilkS"))
    (fp_text value "Conn_01x22_Female" (at 0 -5.6) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -3.7) (layer "B.Fab"))
    (pad "1" smd rect (at -5.25 1.85 180) (size 0.3 1.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND") (pinfunction "Pin_1"))
    (pad "2" smd rect (at -4.75 1.85 180) (size 0.3 1.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 112 "/CAM1_D0_N") (pinfunction "Pin_2"))
    (pad "3" smd rect (at -4.25 1.85 180) (size 0.3 1.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 111 "/CAM1_D0_P") (pinfunction "Pin_3"))
    (pad "4" smd rect (at -3.75 1.85 180) (size 0.3 1.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND") (pinfunction "Pin_4"))
    (pad "5" smd rect (at -3.25 1.85 180) (size 0.3 1.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 110 "/CAM1_D1_N") (pinfunction "Pin_5"))
    (pad "6" smd rect (at -2.75 1.85 180) (size 0.3 1.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 109 "/CAM1_D1_P") (pinfunction "Pin_6"))
    (pad "7" smd rect (at -2.25 1.85 180) (size 0.3 1.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND") (pinfunction "Pin_7"))
    (pad "8" smd rect (at -1.75 1.85 180) (size 0.3 1.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 108 "/CAM1_C_N") (pinfunction "Pin_8"))
    (pad "9" smd rect (at -1.25 1.85 180) (size 0.3 1.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 107 "/CAM1_C_P") (pinfunction "Pin_9"))
    (pad "10" smd rect (at -0.75 1.85 180) (size 0.3 1.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND") (pinfunction "Pin_10"))
    (pad "11" smd rect (at -0.25 1.85 180) (size 0.3 1.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 106 "/CAM1_D2_N") (pinfunction "Pin_11"))
    (pad "12" smd rect (at 0.25 1.85 180) (size 0.3 1.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 105 "/CAM1_D2_P") (pinfunction "Pin_12"))
    (pad "13" smd rect (at 0.75 1.85 180) (size 0.3 1.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND") (pinfunction "Pin_13"))
    (pad "14" smd rect (at 1.25 1.85 180) (size 0.3 1.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 104 "/CAM1_D3_N") (pinfunction "Pin_14"))
    (pad "15" smd rect (at 1.75 1.85 180) (size 0.3 1.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 103 "/CAM1_D3_P") (pinfunction "Pin_15"))
    (pad "16" smd rect (at 2.25 1.85 180) (size 0.3 1.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND") (pinfunction "Pin_16"))
    (pad "17" smd rect (at 2.75 1.85 180) (size 0.3 1.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 102 "/CAM_GPIO") (pinfunction "Pin_17"))
    (pad "18" smd rect (at 3.25 1.85 180) (size 0.3 1.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 101 "no_connect_181") (pinfunction "Pin_18"))
    (pad "19" smd rect (at 3.75 1.85 180) (size 0.3 1.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND") (pinfunction "Pin_19"))
    (pad "20" smd rect (at 4.25 1.85 180) (size 0.3 1.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "/SCL0") (pinfunction "Pin_20"))
    (pad "21" smd rect (at 4.75 1.85 180) (size 0.3 1.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 14 "/SDA0") (pinfunction "Pin_21"))
    (pad "22" smd rect (at 5.25 1.85 180) (size 0.3 1.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 8 "/+3.3v") (pinfunction "Pin_22"))
    (pad "MP" smd rect (at 7.15 -1.4 180) (size 1.8 2.2) (layers "B.Cu" "B.Paste" "B.Mask"))
    (pad "MP" smd rect (at -7.15 -1.4 180) (size 1.8 2.2) (layers "B.Cu" "B.Paste" "B.Mask"))
    (model "${KISYS3DMOD}/Connector_FFC-FPC.3dshapes/Hirose_FH12-22S-0.5SH_1x22-1MP_P0.50mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0402_1005Metric" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 144.43 92.33 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Field4" "Farnell")
    (property "Field5" "1458788")
    (property "Field6" "MCR01MZPF3602")
    (property "Field7" "Rohm")
    (property "Part Description" "Resistor 36K M1005 1% 63mW")
    (property "Sheet file" "CM4_1.kicad_sch")
    (property "Sheet name" "")
    (attr smd)
    (fp_text reference "R7" (at 1.9 0.15 90) (layer "B.SilkS"))
    (fp_text value "36K 1%" (at 0 -1.17 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.51 0 90) (size 0.54 0.64) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 183 "Net-(R7-Pad1)"))
    (pad "2" smd roundrect (at 0.51 0 90) (size 0.54 0.64) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 1 "GND"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0402_1005Metric" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 147.32 99.82 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Field4" "Farnell")
    (property "Field5" "9239367")
    (property "Field6" "MCR01MZPF1202")
    (property "Field7" "Rohm")
    (property "Part Description" "Resistor 12K M1005 1% 63mW")
    (property "Sheet file" "CM4_1.kicad_sch")
    (property "Sheet name" "")
    (attr smd)
    (fp_text reference "R4" (at 0.52 1.38 90) (layer "B.SilkS"))
    (fp_text value "12K 1%" (at 0 -1.17) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.51 0 180) (size 0.54 0.64) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 1 "GND"))
    (pad "2" smd roundrect (at 0.51 0 180) (size 0.54 0.64) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 180 "Net-(R4-Pad2)"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 147.38 121.73 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheet file" "CM4_1.kicad_sch")
    (property "Sheet name" "")
    (attr smd)
    (fp_text reference "C59" (at -3.17 -0.04) (layer "B.SilkS"))
    (fp_text value "22uf" (at 0 -1.68) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.95 0 180) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 3 "/+5v"))
    (pad "2" smd roundrect (at 0.95 0 180) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 1 "GND"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 150.04 99.83 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Field4" "Digikey")
    (property "Field5" "490-17672-1-ND")
    (property "Field6" "GJM1555C1H270JB01D")
    (property "Field7" "Murata")
    (property "Field8" "UCAP00738 ")
    (property "Part Description" "	27pF 5% 50V Ceramic Capacitor C0G, NP0 0402 (1005 Metric)")
    (property "Sheet file" "CM4_1.kicad_sch")
    (property "Sheet name" "")
    (attr smd)
    (fp_text reference "C6" (at -1.95 -0.14) (layer "B.SilkS"))
    (fp_text value "27pF" (at 0 -1.16) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.48 0 180) (size 0.56 0.62) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 6 "Net-(C6-Pad1)"))
    (pad "2" smd roundrect (at 0.48 0 180) (size 0.56 0.62) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 1 "GND"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "B.Cu")
    (tedit 600FD01F)
    (at 118.72 126.23)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Field4" "Digikey")
    (property "Field5" "490-14381-1-ND")
    (property "Field6" "GRM21BR71A106KA73L")
    (property "Field7" "Murata")
    (property "Field8" "111893011")
    (property "Part Description" "	10uF 10% 10V Ceramic Capacitor X7R 0805 (2012 Metric)")
    (property "Sheet file" "CM4_1.kicad_sch")
    (property "Sheet name" "")
    (attr smd)
    (fp_text reference "C66" (at 3.15 -0.06) (layer "B.SilkS"))
    (fp_text value "10u" (at 0 -1.68) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.95 0) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 1 "GND"))
    (pad "2" smd roundrect (at 0.95 0) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 3 "/+5v"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "B.Cu")
    (tedit 60104F05)
    (at 151.32 74.73)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (attr smd)
    (fp_text reference "C59" (at 0.01 -1.66 180) (layer "B.SilkS"))
    (fp_text value "10u" (at 0 -1.68 180) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 180) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.95 0) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 4 "/pcie+3.3v"))
    (pad "2" smd roundrect (at 0.95 0) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 1 "GND"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_SMA" (layer "B.Cu")
    (tedit 586432E5)
    (at 139.04 82.75 -90)
    (descr "Diode SMA (DO-214AC)")
    (tags "Diode SMA (DO-214AC)")
    (property "Sheet file" "CM4_1.kicad_sch")
    (property "Sheet name" "")
    (attr smd)
    (fp_text reference "D2" (at 0 2.5 -90) (layer "B.SilkS"))
    (fp_text value "SS36" (at 0 -2.6 -90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.5 -90) (layer "B.Fab"))
    (pad "1" smd rect (at -2 0 270) (size 2.5 1.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 9 "Net-(D2-Pad1)") (pinfunction "K"))
    (pad "2" smd rect (at 2 0 270) (size 2.5 1.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND") (pinfunction "A"))
    (model "${KISYS3DMOD}/Diode_SMD.3dshapes/D_SMA.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "B.Cu")
    (tedit 60104F05)
    (at 142.68 76.23 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (attr smd)
    (fp_text reference "C60" (at 0 1.68 180) (layer "B.SilkS"))
    (fp_text value "10u" (at 0 -1.68 180) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 180) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.95 0 180) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 4 "/pcie+3.3v"))
    (pad "2" smd roundrect (at 0.95 0 180) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 1 "GND"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 115.9 94.24 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Field4" "Farnell")
    (property "Field5" "2611911")
    (property "Field6" "RM EMK105 B7104KV-F")
    (property "Field7" "TAIYO YUDEN EUROPE GMBH")
    (property "Field8" "110091611")
    (property "Part Description" "	0.1uF 10% 16V Ceramic Capacitor X7R 0402 (1005 Metric)")
    (property "Sheet file" "CM4_1.kicad_sch")
    (property "Sheet name" "")
    (attr smd)
    (fp_text reference "C52" (at 0.3 -1.07 270) (layer "B.SilkS"))
    (fp_text value "100n" (at 0 -1.16 270) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 270) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.48 0 90) (size 0.56 0.62) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 8 "/+3.3v"))
    (pad "2" smd roundrect (at 0.48 0 90) (size 0.56 0.62) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 1 "GND"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_SO:TI_SO-PowerPAD-8" (layer "B.Cu")
    (tedit 5A02F2D3)
    (at 145 83.45 180)
    (descr "8-Lead Plastic PSOP, Exposed Die Pad (TI DDA0008B, see http://www.ti.com/lit/ds/symlink/lm3404.pdf)")
    (tags "SSOP 0.50 exposed pad")
    (property "Sheet file" "CM4_1.kicad_sch")
    (property "Sheet name" "")
    (attr smd)
    (fp_text reference "U2" (at 0.17 -3.5) (layer "B.SilkS"))
    (fp_text value "LM22676MR-ADJ" (at 0 -3.4) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd rect (at -2.78 1.905 180) (size 1.91 0.61) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 5 "Net-(C5-Pad1)") (pinfunction "BOOT"))
    (pad "2" smd rect (at -2.78 0.635 180) (size 1.91 0.61) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 187 "no_connect_204") (pinfunction "NC"))
    (pad "3" smd rect (at -2.78 -0.635 180) (size 1.91 0.61) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 186 "no_connect_205") (pinfunction "NC"))
    (pad "4" smd rect (at -2.78 -1.905 180) (size 1.91 0.61) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 178 "Net-(R1-Pad2)") (pinfunction "FB"))
    (pad "5" smd rect (at 2.78 -1.905 180) (size 1.91 0.61) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 185 "no_connect_206") (pinfunction "EN"))
    (pad "6" smd rect (at 2.78 -0.635 180) (size 1.91 0.61) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND") (pinfunction "GND"))
    (pad "7" smd rect (at 2.78 0.635 180) (size 1.91 0.61) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 3 "/+5v") (pinfunction "VIN"))
    (pad "8" smd rect (at 2.78 1.905 180) (size 1.91 0.61) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 9 "Net-(D2-Pad1)") (pinfunction "SW"))
    (pad "9" smd rect (at -0.6025 0.775 180) (size 1.205 1.55) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND") (pinfunction "EP") (solder_paste_margin_ratio -0.2))
    (pad "9" smd rect (at 0.6025 -0.775 180) (size 1.205 1.55) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND") (pinfunction "EP") (solder_paste_margin_ratio -0.2))
    (pad "9" smd rect (at -0.6025 -0.775 180) (size 1.205 1.55) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND") (pinfunction "EP") (solder_paste_margin_ratio -0.2))
    (pad "9" smd rect (at 0.6025 0.775 180) (size 1.205 1.55) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND") (pinfunction "EP") (solder_paste_margin_ratio -0.2))
    (model "${KISYS3DMOD}/Package_SO.3dshapes/TI_SO-PowerPAD-8.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 147.05 92.26)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Field4" "Digikey")
    (property "Field5" "490-14381-1-ND")
    (property "Field6" "GRM21BR71A106KA73L")
    (property "Field7" "Murata")
    (property "Field8" "111893011")
    (property "Part Description" "	10uF 10% 10V Ceramic Capacitor X7R 0805 (2012 Metric)")
    (property "Sheet file" "CM4_1.kicad_sch")
    (property "Sheet name" "")
    (attr smd)
    (fp_text reference "C48" (at 0 -1.74) (layer "B.SilkS"))
    (fp_text value "10u" (at 0 -1.68) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.95 0) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 8 "/+3.3v"))
    (pad "2" smd roundrect (at 0.95 0) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 1 "GND"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 147.94 100.98)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Field4" "Farnell")
    (property "Field5" "2611911")
    (property "Field6" "RM EMK105 B7104KV-F")
    (property "Field7" "TAIYO YUDEN EUROPE GMBH")
    (property "Field8" "110091611")
    (property "Part Description" "	0.1uF 10% 16V Ceramic Capacitor X7R 0402 (1005 Metric)")
    (property "Sheet file" "CM4_1.kicad_sch")
    (property "Sheet name" "")
    (attr smd)
    (fp_text reference "C49" (at 0 1.16) (layer "B.SilkS"))
    (fp_text value "100n" (at 0 -1.16) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.48 0) (size 0.56 0.62) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 8 "/+3.3v"))
    (pad "2" smd roundrect (at 0.48 0) (size 0.56 0.62) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 1 "GND"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "B.Cu")
    (tedit 60104F05)
    (at 151.29 76.82)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (attr smd)
    (fp_text reference "C61" (at -2.89 0.5 180) (layer "B.SilkS"))
    (fp_text value "10u" (at 0 -1.68 180) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 180) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.95 0) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 4 "/pcie+3.3v"))
    (pad "2" smd roundrect (at 0.95 0) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 1 "GND"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 128.49 121.66 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheet file" "CM4_1.kicad_sch")
    (property "Sheet name" "")
    (attr smd)
    (fp_text reference "C65" (at -2.67 -0.01) (layer "B.SilkS"))
    (fp_text value "22uf" (at 0 -1.68) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.95 0 180) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 3 "/+5v"))
    (pad "2" smd roundrect (at 0.95 0 180) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 1 "GND"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Inductor_SMD:L_1206_3216Metric" (layer "B.Cu")
    (tedit 5F68FEF0)
    (at 143.8 78.66)
    (descr "Inductor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 80, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "inductor")
    (property "Sheet file" "CM4_1.kicad_sch")
    (property "Sheet name" "")
    (attr smd)
    (fp_text reference "L2" (at -3.35 -0.49) (layer "B.SilkS"))
    (fp_text value "6.8uh" (at 0 -1.9) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1.575 0) (size 1.05 1.9) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.238095)
      (net 9 "Net-(D2-Pad1)") (pinfunction "1"))
    (pad "2" smd roundrect (at 1.575 0) (size 1.05 1.9) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.238095)
      (net 4 "/pcie+3.3v") (pinfunction "2"))
    (model "${KISYS3DMOD}/Inductor_SMD.3dshapes/L_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_SO:MSOP-10_3x3mm_P0.5mm" (layer "B.Cu")
    (tedit 5A02F25C)
    (at 135.72 94.78 90)
    (descr "10-Lead Plastic Micro Small Outline Package (MS) [MSOP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SSOP 0.5")
    (property "Field4" "Farnell")
    (property "Field5" "2564479")
    (property "Field6" "FSUSB42MUX")
    (property "Field7" "Onsemi")
    (property "Part Description" "USB Switch IC 1 Channel 10-MSOP")
    (property "Sheet file" "CM4_1.kicad_sch")
    (property "Sheet name" "")
    (attr smd)
    (fp_text reference "U21" (at 0 2.6 90) (layer "B.SilkS"))
    (fp_text value "FSUSB42MUX" (at 0 -2.6 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd rect (at -2.2 1 90) (size 1.4 0.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 8 "/+3.3v") (pinfunction "VCC"))
    (pad "2" smd rect (at -2.2 0.5 90) (size 1.4 0.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 159 "/USBOTG") (pinfunction "SEL"))
    (pad "3" smd rect (at -2.2 0 90) (size 1.4 0.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 156 "/USB2_P") (pinfunction "D_P"))
    (pad "4" smd rect (at -2.2 -0.5 90) (size 1.4 0.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 158 "/USB2_N") (pinfunction "D_N"))
    (pad "5" smd rect (at -2.2 -1 90) (size 1.4 0.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND") (pinfunction "GND"))
    (pad "6" smd rect (at 2.2 -1 90) (size 1.4 0.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 190 "/USBH_N") (pinfunction "HSD0_M"))
    (pad "7" smd rect (at 2.2 -0.5 90) (size 1.4 0.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 189 "/USBH_P") (pinfunction "HSD0_P"))
    (pad "8" smd rect (at 2.2 0 90) (size 1.4 0.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 128 "/USBD_N") (pinfunction "HSD1_M"))
    (pad "9" smd rect (at 2.2 0.5 90) (size 1.4 0.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 127 "/USBD_P") (pinfunction "HSD1_P"))
    (pad "10" smd rect (at 2.2 1 90) (size 1.4 0.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND") (pinfunction "nOE"))
    (model "${KISYS3DMOD}/Package_SO.3dshapes/MSOP-10_3x3mm_P0.5mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1206_3216Metric" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 151.84 80.48 90)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheet file" "CM4_1.kicad_sch")
    (property "Sheet name" "")
    (attr smd)
    (fp_text reference "C56" (at 0 1.85 90) (layer "B.SilkS"))
    (fp_text value "100uf" (at 0 -1.85 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1.475 0 90) (size 1.15 1.8) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.217391)
      (net 4 "/pcie+3.3v"))
    (pad "2" smd roundrect (at 1.475 0 90) (size 1.15 1.8) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.217391)
      (net 1 "GND"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 114.9 88.41 -90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Field4" "Farnell")
    (property "Field5" "2611911")
    (property "Field6" "RM EMK105 B7104KV-F")
    (property "Field7" "TAIYO YUDEN EUROPE GMBH")
    (property "Field8" "110091611")
    (property "Part Description" "	0.1uF 10% 16V Ceramic Capacitor X7R 0402 (1005 Metric)")
    (property "Sheet file" "CM4_1.kicad_sch")
    (property "Sheet name" "")
    (attr smd)
    (fp_text reference "C53" (at 2.5 -0.1 -90) (layer "B.SilkS"))
    (fp_text value "100n" (at 0 -1.16 -90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 -90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.48 0 270) (size 0.56 0.62) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 8 "/+3.3v"))
    (pad "2" smd roundrect (at 0.48 0 270) (size 0.56 0.62) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 1 "GND"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_DFN_QFN:QFN-36-1EP_6x6mm_P0.5mm_EP3.7x3.7mm" (layer "B.Cu")
    (tedit 5DC5F6A4)
    (at 142.63 97.48 90)
    (descr "QFN, 36 Pin (http://ww1.microchip.com/downloads/en/DeviceDoc/36L_QFN_6x6_with_3_7x3_7_EP_Punch_Dimpled_4E_C04-0241A.pdf), generated with kicad-footprint-generator ipc_noLead_generator.py")
    (tags "QFN NoLead")
    (property "Field4" "Farnell")
    (property "Field5" "2775060")
    (property "Field6" "USB2514B-I/M2")
    (property "Field7" "Microchip")
    (property "Field8" "UICC00931")
    (property "Part Description" "	USB Hub Controller USB Interface 36-SQFN (6x6)")
    (property "Sheet file" "CM4_1.kicad_sch")
    (property "Sheet name" "")
    (attr smd)
    (fp_text reference "U3" (at -4.33 -0.17 180) (layer "B.SilkS"))
    (fp_text value "USB2514B-I/M2" (at 0 -4.3 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "" smd roundrect (at 0 0 90) (size 0.99 0.99) (layers "B.Paste") (roundrect_rratio 0.25))
    (pad "" smd roundrect (at -1.23 1.23 90) (size 0.99 0.99) (layers "B.Paste") (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0 -1.23 90) (size 0.99 0.99) (layers "B.Paste") (roundrect_rratio 0.25))
    (pad "" smd roundrect (at -1.23 -1.23 90) (size 0.99 0.99) (layers "B.Paste") (roundrect_rratio 0.25))
    (pad "" smd roundrect (at -1.23 0 90) (size 0.99 0.99) (layers "B.Paste") (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 1.23 0 90) (size 0.99 0.99) (layers "B.Paste") (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 1.23 1.23 90) (size 0.99 0.99) (layers "B.Paste") (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 1.23 -1.23 90) (size 0.99 0.99) (layers "B.Paste") (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0 1.23 90) (size 0.99 0.99) (layers "B.Paste") (roundrect_rratio 0.25))
    (pad "1" smd roundrect (at -2.9375 2 90) (size 0.825 0.25) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 83 "/HD1_N") (pinfunction "USBDM_DN1/PRT_DIS_M1"))
    (pad "2" smd roundrect (at -2.9375 1.5 90) (size 0.825 0.25) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 84 "/HD1_P") (pinfunction "USBDP_DN1/PRT_DIS_P1"))
    (pad "3" smd roundrect (at -2.9375 1 90) (size 0.825 0.25) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 53 "/HD2_N") (pinfunction "USBDM_DN2/PRT_DIS_M2"))
    (pad "4" smd roundrect (at -2.9375 0.5 90) (size 0.825 0.25) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 54 "/HD2_P") (pinfunction "USBDP_DN2/PRT_DIS_P2"))
    (pad "5" smd roundrect (at -2.9375 0 90) (size 0.825 0.25) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 8 "/+3.3v") (pinfunction "VDDA33"))
    (pad "6" smd roundrect (at -2.9375 -0.5 90) (size 0.825 0.25) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 49 "/HD3_N") (pinfunction "USBDM_DN3/PRT_DIS_M3"))
    (pad "7" smd roundrect (at -2.9375 -1 90) (size 0.825 0.25) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 50 "/HD3_P") (pinfunction "USBDP_DN3/PRT_DIS_P3"))
    (pad "8" smd roundrect (at -2.9375 -1.5 90) (size 0.825 0.25) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 51 "/HD4_N") (pinfunction "USBDM_DN4/PRT_DIS_M4"))
    (pad "9" smd roundrect (at -2.9375 -2 90) (size 0.825 0.25) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 52 "/HD4_P") (pinfunction "USBDP_DN4/PRT_DIS_P4"))
    (pad "10" smd roundrect (at -2 -2.9375 90) (size 0.25 0.825) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 8 "/+3.3v") (pinfunction "VDDA33"))
    (pad "11" smd roundrect (at -1.5 -2.9375 90) (size 0.25 0.825) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 200 "Net-(U3-Pad11)") (pinfunction "TEST"))
    (pad "12" smd roundrect (at -1 -2.9375 90) (size 0.25 0.825) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 199 "/PWR1") (pinfunction "PRTPWR1/BC_EN1"))
    (pad "13" smd roundrect (at -0.5 -2.9375 90) (size 0.25 0.825) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 198 "Net-(U3-Pad13)") (pinfunction "OCS_N1"))
    (pad "14" smd roundrect (at 0 -2.9375 90) (size 0.25 0.825) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 197 "no_connect_207") (pinfunction "CRFILT"))
    (pad "15" smd roundrect (at 0.5 -2.9375 90) (size 0.25 0.825) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 8 "/+3.3v") (pinfunction "VDD33"))
    (pad "16" smd roundrect (at 1 -2.9375 90) (size 0.25 0.825) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 196 "Net-(U3-Pad16)") (pinfunction "PRTPWR2/BC_EN2"))
    (pad "17" smd roundrect (at 1.5 -2.9375 90) (size 0.25 0.825) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 195 "Net-(U3-Pad17)") (pinfunction "OCS_N2"))
    (pad "18" smd roundrect (at 2 -2.9375 90) (size 0.25 0.825) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 194 "Net-(U3-Pad18)") (pinfunction "PRTPWR3/BC_EN3"))
    (pad "19" smd roundrect (at 2.9375 -2 90) (size 0.825 0.25) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 193 "Net-(U3-Pad19)") (pinfunction "OCS_N3"))
    (pad "20" smd roundrect (at 2.9375 -1.5 90) (size 0.825 0.25) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 192 "Net-(U3-Pad20)") (pinfunction "PRTPWR4/BC_EN4"))
    (pad "21" smd roundrect (at 2.9375 -1 90) (size 0.825 0.25) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 191 "Net-(U3-Pad21)") (pinfunction "OCS_N4"))
    (pad "22" smd roundrect (at 2.9375 -0.5 90) (size 0.825 0.25) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 182 "Net-(R6-Pad1)") (pinfunction "SDA/SMBDATA/NON_REM1"))
    (pad "23" smd roundrect (at 2.9375 0 90) (size 0.825 0.25) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 8 "/+3.3v") (pinfunction "VDD33"))
    (pad "24" smd roundrect (at 2.9375 0.5 90) (size 0.825 0.25) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 181 "Net-(R5-Pad1)") (pinfunction "SCL/SMBCLK/CFG_SEL0"))
    (pad "25" smd roundrect (at 2.9375 1 90) (size 0.825 0.25) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 183 "Net-(R7-Pad1)") (pinfunction "HS_IND/CFG_SEL1"))
    (pad "26" smd roundrect (at 2.9375 1.5 90) (size 0.825 0.25) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 160 "/nEXTRST") (pinfunction "RESET_N"))
    (pad "27" smd roundrect (at 2.9375 2 90) (size 0.825 0.25) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 8 "/+3.3v") (pinfunction "VBUS_DET"))
    (pad "28" smd roundrect (at 2 2.9375 90) (size 0.25 0.825) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 179 "Net-(R3-Pad1)") (pinfunction "SUSP_IND/LOCAL_PWR/NON_REM0"))
    (pad "29" smd roundrect (at 1.5 2.9375 90) (size 0.25 0.825) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 8 "/+3.3v") (pinfunction "VDDA33"))
    (pad "30" smd roundrect (at 1 2.9375 90) (size 0.25 0.825) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 190 "/USBH_N") (pinfunction "USBDM_UP"))
    (pad "31" smd roundrect (at 0.5 2.9375 90) (size 0.25 0.825) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 189 "/USBH_P") (pinfunction "USBDP_UP"))
    (pad "32" smd roundrect (at 0 2.9375 90) (size 0.25 0.825) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 7 "Net-(C7-Pad1)") (pinfunction "XTALOUT"))
    (pad "33" smd roundrect (at -0.5 2.9375 90) (size 0.25 0.825) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 6 "Net-(C6-Pad1)") (pinfunction "XTALIN/CLKIN"))
    (pad "34" smd roundrect (at -1 2.9375 90) (size 0.25 0.825) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 188 "no_connect_208") (pinfunction "PLLFILT"))
    (pad "35" smd roundrect (at -1.5 2.9375 90) (size 0.25 0.825) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 180 "Net-(R4-Pad2)") (pinfunction "RBIAS"))
    (pad "36" smd roundrect (at -2 2.9375 90) (size 0.25 0.825) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 8 "/+3.3v") (pinfunction "VDDA33"))
    (pad "37" smd rect (at 0 0 90) (size 3.7 3.7) (layers "B.Cu" "B.Mask")
      (net 1 "GND") (pinfunction "VSS"))
    (model "${KISYS3DMOD}/Package_DFN_QFN.3dshapes/QFN-36-1EP_6x6mm_P0.5mm_EP3.7x3.7mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "B.Cu")
    (tedit 60104F05)
    (at 151.95 85.26 -90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (attr smd)
    (fp_text reference "C57" (at 3.18 -0.02 -90) (layer "B.SilkS"))
    (fp_text value "10u" (at 0 -1.68 -90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 -90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.95 0 270) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 4 "/pcie+3.3v"))
    (pad "2" smd roundrect (at 0.95 0 270) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 1 "GND"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0402_1005Metric" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 137.07 99.45 -90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Field4" "Farnell")
    (property "Field5" "9239278")
    (property "Field6" "RK73G1ETQTP2201D         ")
    (property "Field7" "KOA EUROPE GMBH")
    (property "Field8" "120889581")
    (property "Part Description" "Resistor 2.2K M1005 1% 63mW")
    (property "Sheet file" "CM4_1.kicad_sch")
    (property "Sheet name" "")
    (attr smd)
    (fp_text reference "R49" (at -0.35 -1.44 -90) (layer "B.SilkS"))
    (fp_text value "2.2K 1%" (at 0 -1.17 -90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 -90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.51 0 270) (size 0.54 0.64) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 159 "/USBOTG"))
    (pad "2" smd roundrect (at 0.51 0 270) (size 0.54 0.64) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 1 "GND"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "B.Cu")
    (tedit 600FD01F)
    (at 118.75 123.91)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Field4" "Digikey")
    (property "Field5" "490-14381-1-ND")
    (property "Field6" "GRM21BR71A106KA73L")
    (property "Field7" "Murata")
    (property "Field8" "111893011")
    (property "Part Description" "	10uF 10% 10V Ceramic Capacitor X7R 0805 (2012 Metric)")
    (property "Sheet file" "CM4_1.kicad_sch")
    (property "Sheet name" "")
    (attr smd)
    (fp_text reference "C67" (at 3.14 0) (layer "B.SilkS"))
    (fp_text value "10u" (at 0 -1.68) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.95 0) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 1 "GND"))
    (pad "2" smd roundrect (at 0.95 0) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 3 "/+5v"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "B.Cu")
    (tedit 600FD01F)
    (at 128.48 126.35)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Field4" "Digikey")
    (property "Field5" "490-14381-1-ND")
    (property "Field6" "GRM21BR71A106KA73L")
    (property "Field7" "Murata")
    (property "Field8" "111893011")
    (property "Part Description" "	10uF 10% 10V Ceramic Capacitor X7R 0805 (2012 Metric)")
    (property "Sheet file" "CM4_1.kicad_sch")
    (property "Sheet name" "")
    (attr smd)
    (fp_text reference "C63" (at 3.3 0) (layer "B.SilkS"))
    (fp_text value "10u" (at 0 -1.68) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.95 0) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 1 "GND"))
    (pad "2" smd roundrect (at 0.95 0) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 3 "/+5v"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0402_1005Metric" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 147.36 94.72)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Field4" "Farnell")
    (property "Field5" "1458788")
    (property "Field6" "MCR01MZPF3602")
    (property "Field7" "Rohm")
    (property "Part Description" "Resistor 36K M1005 1% 63mW")
    (property "Sheet file" "CM4_1.kicad_sch")
    (property "Sheet name" "")
    (attr smd)
    (fp_text reference "R3" (at -0.03 -0.99) (layer "B.SilkS"))
    (fp_text value "36K 1%" (at 0 -1.17) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.51 0) (size 0.54 0.64) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 179 "Net-(R3-Pad1)"))
    (pad "2" smd roundrect (at 0.51 0) (size 0.54 0.64) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 1 "GND"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 96.96 96.18 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Field4" "Farnell")
    (property "Field5" "2611911")
    (property "Field6" "RM EMK105 B7104KV-F")
    (property "Field7" "TAIYO YUDEN EUROPE GMBH")
    (property "Field8" "110091611")
    (property "Part Description" "	0.1uF 10% 16V Ceramic Capacitor X7R 0402 (1005 Metric)")
    (property "Sheet file" "CM4_1.kicad_sch")
    (property "Sheet name" "")
    (attr smd)
    (fp_text reference "C51" (at 0 1.16) (layer "B.SilkS"))
    (fp_text value "100n" (at 0 -1.16) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.48 0 180) (size 0.56 0.62) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 8 "/+3.3v"))
    (pad "2" smd roundrect (at 0.48 0 180) (size 0.56 0.62) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 1 "GND"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 113.07 129.6)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Field4" "Farnell")
    (property "Field5" "2611911")
    (property "Field6" "RM EMK105 B7104KV-F")
    (property "Field7" "TAIYO YUDEN EUROPE GMBH")
    (property "Field8" "110091611")
    (property "Part Description" "	0.1uF 10% 16V Ceramic Capacitor X7R 0402 (1005 Metric)")
    (property "Sheet file" "CM4_1.kicad_sch")
    (property "Sheet name" "")
    (attr smd)
    (fp_text reference "C50" (at 2.37 0.03) (layer "B.SilkS"))
    (fp_text value "100n" (at 0 -1.16) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.48 0) (size 0.56 0.62) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 8 "/+3.3v"))
    (pad "2" smd roundrect (at 0.48 0) (size 0.56 0.62) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 1 "GND"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "B.Cu")
    (tedit 600FD01F)
    (at 128.48 124.04)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Field4" "Digikey")
    (property "Field5" "490-14381-1-ND")
    (property "Field6" "GRM21BR71A106KA73L")
    (property "Field7" "Murata")
    (property "Field8" "111893011")
    (property "Part Description" "	10uF 10% 10V Ceramic Capacitor X7R 0805 (2012 Metric)")
    (property "Sheet file" "CM4_1.kicad_sch")
    (property "Sheet name" "")
    (attr smd)
    (fp_text reference "C64" (at 3.26 0) (layer "B.SilkS"))
    (fp_text value "10u" (at 0 -1.68) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.95 0) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 1 "GND"))
    (pad "2" smd roundrect (at 0.95 0) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 3 "/+5v"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "B.Cu")
    (tedit 600FD01F)
    (at 147.32 126.43)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Field4" "Digikey")
    (property "Field5" "490-14381-1-ND")
    (property "Field6" "GRM21BR71A106KA73L")
    (property "Field7" "Murata")
    (property "Field8" "111893011")
    (property "Part Description" "	10uF 10% 10V Ceramic Capacitor X7R 0805 (2012 Metric)")
    (property "Sheet file" "CM4_1.kicad_sch")
    (property "Sheet name" "")
    (attr smd)
    (fp_text reference "C57" (at 3.02 0) (layer "B.SilkS"))
    (fp_text value "10u" (at 0 -1.68) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.95 0) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 1 "GND"))
    (pad "2" smd roundrect (at 0.95 0) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 3 "/+5v"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 118.76 121.52 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheet file" "CM4_1.kicad_sch")
    (property "Sheet name" "")
    (attr smd)
    (fp_text reference "C4" (at -2.72 -0.28) (layer "B.SilkS"))
    (fp_text value "22uf" (at 0 -1.68) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.95 0 180) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 3 "/+5v"))
    (pad "2" smd roundrect (at 0.95 0 180) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 1 "GND"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "B.Cu")
    (tedit 600FD01F)
    (at 137.78 126.33)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Field4" "Digikey")
    (property "Field5" "490-14381-1-ND")
    (property "Field6" "GRM21BR71A106KA73L")
    (property "Field7" "Murata")
    (property "Field8" "111893011")
    (property "Part Description" "	10uF 10% 10V Ceramic Capacitor X7R 0805 (2012 Metric)")
    (property "Sheet file" "CM4_1.kicad_sch")
    (property "Sheet name" "")
    (attr smd)
    (fp_text reference "C60" (at 3.13 0.02) (layer "B.SilkS"))
    (fp_text value "10u" (at 0 -1.68) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.95 0) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 1 "GND"))
    (pad "2" smd roundrect (at 0.95 0) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 3 "/+5v"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0402_1005Metric" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 150.38 84.84 -90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheet file" "CM4_1.kicad_sch")
    (property "Sheet name" "")
    (attr smd)
    (fp_text reference "R2" (at -1.94 0.24 90) (layer "B.SilkS"))
    (fp_text value "4.7k" (at 0 -1.17 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.51 0 270) (size 0.54 0.64) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 4 "/pcie+3.3v"))
    (pad "2" smd roundrect (at 0.51 0 270) (size 0.54 0.64) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 178 "Net-(R1-Pad2)"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 149.29 95.26)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Field4" "Digikey")
    (property "Field5" "490-17672-1-ND")
    (property "Field6" "GJM1555C1H270JB01D")
    (property "Field7" "Murata")
    (property "Field8" "UCAP00738 ")
    (property "Part Description" "	27pF 5% 50V Ceramic Capacitor C0G, NP0 0402 (1005 Metric)")
    (property "Sheet file" "CM4_1.kicad_sch")
    (property "Sheet name" "")
    (attr smd)
    (fp_text reference "C7" (at 0.03 -1.03) (layer "B.SilkS"))
    (fp_text value "27pF" (at 0 -1.16) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.48 0) (size 0.56 0.62) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 7 "Net-(C7-Pad1)"))
    (pad "2" smd roundrect (at 0.48 0) (size 0.56 0.62) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 1 "GND"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1206_3216Metric" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 145.33 62.71)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheet file" "CM4_1.kicad_sch")
    (property "Sheet name" "")
    (attr smd)
    (fp_text reference "C58" (at 0 1.85) (layer "B.SilkS"))
    (fp_text value "100uf" (at 0 -1.85) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at -0.072 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1.475 0) (size 1.15 1.8) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.217391)
      (net 4 "/pcie+3.3v"))
    (pad "2" smd roundrect (at 1.475 0) (size 1.15 1.8) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.217391)
      (net 1 "GND"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-353_SC-70-5" (layer "B.Cu")
    (tedit 5A02FF57)
    (at 124.88 59.66 -90)
    (descr "SOT-353, SC-70-5")
    (tags "SOT-353 SC-70-5")
    (property "Field4" "Farnell")
    (property "Field5" "2425492")
    (property "Field6" "74LVC1G07SE-7")
    (property "Field7" "Diodes")
    (property "Part Description" "Buffer, Non-Inverting 1 Element 1 Bit per Element Open Drain Output SOT-353")
    (property "Sheet file" "CM4_1.kicad_sch")
    (property "Sheet name" "")
    (attr smd)
    (fp_text reference "U15" (at 0 2 90) (layer "B.SilkS"))
    (fp_text value "74LVC1G07SE-7" (at 0 -2 -90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 180) (layer "B.Fab"))
    (pad "1" smd rect (at -0.95 0.65 270) (size 0.65 0.4) (layers "B.Cu" "B.Paste" "B.Mask"))
    (pad "2" smd rect (at -0.95 0 270) (size 0.65 0.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 163 "/RUN_PG"))
    (pad "3" smd rect (at -0.95 -0.65 270) (size 0.65 0.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND") (pinfunction "GND"))
    (pad "4" smd rect (at 0.95 -0.65 270) (size 0.65 0.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 93 "Net-(J14-Pad13)"))
    (pad "5" smd rect (at 0.95 0.65 270) (size 0.65 0.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 3 "/+5v") (pinfunction "VCC"))
    (model "${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-353_SC-70-5.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0402_1005Metric" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 135.99 99.45 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Field4" "Farnell")
    (property "Field5" "9239278")
    (property "Field6" "RK73G1ETQTP2201D         ")
    (property "Field7" "KOA EUROPE GMBH")
    (property "Field8" "120889581")
    (property "Part Description" "Resistor 2.2K M1005 1% 63mW")
    (property "Sheet file" "CM4_1.kicad_sch")
    (property "Sheet name" "")
    (attr smd)
    (fp_text reference "R50" (at 0.57 -1.92) (layer "B.SilkS"))
    (fp_text value "2.2K 1%" (at 0 -1.17 270) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 270) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.51 0 90) (size 0.54 0.64) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 129 "/VBUS_OTG"))
    (pad "2" smd roundrect (at 0.51 0 90) (size 0.54 0.64) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 159 "/USBOTG"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-353_SC-70-5" (layer "B.Cu")
    (tedit 5A02FF57)
    (at 107.76 122.98 90)
    (descr "SOT-353, SC-70-5")
    (tags "SOT-353 SC-70-5")
    (property "Field4" "Farnell")
    (property "Field5" "2425492")
    (property "Field6" "74LVC1G07SE-7")
    (property "Field7" "Diodes")
    (property "Part Description" "Buffer, Non-Inverting 1 Element 1 Bit per Element Open Drain Output SOT-353")
    (property "Sheet file" "CM4_1.kicad_sch")
    (property "Sheet name" "")
    (attr smd)
    (fp_text reference "U16" (at 0 2 270) (layer "B.SilkS"))
    (fp_text value "74LVC1G07SE-7" (at 0 -2 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd rect (at -0.95 0.65 90) (size 0.65 0.4) (layers "B.Cu" "B.Paste" "B.Mask"))
    (pad "2" smd rect (at -0.95 0 90) (size 0.65 0.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 162 "/nPWR_LED"))
    (pad "3" smd rect (at -0.95 -0.65 90) (size 0.65 0.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND") (pinfunction "GND"))
    (pad "4" smd rect (at 0.95 -0.65 90) (size 0.65 0.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 184 "Net-(R48-Pad2)"))
    (pad "5" smd rect (at 0.95 0.65 90) (size 0.65 0.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 8 "/+3.3v") (pinfunction "VCC"))
    (model "${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-353_SC-70-5.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 137.56 101.17 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Field4" "Farnell")
    (property "Field5" "2611911")
    (property "Field6" "RM EMK105 B7104KV-F")
    (property "Field7" "TAIYO YUDEN EUROPE GMBH")
    (property "Field8" "110091611")
    (property "Part Description" "	0.1uF 10% 16V Ceramic Capacitor X7R 0402 (1005 Metric)")
    (property "Sheet file" "CM4_1.kicad_sch")
    (property "Sheet name" "")
    (attr smd)
    (fp_text reference "C54" (at 0.01 -1.24 180) (layer "B.SilkS"))
    (fp_text value "100n" (at 0 -1.16 180) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 180) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.48 0 180) (size 0.56 0.62) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 8 "/+3.3v"))
    (pad "2" smd roundrect (at 0.48 0 180) (size 0.56 0.62) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 1 "GND"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "CM4IO:SD_slot" (layer "B.Cu")
    (tedit 60117B21)
    (at 107.47 87.41 90)
    (property "Field4" "Farnell")
    (property "Field5" "2358234")
    (property "Field6" "503398-1892")
    (property "Field7" "Molex")
    (property "Field8" "UCON00512")
    (property "Part Description" "9 (8 + 1) Position Card Connector microSD™ Surface Mount, Right Angle Gold")
    (property "Sheet file" "CM4_1.kicad_sch")
    (property "Sheet name" "")
    (fp_text reference "J13" (at 0 0.5 90 unlocked) (layer "User.5"))
    (fp_text value "Micro_SD_Card_Det" (at 0 -1 90 unlocked) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -2.5 90 unlocked) (layer "B.Fab"))
    (pad "" np_thru_hole circle (at 4.05 -8.2 90) (size 0.95 0.95) (drill 0.95) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at -2.75 -8.2 90) (size 0.95 0.95) (drill 0.95) (layers F&B.Cu *.Mask))
    (pad "1" smd rect (at 3.2 3.22 90) (size 0.7 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 91 "/SD_DAT2") (pinfunction "DAT2"))
    (pad "2" smd rect (at 2.1 3.22 90) (size 0.7 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 90 "/SD_DAT3") (pinfunction "DAT3/CD"))
    (pad "3" smd rect (at 1 3.22 90) (size 0.7 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 89 "/SD_CMD") (pinfunction "CMD"))
    (pad "4" smd rect (at -0.1 3.22 90) (size 0.7 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 8 "/+3.3v") (pinfunction "VDD"))
    (pad "5" smd rect (at -1.2 3.22 90) (size 0.7 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 88 "/SD_CLK") (pinfunction "CLK"))
    (pad "6" smd rect (at -2.3 3.22 90) (size 0.7 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND") (pinfunction "VSS"))
    (pad "7" smd rect (at -3.4 3.22 90) (size 0.7 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 87 "/SD_DAT0") (pinfunction "DAT0"))
    (pad "8" smd rect (at -4.5 3.22 90) (size 0.7 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 86 "/SD_DAT1") (pinfunction "DAT1"))
    (pad "9" smd rect (at -5.6 3.22 90) (size 0.7 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 85 "Net-(J13-Pad9)") (pinfunction "DET_B"))
    (pad "11" smd rect (at 9.2 -7.78 90) (size 1.1 2.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND") (pinfunction "SHIELD"))
    (pad "11" smd rect (at -6.98 -7.78 90) (size 1.1 2.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND") (pinfunction "SHIELD"))
    (pad "11" smd rect (at -6.98 1.22 90) (size 1.1 2.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND") (pinfunction "SHIELD"))
    (pad "11" smd rect (at 9.2 1.22 90) (size 1.1 2.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND") (pinfunction "SHIELD"))
  )
  (footprint "Connector_FFC-FPC:Hirose_FH12-22S-0.5SH_1x22-1MP_P0.50mm_Horizontal" (layer "B.Cu")
    (tedit 5D24667B)
    (at 104.18 98.35 180)
    (descr "Hirose FH12, FFC/FPC connector, FH12-22S-0.5SH, 22 Pins per row (https://www.hirose.com/product/en/products/FH12/FH12-24S-0.5SH(55)/), generated with kicad-footprint-generator")
    (tags "connector Hirose FH12 horizontal")
    (property "Field4" "Mouser")
    (property "Field5" "798-FH12-22S-0.5SH55")
    (property "Field6" "FH12-22S-0.5SH55")
    (property "Field7" "Hirose")
    (property "Part Description" "22 Position FFC, FPC Connector Contacts, Bottom 0.020\" (0.50mm) Surface Mount, Right Angle")
    (property "Sheet file" "CM4_1.kicad_sch")
    (property "Sheet name" "")
    (attr smd)
    (fp_text reference "J2" (at 0 3.7) (layer "B.SilkS"))
    (fp_text value "Conn_01x22_Female" (at 0 -5.6) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -3.7) (layer "B.Fab"))
    (pad "1" smd rect (at -5.25 1.85 180) (size 0.3 1.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND") (pinfunction "Pin_1"))
    (pad "2" smd rect (at -4.75 1.85 180) (size 0.3 1.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 27 "/DSI1_D0_N") (pinfunction "Pin_2"))
    (pad "3" smd rect (at -4.25 1.85 180) (size 0.3 1.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 26 "/DSI1_D0_P") (pinfunction "Pin_3"))
    (pad "4" smd rect (at -3.75 1.85 180) (size 0.3 1.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND") (pinfunction "Pin_4"))
    (pad "5" smd rect (at -3.25 1.85 180) (size 0.3 1.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 25 "/DSI1_D1_N") (pinfunction "Pin_5"))
    (pad "6" smd rect (at -2.75 1.85 180) (size 0.3 1.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 24 "/DSI1_D1_P") (pinfunction "Pin_6"))
    (pad "7" smd rect (at -2.25 1.85 180) (size 0.3 1.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND") (pinfunction "Pin_7"))
    (pad "8" smd rect (at -1.75 1.85 180) (size 0.3 1.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 23 "/DSI1_C_N") (pinfunction "Pin_8"))
    (pad "9" smd rect (at -1.25 1.85 180) (size 0.3 1.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 22 "/DSI1_C_P") (pinfunction "Pin_9"))
    (pad "10" smd rect (at -0.75 1.85 180) (size 0.3 1.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND") (pinfunction "Pin_10"))
    (pad "11" smd rect (at -0.25 1.85 180) (size 0.3 1.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 21 "/DSI1_D2_N") (pinfunction "Pin_11"))
    (pad "12" smd rect (at 0.25 1.85 180) (size 0.3 1.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 20 "/DSI1_D2_P") (pinfunction "Pin_12"))
    (pad "13" smd rect (at 0.75 1.85 180) (size 0.3 1.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND") (pinfunction "Pin_13"))
    (pad "14" smd rect (at 1.25 1.85 180) (size 0.3 1.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 19 "/DSI1_D3_N") (pinfunction "Pin_14"))
    (pad "15" smd rect (at 1.75 1.85 180) (size 0.3 1.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 18 "/DSI1_D3_P") (pinfunction "Pin_15"))
    (pad "16" smd rect (at 2.25 1.85 180) (size 0.3 1.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND") (pinfunction "Pin_16"))
    (pad "17" smd rect (at 2.75 1.85 180) (size 0.3 1.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 17 "no_connect_182") (pinfunction "Pin_17"))
    (pad "18" smd rect (at 3.25 1.85 180) (size 0.3 1.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 16 "no_connect_183") (pinfunction "Pin_18"))
    (pad "19" smd rect (at 3.75 1.85 180) (size 0.3 1.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND") (pinfunction "Pin_19"))
    (pad "20" smd rect (at 4.25 1.85 180) (size 0.3 1.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "/SCL0") (pinfunction "Pin_20"))
    (pad "21" smd rect (at 4.75 1.85 180) (size 0.3 1.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 14 "/SDA0") (pinfunction "Pin_21"))
    (pad "22" smd rect (at 5.25 1.85 180) (size 0.3 1.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 8 "/+3.3v") (pinfunction "Pin_22"))
    (pad "MP" smd rect (at 7.15 -1.4 180) (size 1.8 2.2) (layers "B.Cu" "B.Paste" "B.Mask"))
    (pad "MP" smd rect (at -7.15 -1.4 180) (size 1.8 2.2) (layers "B.Cu" "B.Paste" "B.Mask"))
    (model "${KISYS3DMOD}/Connector_FFC-FPC.3dshapes/Hirose_FH12-22S-0.5SH_1x22-1MP_P0.50mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0402_1005Metric" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 146.9 87.25)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheet file" "CM4_1.kicad_sch")
    (property "Sheet name" "")
    (attr smd)
    (fp_text reference "R1" (at 0 1.17) (layer "B.SilkS"))
    (fp_text value "3k" (at 0 -1.17) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.51 0) (size 0.54 0.64) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 1 "GND"))
    (pad "2" smd roundrect (at 0.51 0) (size 0.54 0.64) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 178 "Net-(R1-Pad2)"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0402_1005Metric" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 112.6 92.5 -90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Field4" "Farnell")
    (property "Field5" "9239235")
    (property "Field6" "RK73H1ETTP1001F")
    (property "Field7" "KOA EUROPE GMBH")
    (property "Field8" "125049511")
    (property "Part Description" "Resistor 1K M1005 1% 63mW")
    (property "Sheet file" "CM4_1.kicad_sch")
    (property "Sheet name" "")
    (attr smd)
    (fp_text reference "R44" (at -0.07 -1.09 -90) (layer "B.SilkS"))
    (fp_text value "nf" (at 0 -1.17 -90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 -90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.51 0 270) (size 0.54 0.64) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 167 "/SD_DET"))
    (pad "2" smd roundrect (at 0.51 0 270) (size 0.54 0.64) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 85 "Net-(J13-Pad9)"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 112.92 88.46 -90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Field4" "Digikey")
    (property "Field5" "490-14381-1-ND")
    (property "Field6" "GRM21BR71A106KA73L")
    (property "Field7" "Murata")
    (property "Field8" "111893011")
    (property "Part Description" "	10uF 10% 10V Ceramic Capacitor X7R 0805 (2012 Metric)")
    (property "Sheet file" "CM4_1.kicad_sch")
    (property "Sheet name" "")
    (attr smd)
    (fp_text reference "C46" (at -3.11 -0.04 90) (layer "B.SilkS"))
    (fp_text value "10u" (at 0 -1.68 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.95 0 270) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 8 "/+3.3v"))
    (pad "2" smd roundrect (at 0.95 0 270) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 1 "GND"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0402_1005Metric" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 143.24 92.34 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Field4" "Farnell")
    (property "Field5" "1458788")
    (property "Field6" "MCR01MZPF3602")
    (property "Field7" "Rohm")
    (property "Part Description" "Resistor 36K M1005 1% 63mW")
    (property "Sheet file" "CM4_1.kicad_sch")
    (property "Sheet name" "")
    (attr smd)
    (fp_text reference "R5" (at 1.88 0.08 90) (layer "B.SilkS"))
    (fp_text value "36K 1%" (at 0 -1.17 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.51 0 90) (size 0.54 0.64) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 181 "Net-(R5-Pad1)"))
    (pad "2" smd roundrect (at 0.51 0 90) (size 0.54 0.64) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 1 "GND"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 113.44 127.96)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Field4" "Digikey")
    (property "Field5" "490-14381-1-ND")
    (property "Field6" "GRM21BR71A106KA73L")
    (property "Field7" "Murata")
    (property "Field8" "111893011")
    (property "Part Description" "	10uF 10% 10V Ceramic Capacitor X7R 0805 (2012 Metric)")
    (property "Sheet file" "CM4_1.kicad_sch")
    (property "Sheet name" "")
    (attr smd)
    (fp_text reference "C47" (at 0.93 -1.69) (layer "B.SilkS"))
    (fp_text value "10u" (at 0 -1.68) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.95 0) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 8 "/+3.3v"))
    (pad "2" smd roundrect (at 0.95 0) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 1 "GND"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 153.14 52.81) (end 153.14 130.81) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 96.81 70.68) (end 95.14 70.68) (layer "Edge.Cuts") (width 0.05))
  (gr_line (start 96.81 52.81) (end 153.14 52.81) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 95.14 130.81) (end 95.14 70.68) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 153.14 130.81) (end 95.14 130.81) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 96.81 70.68) (end 96.81 52.81) (layer "Edge.Cuts") (width 0.05))
  (gr_text "CSI" (at 121.65 104.8) (layer "B.SilkS"))
  (gr_text "DSI" (at 104.394 104.902) (layer "B.SilkS"))
  (gr_text "C57" (at 158.53 80.44) (layer "B.Fab"))
  (zone (net 1) (net_name "GND") (layer "F.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 153.139135 52.814502)
        (xy 153.139135 130.804502)
        (xy 95.129135 130.814502)
        (xy 95.129135 70.674502)
        (xy 96.789135 70.674502)
        (xy 96.799135 52.804502)
      )
    )
  )
  (zone (net 1) (net_name "GND") (layer "B.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 153.15 52.82)
        (xy 153.15 130.81)
        (xy 95.14 130.82)
        (xy 95.14 70.68)
        (xy 96.8 70.68)
        (xy 96.81 52.81)
      )
    )
  )
)
