(kicad_sch (version 20201015) (generator eeschema)
  (paper "A3")
  (title_block
    (title "Compute Module 4-1")
    (rev "0.1")
  )
  (lib_symbols
    (symbol "CM4IO:74LVC1G07_copy" (in_bom yes) (on_board yes)
      (property "Reference" "U" (id 0) (at -2.54 3.81 0))
      (property "Value" "74LVC1G07_copy" (id 1) (at 0 -3.81 0))
      (property "Footprint" "Package_TO_SOT_SMD:SOT-353_SC-70-5" (id 2) (at 0 0 0))
      (property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf" (id 3) (at 0 0 0))
      (property "ki_keywords" "Single Gate Buff LVC CMOS Open Drain" (id 4) (at 0 0 0))
      (property "ki_description" "Single Buffer Gate w/ Open Drain, Low-Voltage CMOS" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "SOT* SG-*" (id 6) (at 0 0 0))
      (symbol "74LVC1G07_copy_0_1"
        (polyline
          (pts
            (xy -2.54 -0.635)
            (xy -1.27 -0.635)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -3.81 2.54)
            (xy -3.81 -2.54)
            (xy 2.54 0)
            (xy -3.81 2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.905 0.635)
            (xy -2.54 0)
            (xy -1.905 -0.635)
            (xy -1.27 0)
            (xy -1.905 0.635)
          )
          (fill (type none))
        )
      )
      (symbol "74LVC1G07_copy_1_1"
        (pin input line (at -7.62 0 0) (length 3.81)
          (name "~")
          (number "2")
        )
        (pin power_in line (at 0 -2.54 270) (length 0)
          (name "GND")
          (number "3")
        )
        (pin open_collector line (at 6.35 0 180) (length 3.81)
          (name "~")
          (number "4")
        )
        (pin power_in line (at 0 2.54 90) (length 0)
          (name "VCC")
          (number "5")
        )
      )
    )
    (symbol "CM4IO:ComputeModule4-CM4" (in_bom yes) (on_board yes)
      (property "Reference" "Module" (id 0) (at 113.03 -68.58 0))
      (property "Value" "ComputeModule4-CM4" (id 1) (at 140.97 2.54 0))
      (property "Footprint" "CM4IO:Raspberry-Pi-4-Compute-Module" (id 2) (at 142.24 -26.67 0))
      (property "Datasheet" "" (id 3) (at 142.24 -26.67 0))
      (property "Field4" "Hirose" (id 4) (at 0 0 0))
      (property "Field5" "2x DF40C-100DS-0.4V" (id 5) (at 0 -2.54 0))
      (property "ki_locked" "" (id 6) (at 0 0 0))
      (symbol "ComputeModule4-CM4_1_0"
        (text "GPIO" (at 0 6.35 0))
      )
      (symbol "ComputeModule4-CM4_1_1"
        (text "600mA Max" (at -8.89 -53.34 0))
        (text "600mA Max" (at -8.89 -48.26 0))
        (text "NB SD signals are only available" (at -1.27 -27.94 0))
        (text "on modules without eMMC" (at -1.27 -30.48 0))
        (rectangle (start -30.48 -71.12) (end 25.4 58.42)
          (fill (type none))
        )
        (pin power_in line (at 27.94 55.88 180) (length 2.54)
          (name "GND")
          (number "1")
        )
        (pin passive line (at -33.02 45.72 0) (length 2.54)
          (name "Ethernet_Pair0_N")
          (number "10")
        )
        (pin output line (at -33.02 -68.58 0) (length 2.54)
          (name "nEXTRST")
          (number "100")
        )
        (pin passive line (at 27.94 43.18 180) (length 2.54)
          (name "Ethernet_Pair2_P")
          (number "11")
        )
        (pin passive line (at -33.02 43.18 0) (length 2.54)
          (name "Ethernet_Pair0_P")
          (number "12")
        )
        (pin power_in line (at 27.94 40.64 180) (length 2.54)
          (name "GND")
          (number "13")
        )
        (pin power_in line (at -33.02 40.64 0) (length 2.54)
          (name "GND")
          (number "14")
        )
        (pin output line (at 27.94 38.1 180) (length 2.54)
          (name "Ethernet_nLED3(3.3v)")
          (number "15")
        )
        (pin input line (at -33.02 38.1 0) (length 2.54)
          (name "Ethernet_SYNC_IN(1.8v)")
          (number "16")
        )
        (pin output line (at 27.94 35.56 180) (length 2.54)
          (name "Ethernet_nLED2(3.3v)")
          (number "17")
        )
        (pin input line (at -33.02 35.56 0) (length 2.54)
          (name "Ethernet_SYNC_OUT(1.8v)")
          (number "18")
        )
        (pin output line (at 27.94 33.02 180) (length 2.54)
          (name "Ethernet_nLED1(3.3v)")
          (number "19")
        )
        (pin power_in line (at -33.02 55.88 0) (length 2.54)
          (name "GND")
          (number "2")
        )
        (pin passive line (at -33.02 33.02 0) (length 2.54)
          (name "EEPROM_nWP")
          (number "20")
        )
        (pin open_collector line (at 27.94 30.48 180) (length 2.54)
          (name "PI_nLED_Activity")
          (number "21")
        )
        (pin power_in line (at -33.02 30.48 0) (length 2.54)
          (name "GND")
          (number "22")
        )
        (pin power_in line (at 27.94 27.94 180) (length 2.54)
          (name "GND")
          (number "23")
        )
        (pin passive line (at -33.02 27.94 0) (length 2.54)
          (name "GPIO26")
          (number "24")
        )
        (pin passive line (at 27.94 25.4 180) (length 2.54)
          (name "GPIO21")
          (number "25")
        )
        (pin passive line (at -33.02 25.4 0) (length 2.54)
          (name "GPIO19")
          (number "26")
        )
        (pin passive line (at 27.94 22.86 180) (length 2.54)
          (name "GPIO20")
          (number "27")
        )
        (pin passive line (at -33.02 22.86 0) (length 2.54)
          (name "GPIO13")
          (number "28")
        )
        (pin passive line (at 27.94 20.32 180) (length 2.54)
          (name "GPIO16")
          (number "29")
        )
        (pin passive line (at 27.94 53.34 180) (length 2.54)
          (name "Ethernet_Pair3_P")
          (number "3")
        )
        (pin passive line (at -33.02 20.32 0) (length 2.54)
          (name "GPIO6")
          (number "30")
        )
        (pin passive line (at 27.94 17.78 180) (length 2.54)
          (name "GPIO12")
          (number "31")
        )
        (pin power_in line (at -33.02 17.78 0) (length 2.54)
          (name "GND")
          (number "32")
        )
        (pin power_in line (at 27.94 15.24 180) (length 2.54)
          (name "GND")
          (number "33")
        )
        (pin passive line (at -33.02 15.24 0) (length 2.54)
          (name "GPIO5")
          (number "34")
        )
        (pin passive line (at 27.94 12.7 180) (length 2.54)
          (name "ID_SC")
          (number "35")
        )
        (pin passive line (at -33.02 12.7 0) (length 2.54)
          (name "ID_SD")
          (number "36")
        )
        (pin passive line (at 27.94 10.16 180) (length 2.54)
          (name "GPIO7")
          (number "37")
        )
        (pin passive line (at -33.02 10.16 0) (length 2.54)
          (name "GPIO11")
          (number "38")
        )
        (pin passive line (at 27.94 7.62 180) (length 2.54)
          (name "GPIO8")
          (number "39")
        )
        (pin passive line (at -33.02 53.34 0) (length 2.54)
          (name "Ethernet_Pair1_P")
          (number "4")
        )
        (pin passive line (at -33.02 7.62 0) (length 2.54)
          (name "GPIO9")
          (number "40")
        )
        (pin passive line (at 27.94 5.08 180) (length 2.54)
          (name "GPIO25")
          (number "41")
        )
        (pin power_in line (at -33.02 5.08 0) (length 2.54)
          (name "GND")
          (number "42")
        )
        (pin power_in line (at 27.94 2.54 180) (length 2.54)
          (name "GND")
          (number "43")
        )
        (pin passive line (at -33.02 2.54 0) (length 2.54)
          (name "GPIO10")
          (number "44")
        )
        (pin passive line (at 27.94 0 180) (length 2.54)
          (name "GPIO24")
          (number "45")
        )
        (pin passive line (at -33.02 0 0) (length 2.54)
          (name "GPIO22")
          (number "46")
        )
        (pin passive line (at 27.94 -2.54 180) (length 2.54)
          (name "GPIO23")
          (number "47")
        )
        (pin passive line (at -33.02 -2.54 0) (length 2.54)
          (name "GPIO27")
          (number "48")
        )
        (pin passive line (at 27.94 -5.08 180) (length 2.54)
          (name "GPIO18")
          (number "49")
        )
        (pin passive line (at 27.94 50.8 180) (length 2.54)
          (name "Ethernet_Pair3_N")
          (number "5")
        )
        (pin passive line (at -33.02 -5.08 0) (length 2.54)
          (name "GPIO17")
          (number "50")
        )
        (pin passive line (at 27.94 -7.62 180) (length 2.54)
          (name "GPIO15")
          (number "51")
        )
        (pin power_in line (at -33.02 -7.62 0) (length 2.54)
          (name "GND")
          (number "52")
        )
        (pin power_in line (at 27.94 -10.16 180) (length 2.54)
          (name "GND")
          (number "53")
        )
        (pin passive line (at -33.02 -10.16 0) (length 2.54)
          (name "GPIO4")
          (number "54")
        )
        (pin passive line (at 27.94 -12.7 180) (length 2.54)
          (name "GPIO14")
          (number "55")
        )
        (pin passive line (at -33.02 -12.7 0) (length 2.54)
          (name "GPIO3")
          (number "56")
        )
        (pin passive line (at 27.94 -15.24 180) (length 2.54)
          (name "SD_CLK")
          (number "57")
        )
        (pin passive line (at -33.02 -15.24 0) (length 2.54)
          (name "GPIO2")
          (number "58")
        )
        (pin power_in line (at 27.94 -17.78 180) (length 2.54)
          (name "GND")
          (number "59")
        )
        (pin passive line (at -33.02 50.8 0) (length 2.54)
          (name "Ethernet_Pair1_N")
          (number "6")
        )
        (pin power_in line (at -33.02 -17.78 0) (length 2.54)
          (name "GND")
          (number "60")
        )
        (pin passive line (at 27.94 -20.32 180) (length 2.54)
          (name "SD_DAT3")
          (number "61")
        )
        (pin passive line (at -33.02 -20.32 0) (length 2.54)
          (name "SD_CMD")
          (number "62")
        )
        (pin passive line (at 27.94 -22.86 180) (length 2.54)
          (name "SD_DAT0")
          (number "63")
        )
        (pin passive line (at -33.02 -22.86 0) (length 2.54)
          (name "SD_DAT5")
          (number "64")
        )
        (pin power_in line (at 27.94 -25.4 180) (length 2.54)
          (name "GND")
          (number "65")
        )
        (pin power_in line (at -33.02 -25.4 0) (length 2.54)
          (name "GND")
          (number "66")
        )
        (pin passive line (at 27.94 -27.94 180) (length 2.54)
          (name "SD_DAT1")
          (number "67")
        )
        (pin passive line (at -33.02 -27.94 0) (length 2.54)
          (name "SD_DAT4")
          (number "68")
        )
        (pin passive line (at 27.94 -30.48 180) (length 2.54)
          (name "SD_DAT2")
          (number "69")
        )
        (pin power_in line (at 27.94 48.26 180) (length 2.54)
          (name "GND")
          (number "7")
        )
        (pin passive line (at -33.02 -30.48 0) (length 2.54)
          (name "SD_DAT7")
          (number "70")
        )
        (pin power_in line (at 27.94 -33.02 180) (length 2.54)
          (name "GND")
          (number "71")
        )
        (pin passive line (at -33.02 -33.02 0) (length 2.54)
          (name "SD_DAT6")
          (number "72")
        )
        (pin input line (at 27.94 -35.56 180) (length 2.54)
          (name "SD_VDD_Override")
          (number "73")
        )
        (pin power_in line (at -33.02 -35.56 0) (length 2.54)
          (name "GND")
          (number "74")
        )
        (pin output line (at 27.94 -38.1 180) (length 2.54)
          (name "SD_PWR_ON")
          (number "75")
        )
        (pin passive line (at -33.02 -38.1 0) (length 2.54)
          (name "Reserved")
          (number "76")
        )
        (pin power_in line (at 27.94 -40.64 180) (length 2.54)
          (name "+5v_(Input)")
          (number "77")
        )
        (pin power_in line (at -33.02 -40.64 0) (length 2.54)
          (name "GPIO_VREF(1.8v/3.3v_Input)")
          (number "78")
        )
        (pin power_in line (at 27.94 -43.18 180) (length 2.54)
          (name "+5v_(Input)")
          (number "79")
        )
        (pin power_in line (at -33.02 48.26 0) (length 2.54)
          (name "GND")
          (number "8")
        )
        (pin passive line (at -33.02 -43.18 0) (length 2.54)
          (name "SCL0")
          (number "80")
        )
        (pin power_in line (at 27.94 -45.72 180) (length 2.54)
          (name "+5v_(Input)")
          (number "81")
        )
        (pin passive line (at -33.02 -45.72 0) (length 2.54)
          (name "SDA0")
          (number "82")
        )
        (pin power_in line (at 27.94 -48.26 180) (length 2.54)
          (name "+5v_(Input)")
          (number "83")
        )
        (pin power_out line (at -33.02 -48.26 0) (length 2.54)
          (name "+3.3v_(Output)")
          (number "84")
        )
        (pin power_in line (at 27.94 -50.8 180) (length 2.54)
          (name "+5v_(Input)")
          (number "85")
        )
        (pin power_out line (at -33.02 -50.8 0) (length 2.54)
          (name "+3.3v_(Output)")
          (number "86")
        )
        (pin power_in line (at 27.94 -53.34 180) (length 2.54)
          (name "+5v_(Input)")
          (number "87")
        )
        (pin power_out line (at -33.02 -53.34 0) (length 2.54)
          (name "+1.8v_(Output)")
          (number "88")
        )
        (pin input line (at 27.94 -55.88 180) (length 2.54)
          (name "WL_nDisable")
          (number "89")
        )
        (pin passive line (at 27.94 45.72 180) (length 2.54)
          (name "Ethernet_Pair2_N")
          (number "9")
        )
        (pin power_out line (at -33.02 -55.88 0) (length 2.54)
          (name "+1.8v_(Output)")
          (number "90")
        )
        (pin input line (at 27.94 -58.42 180) (length 2.54)
          (name "BT_nDisable")
          (number "91")
        )
        (pin passive line (at -33.02 -58.42 0) (length 2.54)
          (name "RUN_PG")
          (number "92")
        )
        (pin input line (at 27.94 -60.96 180) (length 2.54)
          (name "nRPIBOOT")
          (number "93")
        )
        (pin passive line (at -33.02 -60.96 0) (length 2.54)
          (name "AnalogIP1")
          (number "94")
        )
        (pin output line (at 27.94 -63.5 180) (length 2.54)
          (name "nPI_LED_PWR")
          (number "95")
        )
        (pin passive line (at -33.02 -63.5 0) (length 2.54)
          (name "AnalogIP0")
          (number "96")
        )
        (pin passive line (at 27.94 -66.04 180) (length 2.54)
          (name "Camera_GPIO")
          (number "97")
        )
        (pin power_in line (at -33.02 -66.04 0) (length 2.54)
          (name "GND")
          (number "98")
        )
        (pin input line (at 27.94 -68.58 180) (length 2.54)
          (name "Global_EN")
          (number "99")
        )
      )
      (symbol "ComputeModule4-CM4_2_1"
        (text "High Speed Serial" (at 140.97 0 0))
        (rectangle (start 114.3 -66.04) (end 165.1 63.5)
          (fill (type none))
        )
        (pin input line (at 170.18 60.96 180) (length 5.08)
          (name "USB_OTG_ID")
          (number "101")
        )
        (pin input line (at 109.22 60.96 0) (length 5.08)
          (name "PCIe_CLK_nREQ")
          (number "102")
        )
        (pin passive line (at 170.18 58.42 180) (length 5.08)
          (name "USB2_N")
          (number "103")
        )
        (pin passive line (at 109.22 58.42 0) (length 5.08)
          (name "Reserved")
          (number "104")
        )
        (pin passive line (at 170.18 55.88 180) (length 5.08)
          (name "USB2_P")
          (number "105")
        )
        (pin passive line (at 109.22 55.88 0) (length 5.08)
          (name "Reserved")
          (number "106")
        )
        (pin power_in line (at 170.18 53.34 180) (length 5.08)
          (name "GND")
          (number "107")
        )
        (pin power_in line (at 109.22 53.34 0) (length 5.08)
          (name "GND")
          (number "108")
        )
        (pin bidirectional line (at 170.18 50.8 180) (length 5.08)
          (name "PCIe_nRST")
          (number "109")
        )
        (pin output line (at 109.22 50.8 0) (length 5.08)
          (name "PCIe_CLK_P")
          (number "110")
        )
        (pin passive line (at 170.18 48.26 180) (length 5.08)
          (name "VDAC_COMP")
          (number "111")
        )
        (pin output line (at 109.22 48.26 0) (length 5.08)
          (name "PCIe_CLK_N")
          (number "112")
        )
        (pin power_in line (at 170.18 45.72 180) (length 5.08)
          (name "GND")
          (number "113")
        )
        (pin power_in line (at 109.22 45.72 0) (length 5.08)
          (name "GND")
          (number "114")
        )
        (pin input line (at 170.18 43.18 180) (length 5.08)
          (name "CAM1_D0_N")
          (number "115")
        )
        (pin input line (at 109.22 43.18 0) (length 5.08)
          (name "PCIe_RX_P")
          (number "116")
        )
        (pin input line (at 170.18 40.64 180) (length 5.08)
          (name "CAM1_D0_P")
          (number "117")
        )
        (pin input line (at 109.22 40.64 0) (length 5.08)
          (name "PCIe_RX_N")
          (number "118")
        )
        (pin power_in line (at 170.18 38.1 180) (length 5.08)
          (name "GND")
          (number "119")
        )
        (pin power_in line (at 109.22 38.1 0) (length 5.08)
          (name "GND")
          (number "120")
        )
        (pin input line (at 170.18 35.56 180) (length 5.08)
          (name "CAM1_D1_N")
          (number "121")
        )
        (pin output line (at 109.22 35.56 0) (length 5.08)
          (name "PCIe_TX_P")
          (number "122")
        )
        (pin input line (at 170.18 33.02 180) (length 5.08)
          (name "CAM1_D1_P")
          (number "123")
        )
        (pin output line (at 109.22 33.02 0) (length 5.08)
          (name "PCIe_TX_N")
          (number "124")
        )
        (pin power_in line (at 170.18 30.48 180) (length 5.08)
          (name "GND")
          (number "125")
        )
        (pin power_in line (at 109.22 30.48 0) (length 5.08)
          (name "GND")
          (number "126")
        )
        (pin input line (at 170.18 27.94 180) (length 5.08)
          (name "CAM1_C_N")
          (number "127")
        )
        (pin input line (at 109.22 27.94 0) (length 5.08)
          (name "CAM0_D0_N")
          (number "128")
        )
        (pin input line (at 170.18 25.4 180) (length 5.08)
          (name "CAM1_C_P")
          (number "129")
        )
        (pin input line (at 109.22 25.4 0) (length 5.08)
          (name "CAM0_D0_P")
          (number "130")
        )
        (pin power_in line (at 170.18 22.86 180) (length 5.08)
          (name "GND")
          (number "131")
        )
        (pin power_in line (at 109.22 22.86 0) (length 5.08)
          (name "GND")
          (number "132")
        )
        (pin input line (at 170.18 20.32 180) (length 5.08)
          (name "CAM1_D2_N")
          (number "133")
        )
        (pin input line (at 109.22 20.32 0) (length 5.08)
          (name "CAM0_D1_N")
          (number "134")
        )
        (pin input line (at 170.18 17.78 180) (length 5.08)
          (name "CAM1_D2_P")
          (number "135")
        )
        (pin input line (at 109.22 17.78 0) (length 5.08)
          (name "CAM0_D1_P")
          (number "136")
        )
        (pin power_in line (at 170.18 15.24 180) (length 5.08)
          (name "GND")
          (number "137")
        )
        (pin power_in line (at 109.22 15.24 0) (length 5.08)
          (name "GND")
          (number "138")
        )
        (pin input line (at 170.18 12.7 180) (length 5.08)
          (name "CAM1_D3_N")
          (number "139")
        )
        (pin input line (at 109.22 12.7 0) (length 5.08)
          (name "CAM0_C_N")
          (number "140")
        )
        (pin input line (at 170.18 10.16 180) (length 5.08)
          (name "CAM1_D3_P")
          (number "141")
        )
        (pin input line (at 109.22 10.16 0) (length 5.08)
          (name "CAM0_C_P")
          (number "142")
        )
        (pin input line (at 170.18 7.62 180) (length 5.08)
          (name "HDMI1_HOTPLUG")
          (number "143")
        )
        (pin power_in line (at 109.22 7.62 0) (length 5.08)
          (name "GND")
          (number "144")
        )
        (pin bidirectional line (at 170.18 5.08 180) (length 5.08)
          (name "HDMI1_SDA")
          (number "145")
        )
        (pin output line (at 109.22 5.08 0) (length 5.08)
          (name "HDMI1_TX2_P")
          (number "146")
        )
        (pin open_collector line (at 170.18 2.54 180) (length 5.08)
          (name "HDMI1_SCL")
          (number "147")
        )
        (pin output line (at 109.22 2.54 0) (length 5.08)
          (name "HDMI1_TX2_N")
          (number "148")
        )
        (pin open_collector line (at 170.18 0 180) (length 5.08)
          (name "HDMI1_CEC")
          (number "149")
        )
        (pin power_in line (at 109.22 0 0) (length 5.08)
          (name "GND")
          (number "150")
        )
        (pin open_collector line (at 170.18 -2.54 180) (length 5.08)
          (name "HDMI0_CEC")
          (number "151")
        )
        (pin output line (at 109.22 -2.54 0) (length 5.08)
          (name "HDMI1_TX1_P")
          (number "152")
        )
        (pin input line (at 170.18 -5.08 180) (length 5.08)
          (name "HDMI0_HOTPLUG")
          (number "153")
        )
        (pin output line (at 109.22 -5.08 0) (length 5.08)
          (name "HDMI1_TX1_N")
          (number "154")
        )
        (pin power_in line (at 170.18 -7.62 180) (length 5.08)
          (name "GND")
          (number "155")
        )
        (pin power_in line (at 109.22 -7.62 0) (length 5.08)
          (name "GND")
          (number "156")
        )
        (pin output line (at 170.18 -10.16 180) (length 5.08)
          (name "DSI0_D0_N")
          (number "157")
        )
        (pin output line (at 109.22 -10.16 0) (length 5.08)
          (name "HDMI1_TX0_P")
          (number "158")
        )
        (pin output line (at 170.18 -12.7 180) (length 5.08)
          (name "DSI0_D0_P")
          (number "159")
        )
        (pin output line (at 109.22 -12.7 0) (length 5.08)
          (name "HDMI1_TX0_N")
          (number "160")
        )
        (pin power_in line (at 170.18 -15.24 180) (length 5.08)
          (name "GND")
          (number "161")
        )
        (pin power_in line (at 109.22 -15.24 0) (length 5.08)
          (name "GND")
          (number "162")
        )
        (pin output line (at 170.18 -17.78 180) (length 5.08)
          (name "DSI0_D1_N")
          (number "163")
        )
        (pin output line (at 109.22 -17.78 0) (length 5.08)
          (name "HDMI1_CLK_P")
          (number "164")
        )
        (pin output line (at 170.18 -20.32 180) (length 5.08)
          (name "DSI0_D1_P")
          (number "165")
        )
        (pin output line (at 109.22 -20.32 0) (length 5.08)
          (name "HDMI1_CLK_N")
          (number "166")
        )
        (pin power_in line (at 170.18 -22.86 180) (length 5.08)
          (name "GND")
          (number "167")
        )
        (pin power_in line (at 109.22 -22.86 0) (length 5.08)
          (name "GND")
          (number "168")
        )
        (pin output line (at 170.18 -25.4 180) (length 5.08)
          (name "DSI0_C_N")
          (number "169")
        )
        (pin output line (at 109.22 -25.4 0) (length 5.08)
          (name "HDMI0_TX2_P")
          (number "170")
        )
        (pin output line (at 170.18 -27.94 180) (length 5.08)
          (name "DSI0_C_P")
          (number "171")
        )
        (pin output line (at 109.22 -27.94 0) (length 5.08)
          (name "HDMI0_TX2_N")
          (number "172")
        )
        (pin power_in line (at 170.18 -30.48 180) (length 5.08)
          (name "GND")
          (number "173")
        )
        (pin power_in line (at 109.22 -30.48 0) (length 5.08)
          (name "GND")
          (number "174")
        )
        (pin output line (at 170.18 -33.02 180) (length 5.08)
          (name "DSI1_D0_N")
          (number "175")
        )
        (pin output line (at 109.22 -33.02 0) (length 5.08)
          (name "HDMI0_TX1_P")
          (number "176")
        )
        (pin output line (at 170.18 -35.56 180) (length 5.08)
          (name "DSI1_D0_P")
          (number "177")
        )
        (pin output line (at 109.22 -35.56 0) (length 5.08)
          (name "HDMI0_TX1_N")
          (number "178")
        )
        (pin power_in line (at 170.18 -38.1 180) (length 5.08)
          (name "GND")
          (number "179")
        )
        (pin power_in line (at 109.22 -38.1 0) (length 5.08)
          (name "GND")
          (number "180")
        )
        (pin output line (at 170.18 -40.64 180) (length 5.08)
          (name "DSI1_D1_N")
          (number "181")
        )
        (pin output line (at 109.22 -40.64 0) (length 5.08)
          (name "HDMI0_TX0_P")
          (number "182")
        )
        (pin output line (at 170.18 -43.18 180) (length 5.08)
          (name "DSI1_D1_P")
          (number "183")
        )
        (pin output line (at 109.22 -43.18 0) (length 5.08)
          (name "HDMI0_TX0_N")
          (number "184")
        )
        (pin power_in line (at 170.18 -45.72 180) (length 5.08)
          (name "GND")
          (number "185")
        )
        (pin power_in line (at 109.22 -45.72 0) (length 5.08)
          (name "GND")
          (number "186")
        )
        (pin output line (at 170.18 -48.26 180) (length 5.08)
          (name "DSI1_C_N")
          (number "187")
        )
        (pin output line (at 109.22 -48.26 0) (length 5.08)
          (name "HDMI0_CLK_P")
          (number "188")
        )
        (pin output line (at 170.18 -50.8 180) (length 5.08)
          (name "DSI1_C_P")
          (number "189")
        )
        (pin output line (at 109.22 -50.8 0) (length 5.08)
          (name "HDMI0_CLK_N")
          (number "190")
        )
        (pin power_in line (at 170.18 -53.34 180) (length 5.08)
          (name "GND")
          (number "191")
        )
        (pin power_in line (at 109.22 -53.34 0) (length 5.08)
          (name "GND")
          (number "192")
        )
        (pin output line (at 170.18 -55.88 180) (length 5.08)
          (name "DSI1_D2_N")
          (number "193")
        )
        (pin output line (at 109.22 -55.88 0) (length 5.08)
          (name "DSI1_D3_N")
          (number "194")
        )
        (pin output line (at 170.18 -58.42 180) (length 5.08)
          (name "DSI1_D2_P")
          (number "195")
        )
        (pin output line (at 109.22 -58.42 0) (length 5.08)
          (name "DSI1_D3_P")
          (number "196")
        )
        (pin power_in line (at 170.18 -60.96 180) (length 5.08)
          (name "GND")
          (number "197")
        )
        (pin power_in line (at 109.22 -60.96 0) (length 5.08)
          (name "GND")
          (number "198")
        )
        (pin bidirectional line (at 170.18 -63.5 180) (length 5.08)
          (name "HDMI0_SDA")
          (number "199")
        )
        (pin open_collector line (at 109.22 -63.5 0) (length 5.08)
          (name "HDMI0_SCL")
          (number "200")
        )
      )
    )
    (symbol "CM4IO:FSUSB42MX" (in_bom yes) (on_board yes)
      (property "Reference" "U" (id 0) (at -7.62 20.32 0))
      (property "Value" "FSUSB42MX" (id 1) (at -2.54 -2.54 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "" (id 3) (at 0 0 0))
      (symbol "FSUSB42MX_0_0"
        (pin power_in line (at 8.89 16.51 180) (length 2.54)
          (name "VCC")
          (number "1")
        )
        (pin input line (at 8.89 3.81 180) (length 2.54)
          (name "nOE")
          (number "10")
        )
        (pin input line (at 8.89 13.97 180) (length 2.54)
          (name "SEL")
          (number "2")
        )
        (pin bidirectional line (at 8.89 10.16 180) (length 2.54)
          (name "D_P")
          (number "3")
        )
        (pin bidirectional line (at 8.89 7.62 180) (length 2.54)
          (name "D_N")
          (number "4")
        )
        (pin power_in line (at 8.89 1.27 180) (length 2.54)
          (name "GND")
          (number "5")
        )
        (pin bidirectional line (at -11.43 13.97 0) (length 2.54)
          (name "HSD0_M")
          (number "6")
        )
        (pin bidirectional line (at -11.43 16.51 0) (length 2.54)
          (name "HSD0_P")
          (number "7")
        )
        (pin bidirectional line (at -11.43 1.27 0) (length 2.54)
          (name "HSD1_M")
          (number "8")
        )
        (pin bidirectional line (at -11.43 3.81 0) (length 2.54)
          (name "HSD1_P")
          (number "9")
        )
      )
      (symbol "FSUSB42MX_0_1"
        (rectangle (start -8.89 19.05) (end 6.35 -1.27)
          (fill (type none))
        )
      )
    )
    (symbol "CM4IO:HDMI_A_1.4" (in_bom yes) (on_board yes)
      (property "Reference" "J" (id 0) (at -6.35 26.67 0))
      (property "Value" "HDMI_A_1.4" (id 1) (at 10.16 26.67 0))
      (property "Footprint" "" (id 2) (at 0.635 0 0))
      (property "Datasheet" "https://en.wikipedia.org/wiki/HDMI" (id 3) (at 0.635 0 0))
      (property "ki_keywords" "hdmi conn" (id 4) (at 0 0 0))
      (property "ki_description" "HDMI 1.4+ type A connector" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "HDMI*A*" (id 6) (at 0 0 0))
      (symbol "HDMI_A_1.4_0_0"
        (polyline
          (pts
            (xy 8.128 16.51)
            (xy 8.128 18.034)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 16.51)
            (xy 0 18.034)
            (xy 0 17.272)
            (xy 1.905 17.272)
            (xy 1.905 18.034)
            (xy 1.905 16.51)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 2.667 18.034)
            (xy 4.318 18.034)
            (xy 4.572 17.78)
            (xy 4.572 16.764)
            (xy 4.318 16.51)
            (xy 2.667 16.51)
            (xy 2.667 17.272)
          )
          (fill (type none))
        )
        (pin passive line (at 7.62 -27.94 90) (length 2.54)
          (name "SH")
          (number "SH2")
        )
        (pin passive line (at 7.62 -27.94 90) (length 2.54)
          (name "SH")
          (number "SH3")
        )
        (pin passive line (at 7.62 -27.94 90) (length 2.54)
          (name "SH")
          (number "SH4")
        )
      )
      (symbol "HDMI_A_1.4_0_1"
        (rectangle (start -7.62 25.4) (end 10.16 -25.4)
          (fill (type background))
        )
        (polyline
          (pts
            (xy 2.54 8.89)
            (xy 3.81 8.89)
            (xy 5.08 6.35)
            (xy 5.08 -5.715)
            (xy 3.81 -8.255)
            (xy 2.54 -8.255)
            (xy 2.54 8.89)
          )
          (fill (type outline))
        )
        (polyline
          (pts
            (xy 5.334 16.51)
            (xy 5.334 18.034)
            (xy 6.35 18.034)
            (xy 6.35 16.51)
            (xy 6.35 18.034)
            (xy 7.112 18.034)
            (xy 7.366 17.78)
            (xy 7.366 16.51)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 12.7)
            (xy 0 -12.7)
            (xy 3.81 -12.7)
            (xy 5.08 -10.16)
            (xy 7.62 -8.89)
            (xy 7.62 8.89)
            (xy 5.08 10.16)
            (xy 3.81 12.7)
            (xy 0 12.7)
          )
          (fill (type none))
        )
      )
      (symbol "HDMI_A_1.4_1_1"
        (pin passive line (at -10.16 20.32 0) (length 2.54)
          (name "D2+")
          (number "1")
        )
        (pin passive line (at -10.16 5.08 0) (length 2.54)
          (name "CK+")
          (number "10")
        )
        (pin power_in line (at 2.54 -27.94 90) (length 2.54)
          (name "CKS")
          (number "11")
        )
        (pin passive line (at -10.16 2.54 0) (length 2.54)
          (name "CK-")
          (number "12")
        )
        (pin bidirectional line (at -10.16 -2.54 0) (length 2.54)
          (name "CEC")
          (number "13")
        )
        (pin passive line (at -10.16 -15.24 0) (length 2.54)
          (name "UTILITY/HEAC+")
          (number "14")
        )
        (pin passive line (at -10.16 -7.62 0) (length 2.54)
          (name "SCL")
          (number "15")
        )
        (pin bidirectional line (at -10.16 -10.16 0) (length 2.54)
          (name "SDA")
          (number "16")
        )
        (pin power_in line (at 5.08 -27.94 90) (length 2.54)
          (name "GND")
          (number "17")
        )
        (pin power_in line (at 0 27.94 270) (length 2.54)
          (name "+5V")
          (number "18")
        )
        (pin passive line (at -10.16 -17.78 0) (length 2.54)
          (name "HPD/HEAC-")
          (number "19")
        )
        (pin power_in line (at -5.08 -27.94 90) (length 2.54)
          (name "D2S")
          (number "2")
        )
        (pin passive line (at -10.16 17.78 0) (length 2.54)
          (name "D2-")
          (number "3")
        )
        (pin passive line (at -10.16 15.24 0) (length 2.54)
          (name "D1+")
          (number "4")
        )
        (pin power_in line (at -2.54 -27.94 90) (length 2.54)
          (name "D1S")
          (number "5")
        )
        (pin passive line (at -10.16 12.7 0) (length 2.54)
          (name "D1-")
          (number "6")
        )
        (pin passive line (at -10.16 10.16 0) (length 2.54)
          (name "D0+")
          (number "7")
        )
        (pin power_in line (at 0 -27.94 90) (length 2.54)
          (name "D0S")
          (number "8")
        )
        (pin passive line (at -10.16 7.62 0) (length 2.54)
          (name "D0-")
          (number "9")
        )
        (pin passive line (at 7.62 -27.94 90) (length 2.54)
          (name "SH")
          (number "SH1")
        )
      )
    )
    (symbol "CM4IO:PCIe-x1" (in_bom yes) (on_board yes)
      (property "Reference" "J" (id 0) (at -13.97 36.83 0))
      (property "Value" "PCIe-x1" (id 1) (at -5.08 -13.97 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "" (id 3) (at 0 0 0))
      (symbol "PCIe-x1_0_0"
        (pin passive line (at 10.16 33.02 180) (length 5.08)
          (name "nPRSNT1")
          (number "A1")
        )
        (pin power_in line (at 10.16 10.16 180) (length 5.08)
          (name "+3.3V")
          (number "A10")
        )
        (pin input line (at 10.16 7.62 180) (length 5.08)
          (name "nPERST")
          (number "A11")
        )
        (pin power_in line (at 10.16 5.08 180) (length 5.08)
          (name "GND")
          (number "A12")
        )
        (pin input line (at 10.16 2.54 180) (length 5.08)
          (name "REFCLK+")
          (number "A13")
        )
        (pin input line (at 10.16 0 180) (length 5.08)
          (name "REFCLK-")
          (number "A14")
        )
        (pin power_in line (at 10.16 -2.54 180) (length 5.08)
          (name "GND")
          (number "A15")
        )
        (pin output line (at 10.16 -5.08 180) (length 5.08)
          (name "PERP0")
          (number "A16")
        )
        (pin output line (at 10.16 -7.62 180) (length 5.08)
          (name "PERN0")
          (number "A17")
        )
        (pin power_in line (at 10.16 -10.16 180) (length 5.08)
          (name "GND")
          (number "A18")
        )
        (pin power_in line (at 10.16 30.48 180) (length 5.08)
          (name "+12V")
          (number "A2")
        )
        (pin power_in line (at 10.16 27.94 180) (length 5.08)
          (name "+12V")
          (number "A3")
        )
        (pin power_in line (at 10.16 25.4 180) (length 5.08)
          (name "GND")
          (number "A4")
        )
        (pin input line (at 10.16 22.86 180) (length 5.08)
          (name "TCK")
          (number "A5")
        )
        (pin input line (at 10.16 20.32 180) (length 5.08)
          (name "TDI")
          (number "A6")
        )
        (pin output line (at 10.16 17.78 180) (length 5.08)
          (name "TD0")
          (number "A7")
        )
        (pin input line (at 10.16 15.24 180) (length 5.08)
          (name "TMS")
          (number "A8")
        )
        (pin power_in line (at 10.16 12.7 180) (length 5.08)
          (name "+3.3V")
          (number "A9")
        )
        (pin power_in line (at -19.05 33.02 0) (length 5.08)
          (name "+12v")
          (number "B1")
        )
        (pin power_in line (at -19.05 10.16 0) (length 5.08)
          (name "+3.3vAUX")
          (number "B10")
        )
        (pin open_collector line (at -19.05 7.62 0) (length 5.08)
          (name "nWAKE")
          (number "B11")
        )
        (pin open_collector line (at -19.05 5.08 0) (length 5.08)
          (name "nCLKREQ")
          (number "B12")
        )
        (pin power_in line (at -19.05 2.54 0) (length 5.08)
          (name "GND")
          (number "B13")
        )
        (pin input line (at -19.05 0 0) (length 5.08)
          (name "PETP0")
          (number "B14")
        )
        (pin input line (at -19.05 -2.54 0) (length 5.08)
          (name "PETN0")
          (number "B15")
        )
        (pin power_in line (at -19.05 -5.08 0) (length 5.08)
          (name "GND")
          (number "B16")
        )
        (pin passive line (at -19.05 -7.62 0) (length 5.08)
          (name "nPRSNT2")
          (number "B17")
        )
        (pin power_in line (at -19.05 -10.16 0) (length 5.08)
          (name "GND")
          (number "B18")
        )
        (pin power_in line (at -19.05 30.48 0) (length 5.08)
          (name "+12v")
          (number "B2")
        )
        (pin power_in line (at -19.05 27.94 0) (length 5.08)
          (name "+12v")
          (number "B3")
        )
        (pin power_in line (at -19.05 25.4 0) (length 5.08)
          (name "GND")
          (number "B4")
        )
        (pin passive line (at -19.05 22.86 0) (length 5.08)
          (name "SMCLK")
          (number "B5")
        )
        (pin passive line (at -19.05 20.32 0) (length 5.08)
          (name "SMDAT")
          (number "B6")
        )
        (pin power_in line (at -19.05 17.78 0) (length 5.08)
          (name "GND")
          (number "B7")
        )
        (pin power_in line (at -19.05 15.24 0) (length 5.08)
          (name "+3.3v")
          (number "B8")
        )
        (pin input line (at -19.05 12.7 0) (length 5.08)
          (name "nTRST")
          (number "B9")
        )
      )
      (symbol "PCIe-x1_0_1"
        (rectangle (start -13.97 35.56) (end 5.08 -12.7)
          (fill (type none))
        )
      )
    )
    (symbol "Connector:Conn_01x02_Female" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
      (property "Reference" "J" (id 0) (at 0 2.54 0))
      (property "Value" "Conn_01x02_Female" (id 1) (at 0 -5.08 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "~" (id 3) (at 0 0 0))
      (property "ki_keywords" "connector" (id 4) (at 0 0 0))
      (property "ki_description" "Generic connector, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "Connector*:*_1x??_*" (id 6) (at 0 0 0))
      (symbol "Conn_01x02_Female_1_1"
        (arc (start 0 -2.032) (end 0 -3.048) (radius (at 0 -2.54) (length 0.508) (angles 90.1 -90.1))
          (fill (type none))
        )
        (arc (start 0 0.508) (end 0 -0.508) (radius (at 0 0) (length 0.508) (angles 90.1 -90.1))
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.27 -2.54)
            (xy -0.508 -2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.27 0)
            (xy -0.508 0)
          )
          (fill (type none))
        )
        (pin passive line (at -5.08 0 0) (length 3.81)
          (name "Pin_1")
          (number "1")
        )
        (pin passive line (at -5.08 -2.54 0) (length 3.81)
          (name "Pin_2")
          (number "2")
        )
      )
    )
    (symbol "Connector:Conn_01x11_Female" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
      (property "Reference" "J" (id 0) (at 0 15.24 0))
      (property "Value" "Conn_01x11_Female" (id 1) (at 0 -15.24 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "~" (id 3) (at 0 0 0))
      (property "ki_keywords" "connector" (id 4) (at 0 0 0))
      (property "ki_description" "Generic connector, single row, 01x11, script generated (kicad-library-utils/schlib/autogen/connector/)" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "Connector*:*_1x??_*" (id 6) (at 0 0 0))
      (symbol "Conn_01x11_Female_1_1"
        (arc (start 0 -12.192) (end 0 -13.208) (radius (at 0 -12.7) (length 0.508) (angles 90.1 -90.1))
          (fill (type none))
        )
        (arc (start 0 -9.652) (end 0 -10.668) (radius (at 0 -10.16) (length 0.508) (angles 90.1 -90.1))
          (fill (type none))
        )
        (arc (start 0 -7.112) (end 0 -8.128) (radius (at 0 -7.62) (length 0.508) (angles 90.1 -90.1))
          (fill (type none))
        )
        (arc (start 0 -4.572) (end 0 -5.588) (radius (at 0 -5.08) (length 0.508) (angles 90.1 -90.1))
          (fill (type none))
        )
        (arc (start 0 -2.032) (end 0 -3.048) (radius (at 0 -2.54) (length 0.508) (angles 90.1 -90.1))
          (fill (type none))
        )
        (arc (start 0 0.508) (end 0 -0.508) (radius (at 0 0) (length 0.508) (angles 90.1 -90.1))
          (fill (type none))
        )
        (arc (start 0 3.048) (end 0 2.032) (radius (at 0 2.54) (length 0.508) (angles 90.1 -90.1))
          (fill (type none))
        )
        (arc (start 0 5.588) (end 0 4.572) (radius (at 0 5.08) (length 0.508) (angles 90.1 -90.1))
          (fill (type none))
        )
        (arc (start 0 8.128) (end 0 7.112) (radius (at 0 7.62) (length 0.508) (angles 90.1 -90.1))
          (fill (type none))
        )
        (arc (start 0 10.668) (end 0 9.652) (radius (at 0 10.16) (length 0.508) (angles 90.1 -90.1))
          (fill (type none))
        )
        (arc (start 0 13.208) (end 0 12.192) (radius (at 0 12.7) (length 0.508) (angles 90.1 -90.1))
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.27 -12.7)
            (xy -0.508 -12.7)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.27 -10.16)
            (xy -0.508 -10.16)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.27 -7.62)
            (xy -0.508 -7.62)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.27 -5.08)
            (xy -0.508 -5.08)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.27 -2.54)
            (xy -0.508 -2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.27 0)
            (xy -0.508 0)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.27 2.54)
            (xy -0.508 2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.27 5.08)
            (xy -0.508 5.08)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.27 7.62)
            (xy -0.508 7.62)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.27 10.16)
            (xy -0.508 10.16)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.27 12.7)
            (xy -0.508 12.7)
          )
          (fill (type none))
        )
        (pin passive line (at -5.08 12.7 0) (length 3.81)
          (name "Pin_1")
          (number "1")
        )
        (pin passive line (at -5.08 -10.16 0) (length 3.81)
          (name "Pin_10")
          (number "10")
        )
        (pin passive line (at -5.08 -12.7 0) (length 3.81)
          (name "Pin_11")
          (number "11")
        )
        (pin passive line (at -5.08 10.16 0) (length 3.81)
          (name "Pin_2")
          (number "2")
        )
        (pin passive line (at -5.08 7.62 0) (length 3.81)
          (name "Pin_3")
          (number "3")
        )
        (pin passive line (at -5.08 5.08 0) (length 3.81)
          (name "Pin_4")
          (number "4")
        )
        (pin passive line (at -5.08 2.54 0) (length 3.81)
          (name "Pin_5")
          (number "5")
        )
        (pin passive line (at -5.08 0 0) (length 3.81)
          (name "Pin_6")
          (number "6")
        )
        (pin passive line (at -5.08 -2.54 0) (length 3.81)
          (name "Pin_7")
          (number "7")
        )
        (pin passive line (at -5.08 -5.08 0) (length 3.81)
          (name "Pin_8")
          (number "8")
        )
        (pin passive line (at -5.08 -7.62 0) (length 3.81)
          (name "Pin_9")
          (number "9")
        )
      )
    )
    (symbol "Connector:Conn_01x22_Female" (pin_names hide) (in_bom yes) (on_board yes)
      (property "Reference" "J" (id 0) (at 0 27.94 0))
      (property "Value" "Conn_01x22_Female" (id 1) (at 0 -30.48 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "~" (id 3) (at 0 0 0))
      (property "ki_keywords" "connector" (id 4) (at 0 0 0))
      (property "ki_description" "Generic connector, single row, 01x22, script generated (kicad-library-utils/schlib/autogen/connector/)" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "Connector*:*_1x??_*" (id 6) (at 0 0 0))
      (symbol "Conn_01x22_Female_1_1"
        (arc (start 0 -27.432) (end 0 -28.448) (radius (at 0 -27.94) (length 0.508) (angles 90.1 -90.1))
          (fill (type none))
        )
        (arc (start 0 -24.892) (end 0 -25.908) (radius (at 0 -25.4) (length 0.508) (angles 90.1 -90.1))
          (fill (type none))
        )
        (arc (start 0 -22.352) (end 0 -23.368) (radius (at 0 -22.86) (length 0.508) (angles 90.1 -90.1))
          (fill (type none))
        )
        (arc (start 0 -19.812) (end 0 -20.828) (radius (at 0 -20.32) (length 0.508) (angles 90.1 -90.1))
          (fill (type none))
        )
        (arc (start 0 -17.272) (end 0 -18.288) (radius (at 0 -17.78) (length 0.508) (angles 90.1 -90.1))
          (fill (type none))
        )
        (arc (start 0 -14.732) (end 0 -15.748) (radius (at 0 -15.24) (length 0.508) (angles 90.1 -90.1))
          (fill (type none))
        )
        (arc (start 0 -12.192) (end 0 -13.208) (radius (at 0 -12.7) (length 0.508) (angles 90.1 -90.1))
          (fill (type none))
        )
        (arc (start 0 -9.652) (end 0 -10.668) (radius (at 0 -10.16) (length 0.508) (angles 90.1 -90.1))
          (fill (type none))
        )
        (arc (start 0 -7.112) (end 0 -8.128) (radius (at 0 -7.62) (length 0.508) (angles 90.1 -90.1))
          (fill (type none))
        )
        (arc (start 0 -4.572) (end 0 -5.588) (radius (at 0 -5.08) (length 0.508) (angles 90.1 -90.1))
          (fill (type none))
        )
        (arc (start 0 -2.032) (end 0 -3.048) (radius (at 0 -2.54) (length 0.508) (angles 90.1 -90.1))
          (fill (type none))
        )
        (arc (start 0 0.508) (end 0 -0.508) (radius (at 0 0) (length 0.508) (angles 90.1 -90.1))
          (fill (type none))
        )
        (arc (start 0 3.048) (end 0 2.032) (radius (at 0 2.54) (length 0.508) (angles 90.1 -90.1))
          (fill (type none))
        )
        (arc (start 0 5.588) (end 0 4.572) (radius (at 0 5.08) (length 0.508) (angles 90.1 -90.1))
          (fill (type none))
        )
        (arc (start 0 8.128) (end 0 7.112) (radius (at 0 7.62) (length 0.508) (angles 90.1 -90.1))
          (fill (type none))
        )
        (arc (start 0 10.668) (end 0 9.652) (radius (at 0 10.16) (length 0.508) (angles 90.1 -90.1))
          (fill (type none))
        )
        (arc (start 0 13.208) (end 0 12.192) (radius (at 0 12.7) (length 0.508) (angles 90.1 -90.1))
          (fill (type none))
        )
        (arc (start 0 15.748) (end 0 14.732) (radius (at 0 15.24) (length 0.508) (angles 90.1 -90.1))
          (fill (type none))
        )
        (arc (start 0 18.288) (end 0 17.272) (radius (at 0 17.78) (length 0.508) (angles 90.1 -90.1))
          (fill (type none))
        )
        (arc (start 0 20.828) (end 0 19.812) (radius (at 0 20.32) (length 0.508) (angles 90.1 -90.1))
          (fill (type none))
        )
        (arc (start 0 23.368) (end 0 22.352) (radius (at 0 22.86) (length 0.508) (angles 90.1 -90.1))
          (fill (type none))
        )
        (arc (start 0 25.908) (end 0 24.892) (radius (at 0 25.4) (length 0.508) (angles 90.1 -90.1))
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.27 -27.94)
            (xy -0.508 -27.94)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.27 -25.4)
            (xy -0.508 -25.4)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.27 -22.86)
            (xy -0.508 -22.86)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.27 -20.32)
            (xy -0.508 -20.32)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.27 -17.78)
            (xy -0.508 -17.78)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.27 -15.24)
            (xy -0.508 -15.24)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.27 -12.7)
            (xy -0.508 -12.7)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.27 -10.16)
            (xy -0.508 -10.16)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.27 -7.62)
            (xy -0.508 -7.62)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.27 -5.08)
            (xy -0.508 -5.08)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.27 -2.54)
            (xy -0.508 -2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.27 0)
            (xy -0.508 0)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.27 2.54)
            (xy -0.508 2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.27 5.08)
            (xy -0.508 5.08)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.27 7.62)
            (xy -0.508 7.62)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.27 10.16)
            (xy -0.508 10.16)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.27 12.7)
            (xy -0.508 12.7)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.27 15.24)
            (xy -0.508 15.24)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.27 17.78)
            (xy -0.508 17.78)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.27 20.32)
            (xy -0.508 20.32)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.27 22.86)
            (xy -0.508 22.86)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.27 25.4)
            (xy -0.508 25.4)
          )
          (fill (type none))
        )
        (pin passive line (at -5.08 25.4 0) (length 3.81)
          (name "Pin_1")
          (number "1")
        )
        (pin passive line (at -5.08 2.54 0) (length 3.81)
          (name "Pin_10")
          (number "10")
        )
        (pin passive line (at -5.08 0 0) (length 3.81)
          (name "Pin_11")
          (number "11")
        )
        (pin passive line (at -5.08 -2.54 0) (length 3.81)
          (name "Pin_12")
          (number "12")
        )
        (pin passive line (at -5.08 -5.08 0) (length 3.81)
          (name "Pin_13")
          (number "13")
        )
        (pin passive line (at -5.08 -7.62 0) (length 3.81)
          (name "Pin_14")
          (number "14")
        )
        (pin passive line (at -5.08 -10.16 0) (length 3.81)
          (name "Pin_15")
          (number "15")
        )
        (pin passive line (at -5.08 -12.7 0) (length 3.81)
          (name "Pin_16")
          (number "16")
        )
        (pin passive line (at -5.08 -15.24 0) (length 3.81)
          (name "Pin_17")
          (number "17")
        )
        (pin passive line (at -5.08 -17.78 0) (length 3.81)
          (name "Pin_18")
          (number "18")
        )
        (pin passive line (at -5.08 -20.32 0) (length 3.81)
          (name "Pin_19")
          (number "19")
        )
        (pin passive line (at -5.08 22.86 0) (length 3.81)
          (name "Pin_2")
          (number "2")
        )
        (pin passive line (at -5.08 -22.86 0) (length 3.81)
          (name "Pin_20")
          (number "20")
        )
        (pin passive line (at -5.08 -25.4 0) (length 3.81)
          (name "Pin_21")
          (number "21")
        )
        (pin passive line (at -5.08 -27.94 0) (length 3.81)
          (name "Pin_22")
          (number "22")
        )
        (pin passive line (at -5.08 20.32 0) (length 3.81)
          (name "Pin_3")
          (number "3")
        )
        (pin passive line (at -5.08 17.78 0) (length 3.81)
          (name "Pin_4")
          (number "4")
        )
        (pin passive line (at -5.08 15.24 0) (length 3.81)
          (name "Pin_5")
          (number "5")
        )
        (pin passive line (at -5.08 12.7 0) (length 3.81)
          (name "Pin_6")
          (number "6")
        )
        (pin passive line (at -5.08 10.16 0) (length 3.81)
          (name "Pin_7")
          (number "7")
        )
        (pin passive line (at -5.08 7.62 0) (length 3.81)
          (name "Pin_8")
          (number "8")
        )
        (pin passive line (at -5.08 5.08 0) (length 3.81)
          (name "Pin_9")
          (number "9")
        )
      )
    )
    (symbol "Connector:Micro_SD_Card_Det" (in_bom yes) (on_board yes)
      (property "Reference" "J" (id 0) (at -16.51 17.78 0))
      (property "Value" "Micro_SD_Card_Det" (id 1) (at 16.51 17.78 0))
      (property "Footprint" "" (id 2) (at 52.07 17.78 0))
      (property "Datasheet" "https://www.hirose.com/product/en/download_file/key_name/DM3/category/Catalog/doc_file_id/49662/?file_category_id=4&item_id=195&is_series=1" (id 3) (at 0 2.54 0))
      (property "ki_keywords" "connector SD microsd" (id 4) (at 0 0 0))
      (property "ki_description" "Micro SD Card Socket with card detection pins" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "microSD*" (id 6) (at 0 0 0))
      (symbol "Micro_SD_Card_Det_0_1"
        (rectangle (start -7.62 -6.985) (end -5.08 -8.255)
          (fill (type outline))
        )
        (rectangle (start -7.62 -4.445) (end -5.08 -5.715)
          (fill (type outline))
        )
        (rectangle (start -7.62 -1.905) (end -5.08 -3.175)
          (fill (type outline))
        )
        (rectangle (start -7.62 0.635) (end -5.08 -0.635)
          (fill (type outline))
        )
        (rectangle (start -7.62 3.175) (end -5.08 1.905)
          (fill (type outline))
        )
        (rectangle (start -7.62 5.715) (end -5.08 4.445)
          (fill (type outline))
        )
        (rectangle (start -7.62 8.255) (end -5.08 6.985)
          (fill (type outline))
        )
        (rectangle (start -7.62 10.795) (end -5.08 9.525)
          (fill (type outline))
        )
        (polyline
          (pts
            (xy 16.51 15.24)
            (xy 16.51 16.51)
            (xy -19.05 16.51)
            (xy -19.05 -16.51)
            (xy 16.51 -16.51)
            (xy 16.51 -8.89)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -8.89 -8.89)
            (xy -8.89 11.43)
            (xy -1.27 11.43)
            (xy 2.54 15.24)
            (xy 3.81 15.24)
            (xy 3.81 13.97)
            (xy 6.35 13.97)
            (xy 7.62 15.24)
            (xy 20.32 15.24)
            (xy 20.32 -8.89)
            (xy -8.89 -8.89)
          )
          (fill (type background))
        )
      )
      (symbol "Micro_SD_Card_Det_1_1"
        (pin bidirectional line (at -22.86 10.16 0) (length 3.81)
          (name "DAT2")
          (number "1")
        )
        (pin passive line (at -22.86 -10.16 0) (length 3.81)
          (name "DET_A")
          (number "10")
        )
        (pin passive line (at 20.32 -12.7 180) (length 3.81)
          (name "SHIELD")
          (number "11")
        )
        (pin bidirectional line (at -22.86 7.62 0) (length 3.81)
          (name "DAT3/CD")
          (number "2")
        )
        (pin input line (at -22.86 5.08 0) (length 3.81)
          (name "CMD")
          (number "3")
        )
        (pin power_in line (at -22.86 2.54 0) (length 3.81)
          (name "VDD")
          (number "4")
        )
        (pin input line (at -22.86 0 0) (length 3.81)
          (name "CLK")
          (number "5")
        )
        (pin power_in line (at -22.86 -2.54 0) (length 3.81)
          (name "VSS")
          (number "6")
        )
        (pin bidirectional line (at -22.86 -5.08 0) (length 3.81)
          (name "DAT0")
          (number "7")
        )
        (pin bidirectional line (at -22.86 -7.62 0) (length 3.81)
          (name "DAT1")
          (number "8")
        )
        (pin passive line (at -22.86 -12.7 0) (length 3.81)
          (name "DET_B")
          (number "9")
        )
      )
    )
    (symbol "Connector:TestPoint" (pin_numbers hide) (pin_names (offset 0.762) hide) (in_bom yes) (on_board yes)
      (property "Reference" "TP" (id 0) (at 0 6.858 0))
      (property "Value" "TestPoint" (id 1) (at 0 5.08 0))
      (property "Footprint" "" (id 2) (at 5.08 0 0))
      (property "Datasheet" "~" (id 3) (at 5.08 0 0))
      (property "ki_keywords" "test point tp" (id 4) (at 0 0 0))
      (property "ki_description" "test point" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "Pin* Test*" (id 6) (at 0 0 0))
      (symbol "TestPoint_0_1"
        (circle (center 0 3.302) (radius 0.762) (fill (type none)))
      )
      (symbol "TestPoint_1_1"
        (pin passive line (at 0 0 90) (length 2.54)
          (name "1")
          (number "1")
        )
      )
    )
    (symbol "Connector:USB_A" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
      (property "Reference" "J" (id 0) (at -5.08 11.43 0))
      (property "Value" "USB_A" (id 1) (at -5.08 8.89 0))
      (property "Footprint" "" (id 2) (at 3.81 -1.27 0))
      (property "Datasheet" " ~" (id 3) (at 3.81 -1.27 0))
      (property "ki_keywords" "connector USB" (id 4) (at 0 0 0))
      (property "ki_description" "USB Type A connector" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "USB*" (id 6) (at 0 0 0))
      (symbol "USB_A_0_1"
        (circle (center -3.81 2.159) (radius 0.635) (fill (type outline)))
        (circle (center -0.635 3.429) (radius 0.381) (fill (type outline)))
        (rectangle (start -5.08 -7.62) (end 5.08 7.62)
          (fill (type background))
        )
        (rectangle (start -1.524 4.826) (end -4.318 5.334)
          (fill (type outline))
        )
        (rectangle (start -1.27 4.572) (end -4.572 5.842)
          (fill (type none))
        )
        (rectangle (start -0.127 -7.62) (end 0.127 -6.858)
          (fill (type none))
        )
        (rectangle (start 0.254 1.27) (end -0.508 0.508)
          (fill (type outline))
        )
        (rectangle (start 5.08 -2.667) (end 4.318 -2.413)
          (fill (type none))
        )
        (rectangle (start 5.08 -0.127) (end 4.318 0.127)
          (fill (type none))
        )
        (rectangle (start 5.08 4.953) (end 4.318 5.207)
          (fill (type none))
        )
        (polyline
          (pts
            (xy -3.175 2.159)
            (xy -2.54 2.159)
            (xy -1.27 3.429)
            (xy -0.635 3.429)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -2.54 2.159)
            (xy -1.905 2.159)
            (xy -1.27 0.889)
            (xy 0 0.889)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0.635 2.794)
            (xy 0.635 1.524)
            (xy 1.905 2.159)
            (xy 0.635 2.794)
          )
          (fill (type outline))
        )
      )
      (symbol "USB_A_1_1"
        (polyline
          (pts
            (xy -1.905 2.159)
            (xy 0.635 2.159)
          )
          (fill (type none))
        )
        (pin power_in line (at 7.62 5.08 180) (length 2.54)
          (name "VBUS")
          (number "1")
        )
        (pin bidirectional line (at 7.62 -2.54 180) (length 2.54)
          (name "D-")
          (number "2")
        )
        (pin bidirectional line (at 7.62 0 180) (length 2.54)
          (name "D+")
          (number "3")
        )
        (pin power_in line (at 0 -10.16 90) (length 2.54)
          (name "GND")
          (number "4")
        )
        (pin passive line (at -2.54 -10.16 90) (length 2.54)
          (name "Shield")
          (number "5")
        )
      )
    )
    (symbol "Connector:USB_OTG" (in_bom yes) (on_board yes)
      (property "Reference" "J" (id 0) (at -5.08 11.43 0))
      (property "Value" "USB_OTG" (id 1) (at -5.08 8.89 0))
      (property "Footprint" "" (id 2) (at 3.81 -1.27 0))
      (property "Datasheet" " ~" (id 3) (at 3.81 -1.27 0))
      (property "ki_keywords" "connector USB" (id 4) (at 0 0 0))
      (property "ki_description" "USB mini/micro connector" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "USB*" (id 6) (at 0 0 0))
      (symbol "USB_OTG_0_1"
        (circle (center -3.81 2.159) (radius 0.635) (fill (type outline)))
        (circle (center -0.635 3.429) (radius 0.381) (fill (type outline)))
        (rectangle (start -5.08 -7.62) (end 5.08 7.62)
          (fill (type background))
        )
        (rectangle (start -0.127 -7.62) (end 0.127 -6.858)
          (fill (type none))
        )
        (rectangle (start 0.254 1.27) (end -0.508 0.508)
          (fill (type outline))
        )
        (rectangle (start 5.08 -5.207) (end 4.318 -4.953)
          (fill (type none))
        )
        (rectangle (start 5.08 -2.667) (end 4.318 -2.413)
          (fill (type none))
        )
        (rectangle (start 5.08 -0.127) (end 4.318 0.127)
          (fill (type none))
        )
        (rectangle (start 5.08 4.953) (end 4.318 5.207)
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.905 2.159)
            (xy 0.635 2.159)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -3.175 2.159)
            (xy -2.54 2.159)
            (xy -1.27 3.429)
            (xy -0.635 3.429)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -2.54 2.159)
            (xy -1.905 2.159)
            (xy -1.27 0.889)
            (xy 0 0.889)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0.635 2.794)
            (xy 0.635 1.524)
            (xy 1.905 2.159)
            (xy 0.635 2.794)
          )
          (fill (type outline))
        )
        (polyline
          (pts
            (xy -4.318 5.588)
            (xy -1.778 5.588)
            (xy -2.032 4.826)
            (xy -4.064 4.826)
            (xy -4.318 5.588)
          )
          (fill (type outline))
        )
        (polyline
          (pts
            (xy -4.699 5.842)
            (xy -4.699 5.588)
            (xy -4.445 4.826)
            (xy -4.445 4.572)
            (xy -1.651 4.572)
            (xy -1.651 4.826)
            (xy -1.397 5.588)
            (xy -1.397 5.842)
            (xy -4.699 5.842)
          )
          (fill (type none))
        )
      )
      (symbol "USB_OTG_1_1"
        (pin power_in line (at 7.62 5.08 180) (length 2.54)
          (name "VBUS")
          (number "1")
        )
        (pin passive line (at 7.62 -2.54 180) (length 2.54)
          (name "D-")
          (number "2")
        )
        (pin passive line (at 7.62 0 180) (length 2.54)
          (name "D+")
          (number "3")
        )
        (pin passive line (at 7.62 -5.08 180) (length 2.54)
          (name "ID")
          (number "4")
        )
        (pin power_in line (at 0 -10.16 90) (length 2.54)
          (name "GND")
          (number "5")
        )
        (pin passive line (at -2.54 -10.16 90) (length 2.54)
          (name "Shield")
          (number "6")
        )
      )
    )
    (symbol "Connector_Generic:Conn_02x07_Odd_Even" (pin_names hide) (in_bom yes) (on_board yes)
      (property "Reference" "J" (id 0) (at 1.27 10.16 0))
      (property "Value" "Conn_02x07_Odd_Even" (id 1) (at 1.27 -10.16 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "~" (id 3) (at 0 0 0))
      (property "ki_keywords" "connector" (id 4) (at 0 0 0))
      (property "ki_description" "Generic connector, double row, 02x07, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "Connector*:*_2x??_*" (id 6) (at 0 0 0))
      (symbol "Conn_02x07_Odd_Even_1_1"
        (rectangle (start -1.27 -4.953) (end 0 -5.207)
          (fill (type none))
        )
        (rectangle (start -1.27 -7.493) (end 0 -7.747)
          (fill (type none))
        )
        (rectangle (start -1.27 -2.413) (end 0 -2.667)
          (fill (type none))
        )
        (rectangle (start -1.27 2.667) (end 0 2.413)
          (fill (type none))
        )
        (rectangle (start -1.27 5.207) (end 0 4.953)
          (fill (type none))
        )
        (rectangle (start -1.27 7.747) (end 0 7.493)
          (fill (type none))
        )
        (rectangle (start -1.27 8.89) (end 3.81 -8.89)
          (fill (type background))
        )
        (rectangle (start -1.27 0.127) (end 0 -0.127)
          (fill (type none))
        )
        (rectangle (start 3.81 -4.953) (end 2.54 -5.207)
          (fill (type none))
        )
        (rectangle (start 3.81 -7.493) (end 2.54 -7.747)
          (fill (type none))
        )
        (rectangle (start 3.81 -2.413) (end 2.54 -2.667)
          (fill (type none))
        )
        (rectangle (start 3.81 2.667) (end 2.54 2.413)
          (fill (type none))
        )
        (rectangle (start 3.81 5.207) (end 2.54 4.953)
          (fill (type none))
        )
        (rectangle (start 3.81 7.747) (end 2.54 7.493)
          (fill (type none))
        )
        (rectangle (start 3.81 0.127) (end 2.54 -0.127)
          (fill (type none))
        )
        (pin passive line (at -5.08 7.62 0) (length 3.81)
          (name "Pin_1")
          (number "1")
        )
        (pin passive line (at 7.62 -2.54 180) (length 3.81)
          (name "Pin_10")
          (number "10")
        )
        (pin passive line (at -5.08 -5.08 0) (length 3.81)
          (name "Pin_11")
          (number "11")
        )
        (pin passive line (at 7.62 -5.08 180) (length 3.81)
          (name "Pin_12")
          (number "12")
        )
        (pin passive line (at -5.08 -7.62 0) (length 3.81)
          (name "Pin_13")
          (number "13")
        )
        (pin passive line (at 7.62 -7.62 180) (length 3.81)
          (name "Pin_14")
          (number "14")
        )
        (pin passive line (at 7.62 7.62 180) (length 3.81)
          (name "Pin_2")
          (number "2")
        )
        (pin passive line (at -5.08 5.08 0) (length 3.81)
          (name "Pin_3")
          (number "3")
        )
        (pin passive line (at 7.62 5.08 180) (length 3.81)
          (name "Pin_4")
          (number "4")
        )
        (pin passive line (at -5.08 2.54 0) (length 3.81)
          (name "Pin_5")
          (number "5")
        )
        (pin passive line (at 7.62 2.54 180) (length 3.81)
          (name "Pin_6")
          (number "6")
        )
        (pin passive line (at -5.08 0 0) (length 3.81)
          (name "Pin_7")
          (number "7")
        )
        (pin passive line (at 7.62 0 180) (length 3.81)
          (name "Pin_8")
          (number "8")
        )
        (pin passive line (at -5.08 -2.54 0) (length 3.81)
          (name "Pin_9")
          (number "9")
        )
      )
    )
    (symbol "Connector_Generic:Conn_02x17_Odd_Even" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
      (property "Reference" "J" (id 0) (at 1.27 22.86 0))
      (property "Value" "Conn_02x17_Odd_Even" (id 1) (at 1.27 -22.86 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "~" (id 3) (at 0 0 0))
      (property "ki_keywords" "connector" (id 4) (at 0 0 0))
      (property "ki_description" "Generic connector, double row, 02x17, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "Connector*:*_2x??_*" (id 6) (at 0 0 0))
      (symbol "Conn_02x17_Odd_Even_1_1"
        (rectangle (start -1.27 -4.953) (end 0 -5.207)
          (fill (type none))
        )
        (rectangle (start -1.27 -7.493) (end 0 -7.747)
          (fill (type none))
        )
        (rectangle (start -1.27 -10.033) (end 0 -10.287)
          (fill (type none))
        )
        (rectangle (start -1.27 -12.573) (end 0 -12.827)
          (fill (type none))
        )
        (rectangle (start -1.27 -15.113) (end 0 -15.367)
          (fill (type none))
        )
        (rectangle (start -1.27 -17.653) (end 0 -17.907)
          (fill (type none))
        )
        (rectangle (start -1.27 -20.193) (end 0 -20.447)
          (fill (type none))
        )
        (rectangle (start -1.27 -2.413) (end 0 -2.667)
          (fill (type none))
        )
        (rectangle (start -1.27 2.667) (end 0 2.413)
          (fill (type none))
        )
        (rectangle (start -1.27 5.207) (end 0 4.953)
          (fill (type none))
        )
        (rectangle (start -1.27 7.747) (end 0 7.493)
          (fill (type none))
        )
        (rectangle (start -1.27 10.287) (end 0 10.033)
          (fill (type none))
        )
        (rectangle (start -1.27 0.127) (end 0 -0.127)
          (fill (type none))
        )
        (rectangle (start -1.27 12.827) (end 0 12.573)
          (fill (type none))
        )
        (rectangle (start -1.27 15.367) (end 0 15.113)
          (fill (type none))
        )
        (rectangle (start -1.27 17.907) (end 0 17.653)
          (fill (type none))
        )
        (rectangle (start -1.27 20.447) (end 0 20.193)
          (fill (type none))
        )
        (rectangle (start -1.27 21.59) (end 3.81 -21.59)
          (fill (type background))
        )
        (rectangle (start 3.81 -4.953) (end 2.54 -5.207)
          (fill (type none))
        )
        (rectangle (start 3.81 -7.493) (end 2.54 -7.747)
          (fill (type none))
        )
        (rectangle (start 3.81 -10.033) (end 2.54 -10.287)
          (fill (type none))
        )
        (rectangle (start 3.81 -12.573) (end 2.54 -12.827)
          (fill (type none))
        )
        (rectangle (start 3.81 -15.113) (end 2.54 -15.367)
          (fill (type none))
        )
        (rectangle (start 3.81 -17.653) (end 2.54 -17.907)
          (fill (type none))
        )
        (rectangle (start 3.81 -20.193) (end 2.54 -20.447)
          (fill (type none))
        )
        (rectangle (start 3.81 -2.413) (end 2.54 -2.667)
          (fill (type none))
        )
        (rectangle (start 3.81 2.667) (end 2.54 2.413)
          (fill (type none))
        )
        (rectangle (start 3.81 5.207) (end 2.54 4.953)
          (fill (type none))
        )
        (rectangle (start 3.81 7.747) (end 2.54 7.493)
          (fill (type none))
        )
        (rectangle (start 3.81 10.287) (end 2.54 10.033)
          (fill (type none))
        )
        (rectangle (start 3.81 0.127) (end 2.54 -0.127)
          (fill (type none))
        )
        (rectangle (start 3.81 12.827) (end 2.54 12.573)
          (fill (type none))
        )
        (rectangle (start 3.81 15.367) (end 2.54 15.113)
          (fill (type none))
        )
        (rectangle (start 3.81 17.907) (end 2.54 17.653)
          (fill (type none))
        )
        (rectangle (start 3.81 20.447) (end 2.54 20.193)
          (fill (type none))
        )
        (pin passive line (at -5.08 20.32 0) (length 3.81)
          (name "Pin_1")
          (number "1")
        )
        (pin passive line (at 7.62 10.16 180) (length 3.81)
          (name "Pin_10")
          (number "10")
        )
        (pin passive line (at -5.08 7.62 0) (length 3.81)
          (name "Pin_11")
          (number "11")
        )
        (pin passive line (at 7.62 7.62 180) (length 3.81)
          (name "Pin_12")
          (number "12")
        )
        (pin passive line (at -5.08 5.08 0) (length 3.81)
          (name "Pin_13")
          (number "13")
        )
        (pin passive line (at 7.62 5.08 180) (length 3.81)
          (name "Pin_14")
          (number "14")
        )
        (pin passive line (at -5.08 2.54 0) (length 3.81)
          (name "Pin_15")
          (number "15")
        )
        (pin passive line (at 7.62 2.54 180) (length 3.81)
          (name "Pin_16")
          (number "16")
        )
        (pin passive line (at -5.08 0 0) (length 3.81)
          (name "Pin_17")
          (number "17")
        )
        (pin passive line (at 7.62 0 180) (length 3.81)
          (name "Pin_18")
          (number "18")
        )
        (pin passive line (at -5.08 -2.54 0) (length 3.81)
          (name "Pin_19")
          (number "19")
        )
        (pin passive line (at 7.62 20.32 180) (length 3.81)
          (name "Pin_2")
          (number "2")
        )
        (pin passive line (at 7.62 -2.54 180) (length 3.81)
          (name "Pin_20")
          (number "20")
        )
        (pin passive line (at -5.08 -5.08 0) (length 3.81)
          (name "Pin_21")
          (number "21")
        )
        (pin passive line (at 7.62 -5.08 180) (length 3.81)
          (name "Pin_22")
          (number "22")
        )
        (pin passive line (at -5.08 -7.62 0) (length 3.81)
          (name "Pin_23")
          (number "23")
        )
        (pin passive line (at 7.62 -7.62 180) (length 3.81)
          (name "Pin_24")
          (number "24")
        )
        (pin passive line (at -5.08 -10.16 0) (length 3.81)
          (name "Pin_25")
          (number "25")
        )
        (pin passive line (at 7.62 -10.16 180) (length 3.81)
          (name "Pin_26")
          (number "26")
        )
        (pin passive line (at -5.08 -12.7 0) (length 3.81)
          (name "Pin_27")
          (number "27")
        )
        (pin passive line (at 7.62 -12.7 180) (length 3.81)
          (name "Pin_28")
          (number "28")
        )
        (pin passive line (at -5.08 -15.24 0) (length 3.81)
          (name "Pin_29")
          (number "29")
        )
        (pin passive line (at -5.08 17.78 0) (length 3.81)
          (name "Pin_3")
          (number "3")
        )
        (pin passive line (at 7.62 -15.24 180) (length 3.81)
          (name "Pin_30")
          (number "30")
        )
        (pin passive line (at -5.08 -17.78 0) (length 3.81)
          (name "Pin_31")
          (number "31")
        )
        (pin passive line (at 7.62 -17.78 180) (length 3.81)
          (name "Pin_32")
          (number "32")
        )
        (pin passive line (at -5.08 -20.32 0) (length 3.81)
          (name "Pin_33")
          (number "33")
        )
        (pin passive line (at 7.62 -20.32 180) (length 3.81)
          (name "Pin_34")
          (number "34")
        )
        (pin passive line (at 7.62 17.78 180) (length 3.81)
          (name "Pin_4")
          (number "4")
        )
        (pin passive line (at -5.08 15.24 0) (length 3.81)
          (name "Pin_5")
          (number "5")
        )
        (pin passive line (at 7.62 15.24 180) (length 3.81)
          (name "Pin_6")
          (number "6")
        )
        (pin passive line (at -5.08 12.7 0) (length 3.81)
          (name "Pin_7")
          (number "7")
        )
        (pin passive line (at 7.62 12.7 180) (length 3.81)
          (name "Pin_8")
          (number "8")
        )
        (pin passive line (at -5.08 10.16 0) (length 3.81)
          (name "Pin_9")
          (number "9")
        )
      )
    )
    (symbol "Device:C" (pin_numbers hide) (pin_names (offset 0.254)) (in_bom yes) (on_board yes)
      (property "Reference" "C" (id 0) (at 0.635 2.54 0))
      (property "Value" "C" (id 1) (at 0.635 -2.54 0))
      (property "Footprint" "" (id 2) (at 0.9652 -3.81 0))
      (property "Datasheet" "~" (id 3) (at 0 0 0))
      (property "ki_keywords" "cap capacitor" (id 4) (at 0 0 0))
      (property "ki_description" "Unpolarized capacitor" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "C_*" (id 6) (at 0 0 0))
      (symbol "C_0_1"
        (polyline
          (pts
            (xy -2.032 -0.762)
            (xy 2.032 -0.762)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -2.032 0.762)
            (xy 2.032 0.762)
          )
          (fill (type none))
        )
      )
      (symbol "C_1_1"
        (pin passive line (at 0 3.81 270) (length 2.794)
          (name "~")
          (number "1")
        )
        (pin passive line (at 0 -3.81 90) (length 2.794)
          (name "~")
          (number "2")
        )
      )
    )
    (symbol "Device:Crystal" (pin_numbers hide) (pin_names hide) (in_bom yes) (on_board yes)
      (property "Reference" "Y" (id 0) (at 0 3.81 0))
      (property "Value" "Crystal" (id 1) (at 0 -3.81 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "~" (id 3) (at 0 0 0))
      (property "ki_keywords" "quartz ceramic resonator oscillator" (id 4) (at 0 0 0))
      (property "ki_description" "Two pin crystal" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "Crystal*" (id 6) (at 0 0 0))
      (symbol "Crystal_0_1"
        (rectangle (start -1.143 2.54) (end 1.143 -2.54)
          (fill (type none))
        )
        (polyline
          (pts
            (xy -2.54 0)
            (xy -1.905 0)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.905 -1.27)
            (xy -1.905 1.27)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.905 -1.27)
            (xy 1.905 1.27)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 2.54 0)
            (xy 1.905 0)
          )
          (fill (type none))
        )
      )
      (symbol "Crystal_1_1"
        (pin passive line (at -3.81 0 0) (length 1.27)
          (name "1")
          (number "1")
        )
        (pin passive line (at 3.81 0 180) (length 1.27)
          (name "2")
          (number "3")
        )
      )
    )
    (symbol "Device:D" (pin_numbers hide) (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
      (property "Reference" "D" (id 0) (at 0 2.54 0))
      (property "Value" "D" (id 1) (at 0 -2.54 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "~" (id 3) (at 0 0 0))
      (property "ki_keywords" "diode" (id 4) (at 0 0 0))
      (property "ki_description" "Diode" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "TO-???* *_Diode_* *SingleDiode* D_*" (id 6) (at 0 0 0))
      (symbol "D_0_1"
        (polyline
          (pts
            (xy -1.27 1.27)
            (xy -1.27 -1.27)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.27 0)
            (xy -1.27 0)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.27 1.27)
            (xy 1.27 -1.27)
            (xy -1.27 0)
            (xy 1.27 1.27)
          )
          (fill (type none))
        )
      )
      (symbol "D_1_1"
        (pin passive line (at -3.81 0 0) (length 2.54)
          (name "K")
          (number "1")
        )
        (pin passive line (at 3.81 0 180) (length 2.54)
          (name "A")
          (number "2")
        )
      )
    )
    (symbol "Device:LED" (pin_numbers hide) (pin_names hide) (in_bom yes) (on_board yes)
      (property "Reference" "D" (id 0) (at 0 2.54 0))
      (property "Value" "LED" (id 1) (at 0 -2.54 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "~" (id 3) (at 0 0 0))
      (property "ki_keywords" "LED diode" (id 4) (at 0 0 0))
      (property "ki_description" "Light emitting diode" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "LED* LED_SMD:* LED_THT:*" (id 6) (at 0 0 0))
      (symbol "LED_0_1"
        (polyline
          (pts
            (xy -1.27 -1.27)
            (xy -1.27 1.27)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.27 0)
            (xy 1.27 0)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.27 -1.27)
            (xy 1.27 1.27)
            (xy -1.27 0)
            (xy 1.27 -1.27)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -3.048 -0.762)
            (xy -4.572 -2.286)
            (xy -3.81 -2.286)
            (xy -4.572 -2.286)
            (xy -4.572 -1.524)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.778 -0.762)
            (xy -3.302 -2.286)
            (xy -2.54 -2.286)
            (xy -3.302 -2.286)
            (xy -3.302 -1.524)
          )
          (fill (type none))
        )
      )
      (symbol "LED_1_1"
        (pin passive line (at -3.81 0 0) (length 2.54)
          (name "K")
          (number "1")
        )
        (pin passive line (at 3.81 0 180) (length 2.54)
          (name "A")
          (number "2")
        )
      )
    )
    (symbol "Device:LED_1" (pin_numbers hide) (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
      (property "Reference" "D" (id 0) (at 0 2.54 0))
      (property "Value" "LED" (id 1) (at 0 -2.54 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "~" (id 3) (at 0 0 0))
      (property "ki_keywords" "LED diode" (id 4) (at 0 0 0))
      (property "ki_description" "Light emitting diode" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "LED* LED_SMD:* LED_THT:*" (id 6) (at 0 0 0))
      (symbol "LED_1_0_1"
        (polyline
          (pts
            (xy -1.27 -1.27)
            (xy -1.27 1.27)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.27 0)
            (xy 1.27 0)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.27 -1.27)
            (xy 1.27 1.27)
            (xy -1.27 0)
            (xy 1.27 -1.27)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -3.048 -0.762)
            (xy -4.572 -2.286)
            (xy -3.81 -2.286)
            (xy -4.572 -2.286)
            (xy -4.572 -1.524)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.778 -0.762)
            (xy -3.302 -2.286)
            (xy -2.54 -2.286)
            (xy -3.302 -2.286)
            (xy -3.302 -1.524)
          )
          (fill (type none))
        )
      )
      (symbol "LED_1_1_1"
        (pin passive line (at -3.81 0 0) (length 2.54)
          (name "K")
          (number "1")
        )
        (pin passive line (at 3.81 0 180) (length 2.54)
          (name "A")
          (number "2")
        )
      )
    )
    (symbol "Device:R" (pin_numbers hide) (pin_names (offset 0)) (in_bom yes) (on_board yes)
      (property "Reference" "R" (id 0) (at 2.032 0 90))
      (property "Value" "R" (id 1) (at 0 0 90))
      (property "Footprint" "" (id 2) (at -1.778 0 90))
      (property "Datasheet" "~" (id 3) (at 0 0 0))
      (property "ki_keywords" "R res resistor" (id 4) (at 0 0 0))
      (property "ki_description" "Resistor" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "R_*" (id 6) (at 0 0 0))
      (symbol "R_0_1"
        (rectangle (start -1.016 -2.54) (end 1.016 2.54)
          (fill (type none))
        )
      )
      (symbol "R_1_1"
        (pin passive line (at 0 3.81 270) (length 1.27)
          (name "~")
          (number "1")
        )
        (pin passive line (at 0 -3.81 90) (length 1.27)
          (name "~")
          (number "2")
        )
      )
    )
    (symbol "Interface_USB:USB2514B_Bi" (in_bom yes) (on_board yes)
      (property "Reference" "U" (id 0) (at -17.78 40.64 0))
      (property "Value" "USB2514B_Bi" (id 1) (at -20.32 38.1 0))
      (property "Footprint" "Package_DFN_QFN:QFN-36-1EP_6x6mm_P0.5mm_EP3.7x3.7mm" (id 2) (at 33.02 -38.1 0))
      (property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/00001692C.pdf" (id 3) (at 40.64 -40.64 0))
      (property "ki_keywords" "USB2.0 Hi-Speed-USB-Hub Hub-Controller" (id 4) (at 0 0 0))
      (property "ki_description" "USB 2.0 Hi-Speed Hub Controller" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "QFN*6x6mm*P0.5mm*" (id 6) (at 0 0 0))
      (symbol "USB2514B_Bi_0_1"
        (rectangle (start -25.4 35.56) (end 25.4 -35.56)
          (fill (type background))
        )
      )
      (symbol "USB2514B_Bi_1_1"
        (pin bidirectional line (at 27.94 22.86 180) (length 2.54)
          (name "USBDM_DN1/PRT_DIS_M1")
          (number "1")
        )
        (pin power_in line (at -5.08 38.1 270) (length 2.54)
          (name "VDDA33")
          (number "10")
        )
        (pin input line (at -27.94 7.62 0) (length 2.54)
          (name "TEST")
          (number "11")
        )
        (pin bidirectional line (at 27.94 17.78 180) (length 2.54)
          (name "PRTPWR1/BC_EN1")
          (number "12")
        )
        (pin input line (at 27.94 15.24 180) (length 2.54)
          (name "OCS_N1")
          (number "13")
        )
        (pin input line (at -27.94 -12.7 0) (length 2.54)
          (name "CRFILT")
          (number "14")
        )
        (pin power_in line (at 5.08 38.1 270) (length 2.54)
          (name "VDD33")
          (number "15")
        )
        (pin bidirectional line (at 27.94 5.08 180) (length 2.54)
          (name "PRTPWR2/BC_EN2")
          (number "16")
        )
        (pin input line (at 27.94 2.54 180) (length 2.54)
          (name "OCS_N2")
          (number "17")
        )
        (pin bidirectional line (at 27.94 -7.62 180) (length 2.54)
          (name "PRTPWR3/BC_EN3")
          (number "18")
        )
        (pin input line (at 27.94 -10.16 180) (length 2.54)
          (name "OCS_N3")
          (number "19")
        )
        (pin bidirectional line (at 27.94 20.32 180) (length 2.54)
          (name "USBDP_DN1/PRT_DIS_P1")
          (number "2")
        )
        (pin bidirectional line (at 27.94 -20.32 180) (length 2.54)
          (name "PRTPWR4/BC_EN4")
          (number "20")
        )
        (pin input line (at 27.94 -22.86 180) (length 2.54)
          (name "OCS_N4")
          (number "21")
        )
        (pin bidirectional line (at -27.94 -22.86 0) (length 2.54)
          (name "SDA/SMBDATA/NON_REM1")
          (number "22")
        )
        (pin power_in line (at 7.62 38.1 270) (length 2.54)
          (name "VDD33")
          (number "23")
        )
        (pin bidirectional line (at -27.94 -20.32 0) (length 2.54)
          (name "SCL/SMBCLK/CFG_SEL0")
          (number "24")
        )
        (pin bidirectional line (at -27.94 -27.94 0) (length 2.54)
          (name "HS_IND/CFG_SEL1")
          (number "25")
        )
        (pin input line (at -27.94 10.16 0) (length 2.54)
          (name "RESET_N")
          (number "26")
        )
        (pin input line (at -27.94 22.86 0) (length 2.54)
          (name "VBUS_DET")
          (number "27")
        )
        (pin bidirectional line (at -27.94 -25.4 0) (length 2.54)
          (name "SUSP_IND/LOCAL_PWR/NON_REM0")
          (number "28")
        )
        (pin power_in line (at -2.54 38.1 270) (length 2.54)
          (name "VDDA33")
          (number "29")
        )
        (pin bidirectional line (at 27.94 10.16 180) (length 2.54)
          (name "USBDM_DN2/PRT_DIS_M2")
          (number "3")
        )
        (pin bidirectional line (at -27.94 17.78 0) (length 2.54)
          (name "USBDM_UP")
          (number "30")
        )
        (pin bidirectional line (at -27.94 15.24 0) (length 2.54)
          (name "USBDP_UP")
          (number "31")
        )
        (pin output line (at -27.94 -5.08 0) (length 2.54)
          (name "XTALOUT")
          (number "32")
        )
        (pin input clock (at -27.94 -2.54 0) (length 2.54)
          (name "XTALIN/CLKIN")
          (number "33")
        )
        (pin input line (at -27.94 -10.16 0) (length 2.54)
          (name "PLLFILT")
          (number "34")
        )
        (pin input line (at -27.94 2.54 0) (length 2.54)
          (name "RBIAS")
          (number "35")
        )
        (pin power_in line (at 0 38.1 270) (length 2.54)
          (name "VDDA33")
          (number "36")
        )
        (pin power_in line (at 0 -38.1 90) (length 2.54)
          (name "VSS")
          (number "37")
        )
        (pin bidirectional line (at 27.94 7.62 180) (length 2.54)
          (name "USBDP_DN2/PRT_DIS_P2")
          (number "4")
        )
        (pin power_in line (at -7.62 38.1 270) (length 2.54)
          (name "VDDA33")
          (number "5")
        )
        (pin bidirectional line (at 27.94 -2.54 180) (length 2.54)
          (name "USBDM_DN3/PRT_DIS_M3")
          (number "6")
        )
        (pin bidirectional line (at 27.94 -5.08 180) (length 2.54)
          (name "USBDP_DN3/PRT_DIS_P3")
          (number "7")
        )
        (pin bidirectional line (at 27.94 -15.24 180) (length 2.54)
          (name "USBDM_DN4/PRT_DIS_M4")
          (number "8")
        )
        (pin bidirectional line (at 27.94 -17.78 180) (length 2.54)
          (name "USBDP_DN4/PRT_DIS_P4")
          (number "9")
        )
      )
    )
    (symbol "Regulator_Switching:LM22676MR-ADJ" (in_bom yes) (on_board yes)
      (property "Reference" "U" (id 0) (at -6.35 8.89 0))
      (property "Value" "LM22676MR-ADJ" (id 1) (at 5.08 8.89 0))
      (property "Footprint" "Package_SO:TI_SO-PowerPAD-8" (id 2) (at 0 11.43 0))
      (property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm22676.pdf" (id 3) (at 1.27 0 0))
      (property "ki_keywords" "DC/DC Buck Converter 3A" (id 4) (at 0 0 0))
      (property "ki_description" "3A Step-Down Switching Voltage Regulater, 4.5-42V Input, Adjustable Output, 500kHz Switching Frequency, SOIC-8" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "TI*SO*PowerPAD*" (id 6) (at 0 0 0))
      (symbol "LM22676MR-ADJ_0_1"
        (rectangle (start -7.62 7.62) (end 7.62 -7.62)
          (fill (type background))
        )
      )
      (symbol "LM22676MR-ADJ_1_1"
        (pin input line (at 10.16 0 180) (length 2.54)
          (name "BOOT")
          (number "1")
        )
        (pin unconnected line (at -7.62 2.54 0) (length 2.54) hide
          (name "NC")
          (number "2")
        )
        (pin unconnected line (at -7.62 0 0) (length 2.54) hide
          (name "NC")
          (number "3")
        )
        (pin input line (at 10.16 -5.08 180) (length 2.54)
          (name "FB")
          (number "4")
        )
        (pin input line (at -10.16 -2.54 0) (length 2.54)
          (name "EN")
          (number "5")
        )
        (pin power_in line (at 2.54 -10.16 90) (length 2.54)
          (name "GND")
          (number "6")
        )
        (pin power_in line (at -10.16 5.08 0) (length 2.54)
          (name "VIN")
          (number "7")
        )
        (pin power_out line (at 10.16 5.08 180) (length 2.54)
          (name "SW")
          (number "8")
        )
        (pin power_in line (at -2.54 -10.16 90) (length 2.54)
          (name "EP")
          (number "9")
        )
      )
    )
    (symbol "power:GND" (power) (pin_names (offset 0)) (in_bom yes) (on_board yes)
      (property "Reference" "#PWR" (id 0) (at 0 -6.35 0))
      (property "Value" "GND" (id 1) (at 0 -3.81 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "" (id 3) (at 0 0 0))
      (property "ki_keywords" "power-flag" (id 4) (at 0 0 0))
      (property "ki_description" "Power symbol creates a global label with name \"GND\" , ground" (id 5) (at 0 0 0))
      (symbol "GND_0_1"
        (polyline
          (pts
            (xy 0 0)
            (xy 0 -1.27)
            (xy 1.27 -1.27)
            (xy 0 -2.54)
            (xy -1.27 -1.27)
            (xy 0 -1.27)
          )
          (fill (type none))
        )
      )
      (symbol "GND_1_1"
        (pin power_in line (at 0 0 270) (length 0) hide
          (name "GND")
          (number "1")
        )
      )
    )
    (symbol "pspice:INDUCTOR" (pin_numbers hide) (pin_names (offset 0)) (in_bom yes) (on_board yes)
      (property "Reference" "L" (id 0) (at 0 2.54 0))
      (property "Value" "INDUCTOR" (id 1) (at 0 -1.27 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "~" (id 3) (at 0 0 0))
      (property "ki_keywords" "simulation" (id 4) (at 0 0 0))
      (property "ki_description" "Inductor symbol for simulation only" (id 5) (at 0 0 0))
      (symbol "INDUCTOR_0_1"
        (arc (start -2.54 0) (end -5.08 0) (radius (at -3.81 0) (length 1.27) (angles 0.1 179.9))
          (fill (type none))
        )
        (arc (start 0 0) (end -2.54 0) (radius (at -1.27 0) (length 1.27) (angles 0.1 179.9))
          (fill (type none))
        )
        (arc (start 2.54 0) (end 0 0) (radius (at 1.27 0) (length 1.27) (angles 0.1 179.9))
          (fill (type none))
        )
        (arc (start 5.08 0) (end 2.54 0) (radius (at 3.81 0) (length 1.27) (angles 0.1 179.9))
          (fill (type none))
        )
      )
      (symbol "INDUCTOR_1_1"
        (pin input line (at -6.35 0 0) (length 1.27)
          (name "1")
          (number "1")
        )
        (pin input line (at 6.35 0 180) (length 1.27)
          (name "2")
          (number "2")
        )
      )
    )
  )
  (junction (at 21.59 247.65) (diameter 1.016) (color 0 0 0 0))
  (junction (at 27.94 199.39) (diameter 1.016) (color 0 0 0 0))
  (junction (at 27.94 207.01) (diameter 1.016) (color 0 0 0 0))
  (junction (at 29.21 115.57) (diameter 0.9144) (color 0 0 0 0))
  (junction (at 29.21 123.19) (diameter 0.9144) (color 0 0 0 0))
  (junction (at 37.084 199.39) (diameter 1.016) (color 0 0 0 0))
  (junction (at 37.084 207.01) (diameter 1.016) (color 0 0 0 0))
  (junction (at 37.846 26.67) (diameter 1.016) (color 0 0 0 0))
  (junction (at 37.846 34.29) (diameter 1.016) (color 0 0 0 0))
  (junction (at 37.846 44.45) (diameter 1.016) (color 0 0 0 0))
  (junction (at 37.846 57.15) (diameter 1.016) (color 0 0 0 0))
  (junction (at 37.846 69.85) (diameter 1.016) (color 0 0 0 0))
  (junction (at 37.846 82.55) (diameter 1.016) (color 0 0 0 0))
  (junction (at 37.846 92.71) (diameter 1.016) (color 0 0 0 0))
  (junction (at 37.846 100.33) (diameter 1.016) (color 0 0 0 0))
  (junction (at 37.846 110.49) (diameter 1.016) (color 0 0 0 0))
  (junction (at 37.846 140.97) (diameter 1.016) (color 0 0 0 0))
  (junction (at 39.116 123.19) (diameter 1.016) (color 0 0 0 0))
  (junction (at 39.116 128.27) (diameter 1.016) (color 0 0 0 0))
  (junction (at 44.45 189.23) (diameter 0.9144) (color 0 0 0 0))
  (junction (at 46.228 199.39) (diameter 1.016) (color 0 0 0 0))
  (junction (at 46.228 207.01) (diameter 1.016) (color 0 0 0 0))
  (junction (at 53.34 181.61) (diameter 0.9144) (color 0 0 0 0))
  (junction (at 53.34 189.23) (diameter 0.9144) (color 0 0 0 0))
  (junction (at 56.388 199.39) (diameter 1.016) (color 0 0 0 0))
  (junction (at 56.388 207.01) (diameter 1.016) (color 0 0 0 0))
  (junction (at 62.23 181.61) (diameter 0.9144) (color 0 0 0 0))
  (junction (at 62.23 189.23) (diameter 0.9144) (color 0 0 0 0))
  (junction (at 69.85 199.39) (diameter 1.016) (color 0 0 0 0))
  (junction (at 69.85 207.01) (diameter 1.016) (color 0 0 0 0))
  (junction (at 71.12 181.61) (diameter 0.9144) (color 0 0 0 0))
  (junction (at 71.12 189.23) (diameter 0.9144) (color 0 0 0 0))
  (junction (at 80.01 181.61) (diameter 0.9144) (color 0 0 0 0))
  (junction (at 80.01 189.23) (diameter 0.9144) (color 0 0 0 0))
  (junction (at 81.28 199.39) (diameter 1.016) (color 0 0 0 0))
  (junction (at 81.28 207.01) (diameter 1.016) (color 0 0 0 0))
  (junction (at 88.9 181.61) (diameter 0.9144) (color 0 0 0 0))
  (junction (at 88.9 189.23) (diameter 0.9144) (color 0 0 0 0))
  (junction (at 91.44 199.39) (diameter 1.016) (color 0 0 0 0))
  (junction (at 91.44 207.01) (diameter 1.016) (color 0 0 0 0))
  (junction (at 97.79 181.61) (diameter 0.9144) (color 0 0 0 0))
  (junction (at 97.79 189.23) (diameter 0.9144) (color 0 0 0 0))
  (junction (at 100.076 115.57) (diameter 1.016) (color 0 0 0 0))
  (junction (at 100.076 118.11) (diameter 1.016) (color 0 0 0 0))
  (junction (at 100.076 120.65) (diameter 1.016) (color 0 0 0 0))
  (junction (at 100.076 123.19) (diameter 1.016) (color 0 0 0 0))
  (junction (at 100.076 125.73) (diameter 1.016) (color 0 0 0 0))
  (junction (at 101.346 26.67) (diameter 1.016) (color 0 0 0 0))
  (junction (at 101.346 34.29) (diameter 1.016) (color 0 0 0 0))
  (junction (at 101.346 46.99) (diameter 1.016) (color 0 0 0 0))
  (junction (at 101.346 59.69) (diameter 1.016) (color 0 0 0 0))
  (junction (at 101.346 72.39) (diameter 1.016) (color 0 0 0 0))
  (junction (at 101.346 85.09) (diameter 1.016) (color 0 0 0 0))
  (junction (at 101.346 92.71) (diameter 1.016) (color 0 0 0 0))
  (junction (at 101.346 100.33) (diameter 1.016) (color 0 0 0 0))
  (junction (at 101.346 107.95) (diameter 1.016) (color 0 0 0 0))
  (junction (at 101.346 132.08) (diameter 1.016) (color 0 0 0 0))
  (junction (at 106.68 181.61) (diameter 0.9144) (color 0 0 0 0))
  (junction (at 106.68 189.23) (diameter 0.9144) (color 0 0 0 0))
  (junction (at 110.49 44.45) (diameter 0.9144) (color 0 0 0 0))
  (junction (at 115.57 181.61) (diameter 0.9144) (color 0 0 0 0))
  (junction (at 115.57 189.23) (diameter 0.9144) (color 0 0 0 0))
  (junction (at 115.57 231.14) (diameter 1.016) (color 0 0 0 0))
  (junction (at 115.57 238.76) (diameter 1.016) (color 0 0 0 0))
  (junction (at 115.57 246.38) (diameter 1.016) (color 0 0 0 0))
  (junction (at 115.57 254) (diameter 1.016) (color 0 0 0 0))
  (junction (at 115.57 261.62) (diameter 1.016) (color 0 0 0 0))
  (junction (at 115.57 269.24) (diameter 1.016) (color 0 0 0 0))
  (junction (at 124.46 181.61) (diameter 0.9144) (color 0 0 0 0))
  (junction (at 124.46 189.23) (diameter 0.9144) (color 0 0 0 0))
  (junction (at 146.05 231.14) (diameter 1.016) (color 0 0 0 0))
  (junction (at 146.05 238.76) (diameter 1.016) (color 0 0 0 0))
  (junction (at 146.05 246.38) (diameter 1.016) (color 0 0 0 0))
  (junction (at 146.05 254) (diameter 1.016) (color 0 0 0 0))
  (junction (at 146.05 261.62) (diameter 1.016) (color 0 0 0 0))
  (junction (at 146.05 269.24) (diameter 1.016) (color 0 0 0 0))
  (junction (at 149.86 24.13) (diameter 1.016) (color 0 0 0 0))
  (junction (at 151.13 54.61) (diameter 1.016) (color 0 0 0 0))
  (junction (at 151.13 72.39) (diameter 1.016) (color 0 0 0 0))
  (junction (at 157.48 191.77) (diameter 0.9144) (color 0 0 0 0))
  (junction (at 157.48 207.01) (diameter 0.9144) (color 0 0 0 0))
  (junction (at 166.37 24.13) (diameter 1.016) (color 0 0 0 0))
  (junction (at 166.37 39.37) (diameter 1.016) (color 0 0 0 0))
  (junction (at 166.37 46.99) (diameter 1.016) (color 0 0 0 0))
  (junction (at 166.37 59.69) (diameter 1.016) (color 0 0 0 0))
  (junction (at 166.37 64.77) (diameter 1.016) (color 0 0 0 0))
  (junction (at 168.91 207.01) (diameter 0.9144) (color 0 0 0 0))
  (junction (at 173.99 207.01) (diameter 0.9144) (color 0 0 0 0))
  (junction (at 181.61 191.77) (diameter 0.9144) (color 0 0 0 0))
  (junction (at 189.23 196.85) (diameter 0.9144) (color 0 0 0 0))
  (junction (at 191.008 130.429) (diameter 1.016) (color 0 0 0 0))
  (junction (at 194.31 196.85) (diameter 0.9144) (color 0 0 0 0))
  (junction (at 198.12 44.45) (diameter 1.016) (color 0 0 0 0))
  (junction (at 198.12 46.99) (diameter 1.016) (color 0 0 0 0))
  (junction (at 199.39 41.91) (diameter 1.016) (color 0 0 0 0))
  (junction (at 199.39 57.15) (diameter 1.016) (color 0 0 0 0))
  (junction (at 199.39 64.77) (diameter 1.016) (color 0 0 0 0))
  (junction (at 199.39 69.85) (diameter 1.016) (color 0 0 0 0))
  (junction (at 200.66 26.67) (diameter 0.9144) (color 0 0 0 0))
  (junction (at 200.66 29.21) (diameter 1.016) (color 0 0 0 0))
  (junction (at 227.33 121.92) (diameter 1.016) (color 0 0 0 0))
  (junction (at 227.33 129.54) (diameter 1.016) (color 0 0 0 0))
  (junction (at 227.33 137.16) (diameter 1.016) (color 0 0 0 0))
  (junction (at 227.33 144.78) (diameter 1.016) (color 0 0 0 0))
  (junction (at 227.33 152.4) (diameter 1.016) (color 0 0 0 0))
  (junction (at 227.33 160.02) (diameter 1.016) (color 0 0 0 0))
  (junction (at 227.33 167.64) (diameter 1.016) (color 0 0 0 0))
  (junction (at 227.33 175.26) (diameter 1.016) (color 0 0 0 0))
  (junction (at 227.33 182.88) (diameter 1.016) (color 0 0 0 0))
  (junction (at 227.33 190.5) (diameter 1.016) (color 0 0 0 0))
  (junction (at 227.33 198.12) (diameter 1.016) (color 0 0 0 0))
  (junction (at 227.33 205.74) (diameter 1.016) (color 0 0 0 0))
  (junction (at 227.33 213.36) (diameter 1.016) (color 0 0 0 0))
  (junction (at 227.33 220.98) (diameter 1.016) (color 0 0 0 0))
  (junction (at 227.33 228.6) (diameter 1.016) (color 0 0 0 0))
  (junction (at 229.87 29.21) (diameter 1.016) (color 0 0 0 0))
  (junction (at 231.14 54.61) (diameter 1.016) (color 0 0 0 0))
  (junction (at 231.14 62.23) (diameter 1.016) (color 0 0 0 0))
  (junction (at 231.14 69.85) (diameter 1.016) (color 0 0 0 0))
  (junction (at 233.68 36.83) (diameter 1.016) (color 0 0 0 0))
  (junction (at 233.68 39.37) (diameter 1.016) (color 0 0 0 0))
  (junction (at 233.68 44.45) (diameter 1.016) (color 0 0 0 0))
  (junction (at 233.68 46.99) (diameter 1.016) (color 0 0 0 0))
  (junction (at 264.16 26.67) (diameter 1.016) (color 0 0 0 0))
  (junction (at 271.145 26.67) (diameter 0.9144) (color 0 0 0 0))
  (junction (at 273.05 78.74) (diameter 0.9144) (color 0 0 0 0))
  (junction (at 274.32 39.37) (diameter 1.016) (color 0 0 0 0))
  (junction (at 278.13 78.74) (diameter 0.9144) (color 0 0 0 0))
  (junction (at 285.75 63.5) (diameter 0.9144) (color 0 0 0 0))
  (junction (at 293.37 68.58) (diameter 0.9144) (color 0 0 0 0))
  (junction (at 293.37 76.2) (diameter 0.9144) (color 0 0 0 0))
  (junction (at 293.37 121.92) (diameter 1.016) (color 0 0 0 0))
  (junction (at 293.37 129.54) (diameter 1.016) (color 0 0 0 0))
  (junction (at 293.37 137.16) (diameter 1.016) (color 0 0 0 0))
  (junction (at 293.37 144.78) (diameter 1.016) (color 0 0 0 0))
  (junction (at 293.37 152.4) (diameter 1.016) (color 0 0 0 0))
  (junction (at 293.37 175.26) (diameter 1.016) (color 0 0 0 0))
  (junction (at 293.37 182.88) (diameter 1.016) (color 0 0 0 0))
  (junction (at 293.37 190.5) (diameter 1.016) (color 0 0 0 0))
  (junction (at 293.37 198.12) (diameter 1.016) (color 0 0 0 0))
  (junction (at 293.37 205.74) (diameter 1.016) (color 0 0 0 0))
  (junction (at 293.37 213.36) (diameter 1.016) (color 0 0 0 0))
  (junction (at 293.37 220.98) (diameter 1.016) (color 0 0 0 0))
  (junction (at 293.37 228.6) (diameter 1.016) (color 0 0 0 0))
  (junction (at 298.45 68.58) (diameter 0.9144) (color 0 0 0 0))
  (junction (at 313.055 46.99) (diameter 0.9144) (color 0 0 0 0))
  (junction (at 323.85 116.84) (diameter 0.9144) (color 0 0 0 0))
  (junction (at 323.85 124.46) (diameter 0.9144) (color 0 0 0 0))
  (junction (at 331.47 116.84) (diameter 0.9144) (color 0 0 0 0))
  (junction (at 331.47 124.46) (diameter 0.9144) (color 0 0 0 0))
  (junction (at 331.47 125.73) (diameter 0.9144) (color 0 0 0 0))
  (junction (at 332.74 36.83) (diameter 0.9144) (color 0 0 0 0))
  (junction (at 335.28 62.23) (diameter 0.9144) (color 0 0 0 0))
  (junction (at 337.82 214.63) (diameter 1.016) (color 0 0 0 0))
  (junction (at 340.36 214.63) (diameter 1.016) (color 0 0 0 0))
  (junction (at 342.9 214.63) (diameter 1.016) (color 0 0 0 0))
  (junction (at 345.44 214.63) (diameter 1.016) (color 0 0 0 0))
  (junction (at 347.98 214.63) (diameter 1.016) (color 0 0 0 0))
  (junction (at 359.41 36.83) (diameter 0.9144) (color 0 0 0 0))
  (junction (at 360.68 67.31) (diameter 1.016) (color 0 0 0 0))
  (junction (at 361.95 62.23) (diameter 0.9144) (color 0 0 0 0))
  (junction (at 363.22 67.31) (diameter 1.016) (color 0 0 0 0))
  (junction (at 365.76 67.31) (diameter 1.016) (color 0 0 0 0))
  (junction (at 368.3 67.31) (diameter 1.016) (color 0 0 0 0))
  (junction (at 373.38 67.31) (diameter 1.016) (color 0 0 0 0))
  (junction (at 386.08 210.82) (diameter 1.016) (color 0 0 0 0))
  (junction (at 388.62 210.82) (diameter 1.016) (color 0 0 0 0))
  (junction (at 391.16 210.82) (diameter 1.016) (color 0 0 0 0))
  (junction (at 393.7 210.82) (diameter 1.016) (color 0 0 0 0))
  (junction (at 396.24 210.82) (diameter 1.016) (color 0 0 0 0))
  (no_connect (at 200.66 52.07))
  (no_connect (at 39.116 102.87))
  (no_connect (at 39.116 105.41))
  (no_connect (at 100.076 110.49))
  (no_connect (at 200.66 39.37))
  (no_connect (at 229.87 109.22))
  (no_connect (at 340.36 118.11))
  (no_connect (at 118.11 266.7))
  (no_connect (at 229.87 26.67))
  (no_connect (at 100.076 41.91))
  (no_connect (at 39.116 97.79))
  (no_connect (at 265.43 71.12))
  (no_connect (at 229.87 111.76))
  (no_connect (at 200.66 67.31))
  (no_connect (at 148.59 266.7))
  (no_connect (at 148.59 264.16))
  (no_connect (at 332.74 201.93))
  (no_connect (at 39.116 107.95))
  (no_connect (at 161.29 199.39))
  (no_connect (at 229.87 41.91))
  (no_connect (at 305.435 41.91))
  (no_connect (at 200.66 36.83))
  (no_connect (at 340.36 115.57))
  (no_connect (at 381 198.12))
  (wire (pts (xy 13.97 162.56) (xy 27.94 162.56)))
  (wire (pts (xy 14.986 170.18) (xy 20.32 170.18)))
  (wire (pts (xy 21.59 199.39) (xy 27.94 199.39)))
  (wire (pts (xy 21.59 237.49) (xy 29.21 237.49)))
  (wire (pts (xy 21.59 245.11) (xy 21.59 247.65)))
  (wire (pts (xy 21.59 247.65) (xy 21.59 248.92)))
  (wire (pts (xy 21.59 247.65) (xy 43.18 247.65)))
  (wire (pts (xy 23.876 21.59) (xy 39.116 21.59)))
  (wire (pts (xy 23.876 24.13) (xy 39.116 24.13)))
  (wire (pts (xy 23.876 29.21) (xy 39.116 29.21)))
  (wire (pts (xy 23.876 31.75) (xy 39.116 31.75)))
  (wire (pts (xy 23.876 36.83) (xy 39.116 36.83)))
  (wire (pts (xy 23.876 39.37) (xy 39.116 39.37)))
  (wire (pts (xy 23.876 41.91) (xy 39.116 41.91)))
  (wire (pts (xy 24.13 255.27) (xy 35.56 255.27)))
  (wire (pts (xy 24.13 262.89) (xy 35.56 262.89)))
  (wire (pts (xy 25.146 46.99) (xy 39.116 46.99)))
  (wire (pts (xy 25.146 49.53) (xy 39.116 49.53)))
  (wire (pts (xy 25.146 52.07) (xy 39.116 52.07)))
  (wire (pts (xy 25.146 54.61) (xy 39.116 54.61)))
  (wire (pts (xy 25.146 59.69) (xy 39.116 59.69)))
  (wire (pts (xy 25.146 62.23) (xy 39.116 62.23)))
  (wire (pts (xy 25.146 64.77) (xy 39.116 64.77)))
  (wire (pts (xy 25.146 67.31) (xy 39.116 67.31)))
  (wire (pts (xy 25.146 72.39) (xy 39.116 72.39)))
  (wire (pts (xy 25.146 74.93) (xy 39.116 74.93)))
  (wire (pts (xy 25.146 77.47) (xy 39.116 77.47)))
  (wire (pts (xy 25.146 80.01) (xy 39.116 80.01)))
  (wire (pts (xy 25.146 85.09) (xy 39.116 85.09)))
  (wire (pts (xy 25.146 87.63) (xy 39.116 87.63)))
  (wire (pts (xy 25.146 90.17) (xy 39.116 90.17)))
  (wire (pts (xy 25.146 95.25) (xy 39.116 95.25)))
  (wire (pts (xy 25.146 115.57) (xy 29.21 115.57)))
  (wire (pts (xy 25.146 118.11) (xy 39.116 118.11)))
  (wire (pts (xy 25.146 120.65) (xy 39.116 120.65)))
  (wire (pts (xy 25.146 123.19) (xy 29.21 123.19)))
  (wire (pts (xy 25.146 143.51) (xy 39.116 143.51)))
  (wire (pts (xy 25.4 128.27) (xy 39.116 128.27)))
  (wire (pts (xy 25.4 133.35) (xy 39.116 133.35)))
  (wire (pts (xy 25.4 135.89) (xy 39.116 135.89)))
  (wire (pts (xy 25.4 138.43) (xy 39.116 138.43)))
  (wire (pts (xy 25.6032 113.03) (xy 39.116 113.03)))
  (wire (pts (xy 27.94 162.56) (xy 27.94 167.64)))
  (wire (pts (xy 27.94 172.72) (xy 27.94 179.07)))
  (wire (pts (xy 27.94 199.39) (xy 37.084 199.39)))
  (wire (pts (xy 27.94 207.01) (xy 37.084 207.01)))
  (wire (pts (xy 27.94 210.82) (xy 27.94 207.01)))
  (wire (pts (xy 29.21 115.57) (xy 29.21 123.19)))
  (wire (pts (xy 29.21 115.57) (xy 39.116 115.57)))
  (wire (pts (xy 29.21 123.19) (xy 39.116 123.19)))
  (wire (pts (xy 29.21 242.57) (xy 29.21 237.49)))
  (wire (pts (xy 31.75 234.95) (xy 43.18 234.95)))
  (wire (pts (xy 31.75 240.03) (xy 43.18 240.03)))
  (wire (pts (xy 31.75 250.19) (xy 43.18 250.19)))
  (wire (pts (xy 34.29 170.18) (xy 66.294 170.18)))
  (wire (pts (xy 37.084 199.39) (xy 46.228 199.39)))
  (wire (pts (xy 37.084 207.01) (xy 46.228 207.01)))
  (wire (pts (xy 37.846 19.05) (xy 37.846 26.67)))
  (wire (pts (xy 37.846 26.67) (xy 37.846 34.29)))
  (wire (pts (xy 37.846 34.29) (xy 37.846 44.45)))
  (wire (pts (xy 37.846 44.45) (xy 37.846 57.15)))
  (wire (pts (xy 37.846 44.45) (xy 39.116 44.45)))
  (wire (pts (xy 37.846 57.15) (xy 37.846 69.85)))
  (wire (pts (xy 37.846 57.15) (xy 39.116 57.15)))
  (wire (pts (xy 37.846 69.85) (xy 37.846 82.55)))
  (wire (pts (xy 37.846 69.85) (xy 39.116 69.85)))
  (wire (pts (xy 37.846 82.55) (xy 37.846 92.71)))
  (wire (pts (xy 37.846 82.55) (xy 39.116 82.55)))
  (wire (pts (xy 37.846 92.71) (xy 37.846 100.33)))
  (wire (pts (xy 37.846 92.71) (xy 39.116 92.71)))
  (wire (pts (xy 37.846 100.33) (xy 37.846 110.49)))
  (wire (pts (xy 37.846 100.33) (xy 39.116 100.33)))
  (wire (pts (xy 37.846 110.49) (xy 37.846 140.97)))
  (wire (pts (xy 37.846 110.49) (xy 39.116 110.49)))
  (wire (pts (xy 37.846 140.97) (xy 37.846 148.59)))
  (wire (pts (xy 39.116 19.05) (xy 37.846 19.05)))
  (wire (pts (xy 39.116 26.67) (xy 37.846 26.67)))
  (wire (pts (xy 39.116 34.29) (xy 37.846 34.29)))
  (wire (pts (xy 39.116 125.73) (xy 39.116 123.19)))
  (wire (pts (xy 39.116 128.27) (xy 39.37 128.27)))
  (wire (pts (xy 39.116 130.81) (xy 39.116 128.27)))
  (wire (pts (xy 39.116 140.97) (xy 37.846 140.97)))
  (wire (pts (xy 43.18 237.49) (xy 31.75 237.49)))
  (wire (pts (xy 43.18 242.57) (xy 29.21 242.57)))
  (wire (pts (xy 43.18 245.11) (xy 31.75 245.11)))
  (wire (pts (xy 43.18 252.73) (xy 31.75 252.73)))
  (wire (pts (xy 43.18 257.81) (xy 43.18 262.89)))
  (wire (pts (xy 44.45 181.61) (xy 53.34 181.61)))
  (wire (pts (xy 44.45 189.23) (xy 53.34 189.23)))
  (wire (pts (xy 46.228 199.39) (xy 56.388 199.39)))
  (wire (pts (xy 46.228 207.01) (xy 56.388 207.01)))
  (wire (pts (xy 53.34 181.61) (xy 62.23 181.61)))
  (wire (pts (xy 53.34 189.23) (xy 62.23 189.23)))
  (wire (pts (xy 55.88 165.1) (xy 66.294 165.1)))
  (wire (pts (xy 55.88 167.64) (xy 66.294 167.64)))
  (wire (pts (xy 56.134 154.94) (xy 66.294 154.94)))
  (wire (pts (xy 56.134 157.48) (xy 66.294 157.48)))
  (wire (pts (xy 56.134 160.02) (xy 66.294 160.02)))
  (wire (pts (xy 56.134 162.56) (xy 66.294 162.56)))
  (wire (pts (xy 56.388 199.39) (xy 69.85 199.39)))
  (wire (pts (xy 56.388 207.01) (xy 69.85 207.01)))
  (wire (pts (xy 62.23 181.61) (xy 71.12 181.61)))
  (wire (pts (xy 62.23 189.23) (xy 71.12 189.23)))
  (wire (pts (xy 69.85 199.39) (xy 81.28 199.39)))
  (wire (pts (xy 69.85 207.01) (xy 81.28 207.01)))
  (wire (pts (xy 71.12 181.61) (xy 80.01 181.61)))
  (wire (pts (xy 71.12 189.23) (xy 80.01 189.23)))
  (wire (pts (xy 78.994 154.94) (xy 96.774 154.94)))
  (wire (pts (xy 78.994 157.48) (xy 96.774 157.48)))
  (wire (pts (xy 78.994 160.02) (xy 96.774 160.02)))
  (wire (pts (xy 78.994 162.56) (xy 96.774 162.56)))
  (wire (pts (xy 78.994 165.1) (xy 96.774 165.1)))
  (wire (pts (xy 78.994 167.64) (xy 96.774 167.64)))
  (wire (pts (xy 78.994 170.18) (xy 97.028 170.18)))
  (wire (pts (xy 80.01 181.61) (xy 88.9 181.61)))
  (wire (pts (xy 80.01 189.23) (xy 88.9 189.23)))
  (wire (pts (xy 81.28 199.39) (xy 91.44 199.39)))
  (wire (pts (xy 81.28 207.01) (xy 91.44 207.01)))
  (wire (pts (xy 86.36 257.81) (xy 88.9 257.81)))
  (wire (pts (xy 88.9 181.61) (xy 97.79 181.61)))
  (wire (pts (xy 88.9 189.23) (xy 97.79 189.23)))
  (wire (pts (xy 88.9 257.81) (xy 88.9 262.89)))
  (wire (pts (xy 91.44 199.39) (xy 101.854 199.39)))
  (wire (pts (xy 91.44 207.01) (xy 101.854 207.01)))
  (wire (pts (xy 97.79 181.61) (xy 106.68 181.61)))
  (wire (pts (xy 97.79 189.23) (xy 106.68 189.23)))
  (wire (pts (xy 100.076 19.05) (xy 101.346 19.05)))
  (wire (pts (xy 100.076 21.59) (xy 113.03 21.59)))
  (wire (pts (xy 100.076 24.13) (xy 113.03 24.13)))
  (wire (pts (xy 100.076 26.67) (xy 101.346 26.67)))
  (wire (pts (xy 100.076 29.21) (xy 113.03 29.21)))
  (wire (pts (xy 100.076 31.75) (xy 113.03 31.75)))
  (wire (pts (xy 100.076 34.29) (xy 101.346 34.29)))
  (wire (pts (xy 100.076 36.83) (xy 113.03 36.83)))
  (wire (pts (xy 100.076 39.37) (xy 113.03 39.37)))
  (wire (pts (xy 100.076 44.45) (xy 101.6 44.45)))
  (wire (pts (xy 100.076 46.99) (xy 101.346 46.99)))
  (wire (pts (xy 100.076 49.53) (xy 114.046 49.53)))
  (wire (pts (xy 100.076 52.07) (xy 114.046 52.07)))
  (wire (pts (xy 100.076 54.61) (xy 114.046 54.61)))
  (wire (pts (xy 100.076 57.15) (xy 114.046 57.15)))
  (wire (pts (xy 100.076 59.69) (xy 101.346 59.69)))
  (wire (pts (xy 100.076 62.23) (xy 114.046 62.23)))
  (wire (pts (xy 100.076 64.77) (xy 114.046 64.77)))
  (wire (pts (xy 100.076 67.31) (xy 114.046 67.31)))
  (wire (pts (xy 100.076 69.85) (xy 114.046 69.85)))
  (wire (pts (xy 100.076 72.39) (xy 101.346 72.39)))
  (wire (pts (xy 100.076 74.93) (xy 114.046 74.93)))
  (wire (pts (xy 100.076 77.47) (xy 114.046 77.47)))
  (wire (pts (xy 100.076 80.01) (xy 114.046 80.01)))
  (wire (pts (xy 100.076 82.55) (xy 114.046 82.55)))
  (wire (pts (xy 100.076 85.09) (xy 101.346 85.09)))
  (wire (pts (xy 100.076 87.63) (xy 114.046 87.63)))
  (wire (pts (xy 100.076 92.71) (xy 101.346 92.71)))
  (wire (pts (xy 100.076 97.79) (xy 114.046 97.79)))
  (wire (pts (xy 100.076 100.33) (xy 101.346 100.33)))
  (wire (pts (xy 100.076 105.41) (xy 114.046 105.41)))
  (wire (pts (xy 100.076 107.95) (xy 101.346 107.95)))
  (wire (pts (xy 100.076 113.03) (xy 115.316 113.03)))
  (wire (pts (xy 100.076 115.57) (xy 100.076 118.11)))
  (wire (pts (xy 100.076 115.57) (xy 114.046 115.57)))
  (wire (pts (xy 100.076 118.11) (xy 100.076 120.65)))
  (wire (pts (xy 100.076 120.65) (xy 100.076 123.19)))
  (wire (pts (xy 100.076 123.19) (xy 100.076 125.73)))
  (wire (pts (xy 100.076 125.73) (xy 100.076 128.27)))
  (wire (pts (xy 100.076 130.81) (xy 103.632 130.81)))
  (wire (pts (xy 100.076 133.35) (xy 117.856 133.35)))
  (wire (pts (xy 100.076 135.89) (xy 117.856 135.89)))
  (wire (pts (xy 100.076 138.43) (xy 114.046 138.43)))
  (wire (pts (xy 100.076 143.51) (xy 116.586 143.51)))
  (wire (pts (xy 101.346 19.05) (xy 101.346 26.67)))
  (wire (pts (xy 101.346 26.67) (xy 101.346 34.29)))
  (wire (pts (xy 101.346 34.29) (xy 101.346 46.99)))
  (wire (pts (xy 101.346 46.99) (xy 101.346 59.69)))
  (wire (pts (xy 101.346 59.69) (xy 101.346 72.39)))
  (wire (pts (xy 101.346 72.39) (xy 101.346 85.09)))
  (wire (pts (xy 101.346 85.09) (xy 101.346 92.71)))
  (wire (pts (xy 101.346 92.71) (xy 101.346 100.33)))
  (wire (pts (xy 101.346 100.33) (xy 101.346 107.95)))
  (wire (pts (xy 101.346 107.95) (xy 101.346 132.08)))
  (wire (pts (xy 101.346 132.08) (xy 101.346 148.59)))
  (wire (pts (xy 101.346 132.08) (xy 104.7242 132.08)))
  (wire (pts (xy 101.6 226.06) (xy 118.11 226.06)))
  (wire (pts (xy 101.6 228.6) (xy 118.11 228.6)))
  (wire (pts (xy 101.6 233.68) (xy 118.11 233.68)))
  (wire (pts (xy 101.6 236.22) (xy 118.11 236.22)))
  (wire (pts (xy 101.6 241.3) (xy 118.11 241.3)))
  (wire (pts (xy 101.6 243.84) (xy 118.11 243.84)))
  (wire (pts (xy 101.6 248.92) (xy 118.11 248.92)))
  (wire (pts (xy 101.6 251.46) (xy 118.11 251.46)))
  (wire (pts (xy 101.6 256.54) (xy 118.11 256.54)))
  (wire (pts (xy 101.6 259.08) (xy 118.11 259.08)))
  (wire (pts (xy 101.6 264.16) (xy 118.11 264.16)))
  (wire (pts (xy 103.632 128.27) (xy 117.856 128.27)))
  (wire (pts (xy 103.632 130.81) (xy 103.632 128.27)))
  (wire (pts (xy 104.7242 130.81) (xy 117.856 130.81)))
  (wire (pts (xy 104.7242 132.08) (xy 104.7242 130.81)))
  (wire (pts (xy 106.68 181.61) (xy 115.57 181.61)))
  (wire (pts (xy 106.68 189.23) (xy 115.57 189.23)))
  (wire (pts (xy 109.22 44.45) (xy 110.49 44.45)))
  (wire (pts (xy 110.49 44.45) (xy 118.11 44.45)))
  (wire (pts (xy 114.046 90.17) (xy 100.076 90.17)))
  (wire (pts (xy 114.046 95.25) (xy 100.076 95.25)))
  (wire (pts (xy 114.046 102.87) (xy 100.076 102.87)))
  (wire (pts (xy 115.57 181.61) (xy 124.46 181.61)))
  (wire (pts (xy 115.57 189.23) (xy 124.46 189.23)))
  (wire (pts (xy 115.57 223.52) (xy 115.57 231.14)))
  (wire (pts (xy 115.57 231.14) (xy 115.57 238.76)))
  (wire (pts (xy 115.57 231.14) (xy 118.11 231.14)))
  (wire (pts (xy 115.57 238.76) (xy 115.57 246.38)))
  (wire (pts (xy 115.57 238.76) (xy 118.11 238.76)))
  (wire (pts (xy 115.57 246.38) (xy 115.57 254)))
  (wire (pts (xy 115.57 246.38) (xy 118.11 246.38)))
  (wire (pts (xy 115.57 254) (xy 115.57 261.62)))
  (wire (pts (xy 115.57 254) (xy 118.11 254)))
  (wire (pts (xy 115.57 261.62) (xy 115.57 269.24)))
  (wire (pts (xy 115.57 261.62) (xy 118.11 261.62)))
  (wire (pts (xy 115.57 269.24) (xy 115.57 278.13)))
  (wire (pts (xy 115.57 269.24) (xy 118.11 269.24)))
  (wire (pts (xy 118.11 223.52) (xy 115.57 223.52)))
  (wire (pts (xy 118.11 271.78) (xy 101.6 271.78)))
  (wire (pts (xy 118.11 274.32) (xy 101.6 274.32)))
  (wire (pts (xy 118.11 276.86) (xy 101.6 276.86)))
  (wire (pts (xy 124.46 181.61) (xy 133.35 181.61)))
  (wire (pts (xy 124.46 189.23) (xy 133.35 189.23)))
  (wire (pts (xy 129.54 101.6) (xy 140.97 101.6)))
  (wire (pts (xy 129.54 106.68) (xy 140.97 106.68)))
  (wire (pts (xy 132.08 226.06) (xy 148.59 226.06)))
  (wire (pts (xy 132.08 228.6) (xy 148.59 228.6)))
  (wire (pts (xy 132.08 233.68) (xy 148.59 233.68)))
  (wire (pts (xy 132.08 236.22) (xy 148.59 236.22)))
  (wire (pts (xy 132.08 241.3) (xy 148.59 241.3)))
  (wire (pts (xy 132.08 243.84) (xy 148.59 243.84)))
  (wire (pts (xy 132.08 248.92) (xy 148.59 248.92)))
  (wire (pts (xy 132.08 251.46) (xy 148.59 251.46)))
  (wire (pts (xy 132.08 256.54) (xy 148.59 256.54)))
  (wire (pts (xy 132.08 259.08) (xy 148.59 259.08)))
  (wire (pts (xy 140.97 26.67) (xy 152.4 26.67)))
  (wire (pts (xy 140.97 29.21) (xy 152.4 29.21)))
  (wire (pts (xy 140.97 31.75) (xy 152.4 31.75)))
  (wire (pts (xy 140.97 36.83) (xy 152.4 36.83)))
  (wire (pts (xy 140.97 39.37) (xy 152.4 39.37)))
  (wire (pts (xy 140.97 41.91) (xy 152.4 41.91)))
  (wire (pts (xy 140.97 46.99) (xy 152.4 46.99)))
  (wire (pts (xy 140.97 49.53) (xy 152.4 49.53)))
  (wire (pts (xy 140.97 52.07) (xy 152.4 52.07)))
  (wire (pts (xy 140.97 57.15) (xy 152.4 57.15)))
  (wire (pts (xy 140.97 59.69) (xy 152.4 59.69)))
  (wire (pts (xy 140.97 62.23) (xy 152.4 62.23)))
  (wire (pts (xy 140.97 64.77) (xy 152.4 64.77)))
  (wire (pts (xy 140.97 67.31) (xy 152.4 67.31)))
  (wire (pts (xy 140.97 69.85) (xy 152.4 69.85)))
  (wire (pts (xy 140.97 151.13) (xy 152.4 151.13)))
  (wire (pts (xy 143.51 24.13) (xy 149.86 24.13)))
  (wire (pts (xy 146.05 223.52) (xy 146.05 231.14)))
  (wire (pts (xy 146.05 231.14) (xy 146.05 238.76)))
  (wire (pts (xy 146.05 231.14) (xy 148.59 231.14)))
  (wire (pts (xy 146.05 238.76) (xy 146.05 246.38)))
  (wire (pts (xy 146.05 238.76) (xy 148.59 238.76)))
  (wire (pts (xy 146.05 246.38) (xy 146.05 254)))
  (wire (pts (xy 146.05 246.38) (xy 148.59 246.38)))
  (wire (pts (xy 146.05 254) (xy 146.05 261.62)))
  (wire (pts (xy 146.05 254) (xy 148.59 254)))
  (wire (pts (xy 146.05 261.62) (xy 146.05 269.24)))
  (wire (pts (xy 146.05 261.62) (xy 148.59 261.62)))
  (wire (pts (xy 146.05 269.24) (xy 146.05 278.13)))
  (wire (pts (xy 146.05 269.24) (xy 148.59 269.24)))
  (wire (pts (xy 148.59 223.52) (xy 146.05 223.52)))
  (wire (pts (xy 148.59 271.78) (xy 132.08 271.78)))
  (wire (pts (xy 148.59 274.32) (xy 132.08 274.32)))
  (wire (pts (xy 148.59 276.86) (xy 132.08 276.86)))
  (wire (pts (xy 149.86 24.13) (xy 149.86 44.45)))
  (wire (pts (xy 149.86 44.45) (xy 152.4 44.45)))
  (wire (pts (xy 151.13 34.29) (xy 151.13 54.61)))
  (wire (pts (xy 151.13 54.61) (xy 151.13 72.39)))
  (wire (pts (xy 151.13 54.61) (xy 152.4 54.61)))
  (wire (pts (xy 151.13 72.39) (xy 151.13 73.66)))
  (wire (pts (xy 151.13 72.39) (xy 152.4 72.39)))
  (wire (pts (xy 151.13 191.77) (xy 157.48 191.77)))
  (wire (pts (xy 151.13 194.31) (xy 151.13 207.01)))
  (wire (pts (xy 151.13 207.01) (xy 157.48 207.01)))
  (wire (pts (xy 152.4 24.13) (xy 149.86 24.13)))
  (wire (pts (xy 152.4 34.29) (xy 151.13 34.29)))
  (wire (pts (xy 156.21 101.6) (xy 156.21 106.68)))
  (wire (pts (xy 157.48 191.77) (xy 161.29 191.77)))
  (wire (pts (xy 157.48 199.39) (xy 157.48 207.01)))
  (wire (pts (xy 157.48 207.01) (xy 168.91 207.01)))
  (wire (pts (xy 161.798 145.542) (xy 175.768 145.542)))
  (wire (pts (xy 165.1 24.13) (xy 166.37 24.13)))
  (wire (pts (xy 165.1 26.67) (xy 166.37 26.67)))
  (wire (pts (xy 165.1 29.21) (xy 166.37 29.21)))
  (wire (pts (xy 165.1 31.75) (xy 176.53 31.75)))
  (wire (pts (xy 165.1 34.29) (xy 176.53 34.29)))
  (wire (pts (xy 165.1 36.83) (xy 176.53 36.83)))
  (wire (pts (xy 165.1 41.91) (xy 176.53 41.91)))
  (wire (pts (xy 165.1 44.45) (xy 176.53 44.45)))
  (wire (pts (xy 165.1 49.53) (xy 176.53 49.53)))
  (wire (pts (xy 165.1 52.07) (xy 176.53 52.07)))
  (wire (pts (xy 165.1 54.61) (xy 176.53 54.61)))
  (wire (pts (xy 165.1 57.15) (xy 176.53 57.15)))
  (wire (pts (xy 165.1 59.69) (xy 166.37 59.69)))
  (wire (pts (xy 165.1 62.23) (xy 176.53 62.23)))
  (wire (pts (xy 165.1 64.77) (xy 166.37 64.77)))
  (wire (pts (xy 165.1 67.31) (xy 176.53 67.31)))
  (wire (pts (xy 165.1 69.85) (xy 176.53 69.85)))
  (wire (pts (xy 165.1 72.39) (xy 176.53 72.39)))
  (wire (pts (xy 166.37 24.13) (xy 171.45 24.13)))
  (wire (pts (xy 166.37 26.67) (xy 166.37 24.13)))
  (wire (pts (xy 166.37 29.21) (xy 166.37 39.37)))
  (wire (pts (xy 166.37 39.37) (xy 165.1 39.37)))
  (wire (pts (xy 166.37 39.37) (xy 166.37 46.99)))
  (wire (pts (xy 166.37 46.99) (xy 165.1 46.99)))
  (wire (pts (xy 166.37 59.69) (xy 166.37 46.99)))
  (wire (pts (xy 166.37 64.77) (xy 166.37 59.69)))
  (wire (pts (xy 166.37 64.77) (xy 166.37 73.66)))
  (wire (pts (xy 168.91 207.01) (xy 173.99 207.01)))
  (wire (pts (xy 181.61 201.93) (xy 189.23 201.93)))
  (wire (pts (xy 183.388 137.922) (xy 174.498 137.922)))
  (wire (pts (xy 183.388 143.002) (xy 183.388 137.922)))
  (wire (pts (xy 183.388 148.082) (xy 183.388 153.162)))
  (wire (pts (xy 186.0042 130.429) (xy 191.008 130.429)))
  (wire (pts (xy 186.69 44.45) (xy 198.12 44.45)))
  (wire (pts (xy 189.23 196.85) (xy 194.31 196.85)))
  (wire (pts (xy 189.23 201.93) (xy 189.23 196.85)))
  (wire (pts (xy 191.008 121.412) (xy 187.198 121.412)))
  (wire (pts (xy 191.008 122.682) (xy 191.008 121.412)))
  (wire (pts (xy 191.008 130.302) (xy 191.008 130.429)))
  (wire (pts (xy 191.008 130.429) (xy 191.008 131.572)))
  (wire (pts (xy 191.008 139.192) (xy 191.008 145.542)))
  (wire (pts (xy 191.008 145.542) (xy 189.738 145.542)))
  (wire (pts (xy 194.31 191.77) (xy 194.31 196.85)))
  (wire (pts (xy 195.58 26.67) (xy 200.66 26.67)))
  (wire (pts (xy 196.85 54.61) (xy 200.66 54.61)))
  (wire (pts (xy 196.85 59.69) (xy 200.66 59.69)))
  (wire (pts (xy 196.85 62.23) (xy 200.66 62.23)))
  (wire (pts (xy 198.12 44.45) (xy 198.12 46.99)))
  (wire (pts (xy 198.12 44.45) (xy 200.66 44.45)))
  (wire (pts (xy 198.12 46.99) (xy 198.12 49.53)))
  (wire (pts (xy 198.12 46.99) (xy 200.66 46.99)))
  (wire (pts (xy 198.12 49.53) (xy 200.66 49.53)))
  (wire (pts (xy 199.39 34.29) (xy 199.39 41.91)))
  (wire (pts (xy 199.39 41.91) (xy 199.39 57.15)))
  (wire (pts (xy 199.39 57.15) (xy 199.39 64.77)))
  (wire (pts (xy 199.39 64.77) (xy 199.39 69.85)))
  (wire (pts (xy 199.39 69.85) (xy 199.39 73.66)))
  (wire (pts (xy 199.39 69.85) (xy 200.66 69.85)))
  (wire (pts (xy 200.66 29.21) (xy 200.66 26.67)))
  (wire (pts (xy 200.66 31.75) (xy 200.66 29.21)))
  (wire (pts (xy 200.66 34.29) (xy 199.39 34.29)))
  (wire (pts (xy 200.66 41.91) (xy 199.39 41.91)))
  (wire (pts (xy 200.66 57.15) (xy 199.39 57.15)))
  (wire (pts (xy 200.66 64.77) (xy 199.39 64.77)))
  (wire (pts (xy 213.36 154.94) (xy 229.87 154.94)))
  (wire (pts (xy 213.36 157.48) (xy 229.87 157.48)))
  (wire (pts (xy 213.36 162.56) (xy 229.87 162.56)))
  (wire (pts (xy 213.36 165.1) (xy 229.87 165.1)))
  (wire (pts (xy 213.36 170.18) (xy 229.87 170.18)))
  (wire (pts (xy 213.36 172.72) (xy 229.87 172.72)))
  (wire (pts (xy 213.36 177.8) (xy 229.87 177.8)))
  (wire (pts (xy 213.36 180.34) (xy 229.87 180.34)))
  (wire (pts (xy 213.36 193.04) (xy 229.87 193.04)))
  (wire (pts (xy 213.36 195.58) (xy 229.87 195.58)))
  (wire (pts (xy 213.36 208.28) (xy 229.87 208.28)))
  (wire (pts (xy 213.36 210.82) (xy 229.87 210.82)))
  (wire (pts (xy 213.36 223.52) (xy 229.87 223.52)))
  (wire (pts (xy 213.36 226.06) (xy 229.87 226.06)))
  (wire (pts (xy 213.36 231.14) (xy 229.87 231.14)))
  (wire (pts (xy 223.52 106.68) (xy 229.87 106.68)))
  (wire (pts (xy 223.52 116.84) (xy 229.87 116.84)))
  (wire (pts (xy 223.52 119.38) (xy 229.87 119.38)))
  (wire (pts (xy 223.52 132.08) (xy 229.87 132.08)))
  (wire (pts (xy 223.52 134.62) (xy 229.87 134.62)))
  (wire (pts (xy 227.33 114.3) (xy 227.33 121.92)))
  (wire (pts (xy 227.33 121.92) (xy 227.33 129.54)))
  (wire (pts (xy 227.33 121.92) (xy 229.87 121.92)))
  (wire (pts (xy 227.33 129.54) (xy 227.33 137.16)))
  (wire (pts (xy 227.33 129.54) (xy 229.87 129.54)))
  (wire (pts (xy 227.33 137.16) (xy 227.33 144.78)))
  (wire (pts (xy 227.33 137.16) (xy 229.87 137.16)))
  (wire (pts (xy 227.33 144.78) (xy 227.33 152.4)))
  (wire (pts (xy 227.33 144.78) (xy 229.87 144.78)))
  (wire (pts (xy 227.33 152.4) (xy 227.33 160.02)))
  (wire (pts (xy 227.33 152.4) (xy 229.87 152.4)))
  (wire (pts (xy 227.33 160.02) (xy 227.33 167.64)))
  (wire (pts (xy 227.33 160.02) (xy 229.87 160.02)))
  (wire (pts (xy 227.33 167.64) (xy 227.33 175.26)))
  (wire (pts (xy 227.33 167.64) (xy 229.87 167.64)))
  (wire (pts (xy 227.33 175.26) (xy 227.33 182.88)))
  (wire (pts (xy 227.33 175.26) (xy 229.87 175.26)))
  (wire (pts (xy 227.33 182.88) (xy 227.33 190.5)))
  (wire (pts (xy 227.33 182.88) (xy 229.87 182.88)))
  (wire (pts (xy 227.33 190.5) (xy 227.33 198.12)))
  (wire (pts (xy 227.33 190.5) (xy 229.87 190.5)))
  (wire (pts (xy 227.33 198.12) (xy 227.33 205.74)))
  (wire (pts (xy 227.33 198.12) (xy 229.87 198.12)))
  (wire (pts (xy 227.33 205.74) (xy 227.33 213.36)))
  (wire (pts (xy 227.33 205.74) (xy 229.87 205.74)))
  (wire (pts (xy 227.33 213.36) (xy 227.33 220.98)))
  (wire (pts (xy 227.33 213.36) (xy 229.87 213.36)))
  (wire (pts (xy 227.33 220.98) (xy 227.33 228.6)))
  (wire (pts (xy 227.33 228.6) (xy 227.33 237.49)))
  (wire (pts (xy 229.87 29.21) (xy 240.03 29.21)))
  (wire (pts (xy 229.87 31.75) (xy 229.87 29.21)))
  (wire (pts (xy 229.87 34.29) (xy 231.14 34.29)))
  (wire (pts (xy 229.87 36.83) (xy 233.68 36.83)))
  (wire (pts (xy 229.87 39.37) (xy 233.68 39.37)))
  (wire (pts (xy 229.87 44.45) (xy 233.68 44.45)))
  (wire (pts (xy 229.87 46.99) (xy 233.68 46.99)))
  (wire (pts (xy 229.87 49.53) (xy 233.68 49.53)))
  (wire (pts (xy 229.87 52.07) (xy 234.95 52.07)))
  (wire (pts (xy 229.87 54.61) (xy 231.14 54.61)))
  (wire (pts (xy 229.87 57.15) (xy 234.95 57.15)))
  (wire (pts (xy 229.87 59.69) (xy 234.95 59.69)))
  (wire (pts (xy 229.87 62.23) (xy 231.14 62.23)))
  (wire (pts (xy 229.87 64.77) (xy 234.95 64.77)))
  (wire (pts (xy 229.87 67.31) (xy 234.95 67.31)))
  (wire (pts (xy 229.87 114.3) (xy 227.33 114.3)))
  (wire (pts (xy 229.87 124.46) (xy 223.52 124.46)))
  (wire (pts (xy 229.87 127) (xy 223.52 127)))
  (wire (pts (xy 229.87 139.7) (xy 213.36 139.7)))
  (wire (pts (xy 229.87 142.24) (xy 213.36 142.24)))
  (wire (pts (xy 229.87 147.32) (xy 213.36 147.32)))
  (wire (pts (xy 229.87 149.86) (xy 213.36 149.86)))
  (wire (pts (xy 229.87 185.42) (xy 213.36 185.42)))
  (wire (pts (xy 229.87 187.96) (xy 213.36 187.96)))
  (wire (pts (xy 229.87 200.66) (xy 213.36 200.66)))
  (wire (pts (xy 229.87 203.2) (xy 213.36 203.2)))
  (wire (pts (xy 229.87 215.9) (xy 213.36 215.9)))
  (wire (pts (xy 229.87 218.44) (xy 213.36 218.44)))
  (wire (pts (xy 229.87 220.98) (xy 227.33 220.98)))
  (wire (pts (xy 229.87 228.6) (xy 227.33 228.6)))
  (wire (pts (xy 231.14 34.29) (xy 231.14 54.61)))
  (wire (pts (xy 231.14 54.61) (xy 231.14 62.23)))
  (wire (pts (xy 231.14 62.23) (xy 231.14 69.85)))
  (wire (pts (xy 231.14 69.85) (xy 229.87 69.85)))
  (wire (pts (xy 231.14 69.85) (xy 231.14 73.66)))
  (wire (pts (xy 233.68 36.83) (xy 233.68 39.37)))
  (wire (pts (xy 233.68 36.83) (xy 240.03 36.83)))
  (wire (pts (xy 233.68 39.37) (xy 233.68 44.45)))
  (wire (pts (xy 233.68 44.45) (xy 233.68 46.99)))
  (wire (pts (xy 233.68 49.53) (xy 233.68 46.99)))
  (wire (pts (xy 258.445 26.67) (xy 264.16 26.67)))
  (wire (pts (xy 259.08 30.48) (xy 274.32 30.48)))
  (wire (pts (xy 259.08 33.02) (xy 274.32 33.02)))
  (wire (pts (xy 261.62 22.86) (xy 274.32 22.86)))
  (wire (pts (xy 261.62 63.5) (xy 265.43 63.5)))
  (wire (pts (xy 261.62 71.12) (xy 261.62 78.74)))
  (wire (pts (xy 261.62 78.74) (xy 273.05 78.74)))
  (wire (pts (xy 264.16 26.67) (xy 264.16 36.83)))
  (wire (pts (xy 264.16 26.67) (xy 271.145 26.67)))
  (wire (pts (xy 271.145 21.59) (xy 271.145 26.67)))
  (wire (pts (xy 271.145 26.67) (xy 274.32 26.67)))
  (wire (pts (xy 273.05 78.74) (xy 278.13 78.74)))
  (wire (pts (xy 274.32 24.13) (xy 274.32 22.86)))
  (wire (pts (xy 274.32 36.83) (xy 274.32 39.37)))
  (wire (pts (xy 274.32 39.37) (xy 274.32 43.18)))
  (wire (pts (xy 278.13 78.74) (xy 285.75 78.74)))
  (wire (pts (xy 285.75 76.2) (xy 285.75 73.66)))
  (wire (pts (xy 290.83 109.22) (xy 297.18 109.22)))
  (wire (pts (xy 290.83 111.76) (xy 297.18 111.76)))
  (wire (pts (xy 290.83 116.84) (xy 297.18 116.84)))
  (wire (pts (xy 290.83 119.38) (xy 297.18 119.38)))
  (wire (pts (xy 290.83 121.92) (xy 293.37 121.92)))
  (wire (pts (xy 290.83 129.54) (xy 293.37 129.54)))
  (wire (pts (xy 290.83 137.16) (xy 293.37 137.16)))
  (wire (pts (xy 290.83 139.7) (xy 307.34 139.7)))
  (wire (pts (xy 290.83 142.24) (xy 307.34 142.24)))
  (wire (pts (xy 290.83 144.78) (xy 293.37 144.78)))
  (wire (pts (xy 290.83 147.32) (xy 307.34 147.32)))
  (wire (pts (xy 290.83 149.86) (xy 307.34 149.86)))
  (wire (pts (xy 290.83 152.4) (xy 293.37 152.4)))
  (wire (pts (xy 290.83 160.02) (xy 307.34 160.02)))
  (wire (pts (xy 290.83 162.56) (xy 307.34 162.56)))
  (wire (pts (xy 290.83 165.1) (xy 307.34 165.1)))
  (wire (pts (xy 290.83 167.64) (xy 307.34 167.64)))
  (wire (pts (xy 290.83 170.18) (xy 307.34 170.18)))
  (wire (pts (xy 290.83 172.72) (xy 307.34 172.72)))
  (wire (pts (xy 290.83 175.26) (xy 293.37 175.26)))
  (wire (pts (xy 290.83 182.88) (xy 293.37 182.88)))
  (wire (pts (xy 290.83 185.42) (xy 307.34 185.42)))
  (wire (pts (xy 290.83 187.96) (xy 307.34 187.96)))
  (wire (pts (xy 290.83 190.5) (xy 293.37 190.5)))
  (wire (pts (xy 290.83 193.04) (xy 307.34 193.04)))
  (wire (pts (xy 290.83 195.58) (xy 307.34 195.58)))
  (wire (pts (xy 290.83 198.12) (xy 293.37 198.12)))
  (wire (pts (xy 290.83 205.74) (xy 293.37 205.74)))
  (wire (pts (xy 290.83 213.36) (xy 293.37 213.36)))
  (wire (pts (xy 290.83 215.9) (xy 307.34 215.9)))
  (wire (pts (xy 290.83 218.44) (xy 307.34 218.44)))
  (wire (pts (xy 290.83 220.98) (xy 293.37 220.98)))
  (wire (pts (xy 290.83 223.52) (xy 307.34 223.52)))
  (wire (pts (xy 290.83 226.06) (xy 307.34 226.06)))
  (wire (pts (xy 290.83 228.6) (xy 293.37 228.6)))
  (wire (pts (xy 290.83 231.14) (xy 307.34 231.14)))
  (wire (pts (xy 293.37 68.58) (xy 298.45 68.58)))
  (wire (pts (xy 293.37 76.2) (xy 285.75 76.2)))
  (wire (pts (xy 293.37 76.2) (xy 293.37 78.74)))
  (wire (pts (xy 293.37 114.3) (xy 290.83 114.3)))
  (wire (pts (xy 293.37 121.92) (xy 293.37 114.3)))
  (wire (pts (xy 293.37 129.54) (xy 293.37 121.92)))
  (wire (pts (xy 293.37 137.16) (xy 293.37 129.54)))
  (wire (pts (xy 293.37 144.78) (xy 293.37 137.16)))
  (wire (pts (xy 293.37 152.4) (xy 293.37 144.78)))
  (wire (pts (xy 293.37 152.4) (xy 293.37 175.26)))
  (wire (pts (xy 293.37 175.26) (xy 293.37 182.88)))
  (wire (pts (xy 293.37 182.88) (xy 293.37 190.5)))
  (wire (pts (xy 293.37 190.5) (xy 293.37 198.12)))
  (wire (pts (xy 293.37 198.12) (xy 293.37 205.74)))
  (wire (pts (xy 293.37 205.74) (xy 293.37 213.36)))
  (wire (pts (xy 293.37 213.36) (xy 293.37 220.98)))
  (wire (pts (xy 293.37 220.98) (xy 293.37 228.6)))
  (wire (pts (xy 293.37 228.6) (xy 293.37 237.49)))
  (wire (pts (xy 294.64 24.13) (xy 302.895 24.13)))
  (wire (pts (xy 294.64 26.67) (xy 302.895 26.67)))
  (wire (pts (xy 294.64 36.83) (xy 305.435 36.83)))
  (wire (pts (xy 294.64 39.37) (xy 305.435 39.37)))
  (wire (pts (xy 297.18 106.68) (xy 290.83 106.68)))
  (wire (pts (xy 298.45 63.5) (xy 298.45 68.58)))
  (wire (pts (xy 307.34 124.46) (xy 290.83 124.46)))
  (wire (pts (xy 307.34 127) (xy 290.83 127)))
  (wire (pts (xy 307.34 132.08) (xy 290.83 132.08)))
  (wire (pts (xy 307.34 134.62) (xy 290.83 134.62)))
  (wire (pts (xy 307.34 154.94) (xy 290.83 154.94)))
  (wire (pts (xy 307.34 157.48) (xy 290.83 157.48)))
  (wire (pts (xy 307.34 177.8) (xy 290.83 177.8)))
  (wire (pts (xy 307.34 180.34) (xy 290.83 180.34)))
  (wire (pts (xy 307.34 200.66) (xy 290.83 200.66)))
  (wire (pts (xy 307.34 203.2) (xy 290.83 203.2)))
  (wire (pts (xy 307.34 208.28) (xy 290.83 208.28)))
  (wire (pts (xy 307.34 210.82) (xy 290.83 210.82)))
  (wire (pts (xy 313.055 46.99) (xy 315.595 46.99)))
  (wire (pts (xy 316.23 166.37) (xy 332.74 166.37)))
  (wire (pts (xy 316.23 168.91) (xy 332.74 168.91)))
  (wire (pts (xy 316.23 171.45) (xy 332.74 171.45)))
  (wire (pts (xy 316.23 173.99) (xy 332.74 173.99)))
  (wire (pts (xy 316.23 176.53) (xy 332.74 176.53)))
  (wire (pts (xy 316.23 179.07) (xy 332.74 179.07)))
  (wire (pts (xy 316.23 181.61) (xy 332.74 181.61)))
  (wire (pts (xy 316.23 184.15) (xy 332.74 184.15)))
  (wire (pts (xy 316.23 189.23) (xy 332.74 189.23)))
  (wire (pts (xy 316.23 194.31) (xy 332.74 194.31)))
  (wire (pts (xy 316.23 196.85) (xy 332.74 196.85)))
  (wire (pts (xy 316.23 204.47) (xy 332.74 204.47)))
  (wire (pts (xy 320.04 124.46) (xy 323.85 124.46)))
  (wire (pts (xy 323.85 107.95) (xy 323.85 116.84)))
  (wire (pts (xy 323.85 107.95) (xy 340.36 107.95)))
  (wire (pts (xy 323.85 124.46) (xy 331.47 124.46)))
  (wire (pts (xy 325.12 102.87) (xy 325.12 104.14)))
  (wire (pts (xy 327.66 102.87) (xy 325.12 102.87)))
  (wire (pts (xy 328.93 130.81) (xy 340.36 130.81)))
  (wire (pts (xy 328.93 135.89) (xy 328.93 130.81)))
  (wire (pts (xy 328.93 143.51) (xy 328.93 146.05)))
  (wire (pts (xy 330.2 36.83) (xy 332.74 36.83)))
  (wire (pts (xy 330.2 95.25) (xy 340.36 95.25)))
  (wire (pts (xy 331.47 110.49) (xy 331.47 116.84)))
  (wire (pts (xy 331.47 125.73) (xy 331.47 124.46)))
  (wire (pts (xy 331.47 128.27) (xy 331.47 125.73)))
  (wire (pts (xy 332.74 62.23) (xy 335.28 62.23)))
  (wire (pts (xy 332.74 125.73) (xy 331.47 125.73)))
  (wire (pts (xy 332.74 128.27) (xy 331.47 128.27)))
  (wire (pts (xy 334.01 156.21) (xy 342.9 156.21)))
  (wire (pts (xy 335.28 102.87) (xy 340.36 102.87)))
  (wire (pts (xy 336.55 133.35) (xy 340.36 133.35)))
  (wire (pts (xy 336.55 135.89) (xy 336.55 133.35)))
  (wire (pts (xy 336.55 143.51) (xy 336.55 146.05)))
  (wire (pts (xy 337.82 214.63) (xy 337.82 217.17)))
  (wire (pts (xy 337.82 214.63) (xy 340.36 214.63)))
  (wire (pts (xy 339.09 67.31) (xy 360.68 67.31)))
  (wire (pts (xy 339.09 82.55) (xy 339.09 67.31)))
  (wire (pts (xy 340.36 82.55) (xy 339.09 82.55)))
  (wire (pts (xy 340.36 110.49) (xy 331.47 110.49)))
  (wire (pts (xy 340.36 214.63) (xy 342.9 214.63)))
  (wire (pts (xy 342.9 156.21) (xy 342.9 158.75)))
  (wire (pts (xy 342.9 214.63) (xy 345.44 214.63)))
  (wire (pts (xy 345.44 214.63) (xy 347.98 214.63)))
  (wire (pts (xy 347.98 214.63) (xy 350.52 214.63)))
  (wire (pts (xy 356.87 36.83) (xy 359.41 36.83)))
  (wire (pts (xy 359.41 62.23) (xy 361.95 62.23)))
  (wire (pts (xy 360.68 67.31) (xy 363.22 67.31)))
  (wire (pts (xy 363.22 67.31) (xy 365.76 67.31)))
  (wire (pts (xy 364.49 162.56) (xy 381 162.56)))
  (wire (pts (xy 364.49 165.1) (xy 381 165.1)))
  (wire (pts (xy 364.49 167.64) (xy 381 167.64)))
  (wire (pts (xy 364.49 170.18) (xy 381 170.18)))
  (wire (pts (xy 364.49 172.72) (xy 381 172.72)))
  (wire (pts (xy 364.49 175.26) (xy 381 175.26)))
  (wire (pts (xy 364.49 177.8) (xy 381 177.8)))
  (wire (pts (xy 364.49 180.34) (xy 381 180.34)))
  (wire (pts (xy 364.49 185.42) (xy 381 185.42)))
  (wire (pts (xy 364.49 190.5) (xy 381 190.5)))
  (wire (pts (xy 364.49 193.04) (xy 381 193.04)))
  (wire (pts (xy 364.49 200.66) (xy 381 200.66)))
  (wire (pts (xy 365.76 67.31) (xy 368.3 67.31)))
  (wire (pts (xy 368.3 67.31) (xy 373.38 67.31)))
  (wire (pts (xy 368.3 143.51) (xy 368.3 146.05)))
  (wire (pts (xy 373.38 67.31) (xy 375.92 67.31)))
  (wire (pts (xy 382.27 152.4) (xy 391.16 152.4)))
  (wire (pts (xy 386.08 210.82) (xy 386.08 213.36)))
  (wire (pts (xy 386.08 210.82) (xy 388.62 210.82)))
  (wire (pts (xy 388.62 210.82) (xy 391.16 210.82)))
  (wire (pts (xy 391.16 152.4) (xy 391.16 154.94)))
  (wire (pts (xy 391.16 210.82) (xy 393.7 210.82)))
  (wire (pts (xy 393.7 210.82) (xy 396.24 210.82)))
  (wire (pts (xy 396.24 82.55) (xy 405.13 82.55)))
  (wire (pts (xy 396.24 85.09) (xy 405.13 85.09)))
  (wire (pts (xy 396.24 87.63) (xy 405.13 87.63)))
  (wire (pts (xy 396.24 95.25) (xy 405.13 95.25)))
  (wire (pts (xy 396.24 97.79) (xy 405.13 97.79)))
  (wire (pts (xy 396.24 107.95) (xy 405.13 107.95)))
  (wire (pts (xy 396.24 110.49) (xy 405.13 110.49)))
  (wire (pts (xy 396.24 120.65) (xy 405.13 120.65)))
  (wire (pts (xy 396.24 123.19) (xy 405.13 123.19)))
  (wire (pts (xy 396.24 210.82) (xy 398.78 210.82)))
  (polyline (pts (xy 16.51 219.71) (xy 93.98 219.71)))
  (polyline (pts (xy 16.51 281.94) (xy 16.51 219.71)))
  (polyline (pts (xy 93.98 219.71) (xy 93.98 281.94)))
  (polyline (pts (xy 93.98 281.94) (xy 16.51 281.94)))
  (polyline (pts (xy 138.43 13.97) (xy 138.43 80.01)))
  (polyline (pts (xy 138.43 80.01) (xy 179.07 80.01)))
  (polyline (pts (xy 179.07 13.97) (xy 138.43 13.97)))
  (polyline (pts (xy 179.07 13.97) (xy 179.07 80.01)))
  (polyline (pts (xy 179.07 13.97) (xy 248.92 13.97)))
  (polyline (pts (xy 179.07 88.9) (xy 179.07 13.97)))
  (polyline (pts (xy 248.92 13.97) (xy 248.92 88.9)))
  (polyline (pts (xy 248.92 88.9) (xy 179.07 88.9)))
  (text "CM4Lite SDCARD I/F" (at 21.59 226.06 0))
  (text "Activity LED" (at 121.92 40.64 0))
  (text "Force RPIBOOT = Jumper Pins 1-2 \n" (at 133.858 165.608 180))
  (text "EEPROM write protect = Jumper Pins 3-4\n\n" (at 139.7 170.18 180))
  (text "40Way GPIO Header" (at 143.51 19.05 0))
  (text "maximum +12v @0.6A or +3.3v@3A , 10Watts combined" (at 189.23 83.82 0))
  (text "PWR LED" (at 193.675 123.825 0))
  (text "TX and RX have PN swaps to improve routing\n" (at 194.31 87.63 0))
  (text "PCIe x1 connector" (at 222.25 19.05 180))
  (label "+5v" (at 16.51 162.56 0))
  (label "RUN_PG" (at 20.066 170.18 180))
  (label "+3.3v" (at 21.59 199.39 0))
  (label "SCL0" (at 25.146 118.11 180))
  (label "SDA0" (at 25.146 120.65 180))
  (label "nEXTRST" (at 25.146 143.51 180))
  (label "+3.3v" (at 25.4 237.49 180))
  (label "GPIO_VREF" (at 26.67 115.57 0))
  (label "TRD1_P" (at 30.226 21.59 180))
  (label "TRD1_N" (at 30.226 24.13 180))
  (label "TRD0_N" (at 30.226 29.21 180))
  (label "TRD0_P" (at 30.226 31.75 180))
  (label "+3.3v" (at 30.48 255.27 180))
  (label "SYNC_IN" (at 31.496 36.83 180))
  (label "GPIO6" (at 31.496 54.61 180))
  (label "GPIO5" (at 31.496 59.69 180))
  (label "ID_SD" (at 31.496 62.23 180))
  (label "GPIO9" (at 31.496 67.31 180))
  (label "GPIO4" (at 31.496 85.09 180))
  (label "GPIO3" (at 31.496 87.63 180))
  (label "GPIO2" (at 31.496 90.17 180))
  (label "AIN1" (at 31.75 135.89 180))
  (label "AIN0" (at 31.75 138.43 180))
  (label "SD_DET" (at 31.75 262.89 180))
  (label "GPIO26" (at 32.766 46.99 180))
  (label "GPIO19" (at 32.766 49.53 180))
  (label "GPIO13" (at 32.766 52.07 180))
  (label "GPIO11" (at 32.766 64.77 180))
  (label "GPIO10" (at 32.766 72.39 180))
  (label "GPIO22" (at 32.766 74.93 180))
  (label "GPIO27" (at 32.766 77.47 180))
  (label "GPIO17" (at 32.766 80.01 180))
  (label "SD_CMD" (at 32.766 95.25 180))
  (label "SYNC_OUT" (at 33.02 39.37 180))
  (label "+3.3v" (at 33.02 123.19 180))
  (label "+1.8v" (at 33.02 128.27 180))
  (label "SD_DAT2" (at 34.29 234.95 0))
  (label "SD_DAT3" (at 34.29 237.49 0))
  (label "SD_CMD" (at 34.29 240.03 0))
  (label "SD_CLK" (at 34.29 245.11 0))
  (label "SD_DAT0" (at 34.29 250.19 0))
  (label "SD_DAT1" (at 34.29 252.73 0))
  (label "SD_DET" (at 34.671 113.03 180))
  (label "RUN_PG" (at 35.56 133.35 180))
  (label "EEPROM_nWP" (at 36.068 41.91 180))
  (label "+5v" (at 44.45 181.61 0))
  (label "GND" (at 61.214 154.94 180))
  (label "GND" (at 61.214 157.48 180))
  (label "AIN0" (at 61.214 160.02 180))
  (label "GND" (at 61.214 162.56 180))
  (label "TV_OUT" (at 63.246 167.64 180))
  (label "SYNC_OUT" (at 65.786 165.1 180))
  (label "GND" (at 83.566 165.1 180))
  (label "GND" (at 83.566 167.64 180))
  (label "AIN1" (at 84.074 160.02 180))
  (label "SYNC_IN" (at 87.63 162.56 180))
  (label "nRPIBOOT" (at 88.9 154.94 180))
  (label "GLOBAL_EN" (at 90.17 170.18 180))
  (label "EEPROM_nWP" (at 92.202 157.48 180))
  (label "CAM1_D0_N" (at 101.6 226.06 0))
  (label "CAM1_D0_P" (at 101.6 228.6 0))
  (label "CAM1_D1_N" (at 101.6 233.68 0))
  (label "CAM1_D1_P" (at 101.6 236.22 0))
  (label "CAM1_C_N" (at 101.6 241.3 0))
  (label "CAM1_C_P" (at 101.6 243.84 0))
  (label "CAM1_D2_N" (at 101.6 248.92 0))
  (label "CAM1_D2_P" (at 101.6 251.46 0))
  (label "CAM1_D3_N" (at 101.6 256.54 0))
  (label "CAM1_D3_P" (at 101.6 259.08 0))
  (label "CAM_GPIO" (at 101.6 264.16 0))
  (label "SCL0" (at 101.6 271.78 0))
  (label "SDA0" (at 101.6 274.32 0))
  (label "+3.3v" (at 101.6 276.86 0))
  (label "SD_PWR_ON" (at 102.616 113.03 0))
  (label "TRD3_P" (at 102.87 21.59 0))
  (label "TRD3_N" (at 102.87 24.13 0))
  (label "TRD2_N" (at 102.87 29.21 0))
  (label "TRD2_P" (at 102.87 31.75 0))
  (label "ETH_LEDG" (at 102.87 36.83 0))
  (label "ETH_LEDY" (at 102.87 39.37 0))
  (label "nPWR_LED" (at 105.156 138.43 0))
  (label "+5v" (at 106.426 115.57 180))
  (label "ID_SC" (at 108.966 62.23 180))
  (label "GPIO7" (at 108.966 64.77 180))
  (label "GPIO8" (at 108.966 67.31 180))
  (label "GPIO21" (at 110.236 49.53 180))
  (label "GPIO20" (at 110.236 52.07 180))
  (label "GPIO16" (at 110.236 54.61 180))
  (label "GPIO12" (at 110.236 57.15 180))
  (label "GPIO25" (at 110.236 69.85 180))
  (label "GPIO24" (at 110.236 74.93 180))
  (label "GPIO23" (at 110.236 77.47 180))
  (label "GPIO18" (at 110.236 80.01 180))
  (label "GPIO15" (at 110.236 82.55 180))
  (label "GPIO14" (at 110.236 87.63 180))
  (label "SD_CLK" (at 110.236 90.17 180))
  (label "SD_DAT3" (at 111.506 95.25 180))
  (label "SD_DAT0" (at 111.506 97.79 180))
  (label "SD_DAT1" (at 111.506 102.87 180))
  (label "SD_DAT2" (at 111.506 105.41 180))
  (label "BT_nDis" (at 112.6236 133.35 180))
  (label "WL_nDis" (at 113.411 128.27 180))
  (label "GLOBAL_EN" (at 114.046 143.51 180))
  (label "nRPIBOOT" (at 114.5032 135.89 180))
  (label "+3.3v" (at 125.73 44.45 0))
  (label "DSI1_D0_N" (at 132.08 226.06 0))
  (label "DSI1_D0_P" (at 132.08 228.6 0))
  (label "DSI1_D1_N" (at 132.08 233.68 0))
  (label "DSI1_D1_P" (at 132.08 236.22 0))
  (label "DSI1_C_N" (at 132.08 241.3 0))
  (label "DSI1_C_P" (at 132.08 243.84 0))
  (label "DSI1_D2_N" (at 132.08 248.92 0))
  (label "DSI1_D2_P" (at 132.08 251.46 0))
  (label "DSI1_D3_N" (at 132.08 256.54 0))
  (label "DSI1_D3_P" (at 132.08 259.08 0))
  (label "SCL0" (at 132.08 271.78 0))
  (label "SDA0" (at 132.08 274.32 0))
  (label "+3.3v" (at 132.08 276.86 0))
  (label "ETH_LEDY" (at 139.7 101.6 180))
  (label "ETH_LEDG" (at 139.7 106.68 180))
  (label "GPIO2" (at 147.32 26.67 180))
  (label "GPIO3" (at 147.32 29.21 180))
  (label "GPIO4" (at 147.32 31.75 180))
  (label "GPIO9" (at 147.32 49.53 180))
  (label "ID_SD" (at 147.32 57.15 180))
  (label "GPIO5" (at 147.32 59.69 180))
  (label "GPIO6" (at 147.32 62.23 180))
  (label "+3.3v" (at 148.59 24.13 180))
  (label "GPIO17" (at 148.59 36.83 180))
  (label "GPIO27" (at 148.59 39.37 180))
  (label "GPIO22" (at 148.59 41.91 180))
  (label "GPIO10" (at 148.59 46.99 180))
  (label "GPIO11" (at 148.59 52.07 180))
  (label "GPIO13" (at 148.59 64.77 180))
  (label "GPIO19" (at 148.59 67.31 180))
  (label "GPIO26" (at 148.59 69.85 180))
  (label "+12v" (at 152.4 146.05 180))
  (label "+5v" (at 152.4 148.59 180))
  (label "TRD0_P" (at 152.4 153.67 180))
  (label "TRD0_N" (at 152.4 156.21 180))
  (label "TRD1_N" (at 152.4 158.75 180))
  (label "TRD1_P" (at 152.4 161.29 180))
  (label "TRD3_P" (at 152.4 163.83 180))
  (label "TRD3_N" (at 152.4 166.37 180))
  (label "TRD2_N" (at 152.4 168.91 180))
  (label "TRD2_P" (at 152.4 171.45 180))
  (label "+3.3v" (at 156.21 101.6 0))
  (label "+12v" (at 157.48 191.77 180))
  (label "nPWR_LED" (at 164.338 145.542 0))
  (label "+5v" (at 170.18 24.13 180))
  (label "GPIO8" (at 173.99 52.07 180))
  (label "GPIO7" (at 173.99 54.61 180))
  (label "ID_SC" (at 173.99 57.15 180))
  (label "GPIO14" (at 175.26 31.75 180))
  (label "GPIO15" (at 175.26 34.29 180))
  (label "GPIO18" (at 175.26 36.83 180))
  (label "GPIO23" (at 175.26 41.91 180))
  (label "GPIO24" (at 175.26 44.45 180))
  (label "GPIO25" (at 175.26 49.53 180))
  (label "GPIO12" (at 175.26 62.23 180))
  (label "GPIO16" (at 175.26 67.31 180))
  (label "GPIO20" (at 175.26 69.85 180))
  (label "GPIO21" (at 175.26 72.39 180))
  (label "+3.3v" (at 179.578 137.922 180))
  (label "pcie+3.3v" (at 186.69 44.45 0))
  (label "+3.3v" (at 191.008 121.412 180))
  (label "+5v" (at 194.31 191.77 0))
  (label "+12v" (at 195.58 26.67 0))
  (label "PCIE_CLK_nREQ" (at 196.85 54.61 180))
  (label "PCIE_TX_N" (at 196.85 59.69 180))
  (label "PCIE_TX_P" (at 196.85 62.23 180))
  (label "CAM0_C_N" (at 213.36 154.94 0))
  (label "CAM0_C_P" (at 213.36 157.48 0))
  (label "HDMI1_D2_P" (at 213.36 162.56 0))
  (label "HDMI1_D2_N" (at 213.36 165.1 0))
  (label "HDMI1_D1_P" (at 213.36 170.18 0))
  (label "HDMI1_D1_N" (at 213.36 172.72 0))
  (label "HDMI1_D0_P" (at 213.36 177.8 0))
  (label "HDMI1_D0_N" (at 213.36 180.34 0))
  (label "HDMI0_D2_P" (at 213.36 193.04 0))
  (label "HDMI0_D2_N" (at 213.36 195.58 0))
  (label "HDMI0_D0_P" (at 213.36 208.28 0))
  (label "HDMI0_D0_N" (at 213.36 210.82 0))
  (label "DSI1_D3_N" (at 213.36 223.52 0))
  (label "DSI1_D3_P" (at 213.36 226.06 0))
  (label "HDMI0_SCL" (at 213.36 231.14 0))
  (label "PCIE_CLK_nREQ" (at 223.52 106.68 180))
  (label "PCIE_CLK_P" (at 223.52 116.84 180))
  (label "PCIE_CLK_N" (at 223.52 119.38 180))
  (label "PCIE_RX_P" (at 223.52 124.46 180))
  (label "PCIE_RX_N" (at 223.52 127 180))
  (label "PCIE_TX_P" (at 223.52 132.08 180))
  (label "PCIE_TX_N" (at 223.52 134.62 180))
  (label "CAM0_D0_N" (at 224.79 139.7 180))
  (label "CAM0_D0_P" (at 224.79 142.24 180))
  (label "CAM0_D1_N" (at 224.79 147.32 180))
  (label "CAM0_D1_P" (at 224.79 149.86 180))
  (label "HDMI0_D1_P" (at 224.79 200.66 180))
  (label "HDMI0_D1_N" (at 224.79 203.2 180))
  (label "HDMI0_CK_P" (at 224.79 215.9 180))
  (label "HDMI0_CK_N" (at 224.79 218.44 180))
  (label "HDMI1_CK_P" (at 225.425 185.42 180))
  (label "HDMI1_CK_N" (at 225.425 187.96 180))
  (label "+12v" (at 234.95 29.21 0))
  (label "pcie+3.3v" (at 234.95 36.83 0))
  (label "PCIE_nRST" (at 234.95 52.07 0))
  (label "PCIE_CLK_P" (at 234.95 57.15 0))
  (label "PCIE_CLK_N" (at 234.95 59.69 0))
  (label "PCIE_RX_N" (at 234.95 64.77 0))
  (label "PCIE_RX_P" (at 234.95 67.31 0))
  (label "USBOTG" (at 258.445 26.67 180))
  (label "USB2_P" (at 259.08 30.48 180))
  (label "USB2_N" (at 259.08 33.02 180))
  (label "+5v" (at 261.62 63.5 180))
  (label "+3.3v" (at 262.89 22.86 0))
  (label "VBUS_OTG" (at 271.145 13.97 180))
  (label "CAM1_C_N" (at 294.64 139.7 0))
  (label "CAM1_C_P" (at 294.64 142.24 0))
  (label "CAM1_D2_N" (at 294.64 147.32 0))
  (label "CAM1_D2_P" (at 294.64 149.86 0))
  (label "HDMI1_HOTPLUG" (at 294.64 160.02 0))
  (label "HDMI1_SDA" (at 294.64 162.56 0))
  (label "HDMI1_SCL" (at 294.64 165.1 0))
  (label "HDMI1_CEC" (at 294.64 167.64 0))
  (label "HDMI0_CEC" (at 294.64 170.18 0))
  (label "HDMI0_HOTPLUG" (at 294.64 172.72 0))
  (label "DSI0_D1_N" (at 294.64 185.42 0))
  (label "DSI0_D1_P" (at 294.64 187.96 0))
  (label "DSI0_C_N" (at 294.64 193.04 0))
  (label "DSI0_C_P" (at 294.64 195.58 0))
  (label "DSI1_C_N" (at 294.64 215.9 0))
  (label "DSI1_C_P" (at 294.64 218.44 0))
  (label "DSI1_D2_N" (at 294.64 223.52 0))
  (label "DSI1_D2_P" (at 294.64 226.06 0))
  (label "HDMI0_SDA" (at 294.64 231.14 0))
  (label "USBD_P" (at 295.275 36.83 0))
  (label "USBD_N" (at 295.275 39.37 0))
  (label "USBOTG" (at 297.18 106.68 0))
  (label "USB2_N" (at 297.18 109.22 0))
  (label "USB2_P" (at 297.18 111.76 0))
  (label "PCIE_nRST" (at 297.18 116.84 0))
  (label "TV_OUT" (at 297.18 119.38 0))
  (label "pcie+3.3v" (at 298.45 63.5 0))
  (label "USBH_P" (at 302.895 24.13 180))
  (label "USBH_N" (at 302.895 26.67 180))
  (label "DSI0_D0_N" (at 304.8 177.8 180))
  (label "DSI0_D0_P" (at 304.8 180.34 180))
  (label "DSI1_D0_N" (at 304.8 200.66 180))
  (label "DSI1_D0_P" (at 304.8 203.2 180))
  (label "DSI1_D1_N" (at 304.8 208.28 180))
  (label "DSI1_D1_P" (at 304.8 210.82 180))
  (label "VBUS_OTG" (at 305.435 31.75 180))
  (label "CAM1_D0_N" (at 305.435 124.46 180))
  (label "CAM1_D0_P" (at 305.435 127 180))
  (label "CAM1_D1_N" (at 305.435 132.08 180))
  (label "CAM1_D1_P" (at 305.435 134.62 180))
  (label "CAM1_D3_N" (at 305.435 154.94 180))
  (label "CAM1_D3_P" (at 305.435 157.48 180))
  (label "HDMI1_D2_P" (at 316.23 166.37 0))
  (label "HDMI1_D2_N" (at 316.23 168.91 0))
  (label "HDMI1_D1_P" (at 316.23 171.45 0))
  (label "HDMI1_D1_N" (at 316.23 173.99 0))
  (label "HDMI1_D0_P" (at 316.23 176.53 0))
  (label "HDMI1_D0_N" (at 316.23 179.07 0))
  (label "HDMI1_CK_P" (at 316.23 181.61 0))
  (label "HDMI1_CK_N" (at 316.23 184.15 0))
  (label "HDMI1_CEC" (at 316.23 189.23 0))
  (label "HDMI1_SCL" (at 316.23 194.31 0))
  (label "HDMI1_SDA" (at 316.23 196.85 0))
  (label "HDMI1_HOTPLUG" (at 316.23 204.47 0))
  (label "nEXTRST" (at 330.2 95.25 0))
  (label "+5v" (at 335.28 156.21 0))
  (label "VBUS" (at 340.36 21.59 0))
  (label "HD3_P" (at 340.36 26.67 0))
  (label "HD3_N" (at 340.36 29.21 0))
  (label "USBH_N" (at 340.36 87.63 180))
  (label "USBH_P" (at 340.36 90.17 180))
  (label "VBUS" (at 342.9 46.99 0))
  (label "HD4_P" (at 342.9 52.07 0))
  (label "HD4_N" (at 342.9 54.61 0))
  (label "+3.3v" (at 353.314 67.31 0))
  (label "HDMI0_D2_P" (at 364.49 162.56 0))
  (label "HDMI0_D2_N" (at 364.49 165.1 0))
  (label "HDMI0_D1_P" (at 364.49 167.64 0))
  (label "HDMI0_D1_N" (at 364.49 170.18 0))
  (label "HDMI0_D0_P" (at 364.49 172.72 0))
  (label "HDMI0_D0_N" (at 364.49 175.26 0))
  (label "HDMI0_CK_P" (at 364.49 177.8 0))
  (label "HDMI0_CK_N" (at 364.49 180.34 0))
  (label "HDMI0_CEC" (at 364.49 185.42 0))
  (label "HDMI0_SCL" (at 364.49 190.5 0))
  (label "HDMI0_SDA" (at 364.49 193.04 0))
  (label "HDMI0_HOTPLUG" (at 364.49 200.66 0))
  (label "VBUS" (at 367.03 21.59 0))
  (label "HD2_P" (at 367.03 26.67 0))
  (label "HD2_N" (at 367.03 29.21 0))
  (label "VBUS" (at 369.57 46.99 0))
  (label "HD1_P" (at 369.57 52.07 0))
  (label "HD1_N" (at 369.57 54.61 0))
  (label "+5v" (at 374.65 21.59 0))
  (label "+5v" (at 383.54 152.4 0))
  (label "HD1_N" (at 400.05 82.55 0))
  (label "HD1_P" (at 400.05 85.09 0))
  (label "HD2_N" (at 400.05 95.25 0))
  (label "HD2_P" (at 400.05 97.79 0))
  (label "HD3_N" (at 400.05 107.95 0))
  (label "HD3_P" (at 400.05 110.49 0))
  (label "HD4_N" (at 400.05 120.65 0))
  (label "HD4_P" (at 400.05 123.19 0))
  (label "PWR1" (at 405.13 87.63 180))
  (hierarchical_label "P1_P" (shape input) (at 23.876 21.59 180))
  (hierarchical_label "P1_N" (shape input) (at 23.876 24.13 180))
  (hierarchical_label "P0_N" (shape input) (at 23.876 29.21 180))
  (hierarchical_label "P0_P" (shape input) (at 23.876 31.75 180))
  (hierarchical_label "P3_P" (shape input) (at 113.03 21.59 0))
  (hierarchical_label "P3_N" (shape input) (at 113.03 24.13 0))
  (hierarchical_label "P2_N" (shape input) (at 113.03 29.21 0))
  (hierarchical_label "P2_P" (shape input) (at 113.03 31.75 0))
  (symbol (lib_id "Connector:TestPoint") (at 110.49 44.45 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "TP5" (id 0) (at 111.76 40.64 0))
    (property "Value" "TestPoint" (id 1) (at 111.125 41.91 0))
    (property "Footprint" "TestPoint:TestPoint_Pad_2.0x2.0mm" (id 2) (at 115.57 44.45 0))
    (property "Datasheet" "" (id 3) (at 115.57 44.45 0))
    (property "Field4" "nf" (id 4) (at 110.49 44.45 0))
    (property "Field5" "nf" (id 5) (at 110.49 44.45 0))
    (property "Field6" "nf" (id 6) (at 110.49 44.45 0))
    (property "Field7" "nf" (id 7) (at 110.49 44.45 0))
  )
  (symbol (lib_id "Connector:TestPoint") (at 186.0042 130.429 90) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "TP6" (id 0) (at 183.642 127.762 90))
    (property "Value" "TestPoint" (id 1) (at 188.722 132.842 90))
    (property "Footprint" "TestPoint:TestPoint_Pad_2.0x2.0mm" (id 2) (at 186.0042 125.349 0))
    (property "Datasheet" "" (id 3) (at 186.0042 125.349 0))
    (property "Field4" "nf" (id 4) (at 186.0042 130.429 0))
    (property "Field5" "nf" (id 5) (at 186.0042 130.429 0))
    (property "Field6" "nf" (id 6) (at 186.0042 130.429 0))
    (property "Field7" "nf" (id 7) (at 186.0042 130.429 0))
  )
  (symbol (lib_id "power:GND") (at 21.59 248.92 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR061" (id 0) (at 21.59 255.27 0))
    (property "Value" "GND" (id 1) (at 21.717 253.3142 0))
    (property "Footprint" "" (id 2) (at 21.59 248.92 0))
    (property "Datasheet" "" (id 3) (at 21.59 248.92 0))
  )
  (symbol (lib_id "power:GND") (at 27.94 179.07 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR062" (id 0) (at 27.94 185.42 0))
    (property "Value" "GND" (id 1) (at 28.067 183.4642 0))
    (property "Footprint" "" (id 2) (at 27.94 179.07 0))
    (property "Datasheet" "" (id 3) (at 27.94 179.07 0))
  )
  (symbol (lib_id "power:GND") (at 27.94 210.82 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR063" (id 0) (at 27.94 217.17 0))
    (property "Value" "GND" (id 1) (at 28.067 215.2142 0))
    (property "Footprint" "" (id 2) (at 27.94 210.82 0))
    (property "Datasheet" "" (id 3) (at 27.94 210.82 0))
  )
  (symbol (lib_id "power:GND") (at 37.846 148.59 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR064" (id 0) (at 37.846 154.94 0))
    (property "Value" "GND" (id 1) (at 37.973 152.9842 0))
    (property "Footprint" "" (id 2) (at 37.846 148.59 0))
    (property "Datasheet" "" (id 3) (at 37.846 148.59 0))
  )
  (symbol (lib_id "power:GND") (at 44.45 189.23 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR?" (id 0) (at 44.45 195.58 0))
    (property "Value" "GND" (id 1) (at 45.72 194.31 0))
    (property "Footprint" "" (id 2) (at 44.45 189.23 0))
    (property "Datasheet" "" (id 3) (at 44.45 189.23 0))
  )
  (symbol (lib_id "power:GND") (at 88.9 262.89 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR065" (id 0) (at 88.9 269.24 0))
    (property "Value" "GND" (id 1) (at 89.027 267.2842 0))
    (property "Footprint" "" (id 2) (at 88.9 262.89 0))
    (property "Datasheet" "" (id 3) (at 88.9 262.89 0))
  )
  (symbol (lib_id "power:GND") (at 101.346 148.59 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR066" (id 0) (at 101.346 154.94 0))
    (property "Value" "GND" (id 1) (at 101.473 152.9842 0))
    (property "Footprint" "" (id 2) (at 101.346 148.59 0))
    (property "Datasheet" "" (id 3) (at 101.346 148.59 0))
  )
  (symbol (lib_id "power:GND") (at 115.57 278.13 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR067" (id 0) (at 115.57 284.48 0))
    (property "Value" "GND" (id 1) (at 115.697 282.5242 0))
    (property "Footprint" "" (id 2) (at 115.57 278.13 0))
    (property "Datasheet" "" (id 3) (at 115.57 278.13 0))
  )
  (symbol (lib_id "power:GND") (at 140.97 151.13 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR0105" (id 0) (at 140.97 157.48 0))
    (property "Value" "GND" (id 1) (at 141.097 155.5242 0))
    (property "Footprint" "" (id 2) (at 140.97 151.13 0))
    (property "Datasheet" "" (id 3) (at 140.97 151.13 0))
  )
  (symbol (lib_id "power:GND") (at 146.05 278.13 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR0104" (id 0) (at 146.05 284.48 0))
    (property "Value" "GND" (id 1) (at 146.177 282.5242 0))
    (property "Footprint" "" (id 2) (at 146.05 278.13 0))
    (property "Datasheet" "" (id 3) (at 146.05 278.13 0))
  )
  (symbol (lib_id "power:GND") (at 151.13 73.66 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR0103" (id 0) (at 151.13 80.01 0))
    (property "Value" "GND" (id 1) (at 151.257 78.0542 0))
    (property "Footprint" "" (id 2) (at 151.13 73.66 0))
    (property "Datasheet" "" (id 3) (at 151.13 73.66 0))
  )
  (symbol (lib_id "power:GND") (at 166.37 73.66 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR0102" (id 0) (at 166.37 80.01 0))
    (property "Value" "GND" (id 1) (at 166.497 78.0542 0))
    (property "Footprint" "" (id 2) (at 166.37 73.66 0))
    (property "Datasheet" "" (id 3) (at 166.37 73.66 0))
  )
  (symbol (lib_id "power:GND") (at 173.99 207.01 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR0107" (id 0) (at 173.99 213.36 0))
    (property "Value" "GND" (id 1) (at 175.26 212.09 0))
    (property "Footprint" "" (id 2) (at 173.99 207.01 0))
    (property "Datasheet" "" (id 3) (at 173.99 207.01 0))
  )
  (symbol (lib_id "power:GND") (at 181.61 184.15 180) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR0106" (id 0) (at 181.61 177.8 0))
    (property "Value" "GND" (id 1) (at 180.34 179.07 0))
    (property "Footprint" "" (id 2) (at 181.61 184.15 0))
    (property "Datasheet" "" (id 3) (at 181.61 184.15 0))
  )
  (symbol (lib_id "power:GND") (at 183.388 153.162 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR073" (id 0) (at 183.388 159.512 0))
    (property "Value" "GND" (id 1) (at 183.515 157.5562 0))
    (property "Footprint" "" (id 2) (at 183.388 153.162 0))
    (property "Datasheet" "" (id 3) (at 183.388 153.162 0))
  )
  (symbol (lib_id "power:GND") (at 187.96 247.65 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR0122" (id 0) (at 187.96 254 0))
    (property "Value" "GND" (id 1) (at 188.087 252.0442 0))
    (property "Footprint" "" (id 2) (at 187.96 247.65 0))
    (property "Datasheet" "" (id 3) (at 187.96 247.65 0))
  )
  (symbol (lib_id "power:GND") (at 194.31 204.47 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR0101" (id 0) (at 194.31 210.82 0))
    (property "Value" "GND" (id 1) (at 195.58 209.55 0))
    (property "Footprint" "" (id 2) (at 194.31 204.47 0))
    (property "Datasheet" "" (id 3) (at 194.31 204.47 0))
  )
  (symbol (lib_id "power:GND") (at 195.58 247.65 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR0121" (id 0) (at 195.58 254 0))
    (property "Value" "GND" (id 1) (at 195.707 252.0442 0))
    (property "Footprint" "" (id 2) (at 195.58 247.65 0))
    (property "Datasheet" "" (id 3) (at 195.58 247.65 0))
  )
  (symbol (lib_id "power:GND") (at 199.39 73.66 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR075" (id 0) (at 199.39 80.01 0))
    (property "Value" "GND" (id 1) (at 199.517 78.0542 0))
    (property "Footprint" "" (id 2) (at 199.39 73.66 0))
    (property "Datasheet" "" (id 3) (at 199.39 73.66 0))
  )
  (symbol (lib_id "power:GND") (at 227.33 237.49 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR077" (id 0) (at 227.33 243.84 0))
    (property "Value" "GND" (id 1) (at 227.457 241.8842 0))
    (property "Footprint" "" (id 2) (at 227.33 237.49 0))
    (property "Datasheet" "" (id 3) (at 227.33 237.49 0))
  )
  (symbol (lib_id "power:GND") (at 231.14 73.66 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR078" (id 0) (at 231.14 80.01 0))
    (property "Value" "GND" (id 1) (at 231.267 78.0542 0))
    (property "Footprint" "" (id 2) (at 231.14 73.66 0))
    (property "Datasheet" "" (id 3) (at 231.14 73.66 0))
  )
  (symbol (lib_id "power:GND") (at 264.16 44.45 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR079" (id 0) (at 264.16 50.8 0))
    (property "Value" "GND" (id 1) (at 264.287 48.8442 0))
    (property "Footprint" "" (id 2) (at 264.16 44.45 0))
    (property "Datasheet" "" (id 3) (at 264.16 44.45 0))
  )
  (symbol (lib_id "power:GND") (at 274.32 43.18 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR080" (id 0) (at 274.32 49.53 0))
    (property "Value" "GND" (id 1) (at 274.447 47.5742 0))
    (property "Footprint" "" (id 2) (at 274.32 43.18 0))
    (property "Datasheet" "" (id 3) (at 274.32 43.18 0))
  )
  (symbol (lib_id "power:GND") (at 278.13 78.74 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR0111" (id 0) (at 278.13 85.09 0))
    (property "Value" "GND" (id 1) (at 279.4 83.82 0))
    (property "Footprint" "" (id 2) (at 278.13 78.74 0))
    (property "Datasheet" "" (id 3) (at 278.13 78.74 0))
  )
  (symbol (lib_id "power:GND") (at 285.75 55.88 180) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR0109" (id 0) (at 285.75 49.53 0))
    (property "Value" "GND" (id 1) (at 284.48 50.8 0))
    (property "Footprint" "" (id 2) (at 285.75 55.88 0))
    (property "Datasheet" "" (id 3) (at 285.75 55.88 0))
  )
  (symbol (lib_id "power:GND") (at 293.37 237.49 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR081" (id 0) (at 293.37 243.84 0))
    (property "Value" "GND" (id 1) (at 293.497 241.8842 0))
    (property "Footprint" "" (id 2) (at 293.37 237.49 0))
    (property "Datasheet" "" (id 3) (at 293.37 237.49 0))
  )
  (symbol (lib_id "power:GND") (at 298.45 76.2 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR0110" (id 0) (at 298.45 82.55 0))
    (property "Value" "GND" (id 1) (at 299.72 81.28 0))
    (property "Footprint" "" (id 2) (at 298.45 76.2 0))
    (property "Datasheet" "" (id 3) (at 298.45 76.2 0))
  )
  (symbol (lib_id "power:GND") (at 313.055 46.99 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR085" (id 0) (at 313.055 53.34 0))
    (property "Value" "GND" (id 1) (at 313.182 51.3842 0))
    (property "Footprint" "" (id 2) (at 313.055 46.99 0))
    (property "Datasheet" "" (id 3) (at 313.055 46.99 0))
  )
  (symbol (lib_id "power:GND") (at 320.04 124.46 270) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR0114" (id 0) (at 313.69 124.46 0))
    (property "Value" "GND" (id 1) (at 315.6458 124.587 0))
    (property "Footprint" "" (id 2) (at 320.04 124.46 0))
    (property "Datasheet" "" (id 3) (at 320.04 124.46 0))
  )
  (symbol (lib_id "power:GND") (at 325.12 104.14 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR0108" (id 0) (at 325.12 110.49 0))
    (property "Value" "GND" (id 1) (at 325.247 108.5342 0))
    (property "Footprint" "" (id 2) (at 325.12 104.14 0))
    (property "Datasheet" "" (id 3) (at 325.12 104.14 0))
  )
  (symbol (lib_id "power:GND") (at 328.93 146.05 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR0115" (id 0) (at 328.93 152.4 0))
    (property "Value" "GND" (id 1) (at 329.057 150.4442 0))
    (property "Footprint" "" (id 2) (at 328.93 146.05 0))
    (property "Datasheet" "" (id 3) (at 328.93 146.05 0))
  )
  (symbol (lib_id "power:GND") (at 332.74 36.83 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR0113" (id 0) (at 332.74 43.18 0))
    (property "Value" "GND" (id 1) (at 332.867 41.2242 0))
    (property "Footprint" "" (id 2) (at 332.74 36.83 0))
    (property "Datasheet" "" (id 3) (at 332.74 36.83 0))
  )
  (symbol (lib_id "power:GND") (at 335.28 62.23 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR0119" (id 0) (at 335.28 68.58 0))
    (property "Value" "GND" (id 1) (at 335.407 66.6242 0))
    (property "Footprint" "" (id 2) (at 335.28 62.23 0))
    (property "Datasheet" "" (id 3) (at 335.28 62.23 0))
  )
  (symbol (lib_id "power:GND") (at 336.55 146.05 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR0116" (id 0) (at 336.55 152.4 0))
    (property "Value" "GND" (id 1) (at 336.677 150.4442 0))
    (property "Footprint" "" (id 2) (at 336.55 146.05 0))
    (property "Datasheet" "" (id 3) (at 336.55 146.05 0))
  )
  (symbol (lib_id "power:GND") (at 337.82 217.17 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR0117" (id 0) (at 337.82 223.52 0))
    (property "Value" "GND" (id 1) (at 337.947 221.5642 0))
    (property "Footprint" "" (id 2) (at 337.82 217.17 0))
    (property "Datasheet" "" (id 3) (at 337.82 217.17 0))
  )
  (symbol (lib_id "power:GND") (at 359.41 36.83 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR0120" (id 0) (at 359.41 43.18 0))
    (property "Value" "GND" (id 1) (at 359.537 41.2242 0))
    (property "Footprint" "" (id 2) (at 359.41 36.83 0))
    (property "Datasheet" "" (id 3) (at 359.41 36.83 0))
  )
  (symbol (lib_id "power:GND") (at 361.95 62.23 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR0112" (id 0) (at 361.95 68.58 0))
    (property "Value" "GND" (id 1) (at 362.077 66.6242 0))
    (property "Footprint" "" (id 2) (at 361.95 62.23 0))
    (property "Datasheet" "" (id 3) (at 361.95 62.23 0))
  )
  (symbol (lib_id "power:GND") (at 368.3 146.05 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR0118" (id 0) (at 368.3 152.4 0))
    (property "Value" "GND" (id 1) (at 368.427 150.4442 0))
    (property "Footprint" "" (id 2) (at 368.3 146.05 0))
    (property "Datasheet" "" (id 3) (at 368.3 146.05 0))
  )
  (symbol (lib_id "power:GND") (at 386.08 213.36 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR099" (id 0) (at 386.08 219.71 0))
    (property "Value" "GND" (id 1) (at 386.207 217.7542 0))
    (property "Footprint" "" (id 2) (at 386.08 213.36 0))
    (property "Datasheet" "" (id 3) (at 386.08 213.36 0))
  )
  (symbol (lib_id "Device:R") (at 39.37 255.27 90) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R43" (id 0) (at 38.1 257.81 90))
    (property "Value" "nf" (id 1) (at 41.91 257.81 90))
    (property "Footprint" "Resistor_SMD:R_0402_1005Metric" (id 2) (at 39.37 257.048 90))
    (property "Datasheet" "https://fscdn.rohm.com/en/products/databook/datasheet/passive/resistor/chip_resistor/mcr-e.pdf" (id 3) (at 39.37 255.27 0))
    (property "Field4" "Farnell" (id 4) (at 39.37 255.27 0))
    (property "Field5" "9239235" (id 5) (at 39.37 255.27 0))
    (property "Field7" "KOA EUROPE GMBH" (id 6) (at 39.37 255.27 0))
    (property "Field6" "RK73H1ETTP1001F" (id 7) (at 39.37 255.27 0))
    (property "Part Description" "Resistor 1K M1005 1% 63mW" (id 8) (at 39.37 255.27 0))
    (property "Field8" "125049511" (id 9) (at 39.37 255.27 0))
  )
  (symbol (lib_id "Device:R") (at 39.37 262.89 90) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R44" (id 0) (at 37.8206 265.2776 90))
    (property "Value" "nf" (id 1) (at 41.8338 265.2268 90))
    (property "Footprint" "Resistor_SMD:R_0402_1005Metric" (id 2) (at 39.37 264.668 90))
    (property "Datasheet" "https://fscdn.rohm.com/en/products/databook/datasheet/passive/resistor/chip_resistor/mcr-e.pdf" (id 3) (at 39.37 262.89 0))
    (property "Field4" "Farnell" (id 4) (at 39.37 262.89 0))
    (property "Field5" "9239235" (id 5) (at 39.37 262.89 0))
    (property "Field7" "KOA EUROPE GMBH" (id 6) (at 39.37 262.89 0))
    (property "Field6" "RK73H1ETTP1001F" (id 7) (at 39.37 262.89 0))
    (property "Part Description" "Resistor 1K M1005 1% 63mW" (id 8) (at 39.37 262.89 0))
    (property "Field8" "125049511" (id 9) (at 39.37 262.89 0))
  )
  (symbol (lib_id "Device:R") (at 105.41 44.45 90) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R45" (id 0) (at 104.2416 42.672 90))
    (property "Value" "1k" (id 1) (at 107.823 42.672 90))
    (property "Footprint" "Resistor_SMD:R_0402_1005Metric" (id 2) (at 105.41 46.228 90))
    (property "Datasheet" "https://fscdn.rohm.com/en/products/databook/datasheet/passive/resistor/chip_resistor/mcr-e.pdf" (id 3) (at 105.41 44.45 0))
    (property "Field4" "Farnell" (id 4) (at 105.41 44.45 0))
    (property "Field5" "9239235" (id 5) (at 105.41 44.45 0))
    (property "Field7" "KOA EUROPE GMBH" (id 6) (at 105.41 44.45 0))
    (property "Field6" "RK73H1ETTP1001F" (id 7) (at 105.41 44.45 0))
    (property "Part Description" "Resistor 1K M1005 1% 63mW" (id 8) (at 105.41 44.45 0))
    (property "Field8" "125049511" (id 9) (at 105.41 44.45 0))
  )
  (symbol (lib_id "Device:R") (at 144.78 101.6 270) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R46" (id 0) (at 144.78 96.3422 90))
    (property "Value" "470R" (id 1) (at 144.78 98.6536 90))
    (property "Footprint" "Resistor_SMD:R_0402_1005Metric" (id 2) (at 144.78 99.822 90))
    (property "Datasheet" "https://fscdn.rohm.com/en/products/databook/datasheet/passive/resistor/chip_resistor/mcr-e.pdf" (id 3) (at 144.78 101.6 0))
    (property "Field4" "Farnell" (id 4) (at 144.78 101.6 0))
    (property "Field5" "9239197" (id 5) (at 144.78 101.6 0))
    (property "Field7" "KOA EUROPE GMBH" (id 6) (at 144.78 101.6 0))
    (property "Field6" "RK73G1ETQTP4700D         " (id 7) (at 144.78 101.6 0))
    (property "Field8" "120887981" (id 8) (at 144.78 101.6 0))
    (property "Part Description" "Resistor 470R M1005 1% 63mW" (id 9) (at 144.78 101.6 0))
  )
  (symbol (lib_id "Device:R") (at 144.78 106.68 270) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R47" (id 0) (at 144.78 111.76 90))
    (property "Value" "470R" (id 1) (at 144.78 109.22 90))
    (property "Footprint" "Resistor_SMD:R_0402_1005Metric" (id 2) (at 144.78 104.902 90))
    (property "Datasheet" "https://fscdn.rohm.com/en/products/databook/datasheet/passive/resistor/chip_resistor/mcr-e.pdf" (id 3) (at 144.78 106.68 0))
    (property "Field4" "Farnell" (id 4) (at 144.78 106.68 0))
    (property "Field5" "9239197" (id 5) (at 144.78 106.68 0))
    (property "Field7" "KOA EUROPE GMBH" (id 6) (at 144.78 106.68 0))
    (property "Field6" "RK73G1ETQTP4700D         " (id 7) (at 144.78 106.68 0))
    (property "Field8" "120887981" (id 8) (at 144.78 106.68 0))
    (property "Part Description" "Resistor 470R M1005 1% 63mW" (id 9) (at 144.78 106.68 0))
  )
  (symbol (lib_id "Device:R") (at 191.008 135.382 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R48" (id 0) (at 192.786 134.2136 0))
    (property "Value" "1k" (id 1) (at 192.786 136.525 0))
    (property "Footprint" "Resistor_SMD:R_0402_1005Metric" (id 2) (at 189.23 135.382 90))
    (property "Datasheet" "https://fscdn.rohm.com/en/products/databook/datasheet/passive/resistor/chip_resistor/mcr-e.pdf" (id 3) (at 191.008 135.382 0))
    (property "Field4" "Farnell" (id 4) (at 191.008 135.382 0))
    (property "Field5" "9239235" (id 5) (at 191.008 135.382 0))
    (property "Field7" "KOA EUROPE GMBH" (id 6) (at 191.008 135.382 0))
    (property "Field6" "RK73H1ETTP1001F" (id 7) (at 191.008 135.382 0))
    (property "Part Description" "Resistor 1K M1005 1% 63mW" (id 8) (at 191.008 135.382 0))
    (property "Field8" "125049511" (id 9) (at 191.008 135.382 0))
  )
  (symbol (lib_id "Device:R") (at 191.77 247.65 270) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R0" (id 0) (at 191.77 241.3 90))
    (property "Value" "0R" (id 1) (at 191.77 243.84 90))
    (property "Footprint" "Resistor_SMD:R_1206_3216Metric" (id 2) (at 191.77 245.872 90))
    (property "Datasheet" "~" (id 3) (at 191.77 247.65 0))
  )
  (symbol (lib_id "Device:R") (at 264.16 40.64 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R49" (id 0) (at 258.445 39.37 0))
    (property "Value" "2.2K 1%" (id 1) (at 254.635 41.91 0))
    (property "Footprint" "Resistor_SMD:R_0402_1005Metric" (id 2) (at 262.382 40.64 90))
    (property "Datasheet" "https://fscdn.rohm.com/en/products/databook/datasheet/passive/resistor/chip_resistor/mcr-e.pdf" (id 3) (at 264.16 40.64 0))
    (property "Field4" "Farnell" (id 4) (at 264.16 40.64 0))
    (property "Field5" "9239278" (id 5) (at 264.16 40.64 0))
    (property "Field7" "KOA EUROPE GMBH" (id 6) (at 264.16 40.64 0))
    (property "Field6" "RK73G1ETQTP2201D         " (id 7) (at 264.16 40.64 0))
    (property "Part Description" "Resistor 2.2K M1005 1% 63mW" (id 8) (at 264.16 40.64 0))
    (property "Field8" "120889581" (id 4) (at 264.16 40.64 0))
  )
  (symbol (lib_id "Device:R") (at 271.145 17.78 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R50" (id 0) (at 272.923 16.6116 0))
    (property "Value" "2.2K 1%" (id 1) (at 272.923 18.923 0))
    (property "Footprint" "Resistor_SMD:R_0402_1005Metric" (id 2) (at 269.367 17.78 90))
    (property "Datasheet" "https://fscdn.rohm.com/en/products/databook/datasheet/passive/resistor/chip_resistor/mcr-e.pdf" (id 3) (at 271.145 17.78 0))
    (property "Field4" "Farnell" (id 4) (at 271.145 17.78 0))
    (property "Field5" "9239278" (id 5) (at 271.145 17.78 0))
    (property "Field7" "KOA EUROPE GMBH" (id 6) (at 271.145 17.78 0))
    (property "Field6" "RK73G1ETQTP2201D         " (id 7) (at 271.145 17.78 0))
    (property "Part Description" "Resistor 2.2K M1005 1% 63mW" (id 8) (at 271.145 17.78 0))
    (property "Field8" "120889581" (id 4) (at 271.145 17.78 0))
  )
  (symbol (lib_id "Device:R") (at 289.56 78.74 90) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R1" (id 0) (at 288.29 76.2 90))
    (property "Value" "3k" (id 1) (at 292.1 76.2 90))
    (property "Footprint" "Resistor_SMD:R_0402_1005Metric" (id 2) (at 289.56 80.518 90))
    (property "Datasheet" "~" (id 3) (at 289.56 78.74 0))
  )
  (symbol (lib_id "Device:R") (at 293.37 72.39 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R2" (id 0) (at 294.64 71.12 0))
    (property "Value" "4.7k" (id 1) (at 294.64 74.93 0))
    (property "Footprint" "Resistor_SMD:R_0402_1005Metric" (id 2) (at 291.592 72.39 90))
    (property "Datasheet" "~" (id 3) (at 293.37 72.39 0))
  )
  (symbol (lib_id "Device:R") (at 328.93 139.7 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R3" (id 0) (at 324.485 141.605 90))
    (property "Value" "36K 1%" (id 1) (at 326.39 142.875 90))
    (property "Footprint" "Resistor_SMD:R_0402_1005Metric" (id 2) (at 327.152 139.7 90))
    (property "Datasheet" "https://fscdn.rohm.com/en/products/databook/datasheet/passive/resistor/chip_resistor/mcr-e.pdf" (id 3) (at 328.93 139.7 0))
    (property "Field4" "Farnell" (id 4) (at 328.93 139.7 0))
    (property "Field5" "1458788" (id 5) (at 328.93 139.7 0))
    (property "Field7" "Rohm" (id 6) (at 328.93 139.7 0))
    (property "Field6" "MCR01MZPF3602" (id 7) (at 328.93 139.7 0))
    (property "Part Description" "Resistor 36K M1005 1% 63mW" (id 8) (at 328.93 139.7 0))
  )
  (symbol (lib_id "Device:R") (at 331.47 102.87 90) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R4" (id 0) (at 335.28 100.33 90))
    (property "Value" "12K 1%" (id 1) (at 331.47 100.33 90))
    (property "Footprint" "Resistor_SMD:R_0402_1005Metric" (id 2) (at 331.47 104.648 90))
    (property "Datasheet" "https://fscdn.rohm.com/en/products/databook/datasheet/passive/resistor/chip_resistor/mcr-e.pdf" (id 3) (at 331.47 102.87 0))
    (property "Field4" "Farnell" (id 4) (at 331.47 102.87 0))
    (property "Field5" "9239367" (id 5) (at 331.47 102.87 0))
    (property "Field7" "Rohm" (id 6) (at 331.47 102.87 0))
    (property "Field6" "MCR01MZPF1202" (id 7) (at 331.47 102.87 0))
    (property "Part Description" "Resistor 12K M1005 1% 63mW" (id 8) (at 331.47 102.87 0))
  )
  (symbol (lib_id "Device:R") (at 336.55 125.73 270) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R5" (id 0) (at 334.645 121.285 90))
    (property "Value" "36K 1%" (id 1) (at 333.375 123.19 90))
    (property "Footprint" "Resistor_SMD:R_0402_1005Metric" (id 2) (at 336.55 123.952 90))
    (property "Datasheet" "https://fscdn.rohm.com/en/products/databook/datasheet/passive/resistor/chip_resistor/mcr-e.pdf" (id 3) (at 336.55 125.73 0))
    (property "Field4" "Farnell" (id 4) (at 336.55 125.73 0))
    (property "Field5" "1458788" (id 5) (at 336.55 125.73 0))
    (property "Field7" "Rohm" (id 6) (at 336.55 125.73 0))
    (property "Field6" "MCR01MZPF3602" (id 7) (at 336.55 125.73 0))
    (property "Part Description" "Resistor 36K M1005 1% 63mW" (id 8) (at 336.55 125.73 0))
  )
  (symbol (lib_id "Device:R") (at 336.55 128.27 270) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R6" (id 0) (at 327.025 127.635 90))
    (property "Value" "36K 1%" (id 1) (at 325.755 129.54 90))
    (property "Footprint" "Resistor_SMD:R_0402_1005Metric" (id 2) (at 336.55 126.492 90))
    (property "Datasheet" "https://fscdn.rohm.com/en/products/databook/datasheet/passive/resistor/chip_resistor/mcr-e.pdf" (id 3) (at 336.55 128.27 0))
    (property "Field4" "Farnell" (id 4) (at 336.55 128.27 0))
    (property "Field5" "1458788" (id 5) (at 336.55 128.27 0))
    (property "Field7" "Rohm" (id 6) (at 336.55 128.27 0))
    (property "Field6" "MCR01MZPF3602" (id 7) (at 336.55 128.27 0))
    (property "Part Description" "Resistor 36K M1005 1% 63mW" (id 8) (at 336.55 128.27 0))
  )
  (symbol (lib_id "Device:R") (at 336.55 139.7 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R7" (id 0) (at 332.105 141.605 90))
    (property "Value" "36K 1%" (id 1) (at 334.01 142.875 90))
    (property "Footprint" "Resistor_SMD:R_0402_1005Metric" (id 2) (at 334.772 139.7 90))
    (property "Datasheet" "https://fscdn.rohm.com/en/products/databook/datasheet/passive/resistor/chip_resistor/mcr-e.pdf" (id 3) (at 336.55 139.7 0))
    (property "Field4" "Farnell" (id 4) (at 336.55 139.7 0))
    (property "Field5" "1458788" (id 5) (at 336.55 139.7 0))
    (property "Field7" "Rohm" (id 6) (at 336.55 139.7 0))
    (property "Field6" "MCR01MZPF3602" (id 7) (at 336.55 139.7 0))
    (property "Part Description" "Resistor 36K M1005 1% 63mW" (id 8) (at 336.55 139.7 0))
  )
  (symbol (lib_id "pspice:INDUCTOR") (at 187.96 191.77 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "L1" (id 0) (at 186.69 186.69 0))
    (property "Value" "6.8uh" (id 1) (at 186.69 189.23 0))
    (property "Footprint" "Inductor_SMD:L_1206_3216Metric" (id 2) (at 187.96 191.77 0))
    (property "Datasheet" "~" (id 3) (at 187.96 191.77 0))
  )
  (symbol (lib_id "pspice:INDUCTOR") (at 292.1 63.5 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "L2" (id 0) (at 290.83 58.42 0))
    (property "Value" "6.8uh" (id 1) (at 290.83 60.96 0))
    (property "Footprint" "Inductor_SMD:L_1206_3216Metric" (id 2) (at 292.1 63.5 0))
    (property "Datasheet" "~" (id 3) (at 292.1 63.5 0))
  )
  (symbol (lib_id "Device:D") (at 181.61 187.96 90) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "D1" (id 0) (at 184.15 186.69 90))
    (property "Value" "SS36" (id 1) (at 184.15 187.96 90))
    (property "Footprint" "Diode_SMD:D_SMA" (id 2) (at 181.61 187.96 0))
    (property "Datasheet" "~" (id 3) (at 181.61 187.96 0))
  )
  (symbol (lib_id "Device:D") (at 285.75 59.69 90) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "D2" (id 0) (at 288.29 58.42 90))
    (property "Value" "SS36" (id 1) (at 288.29 59.69 90))
    (property "Footprint" "Diode_SMD:D_SMA" (id 2) (at 285.75 59.69 0))
    (property "Datasheet" "~" (id 3) (at 285.75 59.69 0))
  )
  (symbol (lib_id "Device:D") (at 370.84 21.59 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "D3" (id 0) (at 370.84 15.24 0))
    (property "Value" "SS36" (id 1) (at 370.84 17.78 0))
    (property "Footprint" "Diode_SMD:D_SMA" (id 2) (at 370.84 21.59 0))
    (property "Datasheet" "~" (id 3) (at 370.84 21.59 0))
  )
  (symbol (lib_id "Connector:Conn_01x02_Female") (at 146.05 194.31 180) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "J1" (id 0) (at 149.86 199.39 0))
    (property "Value" "Conn_01x02_Female" (id 1) (at 149.86 196.85 0))
    (property "Footprint" "Connector_BarrelJack:BarrelJack_CLIFF_FC681465S_SMT_Horizontal" (id 2) (at 146.05 194.31 0))
    (property "Datasheet" "~" (id 3) (at 146.05 194.31 0))
  )
  (symbol (lib_id "Device:LED") (at 121.92 44.45 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "D16" (id 0) (at 124.1806 41.0718 0))
    (property "Value" "LED Green" (id 1) (at 126.9492 47.4218 0))
    (property "Footprint" "LED_SMD:LED_0603_1608Metric" (id 2) (at 121.92 44.45 0))
    (property "Datasheet" "http://optoelectronics.liteon.com/upload/download/DS22-2000-226/LTST-S270KGKT.pdf" (id 3) (at 121.92 44.45 0))
    (property "Field4" "Digikey " (id 4) (at 121.92 44.45 0))
    (property "Field5" "LTST-S270KGKT" (id 5) (at 121.92 44.45 0))
    (property "Field6" "SML-A12M8TT86N" (id 6) (at 121.92 44.45 0))
    (property "Field7" "Rohm" (id 7) (at 121.92 44.45 0))
    (property "Field8" "650263301" (id 8) (at 121.92 44.45 0))
    (property "Part Description" "	Green 572nm LED Indication - Discrete 2.2V 2-SMD, No Lead" (id 9) (at 121.92 44.45 0))
  )
  (symbol (lib_name "Device:LED_1") (lib_id "Device:LED") (at 152.4 101.6 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "D17" (id 0) (at 152.4 95.25 0))
    (property "Value" "LED yellow" (id 1) (at 152.4 97.79 0))
    (property "Footprint" "LED_SMD:LED_0603_1608Metric" (id 2) (at 152.4 101.6 0))
    (property "Datasheet" "~" (id 3) (at 152.4 101.6 0))
  )
  (symbol (lib_name "Device:LED_1") (lib_id "Device:LED") (at 152.4 106.68 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "D18" (id 0) (at 149.86 105.41 0))
    (property "Value" "LED green" (id 1) (at 158.75 104.14 0))
    (property "Footprint" "LED_SMD:LED_0603_1608Metric" (id 2) (at 152.4 106.68 0))
    (property "Datasheet" "~" (id 3) (at 152.4 106.68 0))
  )
  (symbol (lib_id "Device:LED") (at 191.008 126.492 90) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "D20" (id 0) (at 193.9798 125.5014 90))
    (property "Value" "LED Red" (id 1) (at 193.9798 127.8128 90))
    (property "Footprint" "LED_SMD:LED_0603_1608Metric" (id 2) (at 191.008 126.492 0))
    (property "Datasheet" "http://optoelectronics.liteon.com/upload/download/DS22-2000-210/LTST-S270KRKT.pdf" (id 3) (at 191.008 126.492 0))
    (property "Field4" "Digikey " (id 4) (at 191.008 126.492 0))
    (property "Field5" "	LTST-S270KRKT" (id 5) (at 191.008 126.492 0))
    (property "Field6" "SML-A12U8TT86Q" (id 6) (at 191.008 126.492 0))
    (property "Field7" "Rohm" (id 7) (at 191.008 126.492 0))
    (property "Field8" "650295101" (id 8) (at 191.008 126.492 0))
    (property "Part Description" "	Red 620nm LED Indication - Discrete 2.2V 2-SMD, No Lead" (id 9) (at 191.008 126.492 0))
  )
  (symbol (lib_id "Device:C") (at 21.59 241.3 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C46" (id 0) (at 24.511 240.1316 0))
    (property "Value" "10u" (id 1) (at 24.511 242.443 0))
    (property "Footprint" "Capacitor_SMD:C_0805_2012Metric" (id 2) (at 22.5552 245.11 0))
    (property "Datasheet" "https://search.murata.co.jp/Ceramy/image/img/A01X/G101/ENG/GRM21BR71A106KA73-01.pdf" (id 3) (at 21.59 241.3 0))
    (property "Field5" "490-14381-1-ND" (id 4) (at 21.59 241.3 0))
    (property "Field4" "Digikey" (id 5) (at 21.59 241.3 0))
    (property "Field6" "GRM21BR71A106KA73L" (id 6) (at 21.59 241.3 0))
    (property "Field7" "Murata" (id 7) (at 21.59 241.3 0))
    (property "Part Description" "	10uF 10% 10V Ceramic Capacitor X7R 0805 (2012 Metric)" (id 8) (at 21.59 241.3 0))
    (property "Field8" "111893011" (id 9) (at 21.59 241.3 0))
  )
  (symbol (lib_id "Device:C") (at 27.94 203.2 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C47" (id 0) (at 30.861 202.0316 0))
    (property "Value" "10u" (id 1) (at 30.861 204.343 0))
    (property "Footprint" "Capacitor_SMD:C_0805_2012Metric" (id 2) (at 28.9052 207.01 0))
    (property "Datasheet" "https://search.murata.co.jp/Ceramy/image/img/A01X/G101/ENG/GRM21BR71A106KA73-01.pdf" (id 3) (at 27.94 203.2 0))
    (property "Field5" "490-14381-1-ND" (id 4) (at 27.94 203.2 0))
    (property "Field4" "Digikey" (id 5) (at 27.94 203.2 0))
    (property "Field6" "GRM21BR71A106KA73L" (id 6) (at 27.94 203.2 0))
    (property "Field7" "Murata" (id 7) (at 27.94 203.2 0))
    (property "Part Description" "	10uF 10% 10V Ceramic Capacitor X7R 0805 (2012 Metric)" (id 8) (at 27.94 203.2 0))
    (property "Field8" "111893011" (id 9) (at 27.94 203.2 0))
  )
  (symbol (lib_id "Device:C") (at 37.084 203.2 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C48" (id 0) (at 40.005 202.0316 0))
    (property "Value" "10u" (id 1) (at 40.005 204.343 0))
    (property "Footprint" "Capacitor_SMD:C_0805_2012Metric" (id 2) (at 38.0492 207.01 0))
    (property "Datasheet" "https://search.murata.co.jp/Ceramy/image/img/A01X/G101/ENG/GRM21BR71A106KA73-01.pdf" (id 3) (at 37.084 203.2 0))
    (property "Field5" "490-14381-1-ND" (id 4) (at 37.084 203.2 0))
    (property "Field4" "Digikey" (id 5) (at 37.084 203.2 0))
    (property "Field6" "GRM21BR71A106KA73L" (id 6) (at 37.084 203.2 0))
    (property "Field7" "Murata" (id 7) (at 37.084 203.2 0))
    (property "Part Description" "	10uF 10% 10V Ceramic Capacitor X7R 0805 (2012 Metric)" (id 8) (at 37.084 203.2 0))
    (property "Field8" "111893011" (id 9) (at 37.084 203.2 0))
  )
  (symbol (lib_id "Device:C") (at 44.45 185.42 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C59" (id 0) (at 46.99 184.15 0))
    (property "Value" "22uf" (id 1) (at 45.72 187.96 0))
    (property "Footprint" "Capacitor_SMD:C_0805_2012Metric" (id 2) (at 45.4152 189.23 0))
    (property "Datasheet" "~" (id 3) (at 44.45 185.42 0))
  )
  (symbol (lib_id "Device:C") (at 46.228 203.2 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C49" (id 0) (at 49.149 202.0316 0))
    (property "Value" "100n" (id 1) (at 49.149 204.343 0))
    (property "Footprint" "Capacitor_SMD:C_0402_1005Metric" (id 2) (at 47.1932 207.01 0))
    (property "Datasheet" "https://search.murata.co.jp/Ceramy/image/img/A01X/G101/ENG/GRM155R71C104KA88-01.pdf" (id 3) (at 46.228 203.2 0))
    (property "Field4" "Farnell" (id 4) (at 46.228 203.2 0))
    (property "Field5" "2611911" (id 5) (at 46.228 203.2 0))
    (property "Field6" "RM EMK105 B7104KV-F" (id 6) (at 46.228 203.2 0))
    (property "Field7" "TAIYO YUDEN EUROPE GMBH" (id 7) (at 46.228 203.2 0))
    (property "Part Description" "	0.1uF 10% 16V Ceramic Capacitor X7R 0402 (1005 Metric)" (id 8) (at 46.228 203.2 0))
    (property "Field8" "110091611" (id 9) (at 46.228 203.2 0))
  )
  (symbol (lib_id "Device:C") (at 53.34 185.42 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C62" (id 0) (at 55.88 184.15 0))
    (property "Value" "22uf" (id 1) (at 54.61 187.96 0))
    (property "Footprint" "Capacitor_SMD:C_0805_2012Metric" (id 2) (at 54.3052 189.23 0))
    (property "Datasheet" "~" (id 3) (at 53.34 185.42 0))
  )
  (symbol (lib_id "Device:C") (at 56.388 203.2 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C50" (id 0) (at 59.309 202.0316 0))
    (property "Value" "100n" (id 1) (at 59.309 204.343 0))
    (property "Footprint" "Capacitor_SMD:C_0402_1005Metric" (id 2) (at 57.3532 207.01 0))
    (property "Datasheet" "https://search.murata.co.jp/Ceramy/image/img/A01X/G101/ENG/GRM155R71C104KA88-01.pdf" (id 3) (at 56.388 203.2 0))
    (property "Field4" "Farnell" (id 4) (at 56.388 203.2 0))
    (property "Field5" "2611911" (id 5) (at 56.388 203.2 0))
    (property "Field6" "RM EMK105 B7104KV-F" (id 6) (at 56.388 203.2 0))
    (property "Field7" "TAIYO YUDEN EUROPE GMBH" (id 7) (at 56.388 203.2 0))
    (property "Part Description" "	0.1uF 10% 16V Ceramic Capacitor X7R 0402 (1005 Metric)" (id 8) (at 56.388 203.2 0))
    (property "Field8" "110091611" (id 9) (at 56.388 203.2 0))
  )
  (symbol (lib_id "Device:C") (at 62.23 185.42 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C65" (id 0) (at 64.77 184.15 0))
    (property "Value" "22uf" (id 1) (at 63.5 187.96 0))
    (property "Footprint" "Capacitor_SMD:C_0805_2012Metric" (id 2) (at 63.1952 189.23 0))
    (property "Datasheet" "~" (id 3) (at 62.23 185.42 0))
  )
  (symbol (lib_id "Device:C") (at 69.85 203.2 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C51" (id 0) (at 72.771 202.0316 0))
    (property "Value" "100n" (id 1) (at 72.771 204.343 0))
    (property "Footprint" "Capacitor_SMD:C_0402_1005Metric" (id 2) (at 70.8152 207.01 0))
    (property "Datasheet" "https://search.murata.co.jp/Ceramy/image/img/A01X/G101/ENG/GRM155R71C104KA88-01.pdf" (id 3) (at 69.85 203.2 0))
    (property "Field4" "Farnell" (id 4) (at 69.85 203.2 0))
    (property "Field5" "2611911" (id 5) (at 69.85 203.2 0))
    (property "Field6" "RM EMK105 B7104KV-F" (id 6) (at 69.85 203.2 0))
    (property "Field7" "TAIYO YUDEN EUROPE GMBH" (id 7) (at 69.85 203.2 0))
    (property "Part Description" "	0.1uF 10% 16V Ceramic Capacitor X7R 0402 (1005 Metric)" (id 8) (at 69.85 203.2 0))
    (property "Field8" "110091611" (id 9) (at 69.85 203.2 0))
  )
  (symbol (lib_id "Device:C") (at 71.12 185.42 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C57" (id 0) (at 73.66 184.15 0))
    (property "Value" "10uf" (id 1) (at 72.39 187.96 0))
    (property "Footprint" "Capacitor_SMD:C_0805_2012Metric" (id 2) (at 72.0852 189.23 0))
    (property "Datasheet" "~" (id 3) (at 71.12 185.42 0))
  )
  (symbol (lib_id "Device:C") (at 80.01 185.42 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C58" (id 0) (at 82.55 184.15 0))
    (property "Value" "10uf" (id 1) (at 81.28 187.96 0))
    (property "Footprint" "Capacitor_SMD:C_0805_2012Metric" (id 2) (at 80.9752 189.23 0))
    (property "Datasheet" "~" (id 3) (at 80.01 185.42 0))
  )
  (symbol (lib_id "Device:C") (at 81.28 203.2 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C52" (id 0) (at 84.201 202.0316 0))
    (property "Value" "100n" (id 1) (at 84.201 204.343 0))
    (property "Footprint" "Capacitor_SMD:C_0402_1005Metric" (id 2) (at 82.2452 207.01 0))
    (property "Datasheet" "https://search.murata.co.jp/Ceramy/image/img/A01X/G101/ENG/GRM155R71C104KA88-01.pdf" (id 3) (at 81.28 203.2 0))
    (property "Field4" "Farnell" (id 4) (at 81.28 203.2 0))
    (property "Field5" "2611911" (id 5) (at 81.28 203.2 0))
    (property "Field6" "RM EMK105 B7104KV-F" (id 6) (at 81.28 203.2 0))
    (property "Field7" "TAIYO YUDEN EUROPE GMBH" (id 7) (at 81.28 203.2 0))
    (property "Part Description" "	0.1uF 10% 16V Ceramic Capacitor X7R 0402 (1005 Metric)" (id 8) (at 81.28 203.2 0))
    (property "Field8" "110091611" (id 9) (at 81.28 203.2 0))
  )
  (symbol (lib_id "Device:C") (at 88.9 185.42 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C60" (id 0) (at 91.44 184.15 0))
    (property "Value" "10uf" (id 1) (at 90.17 187.96 0))
    (property "Footprint" "Capacitor_SMD:C_0805_2012Metric" (id 2) (at 89.8652 189.23 0))
    (property "Datasheet" "~" (id 3) (at 88.9 185.42 0))
  )
  (symbol (lib_id "Device:C") (at 91.44 203.2 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C53" (id 0) (at 94.361 202.0316 0))
    (property "Value" "100n" (id 1) (at 94.361 204.343 0))
    (property "Footprint" "Capacitor_SMD:C_0402_1005Metric" (id 2) (at 92.4052 207.01 0))
    (property "Datasheet" "https://search.murata.co.jp/Ceramy/image/img/A01X/G101/ENG/GRM155R71C104KA88-01.pdf" (id 3) (at 91.44 203.2 0))
    (property "Field4" "Farnell" (id 4) (at 91.44 203.2 0))
    (property "Field5" "2611911" (id 5) (at 91.44 203.2 0))
    (property "Field6" "RM EMK105 B7104KV-F" (id 6) (at 91.44 203.2 0))
    (property "Field7" "TAIYO YUDEN EUROPE GMBH" (id 7) (at 91.44 203.2 0))
    (property "Part Description" "	0.1uF 10% 16V Ceramic Capacitor X7R 0402 (1005 Metric)" (id 8) (at 91.44 203.2 0))
    (property "Field8" "110091611" (id 9) (at 91.44 203.2 0))
  )
  (symbol (lib_id "Device:C") (at 97.79 185.42 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C61" (id 0) (at 100.33 184.15 0))
    (property "Value" "10uf" (id 1) (at 99.06 187.96 0))
    (property "Footprint" "Capacitor_SMD:C_0805_2012Metric" (id 2) (at 98.7552 189.23 0))
    (property "Datasheet" "~" (id 3) (at 97.79 185.42 0))
  )
  (symbol (lib_id "Device:C") (at 101.854 203.2 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C54" (id 0) (at 104.775 202.0316 0))
    (property "Value" "100n" (id 1) (at 104.775 204.343 0))
    (property "Footprint" "Capacitor_SMD:C_0402_1005Metric" (id 2) (at 102.8192 207.01 0))
    (property "Datasheet" "https://search.murata.co.jp/Ceramy/image/img/A01X/G101/ENG/GRM155R71C104KA88-01.pdf" (id 3) (at 101.854 203.2 0))
    (property "Field4" "Farnell" (id 4) (at 101.854 203.2 0))
    (property "Field5" "2611911" (id 5) (at 101.854 203.2 0))
    (property "Field6" "RM EMK105 B7104KV-F" (id 6) (at 101.854 203.2 0))
    (property "Field7" "TAIYO YUDEN EUROPE GMBH" (id 7) (at 101.854 203.2 0))
    (property "Part Description" "	0.1uF 10% 16V Ceramic Capacitor X7R 0402 (1005 Metric)" (id 8) (at 101.854 203.2 0))
    (property "Field8" "110091611" (id 9) (at 101.854 203.2 0))
  )
  (symbol (lib_id "Device:C") (at 106.68 185.42 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C63" (id 0) (at 109.22 184.15 0))
    (property "Value" "10uf" (id 1) (at 107.95 187.96 0))
    (property "Footprint" "Capacitor_SMD:C_0805_2012Metric" (id 2) (at 107.6452 189.23 0))
    (property "Datasheet" "~" (id 3) (at 106.68 185.42 0))
  )
  (symbol (lib_id "Device:C") (at 115.57 185.42 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C64" (id 0) (at 118.11 184.15 0))
    (property "Value" "10uf" (id 1) (at 116.84 187.96 0))
    (property "Footprint" "Capacitor_SMD:C_0805_2012Metric" (id 2) (at 116.5352 189.23 0))
    (property "Datasheet" "~" (id 3) (at 115.57 185.42 0))
  )
  (symbol (lib_id "Device:C") (at 124.46 185.42 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C66" (id 0) (at 127 184.15 0))
    (property "Value" "10uf" (id 1) (at 125.73 187.96 0))
    (property "Footprint" "Capacitor_SMD:C_0805_2012Metric" (id 2) (at 125.4252 189.23 0))
    (property "Datasheet" "~" (id 3) (at 124.46 185.42 0))
  )
  (symbol (lib_id "Device:C") (at 133.35 185.42 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C67" (id 0) (at 135.89 184.15 0))
    (property "Value" "10uf" (id 1) (at 134.62 187.96 0))
    (property "Footprint" "Capacitor_SMD:C_0805_2012Metric" (id 2) (at 134.3152 189.23 0))
    (property "Datasheet" "~" (id 3) (at 133.35 185.42 0))
  )
  (symbol (lib_id "Device:C") (at 157.48 195.58 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C1" (id 0) (at 161.29 194.31 0))
    (property "Value" "22uf" (id 1) (at 158.75 198.12 0))
    (property "Footprint" "Capacitor_SMD:C_1206_3216Metric" (id 2) (at 158.4452 199.39 0))
    (property "Datasheet" "~" (id 3) (at 157.48 195.58 0))
  )
  (symbol (lib_id "Device:C") (at 185.42 196.85 90) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C2" (id 0) (at 182.88 194.31 90))
    (property "Value" "100nf" (id 1) (at 187.96 194.31 90))
    (property "Footprint" "Capacitor_SMD:C_0402_1005Metric" (id 2) (at 189.23 195.8848 0))
    (property "Datasheet" "~" (id 3) (at 185.42 196.85 0))
  )
  (symbol (lib_id "Device:C") (at 194.31 200.66 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C3" (id 0) (at 198.12 199.39 0))
    (property "Value" "100uf" (id 1) (at 195.58 203.2 0))
    (property "Footprint" "Capacitor_SMD:C_1206_3216Metric" (id 2) (at 195.2752 204.47 0))
    (property "Datasheet" "~" (id 3) (at 194.31 200.66 0))
  )
  (symbol (lib_id "Device:C") (at 261.62 67.31 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C4" (id 0) (at 265.43 66.04 0))
    (property "Value" "22uf" (id 1) (at 262.89 69.85 0))
    (property "Footprint" "Capacitor_SMD:C_0805_2012Metric" (id 2) (at 262.5852 71.12 0))
    (property "Datasheet" "~" (id 3) (at 261.62 67.31 0))
  )
  (symbol (lib_id "Device:C") (at 289.56 68.58 90) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C5" (id 0) (at 287.02 66.04 90))
    (property "Value" "10nf" (id 1) (at 292.1 66.04 90))
    (property "Footprint" "Capacitor_SMD:C_0402_1005Metric" (id 2) (at 293.37 67.6148 0))
    (property "Datasheet" "~" (id 3) (at 289.56 68.58 0))
  )
  (symbol (lib_id "Device:C") (at 298.45 72.39 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C56" (id 0) (at 302.26 71.12 0))
    (property "Value" "100uf" (id 1) (at 299.72 74.93 0))
    (property "Footprint" "Capacitor_SMD:C_1206_3216Metric" (id 2) (at 299.4152 76.2 0))
    (property "Datasheet" "~" (id 3) (at 298.45 72.39 0))
  )
  (symbol (lib_id "Device:C") (at 323.85 120.65 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C6" (id 0) (at 326.771 119.4816 0))
    (property "Value" "27pF" (id 1) (at 326.771 121.793 0))
    (property "Footprint" "Capacitor_SMD:C_0402_1005Metric" (id 2) (at 324.8152 124.46 0))
    (property "Datasheet" "https://search.murata.co.jp/Ceramy/image/img/A01X/G101/ENG/GJM1555C1H270JB01-01.pdf" (id 3) (at 323.85 120.65 0))
    (property "Field8" "UCAP00738 " (id 4) (at 323.85 120.65 0))
    (property "Field5" "490-17672-1-ND" (id 5) (at 323.85 120.65 0))
    (property "Field6" "GJM1555C1H270JB01D" (id 6) (at 323.85 120.65 0))
    (property "Field7" "Murata" (id 7) (at 323.85 120.65 0))
    (property "Part Description" "	27pF 5% 50V Ceramic Capacitor C0G, NP0 0402 (1005 Metric)" (id 8) (at 323.85 120.65 0))
    (property "Field4" "Digikey" (id 4) (at 323.85 120.65 0))
  )
  (symbol (lib_id "Device:C") (at 331.47 120.65 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C7" (id 0) (at 333.121 118.2116 0))
    (property "Value" "27pF" (id 1) (at 333.121 116.713 0))
    (property "Footprint" "Capacitor_SMD:C_0402_1005Metric" (id 2) (at 332.4352 124.46 0))
    (property "Datasheet" "https://search.murata.co.jp/Ceramy/image/img/A01X/G101/ENG/GJM1555C1H270JB01-01.pdf" (id 3) (at 331.47 120.65 0))
    (property "Field8" "UCAP00738 " (id 4) (at 331.47 120.65 0))
    (property "Field5" "490-17672-1-ND" (id 5) (at 331.47 120.65 0))
    (property "Field6" "GJM1555C1H270JB01D" (id 6) (at 331.47 120.65 0))
    (property "Field7" "Murata" (id 7) (at 331.47 120.65 0))
    (property "Part Description" "	27pF 5% 50V Ceramic Capacitor C0G, NP0 0402 (1005 Metric)" (id 8) (at 331.47 120.65 0))
    (property "Field4" "Digikey" (id 4) (at 331.47 120.65 0))
  )
  (symbol (lib_id "Device:Crystal") (at 327.66 116.84 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "Y1" (id 0) (at 327.66 111.125 0))
    (property "Value" "24MHz" (id 1) (at 327.66 113.03 0))
    (property "Footprint" "Crystal:Crystal_SMD_EuroQuartz_MT-4Pin_3.2x2.5mm" (id 2) (at 327.66 116.84 0))
    (property "Datasheet" "~" (id 3) (at 327.66 116.84 0))
    (property "Field4" "Farnell" (id 4) (at 327.66 116.84 0))
    (property "Field5" "2508493" (id 5) (at 327.66 116.84 0))
    (property "Field7" "AEL" (id 6) (at 327.66 116.84 0))
    (property "Field6" "X24M000000S128" (id 7) (at 327.66 116.84 0))
    (property "Part Description" "24MHz Crystal 18pf 30ppm 30ppm" (id 8) (at 327.66 116.84 0))
  )
  (symbol (lib_id "Connector:Conn_01x11_Female") (at 157.48 158.75 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "J3" (id 0) (at 158.75 158.75 0))
    (property "Value" "Conn_01x10_Female" (id 1) (at 158.75 161.29 0))
    (property "Footprint" "Connector_PinHeader_2.54mm:PinHeader_2x06_P2.54mm_Horizontal" (id 2) (at 157.48 158.75 0))
    (property "Datasheet" "" (id 3) (at 157.48 158.75 0))
  )
  (symbol (lib_id "CM4IO:74LVC1G07_copy") (at 27.94 170.18 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "U15" (id 0) (at 30.48 163.83 0))
    (property "Value" "74LVC1G07SE-7" (id 1) (at 37.084 166.37 0))
    (property "Footprint" "Package_TO_SOT_SMD:SOT-353_SC-70-5" (id 2) (at 27.94 170.18 0))
    (property "Datasheet" "https://www.diodes.com/assets/Datasheets/74LVC1G07.pdf" (id 3) (at 27.94 170.18 0))
    (property "Field4" "Farnell" (id 4) (at 27.94 170.18 0))
    (property "Field5" "2425492" (id 5) (at 27.94 170.18 0))
    (property "Field6" "74LVC1G07SE-7" (id 6) (at 27.94 170.18 0))
    (property "Field7" "Diodes" (id 7) (at 27.94 170.18 0))
    (property "Part Description" "Buffer, Non-Inverting 1 Element 1 Bit per Element Open Drain Output SOT-353" (id 8) (at 27.94 170.18 0))
  )
  (symbol (lib_id "CM4IO:74LVC1G07_copy") (at 183.388 145.542 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "U16" (id 0) (at 184.912 143.002 0))
    (property "Value" "74LVC1G07SE-7" (id 1) (at 184.912 148.082 0))
    (property "Footprint" "Package_TO_SOT_SMD:SOT-353_SC-70-5" (id 2) (at 183.388 145.542 0))
    (property "Datasheet" "https://www.diodes.com/assets/Datasheets/74LVC1G07.pdf" (id 3) (at 183.388 145.542 0))
    (property "Field4" "Farnell" (id 4) (at 183.388 145.542 0))
    (property "Field5" "2425492" (id 5) (at 183.388 145.542 0))
    (property "Field6" "74LVC1G07SE-7" (id 6) (at 183.388 145.542 0))
    (property "Field7" "Diodes" (id 7) (at 183.388 145.542 0))
    (property "Part Description" "Buffer, Non-Inverting 1 Element 1 Bit per Element Open Drain Output SOT-353" (id 8) (at 183.388 145.542 0))
  )
  (symbol (lib_id "Connector:USB_OTG") (at 313.055 36.83 0) (mirror y) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "J21" (id 0) (at 318.897 37.1094 0))
    (property "Value" "USB_OTG" (id 1) (at 318.897 39.4208 0))
    (property "Footprint" "CM4IO:USB_Micro-B_EDAC_UCON00686" (id 2) (at 309.245 38.1 0))
    (property "Datasheet" "https://cdn.amphenol-icc.com/media/wysiwyg/files/documentation/datasheet/inputoutput/io_usb_micro.pd" (id 3) (at 309.245 38.1 0))
    (property "Field4" "Digikey" (id 4) (at 313.055 36.83 0))
    (property "Field5" "609-4050-2-ND" (id 5) (at 313.055 36.83 0))
    (property "Field6" "690-005-298-486" (id 6) (at 313.055 36.83 0))
    (property "Field7" "EDAC" (id 7) (at 313.055 36.83 0))
    (property "Part Description" "USB - micro B USB 2.0 Receptacle Connector 5 Position Surface Mount, Right Angle; Through Hole" (id 8) (at 313.055 36.83 0))
    (property "Field8" "UCON00686" (id 9) (at 313.055 36.83 0))
  )
  (symbol (lib_id "Connector:USB_A") (at 332.74 26.67 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "J5" (id 0) (at 335.28 13.97 0))
    (property "Value" "USB_A" (id 1) (at 335.28 16.51 0))
    (property "Footprint" "Connector_USB:USB_A_Wuerth_614004134726_Horizontal" (id 2) (at 336.55 27.94 0))
    (property "Datasheet" " ~" (id 3) (at 336.55 27.94 0))
  )
  (symbol (lib_id "Connector:USB_A") (at 335.28 52.07 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "J6" (id 0) (at 337.82 39.37 0))
    (property "Value" "USB_A" (id 1) (at 337.82 41.91 0))
    (property "Footprint" "Connector_USB:USB_A_Wuerth_614004134726_Horizontal" (id 2) (at 339.09 53.34 0))
    (property "Datasheet" " ~" (id 3) (at 339.09 53.34 0))
  )
  (symbol (lib_id "Connector:USB_A") (at 359.41 26.67 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "J7" (id 0) (at 361.95 13.97 0))
    (property "Value" "USB_A" (id 1) (at 361.95 16.51 0))
    (property "Footprint" "Connector_USB:USB_A_Wuerth_614004134726_Horizontal" (id 2) (at 363.22 27.94 0))
    (property "Datasheet" " ~" (id 3) (at 363.22 27.94 0))
  )
  (symbol (lib_id "Connector:USB_A") (at 361.95 52.07 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "J9" (id 0) (at 364.49 39.37 0))
    (property "Value" "USB_A" (id 1) (at 364.49 41.91 0))
    (property "Footprint" "Connector_USB:USB_A_Wuerth_614004134726_Horizontal" (id 2) (at 365.76 53.34 0))
    (property "Datasheet" " ~" (id 3) (at 365.76 53.34 0))
  )
  (symbol (lib_id "Connector_Generic:Conn_02x07_Odd_Even") (at 71.374 162.56 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "J14" (id 0) (at 72.644 149.4536 0))
    (property "Value" "Conn_02x07_Odd_Even" (id 1) (at 72.644 151.765 0))
    (property "Footprint" "Connector_PinHeader_2.54mm:PinHeader_2x07_P2.54mm_Vertical" (id 2) (at 71.374 162.56 0))
    (property "Datasheet" "https://www.toby.co.uk/uploads/publications/1673.pdf" (id 3) (at 71.374 162.56 0))
    (property "Field4" "Toby" (id 4) (at 71.374 162.56 0))
    (property "Field5" "THD-07-R" (id 5) (at 71.374 162.56 0))
    (property "Field6" "THD-07-R" (id 6) (at 71.374 162.56 0))
    (property "Field7" "Toby" (id 7) (at 71.374 162.56 0))
    (property "Part Description" "PinHeader_2x07_P2.54mm_Vertical" (id 8) (at 71.374 162.56 0))
  )
  (symbol (lib_id "Connector:Conn_01x22_Female") (at 123.19 248.92 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "J16" (id 0) (at 100.33 219.71 0))
    (property "Value" "Conn_01x22_Female" (id 1) (at 118.11 279.4 0))
    (property "Footprint" "Connector_FFC-FPC:Hirose_FH12-22S-0.5SH_1x22-1MP_P0.50mm_Horizontal" (id 2) (at 123.19 248.92 0))
    (property "Datasheet" "https://www.hirose.com/product/document?clcode=&productname=&series=FH12&documenttype=Catalog&lang=en&documentid=D31648_en" (id 3) (at 123.19 248.92 0))
    (property "Field4" "Mouser" (id 4) (at 123.19 248.92 0))
    (property "Field5" "798-FH12-22S-0.5SH55" (id 5) (at 123.19 248.92 0))
    (property "Field6" "FH12-22S-0.5SH55" (id 6) (at 123.19 248.92 0))
    (property "Field7" "Hirose" (id 7) (at 123.19 248.92 0))
    (property "Part Description" "22 Position FFC, FPC Connector Contacts, Bottom 0.020\" (0.50mm) Surface Mount, Right Angle" (id 8) (at 123.19 248.92 0))
  )
  (symbol (lib_id "Connector:Conn_01x22_Female") (at 153.67 248.92 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "J2" (id 0) (at 130.81 219.71 0))
    (property "Value" "Conn_01x22_Female" (id 1) (at 148.59 279.4 0))
    (property "Footprint" "Connector_FFC-FPC:Hirose_FH12-22S-0.5SH_1x22-1MP_P0.50mm_Horizontal" (id 2) (at 153.67 248.92 0))
    (property "Datasheet" "https://www.hirose.com/product/document?clcode=&productname=&series=FH12&documenttype=Catalog&lang=en&documentid=D31648_en" (id 3) (at 153.67 248.92 0))
    (property "Field4" "Mouser" (id 4) (at 153.67 248.92 0))
    (property "Field5" "798-FH12-22S-0.5SH55" (id 5) (at 153.67 248.92 0))
    (property "Field6" "FH12-22S-0.5SH55" (id 6) (at 153.67 248.92 0))
    (property "Field7" "Hirose" (id 7) (at 153.67 248.92 0))
    (property "Part Description" "22 Position FFC, FPC Connector Contacts, Bottom 0.020\" (0.50mm) Surface Mount, Right Angle" (id 8) (at 153.67 248.92 0))
  )
  (symbol (lib_id "Regulator_Switching:LM22676MR-ADJ") (at 171.45 196.85 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "U1" (id 0) (at 171.45 184.15 0))
    (property "Value" "LM22676MR-5" (id 1) (at 171.45 186.69 0))
    (property "Footprint" "Package_SO:TI_SO-PowerPAD-8" (id 2) (at 171.45 185.42 0))
    (property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm22676.pdf" (id 3) (at 172.72 196.85 0))
  )
  (symbol (lib_id "Regulator_Switching:LM22676MR-ADJ") (at 275.59 68.58 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "U2" (id 0) (at 275.59 55.88 0))
    (property "Value" "LM22676MR-ADJ" (id 1) (at 275.59 58.42 0))
    (property "Footprint" "Package_SO:TI_SO-PowerPAD-8" (id 2) (at 275.59 57.15 0))
    (property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm22676.pdf" (id 3) (at 276.86 68.58 0))
  )
  (symbol (lib_id "CM4IO:FSUSB42MX") (at 283.21 40.64 0) (mirror y) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "U21" (id 0) (at 284.48 17.399 0))
    (property "Value" "FSUSB42MUX" (id 1) (at 284.48 19.7104 0))
    (property "Footprint" "Package_SO:MSOP-10_3x3mm_P0.5mm" (id 2) (at 283.21 40.64 0))
    (property "Datasheet" "https://www.onsemi.com/pub/Collateral/FSUSB42-D.PDF" (id 3) (at 283.21 40.64 0))
    (property "Field4" "Farnell" (id 4) (at 283.21 40.64 0))
    (property "Field5" "2564479" (id 5) (at 283.21 40.64 0))
    (property "Field6" "FSUSB42MUX" (id 6) (at 283.21 40.64 0))
    (property "Field7" "Onsemi" (id 7) (at 283.21 40.64 0))
    (property "Part Description" "USB Switch IC 1 Channel 10-MSOP" (id 8) (at 283.21 40.64 0))
  )
  (symbol (lib_id "Connector_Generic:Conn_02x17_Odd_Even") (at 157.48 44.45 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "J8" (id 0) (at 158.75 17.78 0))
    (property "Value" "THD-20-R" (id 1) (at 158.75 20.32 0))
    (property "Footprint" "Connector_PinHeader_2.54mm:PinHeader_2x17_P2.54mm_Vertical" (id 2) (at 157.48 44.45 0))
    (property "Datasheet" "~" (id 3) (at 157.48 44.45 0))
  )
  (symbol (lib_id "CM4IO:HDMI_A_1.4") (at 342.9 186.69 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "J4" (id 0) (at 347.98 160.02 0))
    (property "Value" "690-019-298-412" (id 1) (at 340.36 218.44 0))
    (property "Footprint" "Connector_HDMI:HDMI_Micro-D_Molex_46765-1x01" (id 2) (at 343.535 186.69 0))
    (property "Datasheet" "https://www.tme.eu/Document/f15dffbcfad8545e17826f72d36911c8/206A-SEAN-R03.pdf" (id 3) (at 343.535 186.69 0))
    (property "Field4" "Farnell" (id 4) (at 342.9 186.69 0))
    (property "Field5" "2614936" (id 5) (at 342.9 186.69 0))
    (property "Field6" "690-019-298-412" (id 6) (at 342.9 186.69 0))
    (property "Field7" "EDAC" (id 7) (at 342.9 186.69 0))
    (property "Part Description" "HDMI Connector, Right Angle, 19 Contacts, Receptacle, Surface Mount, Surface Mount Right Angle" (id 8) (at 342.9 186.69 0))
    (property "Field8" "UCON00802" (id 9) (at 342.9 186.69 0))
  )
  (symbol (lib_id "CM4IO:HDMI_A_1.4") (at 391.16 182.88 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "J25" (id 0) (at 396.24 156.21 0))
    (property "Value" "690-019-298-412" (id 1) (at 388.62 214.63 0))
    (property "Footprint" "Connector_HDMI:HDMI_Micro-D_Molex_46765-1x01" (id 2) (at 391.795 182.88 0))
    (property "Datasheet" "https://www.tme.eu/Document/f15dffbcfad8545e17826f72d36911c8/206A-SEAN-R03.pdf" (id 3) (at 391.795 182.88 0))
    (property "Field4" "Farnell" (id 4) (at 391.16 182.88 0))
    (property "Field5" "2614936" (id 5) (at 391.16 182.88 0))
    (property "Field6" "690-019-298-412" (id 6) (at 391.16 182.88 0))
    (property "Field7" "EDAC" (id 7) (at 391.16 182.88 0))
    (property "Part Description" "HDMI Connector, Right Angle, 19 Contacts, Receptacle, Surface Mount, Surface Mount Right Angle" (id 8) (at 391.16 182.88 0))
    (property "Field8" "UCON00802" (id 9) (at 391.16 182.88 0))
  )
  (symbol (lib_id "CM4IO:PCIe-x1") (at 219.71 59.69 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "J20" (id 0) (at 223.52 22.86 0))
    (property "Value" "10018783-11200TLF" (id 1) (at 215.265 22.2504 0))
    (property "Footprint" "CM4IO:PCIex1-36" (id 2) (at 219.71 59.69 0))
    (property "Datasheet" "https://www.mouser.co.uk/datasheet/2/18/10018783-1525093.pdf" (id 3) (at 219.71 59.69 0))
    (property "Field4" "Mouser" (id 4) (at 219.71 59.69 0))
    (property "Field5" "649-10018783-1200TLF" (id 5) (at 219.71 59.69 0))
    (property "Part Description" "PCI Express/PCI Connectors PCIE THROUGH HOLE 36P" (id 6) (at 219.71 59.69 0))
    (property "Field6" "10018783-11200TLF" (id 7) (at 219.71 59.69 0))
    (property "Field7" "Amphenol FCI" (id 8) (at 219.71 59.69 0))
  )
  (symbol (lib_id "Connector:Micro_SD_Card_Det") (at 66.04 245.11 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "J13" (id 0) (at 64.77 224.3582 0))
    (property "Value" "Micro_SD_Card_Det" (id 1) (at 64.77 226.6696 0))
    (property "Footprint" "CM4IO:SD_slot" (id 2) (at 118.11 227.33 0))
    (property "Datasheet" "https://www.hirose.com/product/en/download_file/key_name/DM3/category/Catalog/doc_file_id/49662/?file_category_id=4&item_id=195&is_series=1" (id 3) (at 66.04 242.57 0))
    (property "Field4" "Farnell" (id 4) (at 66.04 245.11 0))
    (property "Field5" "2358234" (id 5) (at 66.04 245.11 0))
    (property "Field6" "503398-1892" (id 6) (at 66.04 245.11 0))
    (property "Field7" "Molex" (id 7) (at 66.04 245.11 0))
    (property "Part Description" "9 (8 + 1) Position Card Connector microSD™ Surface Mount, Right Angle Gold" (id 8) (at 66.04 245.11 0))
    (property "Field8" "UCON00512" (id 9) (at 66.04 245.11 0))
  )
  (symbol (lib_id "Interface_USB:USB2514B_Bi") (at 368.3 105.41 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "U3" (id 0) (at 368.3 145.7706 0))
    (property "Value" "USB2514B-I/M2" (id 1) (at 351.79 146.05 0))
    (property "Footprint" "Package_DFN_QFN:QFN-36-1EP_6x6mm_P0.5mm_EP3.7x3.7mm" (id 2) (at 401.32 143.51 0))
    (property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/00001692C.pdf" (id 3) (at 408.94 146.05 0))
    (property "Field4" "Farnell" (id 4) (at 368.3 105.41 0))
    (property "Field5" "2775060" (id 5) (at 368.3 105.41 0))
    (property "Field6" "USB2514B-I/M2" (id 6) (at 368.3 105.41 0))
    (property "Field7" "Microchip" (id 7) (at 368.3 105.41 0))
    (property "Part Description" "	USB Hub Controller USB Interface 36-SQFN (6x6)" (id 8) (at 368.3 105.41 0))
    (property "Field8" "UICC00931" (id 9) (at 368.3 105.41 0))
  )
  (symbol (lib_id "CM4IO:ComputeModule4-CM4") (at 72.136 74.93 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "Module2" (id 0) (at 69.596 13.335 0))
    (property "Value" "ComputeModule4" (id 1) (at 69.596 15.6464 0))
    (property "Footprint" "CM4IO:Raspberry-Pi-4-Compute-Module" (id 2) (at 214.376 101.6 0))
    (property "Datasheet" "" (id 3) (at 214.376 101.6 0))
    (property "Field4" "Hirose" (id 4) (at 72.136 74.93 0))
    (property "Field5" "2off DF40C-100DS-0.4V" (id 5) (at 72.136 74.93 0))
    (property "Field6" "2off DF40C-100DS-0.4V" (id 6) (at 72.136 74.93 0))
    (property "Field7" "Hirose" (id 7) (at 72.136 74.93 0))
    (property "Part Description" "	100 Position Connector Receptacle, Center Strip Contacts Surface Mount Gold" (id 8) (at 72.136 74.93 0))
  )
  (symbol (lib_id "CM4IO:ComputeModule4-CM4") (at 120.65 167.64 0) (unit 2)
    (in_bom yes) (on_board yes)
    (property "Reference" "Module2" (id 0) (at 260.35 95.377 0))
    (property "Value" "ComputeModule4" (id 1) (at 260.35 97.6884 0))
    (property "Footprint" "CM4IO:Raspberry-Pi-4-Compute-Module" (id 2) (at 262.89 194.31 0))
    (property "Datasheet" "" (id 3) (at 262.89 194.31 0))
    (property "Field4" "Hirose" (id 4) (at 260.35 99.9744 0))
    (property "Field5" "2off DF40C-100DS-0.4V" (id 5) (at 260.35 102.2858 0))
    (property "Field6" "2off DF40C-100DS-0.4V" (id 6) (at 120.65 167.64 0))
    (property "Field7" "Hirose" (id 7) (at 120.65 167.64 0))
    (property "Part Description" "	100 Position Connector Receptacle, Center Strip Contacts Surface Mount Gold" (id 8) (at 120.65 167.64 0))
  )
  (sheet_instances
    (path (page "1"))
  )
  (symbol_instances
    (path
      (reference "#PWR061") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR062") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR063") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR064") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR065") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR066") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR067") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR073") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR075") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR077") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR078") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR079") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR080") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR081") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR085") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR099") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR0101") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR0102") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR0103") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR0104") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR0105") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR0106") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR0107") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR0108") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR0109") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR0110") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR0111") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR0112") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR0113") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR0114") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR0115") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR0116") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR0117") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR0118") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR0119") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR0120") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR0121") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR0122") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR?") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "C1") (unit 1) (value "22uf") (footprint "Capacitor_SMD:C_1206_3216Metric")
    )
    (path
      (reference "C2") (unit 1) (value "100nf") (footprint "Capacitor_SMD:C_0402_1005Metric")
    )
    (path
      (reference "C3") (unit 1) (value "100uf") (footprint "Capacitor_SMD:C_1206_3216Metric")
    )
    (path
      (reference "C4") (unit 1) (value "22uf") (footprint "Capacitor_SMD:C_0805_2012Metric")
    )
    (path
      (reference "C5") (unit 1) (value "10nf") (footprint "Capacitor_SMD:C_0402_1005Metric")
    )
    (path
      (reference "C6") (unit 1) (value "27pF") (footprint "Capacitor_SMD:C_0402_1005Metric")
    )
    (path
      (reference "C7") (unit 1) (value "27pF") (footprint "Capacitor_SMD:C_0402_1005Metric")
    )
    (path
      (reference "C46") (unit 1) (value "10u") (footprint "Capacitor_SMD:C_0805_2012Metric")
    )
    (path
      (reference "C47") (unit 1) (value "10u") (footprint "Capacitor_SMD:C_0805_2012Metric")
    )
    (path
      (reference "C48") (unit 1) (value "10u") (footprint "Capacitor_SMD:C_0805_2012Metric")
    )
    (path
      (reference "C49") (unit 1) (value "100n") (footprint "Capacitor_SMD:C_0402_1005Metric")
    )
    (path
      (reference "C50") (unit 1) (value "100n") (footprint "Capacitor_SMD:C_0402_1005Metric")
    )
    (path
      (reference "C51") (unit 1) (value "100n") (footprint "Capacitor_SMD:C_0402_1005Metric")
    )
    (path
      (reference "C52") (unit 1) (value "100n") (footprint "Capacitor_SMD:C_0402_1005Metric")
    )
    (path
      (reference "C53") (unit 1) (value "100n") (footprint "Capacitor_SMD:C_0402_1005Metric")
    )
    (path
      (reference "C54") (unit 1) (value "100n") (footprint "Capacitor_SMD:C_0402_1005Metric")
    )
    (path
      (reference "C56") (unit 1) (value "100uf") (footprint "Capacitor_SMD:C_1206_3216Metric")
    )
    (path
      (reference "C57") (unit 1) (value "10uf") (footprint "Capacitor_SMD:C_0805_2012Metric")
    )
    (path
      (reference "C58") (unit 1) (value "10uf") (footprint "Capacitor_SMD:C_0805_2012Metric")
    )
    (path
      (reference "C59") (unit 1) (value "22uf") (footprint "Capacitor_SMD:C_0805_2012Metric")
    )
    (path
      (reference "C60") (unit 1) (value "10uf") (footprint "Capacitor_SMD:C_0805_2012Metric")
    )
    (path
      (reference "C61") (unit 1) (value "10uf") (footprint "Capacitor_SMD:C_0805_2012Metric")
    )
    (path
      (reference "C62") (unit 1) (value "22uf") (footprint "Capacitor_SMD:C_0805_2012Metric")
    )
    (path
      (reference "C63") (unit 1) (value "10uf") (footprint "Capacitor_SMD:C_0805_2012Metric")
    )
    (path
      (reference "C64") (unit 1) (value "10uf") (footprint "Capacitor_SMD:C_0805_2012Metric")
    )
    (path
      (reference "C65") (unit 1) (value "22uf") (footprint "Capacitor_SMD:C_0805_2012Metric")
    )
    (path
      (reference "C66") (unit 1) (value "10uf") (footprint "Capacitor_SMD:C_0805_2012Metric")
    )
    (path
      (reference "C67") (unit 1) (value "10uf") (footprint "Capacitor_SMD:C_0805_2012Metric")
    )
    (path
      (reference "D1") (unit 1) (value "SS36") (footprint "Diode_SMD:D_SMA")
    )
    (path
      (reference "D2") (unit 1) (value "SS36") (footprint "Diode_SMD:D_SMA")
    )
    (path
      (reference "D3") (unit 1) (value "SS36") (footprint "Diode_SMD:D_SMA")
    )
    (path
      (reference "D16") (unit 1) (value "LED Green") (footprint "LED_SMD:LED_0603_1608Metric")
    )
    (path
      (reference "D17") (unit 1) (value "LED yellow") (footprint "LED_SMD:LED_0603_1608Metric")
    )
    (path
      (reference "D18") (unit 1) (value "LED green") (footprint "LED_SMD:LED_0603_1608Metric")
    )
    (path
      (reference "D20") (unit 1) (value "LED Red") (footprint "LED_SMD:LED_0603_1608Metric")
    )
    (path
      (reference "J1") (unit 1) (value "Conn_01x02_Female") (footprint "Connector_BarrelJack:BarrelJack_CLIFF_FC681465S_SMT_Horizontal")
    )
    (path
      (reference "J2") (unit 1) (value "Conn_01x22_Female") (footprint "Connector_FFC-FPC:Hirose_FH12-22S-0.5SH_1x22-1MP_P0.50mm_Horizontal")
    )
    (path
      (reference "J3") (unit 1) (value "Conn_01x10_Female") (footprint "Connector_PinHeader_2.54mm:PinHeader_2x06_P2.54mm_Horizontal")
    )
    (path
      (reference "J4") (unit 1) (value "690-019-298-412") (footprint "Connector_HDMI:HDMI_Micro-D_Molex_46765-1x01")
    )
    (path
      (reference "J5") (unit 1) (value "USB_A") (footprint "Connector_USB:USB_A_Wuerth_614004134726_Horizontal")
    )
    (path
      (reference "J6") (unit 1) (value "USB_A") (footprint "Connector_USB:USB_A_Wuerth_614004134726_Horizontal")
    )
    (path
      (reference "J7") (unit 1) (value "USB_A") (footprint "Connector_USB:USB_A_Wuerth_614004134726_Horizontal")
    )
    (path
      (reference "J8") (unit 1) (value "THD-20-R") (footprint "Connector_PinHeader_2.54mm:PinHeader_2x17_P2.54mm_Vertical")
    )
    (path
      (reference "J9") (unit 1) (value "USB_A") (footprint "Connector_USB:USB_A_Wuerth_614004134726_Horizontal")
    )
    (path
      (reference "J13") (unit 1) (value "Micro_SD_Card_Det") (footprint "CM4IO:SD_slot")
    )
    (path
      (reference "J14") (unit 1) (value "Conn_02x07_Odd_Even") (footprint "Connector_PinHeader_2.54mm:PinHeader_2x07_P2.54mm_Vertical")
    )
    (path
      (reference "J16") (unit 1) (value "Conn_01x22_Female") (footprint "Connector_FFC-FPC:Hirose_FH12-22S-0.5SH_1x22-1MP_P0.50mm_Horizontal")
    )
    (path
      (reference "J20") (unit 1) (value "10018783-11200TLF") (footprint "CM4IO:PCIex1-36")
    )
    (path
      (reference "J21") (unit 1) (value "USB_OTG") (footprint "CM4IO:USB_Micro-B_EDAC_UCON00686")
    )
    (path
      (reference "J25") (unit 1) (value "690-019-298-412") (footprint "Connector_HDMI:HDMI_Micro-D_Molex_46765-1x01")
    )
    (path
      (reference "L1") (unit 1) (value "6.8uh") (footprint "Inductor_SMD:L_1206_3216Metric")
    )
    (path
      (reference "L2") (unit 1) (value "6.8uh") (footprint "Inductor_SMD:L_1206_3216Metric")
    )
    (path
      (reference "Module2") (unit 1) (value "ComputeModule4") (footprint "CM4IO:Raspberry-Pi-4-Compute-Module")
    )
    (path
      (reference "Module2") (unit 2) (value "ComputeModule4") (footprint "CM4IO:Raspberry-Pi-4-Compute-Module")
    )
    (path
      (reference "R0") (unit 1) (value "0R") (footprint "Resistor_SMD:R_1206_3216Metric")
    )
    (path
      (reference "R1") (unit 1) (value "3k") (footprint "Resistor_SMD:R_0402_1005Metric")
    )
    (path
      (reference "R2") (unit 1) (value "4.7k") (footprint "Resistor_SMD:R_0402_1005Metric")
    )
    (path
      (reference "R3") (unit 1) (value "36K 1%") (footprint "Resistor_SMD:R_0402_1005Metric")
    )
    (path
      (reference "R4") (unit 1) (value "12K 1%") (footprint "Resistor_SMD:R_0402_1005Metric")
    )
    (path
      (reference "R5") (unit 1) (value "36K 1%") (footprint "Resistor_SMD:R_0402_1005Metric")
    )
    (path
      (reference "R6") (unit 1) (value "36K 1%") (footprint "Resistor_SMD:R_0402_1005Metric")
    )
    (path
      (reference "R7") (unit 1) (value "36K 1%") (footprint "Resistor_SMD:R_0402_1005Metric")
    )
    (path
      (reference "R43") (unit 1) (value "nf") (footprint "Resistor_SMD:R_0402_1005Metric")
    )
    (path
      (reference "R44") (unit 1) (value "nf") (footprint "Resistor_SMD:R_0402_1005Metric")
    )
    (path
      (reference "R45") (unit 1) (value "1k") (footprint "Resistor_SMD:R_0402_1005Metric")
    )
    (path
      (reference "R46") (unit 1) (value "470R") (footprint "Resistor_SMD:R_0402_1005Metric")
    )
    (path
      (reference "R47") (unit 1) (value "470R") (footprint "Resistor_SMD:R_0402_1005Metric")
    )
    (path
      (reference "R48") (unit 1) (value "1k") (footprint "Resistor_SMD:R_0402_1005Metric")
    )
    (path
      (reference "R49") (unit 1) (value "2.2K 1%") (footprint "Resistor_SMD:R_0402_1005Metric")
    )
    (path
      (reference "R50") (unit 1) (value "2.2K 1%") (footprint "Resistor_SMD:R_0402_1005Metric")
    )
    (path
      (reference "TP5") (unit 1) (value "TestPoint") (footprint "TestPoint:TestPoint_Pad_2.0x2.0mm")
    )
    (path
      (reference "TP6") (unit 1) (value "TestPoint") (footprint "TestPoint:TestPoint_Pad_2.0x2.0mm")
    )
    (path
      (reference "U1") (unit 1) (value "LM22676MR-5") (footprint "Package_SO:TI_SO-PowerPAD-8")
    )
    (path
      (reference "U2") (unit 1) (value "LM22676MR-ADJ") (footprint "Package_SO:TI_SO-PowerPAD-8")
    )
    (path
      (reference "U3") (unit 1) (value "USB2514B-I/M2") (footprint "Package_DFN_QFN:QFN-36-1EP_6x6mm_P0.5mm_EP3.7x3.7mm")
    )
    (path
      (reference "U15") (unit 1) (value "74LVC1G07SE-7") (footprint "Package_TO_SOT_SMD:SOT-353_SC-70-5")
    )
    (path
      (reference "U16") (unit 1) (value "74LVC1G07SE-7") (footprint "Package_TO_SOT_SMD:SOT-353_SC-70-5")
    )
    (path
      (reference "U21") (unit 1) (value "FSUSB42MUX") (footprint "Package_SO:MSOP-10_3x3mm_P0.5mm")
    )
    (path
      (reference "Y1") (unit 1) (value "24MHz") (footprint "Crystal:Crystal_SMD_EuroQuartz_MT-4Pin_3.2x2.5mm")
    )
  )
)
