(module "Hirose_FH12-22S-0.5SH_1x22-1MP_P0.50mm_Horizontal" (layer F.Cu) (tedit 5EBC289E)
  (descr "Molex FH12, FFC/FPC connector, FH12-22S-0.5SH, 22 Pins per row (https://www.hirose.com/product/en/products/FH12/FH12-24S-0.5SH(55)/), generated with kicad-footprint-generator")
  (tags "connector Hirose  top entry")
  (attr smd)
  (fp_text reference "HirsoeFH12-22S-05SH_1x22-1MP4" (at 0 -3.7 180) (layer F.Fab))
  (fp_text value "Conn_01x22_Female" (at 0 5.6 180) (layer F.Fab))
  (fp_text user "${REFERENCE}" (at 0 3.7 180) (layer F.Fab))
  (pad "1" smd rect (at 5.25 -1.85) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "2" smd rect (at 4.75 -1.85) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "3" smd rect (at 4.25 -1.85) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "4" smd rect (at 3.75 -1.85) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "5" smd rect (at 3.25 -1.85) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "6" smd rect (at 2.75 -1.85) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "7" smd rect (at 2.25 -1.85) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "8" smd rect (at 1.75 -1.85) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "9" smd rect (at 1.25 -1.85) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "10" smd rect (at 0.75 -1.85) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "11" smd rect (at 0.25 -1.85) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "12" smd rect (at -0.25 -1.85) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "13" smd rect (at -0.75 -1.85) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "14" smd rect (at -1.25 -1.85) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "15" smd rect (at -1.75 -1.85) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "16" smd rect (at -2.25 -1.85) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "17" smd rect (at -2.75 -1.85) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "18" smd rect (at -3.25 -1.85) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "19" smd rect (at -3.75 -1.85) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "20" smd rect (at -4.25 -1.85) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "21" smd rect (at -4.75 -1.85) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "22" smd rect (at -5.25 -1.85) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "MP" smd rect (at -7.15 1.4) (size 1.8 2.2) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "MP" smd rect (at 7.15 1.4) (size 1.8 2.2) (layers "F.Cu" "F.Paste" "F.Mask"))
  (model "./CM4IO.3dshapes/FH12-22S-0.5SHa.stp"
    (offset (xyz 16.5 -10.6 2))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 90 180))
  )
)
