(footprint "SD_slot" (version 20201116) (generator pcbnew) (layer "F.Cu")
  (tedit 5FED7281)
  (fp_text reference "REF**" (at 0 -0.5 unlocked) (layer "User.5"))
  (fp_text value "SD_slot" (at 0 1 unlocked) (layer "F.Fab"))
  (fp_text user "${REFERENCE}" (at 0 2.5 unlocked) (layer "F.Fab"))
  (pad "" np_thru_hole circle (at -2.75 8.2) (size 0.95 0.95) (drill 0.95) (layers F&B.Cu *.Mask))
  (pad "" np_thru_hole circle (at 4.05 8.2) (size 0.95 0.95) (drill 0.95) (layers F&B.Cu *.Mask))
  (pad "1" smd rect (at 3.2 -3.22) (size 0.7 1.4) (layers "B.Cu" "B.Paste" "B.Mask"))
  (pad "2" smd rect (at 2.1 -3.22) (size 0.7 1.4) (layers "B.Cu" "B.Paste" "B.Mask"))
  (pad "3" smd rect (at 1 -3.22) (size 0.7 1.4) (layers "B.Cu" "B.Paste" "B.Mask"))
  (pad "4" smd rect (at -0.1 -3.22) (size 0.7 1.4) (layers "B.Cu" "B.Paste" "B.Mask"))
  (pad "5" smd rect (at -1.2 -3.22) (size 0.7 1.4) (layers "B.Cu" "B.Paste" "B.Mask"))
  (pad "6" smd rect (at -2.3 -3.22) (size 0.7 1.4) (layers "B.Cu" "B.Paste" "B.Mask"))
  (pad "7" smd rect (at -3.4 -3.22) (size 0.7 1.4) (layers "B.Cu" "B.Paste" "B.Mask"))
  (pad "8" smd rect (at -4.5 -3.22) (size 0.7 1.4) (layers "B.Cu" "B.Paste" "B.Mask"))
  (pad "9" smd rect (at -5.6 -3.22) (size 0.7 1.4) (layers "B.Cu" "B.Paste" "B.Mask"))
  (pad "11" smd rect (at 9.2 -1.22) (size 1.1 2.4) (layers "B.Cu" "B.Paste" "B.Mask"))
  (pad "11" smd rect (at -6.98 -1.22) (size 1.1 2.4) (layers "B.Cu" "B.Paste" "B.Mask"))
  (pad "11" smd rect (at -6.98 7.78) (size 1.1 2.4) (layers "B.Cu" "B.Paste" "B.Mask"))
  (pad "11" smd rect (at 9.2 7.78) (size 1.1 2.4) (layers "B.Cu" "B.Paste" "B.Mask"))
)
