(kicad_pcb (version 20201116) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "GND")
  (net 2 "Net-(C1-Pad1)")
  (net 3 "Net-(C2-Pad1)")
  (net 4 "/+5v")
  (net 5 "Net-(C13-Pad1)")
  (net 6 "Net-(C10-Pad1)")
  (net 7 "Net-(C18-Pad1)")
  (net 8 "Net-(C19-Pad1)")
  (net 9 "Net-(D1-Pad1)")
  (net 10 "Net-(D3-Pad1)")
  (net 11 "/+12v")
  (net 12 "Net-(D6-Pad1)")
  (net 13 "Net-(D7-Pad1)")
  (net 14 "Net-(D8-Pad1)")
  (net 15 "Net-(J2-Pad14)")
  (net 16 "Net-(J2-Pad13)")
  (net 17 "/P1_DN")
  (net 18 "/P1_DP")
  (net 19 "/P1_CN")
  (net 20 "/P1_CP")
  (net 21 "/P1_BN")
  (net 22 "/P1_BP")
  (net 23 "/P1_AN")
  (net 24 "/P1_AP")
  (net 25 "/P2_DN")
  (net 26 "/P2_DP")
  (net 27 "/P2_CN")
  (net 28 "/P2_CP")
  (net 29 "/P2_BN")
  (net 30 "/P2_BP")
  (net 31 "/P2_AN")
  (net 32 "/P2_AP")
  (net 33 "/P3_DN")
  (net 34 "/P3_DP")
  (net 35 "/P3_CN")
  (net 36 "/P3_CP")
  (net 37 "/P3_BN")
  (net 38 "/P3_BP")
  (net 39 "/P3_AN")
  (net 40 "/P3_AP")
  (net 41 "/P4_DN")
  (net 42 "/P4_DP")
  (net 43 "/P4_CN")
  (net 44 "/P4_CP")
  (net 45 "/P4_BN")
  (net 46 "/P4_BP")
  (net 47 "/P4_AN")
  (net 48 "/P4_AP")
  (net 49 "/P5_DN")
  (net 50 "/P5_DP")
  (net 51 "/P5_CN")
  (net 52 "/P5_CP")
  (net 53 "/P5_BN")
  (net 54 "/P5_BP")
  (net 55 "/P5_AN")
  (net 56 "/P5_AP")
  (net 57 "/P6_DN")
  (net 58 "/P6_DP")
  (net 59 "/P6_CN")
  (net 60 "/P6_CP")
  (net 61 "/P6_BN")
  (net 62 "/P6_BP")
  (net 63 "/P6_AN")
  (net 64 "/P6_AP")
  (net 65 "/P7_DN")
  (net 66 "/P7_DP")
  (net 67 "/P7_CN")
  (net 68 "/P7_CP")
  (net 69 "/P7_BN")
  (net 70 "/P7_BP")
  (net 71 "/P7_AN")
  (net 72 "/P7_AP")
  (net 73 "/P0_DN")
  (net 74 "/P0_DP")
  (net 75 "/P0_BN")
  (net 76 "/P0_CN")
  (net 77 "/P0_CP")
  (net 78 "/P0_BP")
  (net 79 "/P0_AN")
  (net 80 "/P0_AP")
  (net 81 "Net-(L3-Pad1)")
  (net 82 "<NO NET>")
  (net 83 "/switch/+1v")
  (net 84 "Net-(R13-Pad2)")
  (net 85 "/switch/nRESET")
  (net 86 "Net-(R33-Pad1)")
  (net 87 "Net-(R34-Pad1)")
  (net 88 "no_connect_126")
  (net 89 "/switch/SDA")
  (net 90 "/switch/SCK")
  (net 91 "Net-(U1-Pad94)")
  (net 92 "Net-(U1-Pad93)")
  (net 93 "Net-(U1-Pad91)")
  (net 94 "Net-(U1-Pad90)")
  (net 95 "Net-(U1-Pad89)")
  (net 96 "Net-(U1-Pad88)")
  (net 97 "Net-(U1-Pad87)")
  (net 98 "Net-(U1-Pad86)")
  (net 99 "Net-(U1-Pad85)")
  (net 100 "Net-(U1-Pad84)")
  (net 101 "Net-(U1-Pad83)")
  (net 102 "Net-(U1-Pad82)")
  (net 103 "Net-(U1-Pad81)")
  (net 104 "Net-(U1-Pad80)")
  (net 105 "Net-(U1-Pad79)")
  (net 106 "Net-(U1-Pad75)")
  (net 107 "Net-(U1-Pad74)")
  (net 108 "Net-(U1-Pad73)")
  (net 109 "Net-(U1-Pad72)")
  (net 110 "Net-(U1-Pad71)")
  (net 111 "/switch/SPI_CS")
  (net 112 "/switch/SPI_D0")
  (net 113 "/switch/SPI_D1")
  (net 114 "/switch/SPI_CLK")
  (net 115 "no_connect_128")
  (net 116 "no_connect_127")
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 117.91 44.97 -90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Field4" "Digikey")
    (property "Field5" "490-10505-1-ND")
    (property "Field6" "GRM21BC8YA106KE11L ")
    (property "Field7" "Murata")
    (property "Field8" "")
    (property "Part Description" "	10uF 10% or 20% 35V Ceramic Capacitor X6S 0805 (2012 Metric)")
    (property "Sheet file" "switch.kicad_sch")
    (property "Sheet name" "switch")
    (attr smd)
    (fp_text reference "C7" (at 2.28 0.56 180) (layer "F.SilkS"))
    (fp_text value "10u" (at 0 1.68 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.95 0 270) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 6 "Net-(C10-Pad1)"))
    (pad "2" smd roundrect (at 0.95 0 270) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (tedit 600ACDB3)
    (at 79.2 46.55 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheet file" "switch.kicad_sch")
    (property "Sheet name" "switch")
    (attr smd)
    (fp_text reference "C8" (at 1.88 1.61 90) (layer "F.SilkS"))
    (fp_text value "22uf" (at 0 1.68 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.95 0 90) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 82 "<NO NET>"))
    (pad "2" smd roundrect (at 0.95 0 90) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:TSOT-23-5" (layer "F.Cu")
    (tedit 60070D02)
    (at 84.9175 29.33 180)
    (descr "TSOT, 5 Pin (https://www.jedec.org/sites/default/files/docs/MO-193D.pdf variant AB), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "TSOT TO_SOT_SMD")
    (property "Sheet file" "switch.kicad_sch")
    (property "Sheet name" "switch")
    (attr smd)
    (fp_text reference "U7" (at 0 -2.4) (layer "F.SilkS"))
    (fp_text value "ADP2108AUJ-1.0" (at 0 2.4) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.1375 -0.95 180) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "/+5v") (pinfunction "Vin"))
    (pad "2" smd roundrect (at -1.1375 0 180) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "GND"))
    (pad "3" smd roundrect (at -1.1375 0.95 180) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "/+5v") (pinfunction "EN"))
    (pad "4" smd roundrect (at 1.1375 0.95 180) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 83 "/switch/+1v") (pinfunction "FB"))
    (pad "5" smd roundrect (at 1.1375 -0.95 180) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 81 "Net-(L3-Pad1)") (pinfunction "SW"))
    (model "${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/TSOT-23-5.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 63.73 66.82 -90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheet file" "switch.kicad_sch")
    (property "Sheet name" "switch")
    (attr smd)
    (fp_text reference "C41" (at 2.35 -0.15 -90) (layer "F.SilkS"))
    (fp_text value "0.1uf" (at 0 1.16 -90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 -90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.48 0 270) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 83 "/switch/+1v"))
    (pad "2" smd roundrect (at 0.48 0 270) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Inductor_SMD:L_1206_3216Metric" (layer "F.Cu")
    (tedit 600E9C4C)
    (at 85.09 50.292)
    (descr "Inductor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 80, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "inductor")
    (attr smd)
    (fp_text reference "L4" (at 2.81 -1.582) (layer "F.SilkS"))
    (fp_text value "6.8uh" (at 0 1.9) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.575 0) (size 1.05 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.238)
      (net 82 "<NO NET>"))
    (pad "2" smd roundrect (at 1.575 0) (size 1.05 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.238095))
    (model "${KISYS3DMOD}/Inductor_SMD.3dshapes/L_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TestPoint:TestPoint_Pad_2.0x2.0mm" (layer "F.Cu")
    (tedit 5A0F774F)
    (at 92.79 37.97)
    (descr "SMD rectangular pad as test Point, square 2.0mm side length")
    (tags "test point SMD pad rectangle square")
    (property "Field4" "nf")
    (property "Field5" "nf")
    (property "Field6" "nf")
    (property "Field7" "nf")
    (property "Sheet file" "switch.kicad_sch")
    (property "Sheet name" "switch")
    (attr exclude_from_pos_files)
    (fp_text reference "TP1" (at 0.66 -2.21) (layer "F.SilkS"))
    (fp_text value "TestPoint" (at 0 2.05) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -2) (layer "F.Fab"))
    (pad "1" smd rect (at 0 0) (size 2 2) (layers "F.Cu" "F.Mask")
      (net 7 "Net-(C18-Pad1)") (pinfunction "1"))
  )
  (footprint "Capacitor_SMD:C_Elec_6.3x7.7" (layer "F.Cu")
    (tedit 6006F11E)
    (at 90.78 44.41 -90)
    (descr "SMD capacitor, aluminum electrolytic nonpolar, 6.3x7.7mm")
    (tags "capacitor electrolyic nonpolar")
    (property "Sheet file" "switch.kicad_sch")
    (property "Sheet name" "switch")
    (attr smd)
    (fp_text reference "C29" (at 4.3 -2.49 180) (layer "F.SilkS"))
    (fp_text value "100uf" (at 0 4.35 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.5375 0 270) (size 3.325 1.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.156)
      (net 7 "Net-(C18-Pad1)"))
    (pad "2" smd roundrect (at 2.5375 0 270) (size 3.325 1.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.15625)
      (net 1 "GND"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_Elec_6.3x7.7.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 62.82 40.47 -90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheet file" "switch.kicad_sch")
    (property "Sheet name" "switch")
    (attr smd)
    (fp_text reference "C1" (at -1.19 -1.47 -90) (layer "F.SilkS"))
    (fp_text value "pf" (at 0 1.43 -90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 -90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.775 0 270) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "Net-(C1-Pad1)"))
    (pad "2" smd roundrect (at 0.775 0 270) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0402_1005Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 73.38 41.98 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheet file" "switch.kicad_sch")
    (property "Sheet name" "switch")
    (attr smd)
    (fp_text reference "R33" (at 0 -1.17 90) (layer "F.SilkS"))
    (fp_text value "1k" (at 0 1.17 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.51 0 90) (size 0.54 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 86 "Net-(R33-Pad1)"))
    (pad "2" smd roundrect (at 0.51 0 90) (size 0.54 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 82 "<NO NET>"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 56.91 29.03 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheet file" "switch.kicad_sch")
    (property "Sheet name" "switch")
    (attr smd)
    (fp_text reference "C9" (at 3.16 -0.06 90) (layer "F.SilkS"))
    (fp_text value "22uf" (at 0 1.68 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.95 0 90) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "Net-(C13-Pad1)"))
    (pad "2" smd roundrect (at 0.95 0 90) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (tedit 60070D0A)
    (at 83.85 24.75 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheet file" "switch.kicad_sch")
    (property "Sheet name" "switch")
    (attr smd)
    (fp_text reference "C32" (at -0.3 1.52 90) (layer "F.SilkS"))
    (fp_text value "10uf" (at 0 1.68 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.95 0 90) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 83 "/switch/+1v"))
    (pad "2" smd roundrect (at 0.95 0 90) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1206_3216Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 102.39 58.62 90)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheet file" "switch.kicad_sch")
    (property "Sheet name" "switch")
    (attr smd)
    (fp_text reference "C33" (at -3.02 0.1) (layer "F.SilkS"))
    (fp_text value "470uf" (at 0 1.85 270) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 270) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.475 0 90) (size 1.15 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.217391)
      (net 4 "/+5v"))
    (pad "2" smd roundrect (at 1.475 0 90) (size 1.15 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.217391)
      (net 1 "GND"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 66.69 43.71 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheet file" "switch.kicad_sch")
    (property "Sheet name" "switch")
    (attr smd)
    (fp_text reference "C52" (at 0 -1.16 90) (layer "F.SilkS"))
    (fp_text value "0.1uf" (at 0 1.16 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.48 0 90) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 82 "<NO NET>"))
    (pad "2" smd roundrect (at 0.48 0 90) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 56.39 66.97 -90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheet file" "switch.kicad_sch")
    (property "Sheet name" "switch")
    (attr smd)
    (fp_text reference "C44" (at 0 -1.16 -90) (layer "F.SilkS"))
    (fp_text value "0.1uf" (at 0 1.16 -90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 -90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.48 0 270) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 82 "<NO NET>"))
    (pad "2" smd roundrect (at 0.48 0 270) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Crystal:Crystal_SMD_5032-4Pin_5.0x3.2mm" (layer "F.Cu")
    (tedit 600705F1)
    (at 58.83 40.04)
    (descr "SMD Crystal SERIES SMD2520/4 http://www.icbase.com/File/PDF/HKC/HKC00061008.pdf, 5.0x3.2mm^2 package")
    (tags "SMD SMT crystal")
    (property "Sheet file" "switch.kicad_sch")
    (property "Sheet name" "switch")
    (attr smd)
    (fp_text reference "Y1" (at 3.73 -1.73) (layer "F.SilkS"))
    (fp_text value "25Mhz" (at 0 2.8) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect (at -1.65 1) (size 1.6 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "Net-(C2-Pad1)") (pinfunction "1"))
    (pad "2" smd rect (at 1.65 1) (size 1.6 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "2"))
    (pad "3" smd rect (at 1.65 -1) (size 1.6 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "Net-(C1-Pad1)"))
    (pad "4" smd rect (at -1.65 -1) (size 1.6 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND"))
    (model "${KISYS3DMOD}/Crystal.3dshapes/Crystal_SMD_5032-4Pin_5.0x3.2mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1206_3216Metric" (layer "F.Cu")
    (tedit 600ACDBD)
    (at 66.85 41.18 180)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheet file" "switch.kicad_sch")
    (property "Sheet name" "switch")
    (attr smd)
    (fp_text reference "C4" (at -1.63 1.9) (layer "F.SilkS"))
    (fp_text value "100uf" (at 0 1.85) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.475 0 180) (size 1.15 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.217)
      (net 82 "<NO NET>"))
    (pad "2" smd roundrect (at 1.475 0 180) (size 1.15 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.217391)
      (net 1 "GND"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 55.08 40.26 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheet file" "switch.kicad_sch")
    (property "Sheet name" "switch")
    (attr smd)
    (fp_text reference "C2" (at 0 -1.43 270) (layer "F.SilkS"))
    (fp_text value "pf" (at 0 1.43 270) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 270) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.775 0 90) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "Net-(C2-Pad1)"))
    (pad "2" smd roundrect (at 0.775 0 90) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 104.41 46.04 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Field4" "Digikey")
    (property "Field5" "490-14381-1-ND")
    (property "Field6" "GRM21BR71A106KA73L")
    (property "Field7" "Murata")
    (property "Field8" "111893011")
    (property "Part Description" "	10uF 10% 10V Ceramic Capacitor X7R 0805 (2012 Metric)")
    (property "Sheet file" "switch.kicad_sch")
    (property "Sheet name" "switch")
    (attr smd)
    (fp_text reference "C18" (at -0.02 1.64 90) (layer "F.SilkS"))
    (fp_text value "10u" (at 0 1.68 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.95 0 90) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 7 "Net-(C18-Pad1)"))
    (pad "2" smd roundrect (at 0.95 0 90) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 99.3 33.23 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Field4" "Digikey")
    (property "Field5" "490-14381-1-ND")
    (property "Field6" "GRM21BR71A106KA73L")
    (property "Field7" "Murata")
    (property "Field8" "111893011")
    (property "Part Description" "	10uF 10% 10V Ceramic Capacitor X7R 0805 (2012 Metric)")
    (property "Sheet file" "switch.kicad_sch")
    (property "Sheet name" "switch")
    (attr smd)
    (fp_text reference "C24" (at -2.52 -0.4 180) (layer "F.SilkS"))
    (fp_text value "10u" (at 0 1.68 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.95 0 90) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 8 "Net-(C19-Pad1)"))
    (pad "2" smd roundrect (at 0.95 0 90) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:CP_Elec_10x10" (layer "F.Cu")
    (tedit 5BCA39D1)
    (at 95.71 54.68 90)
    (descr "SMD capacitor, aluminum electrolytic, Nichicon, 10.0x10.0mm")
    (tags "capacitor electrolytic")
    (property "Sheet file" "switch.kicad_sch")
    (property "Sheet name" "switch")
    (attr smd)
    (fp_text reference "C3" (at -4.56 -6.06 90) (layer "F.SilkS"))
    (fp_text value "470uf" (at 0 6.2 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -4 0 90) (size 4 2.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1)
      (net 4 "/+5v"))
    (pad "2" smd roundrect (at 4 0 90) (size 4 2.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1)
      (net 1 "GND"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/CP_Elec_10x10.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TestPoint:TestPoint_Pad_2.0x2.0mm" (layer "F.Cu")
    (tedit 5A0F774F)
    (at 88.775 37.905)
    (descr "SMD rectangular pad as test Point, square 2.0mm side length")
    (tags "test point SMD pad rectangle square")
    (property "Field4" "nf")
    (property "Field5" "nf")
    (property "Field6" "nf")
    (property "Field7" "nf")
    (property "Sheet file" "switch.kicad_sch")
    (property "Sheet name" "switch")
    (attr exclude_from_pos_files)
    (fp_text reference "TP2" (at 0 -1.998) (layer "F.SilkS"))
    (fp_text value "TestPoint" (at 0 2.05) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -2) (layer "F.Fab"))
    (pad "1" smd rect (at 0 0) (size 2 2) (layers "F.Cu" "F.Mask")
      (net 8 "Net-(C19-Pad1)") (pinfunction "1"))
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 64.83 66.81 -90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheet file" "switch.kicad_sch")
    (property "Sheet name" "switch")
    (attr smd)
    (fp_text reference "C40" (at 2.3 -0.3 -90) (layer "F.SilkS"))
    (fp_text value "0.1uf" (at 0 1.16 -90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 -90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.48 0 270) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 82 "<NO NET>"))
    (pad "2" smd roundrect (at 0.48 0 270) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 118.56 32.21 -90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Field4" "Digikey")
    (property "Field5" "490-10505-1-ND")
    (property "Field6" "GRM21BC8YA106KE11L ")
    (property "Field7" "Murata")
    (property "Field8" "")
    (property "Part Description" "	10uF 10% or 20% 35V Ceramic Capacitor X6S 0805 (2012 Metric)")
    (property "Sheet file" "switch.kicad_sch")
    (property "Sheet name" "switch")
    (attr smd)
    (fp_text reference "C11" (at 0.02 1.48 -90) (layer "F.SilkS"))
    (fp_text value "10u" (at 0 1.68 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.95 0 270) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 6 "Net-(C10-Pad1)"))
    (pad "2" smd roundrect (at 0.95 0 270) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_SMA" (layer "F.Cu")
    (tedit 586432E5)
    (at 105.07 27.47 -90)
    (descr "Diode SMA (DO-214AC)")
    (tags "Diode SMA (DO-214AC)")
    (property "Sheet file" "switch.kicad_sch")
    (property "Sheet name" "switch")
    (attr smd)
    (fp_text reference "D8" (at 2.59 -2.44 90) (layer "F.SilkS"))
    (fp_text value "1n5824" (at 0 2.6 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -2.5 90) (layer "F.Fab"))
    (pad "1" smd rect (at -2 0 270) (size 2.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 14 "Net-(D8-Pad1)") (pinfunction "K"))
    (pad "2" smd rect (at 2 0 270) (size 2.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "A"))
    (model "${KISYS3DMOD}/Diode_SMD.3dshapes/D_SMA.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm" (layer "F.Cu")
    (tedit 5D9F72B1)
    (at 48.75 43.66)
    (descr "SOIC, 8 Pin (JEDEC MS-012AA, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_8.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (property "Sheet file" "switch.kicad_sch")
    (property "Sheet name" "switch")
    (attr smd)
    (fp_text reference "U5" (at 0 -3.4) (layer "F.SilkS"))
    (fp_text value "M24C02-FMN" (at 0 3.4) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.475 -1.905) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "E0"))
    (pad "2" smd roundrect (at -2.475 -0.635) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "E1"))
    (pad "3" smd roundrect (at -2.475 0.635) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "E2"))
    (pad "4" smd roundrect (at -2.475 1.905) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "VSS"))
    (pad "5" smd roundrect (at 2.475 1.905) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 89 "/switch/SDA") (pinfunction "SDA"))
    (pad "6" smd roundrect (at 2.475 0.635) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 90 "/switch/SCK") (pinfunction "SCL"))
    (pad "7" smd roundrect (at 2.475 -0.635) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "~WC"))
    (pad "8" smd roundrect (at 2.475 -1.905) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 82 "<NO NET>") (pinfunction "VCC"))
    (model "${KISYS3DMOD}/Package_SO.3dshapes/SOIC-8_3.9x4.9mm_P1.27mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (tedit 60070D1A)
    (at 75.5 24.74 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheet file" "switch.kicad_sch")
    (property "Sheet name" "switch")
    (attr smd)
    (fp_text reference "C28" (at -0.02 -1.36 90) (layer "F.SilkS"))
    (fp_text value "10uf" (at 0 1.68 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.95 0 90) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 83 "/switch/+1v"))
    (pad "2" smd roundrect (at 0.95 0 90) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinSocket_2.54mm:PinSocket_2x06_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 5A19A42B)
    (at 103.14 82.41 180)
    (descr "Through hole straight socket strip, 2x06, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 2x06 2.54mm double row")
    (property "Sheet file" "cluster4.kicad_sch")
    (property "Sheet name" "")
    (attr through_hole)
    (fp_text reference "J7" (at 0.03 15.4) (layer "F.SilkS"))
    (fp_text value "Conn_01x11_Female" (at -1.27 15.47) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at -1.27 6.35 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 "/+12v") (pinfunction "Pin_1"))
    (pad "2" thru_hole oval (at -2.54 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "/+5v") (pinfunction "Pin_2"))
    (pad "3" thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_3"))
    (pad "4" thru_hole oval (at -2.54 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 56 "/P5_AP") (pinfunction "Pin_4"))
    (pad "5" thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 55 "/P5_AN") (pinfunction "Pin_5"))
    (pad "6" thru_hole oval (at -2.54 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 54 "/P5_BP") (pinfunction "Pin_6"))
    (pad "7" thru_hole oval (at 0 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 53 "/P5_BN") (pinfunction "Pin_7"))
    (pad "8" thru_hole oval (at -2.54 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 52 "/P5_CP") (pinfunction "Pin_8"))
    (pad "9" thru_hole oval (at 0 10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 51 "/P5_CN") (pinfunction "Pin_9"))
    (pad "10" thru_hole oval (at -2.54 10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 50 "/P5_DP") (pinfunction "Pin_10"))
    (pad "11" thru_hole oval (at 0 12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 49 "/P5_DN") (pinfunction "Pin_11"))
    (pad "12" thru_hole oval (at -2.54 12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model "${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_2x06_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "F.Cu")
    (tedit 600E9CDA)
    (at 82.04 50.77 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (attr smd)
    (fp_text reference "C10" (at 0 -1.16 90) (layer "F.SilkS"))
    (fp_text value "10n" (at 0 1.16 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.48 0 90) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25))
    (pad "2" smd roundrect (at 0.48 0 90) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 82 "<NO NET>"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0402_1005Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 62.69 66.83 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheet file" "switch.kicad_sch")
    (property "Sheet name" "switch")
    (attr smd)
    (fp_text reference "C44" (at -2.38 -0.06 90) (layer "F.SilkS"))
    (fp_text value "2.49k" (at 0 1.17 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.51 0 90) (size 0.54 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND"))
    (pad "2" smd roundrect (at 0.51 0 90) (size 0.54 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 84 "Net-(R13-Pad2)"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 48.830001 55.729999 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheet file" "switch.kicad_sch")
    (property "Sheet name" "switch")
    (attr smd)
    (fp_text reference "RC37" (at 0 -1.16 180) (layer "F.SilkS"))
    (fp_text value "0.1uf" (at 0 1.16 180) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 180) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.48 0 180) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 83 "/switch/+1v"))
    (pad "2" smd roundrect (at 0.48 0 180) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0402_1005Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 64.74 33.53 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheet file" "switch.kicad_sch")
    (property "Sheet name" "switch")
    (attr smd)
    (fp_text reference "R24" (at -0.08 1.24) (layer "F.SilkS"))
    (fp_text value "10k" (at 0 1.17) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.51 0 180) (size 0.54 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 12 "Net-(D6-Pad1)"))
    (pad "2" smd roundrect (at 0.51 0 180) (size 0.54 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 85 "/switch/nRESET"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinSocket_2.54mm:PinSocket_2x06_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 5A19A42B)
    (at 86 82.41 180)
    (descr "Through hole straight socket strip, 2x06, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 2x06 2.54mm double row")
    (property "Sheet file" "cluster4.kicad_sch")
    (property "Sheet name" "")
    (attr through_hole)
    (fp_text reference "J6" (at -0.08 15.38) (layer "F.SilkS"))
    (fp_text value "Conn_01x11_Female" (at -1.27 15.47) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at -1.27 6.35 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 "/+12v") (pinfunction "Pin_1"))
    (pad "2" thru_hole oval (at -2.54 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "/+5v") (pinfunction "Pin_2"))
    (pad "3" thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_3"))
    (pad "4" thru_hole oval (at -2.54 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 48 "/P4_AP") (pinfunction "Pin_4"))
    (pad "5" thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 47 "/P4_AN") (pinfunction "Pin_5"))
    (pad "6" thru_hole oval (at -2.54 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 46 "/P4_BP") (pinfunction "Pin_6"))
    (pad "7" thru_hole oval (at 0 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 45 "/P4_BN") (pinfunction "Pin_7"))
    (pad "8" thru_hole oval (at -2.54 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 44 "/P4_CP") (pinfunction "Pin_8"))
    (pad "9" thru_hole oval (at 0 10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 43 "/P4_CN") (pinfunction "Pin_9"))
    (pad "10" thru_hole oval (at -2.54 10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 42 "/P4_DP") (pinfunction "Pin_10"))
    (pad "11" thru_hole oval (at 0 12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 41 "/P4_DN") (pinfunction "Pin_11"))
    (pad "12" thru_hole oval (at -2.54 12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model "${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_2x06_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 50.08 58.24 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheet file" "switch.kicad_sch")
    (property "Sheet name" "switch")
    (attr smd)
    (fp_text reference "C38" (at 0 -1.16 180) (layer "F.SilkS"))
    (fp_text value "0.1uf" (at 0 1.16 180) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 180) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.48 0 180) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 83 "/switch/+1v"))
    (pad "2" smd roundrect (at 0.48 0 180) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0402_1005Metric" (layer "F.Cu")
    (tedit 600B065B)
    (at 51.73 47.23)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (attr smd)
    (fp_text reference "R2" (at -1.93 -0.07) (layer "F.SilkS"))
    (fp_text value "4.7k" (at 0 1.17) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.51 0) (size 0.54 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 89 "/switch/SDA"))
    (pad "2" smd roundrect (at 0.51 0) (size 0.54 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 82 "<NO NET>"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (tedit 600ACDAC)
    (at 81.45 47.49 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheet file" "switch.kicad_sch")
    (property "Sheet name" "switch")
    (attr smd)
    (fp_text reference "C15" (at 3.23 0.69 90) (layer "F.SilkS"))
    (fp_text value "10uf" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.95 0 90) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 82 "<NO NET>"))
    (pad "2" smd roundrect (at 0.95 0 90) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinSocket_2.54mm:PinSocket_2x06_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 5A19A42B)
    (at 120.28 82.41 180)
    (descr "Through hole straight socket strip, 2x06, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 2x06 2.54mm double row")
    (property "Sheet file" "cluster4.kicad_sch")
    (property "Sheet name" "")
    (attr through_hole)
    (fp_text reference "J8" (at 0.13 15.36) (layer "F.SilkS"))
    (fp_text value "Conn_01x11_Female" (at -1.27 15.47) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at -1.27 6.35 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 "/+12v") (pinfunction "Pin_1"))
    (pad "2" thru_hole oval (at -2.54 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "/+5v") (pinfunction "Pin_2"))
    (pad "3" thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_3"))
    (pad "4" thru_hole oval (at -2.54 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 64 "/P6_AP") (pinfunction "Pin_4"))
    (pad "5" thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 63 "/P6_AN") (pinfunction "Pin_5"))
    (pad "6" thru_hole oval (at -2.54 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 62 "/P6_BP") (pinfunction "Pin_6"))
    (pad "7" thru_hole oval (at 0 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 61 "/P6_BN") (pinfunction "Pin_7"))
    (pad "8" thru_hole oval (at -2.54 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 60 "/P6_CP") (pinfunction "Pin_8"))
    (pad "9" thru_hole oval (at 0 10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 59 "/P6_CN") (pinfunction "Pin_9"))
    (pad "10" thru_hole oval (at -2.54 10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 58 "/P6_DP") (pinfunction "Pin_10"))
    (pad "11" thru_hole oval (at 0 12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 57 "/P6_DN") (pinfunction "Pin_11"))
    (pad "12" thru_hole oval (at -2.54 12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model "${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_2x06_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_SMA" (layer "F.Cu")
    (tedit 600EB3A1)
    (at 130.18 34.56)
    (descr "Diode SMA (DO-214AC)")
    (tags "Diode SMA (DO-214AC)")
    (property "Sheet file" "switch.kicad_sch")
    (property "Sheet name" "switch")
    (attr smd)
    (fp_text reference "D4" (at -4.88 -0.09) (layer "F.SilkS"))
    (fp_text value "D" (at 0 2.6) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -2.5) (layer "F.Fab"))
    (pad "1" smd rect (at -2 0) (size 2.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 6 "Net-(C10-Pad1)") (pinfunction "K"))
    (pad "2" smd rect (at 2 0) (size 2.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "Net-(J2-Pad14)") (pinfunction "A"))
    (model "${KISYS3DMOD}/Diode_SMD.3dshapes/D_SMA.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 104.9 33.21 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Field4" "Digikey")
    (property "Field5" "490-14381-1-ND")
    (property "Field6" "GRM21BR71A106KA73L")
    (property "Field7" "Murata")
    (property "Field8" "111893011")
    (property "Part Description" "	10uF 10% 10V Ceramic Capacitor X7R 0805 (2012 Metric)")
    (property "Sheet file" "switch.kicad_sch")
    (property "Sheet name" "switch")
    (attr smd)
    (fp_text reference "C19" (at -2.46 0.05 180) (layer "F.SilkS"))
    (fp_text value "10u" (at 0 1.68 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.95 0 90) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 8 "Net-(C19-Pad1)"))
    (pad "2" smd roundrect (at 0.95 0 90) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1206_3216Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 63.11 28.48 90)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheet file" "switch.kicad_sch")
    (property "Sheet name" "switch")
    (attr smd)
    (fp_text reference "C5" (at 3.41 -0.04 90) (layer "F.SilkS"))
    (fp_text value "100uf" (at 0 1.85 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.475 0 90) (size 1.15 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.217391)
      (net 5 "Net-(C13-Pad1)"))
    (pad "2" smd roundrect (at 1.475 0 90) (size 1.15 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.217391)
      (net 1 "GND"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Inductor_SMD:L_Bourns_SRN6045TA" (layer "F.Cu")
    (tedit 600AB96B)
    (at 78.21 30.24 180)
    (descr "http://www.bourns.com/docs/product-datasheets/srn6045ta.pdf")
    (tags "Semi-shielded Power Inductor")
    (property "Sheet file" "switch.kicad_sch")
    (property "Sheet name" "switch")
    (attr smd)
    (fp_text reference "L3" (at -0.02 -3.98) (layer "F.SilkS"))
    (fp_text value "1uh" (at 0 4.2) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd rect (at -2.075 0 180) (size 2.35 5.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 81 "Net-(L3-Pad1)") (pinfunction "1"))
    (pad "2" smd rect (at 2.075 0 180) (size 2.35 5.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 83 "/switch/+1v") (pinfunction "2"))
    (model "${KISYS3DMOD}/Inductor_SMD.3dshapes/L_Bourns_SRN6045TA.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_RJ:RJ45_Amphenol_54602-x08_Horizontal" (layer "F.Cu")
    (tedit 5B103613)
    (at 39.54 51.69 -90)
    (descr "8 Pol Shallow Latch Connector, Modjack, RJ45 (https://cdn.amphenol-icc.com/media/wysiwyg/files/drawing/c-bmj-0102.pdf)")
    (tags "RJ45")
    (property "Sheet file" "cluster4.kicad_sch")
    (property "Sheet name" "")
    (attr through_hole)
    (fp_text reference "J12" (at 4.445 -5 90) (layer "F.SilkS"))
    (fp_text value "RJ45" (at 4.445 4 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 4.445 2 90) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at -1.27 6.35 270) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 10.16 6.35 270) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.5 1.5) (drill 0.76) (layers *.Cu *.Mask)
      (net 80 "/P0_AP"))
    (pad "2" thru_hole circle (at 1.27 -2.54 270) (size 1.5 1.5) (drill 0.76) (layers *.Cu *.Mask)
      (net 79 "/P0_AN"))
    (pad "3" thru_hole circle (at 2.54 0 270) (size 1.5 1.5) (drill 0.76) (layers *.Cu *.Mask)
      (net 78 "/P0_BP"))
    (pad "4" thru_hole circle (at 3.81 -2.54 270) (size 1.5 1.5) (drill 0.76) (layers *.Cu *.Mask)
      (net 77 "/P0_CP"))
    (pad "5" thru_hole circle (at 5.08 0 270) (size 1.5 1.5) (drill 0.76) (layers *.Cu *.Mask)
      (net 76 "/P0_CN"))
    (pad "6" thru_hole circle (at 6.35 -2.54 270) (size 1.5 1.5) (drill 0.76) (layers *.Cu *.Mask)
      (net 75 "/P0_BN"))
    (pad "7" thru_hole circle (at 7.62 0 270) (size 1.5 1.5) (drill 0.76) (layers *.Cu *.Mask)
      (net 74 "/P0_DP"))
    (pad "8" thru_hole circle (at 8.89 -2.54 270) (size 1.5 1.5) (drill 0.76) (layers *.Cu *.Mask)
      (net 73 "/P0_DN"))
    (model "${KISYS3DMOD}/Connector_RJ.3dshapes/RJ45_Amphenol_54602-x08_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 78.69 53.75)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheet file" "switch.kicad_sch")
    (property "Sheet name" "switch")
    (attr smd)
    (fp_text reference "C48" (at 1.08 1.21) (layer "F.SilkS"))
    (fp_text value "0.1uf" (at 0 1.16) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.48 0) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 82 "<NO NET>"))
    (pad "2" smd roundrect (at 0.48 0) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_SMA" (layer "F.Cu")
    (tedit 586432E5)
    (at 104.42 40.57 -90)
    (descr "Diode SMA (DO-214AC)")
    (tags "Diode SMA (DO-214AC)")
    (property "Sheet file" "switch.kicad_sch")
    (property "Sheet name" "switch")
    (attr smd)
    (fp_text reference "D7" (at 2.04 -2.68 90) (layer "F.SilkS"))
    (fp_text value "1n5824" (at 0 2.6 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -2.5 90) (layer "F.Fab"))
    (pad "1" smd rect (at -2 0 270) (size 2.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 13 "Net-(D7-Pad1)") (pinfunction "K"))
    (pad "2" smd rect (at 2 0 270) (size 2.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "A"))
    (model "${KISYS3DMOD}/Diode_SMD.3dshapes/D_SMA.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_SMC" (layer "F.Cu")
    (tedit 6006F482)
    (at 118.99 54.71 90)
    (descr "Diode SMC (DO-214AB)")
    (tags "Diode SMC (DO-214AB)")
    (attr smd)
    (fp_text reference "D5" (at 5.92 2.74 90) (layer "F.SilkS"))
    (fp_text value "D_SMC" (at 0 4.2 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -1.9 90) (layer "F.Fab"))
    (pad "1" smd rect (at -3.4 0 180) (size 3.3 2.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 11 "/+12v"))
    (pad "2" smd rect (at 3.4 0 180) (size 3.3 2.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 6 "Net-(C10-Pad1)"))
    (model "${KISYS3DMOD}/Diode_SMD.3dshapes/D_SMC.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinSocket_2.54mm:PinSocket_2x06_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 5A19A42B)
    (at 34.56 82.41 180)
    (descr "Through hole straight socket strip, 2x06, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 2x06 2.54mm double row")
    (property "Sheet file" "cluster4.kicad_sch")
    (property "Sheet name" "")
    (attr through_hole)
    (fp_text reference "J3" (at 0 16.05) (layer "F.SilkS"))
    (fp_text value "Conn_01x11_Female" (at -1.27 15.47) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at -1.27 6.35 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 "/+12v") (pinfunction "Pin_1"))
    (pad "2" thru_hole oval (at -2.54 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "/+5v") (pinfunction "Pin_2"))
    (pad "3" thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_3"))
    (pad "4" thru_hole oval (at -2.54 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 "/P1_AP") (pinfunction "Pin_4"))
    (pad "5" thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 "/P1_AN") (pinfunction "Pin_5"))
    (pad "6" thru_hole oval (at -2.54 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 "/P1_BP") (pinfunction "Pin_6"))
    (pad "7" thru_hole oval (at 0 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 "/P1_BN") (pinfunction "Pin_7"))
    (pad "8" thru_hole oval (at -2.54 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 "/P1_CP") (pinfunction "Pin_8"))
    (pad "9" thru_hole oval (at 0 10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 "/P1_CN") (pinfunction "Pin_9"))
    (pad "10" thru_hole oval (at -2.54 10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 "/P1_DP") (pinfunction "Pin_10"))
    (pad "11" thru_hole oval (at 0 12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 "/P1_DN") (pinfunction "Pin_11"))
    (pad "12" thru_hole oval (at -2.54 12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model "${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_2x06_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (tedit 60070D20)
    (at 78.39 24.72 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheet file" "switch.kicad_sch")
    (property "Sheet name" "switch")
    (attr smd)
    (fp_text reference "C27" (at 0.01 -1.42 90) (layer "F.SilkS"))
    (fp_text value "10uf" (at 0 1.68 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.95 0 90) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 83 "/switch/+1v"))
    (pad "2" smd roundrect (at 0.95 0 90) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 78.78 56.1)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheet file" "switch.kicad_sch")
    (property "Sheet name" "switch")
    (attr smd)
    (fp_text reference "C47" (at 0.02 1.24) (layer "F.SilkS"))
    (fp_text value "0.1uf" (at 0 1.16) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.48 0) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 83 "/switch/+1v"))
    (pad "2" smd roundrect (at 0.48 0) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (tedit 600ACDCA)
    (at 77.15 46.55 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheet file" "switch.kicad_sch")
    (property "Sheet name" "switch")
    (attr smd)
    (fp_text reference "C12" (at -0.22 -1.72 90) (layer "F.SilkS"))
    (fp_text value "10uf" (at 0 1.68 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.95 0 90) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 82 "<NO NET>"))
    (pad "2" smd roundrect (at 0.95 0 90) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 48.82 50.77 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheet file" "switch.kicad_sch")
    (property "Sheet name" "switch")
    (attr smd)
    (fp_text reference "C35" (at 0 -1.16 180) (layer "F.SilkS"))
    (fp_text value "0.1uf" (at 0 1.16 180) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 180) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.48 0 180) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 83 "/switch/+1v"))
    (pad "2" smd roundrect (at 0.48 0 180) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 96.99 46.06 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Field4" "Digikey")
    (property "Field5" "490-14381-1-ND")
    (property "Field6" "GRM21BR71A106KA73L")
    (property "Field7" "Murata")
    (property "Field8" "111893011")
    (property "Part Description" "	10uF 10% 10V Ceramic Capacitor X7R 0805 (2012 Metric)")
    (property "Sheet file" "switch.kicad_sch")
    (property "Sheet name" "switch")
    (attr smd)
    (fp_text reference "C25" (at 0 -1.68 90) (layer "F.SilkS"))
    (fp_text value "10u" (at 0 1.68 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.95 0 90) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 7 "Net-(C18-Pad1)"))
    (pad "2" smd roundrect (at 0.95 0 90) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_SMA" (layer "F.Cu")
    (tedit 600EB3A7)
    (at 130.22 38.81 180)
    (descr "Diode SMA (DO-214AC)")
    (tags "Diode SMA (DO-214AC)")
    (property "Sheet file" "switch.kicad_sch")
    (property "Sheet name" "switch")
    (attr smd)
    (fp_text reference "D3" (at 4.69 0.02) (layer "F.SilkS"))
    (fp_text value "D" (at 0 2.6) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -2.5) (layer "F.Fab"))
    (pad "1" smd rect (at -2 0 180) (size 2.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "Net-(J2-Pad14)") (pinfunction "K"))
    (pad "2" smd rect (at 2 0 180) (size 2.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "A"))
    (model "${KISYS3DMOD}/Diode_SMD.3dshapes/D_SMA.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 99.54 46.04 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Field4" "Digikey")
    (property "Field5" "490-14381-1-ND")
    (property "Field6" "GRM21BR71A106KA73L")
    (property "Field7" "Murata")
    (property "Field8" "111893011")
    (property "Part Description" "	10uF 10% 10V Ceramic Capacitor X7R 0805 (2012 Metric)")
    (property "Sheet file" "switch.kicad_sch")
    (property "Sheet name" "switch")
    (attr smd)
    (fp_text reference "C23" (at -2.47 -0.04 180) (layer "F.SilkS"))
    (fp_text value "10u" (at 0 1.68 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.95 0 90) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 7 "Net-(C18-Pad1)"))
    (pad "2" smd roundrect (at 0.95 0 90) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_SMA" (layer "F.Cu")
    (tedit 600EB39A)
    (at 130.25 26.71 180)
    (descr "Diode SMA (DO-214AC)")
    (tags "Diode SMA (DO-214AC)")
    (property "Sheet file" "switch.kicad_sch")
    (property "Sheet name" "switch")
    (attr smd)
    (fp_text reference "D1" (at -4.59 0.38) (layer "F.SilkS"))
    (fp_text value "D" (at 0 2.6) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -2.5) (layer "F.Fab"))
    (pad "1" smd rect (at -2 0 180) (size 2.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 16 "Net-(J2-Pad13)") (pinfunction "K"))
    (pad "2" smd rect (at 2 0 180) (size 2.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "A"))
    (model "${KISYS3DMOD}/Diode_SMD.3dshapes/D_SMA.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 78.68 48.76)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheet file" "switch.kicad_sch")
    (property "Sheet name" "switch")
    (attr smd)
    (fp_text reference "C50" (at 0.08 1.23) (layer "F.SilkS"))
    (fp_text value "0.1uf" (at 0 1.16) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.48 0) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 82 "<NO NET>"))
    (pad "2" smd roundrect (at 0.48 0) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 58.09 43.84 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheet file" "switch.kicad_sch")
    (property "Sheet name" "switch")
    (attr smd)
    (fp_text reference "C54" (at 0 -1.16 90) (layer "F.SilkS"))
    (fp_text value "0.1uf" (at 0 1.16 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.48 0 90) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 82 "<NO NET>"))
    (pad "2" smd roundrect (at 0.48 0 90) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-223-3_TabPin2" (layer "F.Cu")
    (tedit 5A02FF57)
    (at 70.01 27.93 -90)
    (descr "module CMS SOT223 4 pins")
    (tags "CMS SOT")
    (property "Sheet file" "switch.kicad_sch")
    (property "Sheet name" "switch")
    (attr smd)
    (fp_text reference "U3" (at -3.23 4.47 90) (layer "F.SilkS"))
    (fp_text value "AMS1117-3.3" (at 0 4.5 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect (at -3.15 -2.3 270) (size 2 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "GND"))
    (pad "2" smd rect (at 3.15 0 270) (size 2 3.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "Net-(C13-Pad1)") (pinfunction "VO"))
    (pad "2" smd rect (at -3.15 0 270) (size 2 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "Net-(C13-Pad1)") (pinfunction "VO"))
    (pad "3" smd rect (at -3.15 2.3 270) (size 2 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "/+5v") (pinfunction "VI"))
    (model "${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-223.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (tedit 600AF3C7)
    (at 109.4 39.09 -90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Field4" "Digikey")
    (property "Field5" "490-10505-1-ND")
    (property "Field6" "GRM21BC8YA106KE11L ")
    (property "Field7" "Murata")
    (property "Field8" "")
    (property "Part Description" "	10uF 10% or 20% 35V Ceramic Capacitor X6S 0805 (2012 Metric)")
    (property "Sheet file" "switch.kicad_sch")
    (property "Sheet name" "switch")
    (attr smd)
    (fp_text reference "C10" (at 0 -1.68 90) (layer "F.SilkS"))
    (fp_text value "100n" (at 0 1.68 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at -0.12 -0.13 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.95 0 270) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 13 "Net-(D7-Pad1)"))
    (pad "2" smd roundrect (at 0.95 0 270) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 68.57 43.71 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheet file" "switch.kicad_sch")
    (property "Sheet name" "switch")
    (attr smd)
    (fp_text reference "C51" (at 0.06 1.47 90) (layer "F.SilkS"))
    (fp_text value "0.1uf" (at 0 1.16 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.48 0 90) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 83 "/switch/+1v"))
    (pad "2" smd roundrect (at 0.48 0 90) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 102.11 46.04 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Field4" "Digikey")
    (property "Field5" "490-14381-1-ND")
    (property "Field6" "GRM21BR71A106KA73L")
    (property "Field7" "Murata")
    (property "Field8" "111893011")
    (property "Part Description" "	10uF 10% 10V Ceramic Capacitor X7R 0805 (2012 Metric)")
    (property "Sheet file" "switch.kicad_sch")
    (property "Sheet name" "switch")
    (attr smd)
    (fp_text reference "C21" (at -2.39 0.4 180) (layer "F.SilkS"))
    (fp_text value "10u" (at 0 1.68 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.95 0 90) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 7 "Net-(C18-Pad1)"))
    (pad "2" smd roundrect (at 0.95 0 90) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Inductor_SMD:L_Bourns_SRN6045TA" (layer "F.Cu")
    (tedit 5B61DEEA)
    (at 98.55 40.24 -90)
    (descr "http://www.bourns.com/docs/product-datasheets/srn6045ta.pdf")
    (tags "Semi-shielded Power Inductor")
    (property "Sheet file" "switch.kicad_sch")
    (property "Sheet name" "switch")
    (attr smd)
    (fp_text reference "L1" (at -1.87 3.74 90) (layer "F.SilkS"))
    (fp_text value "22uh" (at 0 4.2 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect (at -2.075 0 270) (size 2.35 5.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 13 "Net-(D7-Pad1)") (pinfunction "1"))
    (pad "2" smd rect (at 2.075 0 270) (size 2.35 5.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 7 "Net-(C18-Pad1)") (pinfunction "2"))
    (model "${KISYS3DMOD}/Inductor_SMD.3dshapes/L_Bourns_SRN6045TA.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "CM4IO:BarrelJack_Horizontal" (layer "F.Cu")
    (tedit 600ECE72)
    (at 39.3 33.64)
    (descr "DC Barrel Jack")
    (tags "Power Jack")
    (property "Sheet file" "switch.kicad_sch")
    (property "Sheet name" "switch")
    (fp_text reference "J1" (at -0.65 -5.91 90) (layer "F.SilkS"))
    (fp_text value "Barrel_Jack" (at -6.2 -5.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at -3 -2.95) (layer "F.Fab"))
    (pad "1" thru_hole oval (at 0 0) (size 2.8 5) (drill oval 0.8 3) (layers *.Cu *.Mask)
      (net 9 "Net-(D1-Pad1)"))
    (pad "2" thru_hole roundrect (at -5.8 0) (size 2.8 5) (drill oval 0.8 3) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 10 "Net-(D3-Pad1)"))
    (pad "3" thru_hole roundrect (at -3 4.8) (size 5 2.8) (drill oval 3 0.8) (layers *.Cu *.Mask) (roundrect_rratio 0.25))
    (model "./CM4IO.3dshapes/CUI_DEVICES_PJ-102AH.step"
      (offset (xyz -13.7 0 6.5))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 180))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 101.9 33.23 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Field4" "Digikey")
    (property "Field5" "490-14381-1-ND")
    (property "Field6" "GRM21BR71A106KA73L")
    (property "Field7" "Murata")
    (property "Field8" "111893011")
    (property "Part Description" "	10uF 10% 10V Ceramic Capacitor X7R 0805 (2012 Metric)")
    (property "Sheet file" "switch.kicad_sch")
    (property "Sheet name" "switch")
    (attr smd)
    (fp_text reference "C22" (at -2.5 0.01 180) (layer "F.SilkS"))
    (fp_text value "10u" (at 0 1.68 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.95 0 90) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 8 "Net-(C19-Pad1)"))
    (pad "2" smd roundrect (at 0.95 0 90) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_SMA" (layer "F.Cu")
    (tedit 586432E5)
    (at 45.69 24.65)
    (descr "Diode SMA (DO-214AC)")
    (tags "Diode SMA (DO-214AC)")
    (property "Sheet file" "switch.kicad_sch")
    (property "Sheet name" "switch")
    (attr smd)
    (fp_text reference "D3" (at -5.07 0.08) (layer "F.SilkS"))
    (fp_text value "D" (at 0 2.6) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -2.5) (layer "F.Fab"))
    (pad "1" smd rect (at -2 0) (size 2.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 10 "Net-(D3-Pad1)") (pinfunction "K"))
    (pad "2" smd rect (at 2 0) (size 2.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "A"))
    (model "${KISYS3DMOD}/Diode_SMD.3dshapes/D_SMA.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_SMA" (layer "F.Cu")
    (tedit 586432E5)
    (at 45.45 29.1 180)
    (descr "Diode SMA (DO-214AC)")
    (tags "Diode SMA (DO-214AC)")
    (property "Sheet file" "switch.kicad_sch")
    (property "Sheet name" "switch")
    (attr smd)
    (fp_text reference "D4" (at -4.88 -0.09) (layer "F.SilkS"))
    (fp_text value "D" (at 0 2.6) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -2.5) (layer "F.Fab"))
    (pad "1" smd rect (at -2 0 180) (size 2.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 6 "Net-(C10-Pad1)") (pinfunction "K"))
    (pad "2" smd rect (at 2 0 180) (size 2.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 10 "Net-(D3-Pad1)") (pinfunction "A"))
    (model "${KISYS3DMOD}/Diode_SMD.3dshapes/D_SMA.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_Elec_6.3x7.7" (layer "F.Cu")
    (tedit 5BC8D926)
    (at 91.25 31.55 90)
    (descr "SMD capacitor, aluminum electrolytic nonpolar, 6.3x7.7mm")
    (tags "capacitor electrolyic nonpolar")
    (property "Sheet file" "switch.kicad_sch")
    (property "Sheet name" "switch")
    (attr smd)
    (fp_text reference "C30" (at 6.15 0.08 90) (layer "F.SilkS"))
    (fp_text value "100uf" (at 0 4.35 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.5375 0 90) (size 3.325 1.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.15625)
      (net 8 "Net-(C19-Pad1)"))
    (pad "2" smd roundrect (at 2.5375 0 90) (size 3.325 1.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.15625)
      (net 1 "GND"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_Elec_6.3x7.7.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0402_1005Metric" (layer "F.Cu")
    (tedit 600E9B36)
    (at 85.85 57.658)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (attr smd)
    (fp_text reference "R14" (at 2.29 0.002) (layer "F.SilkS"))
    (fp_text value "3k" (at 0 1.17) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.51 0) (size 0.54 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25))
    (pad "2" smd roundrect (at 0.51 0) (size 0.54 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_SMA" (layer "F.Cu")
    (tedit 586432E5)
    (at 45.4 36.96)
    (descr "Diode SMA (DO-214AC)")
    (tags "Diode SMA (DO-214AC)")
    (property "Sheet file" "switch.kicad_sch")
    (property "Sheet name" "switch")
    (attr smd)
    (fp_text reference "D1" (at -2.65 2.57) (layer "F.SilkS"))
    (fp_text value "D" (at 0 2.6) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -2.5) (layer "F.Fab"))
    (pad "1" smd rect (at -2 0) (size 2.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "Net-(D1-Pad1)") (pinfunction "K"))
    (pad "2" smd rect (at 2 0) (size 2.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "A"))
    (model "${KISYS3DMOD}/Diode_SMD.3dshapes/D_SMA.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 60 29.01 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheet file" "switch.kicad_sch")
    (property "Sheet name" "switch")
    (attr smd)
    (fp_text reference "C13" (at 3.27 0.07 90) (layer "F.SilkS"))
    (fp_text value "10uf" (at 0 1.68 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.95 0 90) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "Net-(C13-Pad1)"))
    (pad "2" smd roundrect (at 0.95 0 90) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 60070D39)
    (at 86.6 24.875 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheet file" "switch.kicad_sch")
    (property "Sheet name" "switch")
    (attr smd)
    (fp_text reference "C20" (at 0.055 1.56 90) (layer "F.SilkS"))
    (fp_text value "4.7uf" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.775 0 90) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "/+5v"))
    (pad "2" smd roundrect (at 0.775 0 90) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 78.69 51.26)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheet file" "switch.kicad_sch")
    (property "Sheet name" "switch")
    (attr smd)
    (fp_text reference "C49" (at 0.15 1.27) (layer "F.SilkS"))
    (fp_text value "0.1uf" (at 0 1.16) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.48 0) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 83 "/switch/+1v"))
    (pad "2" smd roundrect (at 0.48 0) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_SO:SOIC-8-1EP_3.9x4.9mm_P1.27mm_EP2.29x3mm_ThermalVias" (layer "F.Cu")
    (tedit 600EDC00)
    (at 86.36 54.356)
    (descr "SOIC, 8 Pin (https://www.analog.com/media/en/technical-documentation/data-sheets/ada4898-1_4898-2.pdf#page=29), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (property "Sheet file" "switch.kicad_sch")
    (property "Sheet name" "switch")
    (attr smd)
    (fp_text reference "U2" (at 2.09 -3.366) (layer "F.SilkS"))
    (fp_text value "LM22676-ADJ" (at 0 3.4) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" smd roundrect (at 0.57 0.75) (size 0.96 1.25) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0.57 -0.75) (size 0.96 1.25) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "" smd roundrect (at -0.57 -0.75) (size 0.96 1.25) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "" smd roundrect (at -0.57 0.75) (size 0.96 1.25) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "1" smd roundrect (at -2.475 -1.905) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (pinfunction "VIN"))
    (pad "2" smd roundrect (at -2.475 -0.635) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (pinfunction "OUT"))
    (pad "3" smd roundrect (at -2.475 0.635) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (pinfunction "GND"))
    (pad "4" smd roundrect (at -2.475 1.905) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (pinfunction "FB"))
    (pad "5" smd roundrect (at 2.475 1.905) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (pinfunction "~ON~/OFF"))
    (pad "6" smd roundrect (at 2.475 0.635) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND"))
    (pad "7" smd roundrect (at 2.475 -0.635) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "/+5v"))
    (pad "8" smd roundrect (at 2.475 -1.905) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25))
    (pad "9" smd rect (at 0 0) (size 1.8 2.5) (layers "B.Cu")
      (net 1 "GND"))
    (pad "9" thru_hole circle (at -0.65 0) (size 0.5 0.5) (drill 0.3) (layers *.Cu)
      (net 1 "GND"))
    (pad "9" smd rect (at 0 0) (size 2.29 3) (layers "F.Cu" "F.Mask")
      (net 1 "GND"))
    (pad "9" thru_hole circle (at -0.65 1) (size 0.5 0.5) (drill 0.3) (layers *.Cu)
      (net 1 "GND"))
    (pad "9" thru_hole circle (at -0.65 -1) (size 0.5 0.5) (drill 0.3) (layers *.Cu)
      (net 1 "GND"))
    (pad "9" thru_hole circle (at 0.65 -1) (size 0.5 0.5) (drill 0.3) (layers *.Cu)
      (net 1 "GND"))
    (pad "9" thru_hole circle (at 0.65 1) (size 0.5 0.5) (drill 0.3) (layers *.Cu)
      (net 1 "GND"))
    (pad "9" thru_hole circle (at 0.65 0) (size 0.5 0.5) (drill 0.3) (layers *.Cu)
      (net 1 "GND"))
    (model "${KISYS3DMOD}/Package_SO.3dshapes/SOIC-8-1EP_3.9x4.9mm_P1.27mm_EP2.29x3mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_SMA" (layer "F.Cu")
    (tedit 6006ECC7)
    (at 84.89 36.05 90)
    (descr "Diode SMA (DO-214AC)")
    (tags "Diode SMA (DO-214AC)")
    (property "Sheet file" "switch.kicad_sch")
    (property "Sheet name" "switch")
    (attr smd)
    (fp_text reference "D10" (at 0 -2.5 90) (layer "F.SilkS"))
    (fp_text value "D" (at 0 2.6 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -2.5 90) (layer "F.Fab"))
    (pad "1" smd rect (at -2 0 90) (size 2.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "/+5v") (pinfunction "K"))
    (pad "2" smd rect (at 2 0 90) (size 2.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 8 "Net-(C19-Pad1)") (pinfunction "A"))
    (model "${KISYS3DMOD}/Diode_SMD.3dshapes/D_SMA.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 65.94 66.85 -90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheet file" "switch.kicad_sch")
    (property "Sheet name" "switch")
    (attr smd)
    (fp_text reference "C42" (at 0 -1.16 -90) (layer "F.SilkS"))
    (fp_text value "0.1uf" (at 0 1.16 -90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 -90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.48 0 270) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 82 "<NO NET>"))
    (pad "2" smd roundrect (at 0.48 0 270) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "cm4_cluster:RTL8370" (layer "F.Cu")
    (tedit 600702F0)
    (at 63.99 54.96)
    (property "Sheet file" "switch.kicad_sch")
    (property "Sheet name" "switch")
    (fp_text reference "U1" (at -0.74 -10.6 unlocked) (layer "F.SilkS"))
    (fp_text value "RTL8370N" (at -0.1 4.05 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.5 unlocked) (layer "F.Fab"))
    (pad "1" smd oval (at -9.35 8.189999 180) (size 0.279999 1.879999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 28 "/P2_CP") (pinfunction "P2MDICP") (solder_mask_margin 0.0508))
    (pad "2" smd oval (at -8.850001 8.189999 180) (size 0.279999 1.879999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 27 "/P2_CN") (pinfunction "P2MDICN") (solder_mask_margin 0.0508))
    (pad "3" smd oval (at -8.349999 8.189999 180) (size 0.279999 1.879999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 26 "/P2_DP") (pinfunction "P2MDIDP") (solder_mask_margin 0.0508))
    (pad "4" smd oval (at -7.85 8.189999 180) (size 0.279999 1.879999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 25 "/P2_DN") (pinfunction "P2MDIDN") (solder_mask_margin 0.0508))
    (pad "5" smd oval (at -7.349998 8.189999 180) (size 0.279999 1.879999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 82 "<NO NET>") (pinfunction "AVDDH") (solder_mask_margin 0.0508))
    (pad "6" smd oval (at -6.849999 8.189999 180) (size 0.279999 1.879999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 40 "/P3_AP") (pinfunction "P3MDIAP") (solder_mask_margin 0.0508))
    (pad "7" smd oval (at -6.35 8.189999 180) (size 0.279999 1.879999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 39 "/P3_AN") (pinfunction "P3MDIAN") (solder_mask_margin 0.0508))
    (pad "8" smd oval (at -5.849999 8.189999 180) (size 0.279999 1.879999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 38 "/P3_BP") (pinfunction "P3MDIBP") (solder_mask_margin 0.0508))
    (pad "9" smd oval (at -5.35 8.189999 180) (size 0.279999 1.879999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 37 "/P3_BN") (pinfunction "P3MDIBN") (solder_mask_margin 0.0508))
    (pad "10" smd oval (at -4.849998 8.189999 180) (size 0.279999 1.879999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 83 "/switch/+1v") (pinfunction "AVDDL") (solder_mask_margin 0.0508))
    (pad "11" smd oval (at -4.349999 8.189999 180) (size 0.279999 1.879999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 36 "/P3_CP") (pinfunction "P3MDICP") (solder_mask_margin 0.0508))
    (pad "12" smd oval (at -3.85 8.189999 180) (size 0.279999 1.879999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "/P3_CN") (pinfunction "P3MDICN") (solder_mask_margin 0.0508))
    (pad "13" smd oval (at -3.349999 8.189999 180) (size 0.279999 1.879999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 34 "/P3_DP") (pinfunction "P3MDIDP") (solder_mask_margin 0.0508))
    (pad "14" smd oval (at -2.85 8.189999 180) (size 0.279999 1.879999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 33 "/P3_DN") (pinfunction "P3MDIDN") (solder_mask_margin 0.0508))
    (pad "15" smd oval (at -2.349998 8.189999 180) (size 0.279999 1.879999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 82 "<NO NET>") (pinfunction "AVDDH") (solder_mask_margin 0.0508))
    (pad "16" smd oval (at -1.849999 8.189999 180) (size 0.279999 1.879999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "AGND") (solder_mask_margin 0.0508))
    (pad "17" smd oval (at -1.35 8.189999 180) (size 0.279999 1.879999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 84 "Net-(R13-Pad2)") (pinfunction "MDIREF") (solder_mask_margin 0.0508))
    (pad "18" smd oval (at -0.849999 8.189999 180) (size 0.279999 1.879999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 83 "/switch/+1v") (pinfunction "AVDDL") (solder_mask_margin 0.0508))
    (pad "19" smd oval (at -0.35 8.189999 180) (size 0.279999 1.879999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 82 "<NO NET>") (pinfunction "AVDDH") (solder_mask_margin 0.0508))
    (pad "20" smd oval (at 0.150002 8.189999 180) (size 0.279999 1.879999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 83 "/switch/+1v") (pinfunction "DVDDL") (solder_mask_margin 0.0508))
    (pad "21" smd oval (at 0.650001 8.189999 180) (size 0.279999 1.879999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 83 "/switch/+1v") (pinfunction "DVDDL") (solder_mask_margin 0.0508))
    (pad "22" smd oval (at 1.15 8.189999 180) (size 0.279999 1.879999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 83 "/switch/+1v") (pinfunction "DVDDL") (solder_mask_margin 0.0508))
    (pad "23" smd oval (at 1.649999 8.189999 180) (size 0.279999 1.879999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 83 "/switch/+1v") (pinfunction "DVDDL") (solder_mask_margin 0.0508))
    (pad "24" smd oval (at 2.15 8.189999 180) (size 0.279999 1.879999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 82 "<NO NET>") (pinfunction "AVDDH") (solder_mask_margin 0.0508))
    (pad "25" smd oval (at 2.650002 8.189999 180) (size 0.279999 1.879999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 48 "/P4_AP") (pinfunction "P4MDIAP") (solder_mask_margin 0.0508))
    (pad "26" smd oval (at 3.150001 8.189999 180) (size 0.279999 1.879999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 47 "/P4_AN") (pinfunction "P4MDIAN") (solder_mask_margin 0.0508))
    (pad "27" smd oval (at 3.65 8.189999 180) (size 0.279999 1.879999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 46 "/P4_BP") (pinfunction "P4MDIBP") (solder_mask_margin 0.0508))
    (pad "28" smd oval (at 4.149999 8.189999 180) (size 0.279999 1.879999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 45 "/P4_BN") (pinfunction "P4MDIBN") (solder_mask_margin 0.0508))
    (pad "29" smd oval (at 4.65 8.189999 180) (size 0.279999 1.879999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 83 "/switch/+1v") (pinfunction "AVDDL") (solder_mask_margin 0.0508))
    (pad "30" smd oval (at 5.150002 8.189999 180) (size 0.279999 1.879999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 44 "/P4_CP") (pinfunction "P4MDICP") (solder_mask_margin 0.0508))
    (pad "31" smd oval (at 5.650001 8.189999 180) (size 0.279999 1.879999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 43 "/P4_CN") (pinfunction "P4MDICN") (solder_mask_margin 0.0508))
    (pad "32" smd oval (at 6.15 8.189999 180) (size 0.279999 1.879999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 42 "/P4_DP") (pinfunction "P4MDIDP") (solder_mask_margin 0.0508))
    (pad "33" smd oval (at 6.649999 8.189999 180) (size 0.279999 1.879999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 41 "/P4_DN") (pinfunction "P4MDIDN") (solder_mask_margin 0.0508))
    (pad "34" smd oval (at 7.15 8.189999 180) (size 0.279999 1.879999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 82 "<NO NET>") (pinfunction "AVDDH") (solder_mask_margin 0.0508))
    (pad "35" smd oval (at 7.650002 8.189999 180) (size 0.279999 1.879999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 56 "/P5_AP") (pinfunction "P5MDIAP") (solder_mask_margin 0.0508))
    (pad "36" smd oval (at 8.150001 8.189999 180) (size 0.279999 1.879999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 55 "/P5_AN") (pinfunction "P5MDIAN") (solder_mask_margin 0.0508))
    (pad "37" smd oval (at 8.65 8.189999 180) (size 0.279999 1.879999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 54 "/P5_BP") (pinfunction "P5MDIBP") (solder_mask_margin 0.0508))
    (pad "38" smd oval (at 9.149999 8.189999 180) (size 0.279999 1.879999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 53 "/P5_BN") (pinfunction "P5MDIBN") (solder_mask_margin 0.0508))
    (pad "39" smd oval (at 11.04 6.3 270) (size 0.279999 1.879999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 83 "/switch/+1v") (pinfunction "AVDDL") (solder_mask_margin 0.0508))
    (pad "40" smd oval (at 11.04 5.800001 270) (size 0.279999 1.879999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 52 "/P5_CP") (pinfunction "P5MDICP") (solder_mask_margin 0.0508))
    (pad "41" smd oval (at 11.04 5.3 270) (size 0.279999 1.879999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 51 "/P5_CN") (pinfunction "P5MDICN") (solder_mask_margin 0.0508))
    (pad "42" smd oval (at 11.04 4.800001 270) (size 0.279999 1.879999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 50 "/P5_DP") (pinfunction "P5MDIDP") (solder_mask_margin 0.0508))
    (pad "43" smd oval (at 11.04 4.299999 270) (size 0.279999 1.879999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 49 "/P5_DN") (pinfunction "P5MDIDN") (solder_mask_margin 0.0508))
    (pad "44" smd oval (at 11.04 3.8 270) (size 0.279999 1.879999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 83 "/switch/+1v") (pinfunction "PLLVDDL1") (solder_mask_margin 0.0508))
    (pad "45" smd oval (at 11.04 3.300001 270) (size 0.279999 1.879999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 64 "/P6_AP") (pinfunction "P6MDIAP") (solder_mask_margin 0.0508))
    (pad "46" smd oval (at 11.04 2.8 270) (size 0.279999 1.879999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 63 "/P6_AN") (pinfunction "P6MDIAN") (solder_mask_margin 0.0508))
    (pad "47" smd oval (at 11.04 2.300001 270) (size 0.279999 1.879999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 62 "/P6_BP") (pinfunction "P6MDIBP") (solder_mask_margin 0.0508))
    (pad "48" smd oval (at 11.04 1.799999 270) (size 0.279999 1.879999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 61 "/P6_BN") (pinfunction "P6MDIBN") (solder_mask_margin 0.0508))
    (pad "49" smd oval (at 11.04 1.3 270) (size 0.279999 1.879999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 83 "/switch/+1v") (pinfunction "AVDDL") (solder_mask_margin 0.0508))
    (pad "50" smd oval (at 11.04 0.800001 270) (size 0.279999 1.879999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 60 "/P6_CP") (pinfunction "P6MDICP") (solder_mask_margin 0.0508))
    (pad "51" smd oval (at 11.04 0.299999 270) (size 0.279999 1.879999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 59 "/P6_CN") (pinfunction "P6MDICN") (solder_mask_margin 0.0508))
    (pad "52" smd oval (at 11.04 -0.2 270) (size 0.279999 1.879999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 58 "/P6_DP") (pinfunction "P6MDIDP") (solder_mask_margin 0.0508))
    (pad "53" smd oval (at 11.04 -0.700001 270) (size 0.279999 1.879999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 57 "/P6_DN") (pinfunction "P6MDIDN") (solder_mask_margin 0.0508))
    (pad "54" smd oval (at 11.04 -1.2 270) (size 0.279999 1.879999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 82 "<NO NET>") (pinfunction "AVDDH") (solder_mask_margin 0.0508))
    (pad "55" smd oval (at 11.04 -1.699999 270) (size 0.279999 1.879999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 72 "/P7_AP") (pinfunction "P7MDIAP") (solder_mask_margin 0.0508))
    (pad "56" smd oval (at 11.04 -2.200001 270) (size 0.279999 1.879999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 71 "/P7_AN") (pinfunction "P7MDIAN") (solder_mask_margin 0.0508))
    (pad "57" smd oval (at 11.04 -2.7 270) (size 0.279999 1.879999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 70 "/P7_BP") (pinfunction "P7MDIBP") (solder_mask_margin 0.0508))
    (pad "58" smd oval (at 11.04 -3.200001 270) (size 0.279999 1.879999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 69 "/P7_BN") (pinfunction "P7MDIBN") (solder_mask_margin 0.0508))
    (pad "59" smd oval (at 11.04 -3.7 270) (size 0.279999 1.879999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 83 "/switch/+1v") (pinfunction "AVDDL") (solder_mask_margin 0.0508))
    (pad "60" smd oval (at 11.04 -4.199999 270) (size 0.279999 1.879999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 68 "/P7_CP") (pinfunction "P7MDICP") (solder_mask_margin 0.0508))
    (pad "61" smd oval (at 11.04 -4.699998 270) (size 0.279999 1.879999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 67 "/P7_CN") (pinfunction "P7MDICN") (solder_mask_margin 0.0508))
    (pad "62" smd oval (at 11.04 -5.2 270) (size 0.279999 1.879999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 66 "/P7_DP") (pinfunction "P7MDIDP") (solder_mask_margin 0.0508))
    (pad "63" smd oval (at 11.04 -5.700001 270) (size 0.279999 1.879999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 65 "/P7_DN") (pinfunction "P7MDIDN") (solder_mask_margin 0.0508))
    (pad "64" smd oval (at 11.04 -6.2 270) (size 0.279999 1.879999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 82 "<NO NET>") (pinfunction "AVDDH") (solder_mask_margin 0.0508))
    (pad "65" smd oval (at 9.149999 -8.090002) (size 0.279999 1.879999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 116 "no_connect_127") (pinfunction "RESERVED") (solder_mask_margin 0.0508))
    (pad "66" smd oval (at 8.65 -8.090002) (size 0.279999 1.879999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 115 "no_connect_128") (pinfunction "RESERVED") (solder_mask_margin 0.0508))
    (pad "67" smd oval (at 8.149998 -8.090002) (size 0.279999 1.879999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 114 "/switch/SPI_CLK") (pinfunction "P7LED2") (solder_mask_margin 0.0508))
    (pad "68" smd oval (at 7.649999 -8.090002) (size 0.279999 1.879999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 113 "/switch/SPI_D1") (pinfunction "P7LED0") (solder_mask_margin 0.0508))
    (pad "69" smd oval (at 7.149998 -8.090002) (size 0.279999 1.879999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 112 "/switch/SPI_D0") (pinfunction "P7LED1") (solder_mask_margin 0.0508))
    (pad "70" smd oval (at 6.649999 -8.090002) (size 0.279999 1.879999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 111 "/switch/SPI_CS") (pinfunction "P6LED2") (solder_mask_margin 0.0508))
    (pad "71" smd oval (at 6.15 -8.090002) (size 0.279999 1.879999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 110 "Net-(U1-Pad71)") (pinfunction "P6LED0") (solder_mask_margin 0.0508))
    (pad "72" smd oval (at 5.649998 -8.090002) (size 0.279999 1.879999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 109 "Net-(U1-Pad72)") (pinfunction "P6LED1") (solder_mask_margin 0.0508))
    (pad "73" smd oval (at 5.149999 -8.090002) (size 0.279999 1.879999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 108 "Net-(U1-Pad73)") (pinfunction "P5LED2") (solder_mask_margin 0.0508))
    (pad "74" smd oval (at 4.649998 -8.090002) (size 0.279999 1.879999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 107 "Net-(U1-Pad74)") (pinfunction "P5LED0") (solder_mask_margin 0.0508))
    (pad "75" smd oval (at 4.149999 -8.090002) (size 0.279999 1.879999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 106 "Net-(U1-Pad75)") (pinfunction "P5LED1") (solder_mask_margin 0.0508))
    (pad "76" smd oval (at 3.65 -8.090002) (size 0.279999 1.879999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 83 "/switch/+1v") (pinfunction "DVDDL") (solder_mask_margin 0.0508))
    (pad "77" smd oval (at 3.149998 -8.090002) (size 0.279999 1.879999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 82 "<NO NET>") (pinfunction "DVDDIO") (solder_mask_margin 0.0508))
    (pad "78" smd oval (at 2.649999 -8.090002) (size 0.279999 1.879999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 83 "/switch/+1v") (pinfunction "DVDDL") (solder_mask_margin 0.0508))
    (pad "79" smd oval (at 2.149998 -8.090002) (size 0.279999 1.879999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 105 "Net-(U1-Pad79)") (pinfunction "P4LED2") (solder_mask_margin 0.0508))
    (pad "80" smd oval (at 1.649999 -8.090002) (size 0.279999 1.879999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 104 "Net-(U1-Pad80)") (pinfunction "P4LED0") (solder_mask_margin 0.0508))
    (pad "81" smd oval (at 1.15 -8.090002) (size 0.279999 1.879999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 103 "Net-(U1-Pad81)") (pinfunction "P4LED1") (solder_mask_margin 0.0508))
    (pad "82" smd oval (at 0.649998 -8.090002) (size 0.279999 1.879999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 102 "Net-(U1-Pad82)") (pinfunction "P3LED1") (solder_mask_margin 0.0508))
    (pad "83" smd oval (at 0.149999 -8.090002) (size 0.279999 1.879999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 101 "Net-(U1-Pad83)") (pinfunction "P3LED2") (solder_mask_margin 0.0508))
    (pad "84" smd oval (at -0.350002 -8.090002) (size 0.279999 1.879999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 100 "Net-(U1-Pad84)") (pinfunction "P3LED0") (solder_mask_margin 0.0508))
    (pad "85" smd oval (at -0.850001 -8.090002) (size 0.279999 1.879999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 99 "Net-(U1-Pad85)") (pinfunction "P2LED2") (solder_mask_margin 0.0508))
    (pad "86" smd oval (at -1.35 -8.090002) (size 0.279999 1.879999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 98 "Net-(U1-Pad86)") (pinfunction "P2LED0") (solder_mask_margin 0.0508))
    (pad "87" smd oval (at -1.849999 -8.090002) (size 0.279999 1.879999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 97 "Net-(U1-Pad87)") (pinfunction "P2LED1") (solder_mask_margin 0.0508))
    (pad "88" smd oval (at -2.350001 -8.090002) (size 0.279999 1.879999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 96 "Net-(U1-Pad88)") (pinfunction "P1LED2") (solder_mask_margin 0.0508))
    (pad "89" smd oval (at -2.850002 -8.090002) (size 0.279999 1.879999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 95 "Net-(U1-Pad89)") (pinfunction "P1LED0") (solder_mask_margin 0.0508))
    (pad "90" smd oval (at -3.350001 -8.090002) (size 0.279999 1.879999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 94 "Net-(U1-Pad90)") (pinfunction "P1LED1") (solder_mask_margin 0.0508))
    (pad "91" smd oval (at -3.85 -8.090002) (size 0.279999 1.879999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 93 "Net-(U1-Pad91)") (pinfunction "P0LED2") (solder_mask_margin 0.0508))
    (pad "92" smd oval (at -4.349999 -8.090002) (size 0.279999 1.879999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 83 "/switch/+1v") (pinfunction "DVDDL") (solder_mask_margin 0.0508))
    (pad "93" smd oval (at -4.850001 -8.090002) (size 0.279999 1.879999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 92 "Net-(U1-Pad93)") (pinfunction "P0LED1") (solder_mask_margin 0.0508))
    (pad "94" smd oval (at -5.350002 -8.090002) (size 0.279999 1.879999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 91 "Net-(U1-Pad94)") (pinfunction "P0LED0") (solder_mask_margin 0.0508))
    (pad "95" smd oval (at -5.850001 -8.090002) (size 0.279999 1.879999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 83 "/switch/+1v") (pinfunction "DVDDL") (solder_mask_margin 0.0508))
    (pad "96" smd oval (at -6.35 -8.090002) (size 0.279999 1.879999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 82 "<NO NET>") (pinfunction "AVDDH") (solder_mask_margin 0.0508))
    (pad "97" smd oval (at -6.849999 -8.090002) (size 0.279999 1.879999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "Net-(C1-Pad1)") (pinfunction "XTAL0") (solder_mask_margin 0.0508))
    (pad "98" smd oval (at -7.350001 -8.090002) (size 0.279999 1.879999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "Net-(C2-Pad1)") (pinfunction "XTAL1") (solder_mask_margin 0.0508))
    (pad "99" smd oval (at -7.850003 -8.090002) (size 0.279999 1.879999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 85 "/switch/nRESET") (pinfunction "nRESET") (solder_mask_margin 0.0508))
    (pad "100" smd oval (at -8.350002 -8.090002) (size 0.279999 1.879999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 90 "/switch/SCK") (pinfunction "SCK/MDC") (solder_mask_margin 0.0508))
    (pad "101" smd oval (at -8.850001 -8.090002) (size 0.279999 1.879999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 89 "/switch/SDA") (pinfunction "SDA/MDIO") (solder_mask_margin 0.0508))
    (pad "102" smd oval (at -9.35 -8.090002) (size 0.279999 1.879999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 82 "<NO NET>") (pinfunction "AVDDH") (solder_mask_margin 0.0508))
    (pad "103" smd oval (at -11.240001 -6.2 90) (size 0.279999 1.879999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 80 "/P0_AP") (pinfunction "P0MDIAP") (solder_mask_margin 0.0508))
    (pad "104" smd oval (at -11.240001 -5.700001 90) (size 0.279999 1.879999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 79 "/P0_AN") (pinfunction "P0MDIAN") (solder_mask_margin 0.0508))
    (pad "105" smd oval (at -11.240001 -5.2 90) (size 0.279999 1.879999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 78 "/P0_BP") (pinfunction "P0MDIBP") (solder_mask_margin 0.0508))
    (pad "106" smd oval (at -11.240001 -4.700001 90) (size 0.279999 1.879999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 75 "/P0_BN") (pinfunction "P0MDIBN") (solder_mask_margin 0.0508))
    (pad "107" smd oval (at -11.240001 -4.199999 90) (size 0.279999 1.879999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 83 "/switch/+1v") (pinfunction "AVDDL") (solder_mask_margin 0.0508))
    (pad "108" smd oval (at -11.240001 -3.7 90) (size 0.279999 1.879999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 77 "/P0_CP") (pinfunction "P0MDICP") (solder_mask_margin 0.0508))
    (pad "109" smd oval (at -11.240001 -3.200001 90) (size 0.279999 1.879999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 76 "/P0_CN") (pinfunction "P0MDICN") (solder_mask_margin 0.0508))
    (pad "110" smd oval (at -11.240001 -2.7 90) (size 0.279999 1.879999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 74 "/P0_DP") (pinfunction "P0MDIDP") (solder_mask_margin 0.0508))
    (pad "111" smd oval (at -11.240001 -2.200001 90) (size 0.279999 1.879999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 73 "/P0_DN") (pinfunction "P0MDIDN") (solder_mask_margin 0.0508))
    (pad "112" smd oval (at -11.240001 -1.699999 90) (size 0.279999 1.879999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 82 "<NO NET>") (pinfunction "AVDDH") (solder_mask_margin 0.0508))
    (pad "113" smd oval (at -11.240001 -1.2 90) (size 0.279999 1.879999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 24 "/P1_AP") (pinfunction "P1MDIAP") (solder_mask_margin 0.0508))
    (pad "114" smd oval (at -11.240001 -0.700001 90) (size 0.279999 1.879999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 23 "/P1_AN") (pinfunction "P1MDIAN") (solder_mask_margin 0.0508))
    (pad "115" smd oval (at -11.240001 -0.2 90) (size 0.279999 1.879999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 22 "/P1_BP") (pinfunction "P1MDIBP") (solder_mask_margin 0.0508))
    (pad "116" smd oval (at -11.240001 0.299999 90) (size 0.279999 1.879999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 21 "/P1_BN") (pinfunction "P1MDIBN") (solder_mask_margin 0.0508))
    (pad "117" smd oval (at -11.240001 0.800001 90) (size 0.279999 1.879999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 83 "/switch/+1v") (pinfunction "AVDDL") (solder_mask_margin 0.0508))
    (pad "118" smd oval (at -11.240001 1.3 90) (size 0.279999 1.879999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 20 "/P1_CP") (pinfunction "P1MDICP") (solder_mask_margin 0.0508))
    (pad "119" smd oval (at -11.240001 1.799999 90) (size 0.279999 1.879999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 19 "/P1_CN") (pinfunction "P1MDICN") (solder_mask_margin 0.0508))
    (pad "120" smd oval (at -11.240001 2.300001 90) (size 0.279999 1.879999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 18 "/P1_DP") (pinfunction "P1MDIDP") (solder_mask_margin 0.0508))
    (pad "121" smd oval (at -11.240001 2.8 90) (size 0.279999 1.879999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 17 "/P1_DN") (pinfunction "P1MDIDN") (solder_mask_margin 0.0508))
    (pad "122" smd oval (at -11.240001 3.300001 90) (size 0.279999 1.879999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 83 "/switch/+1v") (pinfunction "PLLVDDL0") (solder_mask_margin 0.0508))
    (pad "123" smd oval (at -11.240001 3.8 90) (size 0.279999 1.879999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 88 "no_connect_126") (pinfunction "ATESTCK0") (solder_mask_margin 0.0508))
    (pad "124" smd oval (at -11.240001 4.299999 90) (size 0.279999 1.879999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 32 "/P2_AP") (pinfunction "P2MDIAP") (solder_mask_margin 0.0508))
    (pad "125" smd oval (at -11.240001 4.799998 90) (size 0.279999 1.879999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 31 "/P2_AN") (pinfunction "P2MDIAN") (solder_mask_margin 0.0508))
    (pad "126" smd oval (at -11.240001 5.3 90) (size 0.279999 1.879999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 30 "/P2_BP") (pinfunction "P2MDIBP") (solder_mask_margin 0.0508))
    (pad "127" smd oval (at -11.240001 5.800001 90) (size 0.279999 1.879999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 29 "/P2_BN") (pinfunction "P2MDIBN") (solder_mask_margin 0.0508))
    (pad "128" smd oval (at -11.240001 6.3 90) (size 0.279999 1.879999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 83 "/switch/+1v") (pinfunction "AVDDL") (solder_mask_margin 0.0508))
    (pad "129" smd custom (at -0.1 0.05) (size 6.6 6.100001) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND")
      (options (clearance outline) (anchor rect))
      (primitives
      ))
  )
  (footprint "CM4IO:5557_connector" (layer "F.Cu")
    (tedit 600EAEB3)
    (at 139.16 31.23 90)
    (property "Sheet file" "switch.kicad_sch")
    (property "Sheet name" "switch")
    (fp_text reference "J2" (at -4.61 0) (layer "B.SilkS"))
    (fp_text value "Conn_02x12_Top_Bottom" (at 12.41 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at -2.11 2.1 90) (size 2 2) (drill 1.15) (layers *.Cu *.Mask)
      (net 16 "Net-(J2-Pad13)") (pinfunction "Pin_1"))
    (pad "1" thru_hole circle (at 2.09 2.1 90) (size 2 2) (drill 1.15) (layers *.Cu *.Mask)
      (net 16 "Net-(J2-Pad13)") (pinfunction "Pin_2"))
    (pad "2" thru_hole circle (at 2.09 -2.1 90) (size 2 2) (drill 1.15) (layers *.Cu *.Mask)
      (net 15 "Net-(J2-Pad14)") (pinfunction "Pin_14"))
    (pad "2" thru_hole circle (at -2.11 -2.1 90) (size 2 2) (drill 1.15) (layers *.Cu *.Mask)
      (net 15 "Net-(J2-Pad14)") (pinfunction "Pin_13"))
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 52.75 63.34 -90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheet file" "switch.kicad_sch")
    (property "Sheet name" "switch")
    (attr smd)
    (fp_text reference "C39" (at -0.04 1.21 -90) (layer "F.SilkS"))
    (fp_text value "0.1uf" (at 0 1.16 -90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 -90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.48 0 270) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 83 "/switch/+1v"))
    (pad "2" smd roundrect (at 0.48 0 270) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_SMA" (layer "F.Cu")
    (tedit 6006F126)
    (at 84.92 45.16 90)
    (descr "Diode SMA (DO-214AC)")
    (tags "Diode SMA (DO-214AC)")
    (property "Sheet file" "switch.kicad_sch")
    (property "Sheet name" "switch")
    (attr smd)
    (fp_text reference "D9" (at 3.3 -1.82 90) (layer "F.SilkS"))
    (fp_text value "D" (at 0 2.6 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -2.5 90) (layer "F.Fab"))
    (pad "1" smd rect (at -2 0 90) (size 2.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "/+5v") (pinfunction "K"))
    (pad "2" smd rect (at 2 0 90) (size 2.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 7 "Net-(C18-Pad1)") (pinfunction "A"))
    (model "${KISYS3DMOD}/Diode_SMD.3dshapes/D_SMA.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Inductor_SMD:L_Bourns_SRN6045TA" (layer "F.Cu")
    (tedit 5B61DEEA)
    (at 99.31 27.34 -90)
    (descr "http://www.bourns.com/docs/product-datasheets/srn6045ta.pdf")
    (tags "Semi-shielded Power Inductor")
    (property "Sheet file" "switch.kicad_sch")
    (property "Sheet name" "switch")
    (attr smd)
    (fp_text reference "L2" (at -1.34 4.49 90) (layer "F.SilkS"))
    (fp_text value "22uh" (at 0 4.2 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect (at -2.075 0 270) (size 2.35 5.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 14 "Net-(D8-Pad1)") (pinfunction "1"))
    (pad "2" smd rect (at 2.075 0 270) (size 2.35 5.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 8 "Net-(C19-Pad1)") (pinfunction "2"))
    (model "${KISYS3DMOD}/Inductor_SMD.3dshapes/L_Bourns_SRN6045TA.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinSocket_2.54mm:PinSocket_2x06_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 5A19A42B)
    (at 68.86 82.41 180)
    (descr "Through hole straight socket strip, 2x06, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 2x06 2.54mm double row")
    (property "Sheet file" "cluster4.kicad_sch")
    (property "Sheet name" "")
    (attr through_hole)
    (fp_text reference "J5" (at -3.14 15.16) (layer "F.SilkS"))
    (fp_text value "Conn_01x11_Female" (at -1.27 15.47) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at -1.27 6.35 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 "/+12v") (pinfunction "Pin_1"))
    (pad "2" thru_hole oval (at -2.54 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "/+5v") (pinfunction "Pin_2"))
    (pad "3" thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_3"))
    (pad "4" thru_hole oval (at -2.54 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 40 "/P3_AP") (pinfunction "Pin_4"))
    (pad "5" thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 39 "/P3_AN") (pinfunction "Pin_5"))
    (pad "6" thru_hole oval (at -2.54 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 38 "/P3_BP") (pinfunction "Pin_6"))
    (pad "7" thru_hole oval (at 0 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 37 "/P3_BN") (pinfunction "Pin_7"))
    (pad "8" thru_hole oval (at -2.54 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 36 "/P3_CP") (pinfunction "Pin_8"))
    (pad "9" thru_hole oval (at 0 10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 35 "/P3_CN") (pinfunction "Pin_9"))
    (pad "10" thru_hole oval (at -2.54 10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 "/P3_DP") (pinfunction "Pin_10"))
    (pad "11" thru_hole oval (at 0 12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 33 "/P3_DN") (pinfunction "Pin_11"))
    (pad "12" thru_hole oval (at -2.54 12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model "${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_2x06_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 48.82 53.26 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheet file" "switch.kicad_sch")
    (property "Sheet name" "switch")
    (attr smd)
    (fp_text reference "C36" (at 0 -1.16 180) (layer "F.SilkS"))
    (fp_text value "0.1uf" (at 0 1.16 180) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 180) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.48 0 180) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 82 "<NO NET>"))
    (pad "2" smd roundrect (at 0.48 0 180) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 59.64 43.85 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheet file" "switch.kicad_sch")
    (property "Sheet name" "switch")
    (attr smd)
    (fp_text reference "C53" (at 0.15 1.29 90) (layer "F.SilkS"))
    (fp_text value "0.1uf" (at 0 1.16 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.48 0 90) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 83 "/switch/+1v"))
    (pad "2" smd roundrect (at 0.48 0 90) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0402_1005Metric" (layer "F.Cu")
    (tedit 600E9B4E)
    (at 83.38 57.64)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (attr smd)
    (fp_text reference "R15" (at 0.06 1.2) (layer "F.SilkS"))
    (fp_text value "4.7k" (at 0 1.17) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.51 0) (size 0.54 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 82 "<NO NET>"))
    (pad "2" smd roundrect (at 0.51 0) (size 0.54 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:CP_Elec_10x10" (layer "F.Cu")
    (tedit 600E8663)
    (at 109.1 54.68 90)
    (descr "SMD capacitor, aluminum electrolytic, Nichicon, 10.0x10.0mm")
    (tags "capacitor electrolytic")
    (property "Sheet file" "switch.kicad_sch")
    (property "Sheet name" "switch")
    (attr smd)
    (fp_text reference "C34" (at 0 -6.2 90) (layer "F.SilkS"))
    (fp_text value "470uf" (at 0 6.2 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -4 0 90) (size 4 2.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1)
      (net 11 "/+12v"))
    (pad "2" smd roundrect (at 4 0 90) (size 4 2.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1)
      (net 1 "GND"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/CP_Elec_10x10.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinSocket_2.54mm:PinSocket_2x06_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 5A19A42B)
    (at 51.72 82.41 180)
    (descr "Through hole straight socket strip, 2x06, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 2x06 2.54mm double row")
    (property "Sheet file" "cluster4.kicad_sch")
    (property "Sheet name" "")
    (attr through_hole)
    (fp_text reference "J4" (at 0.07 15.65) (layer "F.SilkS"))
    (fp_text value "Conn_01x11_Female" (at -1.27 15.47) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at -1.27 6.35 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 "/+12v") (pinfunction "Pin_1"))
    (pad "2" thru_hole oval (at -2.54 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "/+5v") (pinfunction "Pin_2"))
    (pad "3" thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_3"))
    (pad "4" thru_hole oval (at -2.54 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 "/P2_AP") (pinfunction "Pin_4"))
    (pad "5" thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 "/P2_AN") (pinfunction "Pin_5"))
    (pad "6" thru_hole oval (at -2.54 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 "/P2_BP") (pinfunction "Pin_6"))
    (pad "7" thru_hole oval (at 0 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 "/P2_BN") (pinfunction "Pin_7"))
    (pad "8" thru_hole oval (at -2.54 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 "/P2_CP") (pinfunction "Pin_8"))
    (pad "9" thru_hole oval (at 0 10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 "/P2_CN") (pinfunction "Pin_9"))
    (pad "10" thru_hole oval (at -2.54 10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 "/P2_DP") (pinfunction "Pin_10"))
    (pad "11" thru_hole oval (at 0 12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 "/P2_DN") (pinfunction "Pin_11"))
    (pad "12" thru_hole oval (at -2.54 12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model "${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_2x06_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 54.41 29.06 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheet file" "switch.kicad_sch")
    (property "Sheet name" "switch")
    (attr smd)
    (fp_text reference "C17" (at 0 -1.68 90) (layer "F.SilkS"))
    (fp_text value "10uf" (at 0 1.68 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.95 0 90) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "Net-(C13-Pad1)"))
    (pad "2" smd roundrect (at 0.95 0 90) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Button_Switch_SMD:SW_SPST_TL3305A" (layer "F.Cu")
    (tedit 5ABC3A97)
    (at 58.49 35.03)
    (descr "https://www.e-switch.com/system/asset/product_line/data_sheet/213/TL3305.pdf")
    (tags "TL3305 Series Tact Switch")
    (property "Sheet file" "switch.kicad_sch")
    (property "Sheet name" "switch")
    (attr smd)
    (fp_text reference "SW2" (at 0 -3.2) (layer "F.SilkS"))
    (fp_text value "SW_Push" (at 0 3.2) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect (at -3.6 -1.5) (size 1.6 1.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 85 "/switch/nRESET") (pinfunction "1"))
    (pad "1" smd rect (at 3.6 -1.5) (size 1.6 1.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 85 "/switch/nRESET") (pinfunction "1"))
    (pad "2" smd rect (at -3.6 1.5) (size 1.6 1.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "2"))
    (pad "2" smd rect (at 3.6 1.5) (size 1.6 1.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "2"))
    (model "${KISYS3DMOD}/Button_Switch_SMD.3dshapes/SW_SPST_TL3305A.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_SO:SOIC-8-1EP_3.9x4.9mm_P1.27mm_EP2.29x3mm_ThermalVias" (layer "F.Cu")
    (tedit 600EDBDC)
    (at 112.22 45.03)
    (descr "SOIC, 8 Pin (https://www.analog.com/media/en/technical-documentation/data-sheets/ada4898-1_4898-2.pdf#page=29), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (property "Sheet file" "switch.kicad_sch")
    (property "Sheet name" "switch")
    (attr smd)
    (fp_text reference "U4" (at 0 -3.4) (layer "F.SilkS"))
    (fp_text value "LM22676-5.0" (at 0 3.4) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" smd roundrect (at 0.57 0.75) (size 0.96 1.25) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0.57 -0.75) (size 0.96 1.25) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "" smd roundrect (at -0.57 -0.75) (size 0.96 1.25) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "" smd roundrect (at -0.57 0.75) (size 0.96 1.25) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "1" smd roundrect (at -2.475 -1.905) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (pinfunction "VIN"))
    (pad "2" smd roundrect (at -2.475 -0.635) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (pinfunction "OUT"))
    (pad "3" smd roundrect (at -2.475 0.635) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (pinfunction "GND"))
    (pad "4" smd roundrect (at -2.475 1.905) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 7 "Net-(C18-Pad1)") (pinfunction "FB"))
    (pad "5" smd roundrect (at 2.475 1.905) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (pinfunction "~ON~/OFF"))
    (pad "6" smd roundrect (at 2.475 0.635) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND"))
    (pad "7" smd roundrect (at 2.475 -0.635) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 6 "Net-(C10-Pad1)"))
    (pad "8" smd roundrect (at 2.475 -1.905) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 13 "Net-(D7-Pad1)"))
    (pad "9" smd rect (at 0 0) (size 1.8 2.5) (layers "B.Cu")
      (net 1 "GND"))
    (pad "9" thru_hole circle (at -0.65 0) (size 0.5 0.5) (drill 0.3) (layers *.Cu)
      (net 1 "GND"))
    (pad "9" smd rect (at 0 0) (size 2.29 3) (layers "F.Cu" "F.Mask")
      (net 1 "GND"))
    (pad "9" thru_hole circle (at -0.65 1) (size 0.5 0.5) (drill 0.3) (layers *.Cu)
      (net 1 "GND"))
    (pad "9" thru_hole circle (at -0.65 -1) (size 0.5 0.5) (drill 0.3) (layers *.Cu)
      (net 1 "GND"))
    (pad "9" thru_hole circle (at 0.65 -1) (size 0.5 0.5) (drill 0.3) (layers *.Cu)
      (net 1 "GND"))
    (pad "9" thru_hole circle (at 0.65 1) (size 0.5 0.5) (drill 0.3) (layers *.Cu)
      (net 1 "GND"))
    (pad "9" thru_hole circle (at 0.65 0) (size 0.5 0.5) (drill 0.3) (layers *.Cu)
      (net 1 "GND"))
    (model "${KISYS3DMOD}/Package_SO.3dshapes/SOIC-8-1EP_3.9x4.9mm_P1.27mm_EP2.29x3mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 120.48 44.94 -90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Field4" "Digikey")
    (property "Field5" "490-10505-1-ND")
    (property "Field6" "GRM21BC8YA106KE11L ")
    (property "Field7" "Murata")
    (property "Field8" "")
    (property "Part Description" "	10uF 10% or 20% 35V Ceramic Capacitor X6S 0805 (2012 Metric)")
    (property "Sheet file" "switch.kicad_sch")
    (property "Sheet name" "switch")
    (attr smd)
    (fp_text reference "C6" (at 0 -1.68 90) (layer "F.SilkS"))
    (fp_text value "10u" (at 0 1.68 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.95 0 270) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 6 "Net-(C10-Pad1)"))
    (pad "2" smd roundrect (at 0.95 0 270) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 120.98 32.22 -90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Field4" "Digikey")
    (property "Field5" "490-10505-1-ND")
    (property "Field6" "GRM21BC8YA106KE11L ")
    (property "Field7" "Murata")
    (property "Field8" "")
    (property "Part Description" "	10uF 10% or 20% 35V Ceramic Capacitor X6S 0805 (2012 Metric)")
    (property "Sheet file" "switch.kicad_sch")
    (property "Sheet name" "switch")
    (attr smd)
    (fp_text reference "C16" (at 0.01 -1.84 90) (layer "F.SilkS"))
    (fp_text value "10u" (at 0 1.68 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.95 0 270) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 6 "Net-(C10-Pad1)"))
    (pad "2" smd roundrect (at 0.95 0 270) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 96.53 33.24 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Field4" "Digikey")
    (property "Field5" "490-14381-1-ND")
    (property "Field6" "GRM21BR71A106KA73L")
    (property "Field7" "Murata")
    (property "Field8" "111893011")
    (property "Part Description" "	10uF 10% 10V Ceramic Capacitor X7R 0805 (2012 Metric)")
    (property "Sheet file" "switch.kicad_sch")
    (property "Sheet name" "switch")
    (attr smd)
    (fp_text reference "C26" (at -2.44 -0.49 180) (layer "F.SilkS"))
    (fp_text value "10u" (at 0 1.68 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.95 0 90) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 8 "Net-(C19-Pad1)"))
    (pad "2" smd roundrect (at 0.95 0 90) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0402_1005Metric" (layer "F.Cu")
    (tedit 600B0654)
    (at 53.43 43.03 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (attr smd)
    (fp_text reference "R1" (at -1.8 0.08 90) (layer "F.SilkS"))
    (fp_text value "4.7k" (at 0 1.17 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.51 0 90) (size 0.54 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 90 "/switch/SCK"))
    (pad "2" smd roundrect (at 0.51 0 90) (size 0.54 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 82 "<NO NET>"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_SMA" (layer "F.Cu")
    (tedit 586432E5)
    (at 67.26 36.25)
    (descr "Diode SMA (DO-214AC)")
    (tags "Diode SMA (DO-214AC)")
    (property "Sheet file" "switch.kicad_sch")
    (property "Sheet name" "switch")
    (attr smd)
    (fp_text reference "D6" (at 0 -2.5) (layer "F.SilkS"))
    (fp_text value "D" (at 0 2.6) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -2.5) (layer "F.Fab"))
    (pad "1" smd rect (at -2 0) (size 2.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "Net-(D6-Pad1)") (pinfunction "K"))
    (pad "2" smd rect (at 2 0) (size 2.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "Net-(C13-Pad1)") (pinfunction "A"))
    (model "${KISYS3DMOD}/Diode_SMD.3dshapes/D_SMA.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0402_1005Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 76.02 34.61 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheet file" "switch.kicad_sch")
    (property "Sheet name" "switch")
    (attr smd)
    (fp_text reference "R34" (at 2.44 0.08) (layer "F.SilkS"))
    (fp_text value "1k" (at 0 1.17) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.51 0 180) (size 0.54 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 87 "Net-(R34-Pad1)"))
    (pad "2" smd roundrect (at 0.51 0 180) (size 0.54 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 82 "<NO NET>"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 76.15 62.71 -90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheet file" "switch.kicad_sch")
    (property "Sheet name" "switch")
    (attr smd)
    (fp_text reference "C46" (at 0.51 2.03 90) (layer "F.SilkS"))
    (fp_text value "0.1uf" (at 0 1.16 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.48 0 270) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 83 "/switch/+1v"))
    (pad "2" smd roundrect (at 0.48 0 270) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (tedit 60070D12)
    (at 81.45 24.75 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheet file" "switch.kicad_sch")
    (property "Sheet name" "switch")
    (attr smd)
    (fp_text reference "C31" (at 0.01 -1.47 90) (layer "F.SilkS"))
    (fp_text value "10uf" (at 0 1.68 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.95 0 90) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 83 "/switch/+1v"))
    (pad "2" smd roundrect (at 0.95 0 90) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_SMA" (layer "F.Cu")
    (tedit 600EB393)
    (at 130.21 30.72)
    (descr "Diode SMA (DO-214AC)")
    (tags "Diode SMA (DO-214AC)")
    (property "Sheet file" "switch.kicad_sch")
    (property "Sheet name" "switch")
    (attr smd)
    (fp_text reference "D2" (at -4.84 -0.13) (layer "F.SilkS"))
    (fp_text value "D" (at 0 2.6) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -2.5) (layer "F.Fab"))
    (pad "1" smd rect (at -2 0) (size 2.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 6 "Net-(C10-Pad1)") (pinfunction "K"))
    (pad "2" smd rect (at 2 0) (size 2.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 16 "Net-(J2-Pad13)") (pinfunction "A"))
    (model "${KISYS3DMOD}/Diode_SMD.3dshapes/D_SMA.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 61.62 66.82 -90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheet file" "switch.kicad_sch")
    (property "Sheet name" "switch")
    (attr smd)
    (fp_text reference "C42" (at 2.37 0.57 -90) (layer "F.SilkS"))
    (fp_text value "0.1uf" (at 0 1.16 -90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 -90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.48 0 270) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 82 "<NO NET>"))
    (pad "2" smd roundrect (at 0.48 0 270) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_SO:SOIC-8-1EP_3.9x4.9mm_P1.27mm_EP2.29x3mm_ThermalVias" (layer "F.Cu")
    (tedit 600EDBBD)
    (at 112.79 31.89)
    (descr "SOIC, 8 Pin (https://www.analog.com/media/en/technical-documentation/data-sheets/ada4898-1_4898-2.pdf#page=29), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (property "Sheet file" "switch.kicad_sch")
    (property "Sheet name" "switch")
    (attr smd)
    (fp_text reference "U6" (at 0 -3.4) (layer "F.SilkS"))
    (fp_text value "LM22676-5.0" (at 0 3.4) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" smd roundrect (at 0.57 0.75) (size 0.96 1.25) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "" smd roundrect (at -0.57 -0.75) (size 0.96 1.25) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "" smd roundrect (at -0.57 0.75) (size 0.96 1.25) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0.57 -0.75) (size 0.96 1.25) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "1" smd roundrect (at -2.475 -1.905) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (pinfunction "VIN"))
    (pad "2" smd roundrect (at -2.475 -0.635) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (pinfunction "OUT"))
    (pad "3" smd roundrect (at -2.475 0.635) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (pinfunction "GND"))
    (pad "4" smd roundrect (at -2.475 1.905) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 8 "Net-(C19-Pad1)") (pinfunction "FB"))
    (pad "5" smd roundrect (at 2.475 1.905) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (pinfunction "~ON~/OFF"))
    (pad "6" smd roundrect (at 2.475 0.635) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND"))
    (pad "7" smd roundrect (at 2.475 -0.635) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 6 "Net-(C10-Pad1)"))
    (pad "8" smd roundrect (at 2.475 -1.905) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 14 "Net-(D8-Pad1)"))
    (pad "9" thru_hole circle (at 0.65 1) (size 0.5 0.5) (drill 0.3) (layers *.Cu)
      (net 1 "GND"))
    (pad "9" thru_hole circle (at 0.65 0) (size 0.5 0.5) (drill 0.3) (layers *.Cu)
      (net 1 "GND"))
    (pad "9" thru_hole circle (at -0.65 -1) (size 0.5 0.5) (drill 0.3) (layers *.Cu)
      (net 1 "GND"))
    (pad "9" smd rect (at 0 0) (size 1.8 2.5) (layers "B.Cu")
      (net 1 "GND"))
    (pad "9" thru_hole circle (at -0.65 1) (size 0.5 0.5) (drill 0.3) (layers *.Cu)
      (net 1 "GND"))
    (pad "9" thru_hole circle (at -0.65 0) (size 0.5 0.5) (drill 0.3) (layers *.Cu)
      (net 1 "GND"))
    (pad "9" smd rect (at 0 0) (size 2.29 3) (layers "F.Cu" "F.Mask")
      (net 1 "GND"))
    (pad "9" thru_hole circle (at 0.65 -1) (size 0.5 0.5) (drill 0.3) (layers *.Cu)
      (net 1 "GND"))
    (model "${KISYS3DMOD}/Package_SO.3dshapes/SOIC-8-1EP_3.9x4.9mm_P1.27mm_EP2.29x3mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_SMA" (layer "F.Cu")
    (tedit 586432E5)
    (at 45.44 32.95 180)
    (descr "Diode SMA (DO-214AC)")
    (tags "Diode SMA (DO-214AC)")
    (property "Sheet file" "switch.kicad_sch")
    (property "Sheet name" "switch")
    (attr smd)
    (fp_text reference "D2" (at -4.84 -0.13) (layer "F.SilkS"))
    (fp_text value "D" (at 0 2.6) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -2.5) (layer "F.Fab"))
    (pad "1" smd rect (at -2 0 180) (size 2.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 6 "Net-(C10-Pad1)") (pinfunction "K"))
    (pad "2" smd rect (at 2 0 180) (size 2.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "Net-(D1-Pad1)") (pinfunction "A"))
    (model "${KISYS3DMOD}/Diode_SMD.3dshapes/D_SMA.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (tedit 600AE68B)
    (at 109.73 26.19 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Field4" "Digikey")
    (property "Field5" "490-10505-1-ND")
    (property "Field6" "GRM21BC8YA106KE11L ")
    (property "Field7" "Murata")
    (property "Field8" "")
    (property "Part Description" "	10uF 10% or 20% 35V Ceramic Capacitor X6S 0805 (2012 Metric)")
    (property "Sheet file" "switch.kicad_sch")
    (property "Sheet name" "switch")
    (attr smd)
    (fp_text reference "C14" (at 0 -1.68 90) (layer "F.SilkS"))
    (fp_text value "100n" (at 0 1.68 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.95 0 90) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25))
    (pad "2" smd roundrect (at 0.95 0 90) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 14 "Net-(D8-Pad1)"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "CM4IO:5557_connector" (layer "F.Cu")
    (tedit 600EAE8C)
    (at 139.18 29.67 90)
    (property "Sheet file" "switch.kicad_sch")
    (property "Sheet name" "switch")
    (fp_text reference "J2" (at -25.6 0) (layer "B.SilkS"))
    (fp_text value "Conn_02x12_Top_Bottom" (at 0 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at -14.7 2.1 90) (size 2 2) (drill 1.15) (layers *.Cu *.Mask)
      (net 16 "Net-(J2-Pad13)") (pinfunction "Pin_3"))
    (pad "1" thru_hole circle (at -23.1 2.1 90) (size 2 2) (drill 1.15) (layers *.Cu *.Mask)
      (net 16 "Net-(J2-Pad13)") (pinfunction "Pin_1"))
    (pad "1" thru_hole circle (at -10.5 2.1) (size 2 2) (drill 1.15) (layers *.Cu *.Mask)
      (net 16 "Net-(J2-Pad13)") (pinfunction "Pin_4"))
    (pad "1" thru_hole circle (at -18.9 2.1 90) (size 2 2) (drill 1.15) (layers *.Cu *.Mask)
      (net 16 "Net-(J2-Pad13)") (pinfunction "Pin_2"))
    (pad "2" thru_hole circle (at -10.5 -2.1 90) (size 2 2) (drill 1.15) (layers *.Cu *.Mask)
      (net 15 "Net-(J2-Pad14)") (pinfunction "Pin_16"))
    (pad "2" thru_hole circle (at -18.9 -2.1 90) (size 2 2) (drill 1.15) (layers *.Cu *.Mask)
      (net 15 "Net-(J2-Pad14)") (pinfunction "Pin_14"))
    (pad "2" thru_hole circle (at -14.7 -2.1 90) (size 2 2) (drill 1.15) (layers *.Cu *.Mask)
      (net 15 "Net-(J2-Pad14)") (pinfunction "Pin_15"))
    (pad "2" thru_hole circle (at -23.1 -2.1 90) (size 2 2) (drill 1.15) (layers *.Cu *.Mask)
      (net 15 "Net-(J2-Pad14)") (pinfunction "Pin_13"))
  )
  (footprint "Connector_PinSocket_2.54mm:PinSocket_2x06_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 5A19A42B)
    (at 137.42 82.41 180)
    (descr "Through hole straight socket strip, 2x06, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 2x06 2.54mm double row")
    (property "Sheet file" "cluster4.kicad_sch")
    (property "Sheet name" "")
    (attr through_hole)
    (fp_text reference "J9" (at -0.05 15.67) (layer "F.SilkS"))
    (fp_text value "Conn_01x11_Female" (at -1.27 15.47) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at -1.27 6.35 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 "/+12v") (pinfunction "Pin_1"))
    (pad "2" thru_hole oval (at -2.54 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "/+5v") (pinfunction "Pin_2"))
    (pad "3" thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_3"))
    (pad "4" thru_hole oval (at -2.54 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 72 "/P7_AP") (pinfunction "Pin_4"))
    (pad "5" thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 71 "/P7_AN") (pinfunction "Pin_5"))
    (pad "6" thru_hole oval (at -2.54 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 70 "/P7_BP") (pinfunction "Pin_6"))
    (pad "7" thru_hole oval (at 0 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 69 "/P7_BN") (pinfunction "Pin_7"))
    (pad "8" thru_hole oval (at -2.54 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 68 "/P7_CP") (pinfunction "Pin_8"))
    (pad "9" thru_hole oval (at 0 10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 67 "/P7_CN") (pinfunction "Pin_9"))
    (pad "10" thru_hole oval (at -2.54 10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 66 "/P7_DP") (pinfunction "Pin_10"))
    (pad "11" thru_hole oval (at 0 12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 65 "/P7_DN") (pinfunction "Pin_11"))
    (pad "12" thru_hole oval (at -2.54 12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model "${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_2x06_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_SO:SOIC-8_5.23x5.23mm_P1.27mm" (layer "F.Cu")
    (tedit 5D9F72B1)
    (at 77.33 40.16 90)
    (descr "SOIC, 8 Pin (http://www.winbond.com/resource-files/w25q32jv%20revg%2003272018%20plus.pdf#page=68), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (property "Sheet file" "switch.kicad_sch")
    (property "Sheet name" "switch")
    (attr smd)
    (fp_text reference "U8" (at 0 -3.56 90) (layer "F.SilkS"))
    (fp_text value "W25Q128JVS" (at -4.78 3.19 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -3.6 -1.905 90) (size 1.6 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 111 "/switch/SPI_CS") (pinfunction "~CS"))
    (pad "2" smd roundrect (at -3.6 -0.635 90) (size 1.6 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 112 "/switch/SPI_D0") (pinfunction "DO(IO1)"))
    (pad "3" smd roundrect (at -3.6 0.635 90) (size 1.6 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 86 "Net-(R33-Pad1)") (pinfunction "IO2"))
    (pad "4" smd roundrect (at -3.6 1.905 90) (size 1.6 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "GND"))
    (pad "5" smd roundrect (at 3.6 1.905 90) (size 1.6 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 113 "/switch/SPI_D1") (pinfunction "DI(IO0)"))
    (pad "6" smd roundrect (at 3.6 0.635 90) (size 1.6 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 114 "/switch/SPI_CLK") (pinfunction "CLK"))
    (pad "7" smd roundrect (at 3.6 -0.635 90) (size 1.6 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 87 "Net-(R34-Pad1)") (pinfunction "IO3"))
    (pad "8" smd roundrect (at 3.6 -1.905 90) (size 1.6 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 82 "<NO NET>") (pinfunction "VCC"))
    (model "${KISYS3DMOD}/Package_SO.3dshapes/SOIC-8_5.23x5.23mm_P1.27mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 75.03 62.71 -90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheet file" "switch.kicad_sch")
    (property "Sheet name" "switch")
    (attr smd)
    (fp_text reference "C45" (at 0.12 -2.25 90) (layer "F.SilkS"))
    (fp_text value "0.1uf" (at 0 1.16 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.48 0 270) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 83 "/switch/+1v"))
    (pad "2" smd roundrect (at 0.48 0 270) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 68.76 66.07 -90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheet file" "switch.kicad_sch")
    (property "Sheet name" "switch")
    (attr smd)
    (fp_text reference "C43" (at 0 -1.16 -90) (layer "F.SilkS"))
    (fp_text value "0.1uf" (at 0 1.16 -90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 -90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.48 0 270) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 83 "/switch/+1v"))
    (pad "2" smd roundrect (at 0.48 0 270) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 25.38 22.65) (end 145.38 22.65) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 145.38 22.65) (end 145.38 84.65) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 25.38 84.65) (end 25.38 22.65) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 145.38 84.65) (end 25.38 84.65) (layer "Edge.Cuts") (width 0.1))
  (dimension (type aligned) (layer "User.1")
    (pts (xy 42.52 75.8) (xy 54.66 75.8))
    (height -1.15)
    (gr_text "12.1400 mm" (at 48.59 73.5) (layer "User.1"))
    (format (units 3) (units_format 1) (precision 4))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (zone (net 1) (net_name "GND") (layer "F.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 145.37 84.64)
        (xy 25.39 84.65)
        (xy 25.39 22.66)
        (xy 145.38 22.66)
      )
    )
  )
  (zone (net 1) (net_name "GND") (layer "B.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 145.38 84.65)
        (xy 25.39 84.64)
        (xy 25.39 22.66)
        (xy 145.37 22.66)
      )
    )
  )
)
