(kicad_symbol_lib (version 20201005) (generator kicad_symbol_editor)
  (symbol "cluster_cm4:RTL8370N" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at 0 -2.54 0))
    (property "Value" "RTL8370N" (id 1) (at 0 2.54 0))
    (property "Footprint" "cm4_cluster:RTL8370" (id 2) (at 0 0 0))
    (property "Datasheet" "DOCUMENTATION" (id 3) (at 0 0 0))
    (symbol "RTL8370N_1_0")
    (symbol "RTL8370N_1_1"
      (pin bidirectional line (at -19.05 161.29 0) (length 7.62)
        (name "P2MDICP")
        (number "1")
      )
      (pin bidirectional line (at -19.05 158.75 0) (length 7.62)
        (name "P2MDICN")
        (number "2")
      )
      (pin bidirectional line (at -19.05 156.21 0) (length 7.62)
        (name "P2MDIDP")
        (number "3")
      )
      (pin bidirectional line (at -19.05 153.67 0) (length 7.62)
        (name "P2MDIDN")
        (number "4")
      )
      (pin bidirectional line (at -19.05 151.13 0) (length 7.62)
        (name "AVDDH")
        (number "5")
      )
      (pin bidirectional line (at -19.05 148.59 0) (length 7.62)
        (name "P3MDIAP")
        (number "6")
      )
      (pin bidirectional line (at -19.05 146.05 0) (length 7.62)
        (name "P3MDIAN")
        (number "7")
      )
      (pin bidirectional line (at -19.05 143.51 0) (length 7.62)
        (name "P3MDIBP")
        (number "8")
      )
      (pin bidirectional line (at -19.05 140.97 0) (length 7.62)
        (name "P3MDIBN")
        (number "9")
      )
      (pin bidirectional line (at -19.05 138.43 0) (length 7.62)
        (name "AVDDL")
        (number "10")
      )
      (pin bidirectional line (at -19.05 135.89 0) (length 7.62)
        (name "P3MDICP")
        (number "11")
      )
      (pin bidirectional line (at -19.05 133.35 0) (length 7.62)
        (name "P3MDICN")
        (number "12")
      )
      (pin bidirectional line (at -19.05 130.81 0) (length 7.62)
        (name "P3MDIDP")
        (number "13")
      )
      (pin bidirectional line (at -19.05 128.27 0) (length 7.62)
        (name "P3MDIDN")
        (number "14")
      )
      (pin bidirectional line (at -19.05 125.73 0) (length 7.62)
        (name "AVDDH")
        (number "15")
      )
      (pin bidirectional line (at -19.05 123.19 0) (length 7.62)
        (name "AGND")
        (number "16")
      )
      (pin bidirectional line (at -19.05 120.65 0) (length 7.62)
        (name "MDIREF")
        (number "17")
      )
      (pin bidirectional line (at -19.05 118.11 0) (length 7.62)
        (name "AVDDL")
        (number "18")
      )
      (pin bidirectional line (at -19.05 115.57 0) (length 7.62)
        (name "AVDDH")
        (number "19")
      )
      (pin bidirectional line (at -19.05 113.03 0) (length 7.62)
        (name "DVDDL")
        (number "20")
      )
      (pin bidirectional line (at -19.05 110.49 0) (length 7.62)
        (name "DVDDL")
        (number "21")
      )
      (pin bidirectional line (at -19.05 107.95 0) (length 7.62)
        (name "DVDDL")
        (number "22")
      )
      (pin bidirectional line (at -19.05 105.41 0) (length 7.62)
        (name "DVDDL")
        (number "23")
      )
      (pin bidirectional line (at -19.05 102.87 0) (length 7.62)
        (name "AVDDH")
        (number "24")
      )
      (pin bidirectional line (at -19.05 100.33 0) (length 7.62)
        (name "P4MDIAP")
        (number "25")
      )
      (pin bidirectional line (at -19.05 97.79 0) (length 7.62)
        (name "P4MDIAN")
        (number "26")
      )
      (pin bidirectional line (at -19.05 95.25 0) (length 7.62)
        (name "P4MDIBP")
        (number "27")
      )
      (pin bidirectional line (at -19.05 92.71 0) (length 7.62)
        (name "P4MDIBN")
        (number "28")
      )
      (pin bidirectional line (at -19.05 90.17 0) (length 7.62)
        (name "AVDDL")
        (number "29")
      )
      (pin bidirectional line (at -19.05 87.63 0) (length 7.62)
        (name "P4MDICP")
        (number "30")
      )
      (pin bidirectional line (at -19.05 85.09 0) (length 7.62)
        (name "P4MDICN")
        (number "31")
      )
      (pin bidirectional line (at -19.05 82.55 0) (length 7.62)
        (name "P4MDIDP")
        (number "32")
      )
      (pin bidirectional line (at -19.05 80.01 0) (length 7.62)
        (name "P4MDIDN")
        (number "33")
      )
      (pin bidirectional line (at -19.05 77.47 0) (length 7.62)
        (name "AVDDH")
        (number "34")
      )
      (pin bidirectional line (at -19.05 74.93 0) (length 7.62)
        (name "P5MDIAP")
        (number "35")
      )
      (pin bidirectional line (at -19.05 72.39 0) (length 7.62)
        (name "P5MDIAN")
        (number "36")
      )
      (pin bidirectional line (at -19.05 69.85 0) (length 7.62)
        (name "P5MDIBP")
        (number "37")
      )
      (pin bidirectional line (at -19.05 67.31 0) (length 7.62)
        (name "P5MDIBN")
        (number "38")
      )
      (pin bidirectional line (at -19.05 64.77 0) (length 7.62)
        (name "AVDDL")
        (number "39")
      )
      (pin bidirectional line (at -19.05 62.23 0) (length 7.62)
        (name "P5MDICP")
        (number "40")
      )
      (pin bidirectional line (at -19.05 59.69 0) (length 7.62)
        (name "P5MDICN")
        (number "41")
      )
      (pin bidirectional line (at -19.05 57.15 0) (length 7.62)
        (name "P5MDIDP")
        (number "42")
      )
      (pin bidirectional line (at -19.05 54.61 0) (length 7.62)
        (name "P5MDIDN")
        (number "43")
      )
      (pin bidirectional line (at -19.05 52.07 0) (length 7.62)
        (name "PLLVDDL1")
        (number "44")
      )
      (pin bidirectional line (at -19.05 49.53 0) (length 7.62)
        (name "P6MDIAP")
        (number "45")
      )
      (pin bidirectional line (at -19.05 46.99 0) (length 7.62)
        (name "P6MDIAN")
        (number "46")
      )
      (pin bidirectional line (at -19.05 44.45 0) (length 7.62)
        (name "P6MDIBP")
        (number "47")
      )
      (pin bidirectional line (at -19.05 41.91 0) (length 7.62)
        (name "P6MDIBN")
        (number "48")
      )
      (pin bidirectional line (at -19.05 39.37 0) (length 7.62)
        (name "AVDDL")
        (number "49")
      )
      (pin bidirectional line (at -19.05 36.83 0) (length 7.62)
        (name "P6MDICP")
        (number "50")
      )
      (pin bidirectional line (at -19.05 34.29 0) (length 7.62)
        (name "P6MDICN")
        (number "51")
      )
      (pin bidirectional line (at -19.05 31.75 0) (length 7.62)
        (name "P6MDIDP")
        (number "52")
      )
      (pin bidirectional line (at -19.05 29.21 0) (length 7.62)
        (name "P6MDIDN")
        (number "53")
      )
      (pin bidirectional line (at -19.05 26.67 0) (length 7.62)
        (name "AVDDH")
        (number "54")
      )
      (pin bidirectional line (at -19.05 24.13 0) (length 7.62)
        (name "P7MDIAP")
        (number "55")
      )
      (pin bidirectional line (at -19.05 21.59 0) (length 7.62)
        (name "P7MDIAN")
        (number "56")
      )
      (pin bidirectional line (at -19.05 19.05 0) (length 7.62)
        (name "P7MDIBP")
        (number "57")
      )
      (pin bidirectional line (at -19.05 16.51 0) (length 7.62)
        (name "P7MDIBN")
        (number "58")
      )
      (pin bidirectional line (at -19.05 13.97 0) (length 7.62)
        (name "AVDDL")
        (number "59")
      )
      (pin bidirectional line (at -19.05 11.43 0) (length 7.62)
        (name "P7MDICP")
        (number "60")
      )
      (pin bidirectional line (at -19.05 8.89 0) (length 7.62)
        (name "P7MDICN")
        (number "61")
      )
      (pin bidirectional line (at -19.05 6.35 0) (length 7.62)
        (name "P7MDIDP")
        (number "62")
      )
      (pin bidirectional line (at -19.05 3.81 0) (length 7.62)
        (name "P7MDIDN")
        (number "63")
      )
      (pin bidirectional line (at -19.05 1.27 0) (length 7.62)
        (name "AVDDH")
        (number "64")
      )
      (pin unconnected line (at 19.05 161.29 180) (length 7.62)
        (name "RESERVED")
        (number "65")
      )
      (pin unconnected line (at 19.05 158.75 180) (length 7.62)
        (name "RESERVED")
        (number "66")
      )
      (pin bidirectional line (at 19.05 156.21 180) (length 7.62)
        (name "P7LED2")
        (number "67")
      )
      (pin bidirectional line (at 19.05 153.67 180) (length 7.62)
        (name "P7LED0")
        (number "68")
      )
      (pin bidirectional line (at 19.05 151.13 180) (length 7.62)
        (name "P7LED1")
        (number "69")
      )
      (pin bidirectional line (at 19.05 148.59 180) (length 7.62)
        (name "P6LED2")
        (number "70")
      )
      (pin bidirectional line (at 19.05 146.05 180) (length 7.62)
        (name "P6LED0")
        (number "71")
      )
      (pin bidirectional line (at 19.05 143.51 180) (length 7.62)
        (name "P6LED1")
        (number "72")
      )
      (pin bidirectional line (at 19.05 140.97 180) (length 7.62)
        (name "P5LED2")
        (number "73")
      )
      (pin bidirectional line (at 19.05 138.43 180) (length 7.62)
        (name "P5LED0")
        (number "74")
      )
      (pin bidirectional line (at 19.05 135.89 180) (length 7.62)
        (name "P5LED1")
        (number "75")
      )
      (pin bidirectional line (at 19.05 133.35 180) (length 7.62)
        (name "DVDDL")
        (number "76")
      )
      (pin bidirectional line (at 19.05 130.81 180) (length 7.62)
        (name "DVDDIO")
        (number "77")
      )
      (pin bidirectional line (at 19.05 128.27 180) (length 7.62)
        (name "DVDDL")
        (number "78")
      )
      (pin bidirectional line (at 19.05 125.73 180) (length 7.62)
        (name "P4LED2")
        (number "79")
      )
      (pin bidirectional line (at 19.05 123.19 180) (length 7.62)
        (name "P4LED0")
        (number "80")
      )
      (pin bidirectional line (at 19.05 120.65 180) (length 7.62)
        (name "P4LED1")
        (number "81")
      )
      (pin bidirectional line (at 19.05 118.11 180) (length 7.62)
        (name "P3LED1")
        (number "82")
      )
      (pin bidirectional line (at 19.05 115.57 180) (length 7.62)
        (name "P3LED2")
        (number "83")
      )
      (pin bidirectional line (at 19.05 113.03 180) (length 7.62)
        (name "P3LED0")
        (number "84")
      )
      (pin bidirectional line (at 19.05 110.49 180) (length 7.62)
        (name "P2LED2")
        (number "85")
      )
      (pin bidirectional line (at 19.05 107.95 180) (length 7.62)
        (name "P2LED0")
        (number "86")
      )
      (pin bidirectional line (at 19.05 105.41 180) (length 7.62)
        (name "P2LED1")
        (number "87")
      )
      (pin bidirectional line (at 19.05 102.87 180) (length 7.62)
        (name "P1LED2")
        (number "88")
      )
      (pin bidirectional line (at 19.05 100.33 180) (length 7.62)
        (name "P1LED0")
        (number "89")
      )
      (pin bidirectional line (at 19.05 97.79 180) (length 7.62)
        (name "P1LED1")
        (number "90")
      )
      (pin bidirectional line (at 19.05 95.25 180) (length 7.62)
        (name "P0LED2")
        (number "91")
      )
      (pin bidirectional line (at 19.05 92.71 180) (length 7.62)
        (name "DVDDL")
        (number "92")
      )
      (pin bidirectional line (at 19.05 90.17 180) (length 7.62)
        (name "P0LED1")
        (number "93")
      )
      (pin bidirectional line (at 19.05 87.63 180) (length 7.62)
        (name "P0LED0")
        (number "94")
      )
      (pin bidirectional line (at 19.05 85.09 180) (length 7.62)
        (name "DVDDL")
        (number "95")
      )
      (pin bidirectional line (at 19.05 82.55 180) (length 7.62)
        (name "AVDDH")
        (number "96")
      )
      (pin bidirectional line (at 19.05 80.01 180) (length 7.62)
        (name "XTAL0")
        (number "97")
      )
      (pin bidirectional line (at 19.05 77.47 180) (length 7.62)
        (name "XTAL1")
        (number "98")
      )
      (pin bidirectional line (at 19.05 74.93 180) (length 7.62)
        (name "nRESET")
        (number "99")
      )
      (pin bidirectional line (at 19.05 72.39 180) (length 7.62)
        (name "SCK/MDC")
        (number "100")
      )
      (pin bidirectional line (at 19.05 69.85 180) (length 7.62)
        (name "SDA/MDIO")
        (number "101")
      )
      (pin bidirectional line (at 19.05 67.31 180) (length 7.62)
        (name "AVDDH")
        (number "102")
      )
      (pin bidirectional line (at 19.05 64.77 180) (length 7.62)
        (name "P0MDIAP")
        (number "103")
      )
      (pin bidirectional line (at 19.05 62.23 180) (length 7.62)
        (name "P0MDIAN")
        (number "104")
      )
      (pin bidirectional line (at 19.05 59.69 180) (length 7.62)
        (name "P0MDIBP")
        (number "105")
      )
      (pin bidirectional line (at 19.05 57.15 180) (length 7.62)
        (name "P0MDIBN")
        (number "106")
      )
      (pin bidirectional line (at 19.05 54.61 180) (length 7.62)
        (name "AVDDL")
        (number "107")
      )
      (pin bidirectional line (at 19.05 52.07 180) (length 7.62)
        (name "P0MDICP")
        (number "108")
      )
      (pin bidirectional line (at 19.05 49.53 180) (length 7.62)
        (name "P0MDICN")
        (number "109")
      )
      (pin bidirectional line (at 19.05 46.99 180) (length 7.62)
        (name "P0MDIDP")
        (number "110")
      )
      (pin bidirectional line (at 19.05 44.45 180) (length 7.62)
        (name "P0MDIDN")
        (number "111")
      )
      (pin bidirectional line (at 19.05 41.91 180) (length 7.62)
        (name "AVDDH")
        (number "112")
      )
      (pin bidirectional line (at 19.05 39.37 180) (length 7.62)
        (name "P1MDIAP")
        (number "113")
      )
      (pin bidirectional line (at 19.05 36.83 180) (length 7.62)
        (name "P1MDIAN")
        (number "114")
      )
      (pin bidirectional line (at 19.05 34.29 180) (length 7.62)
        (name "P1MDIBP")
        (number "115")
      )
      (pin bidirectional line (at 19.05 31.75 180) (length 7.62)
        (name "P1MDIBN")
        (number "116")
      )
      (pin bidirectional line (at 19.05 29.21 180) (length 7.62)
        (name "AVDDL")
        (number "117")
      )
      (pin bidirectional line (at 19.05 26.67 180) (length 7.62)
        (name "P1MDICP")
        (number "118")
      )
      (pin bidirectional line (at 19.05 24.13 180) (length 7.62)
        (name "P1MDICN")
        (number "119")
      )
      (pin bidirectional line (at 19.05 21.59 180) (length 7.62)
        (name "P1MDIDP")
        (number "120")
      )
      (pin bidirectional line (at 19.05 19.05 180) (length 7.62)
        (name "P1MDIDN")
        (number "121")
      )
      (pin bidirectional line (at 19.05 16.51 180) (length 7.62)
        (name "PLLVDDL0")
        (number "122")
      )
      (pin bidirectional line (at 19.05 13.97 180) (length 7.62)
        (name "ATESTCK0")
        (number "123")
      )
      (pin bidirectional line (at 19.05 11.43 180) (length 7.62)
        (name "P2MDIAP")
        (number "124")
      )
      (pin bidirectional line (at 19.05 8.89 180) (length 7.62)
        (name "P2MDIAN")
        (number "125")
      )
      (pin bidirectional line (at 19.05 6.35 180) (length 7.62)
        (name "P2MDIBP")
        (number "126")
      )
      (pin bidirectional line (at 19.05 3.81 180) (length 7.62)
        (name "P2MDIBN")
        (number "127")
      )
      (pin bidirectional line (at 19.05 1.27 180) (length 7.62)
        (name "AVDDL")
        (number "128")
      )
    )
  )
)
