(kicad_pcb (version 4) (host pcbnew 4.0.4-stable)
  (general
    (links 90)
    (no_connects 1)
    (area 141.935999 64.211999 227.409 132.003001)
    (thickness 1.6)
    (drawings 8)
    (tracks 374)
    (zones 0)
    (modules 23)
    (nets 64)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.4)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only yes)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.0254)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.5 1.5)
    (pad_drill 0.6)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 VCC)
  (net 3 "Net-(P1-Pad2)")
  (net 4 +3V3)
  (net 5 "Net-(P1-Pad4)")
  (net 6 "Net-(P1-Pad6)")
  (net 7 "Net-(P1-Pad7)")
  (net 8 "Net-(P2-Pad2)")
  (net 9 "Net-(P2-Pad3)")
  (net 10 "Net-(R1-Pad1)")
  (net 11 "Net-(R2-Pad1)")
  (net 12 "Net-(R3-Pad1)")
  (net 13 "Net-(R3-Pad2)")
  (net 14 "Net-(R4-Pad1)")
  (net 15 "Net-(R4-Pad2)")
  (net 16 "Net-(R5-Pad1)")
  (net 17 "Net-(R5-Pad2)")
  (net 18 "Net-(R6-Pad1)")
  (net 19 "Net-(R6-Pad2)")
  (net 20 "Net-(R7-Pad1)")
  (net 21 "Net-(R7-Pad2)")
  (net 22 "Net-(R8-Pad1)")
  (net 23 "Net-(R9-Pad1)")
  (net 24 "Net-(R11-Pad1)")
  (net 25 "Net-(R12-Pad1)")
  (net 26 "Net-(R13-Pad2)")
  (net 27 "Net-(U1-Pad1)")
  (net 28 "Net-(U1-Pad2)")
  (net 29 "Net-(U1-Pad3)")
  (net 30 "Net-(U1-Pad4)")
  (net 31 "Net-(U1-Pad5)")
  (net 32 "Net-(U1-Pad6)")
  (net 33 "Net-(U1-Pad7)")
  (net 34 "Net-(U1-Pad8)")
  (net 35 "Net-(U1-Pad10)")
  (net 36 "Net-(U1-Pad11)")
  (net 37 "Net-(U1-Pad12)")
  (net 38 "Net-(U1-Pad13)")
  (net 39 "Net-(U1-Pad14)")
  (net 40 "Net-(U1-Pad15)")
  (net 41 "Net-(U1-Pad16)")
  (net 42 "Net-(U1-Pad17)")
  (net 43 "Net-(U2-Pad1)")
  (net 44 "Net-(U2-Pad2)")
  (net 45 "Net-(U2-Pad3)")
  (net 46 "Net-(U2-Pad4)")
  (net 47 "Net-(U2-Pad5)")
  (net 48 "Net-(U2-Pad6)")
  (net 49 "Net-(U2-Pad7)")
  (net 50 "Net-(U2-Pad8)")
  (net 51 "Net-(U2-Pad10)")
  (net 52 "Net-(U2-Pad11)")
  (net 53 "Net-(U2-Pad12)")
  (net 54 "Net-(U2-Pad13)")
  (net 55 "Net-(U2-Pad14)")
  (net 56 "Net-(U2-Pad15)")
  (net 57 "Net-(U2-Pad16)")
  (net 58 "Net-(U2-Pad17)")
  (net 59 "Net-(U3-Pad1)")
  (net 60 "Net-(U3-Pad17)")
  (net 61 "Net-(U3-Pad19)")
  (net 62 "Net-(U4-Pad16)")
  (net 63 "Net-(U4-Pad19)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net GND)
    (add_net "Net-(P1-Pad2)")
    (add_net "Net-(P1-Pad4)")
    (add_net "Net-(P1-Pad6)")
    (add_net "Net-(P1-Pad7)")
    (add_net "Net-(P2-Pad2)")
    (add_net "Net-(P2-Pad3)")
    (add_net "Net-(R1-Pad1)")
    (add_net "Net-(R11-Pad1)")
    (add_net "Net-(R12-Pad1)")
    (add_net "Net-(R13-Pad2)")
    (add_net "Net-(R2-Pad1)")
    (add_net "Net-(R3-Pad1)")
    (add_net "Net-(R3-Pad2)")
    (add_net "Net-(R4-Pad1)")
    (add_net "Net-(R4-Pad2)")
    (add_net "Net-(R5-Pad1)")
    (add_net "Net-(R5-Pad2)")
    (add_net "Net-(R6-Pad1)")
    (add_net "Net-(R6-Pad2)")
    (add_net "Net-(R7-Pad1)")
    (add_net "Net-(R7-Pad2)")
    (add_net "Net-(R8-Pad1)")
    (add_net "Net-(R9-Pad1)")
    (add_net "Net-(U1-Pad1)")
    (add_net "Net-(U1-Pad10)")
    (add_net "Net-(U1-Pad11)")
    (add_net "Net-(U1-Pad12)")
    (add_net "Net-(U1-Pad13)")
    (add_net "Net-(U1-Pad14)")
    (add_net "Net-(U1-Pad15)")
    (add_net "Net-(U1-Pad16)")
    (add_net "Net-(U1-Pad17)")
    (add_net "Net-(U1-Pad2)")
    (add_net "Net-(U1-Pad3)")
    (add_net "Net-(U1-Pad4)")
    (add_net "Net-(U1-Pad5)")
    (add_net "Net-(U1-Pad6)")
    (add_net "Net-(U1-Pad7)")
    (add_net "Net-(U1-Pad8)")
    (add_net "Net-(U2-Pad1)")
    (add_net "Net-(U2-Pad10)")
    (add_net "Net-(U2-Pad11)")
    (add_net "Net-(U2-Pad12)")
    (add_net "Net-(U2-Pad13)")
    (add_net "Net-(U2-Pad14)")
    (add_net "Net-(U2-Pad15)")
    (add_net "Net-(U2-Pad16)")
    (add_net "Net-(U2-Pad17)")
    (add_net "Net-(U2-Pad2)")
    (add_net "Net-(U2-Pad3)")
    (add_net "Net-(U2-Pad4)")
    (add_net "Net-(U2-Pad5)")
    (add_net "Net-(U2-Pad6)")
    (add_net "Net-(U2-Pad7)")
    (add_net "Net-(U2-Pad8)")
    (add_net "Net-(U3-Pad1)")
    (add_net "Net-(U3-Pad17)")
    (add_net "Net-(U3-Pad19)")
    (add_net "Net-(U4-Pad16)")
    (add_net "Net-(U4-Pad19)")
    (add_net VCC)
  )
  (module Capacitors_ThroughHole:C_Radial_D6.3_L11.2_P2.5 (layer F.Cu) (tedit 0)
    (at 188.468 109.22)
    (descr "Radial Electrolytic Capacitor, Diameter 6.3mm x Length 11.2mm, Pitch 2.5mm")
    (tags "Electrolytic Capacitor")
    (fp_text reference C1 (at 1.25 -4.4) (layer F.SilkS))
    (fp_text value CP (at 1.25 4.4) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole rect (at 0 0) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 VCC))
    (model Capacitors_ThroughHole.3dshapes/C_Radial_D6.3_L11.2_P2.5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:C_Radial_D6.3_L11.2_P2.5 (layer F.Cu) (tedit 0)
    (at 188.468 71.628)
    (descr "Radial Electrolytic Capacitor, Diameter 6.3mm x Length 11.2mm, Pitch 2.5mm")
    (tags "Electrolytic Capacitor")
    (fp_text reference C2 (at 1.25 -4.4) (layer F.SilkS))
    (fp_text value CP (at 1.25 4.4) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole rect (at 0 0) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 +3V3))
    (model Capacitors_ThroughHole.3dshapes/C_Radial_D6.3_L11.2_P2.5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x04 (layer F.Cu) (tedit 0)
    (at 189.357 118.364)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P1 (at 0 -5.1) (layer F.SilkS))
    (fp_text value CONN_02X04 (at 0 -3.1) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 3 "Net-(P1-Pad2)"))
    (pad 3 thru_hole oval (at 0 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 4 +3V3))
    (pad 4 thru_hole oval (at 2.54 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 5 "Net-(P1-Pad4)"))
    (pad 5 thru_hole oval (at 0 5.08) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 6 thru_hole oval (at 2.54 5.08) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 6 "Net-(P1-Pad6)"))
    (pad 7 thru_hole oval (at 0 7.62) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 7 "Net-(P1-Pad7)"))
    (pad 8 thru_hole oval (at 2.54 7.62) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 4 +3V3))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x04.wrl
      (at (xyz 0.05 -0.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03 (layer F.Cu) (tedit 0)
    (at 221.234 119.38 270)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P2 (at 0 -5.1 270) (layer F.SilkS))
    (fp_text value CONN_01X03 (at 0 -3.1 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 8 "Net-(P2-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 9 "Net-(P2-Pad3)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x03.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Housings_DIP:DIP-18_W7.62mm_LongPads (layer F.Cu) (tedit 54130A77)
    (at 149.86 106.68)
    (descr "18-lead dip package, row spacing 7.62 mm (300 mils), longer pads")
    (tags "dil dip 2.54 300")
    (fp_text reference U1 (at 0 -5.22) (layer F.SilkS))
    (fp_text value 2114 (at 0 -3.72) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 0) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 27 "Net-(U1-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 28 "Net-(U1-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 29 "Net-(U1-Pad3)"))
    (pad 4 thru_hole oval (at 0 7.62) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 30 "Net-(U1-Pad4)"))
    (pad 5 thru_hole oval (at 0 10.16) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 31 "Net-(U1-Pad5)"))
    (pad 6 thru_hole oval (at 0 12.7) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 32 "Net-(U1-Pad6)"))
    (pad 7 thru_hole oval (at 0 15.24) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 33 "Net-(U1-Pad7)"))
    (pad 8 thru_hole oval (at 0 17.78) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 34 "Net-(U1-Pad8)"))
    (pad 9 thru_hole oval (at 0 20.32) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 10 thru_hole oval (at 7.62 20.32) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 35 "Net-(U1-Pad10)"))
    (pad 11 thru_hole oval (at 7.62 17.78) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 36 "Net-(U1-Pad11)"))
    (pad 12 thru_hole oval (at 7.62 15.24) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 37 "Net-(U1-Pad12)"))
    (pad 13 thru_hole oval (at 7.62 12.7) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 38 "Net-(U1-Pad13)"))
    (pad 14 thru_hole oval (at 7.62 10.16) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 39 "Net-(U1-Pad14)"))
    (pad 15 thru_hole oval (at 7.62 7.62) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 40 "Net-(U1-Pad15)"))
    (pad 16 thru_hole oval (at 7.62 5.08) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 41 "Net-(U1-Pad16)"))
    (pad 17 thru_hole oval (at 7.62 2.54) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 42 "Net-(U1-Pad17)"))
    (pad 18 thru_hole oval (at 7.62 0) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 VCC))
    (model Housings_DIP.3dshapes/DIP-18_W7.62mm_LongPads.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DIP:DIP-18_W7.62mm_LongPads (layer F.Cu) (tedit 54130A77)
    (at 172.72 106.68)
    (descr "18-lead dip package, row spacing 7.62 mm (300 mils), longer pads")
    (tags "dil dip 2.54 300")
    (fp_text reference U2 (at 0 -5.22) (layer F.SilkS))
    (fp_text value 2114 (at 0 -3.72) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 0) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 43 "Net-(U2-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 44 "Net-(U2-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 45 "Net-(U2-Pad3)"))
    (pad 4 thru_hole oval (at 0 7.62) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 46 "Net-(U2-Pad4)"))
    (pad 5 thru_hole oval (at 0 10.16) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 47 "Net-(U2-Pad5)"))
    (pad 6 thru_hole oval (at 0 12.7) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 48 "Net-(U2-Pad6)"))
    (pad 7 thru_hole oval (at 0 15.24) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 49 "Net-(U2-Pad7)"))
    (pad 8 thru_hole oval (at 0 17.78) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 50 "Net-(U2-Pad8)"))
    (pad 9 thru_hole oval (at 0 20.32) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 10 thru_hole oval (at 7.62 20.32) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 51 "Net-(U2-Pad10)"))
    (pad 11 thru_hole oval (at 7.62 17.78) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 52 "Net-(U2-Pad11)"))
    (pad 12 thru_hole oval (at 7.62 15.24) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 53 "Net-(U2-Pad12)"))
    (pad 13 thru_hole oval (at 7.62 12.7) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 54 "Net-(U2-Pad13)"))
    (pad 14 thru_hole oval (at 7.62 10.16) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 55 "Net-(U2-Pad14)"))
    (pad 15 thru_hole oval (at 7.62 7.62) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 56 "Net-(U2-Pad15)"))
    (pad 16 thru_hole oval (at 7.62 5.08) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 57 "Net-(U2-Pad16)"))
    (pad 17 thru_hole oval (at 7.62 2.54) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 58 "Net-(U2-Pad17)"))
    (pad 18 thru_hole oval (at 7.62 0) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 VCC))
    (model Housings_DIP.3dshapes/DIP-18_W7.62mm_LongPads.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DIP:DIP-20_W7.62mm_LongPads (layer F.Cu) (tedit 54130A77)
    (at 149.86 71.12)
    (descr "20-lead dip package, row spacing 7.62 mm (300 mils), longer pads")
    (tags "dil dip 2.54 300")
    (fp_text reference U3 (at 0 -5.22) (layer F.SilkS))
    (fp_text value GAL16V8 (at 0 -3.72) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 0) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 59 "Net-(U3-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 31 "Net-(U1-Pad5)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 32 "Net-(U1-Pad6)"))
    (pad 4 thru_hole oval (at 0 7.62) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 33 "Net-(U1-Pad7)"))
    (pad 5 thru_hole oval (at 0 10.16) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 30 "Net-(U1-Pad4)"))
    (pad 6 thru_hole oval (at 0 12.7) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 29 "Net-(U1-Pad3)"))
    (pad 7 thru_hole oval (at 0 15.24) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 28 "Net-(U1-Pad2)"))
    (pad 8 thru_hole oval (at 0 17.78) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 27 "Net-(U1-Pad1)"))
    (pad 9 thru_hole oval (at 0 20.32) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 42 "Net-(U1-Pad17)"))
    (pad 10 thru_hole oval (at 0 22.86) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 11 thru_hole oval (at 7.62 22.86) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 26 "Net-(R13-Pad2)"))
    (pad 12 thru_hole oval (at 7.62 20.32) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 41 "Net-(U1-Pad16)"))
    (pad 13 thru_hole oval (at 7.62 17.78) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 40 "Net-(U1-Pad15)"))
    (pad 14 thru_hole oval (at 7.62 15.24) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 59 "Net-(U3-Pad1)"))
    (pad 15 thru_hole oval (at 7.62 12.7) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 35 "Net-(U1-Pad10)"))
    (pad 16 thru_hole oval (at 7.62 10.16) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 34 "Net-(U1-Pad8)"))
    (pad 17 thru_hole oval (at 7.62 7.62) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 60 "Net-(U3-Pad17)"))
    (pad 18 thru_hole oval (at 7.62 5.08) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 "Net-(R3-Pad2)"))
    (pad 19 thru_hole oval (at 7.62 2.54) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 61 "Net-(U3-Pad19)"))
    (pad 20 thru_hole oval (at 7.62 0) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 VCC))
    (model Housings_DIP.3dshapes/DIP-20_W7.62mm_LongPads.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DIP:DIP-20_W7.62mm_LongPads (layer F.Cu) (tedit 54130A77)
    (at 172.72 71.12)
    (descr "20-lead dip package, row spacing 7.62 mm (300 mils), longer pads")
    (tags "dil dip 2.54 300")
    (fp_text reference U4 (at 0 -5.22) (layer F.SilkS))
    (fp_text value 74LS273 (at 0 -3.72) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 0) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 VCC))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 "Net-(R6-Pad1)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 39 "Net-(U1-Pad14)"))
    (pad 4 thru_hole oval (at 0 7.62) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 38 "Net-(U1-Pad13)"))
    (pad 5 thru_hole oval (at 0 10.16) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 "Net-(R7-Pad1)"))
    (pad 6 thru_hole oval (at 0 12.7) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 "Net-(R4-Pad2)"))
    (pad 7 thru_hole oval (at 0 15.24) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 37 "Net-(U1-Pad12)"))
    (pad 8 thru_hole oval (at 0 17.78) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 36 "Net-(U1-Pad11)"))
    (pad 9 thru_hole oval (at 0 20.32) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 "Net-(R5-Pad1)"))
    (pad 10 thru_hole oval (at 0 22.86) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 11 thru_hole oval (at 7.62 22.86) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 59 "Net-(U3-Pad1)"))
    (pad 12 thru_hole oval (at 7.62 20.32) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 "Net-(R9-Pad1)"))
    (pad 13 thru_hole oval (at 7.62 17.78) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 55 "Net-(U2-Pad14)"))
    (pad 14 thru_hole oval (at 7.62 15.24) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 54 "Net-(U2-Pad13)"))
    (pad 15 thru_hole oval (at 7.62 12.7) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 22 "Net-(R8-Pad1)"))
    (pad 16 thru_hole oval (at 7.62 10.16) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 62 "Net-(U4-Pad16)"))
    (pad 17 thru_hole oval (at 7.62 7.62) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 53 "Net-(U2-Pad12)"))
    (pad 18 thru_hole oval (at 7.62 5.08) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 52 "Net-(U2-Pad11)"))
    (pad 19 thru_hole oval (at 7.62 2.54) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 63 "Net-(U4-Pad19)"))
    (pad 20 thru_hole oval (at 7.62 0) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 VCC))
    (model Housings_DIP.3dshapes/DIP-20_W7.62mm_LongPads.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ESP8266:ESP-12-Carrier (layer F.Cu) (tedit 583FDCDC)
    (at 214.494 92.202 270)
    (descr "Module, ESP-8266, ESP-12, 16 pad, SMD")
    (tags "Module ESP-8266 ESP8266")
    (fp_text reference U5 (at -3.008 -2 270) (layer F.SilkS))
    (fp_text value ESP-12 (at 6.992 1 270) (layer F.Fab))
    (fp_text user "No Copper" (at 6.892 -5.4 270) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.5 1.1) (drill 0.65 (offset -0.7 0)) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(R1-Pad1)"))
    (pad 2 thru_hole oval (at 0 2 270) (size 2.5 1.1) (drill 0.65 (offset -0.7 0)) (layers *.Cu *.Mask F.SilkS)
      (net 24 "Net-(R11-Pad1)"))
    (pad 3 thru_hole oval (at 0 4 270) (size 2.5 1.1) (drill 0.65 (offset -0.7 0)) (layers *.Cu *.Mask F.SilkS)
      (net 25 "Net-(R12-Pad1)"))
    (pad 4 thru_hole oval (at 0 6 270) (size 2.5 1.1) (drill 0.65 (offset -0.7 0)) (layers *.Cu *.Mask F.SilkS)
      (net 11 "Net-(R2-Pad1)"))
    (pad 5 thru_hole oval (at 0 8 270) (size 2.5 1.1) (drill 0.65 (offset -0.7 0)) (layers *.Cu *.Mask F.SilkS)
      (net 12 "Net-(R3-Pad1)"))
    (pad 6 thru_hole oval (at 0 10 270) (size 2.5 1.1) (drill 0.65 (offset -0.7 0)) (layers *.Cu *.Mask F.SilkS)
      (net 14 "Net-(R4-Pad1)"))
    (pad 7 thru_hole oval (at 0 12 270) (size 2.5 1.1) (drill 0.65 (offset -0.7 0)) (layers *.Cu *.Mask F.SilkS)
      (net 17 "Net-(R5-Pad2)"))
    (pad 8 thru_hole oval (at 0 14 270) (size 2.5 1.1) (drill 0.65 (offset -0.7 0)) (layers *.Cu *.Mask F.SilkS)
      (net 4 +3V3))
    (pad 9 thru_hole oval (at 14 14 270) (size 2.5 1.1) (drill 0.65 (offset 0.7 0)) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 10 thru_hole oval (at 14 12 270) (size 2.5 1.1) (drill 0.65 (offset 0.6 0)) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(P1-Pad2)"))
    (pad 11 thru_hole oval (at 14 10 270) (size 2.5 1.1) (drill 0.65 (offset 0.7 0)) (layers *.Cu *.Mask F.SilkS)
      (net 5 "Net-(P1-Pad4)"))
    (pad 12 thru_hole oval (at 14 8 270) (size 2.5 1.1) (drill 0.65 (offset 0.7 0)) (layers *.Cu *.Mask F.SilkS)
      (net 6 "Net-(P1-Pad6)"))
    (pad 13 thru_hole oval (at 14 6 270) (size 2.5 1.1) (drill 0.65 (offset 0.7 0)) (layers *.Cu *.Mask F.SilkS)
      (net 21 "Net-(R7-Pad2)"))
    (pad 14 thru_hole oval (at 14 4 270) (size 2.5 1.1) (drill 0.65 (offset 0.7 0)) (layers *.Cu *.Mask F.SilkS)
      (net 19 "Net-(R6-Pad2)"))
    (pad 15 thru_hole oval (at 14 2 270) (size 2.5 1.1) (drill 0.65 (offset 0.7 0)) (layers *.Cu *.Mask F.SilkS)
      (net 9 "Net-(P2-Pad3)"))
    (pad 16 thru_hole oval (at 14 0 270) (size 2.5 1.1) (drill 0.65 (offset 0.7 0)) (layers *.Cu *.Mask F.SilkS)
      (net 8 "Net-(P2-Pad2)"))
    (pad 1 thru_hole circle (at -7.62 -1.27 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 10 "Net-(R1-Pad1)"))
    (pad 2 thru_hole circle (at -7.62 1.27 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 24 "Net-(R11-Pad1)"))
    (pad 3 thru_hole circle (at -7.62 3.81 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 25 "Net-(R12-Pad1)"))
    (pad 4 thru_hole circle (at -7.62 6.35 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 11 "Net-(R2-Pad1)"))
    (pad 5 thru_hole circle (at -7.62 8.89 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 12 "Net-(R3-Pad1)"))
    (pad 6 thru_hole circle (at -7.62 11.43 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 14 "Net-(R4-Pad1)"))
    (pad 7 thru_hole circle (at -7.62 13.97 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 17 "Net-(R5-Pad2)"))
    (pad 8 thru_hole circle (at -7.62 16.51 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 4 +3V3))
    (pad 9 thru_hole circle (at 20.32 16.51 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 10 thru_hole circle (at 20.32 13.97 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 3 "Net-(P1-Pad2)"))
    (pad 11 thru_hole circle (at 20.32 11.43 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 5 "Net-(P1-Pad4)"))
    (pad 12 thru_hole circle (at 20.32 8.89 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 6 "Net-(P1-Pad6)"))
    (pad 13 thru_hole circle (at 20.32 6.35 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 21 "Net-(R7-Pad2)"))
    (pad 14 thru_hole circle (at 20.32 3.81 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 19 "Net-(R6-Pad2)"))
    (pad 15 thru_hole circle (at 20.32 1.27 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 9 "Net-(P2-Pad3)"))
    (pad 16 thru_hole circle (at 20.32 -1.27 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 8 "Net-(P2-Pad2)"))
    (model ${ESPLIB}/ESP8266.3dshapes/ESP-12.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Justins:AMS1117-3.3v_2.54mmx22.86mm (layer F.Cu) (tedit 58409AE1)
    (at 189.484 91.44 90)
    (fp_text reference U6 (at 0.635 1.905 90) (layer F.SilkS))
    (fp_text value AMS1117-3.3v (at 0.635 -0.635 90) (layer F.Fab))
    (fp_text user Vout (at 8.89 -1.27 90) (layer F.SilkS))
    (fp_text user GND (at 8.89 1.27 90) (layer F.SilkS))
    (fp_text user GND (at -8.89 1.27 90) (layer F.SilkS))
    (fp_text user Vin (at -8.89 -1.27 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at -11.43 -1.27 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 2 VCC))
    (pad 2 thru_hole circle (at -11.43 1.27 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 3 thru_hole circle (at 11.43 -1.27 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 4 +3V3))
    (pad 4 thru_hole circle (at 11.43 1.27 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module Justins:Resistor_Horizontal_RM10mmx1mm (layer F.Cu) (tedit 58402C9C)
    (at 215.764 80.772 90)
    (descr "Resistor, Axial,  RM 10mm, 1/3W")
    (tags "Resistor Axial RM 10mm 1/3W")
    (fp_text reference R1 (at 5.08 0 90) (layer F.SilkS))
    (fp_text value R (at 7.366 -0.762 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.SilkS *.Mask)
      (net 10 "Net-(R1-Pad1)"))
    (pad 2 thru_hole circle (at 10.16 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.SilkS *.Mask)
      (net 4 +3V3))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Justins:Resistor_Horizontal_RM10mmx1mm (layer F.Cu) (tedit 58402C9C)
    (at 208.144 80.772 90)
    (descr "Resistor, Axial,  RM 10mm, 1/3W")
    (tags "Resistor Axial RM 10mm 1/3W")
    (fp_text reference R2 (at 5.08 0 90) (layer F.SilkS))
    (fp_text value R (at 7.366 -0.762 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.SilkS *.Mask)
      (net 11 "Net-(R2-Pad1)"))
    (pad 2 thru_hole circle (at 10.16 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.SilkS *.Mask)
      (net 4 +3V3))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Justins:Resistor_Horizontal_RM10mmx1mm (layer F.Cu) (tedit 58402C9C)
    (at 205.604 80.772 90)
    (descr "Resistor, Axial,  RM 10mm, 1/3W")
    (tags "Resistor Axial RM 10mm 1/3W")
    (fp_text reference R3 (at 5.08 0 90) (layer F.SilkS))
    (fp_text value R (at 7.366 -0.762 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.SilkS *.Mask)
      (net 12 "Net-(R3-Pad1)"))
    (pad 2 thru_hole circle (at 10.16 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.SilkS *.Mask)
      (net 13 "Net-(R3-Pad2)"))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Justins:Resistor_Horizontal_RM10mmx1mm (layer F.Cu) (tedit 58402C9C)
    (at 203.064 80.772 90)
    (descr "Resistor, Axial,  RM 10mm, 1/3W")
    (tags "Resistor Axial RM 10mm 1/3W")
    (fp_text reference R4 (at 5.08 0 90) (layer F.SilkS))
    (fp_text value R (at 7.366 -0.762 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.SilkS *.Mask)
      (net 14 "Net-(R4-Pad1)"))
    (pad 2 thru_hole circle (at 10.16 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.SilkS *.Mask)
      (net 15 "Net-(R4-Pad2)"))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Justins:Resistor_Horizontal_RM10mmx1mm (layer F.Cu) (tedit 58402C9C)
    (at 200.524 70.612 270)
    (descr "Resistor, Axial,  RM 10mm, 1/3W")
    (tags "Resistor Axial RM 10mm 1/3W")
    (fp_text reference R5 (at 5.08 0 270) (layer F.SilkS))
    (fp_text value R (at 7.366 -0.762 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.SilkS *.Mask)
      (net 16 "Net-(R5-Pad1)"))
    (pad 2 thru_hole circle (at 10.16 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.SilkS *.Mask)
      (net 17 "Net-(R5-Pad2)"))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Justins:Resistor_Horizontal_RM10mmx1mm (layer F.Cu) (tedit 58402C9C)
    (at 210.684 126.492 90)
    (descr "Resistor, Axial,  RM 10mm, 1/3W")
    (tags "Resistor Axial RM 10mm 1/3W")
    (fp_text reference R6 (at 5.08 0 90) (layer F.SilkS))
    (fp_text value R (at 7.366 -0.762 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.SilkS *.Mask)
      (net 18 "Net-(R6-Pad1)"))
    (pad 2 thru_hole circle (at 10.16 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.SilkS *.Mask)
      (net 19 "Net-(R6-Pad2)"))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Justins:Resistor_Horizontal_RM10mmx1mm (layer F.Cu) (tedit 58402C9C)
    (at 208.144 126.492 90)
    (descr "Resistor, Axial,  RM 10mm, 1/3W")
    (tags "Resistor Axial RM 10mm 1/3W")
    (fp_text reference R7 (at 5.08 0 90) (layer F.SilkS))
    (fp_text value R (at 7.366 -0.762 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.SilkS *.Mask)
      (net 20 "Net-(R7-Pad1)"))
    (pad 2 thru_hole circle (at 10.16 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.SilkS *.Mask)
      (net 21 "Net-(R7-Pad2)"))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Justins:Resistor_Horizontal_RM10mmx1mm (layer F.Cu) (tedit 58402C9C)
    (at 205.604 126.492 90)
    (descr "Resistor, Axial,  RM 10mm, 1/3W")
    (tags "Resistor Axial RM 10mm 1/3W")
    (fp_text reference R8 (at 5.08 0 90) (layer F.SilkS))
    (fp_text value R (at 7.366 -0.762 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.SilkS *.Mask)
      (net 22 "Net-(R8-Pad1)"))
    (pad 2 thru_hole circle (at 10.16 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.SilkS *.Mask)
      (net 6 "Net-(P1-Pad6)"))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Justins:Resistor_Horizontal_RM10mmx1mm (layer F.Cu) (tedit 58402C9C)
    (at 203.064 126.492 90)
    (descr "Resistor, Axial,  RM 10mm, 1/3W")
    (tags "Resistor Axial RM 10mm 1/3W")
    (fp_text reference R9 (at 5.08 0 90) (layer F.SilkS))
    (fp_text value R (at 7.366 -0.762 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.SilkS *.Mask)
      (net 23 "Net-(R9-Pad1)"))
    (pad 2 thru_hole circle (at 10.16 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.SilkS *.Mask)
      (net 5 "Net-(P1-Pad4)"))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Justins:Resistor_Horizontal_RM10mmx1mm (layer F.Cu) (tedit 58402C9C)
    (at 200.524 126.492 90)
    (descr "Resistor, Axial,  RM 10mm, 1/3W")
    (tags "Resistor Axial RM 10mm 1/3W")
    (fp_text reference R10 (at 5.08 0 90) (layer F.SilkS))
    (fp_text value R (at 7.366 -0.762 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.SilkS *.Mask)
      (net 7 "Net-(P1-Pad7)"))
    (pad 2 thru_hole circle (at 10.16 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.SilkS *.Mask)
      (net 3 "Net-(P1-Pad2)"))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Justins:Resistor_Horizontal_RM10mmx1mm (layer F.Cu) (tedit 58402C9C)
    (at 213.224 80.772 90)
    (descr "Resistor, Axial,  RM 10mm, 1/3W")
    (tags "Resistor Axial RM 10mm 1/3W")
    (fp_text reference R11 (at 5.08 0 90) (layer F.SilkS))
    (fp_text value R (at 7.366 -0.762 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.SilkS *.Mask)
      (net 24 "Net-(R11-Pad1)"))
    (pad 2 thru_hole circle (at 10.16 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.SilkS *.Mask)
      (net 1 GND))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Justins:Resistor_Horizontal_RM10mmx1mm (layer F.Cu) (tedit 58402C9C)
    (at 210.684 80.772 90)
    (descr "Resistor, Axial,  RM 10mm, 1/3W")
    (tags "Resistor Axial RM 10mm 1/3W")
    (fp_text reference R12 (at 5.08 0 90) (layer F.SilkS))
    (fp_text value R (at 7.366 -0.762 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.SilkS *.Mask)
      (net 25 "Net-(R12-Pad1)"))
    (pad 2 thru_hole circle (at 10.16 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.SilkS *.Mask)
      (net 4 +3V3))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Justins:Resistor_Horizontal_RM10mmx1mm (layer F.Cu) (tedit 58402C9C)
    (at 149.352 99.568)
    (descr "Resistor, Axial,  RM 10mm, 1/3W")
    (tags "Resistor Axial RM 10mm 1/3W")
    (fp_text reference R13 (at 5.08 0) (layer F.SilkS))
    (fp_text value R (at 7.366 -0.762) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.SilkS *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.SilkS *.Mask)
      (net 26 "Net-(R13-Pad2)"))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text GPIO0 (at 196.85 123.19) (layer F.SilkS))
  (gr_text GPIO2 (at 196.85 120.65) (layer F.SilkS))
  (gr_text GPIO15 (at 197.485 118.11) (layer F.SilkS))
  (gr_line (start 141.986 64.262) (end 142.113 64.262) (angle 90) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 141.986 131.953) (end 141.986 64.262) (angle 90) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 226.695 131.953) (end 141.986 131.953) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 226.695 64.262) (end 226.695 131.953) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 141.986 64.262) (end 226.695 64.262) (angle 90) (layer Edge.Cuts) (width 0.0254))
  (zone (net 2) (net_name VCC) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 224.79 130.81) (xy 143.51 130.81) (xy 143.51 66.04) (xy 224.79 66.04)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 224.79 130.81) (xy 143.51 130.81) (xy 143.51 66.04) (xy 224.79 66.04)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 226.06 109.22) (xy 196.85 109.22) (xy 196.85 88.9) (xy 226.06 88.9)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 226.06 109.22) (xy 196.85 109.22) (xy 196.85 88.9) (xy 226.06 88.9)
      )
    )
  )
)
