<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.0.1">
<drawing>
<board>
<plain>
<wire x1="-4.1275" y1="-4.1275" x2="101.2625" y2="-4.1275" width="0" layer="20"/>
<wire x1="101.2625" y1="-4.1275" x2="101.2625" y2="50.3555" width="0" layer="20"/>
<wire x1="101.2625" y1="50.3555" x2="-4.1275" y2="50.3555" width="0" layer="20"/>
<wire x1="-4.1275" y1="50.3555" x2="-4.1275" y2="-4.1275" width="0" layer="20"/>
<hole x="-1.438" y="-1.508" drill="3.1"/>
<hole x="98.511" y="-1.254" drill="3.1"/>
<hole x="98.511" y="47.768" drill="3.1"/>
<hole x="-1.438" y="47.768" drill="3.1"/>
<text>sjm4306</text>
<text>PDSP 16x4</text>
<text>042021</text>
<text>sjm4306</text>
<text>V</text>
<text>G</text>
<text>RST</text>
<text>OE</text>
<text>LAT</text>
<text>SCL</text>
<text>SDA</text>
<text>JLCJLCJLCJLC</text>
</plain>
<libraries>
<library name="sjm4306-custom">
<packages>
<package name="PDSP188X">
</package>
</packages>
</library>
<library name="74xx-us">
<description>&lt;b&gt;TTL Devices, 74xx Series with US Symbols&lt;/b&gt;&lt;p&gt;
Based on the following sources:
&lt;ul&gt;
&lt;li&gt;Texas Instruments &lt;i&gt;TTL Data Book&lt;/i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;Volume 1, 1996.
&lt;li&gt;TTL Data Book, Volume 2 , 1993
&lt;li&gt;National Seminconductor Databook 1990, ALS/LS Logic
&lt;li&gt;ttl 74er digital data dictionary, ECA Electronic + Acustic GmbH, ISBN 3-88109-032-0
&lt;li&gt;http://icmaster.com/ViewCompare.asp
&lt;/ul&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SO16">
<description>&lt;b&gt;Small Outline package&lt;/b&gt; 150 mil</description>
</package>
</packages>
</library>
<library name="sjm4306_LOGO">
<packages>
<package name="SJM4306_MEDIUM_NO_COPPER">
</package>
<package name="SJM4306_LOGO_LARGE">
</package>
<package name="SJM4306_LOGO_SMALL">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X07_LOCK">
<description>&lt;h3&gt;Plated Through Hole -7 Pin Locking Footprint&lt;/h3&gt;
Holes are offset 0.005" from center, locking pins in place during soldering.
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:7&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_07&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="M0805">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
MELF 0.10 W</description>
</package>
<package name="C0805">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="085CS_1AR">
<description>&lt;b&gt;Aluminum electrolytic capacitors&lt;/b&gt; reflow soldering&lt;p&gt;
SMD (Chip) Standard 085 CS&lt;p&gt;
http://www.bccomponents.com/</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U$1" library="sjm4306-custom" package="PDSP188X" value="PDSP188X"/>
<element name="U$2" library="sjm4306-custom" package="PDSP188X" value="PDSP188X"/>
<element name="IC1" library="74xx-us" package="SO16" value="74LS595D">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="0"/>
<attribute name="VALUE"/>
</element>
<element name="IC2" library="74xx-us" package="SO16" value="74LS595D">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="0"/>
<attribute name="VALUE"/>
</element>
<element name="U$18" library="sjm4306_LOGO" package="SJM4306_MEDIUM_NO_COPPER" value=""/>
<element name="U$19" library="sjm4306_LOGO" package="SJM4306_LOGO_LARGE" value=""/>
<element name="U$21" library="sjm4306_LOGO" package="SJM4306_LOGO_SMALL" value=""/>
<element name="U$3" library="sjm4306-custom" package="PDSP188X" value="PDSP188X"/>
<element name="U$4" library="sjm4306-custom" package="PDSP188X" value="PDSP188X"/>
<element name="U$5" library="sjm4306-custom" package="PDSP188X" value="PDSP188X"/>
<element name="U$6" library="sjm4306-custom" package="PDSP188X" value="PDSP188X"/>
<element name="U$7" library="sjm4306-custom" package="PDSP188X" value="PDSP188X"/>
<element name="U$8" library="sjm4306-custom" package="PDSP188X" value="PDSP188X"/>
<element name="IC3" library="74xx-us" package="SO16" value="74LS595D">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="0"/>
<attribute name="VALUE"/>
</element>
<element name="J1" library="SparkFun-Connectors" package="1X07_LOCK" value="">
<attribute name="VALUE"/>
</element>
<element name="R1" library="adafruit" package="M0805" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="adafruit" package="C0805" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="C2" library="adafruit" package="C0805" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="C3" library="adafruit" package="C0805" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="C4" library="adafruit" package="C0805" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="C5" library="adafruit" package="C0805" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="C6" library="adafruit" package="C0805" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="C7" library="adafruit" package="C0805" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="C8" library="adafruit" package="C0805" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="C9" library="adafruit" package="C0805" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="C10" library="adafruit" package="C0805" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="C11" library="adafruit" package="C0805" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="C12" library="adafruit" package="085CS_1AR" value="100uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="IC1" pad="8"/>
<contactref element="U$1" pad="P$15"/>
<contactref element="U$1" pad="P$13"/>
<contactref element="U$2" pad="P$15"/>
<contactref element="U$2" pad="P$13"/>
<contactref element="IC2" pad="8"/>
<contactref element="U$2" pad="P$8"/>
<contactref element="U$3" pad="P$8"/>
<contactref element="U$3" pad="P$13"/>
<contactref element="U$3" pad="P$15"/>
<contactref element="U$4" pad="P$8"/>
<contactref element="U$4" pad="P$13"/>
<contactref element="U$4" pad="P$15"/>
<contactref element="U$5" pad="P$8"/>
<contactref element="U$5" pad="P$13"/>
<contactref element="U$5" pad="P$15"/>
<contactref element="U$6" pad="P$8"/>
<contactref element="U$6" pad="P$13"/>
<contactref element="U$6" pad="P$15"/>
<contactref element="U$7" pad="P$8"/>
<contactref element="U$7" pad="P$13"/>
<contactref element="U$7" pad="P$15"/>
<contactref element="U$8" pad="P$8"/>
<contactref element="U$8" pad="P$13"/>
<contactref element="U$8" pad="P$15"/>
<contactref element="IC3" pad="8"/>
<contactref element="J1" pad="2"/>
<contactref element="C1" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="C4" pad="2"/>
<contactref element="C5" pad="2"/>
<contactref element="C6" pad="2"/>
<contactref element="C7" pad="2"/>
<contactref element="C8" pad="2"/>
<contactref element="C9" pad="2"/>
<contactref element="C10" pad="2"/>
<contactref element="C11" pad="2"/>
<contactref element="C12" pad="-"/>
</signal>
<signal name="VCC">
<contactref element="IC1" pad="16"/>
<contactref element="U$1" pad="P$12"/>
<contactref element="U$2" pad="P$12"/>
<contactref element="IC1" pad="10"/>
<contactref element="IC2" pad="16"/>
<contactref element="IC2" pad="10"/>
<contactref element="U$1" pad="P$8"/>
<contactref element="U$3" pad="P$12"/>
<contactref element="U$4" pad="P$12"/>
<contactref element="U$5" pad="P$12"/>
<contactref element="U$6" pad="P$12"/>
<contactref element="U$7" pad="P$12"/>
<contactref element="U$8" pad="P$12"/>
<contactref element="IC3" pad="16"/>
<contactref element="IC3" pad="10"/>
<contactref element="J1" pad="1"/>
<contactref element="R1" pad="1"/>
<contactref element="C1" pad="1"/>
<contactref element="C2" pad="1"/>
<contactref element="C3" pad="1"/>
<contactref element="C4" pad="1"/>
<contactref element="C5" pad="1"/>
<contactref element="C6" pad="1"/>
<contactref element="C7" pad="1"/>
<contactref element="C8" pad="1"/>
<contactref element="C9" pad="1"/>
<contactref element="C10" pad="1"/>
<contactref element="C11" pad="1"/>
<contactref element="C12" pad="+"/>
</signal>
<signal name="CLK">
<contactref element="U$1" pad="P$9"/>
<contactref element="U$2" pad="P$9"/>
<contactref element="U$3" pad="P$9"/>
<contactref element="U$4" pad="P$9"/>
<contactref element="U$5" pad="P$9"/>
<contactref element="U$6" pad="P$9"/>
<contactref element="U$7" pad="P$9"/>
<contactref element="U$8" pad="P$9"/>
</signal>
<signal name="OE">
<contactref element="IC1" pad="13"/>
<contactref element="IC2" pad="13"/>
<contactref element="IC3" pad="13"/>
<contactref element="J1" pad="4"/>
</signal>
<signal name="LATCH">
<contactref element="IC1" pad="12"/>
<contactref element="IC2" pad="12"/>
<contactref element="IC3" pad="12"/>
<contactref element="J1" pad="5"/>
</signal>
<signal name="CE0">
<contactref element="IC1" pad="15"/>
<contactref element="U$1" pad="P$11"/>
</signal>
<signal name="CE2">
<contactref element="IC1" pad="2"/>
<contactref element="U$3" pad="P$11"/>
</signal>
<signal name="CE3">
<contactref element="IC1" pad="3"/>
<contactref element="U$4" pad="P$11"/>
</signal>
<signal name="CE4">
<contactref element="IC1" pad="4"/>
<contactref element="U$5" pad="P$11"/>
</signal>
<signal name="CE5">
<contactref element="IC1" pad="5"/>
<contactref element="U$6" pad="P$11"/>
</signal>
<signal name="CE6">
<contactref element="IC1" pad="6"/>
<contactref element="U$7" pad="P$11"/>
</signal>
<signal name="CE7">
<contactref element="IC1" pad="7"/>
<contactref element="U$8" pad="P$11"/>
</signal>
<signal name="CE1">
<contactref element="IC1" pad="1"/>
<contactref element="U$2" pad="P$11"/>
</signal>
<signal name="N$1">
<contactref element="IC2" pad="14"/>
<contactref element="IC1" pad="9"/>
</signal>
<signal name="D0">
<contactref element="U$1" pad="P$17"/>
<contactref element="U$2" pad="P$17"/>
<contactref element="U$3" pad="P$17"/>
<contactref element="U$4" pad="P$17"/>
<contactref element="U$5" pad="P$17"/>
<contactref element="U$6" pad="P$17"/>
<contactref element="U$7" pad="P$17"/>
<contactref element="U$8" pad="P$17"/>
<contactref element="IC2" pad="7"/>
</signal>
<signal name="D1">
<contactref element="U$1" pad="P$18"/>
<contactref element="U$2" pad="P$18"/>
<contactref element="U$3" pad="P$18"/>
<contactref element="U$4" pad="P$18"/>
<contactref element="U$5" pad="P$18"/>
<contactref element="U$6" pad="P$18"/>
<contactref element="U$7" pad="P$18"/>
<contactref element="U$8" pad="P$18"/>
<contactref element="IC2" pad="6"/>
</signal>
<signal name="D2">
<contactref element="U$1" pad="P$19"/>
<contactref element="U$2" pad="P$19"/>
<contactref element="U$3" pad="P$19"/>
<contactref element="U$4" pad="P$19"/>
<contactref element="U$5" pad="P$19"/>
<contactref element="U$6" pad="P$19"/>
<contactref element="U$7" pad="P$19"/>
<contactref element="U$8" pad="P$19"/>
<contactref element="IC2" pad="5"/>
</signal>
<signal name="D3">
<contactref element="U$1" pad="P$20"/>
<contactref element="U$2" pad="P$20"/>
<contactref element="U$3" pad="P$20"/>
<contactref element="U$4" pad="P$20"/>
<contactref element="U$5" pad="P$20"/>
<contactref element="U$6" pad="P$20"/>
<contactref element="U$7" pad="P$20"/>
<contactref element="U$8" pad="P$20"/>
<contactref element="IC2" pad="4"/>
</signal>
<signal name="D4">
<contactref element="U$1" pad="P$21"/>
<contactref element="U$2" pad="P$21"/>
<contactref element="U$3" pad="P$21"/>
<contactref element="U$4" pad="P$21"/>
<contactref element="U$5" pad="P$21"/>
<contactref element="U$6" pad="P$21"/>
<contactref element="U$7" pad="P$21"/>
<contactref element="U$8" pad="P$21"/>
<contactref element="IC2" pad="3"/>
</signal>
<signal name="D5">
<contactref element="U$1" pad="P$22"/>
<contactref element="U$2" pad="P$22"/>
<contactref element="U$3" pad="P$22"/>
<contactref element="U$4" pad="P$22"/>
<contactref element="U$5" pad="P$22"/>
<contactref element="U$6" pad="P$22"/>
<contactref element="U$7" pad="P$22"/>
<contactref element="U$8" pad="P$22"/>
<contactref element="IC2" pad="2"/>
</signal>
<signal name="D6">
<contactref element="U$1" pad="P$23"/>
<contactref element="U$2" pad="P$23"/>
<contactref element="U$3" pad="P$23"/>
<contactref element="U$4" pad="P$23"/>
<contactref element="U$5" pad="P$23"/>
<contactref element="U$6" pad="P$23"/>
<contactref element="U$7" pad="P$23"/>
<contactref element="U$8" pad="P$23"/>
<contactref element="IC2" pad="1"/>
</signal>
<signal name="D7">
<contactref element="U$1" pad="P$24"/>
<contactref element="U$2" pad="P$24"/>
<contactref element="U$3" pad="P$24"/>
<contactref element="U$4" pad="P$24"/>
<contactref element="U$5" pad="P$24"/>
<contactref element="U$6" pad="P$24"/>
<contactref element="U$7" pad="P$24"/>
<contactref element="U$8" pad="P$24"/>
<contactref element="IC2" pad="15"/>
</signal>
<signal name="A0">
<contactref element="U$1" pad="P$3"/>
<contactref element="U$2" pad="P$3"/>
<contactref element="U$3" pad="P$3"/>
<contactref element="U$4" pad="P$3"/>
<contactref element="U$5" pad="P$3"/>
<contactref element="U$6" pad="P$3"/>
<contactref element="U$7" pad="P$3"/>
<contactref element="U$8" pad="P$3"/>
<contactref element="IC3" pad="15"/>
</signal>
<signal name="A1">
<contactref element="U$1" pad="P$4"/>
<contactref element="U$2" pad="P$4"/>
<contactref element="U$3" pad="P$4"/>
<contactref element="U$4" pad="P$4"/>
<contactref element="U$5" pad="P$4"/>
<contactref element="U$6" pad="P$4"/>
<contactref element="U$7" pad="P$4"/>
<contactref element="U$8" pad="P$4"/>
<contactref element="IC3" pad="1"/>
</signal>
<signal name="A2">
<contactref element="U$1" pad="P$5"/>
<contactref element="U$2" pad="P$5"/>
<contactref element="U$3" pad="P$5"/>
<contactref element="U$4" pad="P$5"/>
<contactref element="U$5" pad="P$5"/>
<contactref element="U$6" pad="P$5"/>
<contactref element="U$7" pad="P$5"/>
<contactref element="U$8" pad="P$5"/>
<contactref element="IC3" pad="2"/>
</signal>
<signal name="A3">
<contactref element="U$1" pad="P$6"/>
<contactref element="U$2" pad="P$6"/>
<contactref element="U$3" pad="P$6"/>
<contactref element="U$4" pad="P$6"/>
<contactref element="U$5" pad="P$6"/>
<contactref element="U$6" pad="P$6"/>
<contactref element="U$7" pad="P$6"/>
<contactref element="U$8" pad="P$6"/>
<contactref element="IC3" pad="3"/>
</signal>
<signal name="A4">
<contactref element="U$1" pad="P$7"/>
<contactref element="U$2" pad="P$7"/>
<contactref element="U$3" pad="P$7"/>
<contactref element="U$4" pad="P$7"/>
<contactref element="U$5" pad="P$7"/>
<contactref element="U$6" pad="P$7"/>
<contactref element="U$7" pad="P$7"/>
<contactref element="U$8" pad="P$7"/>
<contactref element="IC3" pad="4"/>
</signal>
<signal name="RST">
<contactref element="U$2" pad="P$1"/>
<contactref element="U$1" pad="P$1"/>
<contactref element="U$3" pad="P$1"/>
<contactref element="U$4" pad="P$1"/>
<contactref element="U$5" pad="P$1"/>
<contactref element="U$6" pad="P$1"/>
<contactref element="U$7" pad="P$1"/>
<contactref element="U$8" pad="P$1"/>
<contactref element="J1" pad="3"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="FL">
<contactref element="U$2" pad="P$2"/>
<contactref element="U$1" pad="P$2"/>
<contactref element="U$3" pad="P$2"/>
<contactref element="U$4" pad="P$2"/>
<contactref element="U$5" pad="P$2"/>
<contactref element="U$6" pad="P$2"/>
<contactref element="U$7" pad="P$2"/>
<contactref element="U$8" pad="P$2"/>
<contactref element="IC3" pad="7"/>
</signal>
<signal name="WR">
<contactref element="U$2" pad="P$10"/>
<contactref element="U$1" pad="P$10"/>
<contactref element="U$3" pad="P$10"/>
<contactref element="U$4" pad="P$10"/>
<contactref element="U$5" pad="P$10"/>
<contactref element="U$6" pad="P$10"/>
<contactref element="U$7" pad="P$10"/>
<contactref element="U$8" pad="P$10"/>
<contactref element="IC3" pad="6"/>
</signal>
<signal name="RD">
<contactref element="U$2" pad="P$16" route="any" routetag="G$1._RD"/>
<contactref element="U$1" pad="P$16" route="any" routetag="G$1._RD"/>
<contactref element="U$3" pad="P$16" route="any" routetag="G$1._RD"/>
<contactref element="U$4" pad="P$16" route="any" routetag="G$1._RD"/>
<contactref element="U$5" pad="P$16" route="any" routetag="G$1._RD"/>
<contactref element="U$6" pad="P$16" route="any" routetag="G$1._RD"/>
<contactref element="U$7" pad="P$16" route="any" routetag="G$1._RD"/>
<contactref element="U$8" pad="P$16" route="any" routetag="G$1._RD"/>
<contactref element="IC3" pad="5"/>
</signal>
<signal name="SDA">
<contactref element="IC1" pad="14"/>
<contactref element="J1" pad="7"/>
</signal>
<signal name="SCL">
<contactref element="IC1" pad="11"/>
<contactref element="IC2" pad="11"/>
<contactref element="IC3" pad="11"/>
<contactref element="J1" pad="6"/>
</signal>
<signal name="N$2">
<contactref element="IC2" pad="9"/>
<contactref element="IC3" pad="14"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
