<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="49.51" y2="0" width="0" layer="20"/>
<wire x1="49.51" y1="0" x2="49.51" y2="55.55" width="0" layer="20"/>
<wire x1="49.51" y1="55.55" x2="0" y2="55.55" width="0" layer="20"/>
<wire x1="0" y1="55.55" x2="0" y2="0" width="0" layer="20"/>
<text>CS</text>
<text>CS</text>
<text>MOSI</text>
<text>MOSI</text>
<text>MISO</text>
<text>MISO</text>
<text>SCK</text>
<text>SCK</text>
<text>GND</text>
<text>GND</text>
<text>5V</text>
<text>5V</text>
<text>SDA</text>
<text>SDA</text>
<text>SCL</text>
<text>SCL</text>
<text>5V</text>
<text>5V</text>
<text>GND</text>
<text>GND</text>
<text>PWM</text>
<text>PWM</text>
<text>VIN</text>
<text>GND</text>
<text>EN</text>
<text>VP</text>
<text>VN</text>
<text>EE 327: PanoCama ESP32 DevkitV1 board.</text>
<text>This board is a pretty barebones, and more like a breakout board. 
A more advanced version with the ESP32 module is in the works.</text>
<text>Leo Ling
May 27, 2021</text>
<text>PanoCama V1
LCL
2021-05-27</text>
<hole x="45.085" y="46.99" drill="2"/>
<hole x="45.085" y="4.445" drill="2"/>
<hole x="3.81" y="27.305" drill="2"/>
</plain>
<libraries>
<library name="adafruit">
<packages>
<package name="1X08-BIG">
</package>
<package name="1X03">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="ESP32-DEVKITV1">
<packages>
<package name="ESP32-DEVKITV1">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="ARDUCAM-1" library="adafruit" package="1X08-BIG" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="ARDUCAM-2" library="adafruit" package="1X08-BIG" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SERVO1" library="adafruit" package="1X03" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SERVO2" library="adafruit" package="1X03" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$1" library="ESP32-DEVKITV1" package="ESP32-DEVKITV1" value="ESP32DEVKITV1">
<attribute name="NAME"/>
</element>
</elements>
<signals>
<signal name="MISO">
<contactref element="U$1" pad="10"/>
<contactref element="ARDUCAM-1" pad="3"/>
<contactref element="ARDUCAM-2" pad="3"/>
</signal>
<signal name="MOSI">
<contactref element="U$1" pad="15"/>
<contactref element="ARDUCAM-1" pad="2"/>
<contactref element="ARDUCAM-2" pad="2"/>
</signal>
<signal name="SCK">
<contactref element="U$1" pad="9"/>
<contactref element="ARDUCAM-1" pad="4"/>
<contactref element="ARDUCAM-2" pad="4"/>
</signal>
<signal name="SCL1">
<contactref element="U$1" pad="14"/>
<contactref element="ARDUCAM-1" pad="8"/>
</signal>
<signal name="SDA1">
<contactref element="U$1" pad="11"/>
<contactref element="ARDUCAM-1" pad="7"/>
</signal>
<signal name="CS1">
<contactref element="U$1" pad="8"/>
<contactref element="ARDUCAM-1" pad="1"/>
</signal>
<signal name="GND">
<contactref element="U$1" pad="2"/>
<contactref element="U$1" pad="29"/>
<contactref element="ARDUCAM-1" pad="5"/>
<contactref element="ARDUCAM-2" pad="5"/>
<contactref element="SERVO1" pad="2"/>
<contactref element="SERVO2" pad="2"/>
</signal>
<signal name="5V">
<contactref element="U$1" pad="30"/>
<contactref element="ARDUCAM-1" pad="6"/>
<contactref element="SERVO1" pad="3"/>
<contactref element="SERVO2" pad="3"/>
<contactref element="ARDUCAM-2" pad="6"/>
</signal>
<signal name="PWM1">
<contactref element="U$1" pad="25"/>
<contactref element="SERVO1" pad="1"/>
</signal>
<signal name="PWM2">
<contactref element="U$1" pad="23"/>
<contactref element="SERVO2" pad="1"/>
</signal>
<signal name="CS2">
<contactref element="U$1" pad="3"/>
<contactref element="ARDUCAM-2" pad="1"/>
</signal>
<signal name="SDA2">
<contactref element="ARDUCAM-2" pad="7"/>
<contactref element="U$1" pad="28"/>
</signal>
<signal name="SCL2">
<contactref element="ARDUCAM-2" pad="8"/>
<contactref element="U$1" pad="26"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
