(kicad_pcb (version 20210925) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (title_block
    (title "Remoticon.2 Badge")
    (date "2021-10-12")
    (rev "0.1")
  )
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen") (color "White"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (color "Purple") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (color "Purple") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen") (color "White"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0)
    (grid_origin 80 100)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (footprint "Connectors:PTH_Proto_pad" (layer "F.Cu")
    (tedit 60C6130C)
    (at 93.97 97.46)
    (attr through_hole board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 2.286) (layer "F.SilkS") hide)
    (fp_text value "PTH_Proto_pad" (at 0 -2.286) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
  )
  (footprint "Connectors:PTH_Proto_pad" (layer "F.Cu")
    (tedit 60C6130C)
    (at 88.89 82.22)
    (attr through_hole board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 2.286) (layer "F.SilkS") hide)
    (fp_text value "PTH_Proto_pad" (at 0 -2.286) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
  )
  (footprint "Connectors:PTH_Proto_pad" (layer "F.Cu")
    (tedit 60C6130C)
    (at 76.19 100)
    (attr through_hole board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 2.286) (layer "F.SilkS") hide)
    (fp_text value "PTH_Proto_pad" (at 0 -2.286) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
  )
  (footprint "Connectors:PTH_Proto_pad" (layer "F.Cu")
    (tedit 60C6130C)
    (at 66.03 100)
    (attr through_hole board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 2.286) (layer "F.SilkS") hide)
    (fp_text value "PTH_Proto_pad" (at 0 -2.286) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
  )
  (footprint "Connectors:PTH_Proto_pad" (layer "F.Cu")
    (tedit 60C6130C)
    (at 63.49 102.54)
    (attr through_hole board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 2.286) (layer "F.SilkS") hide)
    (fp_text value "PTH_Proto_pad" (at 0 -2.286) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
  )
  (footprint "Connectors:PTH_Proto_pad" (layer "F.Cu")
    (tedit 60C6130C)
    (at 86.35 94.92)
    (attr through_hole board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 2.286) (layer "F.SilkS") hide)
    (fp_text value "PTH_Proto_pad" (at 0 -2.286) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
  )
  (footprint "LOGO" (layer "F.Cu")
    (tedit 615CA259)
    (at 80 100)
    (attr board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "G***" (at 0 0) (layer "F.SilkS") hide)
    (fp_text value "LOGO" (at 0.75 0) (layer "F.SilkS") hide)
    (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.254)
      (keepout (tracks allowed) (vias allowed) (pads allowed ) (copperpour not_allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 93.85 132.11)
          (xy 86.92 132.11)
          (xy 86.92 125.18)
        )
      )
    )
    (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.254)
      (keepout (tracks allowed) (vias allowed) (pads allowed ) (copperpour not_allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 107.67 125.19)
          (xy 107.66 132.11)
          (xy 100.74 132.11)
          (xy 107.66 125.18)
        )
      )
    )
    (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.254)
      (keepout (tracks allowed) (vias allowed) (pads allowed ) (copperpour not_allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 80.02 118.29)
          (xy 73.11 118.29)
          (xy 80.02 125.2)
          (xy 80.02 132.12)
          (xy 73.09 125.21)
          (xy 66.18 125.21)
          (xy 66.18 132.11)
          (xy 52.34 132.1)
          (xy 59.26 125.18)
          (xy 59.26 111.37)
          (xy 52.33 111.37)
          (xy 52.33 104.43)
          (xy 59.26 111.36)
          (xy 59.26 104.44)
          (xy 66.18 111.36)
          (xy 66.18 104.45)
          (xy 73.1 104.45)
          (xy 59.28 118.28)
          (xy 66.16 125.16)
          (xy 66.09 125.21)
          (xy 59.26 125.21)
          (xy 59.26 132.09)
          (xy 66.18 125.18)
          (xy 66.18 118.28)
          (xy 73.08 125.18)
          (xy 73.08 118.28)
          (xy 79.99 111.37)
          (xy 73.06 111.37)
          (xy 80 104.43)
        )
      )
    )
    (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.254)
      (keepout (tracks allowed) (vias allowed) (pads allowed ) (copperpour not_allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 107.67 111.36)
          (xy 100.75 111.36)
          (xy 93.81 118.3)
          (xy 93.82 111.4)
          (xy 86.91 118.3)
          (xy 86.93 111.33)
          (xy 93.84 104.44)
          (xy 100.78 104.44)
          (xy 93.85 111.38)
          (xy 100.7 111.38)
          (xy 107.67 104.42)
        )
      )
    )
  )
  (footprint "Connectors:PTH_Proto_pad" (layer "F.Cu")
    (tedit 60C6130C)
    (at 101.59 82.22)
    (attr through_hole board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 2.286) (layer "F.SilkS") hide)
    (fp_text value "PTH_Proto_pad" (at 0 -2.286) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
  )
  (footprint "Connectors:PTH_Proto_pad" (layer "F.Cu")
    (tedit 60C6130C)
    (at 86.35 92.38)
    (attr through_hole board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 2.286) (layer "F.SilkS") hide)
    (fp_text value "PTH_Proto_pad" (at 0 -2.286) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
  )
  (footprint "Connectors:PTH_Proto_pad" (layer "F.Cu")
    (tedit 60C6130C)
    (at 106.67 97.46)
    (attr through_hole board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 2.286) (layer "F.SilkS") hide)
    (fp_text value "PTH_Proto_pad" (at 0 -2.286) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
  )
  (footprint "Connectors:PTH_Proto_pad" (layer "F.Cu")
    (tedit 60C6130C)
    (at 93.97 84.76)
    (attr through_hole board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 2.286) (layer "F.SilkS") hide)
    (fp_text value "PTH_Proto_pad" (at 0 -2.286) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
  )
  (footprint "Connectors:PTH_Proto_pad" (layer "F.Cu")
    (tedit 60C6130C)
    (at 101.59 89.84)
    (attr through_hole board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 2.286) (layer "F.SilkS") hide)
    (fp_text value "PTH_Proto_pad" (at 0 -2.286) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
  )
  (footprint "Connectors:PTH_Proto_pad" (layer "F.Cu")
    (tedit 60C6130C)
    (at 88.89 87.3)
    (attr through_hole board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 2.286) (layer "F.SilkS") hide)
    (fp_text value "PTH_Proto_pad" (at 0 -2.286) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
  )
  (footprint "Connectors:PTH_Proto_pad" (layer "F.Cu")
    (tedit 60C6130C)
    (at 60.95 97.46)
    (attr through_hole board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 2.286) (layer "F.SilkS") hide)
    (fp_text value "PTH_Proto_pad" (at 0 -2.286) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
  )
  (footprint "Connectors:PTH_Proto_pad" (layer "F.Cu")
    (tedit 60C6130C)
    (at 81.27 87.3)
    (attr through_hole board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 2.286) (layer "F.SilkS") hide)
    (fp_text value "PTH_Proto_pad" (at 0 -2.286) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
  )
  (footprint "LOGO" (layer "F.Cu")
    (tedit 615CA26C)
    (at 80 100)
    (attr board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "G***" (at 0 0) (layer "F.SilkS") hide)
    (fp_text value "LOGO" (at 0.75 0) (layer "F.SilkS") hide)
  )
  (footprint "Connectors:PTH_Proto_pad" (layer "F.Cu")
    (tedit 60C6130C)
    (at 73.65 84.76)
    (attr through_hole board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 2.286) (layer "F.SilkS") hide)
    (fp_text value "PTH_Proto_pad" (at 0 -2.286) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
  )
  (footprint "Connectors:PTH_Proto_pad" (layer "F.Cu")
    (tedit 60C6130C)
    (at 99.05 92.38)
    (attr through_hole board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 2.286) (layer "F.SilkS") hide)
    (fp_text value "PTH_Proto_pad" (at 0 -2.286) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
  )
  (footprint "Connectors:PTH_Proto_pad" (layer "F.Cu")
    (tedit 60C6130C)
    (at 71.11 94.92)
    (attr through_hole board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 2.286) (layer "F.SilkS") hide)
    (fp_text value "PTH_Proto_pad" (at 0 -2.286) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
  )
  (footprint "Connectors:PTH_Proto_pad" (layer "F.Cu")
    (tedit 60C6130C)
    (at 76.19 94.92)
    (attr through_hole board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 2.286) (layer "F.SilkS") hide)
    (fp_text value "PTH_Proto_pad" (at 0 -2.286) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
  )
  (footprint "Connectors:PTH_Proto_pad" (layer "F.Cu")
    (tedit 60C6130C)
    (at 96.51 94.92)
    (attr through_hole board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 2.286) (layer "F.SilkS") hide)
    (fp_text value "PTH_Proto_pad" (at 0 -2.286) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
  )
  (footprint "Connectors:PTH_Proto_pad" (layer "F.Cu")
    (tedit 60C6130C)
    (at 96.51 87.3)
    (attr through_hole board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 2.286) (layer "F.SilkS") hide)
    (fp_text value "PTH_Proto_pad" (at 0 -2.286) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
  )
  (footprint "Connectors:PTH_Proto_pad" (layer "F.Cu")
    (tedit 60C6130C)
    (at 73.65 89.84)
    (attr through_hole board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 2.286) (layer "F.SilkS") hide)
    (fp_text value "PTH_Proto_pad" (at 0 -2.286) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
  )
  (footprint "Connectors:PTH_Proto_pad" (layer "F.Cu")
    (tedit 60C6130C)
    (at 93.97 82.22)
    (attr through_hole board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 2.286) (layer "F.SilkS") hide)
    (fp_text value "PTH_Proto_pad" (at 0 -2.286) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
  )
  (footprint "Connectors:PTH_Proto_pad" (layer "F.Cu")
    (tedit 60C6130C)
    (at 78.73 94.92)
    (attr through_hole board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 2.286) (layer "F.SilkS") hide)
    (fp_text value "PTH_Proto_pad" (at 0 -2.286) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
  )
  (footprint "Connectors:PTH_Proto_pad" (layer "F.Cu")
    (tedit 60C6130C)
    (at 93.97 87.3)
    (attr through_hole board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 2.286) (layer "F.SilkS") hide)
    (fp_text value "PTH_Proto_pad" (at 0 -2.286) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
  )
  (footprint "Connectors:PTH_Proto_pad" (layer "F.Cu")
    (tedit 60C6130C)
    (at 58.41 82.22)
    (attr through_hole board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 2.286) (layer "F.SilkS") hide)
    (fp_text value "PTH_Proto_pad" (at 0 -2.286) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
  )
  (footprint "Connectors:PTH_Proto_pad" (layer "F.Cu")
    (tedit 60C6130C)
    (at 55.87 97.46)
    (attr through_hole board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 2.286) (layer "F.SilkS") hide)
    (fp_text value "PTH_Proto_pad" (at 0 -2.286) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
  )
  (footprint "Connectors:PTH_Proto_pad" (layer "F.Cu")
    (tedit 60C6130C)
    (at 88.89 100)
    (attr through_hole board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 2.286) (layer "F.SilkS") hide)
    (fp_text value "PTH_Proto_pad" (at 0 -2.286) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
  )
  (footprint "Connectors:PTH_Proto_pad" (layer "F.Cu")
    (tedit 60C6130C)
    (at 83.81 94.92)
    (attr through_hole board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 2.286) (layer "F.SilkS") hide)
    (fp_text value "PTH_Proto_pad" (at 0 -2.286) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
  )
  (footprint "Connectors:PTH_Proto_pad" (layer "F.Cu")
    (tedit 60C6130C)
    (at 91.43 89.84)
    (attr through_hole board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 2.286) (layer "F.SilkS") hide)
    (fp_text value "PTH_Proto_pad" (at 0 -2.286) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
  )
  (footprint "Connectors:PTH_Proto_pad" (layer "F.Cu")
    (tedit 60C6130C)
    (at 91.43 92.38)
    (attr through_hole board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 2.286) (layer "F.SilkS") hide)
    (fp_text value "PTH_Proto_pad" (at 0 -2.286) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
  )
  (footprint "Connectors:PTH_Proto_pad" (layer "F.Cu")
    (tedit 60C6130C)
    (at 104.13 102.54)
    (attr through_hole board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 2.286) (layer "F.SilkS") hide)
    (fp_text value "PTH_Proto_pad" (at 0 -2.286) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
  )
  (footprint "Connectors:PTH_Proto_pad" (layer "F.Cu")
    (tedit 60C6130C)
    (at 60.95 84.76)
    (attr through_hole board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 2.286) (layer "F.SilkS") hide)
    (fp_text value "PTH_Proto_pad" (at 0 -2.286) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
  )
  (footprint "Connectors:PTH_Proto_pad" (layer "F.Cu")
    (tedit 60C6130C)
    (at 96.51 100)
    (attr through_hole board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 2.286) (layer "F.SilkS") hide)
    (fp_text value "PTH_Proto_pad" (at 0 -2.286) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
  )
  (footprint "Connectors:PTH_Proto_pad" (layer "F.Cu")
    (tedit 60C6130C)
    (at 101.59 92.38)
    (attr through_hole board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 2.286) (layer "F.SilkS") hide)
    (fp_text value "PTH_Proto_pad" (at 0 -2.286) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
  )
  (footprint "Connectors:PTH_Proto_pad" (layer "F.Cu")
    (tedit 60C6130C)
    (at 81.27 92.38)
    (attr through_hole board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 2.286) (layer "F.SilkS") hide)
    (fp_text value "PTH_Proto_pad" (at 0 -2.286) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
  )
  (footprint "Connectors:PTH_Proto_pad" (layer "F.Cu")
    (tedit 60C6130C)
    (at 104.13 87.3)
    (attr through_hole board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 2.286) (layer "F.SilkS") hide)
    (fp_text value "PTH_Proto_pad" (at 0 -2.286) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
  )
  (footprint "Connectors:PTH_Proto_pad" (layer "F.Cu")
    (tedit 60C6130C)
    (at 78.73 100)
    (attr through_hole board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 2.286) (layer "F.SilkS") hide)
    (fp_text value "PTH_Proto_pad" (at 0 -2.286) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
  )
  (footprint "Connectors:PTH_Proto_pad" (layer "F.Cu")
    (tedit 60C6130C)
    (at 83.81 97.46)
    (attr through_hole board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 2.286) (layer "F.SilkS") hide)
    (fp_text value "PTH_Proto_pad" (at 0 -2.286) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
  )
  (footprint "Connectors:PTH_Proto_pad" (layer "F.Cu")
    (tedit 60C6130C)
    (at 99.05 87.3)
    (attr through_hole board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 2.286) (layer "F.SilkS") hide)
    (fp_text value "PTH_Proto_pad" (at 0 -2.286) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
  )
  (footprint "Connectors:PTH_Proto_pad" (layer "F.Cu")
    (tedit 60C6130C)
    (at 104.13 89.84)
    (attr through_hole board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 2.286) (layer "F.SilkS") hide)
    (fp_text value "PTH_Proto_pad" (at 0 -2.286) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
  )
  (footprint "Connectors:PTH_Proto_pad" (layer "F.Cu")
    (tedit 60C6130C)
    (at 55.87 102.54)
    (attr through_hole board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 2.286) (layer "F.SilkS") hide)
    (fp_text value "PTH_Proto_pad" (at 0 -2.286) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
  )
  (footprint "Connectors:PTH_Proto_pad" (layer "F.Cu")
    (tedit 60C6130C)
    (at 96.51 82.22)
    (attr through_hole board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 2.286) (layer "F.SilkS") hide)
    (fp_text value "PTH_Proto_pad" (at 0 -2.286) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
  )
  (footprint "Connectors:PTH_Proto_pad" (layer "F.Cu")
    (tedit 60C6130C)
    (at 99.05 82.22)
    (attr through_hole board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 2.286) (layer "F.SilkS") hide)
    (fp_text value "PTH_Proto_pad" (at 0 -2.286) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
  )
  (footprint "Connectors:PTH_Proto_pad" (layer "F.Cu")
    (tedit 60C6130C)
    (at 71.11 87.3)
    (attr through_hole board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 2.286) (layer "F.SilkS") hide)
    (fp_text value "PTH_Proto_pad" (at 0 -2.286) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
  )
  (footprint "Connectors:PTH_Proto_pad" (layer "F.Cu")
    (tedit 60C6130C)
    (at 58.41 92.38)
    (attr through_hole board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 2.286) (layer "F.SilkS") hide)
    (fp_text value "PTH_Proto_pad" (at 0 -2.286) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
  )
  (footprint "Connectors:PTH_Proto_pad" (layer "F.Cu")
    (tedit 60C6130C)
    (at 106.67 100)
    (attr through_hole board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 2.286) (layer "F.SilkS") hide)
    (fp_text value "PTH_Proto_pad" (at 0 -2.286) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
  )
  (footprint "Connectors:PTH_Proto_pad" (layer "F.Cu")
    (tedit 60C6130C)
    (at 78.73 92.38)
    (attr through_hole board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 2.286) (layer "F.SilkS") hide)
    (fp_text value "PTH_Proto_pad" (at 0 -2.286) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
  )
  (footprint "Connectors:PTH_Proto_pad" (layer "F.Cu")
    (tedit 60C6130C)
    (at 53.33 82.22)
    (attr through_hole board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 2.286) (layer "F.SilkS") hide)
    (fp_text value "PTH_Proto_pad" (at 0 -2.286) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
  )
  (footprint "Connectors:PTH_Proto_pad" (layer "F.Cu")
    (tedit 60C6130C)
    (at 99.05 89.84)
    (attr through_hole board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 2.286) (layer "F.SilkS") hide)
    (fp_text value "PTH_Proto_pad" (at 0 -2.286) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
  )
  (footprint "Connectors:PTH_Proto_pad" (layer "F.Cu")
    (tedit 60C6130C)
    (at 86.35 100)
    (attr through_hole board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 2.286) (layer "F.SilkS") hide)
    (fp_text value "PTH_Proto_pad" (at 0 -2.286) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
  )
  (footprint "Connectors:PTH_Proto_pad" (layer "F.Cu")
    (tedit 60C6130C)
    (at 63.49 94.92)
    (attr through_hole board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 2.286) (layer "F.SilkS") hide)
    (fp_text value "PTH_Proto_pad" (at 0 -2.286) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
  )
  (footprint "Connectors:PTH_Proto_pad" (layer "F.Cu")
    (tedit 60C6130C)
    (at 55.87 92.38)
    (attr through_hole board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 2.286) (layer "F.SilkS") hide)
    (fp_text value "PTH_Proto_pad" (at 0 -2.286) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
  )
  (footprint "Connectors:PTH_Proto_pad" (layer "F.Cu")
    (tedit 60C6130C)
    (at 83.81 92.38)
    (attr through_hole board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 2.286) (layer "F.SilkS") hide)
    (fp_text value "PTH_Proto_pad" (at 0 -2.286) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
  )
  (footprint "Connectors:PTH_Proto_pad" (layer "F.Cu")
    (tedit 60C6130C)
    (at 88.89 89.84)
    (attr through_hole board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 2.286) (layer "F.SilkS") hide)
    (fp_text value "PTH_Proto_pad" (at 0 -2.286) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
  )
  (footprint "Connectors:PTH_Proto_pad" (layer "F.Cu")
    (tedit 60C6130C)
    (at 81.27 82.22)
    (attr through_hole board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 2.286) (layer "F.SilkS") hide)
    (fp_text value "PTH_Proto_pad" (at 0 -2.286) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
  )
  (footprint "Connectors:PTH_Proto_pad" (layer "F.Cu")
    (tedit 60C6130C)
    (at 99.05 100)
    (attr through_hole board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 2.286) (layer "F.SilkS") hide)
    (fp_text value "PTH_Proto_pad" (at 0 -2.286) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
  )
  (footprint "Connectors:PTH_Proto_pad" (layer "F.Cu")
    (tedit 60C6130C)
    (at 60.95 102.54)
    (attr through_hole board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 2.286) (layer "F.SilkS") hide)
    (fp_text value "PTH_Proto_pad" (at 0 -2.286) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
  )
  (footprint "Connectors:PTH_Proto_pad" (layer "F.Cu")
    (tedit 60C6130C)
    (at 81.27 102.54)
    (attr through_hole board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 2.286) (layer "F.SilkS") hide)
    (fp_text value "PTH_Proto_pad" (at 0 -2.286) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
  )
  (footprint "Connectors:PTH_Proto_pad" (layer "F.Cu")
    (tedit 60C6130C)
    (at 53.33 87.3)
    (attr through_hole board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 2.286) (layer "F.SilkS") hide)
    (fp_text value "PTH_Proto_pad" (at 0 -2.286) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
  )
  (footprint "Connectors:PTH_Proto_pad" (layer "F.Cu")
    (tedit 60C6130C)
    (at 78.73 102.54)
    (attr through_hole board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 2.286) (layer "F.SilkS") hide)
    (fp_text value "PTH_Proto_pad" (at 0 -2.286) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
  )
  (footprint "Connectors:PTH_Proto_pad" (layer "F.Cu")
    (tedit 60C6130C)
    (at 73.65 102.54)
    (attr through_hole board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 2.286) (layer "F.SilkS") hide)
    (fp_text value "PTH_Proto_pad" (at 0 -2.286) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
  )
  (footprint "Connectors:PTH_Proto_pad" (layer "F.Cu")
    (tedit 60C6130C)
    (at 53.33 92.38)
    (attr through_hole board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 2.286) (layer "F.SilkS") hide)
    (fp_text value "PTH_Proto_pad" (at 0 -2.286) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
  )
  (footprint "Connectors:PTH_Proto_pad" (layer "F.Cu")
    (tedit 60C6130C)
    (at 66.03 87.3)
    (attr through_hole board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 2.286) (layer "F.SilkS") hide)
    (fp_text value "PTH_Proto_pad" (at 0 -2.286) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
  )
  (footprint "Connectors:PTH_Proto_pad" (layer "F.Cu")
    (tedit 60C6130C)
    (at 60.95 100)
    (attr through_hole board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 2.286) (layer "F.SilkS") hide)
    (fp_text value "PTH_Proto_pad" (at 0 -2.286) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
  )
  (footprint "Connectors:PTH_Proto_pad" (layer "F.Cu")
    (tedit 60C6130C)
    (at 81.27 89.84)
    (attr through_hole board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 2.286) (layer "F.SilkS") hide)
    (fp_text value "PTH_Proto_pad" (at 0 -2.286) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
  )
  (footprint "Connectors:PTH_Proto_pad" (layer "F.Cu")
    (tedit 60C6130C)
    (at 55.87 84.76)
    (attr through_hole board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 2.286) (layer "F.SilkS") hide)
    (fp_text value "PTH_Proto_pad" (at 0 -2.286) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
  )
  (footprint "Connectors:PTH_Proto_pad" (layer "F.Cu")
    (tedit 60C6130C)
    (at 71.11 92.38)
    (attr through_hole board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 2.286) (layer "F.SilkS") hide)
    (fp_text value "PTH_Proto_pad" (at 0 -2.286) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
  )
  (footprint "Connectors:PTH_Proto_pad" (layer "F.Cu")
    (tedit 60C6130C)
    (at 63.49 92.38)
    (attr through_hole board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 2.286) (layer "F.SilkS") hide)
    (fp_text value "PTH_Proto_pad" (at 0 -2.286) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
  )
  (footprint "Connectors:PTH_Proto_pad" (layer "F.Cu")
    (tedit 60C6130C)
    (at 68.57 97.46)
    (attr through_hole board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 2.286) (layer "F.SilkS") hide)
    (fp_text value "PTH_Proto_pad" (at 0 -2.286) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
  )
  (footprint "Connectors:PTH_Proto_pad" (layer "F.Cu")
    (tedit 60C6130C)
    (at 58.41 87.3)
    (attr through_hole board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 2.286) (layer "F.SilkS") hide)
    (fp_text value "PTH_Proto_pad" (at 0 -2.286) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
  )
  (footprint "Connectors:PTH_Proto_pad" (layer "F.Cu")
    (tedit 60C6130C)
    (at 76.19 87.3)
    (attr through_hole board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 2.286) (layer "F.SilkS") hide)
    (fp_text value "PTH_Proto_pad" (at 0 -2.286) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
  )
  (footprint "Connectors:PTH_Proto_pad" (layer "F.Cu")
    (tedit 60C6130C)
    (at 88.89 84.76)
    (attr through_hole board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 2.286) (layer "F.SilkS") hide)
    (fp_text value "PTH_Proto_pad" (at 0 -2.286) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
  )
  (footprint "Connectors:PTH_Proto_pad" (layer "F.Cu")
    (tedit 60C6130C)
    (at 68.57 82.22)
    (attr through_hole board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 2.286) (layer "F.SilkS") hide)
    (fp_text value "PTH_Proto_pad" (at 0 -2.286) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
  )
  (footprint "Connectors:PTH_Proto_pad" (layer "F.Cu")
    (tedit 60C6130C)
    (at 58.41 89.84)
    (attr through_hole board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 2.286) (layer "F.SilkS") hide)
    (fp_text value "PTH_Proto_pad" (at 0 -2.286) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
  )
  (footprint "Connectors:PTH_Proto_pad" (layer "F.Cu")
    (tedit 60C6130C)
    (at 99.05 94.92)
    (attr through_hole board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 2.286) (layer "F.SilkS") hide)
    (fp_text value "PTH_Proto_pad" (at 0 -2.286) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
  )
  (footprint "Connectors:PTH_Proto_pad" (layer "F.Cu")
    (tedit 60C6130C)
    (at 104.13 92.38)
    (attr through_hole board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 2.286) (layer "F.SilkS") hide)
    (fp_text value "PTH_Proto_pad" (at 0 -2.286) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
  )
  (footprint "Connectors:PTH_Proto_pad" (layer "F.Cu")
    (tedit 60C6130C)
    (at 88.89 92.38)
    (attr through_hole board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 2.286) (layer "F.SilkS") hide)
    (fp_text value "PTH_Proto_pad" (at 0 -2.286) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
  )
  (footprint "Connectors:PTH_Proto_pad" (layer "F.Cu")
    (tedit 60C6130C)
    (at 83.81 82.22)
    (attr through_hole board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 2.286) (layer "F.SilkS") hide)
    (fp_text value "PTH_Proto_pad" (at 0 -2.286) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
  )
  (footprint "Connectors:PTH_Proto_pad" (layer "F.Cu")
    (tedit 60C6130C)
    (at 60.95 82.22)
    (attr through_hole board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 2.286) (layer "F.SilkS") hide)
    (fp_text value "PTH_Proto_pad" (at 0 -2.286) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
  )
  (footprint "Connectors:PTH_Proto_pad" (layer "F.Cu")
    (tedit 60C6130C)
    (at 106.67 84.76)
    (attr through_hole board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 2.286) (layer "F.SilkS") hide)
    (fp_text value "PTH_Proto_pad" (at 0 -2.286) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
  )
  (footprint "Connectors:PTH_Proto_pad" (layer "F.Cu")
    (tedit 60C6130C)
    (at 96.51 97.46)
    (attr through_hole board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 2.286) (layer "F.SilkS") hide)
    (fp_text value "PTH_Proto_pad" (at 0 -2.286) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
  )
  (footprint "Connectors:PTH_Proto_pad" (layer "F.Cu")
    (tedit 60C6130C)
    (at 88.89 94.92)
    (attr through_hole board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 2.286) (layer "F.SilkS") hide)
    (fp_text value "PTH_Proto_pad" (at 0 -2.286) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
  )
  (footprint "Connectors:PTH_Proto_pad" (layer "F.Cu")
    (tedit 60C6130C)
    (at 71.11 89.84)
    (attr through_hole board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 2.286) (layer "F.SilkS") hide)
    (fp_text value "PTH_Proto_pad" (at 0 -2.286) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
  )
  (footprint "Connectors:PTH_Proto_pad" (layer "F.Cu")
    (tedit 60C6130C)
    (at 73.65 97.46)
    (attr through_hole board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 2.286) (layer "F.SilkS") hide)
    (fp_text value "PTH_Proto_pad" (at 0 -2.286) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
  )
  (footprint "Connectors:PTH_Proto_pad" (layer "F.Cu")
    (tedit 60C6130C)
    (at 60.95 89.84)
    (attr through_hole board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 2.286) (layer "F.SilkS") hide)
    (fp_text value "PTH_Proto_pad" (at 0 -2.286) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
  )
  (footprint "Connectors:PTH_Proto_pad" (layer "F.Cu")
    (tedit 60C6130C)
    (at 86.35 82.22)
    (attr through_hole board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 2.286) (layer "F.SilkS") hide)
    (fp_text value "PTH_Proto_pad" (at 0 -2.286) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
  )
  (footprint "Connectors:PTH_Proto_pad" (layer "F.Cu")
    (tedit 60C6130C)
    (at 83.81 84.76)
    (attr through_hole board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 2.286) (layer "F.SilkS") hide)
    (fp_text value "PTH_Proto_pad" (at 0 -2.286) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
  )
  (footprint "Connectors:PTH_Proto_pad" (layer "F.Cu")
    (tedit 60C6130C)
    (at 55.87 87.3)
    (attr through_hole board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 2.286) (layer "F.SilkS") hide)
    (fp_text value "PTH_Proto_pad" (at 0 -2.286) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
  )
  (footprint "Connectors:PTH_Proto_pad" (layer "F.Cu")
    (tedit 60C6130C)
    (at 78.73 87.3)
    (attr through_hole board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 2.286) (layer "F.SilkS") hide)
    (fp_text value "PTH_Proto_pad" (at 0 -2.286) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
  )
  (footprint "Connectors:PTH_Proto_pad" (layer "F.Cu")
    (tedit 60C6130C)
    (at 66.03 94.92)
    (attr through_hole board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 2.286) (layer "F.SilkS") hide)
    (fp_text value "PTH_Proto_pad" (at 0 -2.286) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
  )
  (footprint "Connectors:PTH_Proto_pad" (layer "F.Cu")
    (tedit 60C6130C)
    (at 101.59 100)
    (attr through_hole board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 2.286) (layer "F.SilkS") hide)
    (fp_text value "PTH_Proto_pad" (at 0 -2.286) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
  )
  (footprint "Connectors:PTH_Proto_pad" (layer "F.Cu")
    (tedit 60C6130C)
    (at 73.65 100)
    (attr through_hole board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 2.286) (layer "F.SilkS") hide)
    (fp_text value "PTH_Proto_pad" (at 0 -2.286) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
  )
  (footprint "Connectors:PTH_Proto_pad" (layer "F.Cu")
    (tedit 60C6130C)
    (at 76.19 92.38)
    (attr through_hole board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 2.286) (layer "F.SilkS") hide)
    (fp_text value "PTH_Proto_pad" (at 0 -2.286) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
  )
  (footprint "Connectors:PTH_Proto_pad" (layer "F.Cu")
    (tedit 60C6130C)
    (at 53.33 102.54)
    (attr through_hole board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 2.286) (layer "F.SilkS") hide)
    (fp_text value "PTH_Proto_pad" (at 0 -2.286) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
  )
  (footprint "Connectors:PTH_Proto_pad" (layer "F.Cu")
    (tedit 60C6130C)
    (at 73.65 87.3)
    (attr through_hole board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 2.286) (layer "F.SilkS") hide)
    (fp_text value "PTH_Proto_pad" (at 0 -2.286) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
  )
  (footprint "Connectors:PTH_Proto_pad" (layer "F.Cu")
    (tedit 60C6130C)
    (at 58.41 84.76)
    (attr through_hole board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 2.286) (layer "F.SilkS") hide)
    (fp_text value "PTH_Proto_pad" (at 0 -2.286) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
  )
  (footprint "Connectors:PTH_Proto_pad" (layer "F.Cu")
    (tedit 60C6130C)
    (at 99.05 84.76)
    (attr through_hole board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 2.286) (layer "F.SilkS") hide)
    (fp_text value "PTH_Proto_pad" (at 0 -2.286) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
  )
  (footprint "Connectors:PTH_Proto_pad" (layer "F.Cu")
    (tedit 60C6130C)
    (at 101.59 84.76)
    (attr through_hole board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 2.286) (layer "F.SilkS") hide)
    (fp_text value "PTH_Proto_pad" (at 0 -2.286) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
  )
  (footprint "Connectors:PTH_Proto_pad" (layer "F.Cu")
    (tedit 60C6130C)
    (at 93.97 100)
    (attr through_hole board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 2.286) (layer "F.SilkS") hide)
    (fp_text value "PTH_Proto_pad" (at 0 -2.286) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
  )
  (footprint "Connectors:PTH_Proto_pad" (layer "F.Cu")
    (tedit 60C6130C)
    (at 71.11 97.46)
    (attr through_hole board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 2.286) (layer "F.SilkS") hide)
    (fp_text value "PTH_Proto_pad" (at 0 -2.286) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
  )
  (footprint "Connectors:PTH_Proto_pad" (layer "F.Cu")
    (tedit 60C6130C)
    (at 60.95 87.3)
    (attr through_hole board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 2.286) (layer "F.SilkS") hide)
    (fp_text value "PTH_Proto_pad" (at 0 -2.286) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
  )
  (footprint "Connectors:PTH_Proto_pad" (layer "F.Cu")
    (tedit 60C6130C)
    (at 76.19 89.84)
    (attr through_hole board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 2.286) (layer "F.SilkS") hide)
    (fp_text value "PTH_Proto_pad" (at 0 -2.286) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
  )
  (footprint "Connectors:PTH_Proto_pad" (layer "F.Cu")
    (tedit 60C6130C)
    (at 106.67 92.38)
    (attr through_hole board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 2.286) (layer "F.SilkS") hide)
    (fp_text value "PTH_Proto_pad" (at 0 -2.286) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
  )
  (footprint "Connectors:PTH_Proto_pad" (layer "F.Cu")
    (tedit 60C6130C)
    (at 76.19 97.46)
    (attr through_hole board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 2.286) (layer "F.SilkS") hide)
    (fp_text value "PTH_Proto_pad" (at 0 -2.286) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
  )
  (footprint "Connectors:PTH_Proto_pad" (layer "F.Cu")
    (tedit 60C6130C)
    (at 58.41 100)
    (attr through_hole board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 2.286) (layer "F.SilkS") hide)
    (fp_text value "PTH_Proto_pad" (at 0 -2.286) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
  )
  (footprint "Connectors:PTH_Proto_pad" (layer "F.Cu")
    (tedit 60C6130C)
    (at 86.35 84.76)
    (attr through_hole board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 2.286) (layer "F.SilkS") hide)
    (fp_text value "PTH_Proto_pad" (at 0 -2.286) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
  )
  (footprint "Connectors:PTH_Proto_pad" (layer "F.Cu")
    (tedit 60C6130C)
    (at 73.65 94.92)
    (attr through_hole board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 2.286) (layer "F.SilkS") hide)
    (fp_text value "PTH_Proto_pad" (at 0 -2.286) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
  )
  (footprint "Connectors:PTH_Proto_pad" (layer "F.Cu")
    (tedit 60C6130C)
    (at 68.57 102.54)
    (attr through_hole board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 2.286) (layer "F.SilkS") hide)
    (fp_text value "PTH_Proto_pad" (at 0 -2.286) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
  )
  (footprint "Connectors:PTH_Proto_pad" (layer "F.Cu")
    (tedit 60C6130C)
    (at 63.49 97.46)
    (attr through_hole board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 2.286) (layer "F.SilkS") hide)
    (fp_text value "PTH_Proto_pad" (at 0 -2.286) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
  )
  (footprint "Connectors:PTH_Proto_pad" (layer "F.Cu")
    (tedit 60C6130C)
    (at 78.73 97.46)
    (attr through_hole board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 2.286) (layer "F.SilkS") hide)
    (fp_text value "PTH_Proto_pad" (at 0 -2.286) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
  )
  (footprint "Connectors:PTH_Proto_pad" (layer "F.Cu")
    (tedit 60C6130C)
    (at 53.33 89.84)
    (attr through_hole board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 2.286) (layer "F.SilkS") hide)
    (fp_text value "PTH_Proto_pad" (at 0 -2.286) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
  )
  (footprint "Connectors:PTH_Proto_pad" (layer "F.Cu")
    (tedit 60C6130C)
    (at 53.33 97.46)
    (attr through_hole board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 2.286) (layer "F.SilkS") hide)
    (fp_text value "PTH_Proto_pad" (at 0 -2.286) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
  )
  (footprint "Connectors:PTH_Proto_pad" (layer "F.Cu")
    (tedit 60C6130C)
    (at 93.97 92.38)
    (attr through_hole board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 2.286) (layer "F.SilkS") hide)
    (fp_text value "PTH_Proto_pad" (at 0 -2.286) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
  )
  (footprint "Connectors:PTH_Proto_pad" (layer "F.Cu")
    (tedit 60C6130C)
    (at 63.49 82.22)
    (attr through_hole board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 2.286) (layer "F.SilkS") hide)
    (fp_text value "PTH_Proto_pad" (at 0 -2.286) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
  )
  (footprint "Connectors:PTH_Proto_pad" (layer "F.Cu")
    (tedit 60C6130C)
    (at 76.19 82.22)
    (attr through_hole board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 2.286) (layer "F.SilkS") hide)
    (fp_text value "PTH_Proto_pad" (at 0 -2.286) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
  )
  (footprint "Connectors:PTH_Proto_pad" (layer "F.Cu")
    (tedit 60C6130C)
    (at 106.67 87.3)
    (attr through_hole board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 2.286) (layer "F.SilkS") hide)
    (fp_text value "PTH_Proto_pad" (at 0 -2.286) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
  )
  (footprint "Connectors:PTH_Proto_pad" (layer "F.Cu")
    (tedit 60C6130C)
    (at 60.95 92.38)
    (attr through_hole board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 2.286) (layer "F.SilkS") hide)
    (fp_text value "PTH_Proto_pad" (at 0 -2.286) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
  )
  (footprint "Connectors:PTH_Proto_pad" (layer "F.Cu")
    (tedit 60C6130C)
    (at 104.13 100)
    (attr through_hole board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 2.286) (layer "F.SilkS") hide)
    (fp_text value "PTH_Proto_pad" (at 0 -2.286) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
  )
  (footprint "Connectors:PTH_Proto_pad" (layer "F.Cu")
    (tedit 60C6130C)
    (at 78.73 84.76)
    (attr through_hole board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 2.286) (layer "F.SilkS") hide)
    (fp_text value "PTH_Proto_pad" (at 0 -2.286) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
  )
  (footprint "Connectors:PTH_Proto_pad" (layer "F.Cu")
    (tedit 60C6130C)
    (at 83.81 100)
    (attr through_hole board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 2.286) (layer "F.SilkS") hide)
    (fp_text value "PTH_Proto_pad" (at 0 -2.286) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
  )
  (footprint "Connectors:PTH_Proto_pad" (layer "F.Cu")
    (tedit 60C6130C)
    (at 71.11 84.76)
    (attr through_hole board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 2.286) (layer "F.SilkS") hide)
    (fp_text value "PTH_Proto_pad" (at 0 -2.286) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
  )
  (footprint "Connectors:PTH_Proto_pad" (layer "F.Cu")
    (tedit 60C6130C)
    (at 66.03 89.84)
    (attr through_hole board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 2.286) (layer "F.SilkS") hide)
    (fp_text value "PTH_Proto_pad" (at 0 -2.286) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
  )
  (footprint "Connectors:PTH_Proto_pad" (layer "F.Cu")
    (tedit 60C6130C)
    (at 66.03 82.22)
    (attr through_hole board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 2.286) (layer "F.SilkS") hide)
    (fp_text value "PTH_Proto_pad" (at 0 -2.286) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
  )
  (footprint "Connectors:PTH_Proto_pad" (layer "F.Cu")
    (tedit 60C6130C)
    (at 63.49 100)
    (attr through_hole board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 2.286) (layer "F.SilkS") hide)
    (fp_text value "PTH_Proto_pad" (at 0 -2.286) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
  )
  (footprint "Connectors:PTH_Proto_pad" (layer "F.Cu")
    (tedit 60C6130C)
    (at 68.57 89.84)
    (attr through_hole board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 2.286) (layer "F.SilkS") hide)
    (fp_text value "PTH_Proto_pad" (at 0 -2.286) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
  )
  (footprint "Connectors:PTH_Proto_pad" (layer "F.Cu")
    (tedit 60C6130C)
    (at 104.13 84.76)
    (attr through_hole board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 2.286) (layer "F.SilkS") hide)
    (fp_text value "PTH_Proto_pad" (at 0 -2.286) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
  )
  (footprint "LOGO" (layer "F.Cu")
    (tedit 615CB24C)
    (at 80 100)
    (attr board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "G***" (at 0 0) (layer "F.SilkS") hide)
    (fp_text value "LOGO" (at 0.75 0) (layer "F.SilkS") hide)
  )
  (footprint "Connectors:PTH_Proto_pad" (layer "F.Cu")
    (tedit 60C6130C)
    (at 53.33 94.92)
    (attr through_hole board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 2.286) (layer "F.SilkS") hide)
    (fp_text value "PTH_Proto_pad" (at 0 -2.286) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
  )
  (footprint "Connectors:PTH_Proto_pad" (layer "F.Cu")
    (tedit 60C6130C)
    (at 83.81 87.3)
    (attr through_hole board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 2.286) (layer "F.SilkS") hide)
    (fp_text value "PTH_Proto_pad" (at 0 -2.286) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
  )
  (footprint "Connectors:PTH_Proto_pad" (layer "F.Cu")
    (tedit 60C6130C)
    (at 81.27 84.76)
    (attr through_hole board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 2.286) (layer "F.SilkS") hide)
    (fp_text value "PTH_Proto_pad" (at 0 -2.286) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
  )
  (footprint "Connectors:PTH_Proto_pad" (layer "F.Cu")
    (tedit 60C6130C)
    (at 99.05 97.46)
    (attr through_hole board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 2.286) (layer "F.SilkS") hide)
    (fp_text value "PTH_Proto_pad" (at 0 -2.286) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
  )
  (footprint "Connectors:PTH_Proto_pad" (layer "F.Cu")
    (tedit 60C6130C)
    (at 93.97 94.92)
    (attr through_hole board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 2.286) (layer "F.SilkS") hide)
    (fp_text value "PTH_Proto_pad" (at 0 -2.286) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
  )
  (footprint "Connectors:PTH_Proto_pad" (layer "F.Cu")
    (tedit 60C6130C)
    (at 106.67 94.92)
    (attr through_hole board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 2.286) (layer "F.SilkS") hide)
    (fp_text value "PTH_Proto_pad" (at 0 -2.286) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
  )
  (footprint "Connectors:PTH_Proto_pad" (layer "F.Cu")
    (tedit 60C6130C)
    (at 86.35 97.46)
    (attr through_hole board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 2.286) (layer "F.SilkS") hide)
    (fp_text value "PTH_Proto_pad" (at 0 -2.286) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
  )
  (footprint "Connectors:PTH_Proto_pad" (layer "F.Cu")
    (tedit 60C6130C)
    (at 101.59 94.92)
    (attr through_hole board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 2.286) (layer "F.SilkS") hide)
    (fp_text value "PTH_Proto_pad" (at 0 -2.286) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
  )
  (footprint "Connectors:PTH_Proto_pad" (layer "F.Cu")
    (tedit 60C6130C)
    (at 66.03 84.76)
    (attr through_hole board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 2.286) (layer "F.SilkS") hide)
    (fp_text value "PTH_Proto_pad" (at 0 -2.286) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
  )
  (footprint "Connectors:PTH_Proto_pad" (layer "F.Cu")
    (tedit 60C6130C)
    (at 91.43 100)
    (attr through_hole board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 2.286) (layer "F.SilkS") hide)
    (fp_text value "PTH_Proto_pad" (at 0 -2.286) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
  )
  (footprint "Connectors:PTH_Proto_pad" (layer "F.Cu")
    (tedit 60C6130C)
    (at 55.87 89.84)
    (attr through_hole board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 2.286) (layer "F.SilkS") hide)
    (fp_text value "PTH_Proto_pad" (at 0 -2.286) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
  )
  (footprint "Connectors:PTH_Proto_pad" (layer "F.Cu")
    (tedit 60C6130C)
    (at 68.57 92.38)
    (attr through_hole board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 2.286) (layer "F.SilkS") hide)
    (fp_text value "PTH_Proto_pad" (at 0 -2.286) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
  )
  (footprint "Connectors:PTH_Proto_pad" (layer "F.Cu")
    (tedit 60C6130C)
    (at 78.73 89.84)
    (attr through_hole board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 2.286) (layer "F.SilkS") hide)
    (fp_text value "PTH_Proto_pad" (at 0 -2.286) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
  )
  (footprint "Connectors:PTH_Proto_pad" (layer "F.Cu")
    (tedit 60C6130C)
    (at 58.41 97.46)
    (attr through_hole board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 2.286) (layer "F.SilkS") hide)
    (fp_text value "PTH_Proto_pad" (at 0 -2.286) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
  )
  (footprint "Connectors:PTH_Proto_pad" (layer "F.Cu")
    (tedit 60C6130C)
    (at 55.87 94.92)
    (attr through_hole board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 2.286) (layer "F.SilkS") hide)
    (fp_text value "PTH_Proto_pad" (at 0 -2.286) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
  )
  (footprint "Connectors:PTH_Proto_pad" (layer "F.Cu")
    (tedit 60C6130C)
    (at 88.89 97.46)
    (attr through_hole board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 2.286) (layer "F.SilkS") hide)
    (fp_text value "PTH_Proto_pad" (at 0 -2.286) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
  )
  (footprint "Connectors:PTH_Proto_pad" (layer "F.Cu")
    (tedit 60C6130C)
    (at 106.67 82.22)
    (attr through_hole board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 2.286) (layer "F.SilkS") hide)
    (fp_text value "PTH_Proto_pad" (at 0 -2.286) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
  )
  (footprint "Connectors:PTH_Proto_pad" (layer "F.Cu")
    (tedit 60C6130C)
    (at 101.59 102.54)
    (attr through_hole board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 2.286) (layer "F.SilkS") hide)
    (fp_text value "PTH_Proto_pad" (at 0 -2.286) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
  )
  (footprint "Connectors:PTH_Proto_pad" (layer "F.Cu")
    (tedit 60C6130C)
    (at 73.65 92.38)
    (attr through_hole board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 2.286) (layer "F.SilkS") hide)
    (fp_text value "PTH_Proto_pad" (at 0 -2.286) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
  )
  (footprint "Connectors:PTH_Proto_pad" (layer "F.Cu")
    (tedit 60C6130C)
    (at 86.35 89.84)
    (attr through_hole board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 2.286) (layer "F.SilkS") hide)
    (fp_text value "PTH_Proto_pad" (at 0 -2.286) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
  )
  (footprint "Connectors:PTH_Proto_pad" (layer "F.Cu")
    (tedit 60C6130C)
    (at 96.51 84.76)
    (attr through_hole board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 2.286) (layer "F.SilkS") hide)
    (fp_text value "PTH_Proto_pad" (at 0 -2.286) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
  )
  (footprint "Connectors:PTH_Proto_pad" (layer "F.Cu")
    (tedit 60C6130C)
    (at 104.13 82.22)
    (attr through_hole board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 2.286) (layer "F.SilkS") hide)
    (fp_text value "PTH_Proto_pad" (at 0 -2.286) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
  )
  (footprint "Connectors:PTH_Proto_pad" (layer "F.Cu")
    (tedit 60C6130C)
    (at 91.43 97.46)
    (attr through_hole board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 2.286) (layer "F.SilkS") hide)
    (fp_text value "PTH_Proto_pad" (at 0 -2.286) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
  )
  (footprint "Connectors:PTH_Proto_pad" (layer "F.Cu")
    (tedit 60C6130C)
    (at 55.87 82.22)
    (attr through_hole board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 2.286) (layer "F.SilkS") hide)
    (fp_text value "PTH_Proto_pad" (at 0 -2.286) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
  )
  (footprint "Connectors:PTH_Proto_pad" (layer "F.Cu")
    (tedit 60C6130C)
    (at 60.95 94.92)
    (attr through_hole board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 2.286) (layer "F.SilkS") hide)
    (fp_text value "PTH_Proto_pad" (at 0 -2.286) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
  )
  (footprint "Connectors:PTH_Proto_pad" (layer "F.Cu")
    (tedit 60C6130C)
    (at 76.19 102.54)
    (attr through_hole board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 2.286) (layer "F.SilkS") hide)
    (fp_text value "PTH_Proto_pad" (at 0 -2.286) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
  )
  (footprint "Connectors:PTH_Proto_pad" (layer "F.Cu")
    (tedit 60C6130C)
    (at 93.97 89.84)
    (attr through_hole board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 2.286) (layer "F.SilkS") hide)
    (fp_text value "PTH_Proto_pad" (at 0 -2.286) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
  )
  (footprint "Connectors:PTH_Proto_pad" (layer "F.Cu")
    (tedit 60C6130C)
    (at 71.11 82.22)
    (attr through_hole board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 2.286) (layer "F.SilkS") hide)
    (fp_text value "PTH_Proto_pad" (at 0 -2.286) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
  )
  (footprint "Connectors:PTH_Proto_pad" (layer "F.Cu")
    (tedit 60C6130C)
    (at 83.81 89.84)
    (attr through_hole board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 2.286) (layer "F.SilkS") hide)
    (fp_text value "PTH_Proto_pad" (at 0 -2.286) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
  )
  (footprint "Connectors:PTH_Proto_pad" (layer "F.Cu")
    (tedit 60C6130C)
    (at 68.57 87.3)
    (attr through_hole board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 2.286) (layer "F.SilkS") hide)
    (fp_text value "PTH_Proto_pad" (at 0 -2.286) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
  )
  (footprint "Connectors:PTH_Proto_pad" (layer "F.Cu")
    (tedit 60C6130C)
    (at 83.81 102.54)
    (attr through_hole board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 2.286) (layer "F.SilkS") hide)
    (fp_text value "PTH_Proto_pad" (at 0 -2.286) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
  )
  (footprint "Connectors:PTH_Proto_pad" (layer "F.Cu")
    (tedit 60C6130C)
    (at 81.27 94.92)
    (attr through_hole board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 2.286) (layer "F.SilkS") hide)
    (fp_text value "PTH_Proto_pad" (at 0 -2.286) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
  )
  (footprint "Connectors:PTH_Proto_pad" (layer "F.Cu")
    (tedit 60C6130C)
    (at 63.49 89.84)
    (attr through_hole board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 2.286) (layer "F.SilkS") hide)
    (fp_text value "PTH_Proto_pad" (at 0 -2.286) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
  )
  (footprint "Connectors:PTH_Proto_pad" (layer "F.Cu")
    (tedit 60C6130C)
    (at 58.41 102.54)
    (attr through_hole board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 2.286) (layer "F.SilkS") hide)
    (fp_text value "PTH_Proto_pad" (at 0 -2.286) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
  )
  (footprint "Connectors:PTH_Proto_pad" (layer "F.Cu")
    (tedit 60C6130C)
    (at 93.97 102.54)
    (attr through_hole board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 2.286) (layer "F.SilkS") hide)
    (fp_text value "PTH_Proto_pad" (at 0 -2.286) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
  )
  (footprint "Connectors:PTH_Proto_pad" (layer "F.Cu")
    (tedit 60C6130C)
    (at 66.03 102.54)
    (attr through_hole board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 2.286) (layer "F.SilkS") hide)
    (fp_text value "PTH_Proto_pad" (at 0 -2.286) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
  )
  (footprint "Connectors:PTH_Proto_pad" (layer "F.Cu")
    (tedit 60C6130C)
    (at 73.65 82.22)
    (attr through_hole board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 2.286) (layer "F.SilkS") hide)
    (fp_text value "PTH_Proto_pad" (at 0 -2.286) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
  )
  (footprint "Connectors:PTH_Proto_pad" (layer "F.Cu")
    (tedit 60C6130C)
    (at 86.35 87.3)
    (attr through_hole board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 2.286) (layer "F.SilkS") hide)
    (fp_text value "PTH_Proto_pad" (at 0 -2.286) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
  )
  (footprint "Connectors:PTH_Proto_pad" (layer "F.Cu")
    (tedit 60C6130C)
    (at 106.67 89.84)
    (attr through_hole board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 2.286) (layer "F.SilkS") hide)
    (fp_text value "PTH_Proto_pad" (at 0 -2.286) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
  )
  (footprint "Connectors:PTH_Proto_pad" (layer "F.Cu")
    (tedit 60C6130C)
    (at 91.43 94.92)
    (attr through_hole board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 2.286) (layer "F.SilkS") hide)
    (fp_text value "PTH_Proto_pad" (at 0 -2.286) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
  )
  (footprint "Connectors:PTH_Proto_pad" (layer "F.Cu")
    (tedit 60C6130C)
    (at 63.49 87.3)
    (attr through_hole board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 2.286) (layer "F.SilkS") hide)
    (fp_text value "PTH_Proto_pad" (at 0 -2.286) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
  )
  (footprint "Connectors:PTH_Proto_pad" (layer "F.Cu")
    (tedit 60C6130C)
    (at 78.73 82.22)
    (attr through_hole board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 2.286) (layer "F.SilkS") hide)
    (fp_text value "PTH_Proto_pad" (at 0 -2.286) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
  )
  (footprint "Connectors:PTH_Proto_pad" (layer "F.Cu")
    (tedit 60C6130C)
    (at 91.43 82.22)
    (attr through_hole board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 2.286) (layer "F.SilkS") hide)
    (fp_text value "PTH_Proto_pad" (at 0 -2.286) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
  )
  (footprint "Connectors:PTH_Proto_pad" (layer "F.Cu")
    (tedit 60C6130C)
    (at 55.87 100)
    (attr through_hole board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 2.286) (layer "F.SilkS") hide)
    (fp_text value "PTH_Proto_pad" (at 0 -2.286) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
  )
  (footprint "Connectors:PTH_Proto_pad" (layer "F.Cu")
    (tedit 60C6130C)
    (at 81.27 100)
    (attr through_hole board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 2.286) (layer "F.SilkS") hide)
    (fp_text value "PTH_Proto_pad" (at 0 -2.286) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
  )
  (footprint "Connectors:PTH_Proto_pad" (layer "F.Cu")
    (tedit 60C6130C)
    (at 88.89 102.54)
    (attr through_hole board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 2.286) (layer "F.SilkS") hide)
    (fp_text value "PTH_Proto_pad" (at 0 -2.286) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
  )
  (footprint "Connectors:PTH_Proto_pad" (layer "F.Cu")
    (tedit 60C6130C)
    (at 71.11 102.54)
    (attr through_hole board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 2.286) (layer "F.SilkS") hide)
    (fp_text value "PTH_Proto_pad" (at 0 -2.286) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
  )
  (footprint "Connectors:PTH_Proto_pad" (layer "F.Cu")
    (tedit 60C6130C)
    (at 104.13 94.92)
    (attr through_hole board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 2.286) (layer "F.SilkS") hide)
    (fp_text value "PTH_Proto_pad" (at 0 -2.286) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
  )
  (footprint "Connectors:PTH_Proto_pad" (layer "F.Cu")
    (tedit 60C6130C)
    (at 96.51 89.84)
    (attr through_hole board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 2.286) (layer "F.SilkS") hide)
    (fp_text value "PTH_Proto_pad" (at 0 -2.286) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
  )
  (footprint "Connectors:PTH_Proto_pad" (layer "F.Cu")
    (tedit 60C6130C)
    (at 58.41 94.92)
    (attr through_hole board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 2.286) (layer "F.SilkS") hide)
    (fp_text value "PTH_Proto_pad" (at 0 -2.286) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
  )
  (footprint "Connectors:PTH_Proto_pad" (layer "F.Cu")
    (tedit 60C6130C)
    (at 99.05 102.54)
    (attr through_hole board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 2.286) (layer "F.SilkS") hide)
    (fp_text value "PTH_Proto_pad" (at 0 -2.286) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
  )
  (footprint "Connectors:PTH_Proto_pad" (layer "F.Cu")
    (tedit 60C6130C)
    (at 101.59 87.3)
    (attr through_hole board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 2.286) (layer "F.SilkS") hide)
    (fp_text value "PTH_Proto_pad" (at 0 -2.286) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
  )
  (footprint "Connectors:PTH_Proto_pad" (layer "F.Cu")
    (tedit 60C6130C)
    (at 66.03 97.46)
    (attr through_hole board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 2.286) (layer "F.SilkS") hide)
    (fp_text value "PTH_Proto_pad" (at 0 -2.286) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
  )
  (footprint "LOGO" (layer "F.Cu")
    (tedit 615CA29C)
    (at 80 100)
    (attr board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "G***" (at 0 0) (layer "F.SilkS") hide)
    (fp_text value "LOGO" (at 0.75 0) (layer "F.SilkS") hide)
  )
  (footprint "Connectors:PTH_Proto_pad" (layer "F.Cu")
    (tedit 60C6130C)
    (at 96.51 92.38)
    (attr through_hole board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 2.286) (layer "F.SilkS") hide)
    (fp_text value "PTH_Proto_pad" (at 0 -2.286) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
  )
  (footprint "Connectors:PTH_Proto_pad" (layer "F.Cu")
    (tedit 60C6130C)
    (at 81.27 97.46)
    (attr through_hole board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 2.286) (layer "F.SilkS") hide)
    (fp_text value "PTH_Proto_pad" (at 0 -2.286) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
  )
  (footprint "Connectors:PTH_Proto_pad" (layer "F.Cu")
    (tedit 60C6130C)
    (at 76.19 84.76)
    (attr through_hole board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 2.286) (layer "F.SilkS") hide)
    (fp_text value "PTH_Proto_pad" (at 0 -2.286) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
  )
  (footprint "Connectors:PTH_Proto_pad" (layer "F.Cu")
    (tedit 60C6130C)
    (at 68.57 84.76)
    (attr through_hole board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 2.286) (layer "F.SilkS") hide)
    (fp_text value "PTH_Proto_pad" (at 0 -2.286) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
  )
  (footprint "Connectors:PTH_Proto_pad" (layer "F.Cu")
    (tedit 60C6130C)
    (at 104.13 97.46)
    (attr through_hole board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 2.286) (layer "F.SilkS") hide)
    (fp_text value "PTH_Proto_pad" (at 0 -2.286) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
  )
  (footprint "Connectors:PTH_Proto_pad" (layer "F.Cu")
    (tedit 60C6130C)
    (at 86.35 102.54)
    (attr through_hole board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 2.286) (layer "F.SilkS") hide)
    (fp_text value "PTH_Proto_pad" (at 0 -2.286) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
  )
  (footprint "Connectors:PTH_Proto_pad" (layer "F.Cu")
    (tedit 60C6130C)
    (at 66.03 92.38)
    (attr through_hole board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 2.286) (layer "F.SilkS") hide)
    (fp_text value "PTH_Proto_pad" (at 0 -2.286) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
  )
  (footprint "Connectors:PTH_Proto_pad" (layer "F.Cu")
    (tedit 60C6130C)
    (at 96.51 102.54)
    (attr through_hole board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 2.286) (layer "F.SilkS") hide)
    (fp_text value "PTH_Proto_pad" (at 0 -2.286) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
  )
  (footprint "Connectors:PTH_Proto_pad" (layer "F.Cu")
    (tedit 60C6130C)
    (at 63.49 84.76)
    (attr through_hole board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 2.286) (layer "F.SilkS") hide)
    (fp_text value "PTH_Proto_pad" (at 0 -2.286) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
  )
  (footprint "Connectors:PTH_Proto_pad" (layer "F.Cu")
    (tedit 60C6130C)
    (at 68.57 100)
    (attr through_hole board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 2.286) (layer "F.SilkS") hide)
    (fp_text value "PTH_Proto_pad" (at 0 -2.286) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
  )
  (footprint "Connectors:PTH_Proto_pad" (layer "F.Cu")
    (tedit 60C6130C)
    (at 91.43 87.3)
    (attr through_hole board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 2.286) (layer "F.SilkS") hide)
    (fp_text value "PTH_Proto_pad" (at 0 -2.286) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
  )
  (footprint "Connectors:PTH_Proto_pad" (layer "F.Cu")
    (tedit 60C6130C)
    (at 53.33 84.76)
    (attr through_hole board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 2.286) (layer "F.SilkS") hide)
    (fp_text value "PTH_Proto_pad" (at 0 -2.286) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
  )
  (footprint "Connectors:PTH_Proto_pad" (layer "F.Cu")
    (tedit 60C6130C)
    (at 101.59 97.46)
    (attr through_hole board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 2.286) (layer "F.SilkS") hide)
    (fp_text value "PTH_Proto_pad" (at 0 -2.286) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
  )
  (footprint "Connectors:PTH_Proto_pad" (layer "F.Cu")
    (tedit 60C6130C)
    (at 91.43 102.54)
    (attr through_hole board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 2.286) (layer "F.SilkS") hide)
    (fp_text value "PTH_Proto_pad" (at 0 -2.286) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
  )
  (footprint "Connectors:PTH_Proto_pad" (layer "F.Cu")
    (tedit 60C6130C)
    (at 71.11 100)
    (attr through_hole board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 2.286) (layer "F.SilkS") hide)
    (fp_text value "PTH_Proto_pad" (at 0 -2.286) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
  )
  (footprint "Connectors:PTH_Proto_pad" (layer "F.Cu")
    (tedit 60C6130C)
    (at 91.43 84.76)
    (attr through_hole board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 2.286) (layer "F.SilkS") hide)
    (fp_text value "PTH_Proto_pad" (at 0 -2.286) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
  )
  (footprint "Connectors:PTH_Proto_pad" (layer "F.Cu")
    (tedit 60C6130C)
    (at 106.67 102.54)
    (attr through_hole board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 2.286) (layer "F.SilkS") hide)
    (fp_text value "PTH_Proto_pad" (at 0 -2.286) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
  )
  (footprint "Connectors:PTH_Proto_pad" (layer "F.Cu")
    (tedit 60C6130C)
    (at 53.33 100)
    (attr through_hole board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 2.286) (layer "F.SilkS") hide)
    (fp_text value "PTH_Proto_pad" (at 0 -2.286) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
  )
  (footprint "Connectors:PTH_Proto_pad" (layer "F.Cu")
    (tedit 60C6130C)
    (at 68.57 94.92)
    (attr through_hole board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 2.286) (layer "F.SilkS") hide)
    (fp_text value "PTH_Proto_pad" (at 0 -2.286) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
  )
  (footprint "LOGO" (layer "B.Cu")
    (tedit 6165E8D4)
    (at 80 100 180)
    (attr board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "G***" (at 0 0) (layer "B.SilkS") hide)
    (fp_text value "LOGO" (at 0.75 0) (layer "B.SilkS") hide)
  )
  (gr_curve (pts (xy 107.00001 149.999995) (xy 108.649995 149.999995) (xy 109.999999 148.649992) (xy 109.999999 146.999985)) (layer "Edge.Cuts") (width 0.2))
  (gr_curve (pts (xy 109.999999 52.999995) (xy 109.999999 51.349988) (xy 108.649995 50.000006) (xy 107.00001 50.000006)) (layer "Edge.Cuts") (width 0.2))
  (gr_curve (pts (xy 80 59.424796) (xy 78.343146 59.424796) (xy 77.000011 58.08164) (xy 77.000011 56.424786)) (layer "Edge.Cuts") (width 0.2))
  (gr_curve (pts (xy 83.00001 56.424786) (xy 83.00001 58.08164) (xy 81.656854 59.424796) (xy 80 59.424796)) (layer "Edge.Cuts") (width 0.2))
  (gr_curve (pts (xy 80 53.424796) (xy 81.656854 53.424796) (xy 83.00001 54.767932) (xy 83.00001 56.424786)) (layer "Edge.Cuts") (width 0.2))
  (gr_curve (pts (xy 50.000001 146.999985) (xy 50.000001 148.649992) (xy 51.350004 149.999995) (xy 53.000011 149.999995)) (layer "Edge.Cuts") (width 0.2))
  (gr_curve (pts (xy 50.000001 52.999995) (xy 50.000001 52.999995) (xy 50.000001 146.999985) (xy 50.000001 146.999985)) (layer "Edge.Cuts") (width 0.2))
  (gr_curve (pts (xy 107.00001 50.000006) (xy 107.00001 50.000006) (xy 53.000011 50.000006) (xy 53.000011 50.000006)) (layer "Edge.Cuts") (width 0.2))
  (gr_curve (pts (xy 77.000011 56.424786) (xy 77.000011 54.767932) (xy 78.343146 53.424796) (xy 80 53.424796)) (layer "Edge.Cuts") (width 0.2))
  (gr_curve (pts (xy 109.999999 146.999985) (xy 109.999999 146.999985) (xy 109.999999 52.999995) (xy 109.999999 52.999995)) (layer "Edge.Cuts") (width 0.2))
  (gr_curve (pts (xy 53.000011 50.000006) (xy 51.350004 50.000006) (xy 50.000001 51.349988) (xy 50.000001 52.999995)) (layer "Edge.Cuts") (width 0.2))
  (gr_curve (pts (xy 53.000011 149.999995) (xy 53.000011 149.999995) (xy 107.00001 149.999995) (xy 107.00001 149.999995)) (layer "Edge.Cuts") (width 0.2))
  (zone (net 0) (net_name "") (layers F&B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.2) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.2) (thermal_bridge_width 0.2))
    (polygon
      (pts
        (xy 110 150)
        (xy 50 150)
        (xy 50 50)
        (xy 110 50)
      )
    )
  )
)
