<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.1">
<drawing>
<board>
<plain>
<text></text>
<wire x1="0" y1="3.5" x2="0" y2="46.5" width="0" layer="20"/>
<wire x1="0" y1="46.5" x2="3.5" y2="50" width="0" layer="20" curve="-90"/>
<wire x1="3.5" y1="50" x2="80.5" y2="50" width="0" layer="20"/>
<wire x1="0" y1="3.5" x2="3.5" y2="0" width="0" layer="20" curve="90"/>
<wire x1="3.5" y1="0" x2="80.5" y2="0" width="0" layer="20"/>
<wire x1="80.5" y1="0" x2="84" y2="3.5" width="0" layer="20" curve="90"/>
<wire x1="80.5" y1="50" x2="84" y2="46.5" width="0" layer="20" curve="-90"/>
<wire x1="84" y1="46.5" x2="84" y2="3.5" width="0" layer="20"/>
<circle x="81" y="3" radius="1.3" width="0.0254" layer="20"/>
<circle x="81" y="47" radius="1.3" width="0.0254" layer="20"/>
<circle x="3" y="3" radius="1.3" width="0.0254" layer="20"/>
<text>Lora AC Dimmer v1.2</text>
<circle x="3" y="47" radius="1.3" width="0.0254" layer="20"/>
<text>www.makerfabs.com</text>
<text>U4</text>
<text>GND</text>
<text>3V3</text>
<text>RST</text>
<text>SCK</text>
<text>MISO</text>
<text>MOSI</text>
<text>RX</text>
<text>TX</text>
<text>DTR</text>
<text>3V3</text>
<text>GND</text>
<text>RFM98W 433MHz</text>
<text>RFM95W 868MHz</text>
<text>RFM95W 915MHz</text>
<text>Lin</text>
<text>Nin</text>
<text>Nout</text>
<text>Lout</text>
<wire x1="47.60090625" y1="34.40993125" x2="47.56290625" y2="15.86796875" width="0.6096" layer="20"/>
<wire x1="47.56290625" y1="15.86796875" x2="50.950896875" y2="15.86796875" width="0.6096" layer="20"/>
<wire x1="50.950896875" y1="15.86796875" x2="50.942896875" y2="34.41393125" width="0.6096" layer="20"/>
<wire x1="50.942896875" y1="34.41393125" x2="47.58490625" y2="34.41593125" width="0.6096" layer="20"/>
<wire x1="47.58490625" y1="34.41593125" x2="47.58290625" y2="34.37293125" width="0.6096" layer="20"/>
<wire x1="33.78393125" y1="24.42395" x2="42.573915625" y2="24.42395" width="0.3048" layer="20"/>
<wire x1="42.573915625" y1="24.42395" x2="42.573915625" y2="23.128953125" width="0.3048" layer="20"/>
<wire x1="42.573915625" y1="23.128953125" x2="33.75893125" y2="23.128953125" width="0.3048" layer="20"/>
<wire x1="33.75893125" y1="23.128953125" x2="33.75893125" y2="24.41495" width="0.3048" layer="20"/>
<text>Lout</text>
<text>Nout</text>
<text>Lin</text>
<text>3V3</text>
<text>GND</text>
<text>RX</text>
<text>TX</text>
<text>DTR</text>
<text>Nin</text>
<text>3V3</text>
<text>GND</text>
<text>RST</text>
<text>+</text>
<text>-</text>
<text>+</text>
<text>-</text>
<text>SCK</text>
<text>MISO</text>
<text>MOSI</text>
<wire x1="34.48493125" y1="45.383909375" x2="34.50693125" y2="45.361909375" width="0.3048" layer="20"/>
<wire x1="34.50693125" y1="45.361909375" x2="34.50693125" y2="35.898928125" width="0.3048" layer="20"/>
<wire x1="34.50693125" y1="35.898928125" x2="34.52993125" y2="35.875928125" width="0.3048" layer="20"/>
<wire x1="34.52993125" y1="35.875928125" x2="36.743925" y2="35.875928125" width="0.3048" layer="20"/>
<wire x1="36.743925" y1="35.875928125" x2="36.766925" y2="35.898928125" width="0.3048" layer="20"/>
<wire x1="36.766925" y1="35.898928125" x2="36.766925" y2="45.346909375" width="0.3048" layer="20"/>
<wire x1="36.766925" y1="45.346909375" x2="36.742925" y2="45.370909375" width="0.3048" layer="20"/>
<wire x1="36.742925" y1="45.370909375" x2="34.49593125" y2="45.370909375" width="0.3048" layer="20"/>
<text>+</text>
</plain>
<libraries>
<library name="Connector">
<packages>
<package name="4P-U-FL">
</package>
<package name="PH2.0-2P-90-DIP">
</package>
<package name="5P-2.54">
</package>
<package name="1P-100/50MIL">
</package>
</packages>
</library>
<library name="IC">
<packages>
<package name="SOT23-5">
<description>&lt;b&gt;Small Outline Transistor&lt;/b&gt;</description>
</package>
<package name="TQFP32">
<description>&lt;B&gt;Thin Plasic Quad Flat Package&lt;/B&gt; Grid 0.8 mm</description>
</package>
</packages>
</library>
<library name="Discrete">
<packages>
<package name="R0603">
</package>
<package name="0603">
<description>&lt;b&gt;0603&lt;b&gt;&lt;p&gt;</description>
</package>
<package name="LED-0603">
</package>
<package name="2P-7.62X3.56-90D">
</package>
</packages>
</library>
<library name="SmartPrj">
<packages>
<package name="RESONATOR">
</package>
</packages>
</library>
<library name="Logo">
<packages>
<package name="MAKERFABS_0.3">
</package>
<package name="HIGH-VOLTAGE-1.5">
</package>
</packages>
</library>
<library name="dragino">
<packages>
<package name="RFM92_93W">
</package>
</packages>
</library>
<library name="OPL Eagle Library">
<packages>
<package name="1X6P-2.54-8.5-BLACK-FEMALE">
</package>
</packages>
</library>
<library name="self">
<packages>
<package name="THROUGH-HOLE-9.5">
</package>
</packages>
</library>
<library name="led">
<description>&lt;b&gt;LEDs&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;&lt;br&gt;
Extended by Federico Battaglin &lt;author&gt;&amp;lt;federico.rd@fdpinternational.com&amp;gt;&lt;/author&gt; with DUOLED</description>
<packages>
<package name="LED5MM">
<description>&lt;B&gt;LED&lt;/B&gt;&lt;p&gt;
5 mm, round</description>
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="SMADIODE">
<description>&lt;b&gt;SMA Surface Mount Diode&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="rectifier">
<packages>
<package name="DBS">
<description>&lt;b&gt;Single Phase 1.0 AMP Glass Passivated Bridge Rectifier&lt;/b&gt;&lt;p&gt;
Taiwan Semiconductor Co.,Ltd. - TSC&lt;br&gt;
Source: http://www.taiwansemi.com/TSCbig5/ezcatfiles/cust/img/img/db101g.pdf</description>
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1206">
</package>
</packages>
</library>
<library name="optocoupler">
<packages>
<package name="DIL6-SMD">
<description>&lt;b&gt;DIL 6 SMD&lt;/b&gt;&lt;p&gt;
Source: http://www.fairchildsemi.com/pf/4N/4N35-M.html</description>
</package>
</packages>
</library>
<library name="triac">
<packages>
<package name="TO220AB">
<description>&lt;B&gt;TO220 AB&lt;/B&gt;&lt;p&gt;
3-lead molded horzintal</description>
</package>
</packages>
</library>
<library name="Moja Knjižnica">
<packages>
<package name="HLK-PM01">
</package>
</packages>
</library>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="EIA3528-KIT">
<description>&lt;h3&gt;EIA3528-KIT&lt;/h3&gt;
&lt;b&gt;Warning:&lt;/b&gt; This is the KIT version of this package. This package has longer pads to make hand soldering easier.&lt;br&gt;</description>
</package>
</packages>
</library>
<library name="P409CP104M275AH151">
<packages>
<package name="RES_P409CP104M275AH151_KEM">
</package>
</packages>
</library>
<library name="A9G">
<description>Generated from &lt;b&gt;Maduino Zero A9G v1.0.sch&lt;/b&gt;&lt;p&gt;
by exp-project-lbr.ulp</description>
<packages>
<package name="DISCRETE_C0512/10.18">
<description>FILM CAP 0.01UF/275V</description>
</package>
</packages>
</library>
<library name="FUSE01">
<packages>
<package name="FUSE01">
</package>
</packages>
</library>
<library name="1mytest">
<packages>
<package name="DIP5_JQC3FF">
</package>
</packages>
</library>
<library name="semicon-smd-ipc">
<description>&lt;b&gt;IPC Standard SMD Semiconductors&lt;/b&gt;&lt;p&gt;
A few devices defined according to the IPC standard.&lt;p&gt;
Based on:&lt;p&gt;
IPC-SM-782&lt;br&gt;
IRevision A, August 1993&lt;br&gt;
Includes Amendment 1, October 1996&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SOT23">
<description>&lt;b&gt;SOT-23&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="adafruit2">
<packages>
<package name="V234/12">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type V234, grid 12.5 mm</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="ANT" library="Connector" package="4P-U-FL" value="">
<attribute name="NAME"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="PWR" library="Discrete" package="LED-0603" value="GREEN">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C9" library="Discrete" package="0603" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="R2" library="Discrete" package="R0603" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="C3" library="Discrete" package="0603" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="C5" library="Discrete" package="0603" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="C8" library="Discrete" package="0603" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="RST" library="Discrete" package="2P-7.62X3.56-90D" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="Discrete" package="R0603" value="1M">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="Y1" library="SmartPrj" package="RESONATOR" value="CSTCE8M00 8MHZ">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="Discrete" package="0603" value="10uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="U8" library="IC" package="SOT23-5" value="SPX3819">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="Discrete" package="R0603" value="1K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="C2" library="Discrete" package="0603" value="10uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="C6" library="Discrete" package="0603" value="10uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="J1" library="Connector" package="PH2.0-2P-90-DIP" value="PH2.0-2P-90-DIP">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="Discrete" package="R0603" value="330R">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="U2" library="IC" package="TQFP32" value="ATMEGA328P">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$1" library="Logo" package="MAKERFABS_0.3" value=""/>
<element name="U4" library="dragino" package="RFM92_93W" value="RFM95_98W"/>
<element name="C13" library="Discrete" package="0603" value="10uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="R8" library="Discrete" package="R0603" value="100K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="J10" library="Connector" package="5P-2.54" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="ISP" library="OPL Eagle Library" package="1X6P-2.54-8.5-BLACK-FEMALE" value="CONNECTOR-HEADER-6P-3460270P1">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="R5" library="Discrete" package="R0603" value="0R">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R6" library="Discrete" package="R0603" value="0R">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R7" library="Discrete" package="R0603" value="0R">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R9" library="Discrete" package="R0603" value="0R">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R13" library="Discrete" package="R0603" value="0R">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C15" library="Discrete" package="0603" value="NC">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="C16" library="Discrete" package="0603" value="NC">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="R15" library="Discrete" package="R0603" value="330R">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="AC" library="self" package="THROUGH-HOLE-9.5" value="DBT50G-9.5-4P">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J2" library="Connector" package="1P-100/50MIL" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R22" library="Discrete" package="R0603" value="0R">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R27" library="Discrete" package="R0603" value="0R">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="STATUS" library="led" package="LED5MM" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$3" library="Logo" package="HIGH-VOLTAGE-1.5" value=""/>
<element name="B1" library="rectifier" package="DBS" value="DBLS201G">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R28" library="SparkFun-Resistors" package="1206" value="100k">
<attribute name="K" value="45K"/>
</element>
<element name="R29" library="SparkFun-Resistors" package="1206" value="100k">
<attribute name="K" value="45K"/>
</element>
<element name="OK3" library="optocoupler" package="DIL6-SMD" value="H11A1SM">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="OK2" library="optocoupler" package="DIL6-SMD" value="MOC3021">
<attribute name="OC_NEWARK" value="34C1335"/>
<attribute name="MPN" value="MOC3031SM"/>
<attribute name="MF" value="FAIRCHILD SEMICONDUCTOR"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R32" library="SparkFun-Resistors" package="1206" value="330R">
<attribute name="K" value="45K"/>
</element>
<element name="T1" library="triac" package="TO220AB" value="BT139"/>
<element name="R33" library="SparkFun-Resistors" package="1206" value="330R">
<attribute name="K" value="45K"/>
</element>
<element name="U5" library="Moja Knjižnica" package="HLK-PM01" value="AC-DCHLK01"/>
<element name="C22" library="SparkFun-Capacitors" package="EIA3528-KIT" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="AC1" library="self" package="THROUGH-HOLE-9.5" value="DBT50G-9.5-3P"/>
<element name="D2" library="adafruit" package="SMADIODE" value="SS24">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R10" library="Discrete" package="R0603" value="0R"/>
<element name="C7" library="Discrete" package="0603" value="NC">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="SNUB1" library="P409CP104M275AH151" package="RES_P409CP104M275AH151_KEM" value="100nF/150Ω">
<attribute name="COPYRIGHT" value="Copyright (C) 2018 Accelerated Designs. All rights reserved"/>
<attribute name="SOURCELIBRARY" value="Kemet_2020-05-21"/>
<attribute name="VENDOR" value="Kemet"/>
<attribute name="DATASHEET" value="https://content.kemet.com/datasheets/KEM_F3089_P409_X2_275.pdf"/>
<attribute name="VALUE" value="100nF 150Ω"/>
<attribute name="BUILT_BY" value="EMA_Cory"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="P409CP104M275AH151"/>
</element>
<element name="C23" library="A9G" package="DISCRETE_C0512/10.18" value="0.01uF"/>
<element name="F1" library="FUSE01" package="FUSE01" value="FUSE01"/>
<element name="R12" library="Discrete" package="R0603" value="100R"/>
<element name="R14" library="Discrete" package="R0603" value="10K"/>
<element name="R21" library="Discrete" package="R0603" value="10K"/>
<element name="K1" library="1mytest" package="DIP5_JQC3FF" value="JQC3FF"/>
<element name="D4" library="adafruit" package="SMADIODE" value="SS24">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R35" library="Discrete" package="R0603" value="1K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R36" library="Discrete" package="R0603" value="1K"/>
<element name="R37" library="Discrete" package="R0603" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RL1" library="Discrete" package="LED-0603" value="BLUE">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q2" library="semicon-smd-ipc" package="SOT23" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R23" library="adafruit2" package="V234/12" value="150R"/>
</elements>
<signals>
<signal name="GND">
<contactref element="ANT" pad="GND3"/>
<contactref element="ANT" pad="GND2"/>
<contactref element="ANT" pad="GND1"/>
<contactref element="C9" pad="1"/>
<contactref element="C5" pad="1"/>
<contactref element="C3" pad="1"/>
<contactref element="Y1" pad="2"/>
<contactref element="RST" pad="P$1"/>
<contactref element="C4" pad="1"/>
<contactref element="U8" pad="2"/>
<contactref element="C2" pad="1"/>
<contactref element="C6" pad="1"/>
<contactref element="PWR" pad="-"/>
<contactref element="J1" pad="2"/>
<contactref element="U2" pad="5"/>
<contactref element="U2" pad="3"/>
<contactref element="U2" pad="21"/>
<contactref element="U4" pad="8"/>
<contactref element="U4" pad="10"/>
<contactref element="U4" pad="1"/>
<contactref element="U4" pad="1"/>
<contactref element="U4" pad="8"/>
<contactref element="C13" pad="1"/>
<contactref element="J10" pad="2"/>
<contactref element="ISP" pad="2"/>
<contactref element="C15" pad="1"/>
<contactref element="C16" pad="1"/>
<contactref element="OK3" pad="4"/>
<contactref element="OK2" pad="2"/>
<contactref element="U5" pad="GND"/>
<contactref element="C22" pad="C"/>
<contactref element="C7" pad="1"/>
<contactref element="R37" pad="2"/>
<contactref element="Q2" pad="2"/>
</signal>
<signal name="A1">
<contactref element="U2" pad="24"/>
</signal>
<signal name="A0">
<contactref element="U2" pad="23"/>
</signal>
<signal name="INT1">
</signal>
<signal name="A2">
<contactref element="U2" pad="25"/>
</signal>
<signal name="A3">
<contactref element="U2" pad="26"/>
<contactref element="STATUS" pad="K"/>
</signal>
<signal name="RESET">
<contactref element="R2" pad="2"/>
<contactref element="C8" pad="2"/>
<contactref element="RST" pad="P$2"/>
<contactref element="U2" pad="29"/>
<contactref element="ISP" pad="3"/>
</signal>
<signal name="D7">
<contactref element="U2" pad="11"/>
<contactref element="R7" pad="1"/>
</signal>
<signal name="DTR">
<contactref element="C8" pad="1"/>
<contactref element="J10" pad="5"/>
</signal>
<signal name="D4">
<contactref element="U2" pad="2"/>
<contactref element="R12" pad="1"/>
</signal>
<signal name="D5">
<contactref element="U2" pad="9"/>
<contactref element="R36" pad="1"/>
</signal>
<signal name="N$27">
<contactref element="RL1" pad="-"/>
<contactref element="D4" pad="A"/>
<contactref element="K1" pad="3"/>
<contactref element="Q2" pad="3"/>
</signal>
<signal name="D10">
<contactref element="U2" pad="14"/>
<contactref element="U4" pad="5"/>
<contactref element="R8" pad="1"/>
</signal>
<signal name="D9">
<contactref element="U2" pad="13"/>
<contactref element="U4" pad="6"/>
</signal>
<signal name="D8">
<contactref element="U2" pad="12"/>
<contactref element="R9" pad="1"/>
</signal>
<signal name="AREF">
<contactref element="C5" pad="2"/>
<contactref element="U2" pad="20"/>
</signal>
<signal name="D13/SCK">
<contactref element="U2" pad="17"/>
<contactref element="U4" pad="4"/>
<contactref element="ISP" pad="4"/>
</signal>
<signal name="D6">
<contactref element="U2" pad="10"/>
<contactref element="R6" pad="1"/>
</signal>
<signal name="D11/MOSI">
<contactref element="U2" pad="15"/>
<contactref element="U4" pad="3"/>
<contactref element="ISP" pad="6"/>
</signal>
<signal name="D12/MISO">
<contactref element="U2" pad="16"/>
<contactref element="U4" pad="2"/>
<contactref element="ISP" pad="5"/>
</signal>
<signal name="XTAL1">
<contactref element="R1" pad="2"/>
<contactref element="Y1" pad="1"/>
<contactref element="U2" pad="7"/>
</signal>
<signal name="XTAL2">
<contactref element="R1" pad="1"/>
<contactref element="Y1" pad="3"/>
<contactref element="U2" pad="8"/>
</signal>
<signal name="A5/SCL">
<contactref element="U2" pad="28"/>
</signal>
<signal name="A4/SDA">
<contactref element="U2" pad="27"/>
</signal>
<signal name="D3/INT1">
<contactref element="U2" pad="1"/>
<contactref element="OK3" pad="5"/>
<contactref element="R14" pad="1"/>
</signal>
<signal name="D2/INT0">
<contactref element="U2" pad="32"/>
<contactref element="R5" pad="1"/>
</signal>
<signal name="N$24">
<contactref element="U8" pad="3"/>
<contactref element="R4" pad="2"/>
</signal>
<signal name="N$7">
<contactref element="PWR" pad="+"/>
<contactref element="R3" pad="2"/>
</signal>
<signal name="D0/RX">
<contactref element="U2" pad="30"/>
<contactref element="J10" pad="3"/>
</signal>
<signal name="D1/TX">
<contactref element="U2" pad="31"/>
<contactref element="J10" pad="4"/>
</signal>
<signal name="3V3">
<contactref element="U4" pad="13"/>
<contactref element="C13" pad="2"/>
<contactref element="R8" pad="2"/>
<contactref element="C9" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="R2" pad="1"/>
<contactref element="U8" pad="5"/>
<contactref element="C4" pad="2"/>
<contactref element="U2" pad="18"/>
<contactref element="U2" pad="4"/>
<contactref element="U2" pad="6"/>
<contactref element="J10" pad="1"/>
<contactref element="R3" pad="1"/>
<contactref element="ISP" pad="1"/>
<contactref element="R15" pad="1"/>
<contactref element="R27" pad="2"/>
<contactref element="R14" pad="2"/>
<contactref element="R21" pad="2"/>
</signal>
<signal name="DIO5">
<contactref element="U4" pad="7"/>
<contactref element="R9" pad="2"/>
</signal>
<signal name="DIO0">
<contactref element="U4" pad="14"/>
<contactref element="R5" pad="2"/>
</signal>
<signal name="DIO1">
<contactref element="U4" pad="15"/>
<contactref element="R6" pad="2"/>
</signal>
<signal name="DIO2">
<contactref element="U4" pad="16"/>
<contactref element="R7" pad="2"/>
</signal>
<signal name="ANT">
<contactref element="U4" pad="9"/>
<contactref element="C16" pad="2"/>
<contactref element="R13" pad="2"/>
</signal>
<signal name="A6">
<contactref element="U2" pad="19"/>
</signal>
<signal name="A7">
<contactref element="U2" pad="22"/>
</signal>
<signal name="VDD">
<contactref element="U8" pad="1"/>
<contactref element="R4" pad="1"/>
<contactref element="C2" pad="2"/>
<contactref element="C6" pad="2"/>
<contactref element="R27" pad="1"/>
<contactref element="D2" pad="C"/>
<contactref element="R35" pad="1"/>
<contactref element="D4" pad="C"/>
<contactref element="K1" pad="1"/>
<contactref element="J1" pad="1"/>
</signal>
<signal name="N$4">
<contactref element="R13" pad="1"/>
<contactref element="C15" pad="2"/>
<contactref element="R22" pad="2"/>
<contactref element="R10" pad="2"/>
</signal>
<signal name="N$5">
<contactref element="R15" pad="2"/>
<contactref element="STATUS" pad="A"/>
</signal>
<signal name="N$12">
<contactref element="J2" pad="1"/>
<contactref element="R22" pad="1"/>
</signal>
<signal name="N">
<contactref element="B1" pad="AC1"/>
<contactref element="AC1" pad="2"/>
<contactref element="AC" pad="1"/>
<contactref element="AC" pad="3"/>
<contactref element="U5" pad="L"/>
</signal>
<signal name="L">
<contactref element="B1" pad="AC2"/>
<contactref element="AC1" pad="3"/>
<contactref element="AC" pad="2"/>
<contactref element="F1" pad="P$2"/>
</signal>
<signal name="N$15">
<contactref element="R28" pad="1"/>
<contactref element="B1" pad="-"/>
</signal>
<signal name="N$17">
<contactref element="R29" pad="1"/>
<contactref element="B1" pad="+"/>
</signal>
<signal name="N$18">
<contactref element="R29" pad="2"/>
<contactref element="OK3" pad="1"/>
</signal>
<signal name="N$19">
<contactref element="R28" pad="2"/>
<contactref element="OK3" pad="2"/>
</signal>
<signal name="VCC">
<contactref element="U5" pad="VCC"/>
<contactref element="C22" pad="A"/>
<contactref element="D2" pad="A"/>
</signal>
<signal name="N$14">
<contactref element="OK2" pad="1"/>
<contactref element="R12" pad="2"/>
<contactref element="R21" pad="1"/>
</signal>
<signal name="N$16">
<contactref element="R32" pad="1"/>
<contactref element="OK2" pad="4"/>
</signal>
<signal name="N$21">
<contactref element="OK2" pad="6"/>
<contactref element="R33" pad="1"/>
<contactref element="T1" pad="3"/>
</signal>
<signal name="N$1">
<contactref element="R10" pad="1"/>
<contactref element="ANT" pad="D"/>
</signal>
<signal name="N$2">
<contactref element="C23" pad="P$1"/>
<contactref element="R23" pad="2"/>
</signal>
<signal name="N$3">
<contactref element="C7" pad="2"/>
<contactref element="U8" pad="4"/>
</signal>
<signal name="N$9">
<contactref element="AC1" pad="1"/>
<contactref element="T1" pad="1"/>
<contactref element="R33" pad="2"/>
<contactref element="SNUB1" pad="2"/>
<contactref element="C23" pad="P$2"/>
</signal>
<signal name="L_WIRE">
<contactref element="K1" pad="2"/>
<contactref element="U5" pad="N"/>
<contactref element="F1" pad="P$1"/>
</signal>
<signal name="N$26">
<contactref element="R35" pad="2"/>
<contactref element="RL1" pad="+"/>
</signal>
<signal name="N$28">
<contactref element="R36" pad="2"/>
<contactref element="Q2" pad="1"/>
<contactref element="R37" pad="1"/>
</signal>
<signal name="LINE">
<contactref element="R32" pad="2"/>
<contactref element="T1" pad="2"/>
<contactref element="SNUB1" pad="1"/>
<contactref element="K1" pad="5"/>
<contactref element="R23" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
