Generated by EAGLE CAM Processor 6.5.0

Drill Station Info File: D:/Proxectos/github/Cable-Test-RJ45-RJ12/Cable-Test-RJ45-RJ12.dri

 Date              : 02/03/2021 13:06:33
 Drills            : generated
 Device            : Excellon drill station

Parameter settings:

 Tolerance Drill + :  0.00 %
 Tolerance Drill - :  0.00 %
 Rotate            : no
 Mirror            : no
 Optimize          : yes
 Auto fit          : yes
 OffsetX           : 0inch
 OffsetY           : 0inch
 Layers            : Drills Holes

Drill File Info:

 Data Mode         : Absolute
 Units             : 1/10000 Inch

Drills used:

 Code  Size       used

 T01   0.0157inch     7
 T02   0.0197inch     4
 T03   0.0320inch    98
 T04   0.0350inch    28
 T05   0.0354inch    24
 T06   0.0400inch     3
 T07   0.0620inch     4
 T08   0.0750inch     2
 T09   0.1280inch     8

Total number of drills: 178

Plotfiles:

 D:/Proxectos/github/Cable-Test-RJ45-RJ12/Cable-Test-RJ45-RJ12.TXT
