(kicad_pcb (version 20211014) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (title_block
    (title "PAWESOME PET")
    (date "2020-08-12")
    (rev "1")
  )
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (41 "Cmts.User" user "User.Comments")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "pawpet_v6_r6/")
    )
  )
  (net 0 "")
  (net 1 "/SWDIO")
  (net 2 "/SWCLK")
  (net 3 "+3V3")
  (net 4 "GND")
  (net 5 "/reset")
  (net 6 "/D+")
  (net 7 "/D-")
  (net 8 "/D7")
  (net 9 "/D6")
  (net 10 "/D10")
  (net 11 "/D11")
  (net 12 "/D5")
  (net 13 "/FLASH_MISO")
  (net 14 "/FLASH_CS")
  (net 15 "/DISP_SCLK")
  (net 16 "/DISP_SI")
  (net 17 "/FLASH_SCK")
  (net 18 "/FLASH_MOSI")
  (net 19 "/D8")
  (net 20 "/A1")
  (net 21 "Net-(C1-Pad1)")
  (net 22 "Net-(LS1-Pad2)")
  (net 23 "Net-(C2-Pad2)")
  (net 24 "Net-(C3-Pad2)")
  (net 25 "/D12")
  (net 26 "/D13")
  (net 27 "/A5")
  (net 28 "/A7")
  (net 29 "unconnected-(J1-PadA8)")
  (net 30 "Net-(J1-PadA5)")
  (net 31 "unconnected-(J1-PadB8)")
  (net 32 "Net-(J1-PadA4_B9)")
  (net 33 "unconnected-(J2-Pad6)")
  (net 34 "unconnected-(J3-PadMP1)")
  (net 35 "unconnected-(J3-PadMP2)")
  (net 36 "/A0")
  (net 37 "/AREF")
  (net 38 "/A2")
  (net 39 "/A3")
  (net 40 "/A4")
  (net 41 "/D1")
  (net 42 "/D0")
  (net 43 "/MISO")
  (net 44 "/SDA")
  (net 45 "/SCL")
  (net 46 "unconnected-(U1-Pad37)")
  (net 47 "unconnected-(U1-Pad38)")
  (net 48 "/TXLED")
  (net 49 "usb_host_en")
  (net 50 "/RXLED")
  (net 51 "Net-(Q1-Pad3)")
  (net 52 "Net-(J1-PadB5)")
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 165.5787 70.2056)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "pawpet.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C1" (at 0.0213 -1.9056) (layer "F.SilkS"))
    (fp_text value "22pF" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.95 0) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 21 "Net-(C1-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.95 0) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 169.55 75.311 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "pawpet.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C3" (at 2.85 0.011) (layer "F.SilkS"))
    (fp_text value "1uF" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.95 0 180) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "GND") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.95 0 180) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 24 "Net-(C3-Pad2)") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 150.298 83)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "pawpet.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C4" (at 2.802 0) (layer "F.SilkS"))
    (fp_text value "1uF" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.95 0) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.95 0) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 150.273 78.65)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "pawpet.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C6" (at 2.827 0.05) (layer "F.SilkS"))
    (fp_text value "0.1uF" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.95 0) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.95 0) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 141.85 67.375 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "pawpet.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R1" (at 2.525 -0.05 180) (layer "F.SilkS"))
    (fp_text value "100k" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2439014634)
      (net 14 "/FLASH_CS") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2439014634)
      (net 3 "+3V3") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 173.7125 70.9)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "pawpet.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R2" (at 2.6875 -0.2) (layer "F.SilkS"))
    (fp_text value "470" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2439014634)
      (net 20 "/A1") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2439014634)
      (net 22 "Net-(LS1-Pad2)") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "pawpet:SW_SPST_PTS810_handsolder" (layer "F.Cu")
    (tedit 5F508437)
    (at 166.365 65.945 180)
    (descr "C&K Components, PTS 810 Series, Microminiature SMT Top Actuated, http://www.ckswitches.com/media/1476/pts810.pdf")
    (tags "SPST Button Switch")
    (property "Sheetfile" "pawpet.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "SW_reset1" (at -3.6 2.95) (layer "F.SilkS") hide)
    (fp_text value "reset" (at 6.165 0.045 180) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect locked (at -2.075 -1.075 180) (size 1.35 0.65) (drill (offset -0.15 0)) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "/reset") (pinfunction "1") (pintype "passive"))
    (pad "1" smd rect locked (at 2.075 -1.075 180) (size 1.35 0.65) (drill (offset 0.15 0)) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "/reset") (pinfunction "1") (pintype "passive"))
    (pad "2" smd rect locked (at 2.075 1.075 180) (size 1.35 0.65) (drill (offset 0.15 0)) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND") (pinfunction "2") (pintype "passive"))
    (pad "2" smd rect locked (at -2.075 1.075 180) (size 1.35 0.65) (drill (offset -0.15 0)) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND") (pinfunction "2") (pintype "passive"))
    (model "${KISYS3DMOD}/Button_Switch_SMD.3dshapes/SW_SPST_PTS810.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Crystal:Crystal_SMD_2012-2Pin_2.0x1.2mm" (layer "F.Cu")
    (tedit 5A0FD1B2)
    (at 161.8382 70.1548 180)
    (descr "SMD Crystal 2012/2 http://txccrystal.com/images/pdf/9ht11.pdf, 2.0x1.2mm^2 package")
    (tags "SMD SMT crystal")
    (property "Sheetfile" "pawpet.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "Y1" (at 0 1.6548) (layer "F.SilkS"))
    (fp_text value "32,768" (at 0 1.8) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect locked (at -0.7 0 180) (size 0.6 1.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 21 "Net-(C1-Pad1)") (pinfunction "1") (pintype "passive"))
    (pad "2" smd rect locked (at 0.7 0 180) (size 0.6 1.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 23 "Net-(C2-Pad2)") (pinfunction "2") (pintype "passive"))
    (model "${KISYS3DMOD}/Crystal.3dshapes/Crystal_SMD_2012-2Pin_2.0x1.2mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 154.0346 72.9742 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "pawpet.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R3" (at 0 -1.65) (layer "F.SilkS"))
    (fp_text value "100k" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2439014634)
      (net 28 "/A7") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2439014634)
      (net 51 "Net-(Q1-Pad3)") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 154.0875 70.7 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "pawpet.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R4" (at -0.0125 0.1) (layer "F.SilkS") hide)
    (fp_text value "100k" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2439014634)
      (net 4 "GND") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2439014634)
      (net 28 "/A7") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_QFP:TQFP-48-1EP_7x7mm_P0.5mm_EP5x5mm" (layer "F.Cu")
    (tedit 61FAFDE1)
    (at 160 78.35 -90)
    (descr "TQFP, 48 Pin (https://www.trinamic.com/fileadmin/assets/Products/ICs_Documents/TMC2100_datasheet_Rev1.08.pdf (page 45)), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "TQFP QFP")
    (property "Sheetfile" "pawpet.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U1" (at 0 -5.85 -90) (layer "F.SilkS") hide)
    (fp_text value "ATSAMD21G18A-A" (at 0 5.85 -90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 -90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -4.1625 -2.75 270) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 21 "Net-(C1-Pad1)") (pinfunction "PA00") (pintype "bidirectional"))
    (pad "2" smd roundrect (at -4.1625 -2.25 270) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 23 "Net-(C2-Pad2)") (pinfunction "PA01") (pintype "bidirectional"))
    (pad "3" smd roundrect (at -4.1625 -1.75 270) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 36 "/A0") (pinfunction "PA02") (pintype "bidirectional+no_connect"))
    (pad "4" smd roundrect (at -4.1625 -1.25 270) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 37 "/AREF") (pinfunction "PA03") (pintype "bidirectional+no_connect"))
    (pad "5" smd roundrect (at -4.1625 -0.75 270) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "GND") (pinfunction "GNDANA") (pintype "power_in"))
    (pad "6" smd roundrect (at -4.1625 -0.25 270) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "+3V3") (pinfunction "VDDANA") (pintype "power_in"))
    (pad "7" smd roundrect (at -4.1625 0.25 270) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 20 "/A1") (pinfunction "PB08") (pintype "bidirectional"))
    (pad "8" smd roundrect (at -4.1625 0.75 270) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 38 "/A2") (pinfunction "PB09") (pintype "bidirectional+no_connect"))
    (pad "9" smd roundrect (at -4.1625 1.25 270) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 39 "/A3") (pinfunction "PA04") (pintype "bidirectional"))
    (pad "10" smd roundrect (at -4.1625 1.75 270) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 40 "/A4") (pinfunction "PA05") (pintype "bidirectional+no_connect"))
    (pad "11" smd roundrect (at -4.1625 2.25 270) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 19 "/D8") (pinfunction "PA06") (pintype "bidirectional"))
    (pad "12" smd roundrect (at -4.1625 2.75 270) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 28 "/A7") (pinfunction "PA07") (pintype "bidirectional"))
    (pad "13" smd roundrect (at -2.75 4.1625 270) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 18 "/FLASH_MOSI") (pinfunction "PA08") (pintype "bidirectional"))
    (pad "14" smd roundrect (at -2.25 4.1625 270) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 17 "/FLASH_SCK") (pinfunction "PA09") (pintype "bidirectional"))
    (pad "15" smd roundrect (at -1.75 4.1625 270) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 41 "/D1") (pinfunction "PA10") (pintype "bidirectional"))
    (pad "16" smd roundrect (at -1.25 4.1625 270) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 42 "/D0") (pinfunction "PA11") (pintype "bidirectional+no_connect"))
    (pad "17" smd roundrect (at -0.75 4.1625 270) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "+3V3") (pinfunction "VDDIO") (pintype "power_in"))
    (pad "18" smd roundrect (at -0.25 4.1625 270) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "19" smd roundrect (at 0.25 4.1625 270) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 16 "/DISP_SI") (pinfunction "PB10") (pintype "bidirectional"))
    (pad "20" smd roundrect (at 0.75 4.1625 270) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 15 "/DISP_SCLK") (pinfunction "PB11") (pintype "bidirectional"))
    (pad "21" smd roundrect (at 1.25 4.1625 270) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 43 "/MISO") (pinfunction "PA12") (pintype "bidirectional+no_connect"))
    (pad "22" smd roundrect (at 1.75 4.1625 270) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 14 "/FLASH_CS") (pinfunction "PA13") (pintype "bidirectional"))
    (pad "23" smd roundrect (at 2.25 4.1625 270) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 13 "/FLASH_MISO") (pinfunction "PA14") (pintype "bidirectional"))
    (pad "24" smd roundrect (at 2.75 4.1625 270) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 12 "/D5") (pinfunction "PA15") (pintype "bidirectional"))
    (pad "25" smd roundrect (at 4.1625 2.75 270) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 11 "/D11") (pinfunction "PA16") (pintype "bidirectional"))
    (pad "26" smd roundrect (at 4.1625 2.25 270) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 26 "/D13") (pinfunction "PA17") (pintype "bidirectional"))
    (pad "27" smd roundrect (at 4.1625 1.75 270) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 10 "/D10") (pinfunction "PA18") (pintype "bidirectional"))
    (pad "28" smd roundrect (at 4.1625 1.25 270) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 25 "/D12") (pinfunction "PA19") (pintype "bidirectional"))
    (pad "29" smd roundrect (at 4.1625 0.75 270) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 9 "/D6") (pinfunction "PA20") (pintype "bidirectional"))
    (pad "30" smd roundrect (at 4.1625 0.25 270) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 8 "/D7") (pinfunction "PA21") (pintype "bidirectional"))
    (pad "31" smd roundrect (at 4.1625 -0.25 270) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 44 "/SDA") (pinfunction "PA22") (pintype "bidirectional+no_connect"))
    (pad "32" smd roundrect (at 4.1625 -0.75 270) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 45 "/SCL") (pinfunction "PA23") (pintype "bidirectional+no_connect"))
    (pad "33" smd roundrect (at 4.1625 -1.25 270) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 7 "/D-") (pinfunction "PA24") (pintype "bidirectional"))
    (pad "34" smd roundrect (at 4.1625 -1.75 270) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 6 "/D+") (pinfunction "PA25") (pintype "bidirectional"))
    (pad "35" smd roundrect (at 4.1625 -2.25 270) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "GND") (pinfunction "GND") (pintype "passive"))
    (pad "36" smd roundrect (at 4.1625 -2.75 270) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "+3V3") (pinfunction "VDDIO") (pintype "power_in"))
    (pad "37" smd roundrect (at 2.75 -4.1625 270) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 46 "unconnected-(U1-Pad37)") (pinfunction "PB22") (pintype "bidirectional+no_connect"))
    (pad "38" smd roundrect (at 2.25 -4.1625 270) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 47 "unconnected-(U1-Pad38)") (pinfunction "PB23") (pintype "bidirectional+no_connect"))
    (pad "39" smd roundrect (at 1.75 -4.1625 270) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 48 "/TXLED") (pinfunction "PA27") (pintype "bidirectional+no_connect"))
    (pad "40" smd roundrect (at 1.25 -4.1625 270) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "/reset") (pinfunction "~{RESET}") (pintype "input"))
    (pad "41" smd roundrect (at 0.75 -4.1625 270) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 49 "usb_host_en") (pinfunction "PA28") (pintype "bidirectional+no_connect"))
    (pad "42" smd roundrect (at 0.25 -4.1625 270) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "GND") (pinfunction "GND") (pintype "passive"))
    (pad "43" smd roundrect (at -0.25 -4.1625 270) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 24 "Net-(C3-Pad2)") (pinfunction "VDDCORE") (pintype "power_out"))
    (pad "44" smd roundrect (at -0.75 -4.1625 270) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "+3V3") (pinfunction "VDDIN") (pintype "power_in"))
    (pad "45" smd roundrect (at -1.25 -4.1625 270) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "/SWCLK") (pinfunction "PA30") (pintype "bidirectional"))
    (pad "46" smd roundrect (at -1.75 -4.1625 270) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "/SWDIO") (pinfunction "PA31") (pintype "bidirectional"))
    (pad "47" smd roundrect (at -2.25 -4.1625 270) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 27 "/A5") (pinfunction "PB02") (pintype "bidirectional"))
    (pad "48" smd roundrect (at -2.75 -4.1625 270) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 50 "/RXLED") (pinfunction "PB03") (pintype "bidirectional+no_connect"))
    (pad "49" smd rect (at 0 0 270) (size 5 5) (layers "F.Cu" "F.Mask")
      (net 4 "GND") (pinfunction "GNDT") (pintype "input"))
    (model "${KICAD6_3DMODEL_DIR}/Package_QFP.3dshapes/TQFP-48-1EP_7x7mm_P0.5mm_EP5x5mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 150.298 80.85)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "pawpet.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C5" (at 2.702 -0.05) (layer "F.SilkS"))
    (fp_text value "1uF" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.95 0) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.95 0) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_SO:SOIC-8_5.23x5.23mm_P1.27mm" (layer "F.Cu")
    (tedit 5D9F72B1)
    (at 147.5 68.125)
    (descr "SOIC, 8 Pin (http://www.winbond.com/resource-files/w25q32jv%20revg%2003272018%20plus.pdf#page=68), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (property "Sheetfile" "pawpet.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U3" (at 0 -3.56) (layer "F.SilkS"))
    (fp_text value "MX25R1635FM1IL0" (at 0 3.56) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -3.6 -1.905) (size 1.6 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 14 "/FLASH_CS") (pinfunction "~{CS}") (pintype "input"))
    (pad "2" smd roundrect (at -3.6 -0.635) (size 1.6 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 13 "/FLASH_MISO") (pinfunction "SO/SIO1") (pintype "bidirectional"))
    (pad "3" smd roundrect (at -3.6 0.635) (size 1.6 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "+3V3") (pinfunction "~{WP}/SIO2") (pintype "bidirectional"))
    (pad "4" smd roundrect (at -3.6 1.905) (size 1.6 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "5" smd roundrect (at 3.6 1.905) (size 1.6 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 18 "/FLASH_MOSI") (pinfunction "SI/SIO0") (pintype "bidirectional"))
    (pad "6" smd roundrect (at 3.6 0.635) (size 1.6 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 17 "/FLASH_SCK") (pinfunction "SCLK") (pintype "input"))
    (pad "7" smd roundrect (at 3.6 -0.635) (size 1.6 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "+3V3") (pinfunction "~{HOLD}/SIO3") (pintype "bidirectional"))
    (pad "8" smd roundrect (at 3.6 -1.905) (size 1.6 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "+3V3") (pinfunction "VCC") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-8_5.23x5.23mm_P1.27mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "molex:Molex-52892-1033-Manufacturer_Recommended" (layer "F.Cu")
    (tedit 5EF2118E)
    (at 144.4 77.7 -90)
    (property "Sheetfile" "pawpet.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J3" (at -6.800004 -3.450002 -90) (layer "F.SilkS"))
    (fp_text value "MOLEX" (at 0 0 -90) (layer "F.SilkS"))
    (pad "1" smd rect locked (at -2.250001 -1.575001 270) (size 0.299999 1.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "/DISP_SCLK") (pinfunction "1") (pintype "passive"))
    (pad "2" smd rect locked (at -1.750002 -1.575001 270) (size 0.299999 1.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 16 "/DISP_SI") (pinfunction "2") (pintype "passive"))
    (pad "3" smd rect locked (at -1.250003 -1.575001 270) (size 0.299999 1.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 19 "/D8") (pinfunction "3") (pintype "passive"))
    (pad "4" smd rect locked (at -0.750001 -1.575001 270) (size 0.299999 1.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 41 "/D1") (pinfunction "4") (pintype "passive"))
    (pad "5" smd rect locked (at -0.250002 -1.575001 270) (size 0.299999 1.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "+3V3") (pinfunction "5") (pintype "passive"))
    (pad "6" smd rect locked (at 0.249997 -1.575001 270) (size 0.299999 1.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "+3V3") (pinfunction "6") (pintype "passive"))
    (pad "7" smd rect locked (at 0.749999 -1.575001 270) (size 0.299999 1.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "+3V3") (pinfunction "7") (pintype "passive"))
    (pad "8" smd rect locked (at 1.249998 -1.575001 270) (size 0.299999 1.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "+3V3") (pinfunction "8") (pintype "passive"))
    (pad "9" smd rect locked (at 1.749996 -1.575001 270) (size 0.299999 1.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND") (pinfunction "9") (pintype "passive"))
    (pad "10" smd rect locked (at 2.249996 -1.575001 270) (size 0.299999 1.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND") (pinfunction "10") (pintype "passive"))
    (pad "MP1" smd rect locked (at -4.9 1.574998 270) (size 1.599999 2.200001) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 34 "unconnected-(J3-PadMP1)") (pinfunction "MP1") (pintype "passive+no_connect"))
    (pad "MP2" smd rect locked (at 4.9 1.574998 270) (size 1.599999 2.200001) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "unconnected-(J3-PadMP2)") (pinfunction "MP2") (pintype "passive+no_connect"))
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 158.0935 70.231)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "pawpet.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C2" (at 0 -1.68) (layer "F.SilkS"))
    (fp_text value "22pF" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.95 0) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "GND") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.95 0) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 23 "Net-(C2-Pad2)") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "pawpet:BAT_BC2AAAPC" (layer "F.Cu")
    (tedit 61F0CC49)
    (at 156.926 96.647)
    (property "Sheetfile" "pawpet.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "BT1" (at 0 -14.4) (layer "F.SilkS") hide)
    (fp_text value "Battery" (at 0.4 13.995) (layer "F.Fab"))
    (fp_text user "-" (at -23.6 0.495) (layer "F.SilkS"))
    (fp_text user "+" (at 24.4 0.495) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at -23.205 -5.69) (size 1.755 1.755) (drill 1.17) (layers *.Cu *.Mask)
      (net 3 "+3V3") (pinfunction "+") (pintype "passive"))
    (pad "2" thru_hole circle (at -23.205 5.69) (size 1.755 1.755) (drill 1.17) (layers *.Cu *.Mask)
      (net 4 "GND") (pinfunction "-") (pintype "passive"))
  )
  (footprint "pawpet:MountingHole_2.7mm_M2.5_ISO14580_insert-edge" locked (layer "F.Cu")
    (tedit 61FAFE39)
    (at 180.55 66.55 180)
    (descr "Mounting Hole 2.7mm, no annular, M2.5, ISO14580")
    (tags "mounting hole 2.7mm no annular m2.5 iso14580")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 -3.25) (layer "F.SilkS") hide)
    (fp_text value "M2.7mm" (at 0 3.25) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0.3 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle locked (at 0 0 180) (size 2.7 2.7) (drill 2.7) (layers F&B.Cu *.Mask))
  )
  (footprint "pawpet:MountingHole_2.7mm_M2.5_ISO14580_insert-edge" locked (layer "F.Cu")
    (tedit 61ED4DD8)
    (at 157.2 113.25 90)
    (descr "Mounting Hole 2.7mm, no annular, M2.5, ISO14580")
    (tags "mounting hole 2.7mm no annular m2.5 iso14580")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 -3.25 90) (layer "F.SilkS") hide)
    (fp_text value "M2.7mm" (at 0 3.25 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0.3 0 90) (layer "F.Fab"))
    (pad "" np_thru_hole circle locked (at 0 0 90) (size 2.7 2.7) (drill 2.7) (layers *.Cu *.Mask))
  )
  (footprint "pawpet:kicad-drawing" locked (layer "F.Cu")
    (tedit 0)
    (at 135.394947 112.825353)
    (attr through_hole)
    (fp_text reference "Ref**" (at 0.55 -0.6) (layer "F.SilkS") hide)
    (fp_text value "Val**" (at 0 0) (layer "F.SilkS") hide)
  )
  (footprint "Connector:Tag-Connect_TC2030-IDC-NL_2x03_P1.27mm_Vertical" (layer "F.Cu")
    (tedit 5A29CEA9)
    (at 172.93 65.844 180)
    (descr "Tag-Connect programming header; http://www.tag-connect.com/Materials/TC2030-IDC-NL.pdf")
    (tags "tag connect programming header pogo pins")
    (property "Sheetfile" "pawpet.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "J2" (at 0 2.7) (layer "F.SilkS") hide)
    (fp_text value "Conn_ARM_JTAG_SWD_10" (at 0 -2.3) (layer "F.Fab"))
    (fp_text user "KEEPOUT" (at 0 0) (layer "Cmts.User"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 2.54 -1.016 180) (size 0.9906 0.9906) (drill 0.9906) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -2.54 0 180) (size 0.9906 0.9906) (drill 0.9906) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 2.54 1.016 180) (size 0.9906 0.9906) (drill 0.9906) (layers *.Cu *.Mask))
    (pad "1" connect circle (at -1.27 0.635 180) (size 0.7874 0.7874) (layers "F.Cu" "F.Mask")
      (net 3 "+3V3") (pinfunction "VTref") (pintype "power_in"))
    (pad "2" connect circle (at -1.27 -0.635 180) (size 0.7874 0.7874) (layers "F.Cu" "F.Mask")
      (net 1 "/SWDIO") (pinfunction "SWDIO/TMS") (pintype "bidirectional"))
    (pad "3" connect circle (at 0 0.635 180) (size 0.7874 0.7874) (layers "F.Cu" "F.Mask")
      (net 4 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "4" connect circle (at 0 -0.635 180) (size 0.7874 0.7874) (layers "F.Cu" "F.Mask")
      (net 2 "/SWCLK") (pinfunction "SWDCLK/TCK") (pintype "output"))
    (pad "5" connect circle (at 1.27 0.635 180) (size 0.7874 0.7874) (layers "F.Cu" "F.Mask")
      (net 4 "GND") (pinfunction "GND") (pintype "passive"))
    (pad "6" connect circle (at 1.27 -0.635 180) (size 0.7874 0.7874) (layers "F.Cu" "F.Mask")
      (net 33 "unconnected-(J2-Pad6)") (pinfunction "SWO/TDO") (pintype "input+no_connect"))
  )
  (footprint "gct:GCT_USB4105-GF-A" (layer "F.Cu")
    (tedit 61A882A1)
    (at 181.864 77.4446 90)
    (property "MANUFACTURER" "GCT")
    (property "MAXIMUM_PACKAGE_HEIGHT" "3.31 mm")
    (property "PARTREV" "A3")
    (property "STANDARD" "Manufacturer Recommendations")
    (property "Sheetfile" "pawpet.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J1" (at 0.0762 -0.1016 90) (layer "F.SilkS") hide)
    (fp_text value "USB4105-GF-A" (at 5.16 -6.635 90) (layer "F.Fab"))
    (fp_text user "PCB-EDGE" (at 5.4 2.5 90) (layer "F.Fab"))
    (pad "" np_thru_hole circle locked (at 2.89 -3.68 90) (size 0.65 0.65) (drill 0.65) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle locked (at -2.89 -3.68 90) (size 0.65 0.65) (drill 0.65) (layers *.Cu *.Mask))
    (pad "A1_B12" smd rect locked (at -3.2 -4.755 90) (size 0.6 1.15) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "A4_B9" smd rect locked (at -2.4 -4.755 90) (size 0.6 1.15) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 32 "Net-(J1-PadA4_B9)") (pinfunction "VBUS") (pintype "power_in"))
    (pad "A5" smd rect locked (at -1.25 -4.755 90) (size 0.3 1.15) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 30 "Net-(J1-PadA5)") (pinfunction "CC1") (pintype "bidirectional"))
    (pad "A6" smd rect locked (at -0.25 -4.755 90) (size 0.3 1.15) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 6 "/D+") (pinfunction "DP1") (pintype "bidirectional"))
    (pad "A7" smd rect locked (at 0.25 -4.755 90) (size 0.3 1.15) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 7 "/D-") (pinfunction "DN1") (pintype "bidirectional"))
    (pad "A8" smd rect locked (at 1.25 -4.755 90) (size 0.3 1.15) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 29 "unconnected-(J1-PadA8)") (pinfunction "SBU1") (pintype "bidirectional+no_connect"))
    (pad "B1_A12" smd rect locked (at 3.2 -4.755 90) (size 0.6 1.15) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "B4_A9" smd rect locked (at 2.4 -4.755 90) (size 0.6 1.15) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 32 "Net-(J1-PadA4_B9)") (pinfunction "VBUS") (pintype "power_in"))
    (pad "B5" smd rect locked (at 1.75 -4.755 90) (size 0.3 1.15) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 52 "Net-(J1-PadB5)") (pinfunction "CC2") (pintype "bidirectional"))
    (pad "B6" smd rect locked (at 0.75 -4.755 90) (size 0.3 1.15) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 6 "/D+") (pinfunction "DP2") (pintype "bidirectional"))
    (pad "B7" smd rect locked (at -0.75 -4.755 90) (size 0.3 1.15) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 7 "/D-") (pinfunction "DN2") (pintype "bidirectional"))
    (pad "B8" smd rect locked (at -1.75 -4.755 90) (size 0.3 1.15) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 31 "unconnected-(J1-PadB8)") (pinfunction "SBU2") (pintype "bidirectional+no_connect"))
    (pad "S1" thru_hole oval locked (at -4.32 -4.18 90) (size 1.05 2.1) (drill oval 0.6 1.7) (layers *.Cu *.Mask)
      (net 4 "GND") (pinfunction "SHELL_GND") (pintype "power_in"))
    (pad "S2" thru_hole oval locked (at -4.32 0 90) (size 1 2) (drill oval 0.6 1.4) (layers *.Cu *.Mask)
      (net 4 "GND") (pinfunction "SHELL_GND") (pintype "power_in"))
    (pad "S3" thru_hole oval locked (at 4.32 0 90) (size 1 2) (drill oval 0.6 1.4) (layers *.Cu *.Mask)
      (net 4 "GND") (pinfunction "SHELL_GND") (pintype "power_in"))
    (pad "S4" thru_hole oval locked (at 4.32 -4.18 90) (size 1.05 2.1) (drill oval 0.6 1.7) (layers *.Cu *.Mask)
      (net 4 "GND") (pinfunction "SHELL_GND") (pintype "power_in"))
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 173.7125 73.1 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "pawpet.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R5" (at -2.5875 0) (layer "F.SilkS") hide)
    (fp_text value "5.1k" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2439014634)
      (net 30 "Net-(J1-PadA5)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2439014634)
      (net 4 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 169.55 77.5208 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "pawpet.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C8" (at 2.85 0.1208) (layer "F.SilkS"))
    (fp_text value "10uF" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.95 0 180) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.95 0 180) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 169.55 73.1)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "pawpet.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C9" (at -2.85 0) (layer "F.SilkS"))
    (fp_text value "10uF" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.95 0) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.95 0) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23" (layer "F.Cu")
    (tedit 5A02FF57)
    (at 150.3426 72.6186)
    (descr "SOT-23, Standard")
    (tags "SOT-23")
    (property "Sheetfile" "pawpet.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "Q1" (at 0 -2.5) (layer "F.SilkS") hide)
    (fp_text value "DMG2301L" (at 0 2.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd rect locked (at -1 -0.95) (size 0.9 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 39 "/A3") (pinfunction "G") (pintype "input"))
    (pad "2" smd rect locked (at -1 0.95) (size 0.9 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "+3V3") (pinfunction "S") (pintype "passive"))
    (pad "3" smd rect locked (at 1 0) (size 0.9 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 51 "Net-(Q1-Pad3)") (pinfunction "D") (pintype "passive"))
    (model "${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 154.1125 68.3 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "pawpet.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R6" (at 0 1.7) (layer "F.SilkS"))
    (fp_text value "100k" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2439014634)
      (net 39 "/A3") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2439014634)
      (net 3 "+3V3") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 173.7125 77.5 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "pawpet.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R7" (at 0 -1.65) (layer "F.SilkS"))
    (fp_text value "1k" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2439014634)
      (net 32 "Net-(J1-PadA4_B9)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2439014634)
      (net 4 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 173.7125 75.311 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "pawpet.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R8" (at -2.6875 0.111) (layer "F.SilkS") hide)
    (fp_text value "5.1k" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2439014634)
      (net 52 "Net-(J1-PadB5)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2439014634)
      (net 4 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "pawpet:MountingHole_2.7mm_M2.5_ISO14580_insert-edge" locked (layer "F.Cu")
    (tedit 61ED4D98)
    (at 133.8453 66.5353)
    (descr "Mounting Hole 2.7mm, no annular, M2.5, ISO14580")
    (tags "mounting hole 2.7mm no annular m2.5 iso14580")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 -3.25 90) (layer "F.SilkS") hide)
    (fp_text value "M2.7mm" (at 0 3.25) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0.3 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle locked (at 0 0) (size 2.7 2.7) (drill 2.7) (layers *.Cu *.Mask))
  )
  (footprint "TestPoint:TestPoint_Pad_1.0x1.0mm" (layer "F.Cu")
    (tedit 5A0F774F)
    (at 139.3 71)
    (descr "SMD rectangular pad as test Point, square 1.0mm side length")
    (tags "test point SMD pad rectangle square")
    (property "Sheetfile" "pawpet.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "TP1" (at 0 -1.448) (layer "F.SilkS") hide)
    (fp_text value "TestPoint_Small" (at 0 1.55) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -1.45) (layer "F.Fab"))
    (pad "1" smd rect (at 0 0) (size 1 1) (layers "F.Cu" "F.Mask")
      (net 41 "/D1") (pinfunction "1") (pintype "passive"))
  )
  (footprint "Buzzer_Beeper:Buzzer_Murata_PKMCS0909E4000-R1" locked (layer "B.Cu")
    (tedit 5A030281)
    (at 176.53 77.597 180)
    (descr "Murata Buzzer http://www.murata.com/en-us/api/pdfdownloadapi?cate=&partno=PKMCS0909E4000-R1")
    (tags "Murata Buzzer Beeper")
    (property "Sheetfile" "pawpet.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "LS1" (at -0.1 -0.05) (layer "B.SilkS") hide)
    (fp_text value "beep" (at 0 -5.5) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd rect locked (at -4.35 0 180) (size 1.3 3.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND") (pinfunction "1") (pintype "input"))
    (pad "2" smd rect locked (at 4.35 0 180) (size 1.3 3.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 22 "Net-(LS1-Pad2)") (pinfunction "2") (pintype "input"))
    (model "${KISYS3DMOD}/Buzzer_Beeper.3dshapes/Buzzer_Murata_PKMCS0909E4000-R1.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "pawpet:Sharp_128x128_LS013B7DH03" locked (layer "B.Cu")
    (tedit 61F0C8F3)
    (at 134.1 77.9 -90)
    (attr through_hole)
    (fp_text reference "hello i am smol" (at 15 -22.9 unlocked) (layer "B.SilkS"))
    (fp_text value "Sharp_128x128_LS013B7DH03" (at -0.3 -7.4 90) (layer "B.Fab"))
    (fp_text user "128x128 display area" (at -1 -24 90) (layer "B.Fab"))
    (fp_text user "Foldable FPC " (at 0.05 -3.85 90) (layer "B.Fab"))
    (fp_text user "PCB EDGE" (at 0.1 -0.9 90) (layer "B.Fab"))
  )
  (footprint "Button_Switch_SMD:SW_SPST_EVQQ2" (layer "B.Cu")
    (tedit 5872491A)
    (at 177.8 104 -90)
    (descr "Light Touch Switch, https://industrial.panasonic.com/cdbs/www-data/pdf/ATK0000/ATK0000CE28.pdf")
    (property "Sheetfile" "pawpet.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "SW_LEFT1" (at 0.05 3.95 90) (layer "B.SilkS") hide)
    (fp_text value "SW_Push" (at 0 -4.25 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0.05 3.95 90) (layer "B.Fab"))
    (pad "1" smd rect locked (at 3.4 2 270) (size 3.2 1) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND") (pinfunction "1") (pintype "passive"))
    (pad "1" smd rect locked (at -3.4 2 270) (size 3.2 1) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND") (pinfunction "1") (pintype "passive"))
    (pad "2" smd rect locked (at 3.4 -2 270) (size 3.2 1) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 8 "/D7") (pinfunction "2") (pintype "passive"))
    (pad "2" smd rect locked (at -3.4 -2 270) (size 3.2 1) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 8 "/D7") (pinfunction "2") (pintype "passive"))
    (model "${KISYS3DMOD}/Button_Switch_SMD.3dshapes/SW_SPST_EVQQ2.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Button_Switch_SMD:SW_SPST_EVQQ2" (layer "B.Cu")
    (tedit 5872491A)
    (at 149.63 108.013 -135)
    (descr "Light Touch Switch, https://industrial.panasonic.com/cdbs/www-data/pdf/ATK0000/ATK0000CE28.pdf")
    (property "Sheetfile" "pawpet.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "SW_A1" (at 0.05 3.95 45) (layer "B.SilkS") hide)
    (fp_text value "SW_Push" (at 0 -4.25 45) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0.05 3.95 45) (layer "B.Fab"))
    (pad "1" smd rect locked (at 3.4 2 225) (size 3.2 1) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND") (pinfunction "1") (pintype "passive"))
    (pad "1" smd rect locked (at -3.4 2 225) (size 3.2 1) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND") (pinfunction "1") (pintype "passive"))
    (pad "2" smd rect locked (at 3.4 -2 225) (size 3.2 1) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 10 "/D10") (pinfunction "2") (pintype "passive"))
    (pad "2" smd rect locked (at -3.4 -2 225) (size 3.2 1) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 10 "/D10") (pinfunction "2") (pintype "passive"))
    (model "${KISYS3DMOD}/Button_Switch_SMD.3dshapes/SW_SPST_EVQQ2.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Button_Switch_SMD:SW_SPST_EVQQ2" (layer "B.Cu")
    (tedit 5872491A)
    (at 171.13 110.704 180)
    (descr "Light Touch Switch, https://industrial.panasonic.com/cdbs/www-data/pdf/ATK0000/ATK0000CE28.pdf")
    (property "Sheetfile" "pawpet.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "SW_DOWN1" (at 0.05 3.95) (layer "B.SilkS") hide)
    (fp_text value "SW_Push" (at 0 -4.25) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0.05 3.95) (layer "B.Fab"))
    (pad "1" smd rect locked (at -3.4 2 180) (size 3.2 1) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND") (pinfunction "1") (pintype "passive"))
    (pad "1" smd rect locked (at 3.4 2 180) (size 3.2 1) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND") (pinfunction "1") (pintype "passive"))
    (pad "2" smd rect locked (at -3.4 -2 180) (size 3.2 1) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 25 "/D12") (pinfunction "2") (pintype "passive"))
    (pad "2" smd rect locked (at 3.4 -2 180) (size 3.2 1) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 25 "/D12") (pinfunction "2") (pintype "passive"))
    (model "${KISYS3DMOD}/Button_Switch_SMD.3dshapes/SW_SPST_EVQQ2.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Button_Switch_SMD:SW_SPST_EVQQ2" (layer "B.Cu")
    (tedit 5872491A)
    (at 139.39 108.124 135)
    (descr "Light Touch Switch, https://industrial.panasonic.com/cdbs/www-data/pdf/ATK0000/ATK0000CE28.pdf")
    (property "Sheetfile" "pawpet.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "SW_P1" (at 0.05 3.95 135) (layer "B.SilkS") hide)
    (fp_text value "SW_Push" (at 0 -4.25 135) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0.05 3.95 135) (layer "B.Fab"))
    (pad "1" smd rect locked (at 3.4 2 135) (size 3.2 1) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND") (pinfunction "1") (pintype "passive"))
    (pad "1" smd rect locked (at -3.4 2 135) (size 3.2 1) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND") (pinfunction "1") (pintype "passive"))
    (pad "2" smd rect locked (at 3.4 -2 135) (size 3.2 1) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 11 "/D11") (pinfunction "2") (pintype "passive"))
    (pad "2" smd rect locked (at -3.4 -2 135) (size 3.2 1) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 11 "/D11") (pinfunction "2") (pintype "passive"))
    (model "${KISYS3DMOD}/Button_Switch_SMD.3dshapes/SW_SPST_EVQQ2.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Button_Switch_SMD:SW_SPST_EVQQ2" (layer "B.Cu")
    (tedit 5872491A)
    (at 171.13 97.3)
    (descr "Light Touch Switch, https://industrial.panasonic.com/cdbs/www-data/pdf/ATK0000/ATK0000CE28.pdf")
    (property "Sheetfile" "pawpet.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "SW_UP1" (at 0.05 3.95) (layer "B.SilkS") hide)
    (fp_text value "SW_Push" (at 0 -4.25) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0.05 3.95) (layer "B.Fab"))
    (pad "1" smd rect locked (at 3.4 2) (size 3.2 1) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND") (pinfunction "1") (pintype "passive"))
    (pad "1" smd rect locked (at -3.4 2) (size 3.2 1) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND") (pinfunction "1") (pintype "passive"))
    (pad "2" smd rect locked (at -3.4 -2) (size 3.2 1) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 27 "/A5") (pinfunction "2") (pintype "passive"))
    (pad "2" smd rect locked (at 3.4 -2) (size 3.2 1) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 27 "/A5") (pinfunction "2") (pintype "passive"))
    (model "${KISYS3DMOD}/Button_Switch_SMD.3dshapes/SW_SPST_EVQQ2.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Button_Switch_SMD:SW_SPST_EVQQ2" (layer "B.Cu")
    (tedit 5872491A)
    (at 147.97 99.6 -45)
    (descr "Light Touch Switch, https://industrial.panasonic.com/cdbs/www-data/pdf/ATK0000/ATK0000CE28.pdf")
    (property "Sheetfile" "pawpet.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "SW_B1" (at 0.05 3.95 135) (layer "B.SilkS") hide)
    (fp_text value "SW_Push" (at 0 -4.25 135) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0.05 3.95 135) (layer "B.Fab"))
    (pad "1" smd rect locked (at -3.4 2 315) (size 3.2 1) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND") (pinfunction "1") (pintype "passive"))
    (pad "1" smd rect locked (at 3.4 2 315) (size 3.2 1) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND") (pinfunction "1") (pintype "passive"))
    (pad "2" smd rect locked (at -3.4 -2 315) (size 3.2 1) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 26 "/D13") (pinfunction "2") (pintype "passive"))
    (pad "2" smd rect locked (at 3.4 -2 315) (size 3.2 1) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 26 "/D13") (pinfunction "2") (pintype "passive"))
    (model "${KISYS3DMOD}/Button_Switch_SMD.3dshapes/SW_SPST_EVQQ2.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Button_Switch_SMD:SW_SPST_EVQQ2" (layer "B.Cu")
    (tedit 5872491A)
    (at 139.5 98.05 45)
    (descr "Light Touch Switch, https://industrial.panasonic.com/cdbs/www-data/pdf/ATK0000/ATK0000CE28.pdf")
    (property "Sheetfile" "pawpet.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "SW_C1" (at 0.05 3.95 45) (layer "B.SilkS") hide)
    (fp_text value "SW_Push" (at 0 -4.25 45) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0.05 3.95 225) (layer "B.Fab"))
    (pad "1" smd rect locked (at -3.4 2 45) (size 3.2 1) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND") (pinfunction "1") (pintype "passive"))
    (pad "1" smd rect locked (at 3.4 2 45) (size 3.2 1) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND") (pinfunction "1") (pintype "passive"))
    (pad "2" smd rect locked (at -3.4 -2 45) (size 3.2 1) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "/D5") (pinfunction "2") (pintype "passive"))
    (pad "2" smd rect locked (at 3.4 -2 45) (size 3.2 1) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "/D5") (pinfunction "2") (pintype "passive"))
    (model "${KISYS3DMOD}/Button_Switch_SMD.3dshapes/SW_SPST_EVQQ2.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model "${KISYS3DMOD}/Button_Switch_SMD.3dshapes/SW_SPST_PTS645.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Button_Switch_SMD:SW_SPST_EVQQ2" (layer "B.Cu")
    (tedit 5872491A)
    (at 164.4 104.05 90)
    (descr "Light Touch Switch, https://industrial.panasonic.com/cdbs/www-data/pdf/ATK0000/ATK0000CE28.pdf")
    (property "Sheetfile" "pawpet.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "SW_RIGHT1" (at 0.05 3.95 90) (layer "B.SilkS") hide)
    (fp_text value "SW_Push" (at 0 -4.25 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0.05 3.95 90) (layer "B.Fab"))
    (pad "1" smd rect locked (at -3.4 2 90) (size 3.2 1) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND") (pinfunction "1") (pintype "passive"))
    (pad "1" smd rect locked (at 3.4 2 90) (size 3.2 1) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND") (pinfunction "1") (pintype "passive"))
    (pad "2" smd rect locked (at -3.4 -2 90) (size 3.2 1) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 9 "/D6") (pinfunction "2") (pintype "passive"))
    (pad "2" smd rect locked (at 3.4 -2 90) (size 3.2 1) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 9 "/D6") (pinfunction "2") (pintype "passive"))
    (model "${KISYS3DMOD}/Button_Switch_SMD.3dshapes/SW_SPST_EVQQ2.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "pawpet:kicad-drawing" locked (layer "B.Cu")
    (tedit 0)
    (at 177.615054 87.795353 180)
    (attr through_hole)
    (fp_text reference "Ref**" (at 0 0) (layer "B.SilkS") hide)
    (fp_text value "Val**" (at 0 0) (layer "B.SilkS") hide)
  )
  (gr_line (start 180.6 64) (end 133.9 64) (layer "Edge.Cuts") (width 0.05))
  (gr_line (start 131.3 84.1) (end 131.3 113.2) (layer "Edge.Cuts") (width 0.05))
  (gr_line (start 131.3 66.6) (end 131.3 71.15) (layer "Edge.Cuts") (width 0.05))
  (gr_line (start 180.5 115.8) (end 133.9 115.8) (layer "Edge.Cuts") (width 0.05))
  (gr_arc (start 133.9 115.8) (mid 132.061522 115.038478) (end 131.3 113.2) (layer "Edge.Cuts") (width 0.05))
  (gr_arc (start 183.1 113.2) (mid 182.338478 115.038478) (end 180.5 115.8) (layer "Edge.Cuts") (width 0.05))
  (gr_line (start 183.1 113.2) (end 183.1 66.6) (layer "Edge.Cuts") (width 0.05))
  (gr_line (start 137.2 71.15) (end 137.2 84.1) (layer "Edge.Cuts") (width 0.05))
  (gr_arc (start 131.3 66.6) (mid 132.061522 64.761522) (end 133.9 64) (layer "Edge.Cuts") (width 0.05))
  (gr_arc (start 180.6 64) (mid 182.373608 64.796531) (end 183.1 66.6) (layer "Edge.Cuts") (width 0.05))
  (gr_line (start 137.2 84.1) (end 131.3 84.1) (layer "Edge.Cuts") (width 0.05))
  (gr_line (start 137.2 71.15) (end 131.3 71.15) (layer "Edge.Cuts") (width 0.05))
  (gr_text "ver 6.6\n" (at 176.345054 91.435353) (layer "B.SilkS"))
  (gr_text "ver 6.6" (at 145.7 112.6) (layer "F.SilkS"))
  (gr_text "UwU from Seattle" (at 171.7 112.6) (layer "F.SilkS"))
)
