(kicad_sch (version 20211123) (generator eeschema)
  (paper "A4")
  (lib_symbols
    (symbol "Connector:TestPoint_Small" (pin_numbers hide) (pin_names (offset 0.762) hide) (in_bom yes) (on_board yes)
      (property "Reference" "TP" (id 0) (at 0 3.81 0))
      (property "Value" "TestPoint_Small" (id 1) (at 0 2.032 0))
      (property "Footprint" "" (id 2) (at 5.08 0 0))
      (property "Datasheet" "~" (id 3) (at 5.08 0 0))
      (property "ki_keywords" "test point tp" (id 4) (at 0 0 0))
      (property "ki_description" "test point" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "Pin* Test*" (id 6) (at 0 0 0))
      (symbol "TestPoint_Small_0_1"
        (circle (center 0 0) (radius 0.508)
          (fill (type none))
        )
      )
      (symbol "TestPoint_Small_1_1"
        (pin passive line (at 0 0 90) (length 0)
          (name "1")
          (number "1")
        )
      )
    )
    (symbol "Device:R_Small" (pin_numbers hide) (pin_names (offset 0.254) hide) (in_bom yes) (on_board yes)
      (property "Reference" "R" (id 0) (at 0.762 0.508 0))
      (property "Value" "R_Small" (id 1) (at 0.762 -1.016 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "~" (id 3) (at 0 0 0))
      (property "ki_keywords" "R resistor" (id 4) (at 0 0 0))
      (property "ki_description" "Resistor, small symbol" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "R_*" (id 6) (at 0 0 0))
      (symbol "R_Small_0_1"
        (rectangle (start -0.762 1.778) (end 0.762 -1.778)
          (fill (type none))
        )
      )
      (symbol "R_Small_1_1"
        (pin passive line (at 0 2.54 270) (length 0.762)
          (name "~")
          (number "1")
        )
        (pin passive line (at 0 -2.54 90) (length 0.762)
          (name "~")
          (number "2")
        )
      )
    )
    (symbol "Transistor_FET:DMG2301L" (pin_names hide) (in_bom yes) (on_board yes)
      (property "Reference" "Q" (id 0) (at 5.08 1.905 0))
      (property "Value" "DMG2301L" (id 1) (at 5.08 0 0))
      (property "Footprint" "Package_TO_SOT_SMD:SOT-23" (id 2) (at 5.08 -1.905 0))
      (property "Datasheet" "https://www.diodes.com/assets/Datasheets/DMG2301L.pdf" (id 3) (at 0 0 0))
      (property "ki_keywords" "P-Channel MOSFET" (id 4) (at 0 0 0))
      (property "ki_description" "-3A Id, -20V Vds, P-Channel MOSFET, SOT-23" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "SOT?23*" (id 6) (at 0 0 0))
      (symbol "DMG2301L_0_1"
        (polyline
          (pts
            (xy 0.254 0)
            (xy -2.54 0)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0.254 1.905)
            (xy 0.254 -1.905)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0.762 -1.27)
            (xy 0.762 -2.286)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0.762 0.508)
            (xy 0.762 -0.508)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0.762 2.286)
            (xy 0.762 1.27)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 2.54 2.54)
            (xy 2.54 1.778)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 2.54 -2.54)
            (xy 2.54 0)
            (xy 0.762 0)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0.762 1.778)
            (xy 3.302 1.778)
            (xy 3.302 -1.778)
            (xy 0.762 -1.778)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 2.286 0)
            (xy 1.27 0.381)
            (xy 1.27 -0.381)
            (xy 2.286 0)
          )
          (fill (type outline))
        )
        (polyline
          (pts
            (xy 2.794 -0.508)
            (xy 2.921 -0.381)
            (xy 3.683 -0.381)
            (xy 3.81 -0.254)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 3.302 -0.381)
            (xy 2.921 0.254)
            (xy 3.683 0.254)
            (xy 3.302 -0.381)
          )
          (fill (type none))
        )
        (circle (center 1.651 0) (radius 2.794)
          (fill (type none))
        )
        (circle (center 2.54 -1.778) (radius 0.254)
          (fill (type outline))
        )
        (circle (center 2.54 1.778) (radius 0.254)
          (fill (type outline))
        )
      )
      (symbol "DMG2301L_1_1"
        (pin input line (at -5.08 0 0) (length 2.54)
          (name "G")
          (number "1")
        )
        (pin passive line (at 2.54 -5.08 90) (length 2.54)
          (name "S")
          (number "2")
        )
        (pin passive line (at 2.54 5.08 270) (length 2.54)
          (name "D")
          (number "3")
        )
      )
    )
    (symbol "pawpet-v5-rescue:+3.3V-power" (power) (pin_names (offset 0)) (in_bom yes) (on_board yes)
      (property "Reference" "#PWR" (id 0) (at 0 -3.81 0))
      (property "Value" "+3.3V-power" (id 1) (at 0 3.556 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "" (id 3) (at 0 0 0))
      (symbol "+3.3V-power_0_1"
        (polyline
          (pts
            (xy -0.762 1.27)
            (xy 0 2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 0)
            (xy 0 2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 2.54)
            (xy 0.762 1.27)
          )
          (fill (type none))
        )
      )
      (symbol "+3.3V-power_1_1"
        (pin power_in line (at 0 0 90) (length 0) hide
          (name "+3V3")
          (number "1")
        )
      )
    )
    (symbol "pawpet-v5-rescue:52892-1033-molex" (pin_names (offset 0)) (in_bom yes) (on_board yes)
      (property "Reference" "J" (id 0) (at 0 12.7 0))
      (property "Value" "52892-1033-molex" (id 1) (at 0 15.24 0))
      (property "Footprint" "Molex-52892-1033-*" (id 2) (at 0 17.78 0))
      (property "Datasheet" "http://www.molex.com/webdocs/datasheets/pdf/en-us/0528921033_FFC_FPC_CONNECTORS.pdf" (id 3) (at 0 20.32 0))
      (property "Circuits Loaded" "10" (id 4) (at 0 22.86 0))
      (property "Component Link 1 Description" "Manufacturer URL" (id 5) (at 0 25.4 0))
      (property "Component Link 1 URL" "http://www.molex.com/molex/index.jsp" (id 6) (at 0 27.94 0))
      (property "Component Link 3 Description" "Package Specification" (id 7) (at 0 30.48 0))
      (property "Component Link 3 URL" "http://www.molex.com/pdm_docs/sd/528921033_sd.pdf" (id 8) (at 0 33.02 0))
      (property "Contact Position" "Bottom" (id 9) (at 0 35.56 0))
      (property "Current Max per Contact" "0.5A" (id 10) (at 0 38.1 0))
      (property "Durability mating cycles max" "20" (id 11) (at 0 40.64 0))
      (property "Entry Angle" "90degrees Angle" (id 12) (at 0 43.18 0))
      (property "Mated Height" "2.00mm" (id 13) (at 0 45.72 0))
      (property "Material   Metal" "Phosphor Bronze" (id 14) (at 0 48.26 0))
      (property "Material   Plating Mating" "Silver, Tin-Bismuth" (id 15) (at 0 50.8 0))
      (property "Material   Plating Termination" "Silver, Tin-Bismuth" (id 16) (at 0 53.34 0))
      (property "Mounting Technology" "Surface Mount" (id 17) (at 0 55.88 0))
      (property "Number of Rows" "1" (id 18) (at 0 58.42 0))
      (property "Orientation" "Right Angle" (id 19) (at 0 60.96 0))
      (property "PCB Locator" "No" (id 20) (at 0 63.5 0))
      (property "PCB Retention" "Yes" (id 21) (at 0 66.04 0))
      (property "Package Description" "10-Lead FPC Connector, Pitch 0.5 mm" (id 22) (at 0 68.58 0))
      (property "Package Version" "Rev. A, 05/2013" (id 23) (at 0 71.12 0))
      (property "Packing" "Tape and Reel" (id 24) (at 0 73.66 0))
      (property "Pitch   Mating Interface" "0.50mm" (id 25) (at 0 76.2 0))
      (property "Pitch   Termination Interface" "0.50mm" (id 26) (at 0 78.74 0))
      (property "Polarized to PCB" "No" (id 27) (at 0 81.28 0))
      (property "Stackable" "No" (id 28) (at 0 83.82 0))
      (property "Voltage Max" "50V" (id 29) (at 0 86.36 0))
      (property "category" "Conn" (id 30) (at 0 88.9 0))
      (property "ciiva ids" "12958041" (id 31) (at 0 91.44 0))
      (property "library id" "ed2c8a3844ca0313" (id 32) (at 0 93.98 0))
      (property "manufacturer" "Molex" (id 33) (at 0 96.52 0))
      (property "package" "52892-1033" (id 34) (at 0 99.06 0))
      (property "release date" "1411372666" (id 35) (at 0 101.6 0))
      (property "rohs" "Yes" (id 36) (at 0 104.14 0))
      (property "vault revision" "2519BB65-6747-4A90-BA56-D26D50506A67" (id 37) (at 0 106.68 0))
      (property "imported" "yes" (id 38) (at 0 109.22 0))
      (property "ki_locked" "" (id 39) (at 0 0 0))
      (symbol "52892-1033-molex_1_1"
        (rectangle (start -2.54 10.16) (end 33.02 5.08)
          (fill (type background))
        )
        (polyline
          (pts
            (xy 0 5.08)
            (xy 0 6.858)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 2.54 5.08)
            (xy 2.54 6.858)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 5.08 5.08)
            (xy 5.08 6.858)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 7.62 5.08)
            (xy 7.62 6.858)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 10.16 5.08)
            (xy 10.16 6.858)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 12.7 5.08)
            (xy 12.7 6.858)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 15.24 5.08)
            (xy 15.24 6.858)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 17.78 5.08)
            (xy 17.78 6.858)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 20.32 5.08)
            (xy 20.32 6.858)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 22.86 5.08)
            (xy 22.86 6.858)
          )
          (fill (type none))
        )
        (circle (center 0 7.62) (radius 0.762)
          (fill (type none))
        )
        (circle (center 2.54 7.62) (radius 0.762)
          (fill (type none))
        )
        (circle (center 5.08 7.62) (radius 0.762)
          (fill (type none))
        )
        (circle (center 7.62 7.62) (radius 0.762)
          (fill (type none))
        )
        (circle (center 10.16 7.62) (radius 0.762)
          (fill (type none))
        )
        (circle (center 12.7 7.62) (radius 0.762)
          (fill (type none))
        )
        (circle (center 15.24 7.62) (radius 0.762)
          (fill (type none))
        )
        (circle (center 17.78 7.62) (radius 0.762)
          (fill (type none))
        )
        (circle (center 20.32 7.62) (radius 0.762)
          (fill (type none))
        )
        (circle (center 22.86 7.62) (radius 0.762)
          (fill (type none))
        )
        (pin passive line (at 0 2.54 90) (length 2.54)
          (name "1")
          (number "1")
        )
        (pin passive line (at 22.86 2.54 90) (length 2.54)
          (name "10")
          (number "10")
        )
        (pin passive line (at 2.54 2.54 90) (length 2.54)
          (name "2")
          (number "2")
        )
        (pin passive line (at 5.08 2.54 90) (length 2.54)
          (name "3")
          (number "3")
        )
        (pin passive line (at 7.62 2.54 90) (length 2.54)
          (name "4")
          (number "4")
        )
        (pin passive line (at 10.16 2.54 90) (length 2.54)
          (name "5")
          (number "5")
        )
        (pin passive line (at 12.7 2.54 90) (length 2.54)
          (name "6")
          (number "6")
        )
        (pin passive line (at 15.24 2.54 90) (length 2.54)
          (name "7")
          (number "7")
        )
        (pin passive line (at 17.78 2.54 90) (length 2.54)
          (name "8")
          (number "8")
        )
        (pin passive line (at 20.32 2.54 90) (length 2.54)
          (name "9")
          (number "9")
        )
        (pin passive line (at 27.94 2.54 90) (length 2.54)
          (name "MP1")
          (number "MP1")
        )
        (pin passive line (at 30.48 2.54 90) (length 2.54)
          (name "MP2")
          (number "MP2")
        )
      )
    )
    (symbol "pawpet-v5-rescue:ATSAMD21G18A-A-MCU_Microchip_SAMD" (in_bom yes) (on_board yes)
      (property "Reference" "U" (id 0) (at -13.97 46.99 0))
      (property "Value" "ATSAMD21G18A-A-MCU_Microchip_SAMD" (id 1) (at 16.51 46.99 0))
      (property "Footprint" "Package_QFP:TQFP-48_7x7mm_P0.5mm" (id 2) (at 22.86 -46.99 0))
      (property "Datasheet" "" (id 3) (at 0 25.4 0))
      (property "ki_fp_filters" "TQFP*7x7mm*P0.5mm*" (id 4) (at 0 0 0))
      (symbol "ATSAMD21G18A-A-MCU_Microchip_SAMD_0_1"
        (rectangle (start -15.24 45.72) (end 15.24 -45.72)
          (fill (type background))
        )
      )
      (symbol "ATSAMD21G18A-A-MCU_Microchip_SAMD_1_1"
        (pin bidirectional line (at -17.78 40.64 0) (length 2.54)
          (name "PA00")
          (number "1")
        )
        (pin bidirectional line (at -17.78 27.94 0) (length 2.54)
          (name "PA05")
          (number "10")
        )
        (pin bidirectional line (at -17.78 25.4 0) (length 2.54)
          (name "PA06")
          (number "11")
        )
        (pin bidirectional line (at -17.78 22.86 0) (length 2.54)
          (name "PA07")
          (number "12")
        )
        (pin bidirectional line (at -17.78 20.32 0) (length 2.54)
          (name "PA08")
          (number "13")
        )
        (pin bidirectional line (at -17.78 17.78 0) (length 2.54)
          (name "PA09")
          (number "14")
        )
        (pin bidirectional line (at -17.78 15.24 0) (length 2.54)
          (name "PA10")
          (number "15")
        )
        (pin bidirectional line (at -17.78 12.7 0) (length 2.54)
          (name "PA11")
          (number "16")
        )
        (pin power_in line (at 2.54 48.26 270) (length 2.54)
          (name "VDDIO")
          (number "17")
        )
        (pin power_in line (at 0 -48.26 90) (length 2.54)
          (name "GND")
          (number "18")
        )
        (pin bidirectional line (at 17.78 15.24 180) (length 2.54)
          (name "PB10")
          (number "19")
        )
        (pin bidirectional line (at -17.78 38.1 0) (length 2.54)
          (name "PA01")
          (number "2")
        )
        (pin bidirectional line (at 17.78 12.7 180) (length 2.54)
          (name "PB11")
          (number "20")
        )
        (pin bidirectional line (at -17.78 10.16 0) (length 2.54)
          (name "PA12")
          (number "21")
        )
        (pin bidirectional line (at -17.78 7.62 0) (length 2.54)
          (name "PA13")
          (number "22")
        )
        (pin bidirectional line (at -17.78 5.08 0) (length 2.54)
          (name "PA14")
          (number "23")
        )
        (pin bidirectional line (at -17.78 2.54 0) (length 2.54)
          (name "PA15")
          (number "24")
        )
        (pin bidirectional line (at -17.78 0 0) (length 2.54)
          (name "PA16")
          (number "25")
        )
        (pin bidirectional line (at -17.78 -2.54 0) (length 2.54)
          (name "PA17")
          (number "26")
        )
        (pin bidirectional line (at -17.78 -5.08 0) (length 2.54)
          (name "PA18")
          (number "27")
        )
        (pin bidirectional line (at -17.78 -7.62 0) (length 2.54)
          (name "PA19")
          (number "28")
        )
        (pin bidirectional line (at -17.78 -10.16 0) (length 2.54)
          (name "PA20")
          (number "29")
        )
        (pin bidirectional line (at -17.78 35.56 0) (length 2.54)
          (name "PA02")
          (number "3")
        )
        (pin bidirectional line (at -17.78 -12.7 0) (length 2.54)
          (name "PA21")
          (number "30")
        )
        (pin bidirectional line (at -17.78 -15.24 0) (length 2.54)
          (name "PA22")
          (number "31")
        )
        (pin bidirectional line (at -17.78 -17.78 0) (length 2.54)
          (name "PA23")
          (number "32")
        )
        (pin bidirectional line (at -17.78 -20.32 0) (length 2.54)
          (name "PA24")
          (number "33")
        )
        (pin bidirectional line (at -17.78 -22.86 0) (length 2.54)
          (name "PA25")
          (number "34")
        )
        (pin passive line (at 0 -48.26 90) (length 2.54) hide
          (name "GND")
          (number "35")
        )
        (pin power_in line (at 0 48.26 270) (length 2.54)
          (name "VDDIO")
          (number "36")
        )
        (pin bidirectional line (at 17.78 -15.24 180) (length 2.54)
          (name "PB22")
          (number "37")
        )
        (pin bidirectional line (at 17.78 -17.78 180) (length 2.54)
          (name "PB23")
          (number "38")
        )
        (pin bidirectional line (at -17.78 -27.94 0) (length 2.54)
          (name "PA27")
          (number "39")
        )
        (pin bidirectional line (at -17.78 33.02 0) (length 2.54)
          (name "PA03")
          (number "4")
        )
        (pin input line (at -17.78 -43.18 0) (length 2.54)
          (name "~{RESET}")
          (number "40")
        )
        (pin bidirectional line (at -17.78 -30.48 0) (length 2.54)
          (name "PA28")
          (number "41")
        )
        (pin passive line (at 0 -48.26 90) (length 2.54) hide
          (name "GND")
          (number "42")
        )
        (pin power_out line (at -7.62 48.26 270) (length 2.54)
          (name "VDDCORE")
          (number "43")
        )
        (pin power_in line (at -2.54 48.26 270) (length 2.54)
          (name "VDDIN")
          (number "44")
        )
        (pin bidirectional line (at -17.78 -35.56 0) (length 2.54)
          (name "PA30")
          (number "45")
        )
        (pin bidirectional line (at -17.78 -38.1 0) (length 2.54)
          (name "PA31")
          (number "46")
        )
        (pin bidirectional line (at 17.78 35.56 180) (length 2.54)
          (name "PB02")
          (number "47")
        )
        (pin bidirectional line (at 17.78 33.02 180) (length 2.54)
          (name "PB03")
          (number "48")
        )
        (pin input line (at 17.78 -34.29 180) (length 2.54)
          (name "GNDT")
          (number "49")
        )
        (pin power_in line (at 2.54 -48.26 90) (length 2.54)
          (name "GNDANA")
          (number "5")
        )
        (pin power_in line (at 7.62 48.26 270) (length 2.54)
          (name "VDDANA")
          (number "6")
        )
        (pin bidirectional line (at 17.78 20.32 180) (length 2.54)
          (name "PB08")
          (number "7")
        )
        (pin bidirectional line (at 17.78 17.78 180) (length 2.54)
          (name "PB09")
          (number "8")
        )
        (pin bidirectional line (at -17.78 30.48 0) (length 2.54)
          (name "PA04")
          (number "9")
        )
      )
    )
    (symbol "pawpet-v5-rescue:Battery-Device" (pin_numbers hide) (pin_names (offset 0) hide) (in_bom yes) (on_board yes)
      (property "Reference" "BT" (id 0) (at 2.54 2.54 0))
      (property "Value" "Battery-Device" (id 1) (at 2.54 0 0))
      (property "Footprint" "" (id 2) (at 0 1.524 90))
      (property "Datasheet" "" (id 3) (at 0 1.524 90))
      (symbol "Battery-Device_0_1"
        (rectangle (start -2.032 -1.397) (end 2.032 -1.651)
          (fill (type outline))
        )
        (rectangle (start -2.032 1.778) (end 2.032 1.524)
          (fill (type outline))
        )
        (rectangle (start -1.3208 -1.9812) (end 1.27 -2.4892)
          (fill (type outline))
        )
        (rectangle (start -1.3208 1.1938) (end 1.27 0.6858)
          (fill (type outline))
        )
        (polyline
          (pts
            (xy 0 -1.524)
            (xy 0 -1.27)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 -1.016)
            (xy 0 -0.762)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 -0.508)
            (xy 0 -0.254)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 0)
            (xy 0 0.254)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 0.508)
            (xy 0 0.762)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 1.778)
            (xy 0 2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0.254 2.667)
            (xy 1.27 2.667)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0.762 3.175)
            (xy 0.762 2.159)
          )
          (fill (type none))
        )
      )
      (symbol "Battery-Device_1_1"
        (pin passive line (at 0 5.08 270) (length 2.54)
          (name "+")
          (number "1")
        )
        (pin passive line (at 0 -5.08 90) (length 2.54)
          (name "-")
          (number "2")
        )
      )
    )
    (symbol "pawpet-v5-rescue:C_Small-Device" (pin_numbers hide) (pin_names (offset 0.254) hide) (in_bom yes) (on_board yes)
      (property "Reference" "C" (id 0) (at 0.254 1.778 0))
      (property "Value" "C_Small-Device" (id 1) (at 0.254 -2.032 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "" (id 3) (at 0 0 0))
      (property "ki_fp_filters" "C_*" (id 4) (at 0 0 0))
      (symbol "C_Small-Device_0_1"
        (polyline
          (pts
            (xy -1.524 -0.508)
            (xy 1.524 -0.508)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.524 0.508)
            (xy 1.524 0.508)
          )
          (fill (type none))
        )
      )
      (symbol "C_Small-Device_1_1"
        (pin passive line (at 0 2.54 270) (length 2.032)
          (name "~")
          (number "1")
        )
        (pin passive line (at 0 -2.54 90) (length 2.032)
          (name "~")
          (number "2")
        )
      )
    )
    (symbol "pawpet-v5-rescue:Conn_ARM_JTAG_SWD_10-Connector" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
      (property "Reference" "J" (id 0) (at -2.54 16.51 0))
      (property "Value" "Conn_ARM_JTAG_SWD_10-Connector" (id 1) (at -2.54 13.97 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "" (id 3) (at -8.89 -31.75 90))
      (property "ki_fp_filters" "PinHeader?2x05?P1.27mm*" (id 4) (at 0 0 0))
      (symbol "Conn_ARM_JTAG_SWD_10-Connector_0_1"
        (rectangle (start -10.16 12.7) (end 10.16 -12.7)
          (fill (type background))
        )
        (rectangle (start -2.794 -12.7) (end -2.286 -11.684)
          (fill (type none))
        )
        (rectangle (start -0.254 -12.7) (end 0.254 -11.684)
          (fill (type none))
        )
        (rectangle (start -0.254 12.7) (end 0.254 11.684)
          (fill (type none))
        )
        (rectangle (start 9.144 2.286) (end 10.16 2.794)
          (fill (type none))
        )
        (rectangle (start 10.16 -2.794) (end 9.144 -2.286)
          (fill (type none))
        )
        (rectangle (start 10.16 -0.254) (end 9.144 0.254)
          (fill (type none))
        )
        (rectangle (start 10.16 7.874) (end 9.144 7.366)
          (fill (type none))
        )
      )
      (symbol "Conn_ARM_JTAG_SWD_10-Connector_1_1"
        (rectangle (start 9.144 -5.334) (end 10.16 -4.826)
          (fill (type none))
        )
        (pin power_in line (at 0 15.24 270) (length 2.54)
          (name "VTref")
          (number "1")
        )
        (pin open_collector line (at 12.7 7.62 180) (length 2.54)
          (name "~{RESET}")
          (number "10")
        )
        (pin bidirectional line (at 12.7 0 180) (length 2.54)
          (name "SWDIO/TMS")
          (number "2")
        )
        (pin power_in line (at 0 -15.24 90) (length 2.54)
          (name "GND")
          (number "3")
        )
        (pin output line (at 12.7 2.54 180) (length 2.54)
          (name "SWDCLK/TCK")
          (number "4")
        )
        (pin passive line (at 0 -15.24 90) (length 2.54) hide
          (name "GND")
          (number "5")
        )
        (pin input line (at 12.7 -2.54 180) (length 2.54)
          (name "SWO/TDO")
          (number "6")
        )
        (pin no_connect line (at -10.16 0 0) (length 2.54) hide
          (name "KEY")
          (number "7")
        )
        (pin output line (at 12.7 -5.08 180) (length 2.54)
          (name "NC/TDI")
          (number "8")
        )
        (pin passive line (at -2.54 -15.24 90) (length 2.54)
          (name "GNDDetect")
          (number "9")
        )
      )
    )
    (symbol "pawpet-v5-rescue:Crystal_Small-Device" (pin_numbers hide) (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
      (property "Reference" "Y" (id 0) (at 0 2.54 0))
      (property "Value" "Crystal_Small-Device" (id 1) (at 0 -2.54 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "" (id 3) (at 0 0 0))
      (property "ki_fp_filters" "Crystal*" (id 4) (at 0 0 0))
      (symbol "Crystal_Small-Device_0_1"
        (rectangle (start -0.762 -1.524) (end 0.762 1.524)
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.27 -0.762)
            (xy -1.27 0.762)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.27 -0.762)
            (xy 1.27 0.762)
          )
          (fill (type none))
        )
      )
      (symbol "Crystal_Small-Device_1_1"
        (pin passive line (at -2.54 0 0) (length 1.27)
          (name "1")
          (number "1")
        )
        (pin passive line (at 2.54 0 180) (length 1.27)
          (name "2")
          (number "2")
        )
      )
    )
    (symbol "pawpet-v5-rescue:GND-power" (power) (pin_names (offset 0)) (in_bom yes) (on_board yes)
      (property "Reference" "#PWR" (id 0) (at 0 -6.35 0))
      (property "Value" "GND-power" (id 1) (at 0 -3.81 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "" (id 3) (at 0 0 0))
      (symbol "GND-power_0_1"
        (polyline
          (pts
            (xy 0 0)
            (xy 0 -1.27)
            (xy 1.27 -1.27)
            (xy 0 -2.54)
            (xy -1.27 -1.27)
            (xy 0 -1.27)
          )
          (fill (type none))
        )
      )
      (symbol "GND-power_1_1"
        (pin power_in line (at 0 0 270) (length 0) hide
          (name "GND")
          (number "1")
        )
      )
    )
    (symbol "pawpet-v5-rescue:MX25V1635FM1I-macronix" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
      (property "Reference" "U" (id 0) (at 0 5.08 0))
      (property "Value" "MX25V1635FM1I-macronix" (id 1) (at 0 7.62 0))
      (property "Footprint" "Macronix-SOP-8-150MIL-0-0-*" (id 2) (at 0 10.16 0))
      (property "Datasheet" "https://www.macronix.com/Lists/Datasheet/Attachments/7409/MX25V1635F,%202.5V,%2016Mb,%20v1.4.pdf" (id 3) (at 0 12.7 0))
      (property "access time" "8ns" (id 4) (at 0 15.24 0))
      (property "ambient temperature range high" "+85°C" (id 5) (at 0 17.78 0))
      (property "ambient temperature range low" "-40°C" (id 6) (at 0 20.32 0))
      (property "automotive" "No" (id 7) (at 0 22.86 0))
      (property "category" "IC" (id 8) (at 0 25.4 0))
      (property "device class L1" "Integrated Circuits (ICs)" (id 9) (at 0 27.94 0))
      (property "device class L2" "Memory" (id 10) (at 0 30.48 0))
      (property "device class L3" "Flash" (id 11) (at 0 33.02 0))
      (property "digikey description" "IC FLASH 16M SPI 80MHZ 8SOP" (id 12) (at 0 35.56 0))
      (property "digikey part number" "1092-1190-ND" (id 13) (at 0 38.1 0))
      (property "footprint url" "https://www.macronix.com/Lists/ApplicationNote/Attachments/1897/AN0239V1%20-%20Macronix%20150mil%208SOP_6x5mm8WSON_dual%20layout.pdf" (id 14) (at 0 40.64 0))
      (property "frequency" "80MHz" (id 15) (at 0 43.18 0))
      (property "height" "1.75mm" (id 16) (at 0 45.72 0))
      (property "interface" "SPI" (id 17) (at 0 48.26 0))
      (property "ipc land pattern name" "SOIC127P599X175-8" (id 18) (at 0 50.8 0))
      (property "lead free" "Yes" (id 19) (at 0 53.34 0))
      (property "library id" "b395dce75c947a4f" (id 20) (at 0 55.88 0))
      (property "manufacturer" "Macronix" (id 21) (at 0 58.42 0))
      (property "max supply voltage" "3.6V" (id 22) (at 0 60.96 0))
      (property "memory size" "16Mbits" (id 23) (at 0 63.5 0))
      (property "memory type" "FLASH" (id 24) (at 0 66.04 0))
      (property "min supply voltage" "2.3V" (id 25) (at 0 68.58 0))
      (property "nominal supply current" "3.5-6.5mA" (id 26) (at 0 71.12 0))
      (property "package" "SOP8" (id 27) (at 0 73.66 0))
      (property "rohs" "Yes" (id 28) (at 0 76.2 0))
      (property "standoff height" "0.1mm" (id 29) (at 0 78.74 0))
      (property "temperature range high" "+85°C" (id 30) (at 0 81.28 0))
      (property "temperature range low" "-40°C" (id 31) (at 0 83.82 0))
      (property "ki_locked" "" (id 32) (at 0 0 0))
      (symbol "MX25V1635FM1I-macronix_1_1"
        (rectangle (start 5.08 2.54) (end 38.1 -17.78)
          (fill (type background))
        )
        (pin input line (at 40.64 -7.62 180) (length 2.54)
          (name "~{CS}")
          (number "1")
        )
        (pin bidirectional line (at 40.64 -5.08 180) (length 2.54)
          (name "SO/SIO1")
          (number "2")
        )
        (pin bidirectional line (at 2.54 -7.62 0) (length 2.54)
          (name "~{WP}/SIO2")
          (number "3")
        )
        (pin power_in line (at 40.64 -15.24 180) (length 2.54)
          (name "GND")
          (number "4")
        )
        (pin bidirectional line (at 40.64 -2.54 180) (length 2.54)
          (name "SI/SIO0")
          (number "5")
        )
        (pin input clock (at 40.64 0 180) (length 2.54)
          (name "SCLK")
          (number "6")
        )
        (pin bidirectional line (at 2.54 -15.24 0) (length 2.54)
          (name "~{HOLD}/SIO3")
          (number "7")
        )
        (pin power_in line (at 2.54 0 0) (length 2.54)
          (name "VCC")
          (number "8")
        )
      )
    )
    (symbol "pawpet-v5-rescue:R_Small-Device" (pin_numbers hide) (pin_names (offset 0.254) hide) (in_bom yes) (on_board yes)
      (property "Reference" "R" (id 0) (at 0.762 0.508 0))
      (property "Value" "R_Small-Device" (id 1) (at 0.762 -1.016 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "" (id 3) (at 0 0 0))
      (property "ki_fp_filters" "R_*" (id 4) (at 0 0 0))
      (symbol "R_Small-Device_0_1"
        (rectangle (start -0.762 1.778) (end 0.762 -1.778)
          (fill (type none))
        )
      )
      (symbol "R_Small-Device_1_1"
        (pin passive line (at 0 2.54 270) (length 0.762)
          (name "~")
          (number "1")
        )
        (pin passive line (at 0 -2.54 90) (length 0.762)
          (name "~")
          (number "2")
        )
      )
    )
    (symbol "pawpet-v5-rescue:SW_Push-Switch" (pin_numbers hide) (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
      (property "Reference" "SW" (id 0) (at 1.27 2.54 0))
      (property "Value" "SW_Push-Switch" (id 1) (at 0 -1.524 0))
      (property "Footprint" "" (id 2) (at 0 5.08 0))
      (property "Datasheet" "" (id 3) (at 0 5.08 0))
      (symbol "SW_Push-Switch_0_1"
        (circle (center -2.032 0) (radius 0.508)
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 1.27)
            (xy 0 3.048)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 2.54 1.27)
            (xy -2.54 1.27)
          )
          (fill (type none))
        )
        (circle (center 2.032 0) (radius 0.508)
          (fill (type none))
        )
        (pin passive line (at -5.08 0 0) (length 2.54)
          (name "1")
          (number "1")
        )
        (pin passive line (at 5.08 0 180) (length 2.54)
          (name "2")
          (number "2")
        )
      )
    )
    (symbol "pawpet-v5-rescue:Speaker_Crystal-Device" (pin_names (offset 0) hide) (in_bom yes) (on_board yes)
      (property "Reference" "LS" (id 0) (at 0.635 5.715 0))
      (property "Value" "Speaker_Crystal-Device" (id 1) (at 0.635 3.81 0))
      (property "Footprint" "" (id 2) (at -0.889 -1.27 0))
      (property "Datasheet" "" (id 3) (at -0.889 -1.27 0))
      (symbol "Speaker_Crystal-Device_0_0"
        (rectangle (start -2.54 1.27) (end 1.143 -3.81)
          (fill (type none))
        )
        (rectangle (start -2.032 -0.635) (end 0.635 -1.905)
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.651 -2.286)
            (xy 0.381 -2.286)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.651 -0.254)
            (xy 0.381 -0.254)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -0.635 -2.286)
            (xy -0.635 -3.048)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -0.635 -0.254)
            (xy -0.635 0.508)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.143 1.27)
            (xy 3.683 3.81)
            (xy 3.683 -6.35)
            (xy 1.143 -3.81)
          )
          (fill (type none))
        )
      )
      (symbol "Speaker_Crystal-Device_1_1"
        (pin input line (at -5.08 0 0) (length 2.54)
          (name "1")
          (number "1")
        )
        (pin input line (at -5.08 -2.54 0) (length 2.54)
          (name "2")
          (number "2")
        )
      )
    )
    (symbol "power:+3.3V" (power) (pin_names (offset 0)) (in_bom yes) (on_board yes)
      (property "Reference" "#PWR" (id 0) (at 0 -3.81 0))
      (property "Value" "+3.3V" (id 1) (at 0 3.556 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "" (id 3) (at 0 0 0))
      (property "ki_keywords" "power-flag" (id 4) (at 0 0 0))
      (property "ki_description" "Power symbol creates a global label with name \"+3.3V\"" (id 5) (at 0 0 0))
      (symbol "+3.3V_0_1"
        (polyline
          (pts
            (xy -0.762 1.27)
            (xy 0 2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 0)
            (xy 0 2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 2.54)
            (xy 0.762 1.27)
          )
          (fill (type none))
        )
      )
      (symbol "+3.3V_1_1"
        (pin power_in line (at 0 0 90) (length 0) hide
          (name "+3V3")
          (number "1")
        )
      )
    )
    (symbol "power:GND" (power) (pin_names (offset 0)) (in_bom yes) (on_board yes)
      (property "Reference" "#PWR" (id 0) (at 0 -6.35 0))
      (property "Value" "GND" (id 1) (at 0 -3.81 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "" (id 3) (at 0 0 0))
      (property "ki_keywords" "power-flag" (id 4) (at 0 0 0))
      (property "ki_description" "Power symbol creates a global label with name \"GND\" , ground" (id 5) (at 0 0 0))
      (symbol "GND_0_1"
        (polyline
          (pts
            (xy 0 0)
            (xy 0 -1.27)
            (xy 1.27 -1.27)
            (xy 0 -2.54)
            (xy -1.27 -1.27)
            (xy 0 -1.27)
          )
          (fill (type none))
        )
      )
      (symbol "GND_1_1"
        (pin power_in line (at 0 0 270) (length 0) hide
          (name "GND")
          (number "1")
        )
      )
    )
    (symbol "usb-c:USB4105-GF-A" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
      (property "Reference" "J" (id 0) (at -15.24 13.97 0))
      (property "Value" "USB4105-GF-A" (id 1) (at -15.24 -15.24 0))
      (property "Footprint" "GCT_USB4105-GF-A" (id 2) (at 0 0 0))
      (property "Datasheet" "" (id 3) (at 0 0 0))
      (property "MANUFACTURER" "GCT" (id 4) (at 0 0 0))
      (property "PARTREV" "A3" (id 5) (at 0 0 0))
      (property "STANDARD" "Manufacturer Recommendations" (id 6) (at 0 0 0))
      (property "MAXIMUM_PACKAGE_HEIGHT" "3.31 mm" (id 7) (at 0 0 0))
      (property "ki_locked" "" (id 8) (at 0 0 0))
      (symbol "USB4105-GF-A_0_0"
        (rectangle (start -15.24 -12.7) (end 15.24 12.7)
          (fill (type background))
        )
        (pin power_in line (at 20.32 -7.62 180) (length 5.08)
          (name "GND")
          (number "A1_B12")
        )
        (pin power_in line (at 20.32 11.43 180) (length 5.08)
          (name "VBUS")
          (number "A4_B9")
        )
        (pin bidirectional line (at -20.32 5.08 0) (length 5.08)
          (name "CC1")
          (number "A5")
        )
        (pin bidirectional line (at -20.32 2.54 0) (length 5.08)
          (name "DP1")
          (number "A6")
        )
        (pin bidirectional line (at -20.32 0 0) (length 5.08)
          (name "DN1")
          (number "A7")
        )
        (pin bidirectional line (at -20.32 -2.54 0) (length 5.08)
          (name "SBU1")
          (number "A8")
        )
        (pin power_in line (at 20.32 -7.62 180) (length 5.08)
          (name "GND")
          (number "B1_A12")
        )
        (pin power_in line (at 20.32 8.89 180) (length 5.08)
          (name "VBUS")
          (number "B4_A9")
        )
        (pin bidirectional line (at 20.32 5.08 180) (length 5.08)
          (name "CC2")
          (number "B5")
        )
        (pin bidirectional line (at 20.32 2.54 180) (length 5.08)
          (name "DP2")
          (number "B6")
        )
        (pin bidirectional line (at 20.32 0 180) (length 5.08)
          (name "DN2")
          (number "B7")
        )
        (pin bidirectional line (at 20.32 -2.54 180) (length 5.08)
          (name "SBU2")
          (number "B8")
        )
        (pin power_in line (at 20.32 -10.16 180) (length 5.08)
          (name "SHELL_GND")
          (number "S1")
        )
        (pin power_in line (at 20.32 -10.16 180) (length 5.08)
          (name "SHELL_GND")
          (number "S2")
        )
        (pin power_in line (at 20.32 -10.16 180) (length 5.08)
          (name "SHELL_GND")
          (number "S3")
        )
        (pin power_in line (at 20.32 -10.16 180) (length 5.08)
          (name "SHELL_GND")
          (number "S4")
        )
      )
    )
  )
  (junction (at 228.6 151.13) (diameter 0) (color 0 0 0 0))
  (junction (at 54.61 100.33) (diameter 0) (color 0 0 0 0))
  (junction (at 63.5 21.59) (diameter 0) (color 0 0 0 0))
  (junction (at 76.2 26.67) (diameter 0) (color 0 0 0 0))
  (junction (at 62.23 100.33) (diameter 0) (color 0 0 0 0))
  (junction (at 143.51 156.21) (diameter 0) (color 0 0 0 0))
  (junction (at 198.12 63.5) (diameter 0) (color 0 0 0 0))
  (junction (at 45.72 76.2) (diameter 0) (color 0 0 0 0))
  (junction (at 177.8 63.5) (diameter 0) (color 0 0 0 0))
  (junction (at 72.39 45.72) (diameter 0) (color 0 0 0 0))
  (junction (at 223.52 44.45) (diameter 0) (color 0 0 0 0))
  (junction (at 162.56 45.72) (diameter 0) (color 0 0 0 0))
  (junction (at 228.6 44.45) (diameter 0) (color 0 0 0 0))
  (junction (at 226.06 44.45) (diameter 0) (color 0 0 0 0))
  (junction (at 83.82 148.59) (diameter 0) (color 0 0 0 0))
  (junction (at 83.82 156.21) (diameter 0) (color 0 0 0 0))
  (junction (at 138.43 121.92) (diameter 0) (color 0 0 0 0))
  (junction (at 198.12 58.42) (diameter 0) (color 0 0 0 0))
  (junction (at 54.61 88.9) (diameter 0) (color 0 0 0 0))
  (junction (at 45.72 100.33) (diameter 0) (color 0 0 0 0))
  (junction (at 45.72 83.82) (diameter 0) (color 0 0 0 0))
  (junction (at 35.56 20.32) (diameter 0) (color 0 0 0 0))
  (junction (at 154.94 64.77) (diameter 0) (color 0 0 0 0))
  (junction (at 240.03 151.13) (diameter 0) (color 0 0 0 0))
  (junction (at 34.29 86.36) (diameter 0) (color 0 0 0 0))
  (junction (at 54.61 81.28) (diameter 0) (color 0 0 0 0))
  (no_connect (at 193.04 88.9))
  (no_connect (at 193.04 132.08))
  (no_connect (at 193.04 66.04))
  (no_connect (at 154.94 57.15))
  (no_connect (at 193.04 129.54))
  (no_connect (at 250.19 68.58))
  (no_connect (at 114.3 57.15))
  (no_connect (at 193.04 119.38))
  (no_connect (at 193.04 68.58))
  (no_connect (at 193.04 73.66))
  (no_connect (at 153.67 111.76))
  (no_connect (at 193.04 91.44))
  (no_connect (at 250.19 83.82))
  (no_connect (at 243.84 119.38))
  (no_connect (at 153.67 109.22))
  (no_connect (at 80.01 101.6))
  (no_connect (at 193.04 116.84))
  (no_connect (at 243.84 116.84))
  (no_connect (at 80.01 99.06))
  (wire (pts (xy 208.28 68.58) (xy 193.04 68.58)))
  (wire (pts (xy 181.61 78.74) (xy 208.28 78.74)))
  (wire (pts (xy 193.04 66.04) (xy 208.28 66.04)))
  (wire (pts (xy 193.04 114.3) (xy 208.28 114.3)))
  (wire (pts (xy 46.99 184.15) (xy 53.34 184.15)))
  (wire (pts (xy 154.94 67.31) (xy 154.94 64.77)))
  (wire (pts (xy 76.2 21.59) (xy 76.2 26.67)))
  (wire (pts (xy 62.23 91.44) (xy 80.01 91.44)))
  (wire (pts (xy 45.72 83.82) (xy 80.01 83.82)))
  (wire (pts (xy 193.04 144.78) (xy 208.28 144.78)))
  (wire (pts (xy 193.04 111.76) (xy 208.28 111.76)))
  (wire (pts (xy 114.3 49.53) (xy 105.41 49.53)))
  (wire (pts (xy 243.84 135.89) (xy 243.84 151.13)))
  (wire (pts (xy 228.6 151.13) (xy 228.6 149.86)))
  (wire (pts (xy 162.56 45.72) (xy 162.56 50.8)))
  (wire (pts (xy 193.04 96.52) (xy 208.28 96.52)))
  (wire (pts (xy 218.44 48.26) (xy 215.9 48.26)))
  (wire (pts (xy 167.64 49.53) (xy 167.64 58.42)))
  (wire (pts (xy 46.99 151.13) (xy 53.34 151.13)))
  (wire (pts (xy 223.52 44.45) (xy 208.28 44.45)))
  (wire (pts (xy 193.04 129.54) (xy 208.28 129.54)))
  (wire (pts (xy 233.68 44.45) (xy 233.68 53.34)))
  (wire (pts (xy 19.05 20.32) (xy 19.05 21.59)))
  (wire (pts (xy 154.94 54.61) (xy 158.75 54.61)))
  (wire (pts (xy 243.84 151.13) (xy 240.03 151.13)))
  (wire (pts (xy 243.84 88.9) (xy 260.35 88.9)))
  (wire (pts (xy 85.09 123.19) (xy 87.63 123.19)))
  (wire (pts (xy 105.41 63.5) (xy 105.41 67.31)))
  (wire (pts (xy 107.95 52.07) (xy 114.3 52.07)))
  (wire (pts (xy 193.04 81.28) (xy 208.28 81.28)))
  (wire (pts (xy 167.64 63.5) (xy 167.64 67.31)))
  (wire (pts (xy 143.51 156.21) (xy 143.51 151.13)))
  (wire (pts (xy 154.94 43.18) (xy 162.56 43.18)))
  (wire (pts (xy 162.56 43.18) (xy 162.56 45.72)))
  (wire (pts (xy 243.84 86.36) (xy 260.35 86.36)))
  (wire (pts (xy 34.29 86.36) (xy 34.29 91.44)))
  (wire (pts (xy 53.34 162.56) (xy 46.99 162.56)))
  (wire (pts (xy 90.17 120.65) (xy 91.44 120.65)))
  (wire (pts (xy 180.34 86.36) (xy 208.28 86.36)))
  (wire (pts (xy 62.23 91.44) (xy 62.23 100.33)))
  (wire (pts (xy 46.99 195.58) (xy 53.34 195.58)))
  (wire (pts (xy 228.6 44.45) (xy 228.6 53.34)))
  (wire (pts (xy 193.04 109.22) (xy 208.28 109.22)))
  (wire (pts (xy 226.06 44.45) (xy 223.52 44.45)))
  (wire (pts (xy 210.82 48.26) (xy 208.28 48.26)))
  (wire (pts (xy 35.56 35.56) (xy 35.56 50.8)))
  (wire (pts (xy 86.36 163.83) (xy 83.82 163.83)))
  (wire (pts (xy 233.68 44.45) (xy 228.6 44.45)))
  (wire (pts (xy 69.85 21.59) (xy 76.2 21.59)))
  (wire (pts (xy 226.06 149.86) (xy 226.06 151.13)))
  (wire (pts (xy 208.28 137.16) (xy 193.04 137.16)))
  (wire (pts (xy 63.5 21.59) (xy 63.5 17.78)))
  (wire (pts (xy 86.36 156.21) (xy 83.82 156.21)))
  (wire (pts (xy 72.39 45.72) (xy 72.39 38.1)))
  (wire (pts (xy 124.46 153.67) (xy 127 153.67)))
  (wire (pts (xy 69.85 45.72) (xy 72.39 45.72)))
  (wire (pts (xy 223.52 44.45) (xy 223.52 53.34)))
  (wire (pts (xy 181.61 58.42) (xy 177.8 58.42)))
  (wire (pts (xy 83.82 148.59) (xy 86.36 148.59)))
  (wire (pts (xy 54.61 88.9) (xy 54.61 91.44)))
  (wire (pts (xy 45.72 83.82) (xy 45.72 76.2)))
  (wire (pts (xy 107.95 54.61) (xy 114.3 54.61)))
  (wire (pts (xy 76.2 26.67) (xy 76.2 30.48)))
  (wire (pts (xy 243.84 66.04) (xy 250.19 66.04)))
  (wire (pts (xy 66.04 93.98) (xy 66.04 100.33)))
  (wire (pts (xy 247.65 27.94) (xy 254 27.94)))
  (wire (pts (xy 154.94 62.23) (xy 154.94 64.77)))
  (wire (pts (xy 193.04 101.6) (xy 208.28 101.6)))
  (wire (pts (xy 63.5 21.59) (xy 64.77 21.59)))
  (wire (pts (xy 80.01 93.98) (xy 66.04 93.98)))
  (wire (pts (xy 158.75 99.06) (xy 153.67 99.06)))
  (wire (pts (xy 46.99 138.43) (xy 53.34 138.43)))
  (wire (pts (xy 124.46 163.83) (xy 124.46 170.18)))
  (wire (pts (xy 35.56 20.32) (xy 35.56 19.05)))
  (wire (pts (xy 154.94 49.53) (xy 167.64 49.53)))
  (wire (pts (xy 193.04 121.92) (xy 208.28 121.92)))
  (wire (pts (xy 162.56 55.88) (xy 162.56 64.77)))
  (wire (pts (xy 83.82 156.21) (xy 83.82 148.59)))
  (wire (pts (xy 76.2 26.67) (xy 82.55 26.67)))
  (wire (pts (xy 35.56 20.32) (xy 35.56 30.48)))
  (wire (pts (xy 250.19 83.82) (xy 243.84 83.82)))
  (wire (pts (xy 54.61 81.28) (xy 80.01 81.28)))
  (wire (pts (xy 45.72 76.2) (xy 45.72 72.39)))
  (wire (pts (xy 243.84 81.28) (xy 250.19 81.28)))
  (wire (pts (xy 34.29 86.36) (xy 80.01 86.36)))
  (wire (pts (xy 181.61 63.5) (xy 177.8 63.5)))
  (wire (pts (xy 83.82 163.83) (xy 83.82 156.21)))
  (wire (pts (xy 240.03 151.13) (xy 228.6 151.13)))
  (wire (pts (xy 54.61 81.28) (xy 54.61 76.2)))
  (wire (pts (xy 45.72 100.33) (xy 34.29 100.33)))
  (wire (pts (xy 190.5 26.67) (xy 190.5 21.59)))
  (wire (pts (xy 45.72 100.33) (xy 54.61 100.33)))
  (wire (pts (xy 250.19 68.58) (xy 243.84 68.58)))
  (wire (pts (xy 45.72 91.44) (xy 45.72 83.82)))
  (wire (pts (xy 177.8 58.42) (xy 177.8 63.5)))
  (wire (pts (xy 156.21 156.21) (xy 143.51 156.21)))
  (wire (pts (xy 124.46 148.59) (xy 127 148.59)))
  (wire (pts (xy 193.04 99.06) (xy 208.28 99.06)))
  (wire (pts (xy 138.43 121.92) (xy 140.97 121.92)))
  (wire (pts (xy 60.96 78.74) (xy 80.01 78.74)))
  (wire (pts (xy 34.29 100.33) (xy 34.29 96.52)))
  (wire (pts (xy 72.39 45.72) (xy 74.93 45.72)))
  (wire (pts (xy 228.6 44.45) (xy 226.06 44.45)))
  (wire (pts (xy 46.99 173.99) (xy 53.34 173.99)))
  (wire (pts (xy 193.04 91.44) (xy 208.28 91.44)))
  (wire (pts (xy 45.72 96.52) (xy 45.72 100.33)))
  (wire (pts (xy 46.99 115.57) (xy 53.34 115.57)))
  (wire (pts (xy 193.04 106.68) (xy 208.28 106.68)))
  (wire (pts (xy 83.82 143.51) (xy 83.82 148.59)))
  (wire (pts (xy 124.46 156.21) (xy 143.51 156.21)))
  (wire (pts (xy 154.94 45.72) (xy 162.56 45.72)))
  (wire (pts (xy 66.04 100.33) (xy 62.23 100.33)))
  (wire (pts (xy 66.04 71.12) (xy 80.01 71.12)))
  (wire (pts (xy 208.28 58.42) (xy 208.28 60.96)))
  (wire (pts (xy 208.28 44.45) (xy 208.28 43.18)))
  (wire (pts (xy 218.44 48.26) (xy 218.44 53.34)))
  (wire (pts (xy 87.63 123.19) (xy 87.63 124.46)))
  (wire (pts (xy 208.28 83.82) (xy 193.04 83.82)))
  (wire (pts (xy 19.05 31.75) (xy 19.05 50.8)))
  (wire (pts (xy 208.28 88.9) (xy 193.04 88.9)))
  (wire (pts (xy 193.04 104.14) (xy 208.28 104.14)))
  (wire (pts (xy 226.06 151.13) (xy 228.6 151.13)))
  (wire (pts (xy 76.2 30.48) (xy 71.12 30.48)))
  (wire (pts (xy 54.61 96.52) (xy 54.61 100.33)))
  (wire (pts (xy 53.34 127) (xy 46.99 127)))
  (wire (pts (xy 63.5 35.56) (xy 63.5 45.72)))
  (wire (pts (xy 127 151.13) (xy 124.46 151.13)))
  (wire (pts (xy 19.05 20.32) (xy 35.56 20.32)))
  (wire (pts (xy 54.61 76.2) (xy 45.72 76.2)))
  (wire (pts (xy 186.69 63.5) (xy 198.12 63.5)))
  (wire (pts (xy 54.61 88.9) (xy 80.01 88.9)))
  (wire (pts (xy 83.82 50.8) (xy 83.82 45.72)))
  (wire (pts (xy 186.69 58.42) (xy 198.12 58.42)))
  (wire (pts (xy 193.04 116.84) (xy 208.28 116.84)))
  (wire (pts (xy 226.06 44.45) (xy 226.06 53.34)))
  (wire (pts (xy 208.28 73.66) (xy 193.04 73.66)))
  (wire (pts (xy 184.15 71.12) (xy 208.28 71.12)))
  (wire (pts (xy 54.61 100.33) (xy 62.23 100.33)))
  (wire (pts (xy 63.5 25.4) (xy 63.5 21.59)))
  (wire (pts (xy 105.41 49.53) (xy 105.41 58.42)))
  (wire (pts (xy 193.04 124.46) (xy 208.28 124.46)))
  (wire (pts (xy 80.01 45.72) (xy 83.82 45.72)))
  (wire (pts (xy 64.77 45.72) (xy 63.5 45.72)))
  (wire (pts (xy 193.04 119.38) (xy 208.28 119.38)))
  (wire (pts (xy 190.5 38.1) (xy 190.5 31.75)))
  (wire (pts (xy 162.56 64.77) (xy 154.94 64.77)))
  (wire (pts (xy 54.61 81.28) (xy 54.61 88.9)))
  (wire (pts (xy 80.01 73.66) (xy 66.04 73.66)))
  (wire (pts (xy 193.04 132.08) (xy 208.28 132.08)))
  (wire (pts (xy 193.04 139.7) (xy 208.28 139.7)))
  (wire (pts (xy 208.28 63.5) (xy 198.12 63.5)))
  (wire (pts (xy 34.29 86.36) (xy 34.29 76.2)))
  (wire (pts (xy 198.12 58.42) (xy 208.28 58.42)))
  (wire (pts (xy 154.94 52.07) (xy 158.75 52.07)))
  (wire (pts (xy 66.04 76.2) (xy 80.01 76.2)))
  (wire (pts (xy 181.61 76.2) (xy 208.28 76.2)))
  (wire (pts (xy 72.39 38.1) (xy 82.55 38.1)))
  (wire (pts (xy 34.29 76.2) (xy 45.72 76.2)))
  (wire (pts (xy 193.04 93.98) (xy 208.28 93.98)))
  (text "vbat 2xAAA\n" (at 22.86 41.91 90))
  (label "VDDA" (at 66.04 83.82 0))
  (label "D10" (at 193.04 106.68 0))
  (label "RXD" (at 250.19 119.38 0))
  (label "FLASH_CS" (at 193.04 93.98 0))
  (label "DISP_SCS" (at 181.61 76.2 0))
  (label "FLASH_MISO" (at 193.04 96.52 0))
  (label "DISP_SCS" (at 66.04 76.2 0))
  (label "vmon_en" (at 184.15 71.12 0))
  (label "A7" (at 193.04 78.74 0))
  (label "reset" (at 193.04 144.78 0))
  (label "reset" (at 247.65 27.94 0))
  (label "DISP_SI" (at 66.04 73.66 0))
  (label "SWCLK" (at 153.67 104.14 0))
  (label "vmon" (at 82.55 38.1 0))
  (label "D8" (at 193.04 76.2 0))
  (label "A3" (at 193.04 71.12 0))
  (label "DISP_MODE" (at 66.04 88.9 0))
  (label "DISP_COMIN" (at 66.04 78.74 0))
  (label "D5" (at 193.04 99.06 0))
  (label "FLASH_CS" (at 156.21 156.21 180))
  (label "D-" (at 193.04 121.92 0))
  (label "DISP_SCLK" (at 66.04 71.12 0))
  (label "D10" (at 53.34 115.57 0))
  (label "SWCLK" (at 193.04 137.16 0))
  (label "D5" (at 53.34 138.43 0))
  (label "D-" (at 158.75 54.61 0))
  (label "MOSI" (at 250.19 86.36 0))
  (label "A2" (at 250.19 83.82 0))
  (label "RXLED" (at 250.19 68.58 0))
  (label "TXLED" (at 193.04 129.54 0))
  (label "VDD" (at 66.04 86.36 0))
  (label "D7" (at 53.34 162.56 0))
  (label "DISP_COMIN" (at 180.34 86.36 0))
  (label "SDA" (at 193.04 116.84 0))
  (label "D-" (at 107.95 54.61 0))
  (label "reset" (at 158.75 99.06 0))
  (label "AREF" (at 193.04 68.58 0))
  (label "FLASH_MOSI" (at 127 151.13 0))
  (label "FLASH_SCK" (at 193.04 83.82 0))
  (label "D0" (at 193.04 88.9 0))
  (label "FLASH_MISO" (at 127 153.67 0))
  (label "D12" (at 53.34 195.58 0))
  (label "FLASH_MOSI" (at 193.04 81.28 0))
  (label "D+" (at 107.95 52.07 0))
  (label "SCL" (at 193.04 119.38 0))
  (label "D12" (at 193.04 109.22 0))
  (label "D11" (at 193.04 101.6 0))
  (label "A4" (at 193.04 73.66 0))
  (label "SWDIO" (at 193.04 139.7 0))
  (label "D13" (at 193.04 104.14 0))
  (label "VSS" (at 66.04 91.44 0))
  (label "D7" (at 193.04 114.3 0))
  (label "MISO" (at 193.04 91.44 0))
  (label "DISP_SI" (at 260.35 86.36 0))
  (label "A5" (at 53.34 184.15 0))
  (label "A1" (at 250.19 81.28 0))
  (label "D+" (at 158.75 52.07 0))
  (label "D6" (at 53.34 173.99 0))
  (label "FLASH_SCK" (at 127 148.59 0))
  (label "D1" (at 193.04 86.36 0))
  (label "A0" (at 193.04 66.04 0))
  (label "D11" (at 53.34 151.13 0))
  (label "D+" (at 193.04 124.46 0))
  (label "DISP_SCLK" (at 260.35 88.9 0))
  (label "SCK" (at 250.19 88.9 0))
  (label "A1" (at 91.44 120.65 0))
  (label "TXD" (at 250.19 116.84 0))
  (label "vmon_en" (at 82.55 26.67 0))
  (label "D6" (at 193.04 111.76 0))
  (label "A5" (at 250.19 66.04 0))
  (label "SWDIO" (at 153.67 106.68 0))
  (label "vmon" (at 181.61 78.74 0))
  (label "VSSA" (at 66.04 93.98 0))
  (label "DISP_EN" (at 66.04 81.28 0))
  (label "D13" (at 53.34 127 0))
  (global_label "usb_host_en" (shape input) (at 193.04 132.08 180) (fields_autoplaced)
    (property "Intersheet References" "${INTERSHEET_REFS}" (id 0) (at 0 0 0))
  )
  (symbol (lib_id "pawpet-v5-rescue:ATSAMD21G18A-A-MCU_Microchip_SAMD") (at 226.06 101.6 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "U1" (id 0) (at 226.06 152.1206 0))
    (property "Value" "ATSAMD21G18A-A" (id 1) (at 226.06 154.432 0))
    (property "Footprint" "Package_QFP:TQFP-48-1EP_7x7mm_P0.5mm_EP5x5mm" (id 2) (at 248.92 148.59 0))
    (property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/SAM_D21_DA1_Family_Data%20Sheet_DS40001882E.pdf" (id 3) (at 226.06 76.2 0))
    (pin "1")
    (pin "10")
    (pin "11")
    (pin "12")
    (pin "13")
    (pin "14")
    (pin "15")
    (pin "16")
    (pin "17")
    (pin "18")
    (pin "19")
    (pin "2")
    (pin "20")
    (pin "21")
    (pin "22")
    (pin "23")
    (pin "24")
    (pin "25")
    (pin "26")
    (pin "27")
    (pin "28")
    (pin "29")
    (pin "3")
    (pin "30")
    (pin "31")
    (pin "32")
    (pin "33")
    (pin "34")
    (pin "35")
    (pin "36")
    (pin "37")
    (pin "38")
    (pin "39")
    (pin "4")
    (pin "40")
    (pin "41")
    (pin "42")
    (pin "43")
    (pin "44")
    (pin "45")
    (pin "46")
    (pin "47")
    (pin "48")
    (pin "49")
    (pin "5")
    (pin "6")
    (pin "7")
    (pin "8")
    (pin "9")
  )
  (symbol (lib_id "pawpet-v5-rescue:C_Small-Device") (at 54.61 93.98 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C6" (id 0) (at 56.9468 92.8116 0))
    (property "Value" "0.1uF" (id 1) (at 56.9468 95.123 0))
    (property "Footprint" "Capacitor_SMD:C_0805_2012Metric" (id 2) (at 54.61 93.98 0))
    (property "Datasheet" "~" (id 3) (at 54.61 93.98 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "pawpet-v5-rescue:SW_Push-Switch") (at 41.91 115.57 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "SW_A1" (id 0) (at 41.91 108.331 0))
    (property "Value" "SW_Push" (id 1) (at 41.91 110.6424 0))
    (property "Footprint" "Button_Switch_SMD:SW_SPST_EVQQ2" (id 2) (at 41.91 110.49 0))
    (property "Datasheet" "~" (id 3) (at 41.91 110.49 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "pawpet-v5-rescue:C_Small-Device") (at 45.72 93.98 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C5" (id 0) (at 48.0568 92.8116 0))
    (property "Value" "1uF" (id 1) (at 48.0568 95.123 0))
    (property "Footprint" "Capacitor_SMD:C_0805_2012Metric" (id 2) (at 45.72 93.98 0))
    (property "Datasheet" "~" (id 3) (at 45.72 93.98 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "pawpet-v5-rescue:C_Small-Device") (at 34.29 93.98 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C4" (id 0) (at 36.6268 92.8116 0))
    (property "Value" "1uF" (id 1) (at 36.6268 95.123 0))
    (property "Footprint" "Capacitor_SMD:C_0805_2012Metric" (id 2) (at 34.29 93.98 0))
    (property "Datasheet" "~" (id 3) (at 34.29 93.98 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "pawpet-v5-rescue:SW_Push-Switch") (at 41.91 127 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "SW_B1" (id 0) (at 41.91 119.761 0))
    (property "Value" "SW_Push" (id 1) (at 41.91 122.0724 0))
    (property "Footprint" "Button_Switch_SMD:SW_SPST_EVQQ2" (id 2) (at 41.91 121.92 0))
    (property "Datasheet" "~" (id 3) (at 41.91 121.92 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "pawpet-v5-rescue:SW_Push-Switch") (at 41.91 138.43 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "SW_C1" (id 0) (at 41.91 131.191 0))
    (property "Value" "SW_Push" (id 1) (at 41.91 133.5024 0))
    (property "Footprint" "Button_Switch_SMD:SW_SPST_EVQQ2" (id 2) (at 41.91 133.35 0))
    (property "Datasheet" "~" (id 3) (at 41.91 133.35 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "pawpet-v5-rescue:SW_Push-Switch") (at 41.91 151.13 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "SW_P1" (id 0) (at 41.91 143.891 0))
    (property "Value" "SW_Push" (id 1) (at 41.91 146.2024 0))
    (property "Footprint" "Button_Switch_SMD:SW_SPST_EVQQ2" (id 2) (at 41.91 146.05 0))
    (property "Datasheet" "~" (id 3) (at 41.91 146.05 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "pawpet-v5-rescue:SW_Push-Switch") (at 41.91 162.56 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "SW_LEFT1" (id 0) (at 41.91 155.321 0))
    (property "Value" "SW_Push" (id 1) (at 41.91 157.6324 0))
    (property "Footprint" "Button_Switch_SMD:SW_SPST_EVQQ2" (id 2) (at 41.91 157.48 0))
    (property "Datasheet" "~" (id 3) (at 41.91 157.48 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "pawpet-v5-rescue:SW_Push-Switch") (at 41.91 173.99 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "SW_RIGHT1" (id 0) (at 41.91 166.751 0))
    (property "Value" "SW_Push" (id 1) (at 41.91 169.0624 0))
    (property "Footprint" "Button_Switch_SMD:SW_SPST_EVQQ2" (id 2) (at 41.91 168.91 0))
    (property "Datasheet" "~" (id 3) (at 41.91 168.91 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "pawpet-v5-rescue:SW_Push-Switch") (at 41.91 184.15 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "SW_UP1" (id 0) (at 41.91 176.911 0))
    (property "Value" "SW_Push" (id 1) (at 41.91 179.2224 0))
    (property "Footprint" "Button_Switch_SMD:SW_SPST_EVQQ2" (id 2) (at 41.91 179.07 0))
    (property "Datasheet" "~" (id 3) (at 41.91 179.07 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "pawpet-v5-rescue:SW_Push-Switch") (at 41.91 195.58 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "SW_DOWN1" (id 0) (at 41.91 188.341 0))
    (property "Value" "SW_Push" (id 1) (at 41.91 190.6524 0))
    (property "Footprint" "Button_Switch_SMD:SW_SPST_EVQQ2" (id 2) (at 41.91 190.5 0))
    (property "Datasheet" "~" (id 3) (at 41.91 190.5 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "pawpet-v5-rescue:GND-power") (at 45.72 100.33 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR03" (id 0) (at 45.72 106.68 0))
    (property "Value" "GND" (id 1) (at 45.847 104.7242 0))
    (property "Footprint" "" (id 2) (at 45.72 100.33 0))
    (property "Datasheet" "" (id 3) (at 45.72 100.33 0))
    (pin "1")
  )
  (symbol (lib_id "pawpet-v5-rescue:+3.3V-power") (at 45.72 72.39 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR02" (id 0) (at 45.72 76.2 0))
    (property "Value" "+3.3V" (id 1) (at 46.101 67.9958 0))
    (property "Footprint" "" (id 2) (at 45.72 72.39 0))
    (property "Datasheet" "" (id 3) (at 45.72 72.39 0))
    (pin "1")
  )
  (symbol (lib_id "pawpet-v5-rescue:+3.3V-power") (at 208.28 43.18 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR0101" (id 0) (at 208.28 46.99 0))
    (property "Value" "+3.3V" (id 1) (at 208.661 38.7858 0))
    (property "Footprint" "" (id 2) (at 208.28 43.18 0))
    (property "Datasheet" "" (id 3) (at 208.28 43.18 0))
    (pin "1")
  )
  (symbol (lib_id "pawpet-v5-rescue:C_Small-Device") (at 213.36 48.26 90) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C3" (id 0) (at 213.36 54.0766 90))
    (property "Value" "1uF" (id 1) (at 213.36 51.7652 90))
    (property "Footprint" "Capacitor_SMD:C_0805_2012Metric" (id 2) (at 213.36 48.26 0))
    (property "Datasheet" "~" (id 3) (at 213.36 48.26 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "pawpet-v5-rescue:GND-power") (at 208.28 48.26 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR0102" (id 0) (at 208.28 54.61 0))
    (property "Value" "GND" (id 1) (at 208.407 51.5112 90))
    (property "Footprint" "" (id 2) (at 208.28 48.26 0))
    (property "Datasheet" "" (id 3) (at 208.28 48.26 0))
    (pin "1")
  )
  (symbol (lib_id "pawpet-v5-rescue:GND-power") (at 240.03 151.13 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR0103" (id 0) (at 240.03 157.48 0))
    (property "Value" "GND" (id 1) (at 240.157 154.3812 90))
    (property "Footprint" "" (id 2) (at 240.03 151.13 0))
    (property "Datasheet" "" (id 3) (at 240.03 151.13 0))
    (pin "1")
  )
  (symbol (lib_id "pawpet-v5-rescue:C_Small-Device") (at 184.15 58.42 270) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C1" (id 0) (at 184.15 52.6034 90))
    (property "Value" "22pF" (id 1) (at 184.15 54.9148 90))
    (property "Footprint" "Capacitor_SMD:C_0805_2012Metric" (id 2) (at 184.15 58.42 0))
    (property "Datasheet" "~" (id 3) (at 184.15 58.42 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "pawpet-v5-rescue:C_Small-Device") (at 184.15 63.5 90) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C2" (id 0) (at 184.15 69.3166 90))
    (property "Value" "22pF" (id 1) (at 184.15 67.0052 90))
    (property "Footprint" "Capacitor_SMD:C_0805_2012Metric" (id 2) (at 184.15 63.5 0))
    (property "Datasheet" "~" (id 3) (at 184.15 63.5 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "pawpet-v5-rescue:Crystal_Small-Device") (at 198.12 60.96 270) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "Y1" (id 0) (at 200.3552 59.7916 90))
    (property "Value" "32,768" (id 1) (at 200.3552 62.103 90))
    (property "Footprint" "Crystal:Crystal_SMD_2012-2Pin_2.0x1.2mm" (id 2) (at 198.12 60.96 0))
    (property "Datasheet" "~" (id 3) (at 198.12 60.96 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "pawpet-v5-rescue:GND-power") (at 177.8 63.5 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR0105" (id 0) (at 177.8 69.85 0))
    (property "Value" "GND" (id 1) (at 177.927 66.7512 90))
    (property "Footprint" "" (id 2) (at 177.8 63.5 0))
    (property "Datasheet" "" (id 3) (at 177.8 63.5 0))
    (pin "1")
  )
  (symbol (lib_id "pawpet-v5-rescue:GND-power") (at 36.83 115.57 270) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR0106" (id 0) (at 30.48 115.57 0))
    (property "Value" "GND" (id 1) (at 33.5788 115.697 90))
    (property "Footprint" "" (id 2) (at 36.83 115.57 0))
    (property "Datasheet" "" (id 3) (at 36.83 115.57 0))
    (pin "1")
  )
  (symbol (lib_id "pawpet-v5-rescue:GND-power") (at 36.83 127 270) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR0107" (id 0) (at 30.48 127 0))
    (property "Value" "GND" (id 1) (at 33.5788 127.127 90))
    (property "Footprint" "" (id 2) (at 36.83 127 0))
    (property "Datasheet" "" (id 3) (at 36.83 127 0))
    (pin "1")
  )
  (symbol (lib_id "pawpet-v5-rescue:GND-power") (at 36.83 151.13 270) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR0108" (id 0) (at 30.48 151.13 0))
    (property "Value" "GND" (id 1) (at 33.5788 151.257 90))
    (property "Footprint" "" (id 2) (at 36.83 151.13 0))
    (property "Datasheet" "" (id 3) (at 36.83 151.13 0))
    (pin "1")
  )
  (symbol (lib_id "pawpet-v5-rescue:GND-power") (at 36.83 138.43 270) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR0109" (id 0) (at 30.48 138.43 0))
    (property "Value" "GND" (id 1) (at 33.5788 138.557 90))
    (property "Footprint" "" (id 2) (at 36.83 138.43 0))
    (property "Datasheet" "" (id 3) (at 36.83 138.43 0))
    (pin "1")
  )
  (symbol (lib_id "pawpet-v5-rescue:GND-power") (at 36.83 162.56 270) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR0110" (id 0) (at 30.48 162.56 0))
    (property "Value" "GND" (id 1) (at 33.5788 162.687 90))
    (property "Footprint" "" (id 2) (at 36.83 162.56 0))
    (property "Datasheet" "" (id 3) (at 36.83 162.56 0))
    (pin "1")
  )
  (symbol (lib_id "pawpet-v5-rescue:GND-power") (at 36.83 173.99 270) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR0111" (id 0) (at 30.48 173.99 0))
    (property "Value" "GND" (id 1) (at 33.5788 174.117 90))
    (property "Footprint" "" (id 2) (at 36.83 173.99 0))
    (property "Datasheet" "" (id 3) (at 36.83 173.99 0))
    (pin "1")
  )
  (symbol (lib_id "pawpet-v5-rescue:GND-power") (at 36.83 184.15 270) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR0112" (id 0) (at 30.48 184.15 0))
    (property "Value" "GND" (id 1) (at 33.5788 184.277 90))
    (property "Footprint" "" (id 2) (at 36.83 184.15 0))
    (property "Datasheet" "" (id 3) (at 36.83 184.15 0))
    (pin "1")
  )
  (symbol (lib_id "pawpet-v5-rescue:GND-power") (at 36.83 195.58 270) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR0113" (id 0) (at 30.48 195.58 0))
    (property "Value" "GND" (id 1) (at 33.5788 195.707 90))
    (property "Footprint" "" (id 2) (at 36.83 195.58 0))
    (property "Datasheet" "" (id 3) (at 36.83 195.58 0))
    (pin "1")
  )
  (symbol (lib_id "pawpet-v5-rescue:52892-1033-molex") (at 77.47 71.12 270) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "J3" (id 0) (at 76.0984 76.6318 90))
    (property "Value" "MOLEX" (id 1) (at 76.0984 78.6384 90))
    (property "Footprint" "molex:Molex-52892-1033-Manufacturer_Recommended" (id 2) (at 77.47 71.12 0))
    (property "Datasheet" "~" (id 3) (at 77.47 71.12 0))
    (pin "1")
    (pin "10")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
    (pin "6")
    (pin "7")
    (pin "8")
    (pin "9")
    (pin "MP1")
    (pin "MP2")
  )
  (symbol (lib_id "pawpet-v5-rescue:GND-power") (at 19.05 50.8 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR018" (id 0) (at 19.05 57.15 0))
    (property "Value" "GND" (id 1) (at 19.177 55.1942 0))
    (property "Footprint" "" (id 2) (at 19.05 50.8 0))
    (property "Datasheet" "" (id 3) (at 19.05 50.8 0))
    (pin "1")
  )
  (symbol (lib_id "pawpet-v5-rescue:C_Small-Device") (at 35.56 33.02 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C8" (id 0) (at 37.8968 31.8516 0))
    (property "Value" "10uF" (id 1) (at 37.8968 34.163 0))
    (property "Footprint" "Capacitor_SMD:C_0805_2012Metric" (id 2) (at 35.56 33.02 0))
    (property "Datasheet" "~" (id 3) (at 35.56 33.02 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "pawpet-v5-rescue:MX25V1635FM1I-macronix") (at 83.82 148.59 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "U3" (id 0) (at 105.41 141.859 0))
    (property "Value" "MX25R1635FM1IL0" (id 1) (at 105.41 144.1704 0))
    (property "Footprint" "Package_SO:SOIC-8_5.23x5.23mm_P1.27mm" (id 2) (at 83.82 163.83 0))
    (property "Datasheet" "http://www.macronix.com/Lists/Datasheet/Attachments/7534/MX25R3235F,%20Wide%20Range,%2032Mb,%20v1.6.pdf" (id 3) (at 83.82 148.59 0))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
    (pin "6")
    (pin "7")
    (pin "8")
  )
  (symbol (lib_id "pawpet-v5-rescue:GND-power") (at 124.46 170.18 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR013" (id 0) (at 124.46 176.53 0))
    (property "Value" "GND" (id 1) (at 124.587 174.5742 0))
    (property "Footprint" "" (id 2) (at 124.46 170.18 0))
    (property "Datasheet" "" (id 3) (at 124.46 170.18 0))
    (pin "1")
  )
  (symbol (lib_id "pawpet-v5-rescue:+3.3V-power") (at 83.82 143.51 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR012" (id 0) (at 83.82 147.32 0))
    (property "Value" "+3.3V" (id 1) (at 84.201 139.1158 0))
    (property "Footprint" "" (id 2) (at 83.82 143.51 0))
    (property "Datasheet" "" (id 3) (at 83.82 143.51 0))
    (pin "1")
  )
  (symbol (lib_id "pawpet-v5-rescue:R_Small-Device") (at 143.51 148.59 180) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R1" (id 0) (at 142.0114 149.7584 0))
    (property "Value" "100k" (id 1) (at 142.0114 147.447 0))
    (property "Footprint" "Resistor_SMD:R_0805_2012Metric" (id 2) (at 143.51 148.59 0))
    (property "Datasheet" "~" (id 3) (at 143.51 148.59 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "pawpet-v5-rescue:+3.3V-power") (at 143.51 146.05 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR07" (id 0) (at 143.51 149.86 0))
    (property "Value" "+3.3V" (id 1) (at 143.891 141.6558 0))
    (property "Footprint" "" (id 2) (at 143.51 146.05 0))
    (property "Datasheet" "" (id 3) (at 143.51 146.05 0))
    (pin "1")
  )
  (symbol (lib_id "pawpet-v5-rescue:SW_Push-Switch") (at 259.08 27.94 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "SW_reset1" (id 0) (at 259.08 20.701 0))
    (property "Value" "reset" (id 1) (at 259.08 23.0124 0))
    (property "Footprint" "pawpet:SW_SPST_PTS810_handsolder" (id 2) (at 259.08 22.86 0))
    (property "Datasheet" "~" (id 3) (at 259.08 22.86 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "pawpet-v5-rescue:GND-power") (at 264.16 27.94 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR020" (id 0) (at 264.16 34.29 0))
    (property "Value" "GND" (id 1) (at 264.287 32.3342 0))
    (property "Footprint" "" (id 2) (at 264.16 27.94 0))
    (property "Datasheet" "" (id 3) (at 264.16 27.94 0))
    (pin "1")
  )
  (symbol (lib_id "pawpet-v5-rescue:Speaker_Crystal-Device") (at 80.01 123.19 180) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "LS1" (id 0) (at 80.8736 112.5982 0))
    (property "Value" "beep" (id 1) (at 80.8736 114.9096 0))
    (property "Footprint" "Buzzer_Beeper:Buzzer_Murata_PKMCS0909E4000-R1" (id 2) (at 80.899 121.92 0))
    (property "Datasheet" "~" (id 3) (at 80.899 121.92 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "pawpet-v5-rescue:GND-power") (at 87.63 124.46 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR019" (id 0) (at 87.63 130.81 0))
    (property "Value" "GND" (id 1) (at 87.757 128.8542 0))
    (property "Footprint" "" (id 2) (at 87.63 124.46 0))
    (property "Datasheet" "" (id 3) (at 87.63 124.46 0))
    (pin "1")
  )
  (symbol (lib_id "pawpet-v5-rescue:R_Small-Device") (at 87.63 120.65 270) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R2" (id 0) (at 87.63 115.6716 90))
    (property "Value" "470" (id 1) (at 87.63 117.983 90))
    (property "Footprint" "Resistor_SMD:R_0805_2012Metric" (id 2) (at 87.63 120.65 0))
    (property "Datasheet" "~" (id 3) (at 87.63 120.65 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "pawpet-v5-rescue:Conn_ARM_JTAG_SWD_10-Connector") (at 140.97 106.68 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "J2" (id 0) (at 129.7178 105.5116 0))
    (property "Value" "Conn_ARM_JTAG_SWD_10" (id 1) (at 129.7178 107.823 0))
    (property "Footprint" "Connector:Tag-Connect_TC2030-IDC-NL_2x03_P1.27mm_Vertical" (id 2) (at 140.97 106.68 0))
    (property "Datasheet" "http://infocenter.arm.com/help/topic/com.arm.doc.ddi0314h/DDI0314H_coresight_components_trm.pdf" (id 3) (at 132.08 138.43 90))
    (pin "1")
    (pin "10")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
    (pin "6")
    (pin "7")
    (pin "8")
    (pin "9")
  )
  (symbol (lib_id "pawpet-v5-rescue:GND-power") (at 138.43 121.92 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR0114" (id 0) (at 138.43 128.27 0))
    (property "Value" "GND" (id 1) (at 138.557 125.1712 90))
    (property "Footprint" "" (id 2) (at 138.43 121.92 0))
    (property "Datasheet" "" (id 3) (at 138.43 121.92 0))
    (pin "1")
  )
  (symbol (lib_id "pawpet-v5-rescue:+3.3V-power") (at 140.97 91.44 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR0115" (id 0) (at 140.97 95.25 0))
    (property "Value" "+3.3V" (id 1) (at 141.351 88.1888 90))
    (property "Footprint" "" (id 2) (at 140.97 91.44 0))
    (property "Datasheet" "" (id 3) (at 140.97 91.44 0))
    (pin "1")
  )
  (symbol (lib_id "pawpet-v5-rescue:R_Small-Device") (at 67.31 45.72 270) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R3" (id 0) (at 67.31 40.7416 90))
    (property "Value" "100k" (id 1) (at 67.31 43.053 90))
    (property "Footprint" "Resistor_SMD:R_0805_2012Metric" (id 2) (at 67.31 45.72 0))
    (property "Datasheet" "~" (id 3) (at 67.31 45.72 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "pawpet-v5-rescue:R_Small-Device") (at 77.47 45.72 270) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R4" (id 0) (at 77.47 40.7416 90))
    (property "Value" "100k" (id 1) (at 77.47 43.053 90))
    (property "Footprint" "Resistor_SMD:R_0805_2012Metric" (id 2) (at 77.47 45.72 0))
    (property "Datasheet" "~" (id 3) (at 77.47 45.72 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "pawpet-v5-rescue:GND-power") (at 83.82 50.8 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR0104" (id 0) (at 83.82 57.15 0))
    (property "Value" "GND" (id 1) (at 83.947 55.1942 0))
    (property "Footprint" "" (id 2) (at 83.82 50.8 0))
    (property "Datasheet" "" (id 3) (at 83.82 50.8 0))
    (pin "1")
  )
  (symbol (lib_id "pawpet-v5-rescue:Battery-Device") (at 19.05 26.67 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "BT1" (id 0) (at 21.7932 25.5016 0))
    (property "Value" "Battery" (id 1) (at 21.7932 27.813 0))
    (property "Footprint" "pawpet:BAT_BC2AAAPC" (id 2) (at 19.05 25.146 90))
    (property "Datasheet" "~" (id 3) (at 19.05 25.146 90))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "pawpet-v5-rescue:C_Small-Device") (at 190.5 29.21 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C9" (id 0) (at 192.8368 28.0416 0))
    (property "Value" "10uF" (id 1) (at 192.8368 30.353 0))
    (property "Footprint" "Capacitor_SMD:C_0805_2012Metric" (id 2) (at 190.5 29.21 0))
    (property "Datasheet" "~" (id 3) (at 190.5 29.21 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "power:+3.3V") (at 190.5 21.59 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR0121" (id 0) (at 190.5 25.4 0))
    (property "Value" "+3.3V" (id 1) (at 190.881 17.1958 0))
    (property "Footprint" "" (id 2) (at 190.5 21.59 0))
    (property "Datasheet" "" (id 3) (at 190.5 21.59 0))
    (pin "1")
  )
  (symbol (lib_id "power:GND") (at 190.5 38.1 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR0122" (id 0) (at 190.5 44.45 0))
    (property "Value" "GND" (id 1) (at 190.627 42.4942 0))
    (property "Footprint" "" (id 2) (at 190.5 38.1 0))
    (property "Datasheet" "" (id 3) (at 190.5 38.1 0))
    (pin "1")
  )
  (symbol (lib_id "power:+3.3V") (at 35.56 19.05 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR0116" (id 0) (at 35.56 22.86 0))
    (property "Value" "+3.3V" (id 1) (at 35.941 14.6558 0))
    (property "Footprint" "" (id 2) (at 35.56 19.05 0))
    (property "Datasheet" "" (id 3) (at 35.56 19.05 0))
    (pin "1")
  )
  (symbol (lib_id "Transistor_FET:DMG2301L") (at 66.04 30.48 180) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "Q1" (id 0) (at 60.833 29.3116 0))
    (property "Value" "DMG2301L" (id 1) (at 60.833 31.623 0))
    (property "Footprint" "Package_TO_SOT_SMD:SOT-23" (id 2) (at 60.96 28.575 0))
    (property "Datasheet" "https://www.diodes.com/assets/Datasheets/DMG2301L.pdf" (id 3) (at 66.04 30.48 0))
    (pin "1")
    (pin "2")
    (pin "3")
  )
  (symbol (lib_id "Device:R_Small") (at 162.56 53.34 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R7" (id 0) (at 164.0586 52.1716 0))
    (property "Value" "1k" (id 1) (at 164.0586 54.483 0))
    (property "Footprint" "Resistor_SMD:R_0805_2012Metric" (id 2) (at 162.56 53.34 0))
    (property "Datasheet" "~" (id 3) (at 162.56 53.34 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "pawpet-v5-rescue:R_Small-Device") (at 67.31 21.59 270) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R6" (id 0) (at 67.31 16.6116 90))
    (property "Value" "100k" (id 1) (at 67.31 18.923 90))
    (property "Footprint" "Resistor_SMD:R_0805_2012Metric" (id 2) (at 67.31 21.59 0))
    (property "Datasheet" "~" (id 3) (at 67.31 21.59 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "usb-c:USB4105-GF-A") (at 134.62 54.61 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "J1" (id 0) (at 134.62 37.6682 0))
    (property "Value" "USB4105-GF-A" (id 1) (at 134.62 39.9796 0))
    (property "Footprint" "gct:GCT_USB4105-GF-A" (id 2) (at 134.62 54.61 0))
    (property "Datasheet" "" (id 3) (at 134.62 54.61 0))
    (property "MANUFACTURER" "GCT" (id 4) (at 134.62 54.61 0))
    (property "PARTREV" "A3" (id 5) (at 134.62 54.61 0))
    (property "STANDARD" "Manufacturer Recommendations" (id 6) (at 134.62 54.61 0))
    (property "MAXIMUM_PACKAGE_HEIGHT" "3.31 mm" (id 7) (at 134.62 54.61 0))
    (pin "A1_B12")
    (pin "A4_B9")
    (pin "A5")
    (pin "A6")
    (pin "A7")
    (pin "A8")
    (pin "B1_A12")
    (pin "B4_A9")
    (pin "B5")
    (pin "B6")
    (pin "B7")
    (pin "B8")
    (pin "S1")
    (pin "S2")
    (pin "S3")
    (pin "S4")
  )
  (symbol (lib_id "power:GND") (at 35.56 50.8 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR0123" (id 0) (at 35.56 57.15 0))
    (property "Value" "GND" (id 1) (at 35.687 55.1942 0))
    (property "Footprint" "" (id 2) (at 35.56 50.8 0))
    (property "Datasheet" "" (id 3) (at 35.56 50.8 0))
    (pin "1")
  )
  (symbol (lib_id "pawpet-v5-rescue:GND-power") (at 154.94 67.31 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR0118" (id 0) (at 154.94 73.66 0))
    (property "Value" "GND" (id 1) (at 155.067 71.7042 0))
    (property "Footprint" "" (id 2) (at 154.94 67.31 0))
    (property "Datasheet" "" (id 3) (at 154.94 67.31 0))
    (pin "1")
  )
  (symbol (lib_id "Device:R_Small") (at 105.41 60.96 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R5" (id 0) (at 106.9086 59.7916 0))
    (property "Value" "5.1k" (id 1) (at 106.9086 62.103 0))
    (property "Footprint" "Resistor_SMD:R_0805_2012Metric" (id 2) (at 105.41 60.96 0))
    (property "Datasheet" "~" (id 3) (at 105.41 60.96 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "pawpet-v5-rescue:GND-power") (at 105.41 67.31 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR0119" (id 0) (at 105.41 73.66 0))
    (property "Value" "GND" (id 1) (at 105.537 71.7042 0))
    (property "Footprint" "" (id 2) (at 105.41 67.31 0))
    (property "Datasheet" "" (id 3) (at 105.41 67.31 0))
    (pin "1")
  )
  (symbol (lib_id "Device:R_Small") (at 167.64 60.96 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R8" (id 0) (at 169.1386 59.7916 0))
    (property "Value" "5.1k" (id 1) (at 169.1386 62.103 0))
    (property "Footprint" "Resistor_SMD:R_0805_2012Metric" (id 2) (at 167.64 60.96 0))
    (property "Datasheet" "~" (id 3) (at 167.64 60.96 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "pawpet-v5-rescue:GND-power") (at 167.64 67.31 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR04" (id 0) (at 167.64 73.66 0))
    (property "Value" "GND" (id 1) (at 167.767 71.7042 0))
    (property "Footprint" "" (id 2) (at 167.64 67.31 0))
    (property "Datasheet" "" (id 3) (at 167.64 67.31 0))
    (pin "1")
  )
  (symbol (lib_id "power:+3.3V") (at 63.5 17.78 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR01" (id 0) (at 63.5 21.59 0))
    (property "Value" "+3.3V" (id 1) (at 63.881 13.3858 0))
    (property "Footprint" "" (id 2) (at 63.5 17.78 0))
    (property "Datasheet" "" (id 3) (at 63.5 17.78 0))
    (pin "1")
  )
  (symbol (lib_id "Connector:TestPoint_Small") (at 60.96 78.74 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "TP1" (id 0) (at 62.103 77.8315 0))
    (property "Value" "TestPoint_Small" (id 1) (at 62.103 80.6066 0))
    (property "Footprint" "TestPoint:TestPoint_Pad_1.0x1.0mm" (id 2) (at 66.04 78.74 0))
    (property "Datasheet" "~" (id 3) (at 66.04 78.74 0))
    (pin "1")
  )
  (sheet_instances
    (path (page "1"))
  )
  (symbol_instances
    (path
      (reference "#PWR01") (unit 1) (value "+3.3V") (footprint "")
    )
    (path
      (reference "#PWR02") (unit 1) (value "+3.3V") (footprint "")
    )
    (path
      (reference "#PWR03") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR04") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR07") (unit 1) (value "+3.3V") (footprint "")
    )
    (path
      (reference "#PWR012") (unit 1) (value "+3.3V") (footprint "")
    )
    (path
      (reference "#PWR013") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR018") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR019") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR020") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR0101") (unit 1) (value "+3.3V") (footprint "")
    )
    (path
      (reference "#PWR0102") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR0103") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR0104") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR0105") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR0106") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR0107") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR0108") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR0109") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR0110") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR0111") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR0112") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR0113") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR0114") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR0115") (unit 1) (value "+3.3V") (footprint "")
    )
    (path
      (reference "#PWR0116") (unit 1) (value "+3.3V") (footprint "")
    )
    (path
      (reference "#PWR0118") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR0119") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR0121") (unit 1) (value "+3.3V") (footprint "")
    )
    (path
      (reference "#PWR0122") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR0123") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "BT1") (unit 1) (value "Battery") (footprint "pawpet:BAT_BC2AAAPC")
    )
    (path
      (reference "C1") (unit 1) (value "22pF") (footprint "Capacitor_SMD:C_0805_2012Metric")
    )
    (path
      (reference "C2") (unit 1) (value "22pF") (footprint "Capacitor_SMD:C_0805_2012Metric")
    )
    (path
      (reference "C3") (unit 1) (value "1uF") (footprint "Capacitor_SMD:C_0805_2012Metric")
    )
    (path
      (reference "C4") (unit 1) (value "1uF") (footprint "Capacitor_SMD:C_0805_2012Metric")
    )
    (path
      (reference "C5") (unit 1) (value "1uF") (footprint "Capacitor_SMD:C_0805_2012Metric")
    )
    (path
      (reference "C6") (unit 1) (value "0.1uF") (footprint "Capacitor_SMD:C_0805_2012Metric")
    )
    (path
      (reference "C8") (unit 1) (value "10uF") (footprint "Capacitor_SMD:C_0805_2012Metric")
    )
    (path
      (reference "C9") (unit 1) (value "10uF") (footprint "Capacitor_SMD:C_0805_2012Metric")
    )
    (path
      (reference "J1") (unit 1) (value "USB4105-GF-A") (footprint "gct:GCT_USB4105-GF-A")
    )
    (path
      (reference "J2") (unit 1) (value "Conn_ARM_JTAG_SWD_10") (footprint "Connector:Tag-Connect_TC2030-IDC-NL_2x03_P1.27mm_Vertical")
    )
    (path
      (reference "J3") (unit 1) (value "MOLEX") (footprint "molex:Molex-52892-1033-Manufacturer_Recommended")
    )
    (path
      (reference "LS1") (unit 1) (value "beep") (footprint "Buzzer_Beeper:Buzzer_Murata_PKMCS0909E4000-R1")
    )
    (path
      (reference "Q1") (unit 1) (value "DMG2301L") (footprint "Package_TO_SOT_SMD:SOT-23")
    )
    (path
      (reference "R1") (unit 1) (value "100k") (footprint "Resistor_SMD:R_0805_2012Metric")
    )
    (path
      (reference "R2") (unit 1) (value "470") (footprint "Resistor_SMD:R_0805_2012Metric")
    )
    (path
      (reference "R3") (unit 1) (value "100k") (footprint "Resistor_SMD:R_0805_2012Metric")
    )
    (path
      (reference "R4") (unit 1) (value "100k") (footprint "Resistor_SMD:R_0805_2012Metric")
    )
    (path
      (reference "R5") (unit 1) (value "5.1k") (footprint "Resistor_SMD:R_0805_2012Metric")
    )
    (path
      (reference "R6") (unit 1) (value "100k") (footprint "Resistor_SMD:R_0805_2012Metric")
    )
    (path
      (reference "R7") (unit 1) (value "1k") (footprint "Resistor_SMD:R_0805_2012Metric")
    )
    (path
      (reference "R8") (unit 1) (value "5.1k") (footprint "Resistor_SMD:R_0805_2012Metric")
    )
    (path
      (reference "SW_A1") (unit 1) (value "SW_Push") (footprint "Button_Switch_SMD:SW_SPST_EVQQ2")
    )
    (path
      (reference "SW_B1") (unit 1) (value "SW_Push") (footprint "Button_Switch_SMD:SW_SPST_EVQQ2")
    )
    (path
      (reference "SW_C1") (unit 1) (value "SW_Push") (footprint "Button_Switch_SMD:SW_SPST_EVQQ2")
    )
    (path
      (reference "SW_DOWN1") (unit 1) (value "SW_Push") (footprint "Button_Switch_SMD:SW_SPST_EVQQ2")
    )
    (path
      (reference "SW_LEFT1") (unit 1) (value "SW_Push") (footprint "Button_Switch_SMD:SW_SPST_EVQQ2")
    )
    (path
      (reference "SW_P1") (unit 1) (value "SW_Push") (footprint "Button_Switch_SMD:SW_SPST_EVQQ2")
    )
    (path
      (reference "SW_RIGHT1") (unit 1) (value "SW_Push") (footprint "Button_Switch_SMD:SW_SPST_EVQQ2")
    )
    (path
      (reference "SW_UP1") (unit 1) (value "SW_Push") (footprint "Button_Switch_SMD:SW_SPST_EVQQ2")
    )
    (path
      (reference "SW_reset1") (unit 1) (value "reset") (footprint "pawpet:SW_SPST_PTS810_handsolder")
    )
    (path
      (reference "TP1") (unit 1) (value "TestPoint_Small") (footprint "TestPoint:TestPoint_Pad_1.0x1.0mm")
    )
    (path
      (reference "U1") (unit 1) (value "ATSAMD21G18A-A") (footprint "Package_QFP:TQFP-48-1EP_7x7mm_P0.5mm_EP5x5mm")
    )
    (path
      (reference "U3") (unit 1) (value "MX25R1635FM1IL0") (footprint "Package_SO:SOIC-8_5.23x5.23mm_P1.27mm")
    )
    (path
      (reference "Y1") (unit 1) (value "32,768") (footprint "Crystal:Crystal_SMD_2012-2Pin_2.0x1.2mm")
    )
  )
)
