<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.0.1">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="43.485" y2="0" width="0" layer="20"/>
<wire x1="43.485" y1="0" x2="43.485" y2="35.55" width="0" layer="20"/>
<wire x1="43.485" y1="35.55" x2="0" y2="35.55" width="0" layer="20"/>
<wire x1="0" y1="35.55" x2="0" y2="0" width="0" layer="20"/>
<text>USB</text>
<text>3V3</text>
<text>Gnd</text>
<text>GP0</text>
<text>GP1</text>
<text>GP2</text>
<text>GP3</text>
<text>RST</text>
<text>Gnd</text>
<text>R</text>
<text>T</text>
<text>Wireless Laser</text>
<text>sjm4306</text>
<text>110321</text>
<text>JLCJLCJLCJLC</text>
<text>5V</text>
<text>HC-06</text>
<hole x="2.54" y="33.02" drill="3.1"/>
<hole x="2.54" y="2.54" drill="3.1"/>
<text>3.3V</text>
</plain>
<libraries>
<library name="adafruit">
<packages>
<package name="C0603K">
<description>&lt;b&gt;Ceramic Chip Capacitor KEMET 0603 Reflow solder&lt;/b&gt;&lt;p&gt;
Metric Code Size 1608</description>
</package>
<package name="R0603">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="PANASONIC_B">
<description>&lt;b&gt;Panasonic Aluminium Electrolytic Capacitor VS-Serie Package B&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="CHIP-LED0805">
<description>&lt;b&gt;Hyper CHIPLED Hyper-Bright LED&lt;/b&gt;&lt;p&gt;
LB R99A&lt;br&gt;
Source: http://www.osram.convergy.de/ ... lb_r99a.pdf</description>
</package>
</packages>
</library>
<library name="esp8266modules">
<packages>
<package name="ESP01">
<description>ESP8266 Module 01</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X09_LOCK">
<description>&lt;h3&gt;Plated Through Hole -9 Pin Locking Footprint&lt;/h3&gt;
Holes are offset 0.005" to lock pins in place during soldering. 
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:9&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_09&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X04_LOCK">
<description>&lt;h3&gt;Plated Through Hole - 4 Pin Locking Footprint&lt;/h3&gt;
Pins are offset 0.005" from center to lock pins in place during soldering. 
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:4&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_04&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="sjm4306_LOGO">
<packages>
<package name="SJM4306_MEDIUM_NO_MASK">
</package>
<package name="SJM4306_LOGO_SMALL">
</package>
<package name="SJM4306_LOGO_LARGE">
</package>
</packages>
</library>
<library name="IC">
<description>&lt;h3&gt; PCBLayout.com - Frequently Used &lt;i&gt;  IC's, Voltage regulators, Op-amps,Timer and RTCs IC's&lt;/i&gt;&lt;/h3&gt;

Visit us at &lt;a href="http://www.PCBLayout.com"&gt;PCBLayout.com&lt;/a&gt; for quick and hassle-free PCB Layout/Manufacturing ordering experience.
&lt;BR&gt;
&lt;BR&gt;
This library has been generated by our experienced pcb layout engineers using current IPC and/or industry standards. We &lt;b&gt;believe&lt;/b&gt; the content to be accurate, complete and current. But, this content is provided as a courtesy and &lt;u&gt;user assumes all risk and responsiblity of it's usage&lt;/u&gt;.
&lt;BR&gt;
&lt;BR&gt;
Feel free to contact us at &lt;a href="mailto:Support@PCBLayout.com"&gt;Support@PCBLayout.com&lt;/a&gt; if you have any questions/concerns regarding any of our content or services.</description>
<packages>
<package name="SOT-223">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="adafruit" package="C0603K" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="adafruit" package="PANASONIC_B" value="100uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="adafruit" package="C0603K" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C8" library="adafruit" package="C0603K" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C9" library="adafruit" package="C0603K" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="L" library="adafruit" package="CHIP-LED0805" value="Green">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="P" library="adafruit" package="CHIP-LED0805" value="Red">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="adafruit" package="R0603" value="1K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="adafruit" package="R0603" value="1K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$1" library="esp8266modules" package="ESP01" value="ESP01">
<attribute name="VALUE"/>
</element>
<element name="R1" library="adafruit" package="R0603" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="adafruit" package="R0603" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R8" library="adafruit" package="R0603" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$4" library="sjm4306_LOGO" package="SJM4306_MEDIUM_NO_MASK" value=""/>
<element name="U$5" library="sjm4306_LOGO" package="SJM4306_LOGO_SMALL" value=""/>
<element name="U$6" library="sjm4306_LOGO" package="SJM4306_LOGO_LARGE" value=""/>
<element name="U2" library="IC" package="SOT-223" value="NCP1117ST33T3G">
<attribute name="CREATED_BY" value="PCBLayout.com"/>
<attribute name="DIGIKEY_PART_NUMBER" value="NCP1117ST33T3GOSTR-ND"/>
<attribute name="MANUFACTURER" value="ON Semiconductor"/>
<attribute name="MPN" value="NCP1117ST33T3G"/>
<attribute name="NAME"/>
<attribute name="PACKAGE" value="SOT-223"/>
</element>
<element name="J2" library="SparkFun-Connectors" package="1X09_LOCK" value="">
<attribute name="VALUE"/>
</element>
<element name="R10" library="adafruit" package="R0603" value="1K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R11" library="adafruit" package="R0603" value="2K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J1" library="SparkFun-Connectors" package="1X04_LOCK" value="">
<attribute name="PROD_ID" value="CONN-09696"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="C1" pad="2"/>
<contactref element="R2" pad="1"/>
<contactref element="C4" pad="2"/>
<contactref element="C2" pad="-"/>
<contactref element="C8" pad="2"/>
<contactref element="C9" pad="2"/>
<contactref element="U$1" pad="GND"/>
<contactref element="U2" pad="1"/>
<contactref element="J2" pad="3"/>
<contactref element="J2" pad="9"/>
<contactref element="J1" pad="2"/>
<contactref element="R11" pad="1"/>
</signal>
<signal name="RST">
<contactref element="U$1" pad="RST"/>
<contactref element="R1" pad="2"/>
<contactref element="J2" pad="8"/>
</signal>
<signal name="N$4">
<contactref element="P" pad="C"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="+5V">
<contactref element="C9" pad="1"/>
<contactref element="C1" pad="1"/>
<contactref element="P" pad="A"/>
<contactref element="U2" pad="3"/>
<contactref element="J2" pad="1"/>
<contactref element="J1" pad="1"/>
</signal>
<signal name="+3V3">
<contactref element="C8" pad="1"/>
<contactref element="U$1" pad="VCC"/>
<contactref element="C4" pad="1"/>
<contactref element="C2" pad="+"/>
<contactref element="R1" pad="1"/>
<contactref element="U$1" pad="CH_PD"/>
<contactref element="R4" pad="1"/>
<contactref element="R8" pad="1"/>
<contactref element="R3" pad="2"/>
<contactref element="J2" pad="2"/>
<contactref element="U2" pad="2"/>
<contactref element="U2" pad="4"/>
</signal>
<signal name="RXE">
<contactref element="J2" pad="7"/>
<contactref element="R10" pad="1"/>
</signal>
<signal name="TXE">
<contactref element="U$1" pad="TX"/>
<contactref element="J2" pad="5"/>
<contactref element="J1" pad="3"/>
</signal>
<signal name="FLSH">
<contactref element="R8" pad="2"/>
<contactref element="U$1" pad="GPIO0"/>
<contactref element="J2" pad="4"/>
</signal>
<signal name="N$1">
<contactref element="R3" pad="1"/>
<contactref element="L" pad="A"/>
</signal>
<signal name="GPIO2">
<contactref element="L" pad="C"/>
<contactref element="U$1" pad="GPIO2"/>
<contactref element="R4" pad="2"/>
<contactref element="J2" pad="6"/>
</signal>
<signal name="RXD">
<contactref element="U$1" pad="RX"/>
<contactref element="R10" pad="2"/>
<contactref element="R11" pad="2"/>
<contactref element="J1" pad="4"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
