(kicad_pcb (version 20211014) (generator pcbnew)
  (general
    (thickness 4.69)
  )
  (paper "A4")
  (title_block
    (title "NC085PSU-01-02 Solar Super Cap Power Supply")
    (date "2022-02-01")
    (rev "A")
    (company "NorTroN Microelectronics")
    (comment 1 "8 Cooper Close")
    (comment 2 "Glenroy NSW 2640")
  )
  (layers
    (0 "F.Cu" signal)
    (1 "In1.Cu" power "GND")
    (2 "In2.Cu" power "VCC")
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "In1.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 2" (type "prepreg") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "In2.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 3" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (grid_origin 100 160)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (disableapertmacros false)
      (usegerberextensions true)
      (usegerberattributes true)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue false)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk true)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "GND")
  (net 2 "/SN1")
  (net 3 "Net-(C6-Pad1)")
  (net 4 "Net-(D1-PadK)")
  (net 5 "/L")
  (net 6 "Net-(D1-PadA)")
  (net 7 "Net-(LK4-Pad1)")
  (net 8 "Net-(Q2-Pad3)")
  (net 9 "Net-(LK5-Pad1)")
  (net 10 "Net-(Q4-Pad1)")
  (net 11 "/DN1")
  (net 12 "Net-(Q5-Pad1)")
  (net 13 "/DN2")
  (net 14 "Net-(Q6-Pad1)")
  (net 15 "/Power")
  (net 16 "VCC")
  (net 17 "Net-(LK1-Pad3)")
  (net 18 "Net-(LK1-Pad2)")
  (net 19 "Net-(LK1-Pad1)")
  (net 20 "Net-(R14-Pad2)")
  (net 21 "Net-(C8-Pad1)")
  (net 22 "Net-(Q4-Pad3)")
  (net 23 "unconnected-(H1-Pad1)")
  (net 24 "Net-(FB2-Pad1)")
  (net 25 "Net-(J1-Pad3)")
  (net 26 "Net-(J1-Pad6)")
  (net 27 "Net-(J1-Pad7)")
  (net 28 "Net-(LK2-Pad1)")
  (net 29 "unconnected-(U3-Pad6)")
  (net 30 "unconnected-(U3-Pad7)")
  (net 31 "unconnected-(U3-Pad5)")
  (net 32 "Net-(Q2-Pad1)")
  (net 33 "Net-(J1-Pad4)")
  (net 34 "Net-(J1-Pad5)")
  (footprint "Capacitor_Tantalum_SMD:CP_EIA-3216-10_Kemet-I" (layer "F.Cu")
    (tedit 5B301BBE)
    (at 143 99.2 90)
    (descr "Tantalum Capacitor SMD Kemet-I (3216-10 Metric), IPC_7351 nominal, (Body size from: http://www.kemet.com/Lists/ProductCatalog/Attachments/253/KEM_TC101_STD.pdf), generated with kicad-footprint-generator")
    (tags "capacitor tantalum")
    (property "Sheetfile" "NC085PSU.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C1" (at 2.55 1.2 -180) (layer "F.SilkS"))
    (fp_text value "10uF  X7R Ceramic" (at -0.1 -1.2 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -1.35 0 90) (size 1.4 1.35) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1851851852)
      (net 15 "/Power") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1.35 0 90) (size 1.4 1.35) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1851851852)
      (net 1 "GND") (pintype "passive"))
    (model "Capacitor_Tantalum_SMD.3dshapes/CP_EIA-3216-10_Kemet-I.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "F.Cu")
    (tedit 5B301BBE)
    (at 144.75 104 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "NC085PSU.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C2" (at 0 -1) (layer "F.SilkS"))
    (fp_text value "100nF" (at 0 -1.55) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.485 0 90) (size 0.59 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 15 "/Power") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.485 0 90) (size 0.59 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3_Pad" (layer "F.Cu")
    (tedit 6212D45C)
    (at 135 112)
    (descr "Mounting Hole 3.2mm, M3")
    (tags "mounting hole 3.2mm m3")
    (property "Sheetfile" "NC085PSU.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "H1" (at 3.9 -1.8) (layer "F.SilkS"))
    (fp_text value "MountingHole_Pad" (at 0 1.75) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0) (size 6 6) (drill 3) (layers *.Cu *.Mask)
      (net 23 "unconnected-(H1-Pad1)") (pinfunction "1") (pintype "input") (clearance 0.5))
  )
  (footprint "Resistor_SMD:R_0402_1005Metric" (layer "F.Cu")
    (tedit 5B301BBD)
    (at 147.75 106.4)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "NC085PSU.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R20" (at 0 1.25) (layer "F.SilkS"))
    (fp_text value "220K" (at 0 0.8) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.485 0) (size 0.59 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 20 "Net-(R14-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.485 0) (size 0.59 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0402_1005Metric" (layer "F.Cu")
    (tedit 5B301BBD)
    (at 150.7 106.2 -90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "NC085PSU.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R21" (at 1.45 -1.05) (layer "F.SilkS"))
    (fp_text value "220K" (at 0.4 -1.35) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 -90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.485 0 270) (size 0.59 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 18 "Net-(LK1-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.485 0 270) (size 0.59 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "F.Cu")
    (tedit 5B301BBE)
    (at 150.5 99.55 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "NC085PSU.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C7" (at 0.55 1.15) (layer "F.SilkS"))
    (fp_text value "100nF" (at 1.15 0 180) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.485 0 90) (size 0.59 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 16 "VCC") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.485 0 90) (size 0.59 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_Tantalum_SMD:CP_EIA-3216-10_Kemet-I" (layer "F.Cu")
    (tedit 5B301BBE)
    (at 155.2 102 -90)
    (descr "Tantalum Capacitor SMD Kemet-I (3216-10 Metric), IPC_7351 nominal, (Body size from: http://www.kemet.com/Lists/ProductCatalog/Attachments/253/KEM_TC101_STD.pdf), generated with kicad-footprint-generator")
    (tags "capacitor tantalum")
    (property "Sheetfile" "NC085PSU.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C4" (at -2.9 0) (layer "F.SilkS"))
    (fp_text value "22uF/6V" (at 0 -1.25 -90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 -90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -1.35 0 270) (size 1.4 1.35) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1851851852)
      (net 16 "VCC") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1.35 0 270) (size 1.4 1.35) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1851851852)
      (net 1 "GND") (pintype "passive"))
    (model "Capacitor_Tantalum_SMD.3dshapes/CP_EIA-3216-10_Kemet-I.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "F.Cu")
    (tedit 5B301BBE)
    (at 151.45 102.1 -90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "NC085PSU.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C6" (at -0.35 -1.1) (layer "F.SilkS"))
    (fp_text value "100nF" (at -0.1 -1.45) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 -90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.485 0 270) (size 0.59 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "Net-(C6-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.485 0 270) (size 0.59 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0402_1005Metric" (layer "F.Cu")
    (tedit 5B301BBD)
    (at 143.2 128.2 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "NC085PSU.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R18" (at -2 0.1 180) (layer "F.SilkS"))
    (fp_text value "1M6" (at 0 -0.7 180) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 180) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.485 0 180) (size 0.59 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "/SN1") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.485 0 180) (size 0.59 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 14 "Net-(Q6-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23" (layer "F.Cu")
    (tedit 5A02FF57)
    (at 148.4 125.6 90)
    (descr "SOT-23, Standard")
    (tags "SOT-23")
    (property "Power" "1.3W")
    (property "Sheetfile" "NC085PSU.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "Q5" (at 1.5 1.5) (layer "F.SilkS"))
    (fp_text value "DMP1045U-7" (at -1.9 1.65 180) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 -180) (layer "F.Fab"))
    (pad "1" smd rect locked (at -1 -0.95 90) (size 0.9 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "Net-(Q5-Pad1)") (pinfunction "G") (pintype "input"))
    (pad "2" smd rect locked (at -1 0.95 90) (size 0.9 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "/Power") (pinfunction "S") (pintype "passive"))
    (pad "3" smd rect locked (at 1 0 90) (size 0.9 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 11 "/DN1") (pinfunction "D") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm" (layer "F.Cu")
    (tedit 5A02F2D3)
    (at 146.2 119.9)
    (descr "8-Lead Plastic Small Outline (SN) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification http://ww1.microchip.com/downloads/en/PackagingSpec/00000049BQ.pdf)")
    (tags "SOIC 1.27")
    (property "Sheetfile" "NC085PSU.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U1" (at 4.5 -2.1 180) (layer "F.SilkS"))
    (fp_text value "ALD910026SALI" (at 0.05 2.9) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect locked (at -2.7 -1.905) (size 1.55 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "V-") (pintype "power_in"))
    (pad "2" smd rect locked (at -2.7 -0.635) (size 1.55 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "/Power") (pinfunction "GN1") (pintype "power_in"))
    (pad "3" smd rect locked (at -2.7 0.635) (size 1.55 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "Net-(Q5-Pad1)") (pinfunction "DN1") (pintype "passive"))
    (pad "4" smd rect locked (at -2.7 1.905) (size 1.55 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "/SN1") (pinfunction "SN1") (pintype "power_in"))
    (pad "5" smd rect locked (at 2.7 1.905) (size 1.55 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "SN2") (pintype "power_in"))
    (pad "6" smd rect locked (at 2.7 0.635) (size 1.55 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 14 "Net-(Q6-Pad1)") (pinfunction "DN2") (pintype "passive"))
    (pad "7" smd rect locked (at 2.7 -0.635) (size 1.55 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "/SN1") (pinfunction "GN2") (pintype "power_out"))
    (pad "8" smd rect locked (at 2.7 -1.905) (size 1.55 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "/Power") (pinfunction "V+") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-8_3.9x4.9mm_P1.27mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_2512_6332Metric" (layer "F.Cu")
    (tedit 5B301BBD)
    (at 154.4 111.9 -90)
    (descr "Resistor SMD 2512 (6332 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "NC085PSU.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R16" (at 4.586 0.068) (layer "F.SilkS"))
    (fp_text value "24R/3W" (at 4 0) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 -90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -2.9 0 270) (size 1.35 3.35) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1851851852)
      (net 11 "/DN1") (pintype "passive"))
    (pad "2" smd roundrect locked (at 2.9 0 270) (size 1.35 3.35) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1851851852)
      (net 2 "/SN1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_2512_6332Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23" (layer "F.Cu")
    (tedit 5A02FF57)
    (at 144 125.6 90)
    (descr "SOT-23, Standard")
    (tags "SOT-23")
    (property "Power" "1.3W")
    (property "Sheetfile" "NC085PSU.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "Q6" (at 1.4 1.2) (layer "F.SilkS"))
    (fp_text value "DMP1045U-7" (at -1.85 0 180) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 -180) (layer "F.Fab"))
    (pad "1" smd rect locked (at -1 -0.95 90) (size 0.9 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 14 "Net-(Q6-Pad1)") (pinfunction "G") (pintype "input"))
    (pad "2" smd rect locked (at -1 0.95 90) (size 0.9 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "/SN1") (pinfunction "S") (pintype "passive"))
    (pad "3" smd rect locked (at 1 0 90) (size 0.9 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 13 "/DN2") (pinfunction "D") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Fiducial:Fiducial_0.5mm_Mask1mm" (layer "F.Cu")
    (tedit 5C18CB26)
    (at 163.4 95.6)
    (descr "Circular Fiducial, 0.5mm bare copper, 1mm soldermask opening (Level C)")
    (tags "fiducial")
    (property "Sheetfile" "NC085PSU.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "FID1" (at -1.95 0.3) (layer "F.SilkS"))
    (fp_text value "FIDUCIAL" (at 0 0.8) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" smd circle locked (at 0 0) (size 0.5 0.5) (layers "F.Cu" "F.Mask")
      (solder_mask_margin 0.25) (clearance 0.25))
  )
  (footprint "Resistor_SMD:R_2512_6332Metric" (layer "F.Cu")
    (tedit 5B301BBD)
    (at 154.4 122.4 -90)
    (descr "Resistor SMD 2512 (6332 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "NC085PSU.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R19" (at 4.5 0.068) (layer "F.SilkS"))
    (fp_text value "24R/3W" (at 4.05 -0.05) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 -90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -2.9 0 270) (size 1.35 3.35) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1851851852)
      (net 13 "/DN2") (pintype "passive"))
    (pad "2" smd roundrect locked (at 2.9 0 270) (size 1.35 3.35) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1851851852)
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_2512_6332Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23" (layer "F.Cu")
    (tedit 5A02FF57)
    (at 138 100.3 90)
    (descr "SOT-23, Standard")
    (tags "SOT-23")
    (property "Sheetfile" "NC085PSU.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "Q2" (at 0.75 2.2 180) (layer "F.SilkS"))
    (fp_text value "FDV304P" (at -1.85 0.05 180) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 180) (layer "F.Fab"))
    (pad "1" smd rect locked (at -1 -0.95 90) (size 0.9 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 32 "Net-(Q2-Pad1)") (pinfunction "G") (pintype "input"))
    (pad "2" smd rect locked (at -1 0.95 90) (size 0.9 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "/Power") (pinfunction "S") (pintype "passive"))
    (pad "3" smd rect locked (at 1 0 90) (size 0.9 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 8 "Net-(Q2-Pad3)") (pinfunction "D") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0402_1005Metric" (layer "F.Cu")
    (tedit 5B301BBD)
    (at 135.1 96.9 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "NC085PSU.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R12" (at 0 -1.3 270) (layer "F.SilkS"))
    (fp_text value "10K/±0.1%" (at 0.3 0.75 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.485 0 90) (size 0.59 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.485 0 90) (size 0.59 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 28 "Net-(LK2-Pad1)") (pintype "passive"))
    (model "Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23" (layer "F.Cu")
    (tedit 5FA16958)
    (at 139 104.5 180)
    (descr "SOT, 3 Pin (https://www.jedec.org/system/files/docs/to-236h.pdf variant AB), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "Category" "Discrete Semiconductor Products")
    (property "DK_Datasheet_Link" "https://www.diodes.com/assets/Datasheets/ds30041.pdf")
    (property "DK_Detail_Page" "/product-detail/en/diodes-incorporated/MMBT2222A-7-F/MMBT2222A-FDICT-ND/815723")
    (property "Description" "TRANS NPN 40V 0.6A SMD SOT23-3")
    (property "Digi-Key_PN" "MMBT2222A-FDICT-ND")
    (property "Family" "Transistors - Bipolar (BJT) - Single")
    (property "MPN" "MMBT2222A-7-F")
    (property "Manufacturer" "Diodes Incorporated")
    (property "Sheetfile" "NC085PSU.kicad_sch")
    (property "Sheetname" "")
    (property "Status" "Active")
    (attr smd)
    (fp_text reference "Q4" (at -2.6 -0.7 180) (layer "F.SilkS"))
    (fp_text value "MMBT2222A-7-F" (at -0.8 -1.85 180) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 180) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9375 -0.95 180) (size 1.475 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 10 "Net-(Q4-Pad1)") (pinfunction "B") (pintype "input"))
    (pad "2" smd roundrect (at -0.9375 0.95 180) (size 1.475 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "E") (pintype "input"))
    (pad "3" smd roundrect (at 0.9375 0 180) (size 1.475 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "Net-(Q4-Pad3)") (pinfunction "C") (pintype "input"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Inductor_SMD:L_Wuerth_MAPI-3015" (layer "F.Cu")
    (tedit 5990349D)
    (at 147.25 98.1)
    (descr "Inductor, Wuerth Elektronik, Wuerth_MAPI-3015, 3.0mmx3.0mm")
    (tags "inductor Wuerth smd")
    (property "Data" "SRN3015TA Shielded Wire-wound SMD Inductor with a Ferrite Core, 4.7 μH ±20% Semi-Shielded 1.2A Idc Q:12")
    (property "MPN" "SWPA5040S100MT")
    (property "SKU" "303010147")
    (property "Sheetfile" "NC085PSU.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "L1" (at 2.5 0) (layer "F.SilkS"))
    (fp_text value "4.7 μH 1.2A SRN3015TA" (at 0.2 -2.05) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect locked (at -1.05 0) (size 1.3 3.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "/Power") (pinfunction "1") (pintype "passive"))
    (pad "2" smd rect locked (at 1.05 0) (size 1.3 3.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "/L") (pinfunction "2") (pintype "passive"))
    (model "Inductor_SMD.3dshapes/L_Wuerth_MAPI-3015.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_SON:Texas_S-PVSON-N10_ThermalVias" (layer "F.Cu")
    (tedit 5A8E06E8)
    (at 147.75 102.8 -90)
    (descr "3x3mm Body, 0.5mm Pitch, S-PVSON-N10, DRC, http://www.ti.com/lit/ds/symlink/tps61201.pdf")
    (tags "0.5 S-PVSON-N10 DRC")
    (property "Sheetfile" "NC085PSU.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U2" (at 1.1 -2.35) (layer "F.SilkS"))
    (fp_text value "TPS61200DRC" (at -2.15 0) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.25 -0.75) (layer "F.Fab"))
    (pad "1" smd oval locked (at -1.475 -1 270) (size 0.85 0.28) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "Net-(C6-Pad1)") (pinfunction "VAUX") (pintype "bidirectional") (solder_mask_margin 0.07) (solder_paste_margin -0.025))
    (pad "1" smd rect locked (at -1.76 -1 270) (size 0.28 0.28) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "Net-(C6-Pad1)") (pinfunction "VAUX") (pintype "bidirectional") (solder_mask_margin 0.07) (solder_paste_margin -0.025))
    (pad "2" smd rect locked (at -1.76 -0.5 270) (size 0.28 0.28) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 16 "VCC") (pinfunction "VOUT") (pintype "power_out") (solder_mask_margin 0.07) (solder_paste_margin -0.025))
    (pad "2" smd oval locked (at -1.475 -0.5 270) (size 0.85 0.28) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 16 "VCC") (pinfunction "VOUT") (pintype "power_out") (solder_mask_margin 0.07) (solder_paste_margin -0.025))
    (pad "3" smd oval locked (at -1.475 0 270) (size 0.85 0.28) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "/L") (pinfunction "L") (pintype "input") (solder_mask_margin 0.07) (solder_paste_margin -0.025))
    (pad "3" smd rect locked (at -1.76 0 270) (size 0.28 0.28) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "/L") (pinfunction "L") (pintype "input") (solder_mask_margin 0.07) (solder_paste_margin -0.025))
    (pad "4" smd rect locked (at -1.76 0.5 270) (size 0.28 0.28) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "PGND") (pintype "power_in") (solder_mask_margin 0.07) (solder_paste_margin -0.025))
    (pad "4" smd oval locked (at -1.475 0.5 270) (size 0.85 0.28) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "PGND") (pintype "power_in") (solder_mask_margin 0.07) (solder_paste_margin -0.025))
    (pad "5" smd oval locked (at -1.475 1 270) (size 0.85 0.28) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "/Power") (pinfunction "VIN") (pintype "power_in") (solder_mask_margin 0.07) (solder_paste_margin -0.025))
    (pad "5" smd rect locked (at -1.76 1 270) (size 0.28 0.28) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "/Power") (pinfunction "VIN") (pintype "power_in") (solder_mask_margin 0.07) (solder_paste_margin -0.025))
    (pad "6" smd rect locked (at 1.76 1 270) (size 0.28 0.28) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "/Power") (pinfunction "EN") (pintype "input") (solder_mask_margin 0.07) (solder_paste_margin -0.025))
    (pad "6" smd oval locked (at 1.475 1 270) (size 0.85 0.28) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "/Power") (pinfunction "EN") (pintype "input") (solder_mask_margin 0.07) (solder_paste_margin -0.025))
    (pad "7" smd oval locked (at 1.475 0.5 270) (size 0.85 0.28) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 20 "Net-(R14-Pad2)") (pinfunction "UVLO") (pintype "input") (solder_mask_margin 0.07) (solder_paste_margin -0.025))
    (pad "7" smd rect locked (at 1.76 0.5 270) (size 0.28 0.28) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 20 "Net-(R14-Pad2)") (pinfunction "UVLO") (pintype "input") (solder_mask_margin 0.07) (solder_paste_margin -0.025))
    (pad "8" smd rect locked (at 1.76 0 270) (size 0.28 0.28) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "/Power") (pinfunction "PS") (pintype "input") (solder_mask_margin 0.07) (solder_paste_margin -0.025))
    (pad "8" smd oval locked (at 1.475 0 270) (size 0.85 0.28) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "/Power") (pinfunction "PS") (pintype "input") (solder_mask_margin 0.07) (solder_paste_margin -0.025))
    (pad "9" smd rect locked (at 1.76 -0.5 270) (size 0.28 0.28) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "GND") (pintype "power_in") (solder_mask_margin 0.07) (solder_paste_margin -0.025))
    (pad "9" smd oval locked (at 1.475 -0.5 270) (size 0.85 0.28) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "GND") (pintype "power_in") (solder_mask_margin 0.07) (solder_paste_margin -0.025))
    (pad "10" smd rect locked (at 1.76 -1 270) (size 0.28 0.28) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 18 "Net-(LK1-Pad2)") (pinfunction "FB") (pintype "input") (solder_mask_margin 0.07) (solder_paste_margin -0.025))
    (pad "10" smd oval locked (at 1.475 -1 270) (size 0.85 0.28) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 18 "Net-(LK1-Pad2)") (pinfunction "FB") (pintype "input") (solder_mask_margin 0.07) (solder_paste_margin -0.025))
    (pad "11" thru_hole circle locked (at 0.5 -0.75 270) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "PAD") (pintype "power_in"))
    (pad "11" thru_hole circle locked (at 0.5 0.75 270) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "PAD") (pintype "power_in"))
    (pad "11" smd rect locked (at 0 0 270) (size 1.65 2.4) (layers "F.Cu" "F.Mask")
      (net 1 "GND") (pinfunction "PAD") (pintype "power_in"))
    (pad "11" smd rect locked (at 0.25 -1.55 270) (size 0.28 0.7) (layers "F.Cu" "F.Mask")
      (net 1 "GND") (pinfunction "PAD") (pintype "power_in"))
    (pad "11" smd rect locked (at 0.25 -1.63 270) (size 0.26 0.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "PAD") (pintype "power_in"))
    (pad "11" smd rect locked (at 0 0 270) (size 2.3 2.8) (layers "B.Cu")
      (net 1 "GND") (pinfunction "PAD") (pintype "power_in"))
    (pad "11" smd rect locked (at 0.45 0.635 270) (size 0.68 1.05) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "PAD") (pintype "power_in"))
    (pad "11" smd rect locked (at 0.25 1.63 270) (size 0.26 0.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "PAD") (pintype "power_in"))
    (pad "11" thru_hole circle locked (at -0.5 -0.75 270) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "PAD") (pintype "power_in"))
    (pad "11" smd rect locked (at -0.45 -0.635 270) (size 0.68 1.05) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "PAD") (pintype "power_in"))
    (pad "11" smd rect locked (at -0.45 0.635 270) (size 0.68 1.05) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "PAD") (pintype "power_in"))
    (pad "11" smd rect locked (at -0.25 -1.63 270) (size 0.26 0.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "PAD") (pintype "power_in"))
    (pad "11" smd rect locked (at 0.45 -0.635 270) (size 0.68 1.05) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "PAD") (pintype "power_in"))
    (pad "11" smd rect locked (at -0.25 1.63 270) (size 0.26 0.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "PAD") (pintype "power_in"))
    (pad "11" smd rect locked (at 0.25 1.55 270) (size 0.28 0.7) (layers "F.Cu" "F.Mask")
      (net 1 "GND") (pinfunction "PAD") (pintype "power_in"))
    (pad "11" thru_hole circle locked (at 0 0 270) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "PAD") (pintype "power_in"))
    (pad "11" thru_hole circle locked (at -0.5 0.75 270) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "PAD") (pintype "power_in"))
    (pad "11" smd rect locked (at -0.25 -1.55 270) (size 0.28 0.7) (layers "F.Cu" "F.Mask")
      (net 1 "GND") (pinfunction "PAD") (pintype "power_in"))
    (pad "11" smd rect locked (at -0.25 1.55 270) (size 0.28 0.7) (layers "F.Cu" "F.Mask")
      (net 1 "GND") (pinfunction "PAD") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_SON.3dshapes/Texas_S-PVSON-N10.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "digikey-footprints:DO-214AC" (layer "F.Cu")
    (tedit 5AD0AAF4)
    (at 136.6 127.4)
    (property "Sheetfile" "NC085PSU.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "D1" (at 4.1 0.9 180) (layer "F.SilkS"))
    (fp_text value "SS14/1A" (at 0 1.75) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "A" smd rect locked (at 2 0) (size 2.5 1.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 6 "Net-(D1-PadA)") (pinfunction "A") (pintype "passive"))
    (pad "K" smd rect locked (at -2 0) (size 2.5 1.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "Net-(D1-PadK)") (pinfunction "K") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SMA.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "digikey-footprints:SOD-123" (layer "F.Cu")
    (tedit 5AD0B3EC)
    (at 136.6 124.4 180)
    (property "Category" "Discrete Semiconductor Products")
    (property "DK_Datasheet_Link" "https://www.diodes.com/assets/Datasheets/ds18010.pdf")
    (property "DK_Detail_Page" "/product-detail/en/diodes-incorporated/MMSZ5231B-7-F/MMSZ5231B-FDICT-ND/755506")
    (property "Description" "DIODE ZENER 5.1V 500MW SOD123")
    (property "Digi-Key_PN" "MMSZ5231B-FDICT-ND")
    (property "Family" "Diodes - Zener - Single")
    (property "MPN" "MMSZ5231B-7-F")
    (property "Manufacturer" "Diodes Incorporated")
    (property "Sheetfile" "NC085PSU.kicad_sch")
    (property "Sheetname" "")
    (property "Status" "Active")
    (property "Value2" "5V6/1W")
    (attr through_hole)
    (fp_text reference "Z1" (at -3.8 0) (layer "F.SilkS"))
    (fp_text value "KDZVTFTR5.6B" (at 0 -1.25 180) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 180) (layer "F.Fab"))
    (pad "A" smd rect locked (at 2.475 0 180) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pintype "passive"))
    (pad "K" smd rect locked (at -2.475 0 180) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "/Power") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SOD-123F.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1.4 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_2512_6332Metric" (layer "F.Cu")
    (tedit 5B301BBD)
    (at 136.6 121.3)
    (descr "Resistor SMD 2512 (6332 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "NC085PSU.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R13" (at -4.6 0.35) (layer "F.SilkS"))
    (fp_text value "PT2512FK-070R15L" (at -0.05 1.95) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -2.9 0) (size 1.35 3.35) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1851851852)
      (net 4 "Net-(D1-PadK)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 2.9 0) (size 1.35 3.35) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1851851852)
      (net 15 "/Power") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_2512_6332Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Fiducial:Fiducial_0.5mm_Mask1mm" (layer "F.Cu")
    (tedit 5C18CB26)
    (at 163.4 128.4)
    (descr "Circular Fiducial, 0.5mm bare copper, 1mm soldermask opening (Level C)")
    (tags "fiducial")
    (property "Sheetfile" "NC085PSU.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "FID2" (at -1.75 0) (layer "F.SilkS"))
    (fp_text value "FIDUCIAL" (at 0 0.9) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" smd circle locked (at 0 0) (size 0.5 0.5) (layers "F.Cu" "F.Mask")
      (solder_mask_margin 0.25) (clearance 0.25))
  )
  (footprint "Fiducial:Fiducial_0.5mm_Mask1mm" (layer "F.Cu")
    (tedit 5C18CB26)
    (at 131.6 128.4)
    (descr "Circular Fiducial, 0.5mm bare copper, 1mm soldermask opening (Level C)")
    (tags "fiducial")
    (property "Sheetfile" "NC085PSU.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "FID3" (at 1.1 -1.3 90) (layer "F.SilkS"))
    (fp_text value "FIDUCIAL" (at 0 0.75) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" smd circle locked (at 0 0) (size 0.5 0.5) (layers "F.Cu" "F.Mask")
      (solder_mask_margin 0.25) (clearance 0.25))
  )
  (footprint "Resistor_SMD:R_0402_1005Metric" (layer "F.Cu")
    (tedit 5B301BBD)
    (at 136.9 96.9 -90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "NC085PSU.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R8" (at 1.6 0 90) (layer "F.SilkS"))
    (fp_text value "10K/±0.1%" (at -0.3 -0.7 -90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 -90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.485 0 270) (size 0.59 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 28 "Net-(LK2-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.485 0 270) (size 0.59 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 8 "Net-(Q2-Pad3)") (pintype "passive"))
    (model "Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0402_1005Metric" (layer "F.Cu")
    (tedit 5B301BBD)
    (at 139 107.2)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "NC085PSU.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R7" (at 1.528 0 180) (layer "F.SilkS"))
    (fp_text value "10K" (at 0.05 0.7) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.485 0) (size 0.59 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 10 "Net-(Q4-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.485 0) (size 0.59 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 27 "Net-(J1-Pad7)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0402_1005Metric" (layer "F.Cu")
    (tedit 5B301BBD)
    (at 138.7 96.9 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "NC085PSU.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R2" (at -1.6 0.5 90) (layer "F.SilkS"))
    (fp_text value "10K" (at -1.05 0 180) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.485 0 90) (size 0.59 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 32 "Net-(Q2-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.485 0 90) (size 0.59 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 15 "/Power") (pintype "passive"))
    (model "Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0402_1005Metric" (layer "F.Cu")
    (tedit 5B301BBD)
    (at 147.6 128.2 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "NC085PSU.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R15" (at -1.9 0 180) (layer "F.SilkS"))
    (fp_text value "1M6" (at 0 -0.7 180) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 180) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.485 0 180) (size 0.59 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 15 "/Power") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.485 0 180) (size 0.59 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 12 "Net-(Q5-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "NorTroN:S-Link-3Way" (layer "F.Cu")
    (tedit 621D5463)
    (at 152.2 104.55 90)
    (descr "Solder Link 3way")
    (tags "Solder, Link")
    (property "Sheetfile" "NC085PSU.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "LK1" (at -1.85 0 180) (layer "F.SilkS"))
    (fp_text value "S-LINK-3WAY" (at 0.05 0.8 90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0.05 -1.1 90 unlocked) (layer "F.Fab"))
    (pad "1" smd rect (at -0.7 0 90) (size 0.5 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 19 "Net-(LK1-Pad1)") (pinfunction "1") (pintype "input"))
    (pad "2" smd rect (at 0 0 90) (size 0.5 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 18 "Net-(LK1-Pad2)") (pinfunction "2") (pintype "input"))
    (pad "3" smd rect (at 0.7 0 90) (size 0.5 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 17 "Net-(LK1-Pad3)") (pinfunction "3") (pintype "input"))
  )
  (footprint "Resistor_SMD:R_0402_1005Metric" (layer "F.Cu")
    (tedit 5B301BBD)
    (at 144.75 106.2 -90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "NC085PSU.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R14" (at -0.1 1.3) (layer "F.SilkS"))
    (fp_text value "820K" (at 1.2 0) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 -90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.485 0 270) (size 0.59 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 15 "/Power") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.485 0 270) (size 0.59 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 20 "Net-(R14-Pad2)") (pintype "passive"))
    (model "Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0402_1005Metric" (layer "F.Cu")
    (tedit 5B301BBD)
    (at 155.2 105.15 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "NC085PSU.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R17" (at 1.55 0.3) (layer "F.SilkS"))
    (fp_text value "2M" (at -1.35 0 180) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 180) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.485 0 180) (size 0.59 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 16 "VCC") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.485 0 180) (size 0.59 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 17 "Net-(LK1-Pad3)") (pintype "passive"))
    (model "Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0402_1005Metric" (layer "F.Cu")
    (tedit 5B301BBD)
    (at 155.2 106.35 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "NC085PSU.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R22" (at 0 -1.05) (layer "F.SilkS"))
    (fp_text value "1.2M" (at -1.7 0 180) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 180) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.485 0 180) (size 0.59 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 16 "VCC") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.485 0 180) (size 0.59 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 19 "Net-(LK1-Pad1)") (pintype "passive"))
    (model "Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0402_1005Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 146.1 110.8 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "NC085PSU.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R23" (at 1.55 -1.2 180) (layer "F.SilkS"))
    (fp_text value "10K" (at -1.15 0) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.51 0 90) (size 0.54 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 34 "Net-(J1-Pad5)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.51 0 90) (size 0.54 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 16 "VCC") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0402_1005Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 144.5 110.8 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "NC085PSU.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R26" (at 0 -1 270) (layer "F.SilkS"))
    (fp_text value "10K" (at 1.2 0) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.51 0 90) (size 0.54 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.51 0 90) (size 0.54 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 26 "Net-(J1-Pad6)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 142 111.7 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "NC085PSU.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "FB2" (at 0 -1.8 90) (layer "F.SilkS"))
    (fp_text value "MMZ2012Y152B" (at 1.55 -3.7 180) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 1.05 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1 0 90) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2083333333)
      (net 24 "Net-(FB2-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 1 0 90) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2083333333)
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0402_1005Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 147.3 110.8 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "NC085PSU.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R24" (at 1.4 0 180) (layer "F.SilkS"))
    (fp_text value "10K" (at 1.15 0 180) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.51 0 90) (size 0.54 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 33 "Net-(J1-Pad4)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.51 0 90) (size 0.54 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 16 "VCC") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0402_1005Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 133.3 103.3)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "NC085PSU.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R1" (at -1.5 0) (layer "F.SilkS"))
    (fp_text value "100R" (at -1.9 0) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.51 0) (size 0.54 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 32 "Net-(Q2-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.51 0) (size 0.54 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "Net-(Q4-Pad3)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0402_1005Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 133.3 104.7)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "NC085PSU.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R5" (at -1.5 0) (layer "F.SilkS"))
    (fp_text value "10K" (at -1.9 0) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.51 0) (size 0.54 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.51 0) (size 0.54 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 9 "Net-(LK5-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23-8" (layer "F.Cu")
    (tedit 5F6F9B37)
    (at 136.4 117.6 180)
    (descr "SOT, 8 Pin (https://www.jedec.org/sites/default/files/docs/Mo-178c.PDF variant BA), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "Sheetfile" "NC085PSU.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U4" (at 2.5 0.9) (layer "F.SilkS"))
    (fp_text value "INA219AxDCN" (at 0 1.85) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.1375 -0.975 180) (size 1.325 0.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "Net-(D1-PadK)") (pinfunction "IN+") (pintype "input"))
    (pad "2" smd roundrect (at -1.1375 -0.325 180) (size 1.325 0.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 15 "/Power") (pinfunction "IN-") (pintype "input"))
    (pad "3" smd roundrect (at -1.1375 0.325 180) (size 1.325 0.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "4" smd roundrect (at -1.1375 0.975 180) (size 1.325 0.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 16 "VCC") (pinfunction "VS") (pintype "power_in"))
    (pad "5" smd roundrect (at 1.1375 0.975 180) (size 1.325 0.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 34 "Net-(J1-Pad5)") (pinfunction "SCL") (pintype "input"))
    (pad "6" smd roundrect (at 1.1375 0.325 180) (size 1.325 0.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 33 "Net-(J1-Pad4)") (pinfunction "SDA") (pintype "bidirectional"))
    (pad "7" smd roundrect (at 1.1375 -0.325 180) (size 1.325 0.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 9 "Net-(LK5-Pad1)") (pinfunction "A0") (pintype "input"))
    (pad "8" smd roundrect (at 1.1375 -0.975 180) (size 1.325 0.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 7 "Net-(LK4-Pad1)") (pinfunction "A1") (pintype "input"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-8.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0402_1005Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 133.3 106.1)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "NC085PSU.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R4" (at -1.5 0) (layer "F.SilkS"))
    (fp_text value "10K" (at -1.9 0) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.51 0) (size 0.54 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.51 0) (size 0.54 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 7 "Net-(LK4-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "NorTroN:S-Link-2Way" (layer "F.Cu")
    (tedit 621D5402)
    (at 135.7 104.7)
    (descr "Solder Link 2way")
    (tags "Solder, Link")
    (property "Sheetfile" "NC085PSU.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "LK5" (at 1 -1.2) (layer "F.SilkS"))
    (fp_text value "S-LINK-2WAY" (at -1.1 0 90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -1 unlocked) (layer "F.Fab"))
    (pad "1" smd rect (at -0.35 0) (size 0.5 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "Net-(LK5-Pad1)") (pinfunction "1") (pintype "input"))
    (pad "2" smd rect (at 0.35 0) (size 0.5 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 16 "VCC") (pinfunction "2") (pintype "input"))
  )
  (footprint "Resistor_SMD:R_0402_1005Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 148.5 110.8 -90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "NC085PSU.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R25" (at -1.2 -1.1) (layer "F.SilkS"))
    (fp_text value "10K" (at 0 -0.75 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.51 0 270) (size 0.54 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 25 "Net-(J1-Pad3)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.51 0 270) (size 0.54 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 16 "VCC") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_SO:TSSOP-10_3x3mm_P0.5mm" (layer "F.Cu")
    (tedit 5F3E4A84)
    (at 145.9 114.2)
    (descr "TSSOP10: plastic thin shrink small outline package; 10 leads; body width 3 mm; (see NXP SSOP-TSSOP-VSO-REFLOW.pdf and sot552-1_po.pdf)")
    (tags "SSOP 0.5")
    (property "Sheetfile" "NC085PSU.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U3" (at 2.6 -1.8) (layer "F.SilkS"))
    (fp_text value "ADS1114IDGS" (at 0.05 1.9) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect (at -2.15 -1) (size 1.1 0.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 25 "Net-(J1-Pad3)") (pinfunction "ADDR") (pintype "input"))
    (pad "2" smd rect (at -2.15 -0.5) (size 1.1 0.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 26 "Net-(J1-Pad6)") (pinfunction "ALERT/RDY") (pintype "output"))
    (pad "3" smd rect (at -2.15 0) (size 1.1 0.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 24 "Net-(FB2-Pad1)") (pinfunction "GND") (pintype "power_in"))
    (pad "4" smd rect (at -2.15 0.5) (size 1.1 0.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 28 "Net-(LK2-Pad1)") (pinfunction "AIN0") (pintype "input"))
    (pad "5" smd rect (at -2.15 1) (size 1.1 0.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 31 "unconnected-(U3-Pad5)") (pinfunction "AIN1") (pintype "input"))
    (pad "6" smd rect (at 2.15 1) (size 1.1 0.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 29 "unconnected-(U3-Pad6)") (pintype "no_connect"))
    (pad "7" smd rect (at 2.15 0.5) (size 1.1 0.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 30 "unconnected-(U3-Pad7)") (pintype "no_connect"))
    (pad "8" smd rect (at 2.15 0) (size 1.1 0.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 21 "Net-(C8-Pad1)") (pinfunction "VDD") (pintype "power_in"))
    (pad "9" smd rect (at 2.15 -0.5) (size 1.1 0.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 33 "Net-(J1-Pad4)") (pinfunction "SDA") (pintype "bidirectional"))
    (pad "10" smd rect (at 2.15 -1) (size 1.1 0.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 34 "Net-(J1-Pad5)") (pinfunction "SCL") (pintype "input"))
    (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/TSSOP-10_3x3mm_P0.5mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "NorTroN:S-Link-2Way" (layer "F.Cu")
    (tedit 621D56B6)
    (at 159 111.1)
    (descr "Solder Link 2way")
    (tags "Solder, Link")
    (property "Sheetfile" "NC085PSU.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "LK2" (at -1.3 1.3) (layer "F.SilkS"))
    (fp_text value "S-LINK-2WAY" (at 0 0.9) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -1.05 unlocked) (layer "F.Fab"))
    (pad "1" smd rect (at -0.35 0) (size 0.5 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 28 "Net-(LK2-Pad1)") (pinfunction "1") (pintype "input"))
    (pad "2" smd rect (at 0.35 0) (size 0.5 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 34 "Net-(J1-Pad5)") (pinfunction "2") (pintype "input"))
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 139.6 116.6)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "NC085PSU.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C10" (at 0 -2) (layer "F.SilkS"))
    (fp_text value "100nF" (at 0 0.8) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.48 0) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 16 "VCC") (pintype "passive"))
    (pad "2" smd roundrect (at 0.48 0) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 150.4 111.8 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "NC085PSU.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "FB1" (at 0 -1.6 90) (layer "F.SilkS"))
    (fp_text value "MMZ2012Y152B" (at 0 -1.15 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0.85 1.05 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1 0 270) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2083333333)
      (net 16 "VCC") (pintype "passive"))
    (pad "2" smd roundrect (at 1 0 270) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2083333333)
      (net 21 "Net-(C8-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 158.4 101.9 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "NC085PSU.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C9" (at 0.2 -1.2) (layer "F.SilkS"))
    (fp_text value "100nF" (at 0 -0.7) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.48 0 180) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 16 "VCC") (pintype "passive"))
    (pad "2" smd roundrect (at 0.48 0 180) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0402_1005Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 133.3 107.5 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "NC085PSU.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R3" (at 1.5 0) (layer "F.SilkS"))
    (fp_text value "100K" (at 1.9 0) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.51 0 180) (size 0.54 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 27 "Net-(J1-Pad7)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.51 0 180) (size 0.54 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 149.8 114.8 -90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "NC085PSU.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C8" (at 0 -1.1 180) (layer "F.SilkS"))
    (fp_text value "100nF" (at 0.95 -1.4 180) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.48 0 270) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 21 "Net-(C8-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.48 0 270) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "NorTroN:S-Link-2Way" (layer "F.Cu")
    (tedit 621D5435)
    (at 135.7 106.1)
    (descr "Solder Link 2way")
    (tags "Solder, Link")
    (property "Sheetfile" "NC085PSU.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "LK4" (at 0 1.3) (layer "F.SilkS"))
    (fp_text value "S-LINK-2WAY" (at 0 2.2) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 1.05 unlocked) (layer "F.Fab"))
    (pad "1" smd rect (at -0.35 0) (size 0.5 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 7 "Net-(LK4-Pad1)") (pinfunction "1") (pintype "input"))
    (pad "2" smd rect (at 0.35 0) (size 0.5 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 16 "VCC") (pinfunction "2") (pintype "input"))
  )
  (footprint "NorTroN:CP_Axial_L40.0mm_D16.0mm_P300mil" locked (layer "B.Cu")
    (tedit 621C0A05)
    (at 159 121 180)
    (descr "CP, Axial series, Axial, Horizontal, pin pitch=48mm, , length*diameter=40*16mm^2, Electrolytic Capacitor")
    (tags "CP Axial series Axial Horizontal pin pitch 48mm  length 40mm diameter 16mm Electrolytic Capacitor")
    (property "Purchase" "https://au.rs-online.com/web/p/supercapacitors/1967900")
    (property "Sheetfile" "NC085PSU.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C5" (at -2.3 4.8 180) (layer "F.SilkS"))
    (fp_text value "50F/3V 235EDLC-HVR ENYCAP" (at 24 -9.12 180) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 24 0 180) (layer "B.Fab"))
    (pad "1" thru_hole rect locked (at 0 3.81 180) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 2 "/SN1") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 0 -3.81 180) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 1 "GND") (pintype "passive"))
    (model "Capacitor_THT.3dshapes/CP_Axial_L40.0mm_D16.0mm_P48.00mm_Horizontal.wrl" hide
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical" (layer "B.Cu")
    (tedit 59FED5CC)
    (at 162.6 123.26 180)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (property "Sheetfile" "NC085PSU.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "SOL1" (at 1.9 0.66 90) (layer "B.SilkS"))
    (fp_text value "5V/100mA SOLAR PANEL" (at 0 -4.87) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -1.27 90) (layer "B.Fab"))
    (pad "1" thru_hole rect locked (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 "Net-(D1-PadA)") (pinfunction "+") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 0 -2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "-") (pintype "passive"))
    (model "Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "NorTroN:CP_Axial_L40.0mm_D16.0mm_P300mil" locked (layer "B.Cu")
    (tedit 621C0990)
    (at 159 102.94 180)
    (descr "CP, Axial series, Axial, Horizontal, pin pitch=48mm, , length*diameter=40*16mm^2, Electrolytic Capacitor")
    (tags "CP Axial series Axial Horizontal pin pitch 48mm  length 40mm diameter 16mm Electrolytic Capacitor")
    (property "Purchase" "https://au.rs-online.com/web/p/supercapacitors/1967900")
    (property "Sheetfile" "NC085PSU.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C3" (at 2.1 5.74 180) (layer "F.SilkS"))
    (fp_text value "50F/3V 235EDLC-HVR ENYCAP" (at 24 -9.12 180) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 24 0 180) (layer "B.Fab"))
    (pad "1" thru_hole rect locked (at 0 3.81 180) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 15 "/Power") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 0 -3.81 180) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 2 "/SN1") (pintype "passive"))
  )
  (footprint "Symbol:OSHW-Logo2_7.3x6mm_SilkScreen" (layer "B.Cu")
    (tedit 0)
    (at 135.4 101.8 180)
    (descr "Open Source Hardware Symbol")
    (tags "Logo Symbol OSHW")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 0) (layer "B.SilkS") hide)
    (fp_text value "OSHW-Logo2_7.3x6mm_SilkScreen" (at 0.75 0) (layer "B.Fab") hide)
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x07_P2.54mm_Vertical" (layer "B.Cu")
    (tedit 59FED5CC)
    (at 162.4 98.2 180)
    (descr "Through hole straight pin header, 1x07, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x07 2.54mm single row")
    (property "Sheetfile" "NC085PSU.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J1" (at 0 -17.624) (layer "B.SilkS"))
    (fp_text value "Conn_01x07" (at 0 -17.57) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -7.62 90) (layer "B.Fab"))
    (pad "1" thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 -2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 "VCC") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 -5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 "Net-(J1-Pad3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 -7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 33 "Net-(J1-Pad4)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 -10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 "Net-(J1-Pad5)") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 0 -12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 "Net-(J1-Pad6)") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole oval (at 0 -15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 "Net-(J1-Pad7)") (pinfunction "Pin_7") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x07_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "NC085PSU:Logo_Nortron" (layer "B.Cu")
    (tedit 0)
    (at 135.9 96.5 180)
    (attr board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "G***" (at 0 0) (layer "B.SilkS") hide)
    (fp_text value "LOGO" (at 0.75 0) (layer "B.SilkS") hide)
  )
  (gr_line (start 130 130) (end 130 94) (layer "Edge.Cuts") (width 0.05))
  (gr_circle (center 146 153) (end 146.1 153) (layer "Edge.Cuts") (width 0.2) (fill none))
  (gr_line (start 130 94) (end 165 94) (layer "Edge.Cuts") (width 0.05))
  (gr_line (start 165 94) (end 165 130) (layer "Edge.Cuts") (width 0.05))
  (gr_line (start 165 130) (end 130 130) (layer "Edge.Cuts") (width 0.05))
  (gr_text "RDY" (at 160.4 110.9) (layer "B.SilkS"))
  (gr_text "ADD" (at 160.4 102.7) (layer "B.SilkS"))
  (gr_text "SCL" (at 160.4 108.7) (layer "B.SilkS"))
  (gr_text "SDA" (at 160.4 104.9) (layer "B.SilkS"))
  (gr_text "GND" (at 163.4 128.3) (layer "B.SilkS"))
  (gr_text "CEN" (at 160.4 113.5) (layer "B.SilkS"))
  (gr_text "+" (at 163.1 120.8) (layer "B.SilkS"))
  (gr_text "GND" (at 162.2 96.3) (layer "B.SilkS"))
  (gr_text "NC085PSU-01" (at 148.3 96.5) (layer "B.SilkS"))
  (gr_text "VCC" (at 160.5 101.3) (layer "B.SilkS"))
  (gr_text "+" (at 159 114.9) (layer "F.SilkS"))
  (gr_text "+" (at 154 99.4) (layer "F.SilkS"))
  (gr_text "+" (at 159 96.7) (layer "F.SilkS"))
  (gr_text "+" (at 144.2 101.7) (layer "F.SilkS"))
  (dimension (type aligned) (layer "B.SilkS")
    (pts (xy 165 94) (xy 165 130))
    (height -5.9)
    (gr_text "36.0000 mm" (at 169.75 112 90) (layer "B.SilkS"))
    (format (units 3) (units_format 1) (precision 4))
    (style (thickness 0.12) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (dimension (type aligned) (layer "B.SilkS")
    (pts (xy 165 130) (xy 130 130))
    (height -4.2)
    (gr_text "35.0000 mm" (at 147.5 133.05) (layer "B.SilkS"))
    (format (units 3) (units_format 1) (precision 4))
    (style (thickness 0.12) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (zone (net 15) (net_name "/Power") (layer "F.Cu") (hatch full 0.508)
    (connect_pads (clearance 0.5))
    (min_thickness 0.254)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 147.3 101)
        (xy 143.9 101)
        (xy 143.9 102.4)
        (xy 137.6 102.4)
        (xy 137.6 95.5)
        (xy 147.3 95.5)
      )
    )
  )
  (zone (net 1) (net_name "GND") (layer "F.Cu") (hatch full 0.508)
    (connect_pads (clearance 0.5))
    (min_thickness 0.254)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 137.4 102.6)
        (xy 144.1 102.6)
        (xy 144.1 101.2)
        (xy 147 101.2)
        (xy 147 101.9)
        (xy 156.6 101.9)
        (xy 156.6 99.3)
        (xy 151.1 99.3)
        (xy 151.1 94)
        (xy 165 94)
        (xy 165 130)
        (xy 130 130)
        (xy 130 94)
        (xy 137.4 94)
      )
    )
  )
  (zone (net 16) (net_name "VCC") (layer "F.Cu") (hatch full 0.508)
    (connect_pads (clearance 0.5))
    (min_thickness 0.254)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 156.4 101.7)
        (xy 147.9 101.7)
        (xy 147.9 99.5)
        (xy 156.4 99.5)
      )
    )
  )
  (zone (net 1) (net_name "GND") (layer "In1.Cu") (name "GND") (hatch full 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 165 130)
        (xy 130 130)
        (xy 130 94)
        (xy 165 94)
      )
    )
  )
  (zone (net 16) (net_name "VCC") (layer "In2.Cu") (hatch full 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 165 130)
        (xy 130 130)
        (xy 130 94)
        (xy 165 94)
      )
    )
  )
  (zone (net 1) (net_name "GND") (layer "B.Cu") (hatch full 0.508)
    (connect_pads (clearance 0.5))
    (min_thickness 0.254)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 165 130)
        (xy 130 130)
        (xy 130 94)
        (xy 165 94)
      )
    )
  )
)
