<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="139.7" y2="0" width="0" layer="20"/>
<wire x1="139.7" y1="0" x2="139.7" y2="44.45" width="0" layer="20"/>
<wire x1="139.7" y1="44.45" x2="0" y2="44.45" width="0" layer="20"/>
<wire x1="0" y1="44.45" x2="0" y2="26.035" width="0" layer="20"/>
<wire x1="0" y1="18.415" x2="0" y2="0" width="0" layer="20"/>
<text>3.3v
ONLY!</text>
<text>Geppetto
Electronics
GPS Clock
v7.1</text>
<text>4-9 VDC
300 mA</text>
<text>GND</text>
<text>RXD</text>
<text>TXD</text>
<text>PPS</text>
<text>C7</text>
<wire x1="0" y1="18.415" x2="1.27" y2="18.415" width="0" layer="20"/>
<wire x1="1.27" y1="18.415" x2="1.27" y2="26.035" width="0" layer="20"/>
<wire x1="1.27" y1="26.035" x2="0" y2="26.035" width="0" layer="20"/>
</plain>
<libraries>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805">
</package>
<package name="EIA3528">
</package>
</packages>
</library>
<library name="SparkFun-DiscreteSemi">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find discrete semiconductors- transistors, diodes, TRIACs, optoisolators, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SMA-DIODE">
<description>&lt;B&gt;Diode&lt;/B&gt;&lt;p&gt;
Basic SMA packaged diode. Good for reverse polarization protection. Common part #: MBRA140</description>
</package>
<package name="0402TVS">
</package>
</packages>
</library>
<library name="avr-7">
<description>&lt;b&gt;AVR Devices&lt;/b&gt;&lt;p&gt;
Version 7 - August 1, 2011.&lt;br&gt;&lt;br&gt;
Added ATmega164P/324P/644P devices for DIP and TQFP.
&lt;p&gt;
Version 4 - March 11, 2008.&lt;br&gt;&lt;br&gt;
This library now includes ONLY ATMEL AVR microcontrollers.  It is the result of merging all other available device libraries available at http://www.cadsoft.de/download as of the time it was made.  In addition to the legacy AT90* devices, it includes most ATMEGA devices including the new 48/88/168, most ATTiny devices and a set of ISP and JTAG pin headers.&lt;p&gt;
Based on the following sources:&lt;p&gt;
&lt;ul&gt;
&lt;li&gt;www.atmel.com
&lt;li&gt; file at90smcu_v400.zip
&lt;li&gt;avr.lbr and atmel.lbr as provided by CadSoft
&lt;li&gt;avr-1.lbr by David Blundell
&lt;li&gt;avr-2.lbr by Boris Zalokar
&lt;li&gt;avr-3.lbr by Carson Reynolds
&lt;li&gt;attiny24_44_84.lbr by Pawel Szramowski (ATTiny24/44/84 devices)
&lt;li&gt;atmel.lbr by Bob Starr (ISP headers)
&lt;li&gt;moates_custom_parts.lbr (edge ISP)
&lt;li&gt;other misc sources
&lt;/ul&gt;
&lt;author&gt;Revised by David Blundell (blundar at gmail dot com) and others.&lt;/author&gt;
&lt;p&gt;
&lt;author&gt;Added Mega162, Tiny2313 John Lussmyer (cougar at casadelgato.com)&lt;/author&gt;
&lt;p&gt;
&lt;author&gt;Added XMega A1,A3,A4,D3,D4 John Lussmyer Aug 1, 2011(cougar at casadelgato.com)&lt;/author&gt;</description>
<packages>
<package name="AVR-ISP-6">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;&lt;p&gt; JTAG 6 Pin, 0.1" Straight</description>
</package>
<package name="TQFP32-08">
<description>&lt;B&gt;Thin Plasic Quad Flat Package&lt;/B&gt; Grid 0.8 mm</description>
</package>
</packages>
</library>
<library name="AP2331">
<packages>
<package name="SSOP18">
<description>&lt;b&gt;SSOP18&lt;/b&gt;&lt;p&gt;
Auto generated by &lt;i&gt;make-symbol-device-package-bsdl.ulp Rev. 44&lt;/i&gt;&lt;br&gt;</description>
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="DCJACK_2MM_SMT">
<description>2.0/2.1mm DC Jack - SMT
&lt;p&gt;4UConnector: 03267&lt;/p&gt;
&lt;p&gt;Note: Small tRestrict polygon's were added to the ground pads to improve solderability when this part is used in combination with a ground pour.  By default, Eagle will product four large bridges to the ground pour significantly increasing the heat distribution on the pads and preventing lead-free solder from reflowing in certain situations.  For more details, see: http://www.microbuilder.eu/Blog/09-12-14/Reducing_Thermals_for_Large_Pads_in_Eagle.aspx&lt;/p&gt;</description>
</package>
<package name="NX3225">
</package>
<package name="FIDUCIAL_1MM">
</package>
<package name="CHIP-LED0805">
<description>&lt;b&gt;Hyper CHIPLED Hyper-Bright LED&lt;/b&gt;&lt;p&gt;
LB R99A&lt;br&gt;
Source: http://www.osram.convergy.de/ ... lb_r99a.pdf</description>
</package>
</packages>
</library>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805">
</package>
</packages>
</library>
<library name="special">
<description>&lt;b&gt;Special Devices&lt;/b&gt;&lt;p&gt;
7-segment displays, switches, heatsinks, crystals, transformers, etc.&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="7SEG-13">
<description>7-segment &lt;B&gt;DISPLAY&lt;/B&gt;&lt;p&gt;
13 mm</description>
</package>
<package name="7SEG-7">
<description>7-segment &lt;B&gt;DISPLAY&lt;/B&gt;&lt;p&gt;
10 mm</description>
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805">
</package>
</packages>
</library>
<library name="SparkFun-Electromechanical">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find anything that moves- switches, relays, buttons, potentiometers. Also, anything that goes on a board but isn't electrical in nature- screws, standoffs, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="STANDOFF-ELECTRICAL">
</package>
</packages>
</library>
<library name="SparkFun-LED">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find discrete LEDs for illumination or indication, but no displays.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="LED5MM">
<description>&lt;B&gt;LED&lt;/B&gt;&lt;p&gt;
5 mm, round</description>
</package>
<package name="LED3MM">
<description>&lt;B&gt;LED&lt;/B&gt;&lt;p&gt;
3 mm, round</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X04">
</package>
<package name="1X01">
</package>
</packages>
</library>
<library name="diode">
<description>&lt;b&gt;Diodes&lt;/b&gt;&lt;p&gt;
Based on the following sources:
&lt;ul&gt;
&lt;li&gt;Motorola : www.onsemi.com
&lt;li&gt;Fairchild : www.fairchildsemi.com
&lt;li&gt;Philips : www.semiconductors.com
&lt;li&gt;Vishay : www.vishay.de
&lt;/ul&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SOT23">
<description>&lt;B&gt;DIODE&lt;/B&gt;</description>
</package>
</packages>
</library>
<library name="CR1220">
<packages>
<package name="CR1220-SMD">
</package>
</packages>
</library>
<library name="SparkFun-Connectors-new">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SMA-EDGE">
<description>&lt;b&gt;SMA Antenna Connector&lt;/b&gt;&lt;p&gt;
This is a footprint for an edge mount RF antenna. Works pretty well with SMA type connectors but may also work with other edge mount RF connectors. Keep in mind, these edge mount connectors assume you are using a 0.062" PCB thickness.</description>
</package>
</packages>
</library>
<library name="TE_relay">
<packages>
<package name="FSMJ">
</package>
</packages>
</library>
<library name="SparkFun-PowerIC">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find drivers, regulators, and amplifiers.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SOT23-5">
<description>&lt;b&gt;Small Outline Transistor&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="diode">
<description>&lt;b&gt;Diodes&lt;/b&gt;&lt;p&gt;
Based on the following sources:
&lt;ul&gt;
&lt;li&gt;Motorola : www.onsemi.com
&lt;li&gt;Fairchild : www.fairchildsemi.com
&lt;li&gt;Philips : www.semiconductors.com
&lt;li&gt;Vishay : www.vishay.de
&lt;/ul&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SOD123">
<description>&lt;b&gt;Diode&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SkyTraqGPS">
<packages>
<package name="PLX11X0T">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C6" library="SparkFun-Capacitors" package="0805" value="0.01µF">
<attribute name="NAME"/>
</element>
<element name="C7" library="SparkFun-Capacitors" package="0805" value="0.1µF">
<attribute name="NAME"/>
</element>
<element name="C5" library="SparkFun-Capacitors" package="0805" value="0.1µF">
<attribute name="NAME"/>
</element>
<element name="D1" library="SparkFun-DiscreteSemi" package="SMA-DIODE" value="S1M">
<attribute name="NAME"/>
</element>
<element name="JP2" library="adafruit" package="DCJACK_2MM_SMT" value="2.1MMJACKSMT"/>
<element name="LED1" library="special" package="7SEG-13" value="10 Hour">
<attribute name="NAME"/>
</element>
<element name="LED2" library="special" package="7SEG-13" value="1 Hour">
<attribute name="NAME"/>
</element>
<element name="LED3" library="special" package="7SEG-13" value="10 Min">
<attribute name="NAME"/>
</element>
<element name="LED4" library="special" package="7SEG-13" value="1 Min">
<attribute name="NAME"/>
</element>
<element name="LED5" library="special" package="7SEG-13" value="10 Sec">
<attribute name="NAME"/>
</element>
<element name="LED6" library="special" package="7SEG-13" value="1 Sec">
<attribute name="NAME"/>
</element>
<element name="LED9" library="SparkFun-LED" package="LED5MM" value="PM">
<attribute name="NAME"/>
</element>
<element name="LED8" library="SparkFun-LED" package="LED5MM" value="AM">
<attribute name="NAME"/>
</element>
<element name="R1" library="SparkFun-Resistors" package="0805" value="10kΩ">
<attribute name="NAME"/>
</element>
<element name="SW1" library="TE_relay" package="FSMJ" value="SPST_TACT-FSMJ">
<attribute name="NAME"/>
</element>
<element name="SW2" library="TE_relay" package="FSMJ" value="SPST_TACT-FSMJ">
<attribute name="NAME"/>
</element>
<element name="D2" library="SparkFun-DiscreteSemi" package="0402TVS" value="0402TVS">
<attribute name="NAME"/>
</element>
<element name="S1" library="SparkFun-Electromechanical" package="STANDOFF-ELECTRICAL" value="STANDOFF_ELECTRICAL"/>
<element name="S2" library="SparkFun-Electromechanical" package="STANDOFF-ELECTRICAL" value="STANDOFF_ELECTRICAL"/>
<element name="S3" library="SparkFun-Electromechanical" package="STANDOFF-ELECTRICAL" value="STANDOFF_ELECTRICAL"/>
<element name="S4" library="SparkFun-Electromechanical" package="STANDOFF-ELECTRICAL" value="STANDOFF_ELECTRICAL"/>
<element name="C1" library="SparkFun-Capacitors" package="EIA3528" value="56µF">
<attribute name="NAME"/>
</element>
<element name="LED7" library="special" package="7SEG-7" value="10th Sec">
<attribute name="NAME"/>
</element>
<element name="LED11" library="SparkFun-LED" package="LED3MM" value="MSB">
<attribute name="NAME"/>
</element>
<element name="LED12" library="SparkFun-LED" package="LED3MM" value="MSA">
<attribute name="NAME"/>
</element>
<element name="LED13" library="SparkFun-LED" package="LED3MM" value="HMB">
<attribute name="NAME"/>
</element>
<element name="LED14" library="SparkFun-LED" package="LED3MM" value="HMA">
<attribute name="NAME"/>
</element>
<element name="FID1" library="adafruit" package="FIDUCIAL_1MM" value="FIDUCIAL"/>
<element name="FID2" library="adafruit" package="FIDUCIAL_1MM" value="FIDUCIAL"/>
<element name="FID3" library="adafruit" package="FIDUCIAL_1MM" value="FIDUCIAL"/>
<element name="C8" library="SparkFun-Capacitors" package="0805" value="1µF">
<attribute name="NAME"/>
</element>
<element name="JP4" library="SparkFun-Connectors" package="1X04" value="DIAG">
<attribute name="NAME"/>
</element>
<element name="C4" library="SparkFun-Capacitors" package="0805" value="0.1µF">
<attribute name="NAME"/>
</element>
<element name="JP1" library="avr-7" package="AVR-ISP-6" value="AVR-PDIVERT"/>
<element name="IC1" library="avr-7" package="TQFP32-08" value="ATXMEGA32E5-AU">
<attribute name="NAME"/>
</element>
<element name="IC5" library="AP2331" package="SSOP18" value="TBD62783AFNG">
<attribute name="NAME"/>
</element>
<element name="IC4" library="AP2331" package="SSOP18" value="TBD62083AFNG">
<attribute name="NAME"/>
</element>
<element name="JP5" library="SparkFun-Connectors" package="1X01" value="M01PTH"/>
<element name="X1" library="adafruit" package="NX3225" value="16 MHz">
<attribute name="NAME"/>
</element>
<element name="C13" library="SparkFun-Capacitors" package="0805" value="22pF">
<attribute name="NAME"/>
</element>
<element name="C12" library="SparkFun-Capacitors" package="0805" value="22pF">
<attribute name="NAME"/>
</element>
<element name="D3" library="diode" package="SOT23" value="BAT54C">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="6"/>
</element>
<element name="B1" library="CR1220" package="CR1220-SMD" value="CR1220-SMD"/>
<element name="L1" library="SparkFun-Passives" package="0805" value="400Ω">
<attribute name="NAME"/>
</element>
<element name="L3" library="SparkFun-Passives" package="0805" value="400Ω">
<attribute name="NAME"/>
</element>
<element name="JP3" library="SparkFun-Connectors-new" package="SMA-EDGE" value="SMA_EDGE"/>
<element name="R5" library="SparkFun-Resistors" package="0805" value="1kΩ">
<attribute name="NAME"/>
</element>
<element name="R6" library="SparkFun-Resistors" package="0805" value="1kΩ">
<attribute name="NAME"/>
</element>
<element name="R7" library="SparkFun-Resistors" package="0805" value="1kΩ">
<attribute name="NAME"/>
</element>
<element name="R8" library="SparkFun-Resistors" package="0805" value="1kΩ">
<attribute name="NAME"/>
</element>
<element name="R9" library="SparkFun-Resistors" package="0805" value="1kΩ">
<attribute name="NAME"/>
</element>
<element name="R10" library="SparkFun-Resistors" package="0805" value="1kΩ">
<attribute name="NAME"/>
</element>
<element name="R11" library="SparkFun-Resistors" package="0805" value="1kΩ">
<attribute name="NAME"/>
</element>
<element name="R12" library="SparkFun-Resistors" package="0805" value="1kΩ">
<attribute name="NAME"/>
</element>
<element name="IC2" library="SparkFun-PowerIC" package="SOT23-5" value="NCP718BSN330T1G">
<attribute name="NAME"/>
</element>
<element name="C2" library="SparkFun-Capacitors" package="0805" value="1µF">
<attribute name="NAME"/>
</element>
<element name="C3" library="SparkFun-Capacitors" package="0805" value="1µF">
<attribute name="NAME"/>
</element>
<element name="D4" library="diode" package="SOD123" value="NSI45030AT1G">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="22"/>
</element>
<element name="D5" library="diode" package="SOD123" value="NSI45030AT1G">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="22"/>
</element>
<element name="D6" library="diode" package="SOD123" value="NSI45030AT1G">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="22"/>
</element>
<element name="D7" library="diode" package="SOD123" value="NSI45030AT1G">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="22"/>
</element>
<element name="D8" library="diode" package="SOD123" value="NSI45030AT1G">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="22"/>
</element>
<element name="D9" library="diode" package="SOD123" value="NSI45030AT1G">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="22"/>
</element>
<element name="D10" library="diode" package="SOD123" value="NSI45030AT1G">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="22"/>
</element>
<element name="D11" library="diode" package="SOD123" value="NSI45030AT1G">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="22"/>
</element>
<element name="U1" library="SkyTraqGPS" package="PLX11X0T" value="PLX1100T">
<attribute name="NAME"/>
</element>
<element name="R2" library="SparkFun-Resistors" package="0805" value="150Ω">
<attribute name="NAME"/>
</element>
<element name="LED10" library="adafruit" package="CHIP-LED0805" value="FIX">
<attribute name="NAME"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="C7" pad="1"/>
<contactref element="C6" pad="1"/>
<contactref element="C5" pad="1"/>
<contactref element="SW2" pad="P$3"/>
<contactref element="SW2" pad="P$4"/>
<contactref element="SW1" pad="P$3"/>
<contactref element="SW1" pad="P$4"/>
<contactref element="JP2" pad="GNDBREAK"/>
<contactref element="JP2" pad="GND"/>
<contactref element="D1" pad="A"/>
<contactref element="S1" pad="P1"/>
<contactref element="S4" pad="P1"/>
<contactref element="S2" pad="P1"/>
<contactref element="S3" pad="P1"/>
<contactref element="C1" pad="C"/>
<contactref element="C8" pad="1"/>
<contactref element="JP4" pad="1"/>
<contactref element="C4" pad="1"/>
<contactref element="JP1" pad="6"/>
<contactref element="IC1" pad="1"/>
<contactref element="IC1" pad="18"/>
<contactref element="IC5" pad="10"/>
<contactref element="IC4" pad="9"/>
<contactref element="C12" pad="2"/>
<contactref element="C13" pad="1"/>
<contactref element="X1" pad="4"/>
<contactref element="X1" pad="2"/>
<contactref element="B1" pad="CENTER"/>
<contactref element="R5" pad="2"/>
<contactref element="R6" pad="2"/>
<contactref element="R7" pad="2"/>
<contactref element="R8" pad="2"/>
<contactref element="R9" pad="2"/>
<contactref element="R10" pad="2"/>
<contactref element="R11" pad="2"/>
<contactref element="R12" pad="2"/>
<contactref element="IC2" pad="2"/>
<contactref element="C2" pad="1"/>
<contactref element="C3" pad="1"/>
<contactref element="U1" pad="P$1"/>
<contactref element="U1" pad="P$10"/>
<contactref element="U1" pad="P$12"/>
<contactref element="JP3" pad="GND@0"/>
<contactref element="JP3" pad="GND@2"/>
<contactref element="JP3" pad="GND@1"/>
<contactref element="JP3" pad="GND@3"/>
<contactref element="D2" pad="A"/>
<contactref element="LED10" pad="C"/>
</signal>
<signal name="PPS">
<contactref element="JP4" pad="4"/>
<contactref element="IC1" pad="16"/>
<contactref element="U1" pad="P$4"/>
</signal>
<signal name="TXD">
<contactref element="JP4" pad="3"/>
<contactref element="IC1" pad="14"/>
<contactref element="U1" pad="P$2"/>
</signal>
<signal name="N$7">
<contactref element="D2" pad="C"/>
<contactref element="JP3" pad="SIG"/>
<contactref element="U1" pad="P$11"/>
</signal>
<signal name="VCC">
<contactref element="C5" pad="2"/>
<contactref element="R1" pad="2"/>
<contactref element="C4" pad="2"/>
<contactref element="JP1" pad="2"/>
<contactref element="IC1" pad="17"/>
<contactref element="IC1" pad="32"/>
<contactref element="D3" pad="2"/>
<contactref element="L1" pad="2"/>
<contactref element="IC2" pad="5"/>
<contactref element="C3" pad="2"/>
</signal>
<signal name="RXD">
<contactref element="JP4" pad="2"/>
<contactref element="IC1" pad="13"/>
<contactref element="U1" pad="P$3"/>
</signal>
<signal name="N$18">
<contactref element="C7" pad="2"/>
<contactref element="C6" pad="2"/>
<contactref element="L1" pad="1"/>
<contactref element="U1" pad="P$8"/>
</signal>
<signal name="PDI-C/!RESET">
<contactref element="R1" pad="1"/>
<contactref element="JP1" pad="5"/>
<contactref element="IC1" pad="8"/>
</signal>
<signal name="!SW1">
<contactref element="SW2" pad="P$2"/>
<contactref element="SW2" pad="P$1"/>
<contactref element="IC1" pad="12"/>
</signal>
<signal name="!SW0">
<contactref element="SW1" pad="P$2"/>
<contactref element="SW1" pad="P$1"/>
<contactref element="IC1" pad="11"/>
</signal>
<signal name="+5V">
<contactref element="L3" pad="2"/>
<contactref element="IC5" pad="9"/>
<contactref element="IC2" pad="1"/>
<contactref element="IC2" pad="3"/>
<contactref element="C2" pad="2"/>
</signal>
<signal name="N$5">
<contactref element="JP2" pad="PWR1"/>
<contactref element="JP2" pad="PWR2"/>
<contactref element="D1" pad="C"/>
<contactref element="C1" pad="A"/>
<contactref element="L3" pad="1"/>
</signal>
<signal name="VBATT">
<contactref element="D3" pad="3"/>
<contactref element="C8" pad="2"/>
<contactref element="U1" pad="P$6"/>
</signal>
<signal name="PDI-D">
<contactref element="JP1" pad="1"/>
<contactref element="IC1" pad="7"/>
</signal>
<signal name="PA0">
<contactref element="IC1" pad="6"/>
<contactref element="IC5" pad="1"/>
</signal>
<signal name="PA1">
<contactref element="IC1" pad="5"/>
<contactref element="IC5" pad="2"/>
</signal>
<signal name="PA3">
<contactref element="IC1" pad="3"/>
<contactref element="IC5" pad="4"/>
</signal>
<signal name="PA7">
<contactref element="IC1" pad="29"/>
<contactref element="IC5" pad="8"/>
</signal>
<signal name="DP">
<contactref element="LED7" pad="7"/>
<contactref element="LED6" pad="5"/>
<contactref element="LED5" pad="5"/>
<contactref element="LED4" pad="5"/>
<contactref element="LED1" pad="5"/>
<contactref element="LED2" pad="5"/>
<contactref element="LED3" pad="5"/>
<contactref element="R12" pad="1"/>
<contactref element="D11" pad="C"/>
</signal>
<signal name="G">
<contactref element="LED7" pad="3"/>
<contactref element="LED6" pad="10"/>
<contactref element="LED5" pad="10"/>
<contactref element="LED4" pad="10"/>
<contactref element="LED1" pad="10"/>
<contactref element="LED2" pad="10"/>
<contactref element="LED3" pad="10"/>
<contactref element="R11" pad="1"/>
<contactref element="D10" pad="C"/>
</signal>
<signal name="F">
<contactref element="LED14" pad="A"/>
<contactref element="LED7" pad="2"/>
<contactref element="LED6" pad="9"/>
<contactref element="LED5" pad="9"/>
<contactref element="LED4" pad="9"/>
<contactref element="LED1" pad="9"/>
<contactref element="LED2" pad="9"/>
<contactref element="LED3" pad="9"/>
<contactref element="R10" pad="1"/>
<contactref element="D9" pad="C"/>
</signal>
<signal name="E">
<contactref element="LED1" pad="1"/>
<contactref element="LED2" pad="1"/>
<contactref element="LED3" pad="1"/>
<contactref element="LED4" pad="1"/>
<contactref element="LED13" pad="A"/>
<contactref element="LED5" pad="1"/>
<contactref element="LED6" pad="1"/>
<contactref element="LED7" pad="4"/>
<contactref element="R9" pad="1"/>
<contactref element="D8" pad="C"/>
</signal>
<signal name="D">
<contactref element="LED1" pad="2"/>
<contactref element="LED2" pad="2"/>
<contactref element="LED3" pad="2"/>
<contactref element="LED4" pad="2"/>
<contactref element="LED9" pad="A"/>
<contactref element="LED5" pad="2"/>
<contactref element="LED6" pad="2"/>
<contactref element="LED7" pad="5"/>
<contactref element="R8" pad="1"/>
<contactref element="D7" pad="C"/>
</signal>
<signal name="C">
<contactref element="LED1" pad="4"/>
<contactref element="LED2" pad="4"/>
<contactref element="LED3" pad="4"/>
<contactref element="LED4" pad="4"/>
<contactref element="LED11" pad="A"/>
<contactref element="LED5" pad="4"/>
<contactref element="LED6" pad="4"/>
<contactref element="LED7" pad="8"/>
<contactref element="R7" pad="1"/>
<contactref element="D6" pad="C"/>
</signal>
<signal name="B">
<contactref element="LED1" pad="6"/>
<contactref element="LED2" pad="6"/>
<contactref element="LED3" pad="6"/>
<contactref element="LED4" pad="6"/>
<contactref element="LED12" pad="A"/>
<contactref element="LED5" pad="6"/>
<contactref element="LED6" pad="6"/>
<contactref element="LED7" pad="9"/>
<contactref element="R6" pad="1"/>
<contactref element="D5" pad="C"/>
</signal>
<signal name="A">
<contactref element="LED1" pad="7"/>
<contactref element="LED2" pad="7"/>
<contactref element="LED3" pad="7"/>
<contactref element="LED4" pad="7"/>
<contactref element="LED8" pad="A"/>
<contactref element="LED5" pad="7"/>
<contactref element="LED6" pad="7"/>
<contactref element="LED7" pad="10"/>
<contactref element="R5" pad="1"/>
<contactref element="D4" pad="C"/>
</signal>
<signal name="PD0">
<contactref element="IC4" pad="1"/>
<contactref element="IC1" pad="28"/>
</signal>
<signal name="PD1">
<contactref element="IC4" pad="2"/>
<contactref element="IC1" pad="27"/>
</signal>
<signal name="PD2">
<contactref element="IC4" pad="3"/>
<contactref element="IC1" pad="26"/>
</signal>
<signal name="PD3">
<contactref element="IC4" pad="4"/>
<contactref element="IC1" pad="25"/>
</signal>
<signal name="PD4">
<contactref element="IC4" pad="5"/>
<contactref element="IC1" pad="24"/>
</signal>
<signal name="PD5">
<contactref element="IC4" pad="6"/>
<contactref element="IC1" pad="23"/>
</signal>
<signal name="PD6">
<contactref element="IC4" pad="7"/>
<contactref element="IC1" pad="22"/>
</signal>
<signal name="PD7">
<contactref element="IC4" pad="8"/>
<contactref element="IC1" pad="21"/>
</signal>
<signal name="K8">
<contactref element="LED8" pad="K"/>
<contactref element="LED11" pad="K"/>
<contactref element="LED12" pad="K"/>
<contactref element="LED13" pad="K"/>
<contactref element="LED14" pad="K"/>
<contactref element="LED9" pad="K"/>
<contactref element="IC4" pad="11"/>
</signal>
<signal name="K7">
<contactref element="LED7" pad="1"/>
<contactref element="LED7" pad="6"/>
<contactref element="IC4" pad="12"/>
</signal>
<signal name="K6">
<contactref element="LED6" pad="3"/>
<contactref element="LED6" pad="8"/>
<contactref element="IC4" pad="13"/>
</signal>
<signal name="K5">
<contactref element="LED5" pad="3"/>
<contactref element="LED5" pad="8"/>
<contactref element="IC4" pad="14"/>
</signal>
<signal name="K4">
<contactref element="LED4" pad="3"/>
<contactref element="LED4" pad="8"/>
<contactref element="IC4" pad="15"/>
</signal>
<signal name="K3">
<contactref element="LED3" pad="3"/>
<contactref element="LED3" pad="8"/>
<contactref element="IC4" pad="16"/>
</signal>
<signal name="K2">
<contactref element="LED2" pad="3"/>
<contactref element="LED2" pad="8"/>
<contactref element="IC4" pad="17"/>
</signal>
<signal name="K1">
<contactref element="LED1" pad="3"/>
<contactref element="LED1" pad="8"/>
<contactref element="IC4" pad="18"/>
</signal>
<signal name="PA2">
<contactref element="IC1" pad="4"/>
<contactref element="IC5" pad="3"/>
</signal>
<signal name="PA6">
<contactref element="IC1" pad="30"/>
<contactref element="IC5" pad="7"/>
</signal>
<signal name="PA5">
<contactref element="IC1" pad="31"/>
<contactref element="IC5" pad="6"/>
</signal>
<signal name="PA4">
<contactref element="IC1" pad="2"/>
<contactref element="IC5" pad="5"/>
</signal>
<signal name="COM">
<contactref element="IC4" pad="10"/>
</signal>
<signal name="N$4">
<contactref element="IC1" pad="9"/>
<contactref element="JP5" pad="1"/>
</signal>
<signal name="N$12">
<contactref element="X1" pad="1"/>
<contactref element="C13" pad="2"/>
<contactref element="IC1" pad="20"/>
</signal>
<signal name="N$13">
<contactref element="X1" pad="3"/>
<contactref element="C12" pad="1"/>
<contactref element="IC1" pad="19"/>
</signal>
<signal name="N$6">
<contactref element="D3" pad="1"/>
<contactref element="B1" pad="LEFT"/>
<contactref element="B1" pad="RIGHT"/>
</signal>
<signal name="N$16">
<contactref element="IC5" pad="18"/>
<contactref element="D4" pad="A"/>
</signal>
<signal name="N$17">
<contactref element="IC5" pad="17"/>
<contactref element="D5" pad="A"/>
</signal>
<signal name="N$19">
<contactref element="IC5" pad="16"/>
<contactref element="D6" pad="A"/>
</signal>
<signal name="N$20">
<contactref element="IC5" pad="15"/>
<contactref element="D7" pad="A"/>
</signal>
<signal name="N$21">
<contactref element="IC5" pad="14"/>
<contactref element="D8" pad="A"/>
</signal>
<signal name="N$22">
<contactref element="IC5" pad="13"/>
<contactref element="D9" pad="A"/>
</signal>
<signal name="N$23">
<contactref element="IC5" pad="12"/>
<contactref element="D10" pad="A"/>
</signal>
<signal name="N$24">
<contactref element="IC5" pad="11"/>
<contactref element="D11" pad="A"/>
</signal>
<signal name="FIX">
<contactref element="R2" pad="2"/>
<contactref element="IC1" pad="15"/>
</signal>
<signal name="N$1">
<contactref element="LED10" pad="A"/>
<contactref element="R2" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
