<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.0.1">
<drawing>
<board>
<plain>
<wire x1="10.16" y1="0" x2="55.88" y2="0" width="0" layer="20"/>
<wire x1="55.88" y1="0" x2="55.88" y2="45.72" width="0" layer="20"/>
<wire x1="55.88" y1="45.72" x2="10.16" y2="45.72" width="0" layer="20"/>
<wire x1="10.16" y1="45.72" x2="10.16" y2="27.94" width="0" layer="20"/>
<wire x1="10.16" y1="27.94" x2="0" y2="27.94" width="0" layer="20"/>
<wire x1="0" y1="27.94" x2="0" y2="17.78" width="0" layer="20"/>
<wire x1="0" y1="17.78" x2="10.16" y2="17.78" width="0" layer="20"/>
<wire x1="10.16" y1="17.78" x2="10.16" y2="0" width="0" layer="20"/>
<text>70mm</text>
<hole x="53.34" y="43.18" drill="3"/>
<hole x="12.7" y="2.54" drill="3"/>
<text>sjm4306</text>
<text>TouchLamp</text>
<text>041922</text>
<text>JLCJLCJLCJLC</text>
</plain>
<libraries>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X02_LOCK">
<description>&lt;h3&gt;Plated Through Hole - Locking Footprint&lt;/h3&gt;
Holes are staggered by 0.005" from center to hold pins while soldering. 
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:2&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_02&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="2X3">
<description>&lt;h3&gt;Plated Through Hole - 2x3&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:6&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_03x2&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="C0603">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="LED3MM">
<description>&lt;B&gt;LED&lt;/B&gt;&lt;p&gt;
3 mm, round</description>
</package>
<package name="M0805">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
MELF 0.10 W</description>
</package>
<package name="E3,5-8">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 3.5 mm, diameter 8 mm</description>
</package>
</packages>
</library>
<library name="SparkFun-DiscreteSemi">
<description>&lt;h3&gt;SparkFun Discrete Semiconductors&lt;/h3&gt;
This library contains diodes, optoisolators, TRIACs, MOSFETs, transistors, etc. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SOT23-3">
<description>SOT23-3</description>
</package>
</packages>
</library>
<library name="SparkFun-IC-Microcontroller">
<description>&lt;h3&gt;SparkFun Microcontrollers&lt;/h3&gt;
This library contains microcontrollers.
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SO14">
<description>SOIC, 0.15 inch width</description>
</package>
</packages>
</library>
<library name="sjm4306-custom">
<packages>
<package name="MICRO_USB_4PTH">
</package>
</packages>
</library>
<library name="testpad">
<description>&lt;b&gt;Test Pins/Pads&lt;/b&gt;&lt;p&gt;
Cream on SMD OFF.&lt;br&gt;
new: Attribute TP_SIGNAL_NAME&lt;br&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="TP20SQ">
<description>&lt;b&gt;TEST PAD&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="sjm4306_LOGO">
<packages>
<package name="SJM4306_LOGO_LARGE">
</package>
<package name="SJM4306_MEDIUM_NO_MASK">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="BATTERY" library="SparkFun-Connectors" package="1X02_LOCK" value=""/>
<element name="C1" library="adafruit" package="C0603" value="0.1uF"/>
<element name="C2" library="adafruit" package="E3,5-8" value="100uF"/>
<element name="ICSP" library="SparkFun-Connectors" package="2X3" value="ICSP">
<attribute name="PROD_ID" value="CONN-09701"/>
<attribute name="VALUE"/>
</element>
<element name="LED1" library="adafruit" package="LED3MM" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED2" library="adafruit" package="LED3MM" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED3" library="adafruit" package="LED3MM" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED4" library="adafruit" package="LED3MM" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q1" library="SparkFun-DiscreteSemi" package="SOT23-3" value="600mA/40V">
<attribute name="PROD_ID" value="TRANS-08049"/>
</element>
<element name="Q2" library="SparkFun-DiscreteSemi" package="SOT23-3" value="600mA/40V">
<attribute name="PROD_ID" value="TRANS-08049"/>
</element>
<element name="Q3" library="SparkFun-DiscreteSemi" package="SOT23-3" value="600mA/40V">
<attribute name="PROD_ID" value="TRANS-08049"/>
</element>
<element name="Q4" library="SparkFun-DiscreteSemi" package="SOT23-3" value="600mA/40V">
<attribute name="PROD_ID" value="TRANS-08049"/>
</element>
<element name="R1" library="adafruit" package="M0805" value="10K"/>
<element name="R2" library="adafruit" package="M0805" value="1K"/>
<element name="R3" library="adafruit" package="M0805" value="1K"/>
<element name="R4" library="adafruit" package="M0805" value="1K"/>
<element name="R5" library="adafruit" package="M0805" value="1K"/>
<element name="R6" library="adafruit" package="M0805" value="1K"/>
<element name="R7" library="adafruit" package="M0805" value="1K"/>
<element name="R8" library="adafruit" package="M0805" value="1K"/>
<element name="R9" library="adafruit" package="M0805" value="1K"/>
<element name="U$1" library="SparkFun-IC-Microcontroller" package="SO14" value="ATTINY84">
<attribute name="PROD_ID" value="IC-11285"/>
</element>
<element name="U$2" library="sjm4306-custom" package="MICRO_USB_4PTH" value="MICRO_USB_4PTH"/>
<element name="TOUCH" library="testpad" package="TP20SQ" value="TPTP20SQ">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="2"/>
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="VALUE"/>
</element>
<element name="E$1" library="sjm4306_LOGO" package="SJM4306_LOGO_LARGE" value=""/>
<element name="E$3" library="sjm4306_LOGO" package="SJM4306_MEDIUM_NO_MASK" value=""/>
</elements>
<signals>
<signal name="GND">
<contactref element="ICSP" pad="6"/>
<contactref element="BATTERY" pad="1"/>
<contactref element="U$1" pad="14"/>
<contactref element="Q3" pad="2"/>
<contactref element="C1" pad="2"/>
<contactref element="C2" pad="-"/>
<contactref element="Q1" pad="2"/>
<contactref element="Q2" pad="2"/>
<contactref element="Q4" pad="2"/>
<contactref element="U$2" pad="P$7"/>
<contactref element="U$2" pad="P$6"/>
<contactref element="U$2" pad="P$8"/>
<contactref element="U$2" pad="P$9"/>
<contactref element="U$2" pad="P$5"/>
</signal>
<signal name="VCC">
<contactref element="ICSP" pad="2"/>
<contactref element="C1" pad="1"/>
<contactref element="U$1" pad="1"/>
<contactref element="C2" pad="+"/>
<contactref element="R1" pad="1"/>
<contactref element="R6" pad="1"/>
<contactref element="BATTERY" pad="2"/>
<contactref element="R2" pad="1"/>
<contactref element="R4" pad="1"/>
<contactref element="R8" pad="1"/>
<contactref element="U$2" pad="P$1"/>
</signal>
<signal name="RST">
<contactref element="ICSP" pad="5"/>
<contactref element="U$1" pad="4"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="MOSI">
<contactref element="ICSP" pad="4"/>
<contactref element="U$1" pad="7"/>
<contactref element="R5" pad="1"/>
</signal>
<signal name="MISO">
<contactref element="ICSP" pad="1"/>
<contactref element="U$1" pad="8"/>
<contactref element="R3" pad="1"/>
</signal>
<signal name="SCK">
<contactref element="ICSP" pad="3"/>
<contactref element="U$1" pad="9"/>
</signal>
<signal name="N$3">
<contactref element="R6" pad="2"/>
<contactref element="LED3" pad="A"/>
</signal>
<signal name="N$7">
<contactref element="Q3" pad="1"/>
<contactref element="R7" pad="2"/>
</signal>
<signal name="N$1">
<contactref element="Q3" pad="3"/>
<contactref element="LED3" pad="K"/>
</signal>
<signal name="L3">
<contactref element="R7" pad="1"/>
<contactref element="U$1" pad="6"/>
</signal>
<signal name="N$4">
<contactref element="R2" pad="2"/>
<contactref element="LED1" pad="A"/>
</signal>
<signal name="N$5">
<contactref element="Q1" pad="1"/>
<contactref element="R3" pad="2"/>
</signal>
<signal name="N$6">
<contactref element="Q1" pad="3"/>
<contactref element="LED1" pad="K"/>
</signal>
<signal name="N$9">
<contactref element="R4" pad="2"/>
<contactref element="LED2" pad="A"/>
</signal>
<signal name="N$10">
<contactref element="Q2" pad="1"/>
<contactref element="R5" pad="2"/>
</signal>
<signal name="N$11">
<contactref element="Q2" pad="3"/>
<contactref element="LED2" pad="K"/>
</signal>
<signal name="N$13">
<contactref element="R8" pad="2"/>
<contactref element="LED4" pad="A"/>
</signal>
<signal name="N$14">
<contactref element="Q4" pad="1"/>
<contactref element="R9" pad="2"/>
</signal>
<signal name="N$15">
<contactref element="Q4" pad="3"/>
<contactref element="LED4" pad="K"/>
</signal>
<signal name="L4">
<contactref element="R9" pad="1"/>
<contactref element="U$1" pad="5"/>
</signal>
<signal name="N$8">
<contactref element="U$1" pad="3"/>
</signal>
<signal name="N$12">
<contactref element="U$1" pad="2"/>
</signal>
<signal name="N$17">
<contactref element="U$1" pad="10"/>
</signal>
<signal name="N$18">
<contactref element="U$1" pad="11"/>
</signal>
<signal name="TOUCH">
<contactref element="U$1" pad="12"/>
<contactref element="TOUCH" pad="TP"/>
</signal>
<signal name="N$20">
<contactref element="U$1" pad="13"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
