(kicad_pcb (version 20211014) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0)
    (aux_axis_origin 123.19 128.27)
    (grid_origin 123.19 128.27)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "ROTADUCKPLOTS/")
    )
  )
  (net 0 "")
  (net 1 "Moved")
  (net 2 "GND")
  (net 3 "Net-(BT2-Pad1)")
  (net 4 "+5V")
  (net 5 "Net-(D1-Pad1)")
  (net 6 "Net-(D1-Pad2)")
  (net 7 "Net-(M1-Pad1)")
  (net 8 "Net-(M1-Pad9)")
  (net 9 "Net-(M1-Pad2)")
  (net 10 "Net-(M1-Pad10)")
  (net 11 "A1")
  (net 12 "Net-(M1-Pad11)")
  (net 13 "D1")
  (net 14 "Net-(M1-Pad13)")
  (net 15 "B1")
  (net 16 "Net-(M1-Pad14)")
  (net 17 "C1")
  (net 18 "Net-(M1-Pad15)")
  (net 19 "Net-(M1-Pad8)")
  (net 20 "Net-(M1-Pad16)")
  (net 21 "Net-(M2-Pad1)")
  (net 22 "Net-(M2-Pad9)")
  (net 23 "Net-(M2-Pad2)")
  (net 24 "Net-(M2-Pad10)")
  (net 25 "A2")
  (net 26 "Net-(M2-Pad11)")
  (net 27 "D2")
  (net 28 "Net-(M2-Pad13)")
  (net 29 "B2")
  (net 30 "Net-(M2-Pad14)")
  (net 31 "C2")
  (net 32 "Net-(M2-Pad15)")
  (net 33 "Net-(M2-Pad8)")
  (net 34 "Net-(M2-Pad16)")
  (net 35 "Net-(M3-Pad1)")
  (net 36 "Net-(M3-Pad9)")
  (net 37 "Net-(M3-Pad2)")
  (net 38 "Net-(M3-Pad10)")
  (net 39 "A3")
  (net 40 "Net-(M3-Pad11)")
  (net 41 "D3")
  (net 42 "Net-(M3-Pad13)")
  (net 43 "B3")
  (net 44 "Net-(M3-Pad14)")
  (net 45 "C3")
  (net 46 "Net-(M3-Pad15)")
  (net 47 "Net-(M3-Pad8)")
  (net 48 "Net-(M3-Pad16)")
  (net 49 "Net-(NX1-PadLHDP)")
  (net 50 "HT")
  (net 51 "Net-(NX2-PadLHDP)")
  (net 52 "Net-(NX3-PadLHDP)")
  (net 53 "Net-(Q1-Pad2)")
  (net 54 "Net-(Q1-Pad1)")
  (net 55 "Net-(Q2-Pad1)")
  (net 56 "Net-(Q3-Pad1)")
  (net 57 "Net-(Q4-Pad1)")
  (net 58 "DP1")
  (net 59 "DP2")
  (net 60 "DP3")
  (net 61 "Net-(TP1-Pad1)")
  (net 62 "Net-(U1-Pad11)")
  (footprint "Package_TO_SOT_THT:TO-92" (layer "F.Cu")
    (tedit 5A279852)
    (at 130.175 84.815)
    (descr "TO-92 leads molded, narrow, drill 0.75mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (property "Sheetfile" "Rotaduck.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "Q4" (at -0.6096 -1.5792) (layer "B.SilkS"))
    (fp_text value "Q_NPN_BCE" (at 1.27 2.79) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.27 0) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0) (size 1.3 1.3) (drill 0.75) (layers *.Cu *.Mask)
      (net 57 "Net-(Q4-Pad1)") (pinfunction "B") (pintype "input"))
    (pad "2" thru_hole circle locked (at 1.27 -1.27) (size 1.3 1.3) (drill 0.75) (layers *.Cu *.Mask)
      (net 52 "Net-(NX3-PadLHDP)") (pinfunction "C") (pintype "passive"))
    (pad "3" thru_hole circle locked (at 2.54 0) (size 1.3 1.3) (drill 0.75) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "E") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-92.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "nixies-us:nixies-us-IN-12-DSUB" (layer "F.Cu")
    (tedit 200000)
    (at 144.78 72.39 -5)
    (descr "FOR USE WITH FEMALE D-SUB PINS")
    (tags "FOR USE WITH FEMALE D-SUB PINS")
    (property "Sheetfile" "Rotaduck.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "NX3" (at 0.107591 -4.598877 -5 unlocked) (layer "F.SilkS"))
    (fp_text value "IN-12BNOHOLE" (at 0 0 175) (layer "F.SilkS") hide)
    (pad "" np_thru_hole circle (at 0 0 355) (size 4.99872 4.99872) (drill 4.99872) (layers *.Cu *.Mask))
    (pad "0" thru_hole circle (at 5.74802 4.49834 355) (size 2.39776 2.39776) (drill 1.59766) (layers *.Cu *.Mask)
      (net 48 "Net-(M3-Pad16)") (pinfunction "0") (pintype "bidirectional"))
    (pad "1" thru_hole circle (at -3.99796 7.99846 355) (size 2.39776 2.39776) (drill 1.59766) (layers *.Cu *.Mask)
      (net 46 "Net-(M3-Pad15)") (pinfunction "1") (pintype "bidirectional"))
    (pad "2" thru_hole circle (at -5.74802 4.49834 355) (size 2.39776 2.39776) (drill 1.59766) (layers *.Cu *.Mask)
      (net 47 "Net-(M3-Pad8)") (pinfunction "2") (pintype "bidirectional"))
    (pad "3" thru_hole circle (at -5.74802 0 355) (size 2.39776 2.39776) (drill 1.59766) (layers *.Cu *.Mask)
      (net 36 "Net-(M3-Pad9)") (pinfunction "3") (pintype "bidirectional"))
    (pad "4" thru_hole circle (at -5.74802 -4.49834 355) (size 2.39776 2.39776) (drill 1.59766) (layers *.Cu *.Mask)
      (net 42 "Net-(M3-Pad13)") (pinfunction "4") (pintype "bidirectional"))
    (pad "5" thru_hole circle (at -3.99796 -7.99846 355) (size 2.39776 2.39776) (drill 1.59766) (layers *.Cu *.Mask)
      (net 44 "Net-(M3-Pad14)") (pinfunction "5") (pintype "bidirectional"))
    (pad "6" thru_hole circle (at 0 -8.99922 355) (size 2.39776 2.39776) (drill 1.59766) (layers *.Cu *.Mask)
      (net 40 "Net-(M3-Pad11)") (pinfunction "6") (pintype "bidirectional"))
    (pad "7" thru_hole circle (at 3.99796 -7.99846 355) (size 2.39776 2.39776) (drill 1.59766) (layers *.Cu *.Mask)
      (net 38 "Net-(M3-Pad10)") (pinfunction "7") (pintype "bidirectional"))
    (pad "8" thru_hole circle (at 5.74802 -4.49834 355) (size 2.39776 2.39776) (drill 1.59766) (layers *.Cu *.Mask)
      (net 35 "Net-(M3-Pad1)") (pinfunction "8") (pintype "bidirectional"))
    (pad "9" thru_hole circle (at 5.74802 0 355) (size 2.39776 2.39776) (drill 1.59766) (layers *.Cu *.Mask)
      (net 37 "Net-(M3-Pad2)") (pinfunction "9") (pintype "bidirectional"))
    (pad "A" thru_hole circle (at 3.99796 7.99846 355) (size 2.39776 2.39776) (drill 1.59766) (layers *.Cu *.Mask)
      (net 50 "HT") (pinfunction "A") (pintype "bidirectional"))
    (pad "LHDP" thru_hole circle (at 0 8.99922 355) (size 2.39776 2.39776) (drill 1.59766) (layers *.Cu *.Mask)
      (net 52 "Net-(NX3-PadLHDP)") (pinfunction "LHDP") (pintype "bidirectional"))
  )
  (footprint "nixies-us:nixies-us-IN-12-DSUB" (layer "F.Cu")
    (tedit 200000)
    (at 123.19 68.58)
    (descr "FOR USE WITH FEMALE D-SUB PINS")
    (tags "FOR USE WITH FEMALE D-SUB PINS")
    (property "Sheetfile" "Rotaduck.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "NX2" (at 0 -5.08 180) (layer "F.SilkS"))
    (fp_text value "IN-12BNOHOLE" (at 0 0) (layer "F.SilkS") hide)
    (pad "" np_thru_hole circle (at 0 0) (size 4.99872 4.99872) (drill 4.99872) (layers *.Cu *.Mask))
    (pad "0" thru_hole circle (at 5.74802 4.49834) (size 2.39776 2.39776) (drill 1.59766) (layers *.Cu *.Mask)
      (net 34 "Net-(M2-Pad16)") (pinfunction "0") (pintype "bidirectional"))
    (pad "1" thru_hole circle (at -3.99796 7.99846) (size 2.39776 2.39776) (drill 1.59766) (layers *.Cu *.Mask)
      (net 32 "Net-(M2-Pad15)") (pinfunction "1") (pintype "bidirectional"))
    (pad "2" thru_hole circle (at -5.74802 4.49834) (size 2.39776 2.39776) (drill 1.59766) (layers *.Cu *.Mask)
      (net 33 "Net-(M2-Pad8)") (pinfunction "2") (pintype "bidirectional"))
    (pad "3" thru_hole circle (at -5.74802 0) (size 2.39776 2.39776) (drill 1.59766) (layers *.Cu *.Mask)
      (net 22 "Net-(M2-Pad9)") (pinfunction "3") (pintype "bidirectional"))
    (pad "4" thru_hole circle (at -5.74802 -4.49834) (size 2.39776 2.39776) (drill 1.59766) (layers *.Cu *.Mask)
      (net 28 "Net-(M2-Pad13)") (pinfunction "4") (pintype "bidirectional"))
    (pad "5" thru_hole circle (at -3.99796 -7.99846) (size 2.39776 2.39776) (drill 1.59766) (layers *.Cu *.Mask)
      (net 30 "Net-(M2-Pad14)") (pinfunction "5") (pintype "bidirectional"))
    (pad "6" thru_hole circle (at 0 -8.99922) (size 2.39776 2.39776) (drill 1.59766) (layers *.Cu *.Mask)
      (net 26 "Net-(M2-Pad11)") (pinfunction "6") (pintype "bidirectional"))
    (pad "7" thru_hole circle (at 3.99796 -7.99846) (size 2.39776 2.39776) (drill 1.59766) (layers *.Cu *.Mask)
      (net 24 "Net-(M2-Pad10)") (pinfunction "7") (pintype "bidirectional"))
    (pad "8" thru_hole circle (at 5.74802 -4.49834) (size 2.39776 2.39776) (drill 1.59766) (layers *.Cu *.Mask)
      (net 21 "Net-(M2-Pad1)") (pinfunction "8") (pintype "bidirectional"))
    (pad "9" thru_hole circle (at 5.74802 0) (size 2.39776 2.39776) (drill 1.59766) (layers *.Cu *.Mask)
      (net 23 "Net-(M2-Pad2)") (pinfunction "9") (pintype "bidirectional"))
    (pad "A" thru_hole circle (at 3.99796 7.99846) (size 2.39776 2.39776) (drill 1.59766) (layers *.Cu *.Mask)
      (net 50 "HT") (pinfunction "A") (pintype "bidirectional"))
    (pad "LHDP" thru_hole circle (at 0 8.99922) (size 2.39776 2.39776) (drill 1.59766) (layers *.Cu *.Mask)
      (net 51 "Net-(NX2-PadLHDP)") (pinfunction "LHDP") (pintype "bidirectional"))
  )
  (footprint "Package_TO_SOT_THT:TO-92" (layer "F.Cu")
    (tedit 5A279852)
    (at 113.665 84.815)
    (descr "TO-92 leads molded, narrow, drill 0.75mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (property "Sheetfile" "Rotaduck.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "Q3" (at 3.1242 -1.6808) (layer "B.SilkS"))
    (fp_text value "Q_NPN_BCE" (at 1.27 2.79) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.27 0) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0) (size 1.3 1.3) (drill 0.75) (layers *.Cu *.Mask)
      (net 56 "Net-(Q3-Pad1)") (pinfunction "B") (pintype "input"))
    (pad "2" thru_hole circle locked (at 1.27 -1.27) (size 1.3 1.3) (drill 0.75) (layers *.Cu *.Mask)
      (net 51 "Net-(NX2-PadLHDP)") (pinfunction "C") (pintype "passive"))
    (pad "3" thru_hole circle locked (at 2.54 0) (size 1.3 1.3) (drill 0.75) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "E") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-92.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "nixies-us:nixies-us-IN-12-DSUB" (layer "F.Cu")
    (tedit 200000)
    (at 101.6 72.39 5)
    (descr "FOR USE WITH FEMALE D-SUB PINS")
    (tags "FOR USE WITH FEMALE D-SUB PINS")
    (property "Sheetfile" "Rotaduck.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "NX1" (at 0.16758 -4.829773 185) (layer "F.SilkS"))
    (fp_text value "IN-12BNOHOLE" (at 0 0 5) (layer "F.SilkS") hide)
    (pad "" np_thru_hole circle (at 0 0 5) (size 4.99872 4.99872) (drill 4.99872) (layers *.Cu *.Mask))
    (pad "0" thru_hole circle (at 5.74802 4.49834 5) (size 2.39776 2.39776) (drill 1.59766) (layers *.Cu *.Mask)
      (net 20 "Net-(M1-Pad16)") (pinfunction "0") (pintype "bidirectional"))
    (pad "1" thru_hole circle (at -3.99796 7.99846 5) (size 2.39776 2.39776) (drill 1.59766) (layers *.Cu *.Mask)
      (net 18 "Net-(M1-Pad15)") (pinfunction "1") (pintype "bidirectional"))
    (pad "2" thru_hole circle (at -5.74802 4.49834 5) (size 2.39776 2.39776) (drill 1.59766) (layers *.Cu *.Mask)
      (net 19 "Net-(M1-Pad8)") (pinfunction "2") (pintype "bidirectional"))
    (pad "3" thru_hole circle (at -5.74802 0 5) (size 2.39776 2.39776) (drill 1.59766) (layers *.Cu *.Mask)
      (net 8 "Net-(M1-Pad9)") (pinfunction "3") (pintype "bidirectional"))
    (pad "4" thru_hole circle (at -5.74802 -4.49834 5) (size 2.39776 2.39776) (drill 1.59766) (layers *.Cu *.Mask)
      (net 14 "Net-(M1-Pad13)") (pinfunction "4") (pintype "bidirectional"))
    (pad "5" thru_hole circle (at -3.99796 -7.99846 5) (size 2.39776 2.39776) (drill 1.59766) (layers *.Cu *.Mask)
      (net 16 "Net-(M1-Pad14)") (pinfunction "5") (pintype "bidirectional"))
    (pad "6" thru_hole circle (at 0 -8.99922 5) (size 2.39776 2.39776) (drill 1.59766) (layers *.Cu *.Mask)
      (net 12 "Net-(M1-Pad11)") (pinfunction "6") (pintype "bidirectional"))
    (pad "7" thru_hole circle (at 3.99796 -7.99846 5) (size 2.39776 2.39776) (drill 1.59766) (layers *.Cu *.Mask)
      (net 10 "Net-(M1-Pad10)") (pinfunction "7") (pintype "bidirectional"))
    (pad "8" thru_hole circle (at 5.74802 -4.49834 5) (size 2.39776 2.39776) (drill 1.59766) (layers *.Cu *.Mask)
      (net 7 "Net-(M1-Pad1)") (pinfunction "8") (pintype "bidirectional"))
    (pad "9" thru_hole circle (at 5.74802 0 5) (size 2.39776 2.39776) (drill 1.59766) (layers *.Cu *.Mask)
      (net 9 "Net-(M1-Pad2)") (pinfunction "9") (pintype "bidirectional"))
    (pad "A" thru_hole circle (at 3.99796 7.99846 5) (size 2.39776 2.39776) (drill 1.59766) (layers *.Cu *.Mask)
      (net 50 "HT") (pinfunction "A") (pintype "bidirectional"))
    (pad "LHDP" thru_hole circle (at 0 8.99922 5) (size 2.39776 2.39776) (drill 1.59766) (layers *.Cu *.Mask)
      (net 49 "Net-(NX1-PadLHDP)") (pinfunction "LHDP") (pintype "bidirectional"))
  )
  (footprint "LED_SMD:LED_0805_2012Metric_Pad1.15x1.40mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEF1)
    (at 123.19 85.1408 180)
    (descr "LED SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "LED handsolder")
    (property "Sheetfile" "Rotaduck.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D1" (at 0 1.524) (layer "B.SilkS") hide)
    (fp_text value "LED" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -1.025 0 180) (size 1.15 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2173913043)
      (net 5 "Net-(D1-Pad1)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1.025 0 180) (size 1.15 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2173913043)
      (net 6 "Net-(D1-Pad2)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEF)
    (at 139.065 132.715 -135)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "Rotaduck.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C1" (at 0 1.85 45) (layer "B.SilkS"))
    (fp_text value "100uF" (at 0 -1.85 45) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 45) (layer "B.Fab"))
    (pad "1" smd roundrect locked (at -1.5625 0 225) (size 1.325 1.8) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.1886792453)
      (net 1 "Moved") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1.5625 0 225) (size 1.325 1.8) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.1886792453)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_THT:TO-92" (layer "B.Cu")
    (tedit 5A279852)
    (at 103.703835 147.708337 145)
    (descr "TO-92 leads molded, narrow, drill 0.75mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (property "Sheetfile" "Rotaduck.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "Q1" (at 1.27 3.56 325 unlocked) (layer "B.SilkS"))
    (fp_text value "Q_NPN_BCE" (at 1.27 -2.79 145) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 1.27 0 145) (layer "B.Fab"))
    (pad "1" thru_hole rect locked (at 0 0 145) (size 1.3 1.3) (drill 0.75) (layers *.Cu *.Mask)
      (net 54 "Net-(Q1-Pad1)") (pinfunction "B") (pintype "input"))
    (pad "2" thru_hole circle locked (at 1.27 1.27 145) (size 1.3 1.3) (drill 0.75) (layers *.Cu *.Mask)
      (net 53 "Net-(Q1-Pad2)") (pinfunction "C") (pintype "passive"))
    (pad "3" thru_hole circle locked (at 2.54 0 145) (size 1.3 1.3) (drill 0.75) (layers *.Cu *.Mask)
      (net 3 "Net-(BT2-Pad1)") (pinfunction "E") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-92.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_DIP:DIP-16_W7.62mm" (layer "B.Cu")
    (tedit 5A02E8C5)
    (at 111.115 90.82 180)
    (descr "16-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (property "Sheetfile" "Rotaduck.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "M1" (at 3.81 2.33) (layer "B.SilkS") hide)
    (fp_text value "74141DIP16" (at 3.81 -20.11) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 -8.89) (layer "B.Fab"))
    (pad "1" thru_hole rect locked (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(M1-Pad1)") (pinfunction "8") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 0 -2.54 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 "Net-(M1-Pad2)") (pinfunction "9") (pintype "passive"))
    (pad "3" thru_hole oval locked (at 0 -5.08 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 "A1") (pinfunction "A") (pintype "passive"))
    (pad "4" thru_hole oval locked (at 0 -7.62 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 "D1") (pinfunction "D") (pintype "passive"))
    (pad "5" thru_hole oval locked (at 0 -10.16 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "+5V") (pinfunction "VCC") (pintype "power_in"))
    (pad "6" thru_hole oval locked (at 0 -12.7 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 "B1") (pinfunction "B") (pintype "passive"))
    (pad "7" thru_hole oval locked (at 0 -15.24 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 "C1") (pinfunction "C") (pintype "passive"))
    (pad "8" thru_hole oval locked (at 0 -17.78 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 "Net-(M1-Pad8)") (pinfunction "2") (pintype "passive"))
    (pad "9" thru_hole oval locked (at 7.62 -17.78 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 "Net-(M1-Pad9)") (pinfunction "3") (pintype "passive"))
    (pad "10" thru_hole oval locked (at 7.62 -15.24 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "Net-(M1-Pad10)") (pinfunction "7") (pintype "passive"))
    (pad "11" thru_hole oval locked (at 7.62 -12.7 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 "Net-(M1-Pad11)") (pinfunction "6") (pintype "passive"))
    (pad "12" thru_hole oval locked (at 7.62 -10.16 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "13" thru_hole oval locked (at 7.62 -7.62 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 "Net-(M1-Pad13)") (pinfunction "4") (pintype "passive"))
    (pad "14" thru_hole oval locked (at 7.62 -5.08 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 "Net-(M1-Pad14)") (pinfunction "5") (pintype "passive"))
    (pad "15" thru_hole oval locked (at 7.62 -2.54 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 "Net-(M1-Pad15)") (pinfunction "1") (pintype "passive"))
    (pad "16" thru_hole oval locked (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 "Net-(M1-Pad16)") (pinfunction "0") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-16_W7.62mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TestPoint:TestPoint_Plated_Hole_D2.0mm" (layer "B.Cu")
    (tedit 61E60EC2)
    (at 140.97 155.702 180)
    (descr "Plated Hole as test Point, diameter 2.0mm")
    (tags "test point plated hole")
    (property "Sheetfile" "Rotaduck.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "UPDI" (at 3.556 -0.762) (layer "B.SilkS"))
    (fp_text value "UPDI" (at 0 -2.45) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.5) (layer "B.Fab"))
    (pad "1" thru_hole circle locked (at 0 0 180) (size 3 3) (drill 1.5) (layers *.Cu *.Mask)
      (net 61 "Net-(TP1-Pad1)") (pinfunction "1") (pintype "passive"))
  )
  (footprint "digikey-footprints:Test_Point_D1.02mm" (layer "B.Cu")
    (tedit 61E60E5E)
    (at 143.764 153.162 180)
    (attr through_hole)
    (fp_text reference "GND" (at 1.016 2.032) (layer "B.SilkS"))
    (fp_text value "Test_Point_D1.02mm" (at 0 -3.93) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -2.41) (layer "B.Fab"))
    (pad "1" thru_hole circle locked (at 0 0 180) (size 2.02 2.02) (drill 1.02) (layers *.Cu *.Mask)
      (net 2 "GND"))
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical" (layer "B.Cu")
    (tedit 59FED5CC)
    (at 137.997889 120.266573 -155)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (property "Sheetfile" "Rotaduck.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "Dial" (at 0 2.33 25) (layer "B.SilkS"))
    (fp_text value "Rotary_Dial" (at 0 -7.41 25) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -2.54 115) (layer "B.Fab"))
    (pad "1" thru_hole rect locked (at 0 0 205) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Moved") (pinfunction "Power") (pintype "power_in"))
    (pad "2" thru_hole oval locked (at 0 -2.54 205) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "+5V") (pinfunction "Moved") (pintype "output"))
    (pad "3" thru_hole oval locked (at 0 -5.08 205) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 62 "Net-(U1-Pad11)") (pinfunction "Dial_Signal") (pintype "output"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEF)
    (at 148.59 111.125 -90)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "Rotaduck.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C2" (at 0 1.85 90) (layer "B.SilkS"))
    (fp_text value "100uF" (at 0 -1.85 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect locked (at -1.5625 0 270) (size 1.325 1.8) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.1886792453)
      (net 4 "+5V") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1.5625 0 270) (size 1.325 1.8) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.1886792453)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical" (layer "B.Cu")
    (tedit 59FED5CC)
    (at 135.885 114.935 -90)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (property "Sheetfile" "Rotaduck.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "5V" (at -2.413 -1.275 180) (layer "B.SilkS"))
    (fp_text value "Battery_Cell" (at 0 -4.87 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -1.27) (layer "B.Fab"))
    (pad "1" thru_hole rect locked (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Moved") (pinfunction "+") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 0 -2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "-") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "digikey-footprints:Test_Point_D1.02mm" (layer "B.Cu")
    (tedit 61E60DDB)
    (at 146.304 150.622 180)
    (attr through_hole)
    (fp_text reference "5V" (at 0.508 2.032) (layer "B.SilkS"))
    (fp_text value "Test_Point_D1.02mm" (at 0 -3.93) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -2.41) (layer "B.Fab"))
    (pad "1" thru_hole circle locked (at 0 0 180) (size 2.02 2.02) (drill 1.02) (layers *.Cu *.Mask)
      (net 1 "Moved"))
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical" (layer "B.Cu")
    (tedit 59FED5CC)
    (at 96.294419 140.97 55)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (property "Sheetfile" "Rotaduck.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "HV" (at 0 2.33 55) (layer "B.SilkS"))
    (fp_text value "Battery" (at 0 -4.87 55) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -1.27 145) (layer "B.Fab"))
    (pad "1" thru_hole rect locked (at 0 0 55) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(BT2-Pad1)") (pinfunction "+") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 0 -2.54 55) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "-") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 97.79 135.316424 -35)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Rotaduck.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R1" (at -0.212324 -1.631736 -35 unlocked) (layer "B.SilkS"))
    (fp_text value "20K" (at 0 -1.65 145) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 145) (layer "B.Fab"))
    (pad "1" smd roundrect locked (at -1 0 325) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2083333333)
      (net 50 "HT") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1 0 325) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2083333333)
      (net 53 "Net-(Q1-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 137.795 87.63 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Rotaduck.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R6" (at 0 1.65) (layer "B.SilkS"))
    (fp_text value "10K" (at 0 -1.65) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect locked (at -1 0 180) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2083333333)
      (net 57 "Net-(Q4-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1 0 180) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2083333333)
      (net 60 "DP3") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 96.52 113.03 -125)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Rotaduck.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R4" (at 0 1.65 55) (layer "B.SilkS"))
    (fp_text value "10K" (at 0 -1.65 55) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 55) (layer "B.Fab"))
    (pad "1" smd roundrect locked (at -1 0 235) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2083333333)
      (net 55 "Net-(Q2-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1 0 235) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2083333333)
      (net 58 "DP1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_THT:TO-92" (layer "B.Cu")
    (tedit 5A279852)
    (at 99.42 105.41 -90)
    (descr "TO-92 leads molded, narrow, drill 0.75mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (property "Sheetfile" "Rotaduck.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "Q2" (at -2.032 -0.148 180) (layer "B.SilkS"))
    (fp_text value "Q_NPN_BCE" (at 1.27 -2.79 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 1.27 0 90) (layer "B.Fab"))
    (pad "1" thru_hole rect locked (at 0 0 270) (size 1.3 1.3) (drill 0.75) (layers *.Cu *.Mask)
      (net 55 "Net-(Q2-Pad1)") (pinfunction "B") (pintype "input"))
    (pad "2" thru_hole circle locked (at 1.27 1.27 270) (size 1.3 1.3) (drill 0.75) (layers *.Cu *.Mask)
      (net 49 "Net-(NX1-PadLHDP)") (pinfunction "C") (pintype "passive"))
    (pad "3" thru_hole circle locked (at 2.54 0 270) (size 1.3 1.3) (drill 0.75) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "E") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-92.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_SO:SOIC-20W_7.5x12.8mm_P1.27mm" (layer "B.Cu")
    (tedit 5D9F72B1)
    (at 149.225 137.795 -135)
    (descr "SOIC, 20 Pin (JEDEC MS-013AC, https://www.analog.com/media/en/package-pcb-resources/package/233848rw_20.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (property "Sheetfile" "Rotaduck.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U1" (at 0 0.179605 45) (layer "B.SilkS"))
    (fp_text value "ATtiny416-S" (at 0 -7.35 45) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 45) (layer "B.Fab"))
    (pad "1" smd roundrect locked (at -4.65 5.715 225) (size 2.05 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 4 "+5V") (pinfunction "VCC") (pintype "power_in"))
    (pad "2" smd roundrect locked (at -4.65 4.445 225) (size 2.05 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 13 "D1") (pinfunction "PA4") (pintype "bidirectional"))
    (pad "3" smd roundrect locked (at -4.65 3.175 225) (size 2.05 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 58 "DP1") (pinfunction "PA5") (pintype "bidirectional"))
    (pad "4" smd roundrect locked (at -4.65 1.905 225) (size 2.05 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 59 "DP2") (pinfunction "PA6") (pintype "bidirectional"))
    (pad "5" smd roundrect locked (at -4.65 0.635 225) (size 2.05 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 60 "DP3") (pinfunction "PA7") (pintype "bidirectional"))
    (pad "6" smd roundrect locked (at -4.65 -0.635 225) (size 2.05 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 6 "Net-(D1-Pad2)") (pinfunction "PB5") (pintype "bidirectional"))
    (pad "7" smd roundrect locked (at -4.65 -1.905 225) (size 2.05 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 27 "D2") (pinfunction "PB4") (pintype "bidirectional"))
    (pad "8" smd roundrect locked (at -4.65 -3.175 225) (size 2.05 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 31 "C2") (pinfunction "PB3") (pintype "bidirectional"))
    (pad "9" smd roundrect locked (at -4.65 -4.445 225) (size 2.05 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 29 "B2") (pinfunction "PB2") (pintype "bidirectional"))
    (pad "10" smd roundrect locked (at -4.65 -5.715 225) (size 2.05 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 25 "A2") (pinfunction "PB1") (pintype "bidirectional"))
    (pad "11" smd roundrect locked (at 4.65 -5.715 225) (size 2.05 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 62 "Net-(U1-Pad11)") (pinfunction "PB0") (pintype "bidirectional"))
    (pad "12" smd roundrect locked (at 4.65 -4.445 225) (size 2.05 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 39 "A3") (pinfunction "PC0") (pintype "bidirectional"))
    (pad "13" smd roundrect locked (at 4.65 -3.175 225) (size 2.05 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 43 "B3") (pinfunction "PC1") (pintype "bidirectional"))
    (pad "14" smd roundrect locked (at 4.65 -1.905 225) (size 2.05 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 45 "C3") (pinfunction "PC2") (pintype "bidirectional"))
    (pad "15" smd roundrect locked (at 4.65 -0.635 225) (size 2.05 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 41 "D3") (pinfunction "PC3") (pintype "bidirectional"))
    (pad "16" smd roundrect locked (at 4.65 0.635 225) (size 2.05 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 61 "Net-(TP1-Pad1)") (pinfunction "~{RESET}/PA0") (pintype "bidirectional"))
    (pad "17" smd roundrect locked (at 4.65 1.905 225) (size 2.05 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 11 "A1") (pinfunction "PA1") (pintype "bidirectional"))
    (pad "18" smd roundrect locked (at 4.65 3.175 225) (size 2.05 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 15 "B1") (pinfunction "PA2") (pintype "bidirectional"))
    (pad "19" smd roundrect locked (at 4.65 4.445 225) (size 2.05 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 17 "C1") (pinfunction "PA3") (pintype "bidirectional"))
    (pad "20" smd roundrect locked (at 4.65 5.715 225) (size 2.05 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "GND") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-20W_7.5x12.8mm_P1.27mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 108.585 87.63 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Rotaduck.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R5" (at -0.127 1.65) (layer "B.SilkS"))
    (fp_text value "10K" (at 0 -1.65) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect locked (at -1 0 180) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2083333333)
      (net 56 "Net-(Q3-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1 0 180) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2083333333)
      (net 59 "DP2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 151.765 116.84 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Rotaduck.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R3" (at 0 1.65) (layer "B.SilkS"))
    (fp_text value "1K" (at 0 -1.65) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect locked (at -1 0 180) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2083333333)
      (net 5 "Net-(D1-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1 0 180) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2083333333)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 108.022107 152.4 -35)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Rotaduck.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R2" (at 0.04475 -1.581718 -35 unlocked) (layer "B.SilkS"))
    (fp_text value "10K" (at 0 -1.65 145) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 145) (layer "B.Fab"))
    (pad "1" smd roundrect locked (at -1 0 325) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2083333333)
      (net 54 "Net-(Q1-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1 0 325) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2083333333)
      (net 4 "+5V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_DIP:DIP-16_W7.62mm" (layer "B.Cu")
    (tedit 5A02E8C5)
    (at 142.865 90.82 180)
    (descr "16-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (property "Sheetfile" "Rotaduck.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "M3" (at 3.81 2.33) (layer "B.SilkS") hide)
    (fp_text value "74141DIP16" (at 3.81 -20.11) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 -8.89) (layer "B.Fab"))
    (pad "1" thru_hole rect locked (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 35 "Net-(M3-Pad1)") (pinfunction "8") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 0 -2.54 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 37 "Net-(M3-Pad2)") (pinfunction "9") (pintype "passive"))
    (pad "3" thru_hole oval locked (at 0 -5.08 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 39 "A3") (pinfunction "A") (pintype "passive"))
    (pad "4" thru_hole oval locked (at 0 -7.62 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 41 "D3") (pinfunction "D") (pintype "passive"))
    (pad "5" thru_hole oval locked (at 0 -10.16 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "+5V") (pinfunction "VCC") (pintype "power_in"))
    (pad "6" thru_hole oval locked (at 0 -12.7 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 43 "B3") (pinfunction "B") (pintype "passive"))
    (pad "7" thru_hole oval locked (at 0 -15.24 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 45 "C3") (pinfunction "C") (pintype "passive"))
    (pad "8" thru_hole oval locked (at 0 -17.78 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 47 "Net-(M3-Pad8)") (pinfunction "2") (pintype "passive"))
    (pad "9" thru_hole oval locked (at 7.62 -17.78 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 36 "Net-(M3-Pad9)") (pinfunction "3") (pintype "passive"))
    (pad "10" thru_hole oval locked (at 7.62 -15.24 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 38 "Net-(M3-Pad10)") (pinfunction "7") (pintype "passive"))
    (pad "11" thru_hole oval locked (at 7.62 -12.7 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 40 "Net-(M3-Pad11)") (pinfunction "6") (pintype "passive"))
    (pad "12" thru_hole oval locked (at 7.62 -10.16 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "13" thru_hole oval locked (at 7.62 -7.62 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 42 "Net-(M3-Pad13)") (pinfunction "4") (pintype "passive"))
    (pad "14" thru_hole oval locked (at 7.62 -5.08 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 44 "Net-(M3-Pad14)") (pinfunction "5") (pintype "passive"))
    (pad "15" thru_hole oval locked (at 7.62 -2.54 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 46 "Net-(M3-Pad15)") (pinfunction "1") (pintype "passive"))
    (pad "16" thru_hole oval locked (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 48 "Net-(M3-Pad16)") (pinfunction "0") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-16_W7.62mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_DIP:DIP-16_W7.62mm" (layer "B.Cu")
    (tedit 5A02E8C5)
    (at 114.315 87.64 -90)
    (descr "16-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (property "Sheetfile" "Rotaduck.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "M2" (at 3.81 2.33 90) (layer "B.SilkS") hide)
    (fp_text value "74141DIP16" (at 3.81 -20.11 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 -8.89 90) (layer "B.Fab"))
    (pad "1" thru_hole rect locked (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 21 "Net-(M2-Pad1)") (pinfunction "8") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 0 -2.54 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 "Net-(M2-Pad2)") (pinfunction "9") (pintype "passive"))
    (pad "3" thru_hole oval locked (at 0 -5.08 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 25 "A2") (pinfunction "A") (pintype "passive"))
    (pad "4" thru_hole oval locked (at 0 -7.62 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 27 "D2") (pinfunction "D") (pintype "passive"))
    (pad "5" thru_hole oval locked (at 0 -10.16 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "+5V") (pinfunction "VCC") (pintype "power_in"))
    (pad "6" thru_hole oval locked (at 0 -12.7 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 29 "B2") (pinfunction "B") (pintype "passive"))
    (pad "7" thru_hole oval locked (at 0 -15.24 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 31 "C2") (pinfunction "C") (pintype "passive"))
    (pad "8" thru_hole oval locked (at 0 -17.78 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 33 "Net-(M2-Pad8)") (pinfunction "2") (pintype "passive"))
    (pad "9" thru_hole oval locked (at 7.62 -17.78 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 22 "Net-(M2-Pad9)") (pinfunction "3") (pintype "passive"))
    (pad "10" thru_hole oval locked (at 7.62 -15.24 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 24 "Net-(M2-Pad10)") (pinfunction "7") (pintype "passive"))
    (pad "11" thru_hole oval locked (at 7.62 -12.7 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 26 "Net-(M2-Pad11)") (pinfunction "6") (pintype "passive"))
    (pad "12" thru_hole oval locked (at 7.62 -10.16 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "13" thru_hole oval locked (at 7.62 -7.62 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 28 "Net-(M2-Pad13)") (pinfunction "4") (pintype "passive"))
    (pad "14" thru_hole oval locked (at 7.62 -5.08 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 30 "Net-(M2-Pad14)") (pinfunction "5") (pintype "passive"))
    (pad "15" thru_hole oval locked (at 7.62 -2.54 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 32 "Net-(M2-Pad15)") (pinfunction "1") (pintype "passive"))
    (pad "16" thru_hole oval locked (at 7.62 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 34 "Net-(M2-Pad16)") (pinfunction "0") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-16_W7.62mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 102.09664 137.808782) (end 102.115718 137.658644) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 124.828246 159.267152) (end 124.886535 159.30452) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 155.429316 130.58978) (end 155.37299 130.549726) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 149.92073 121.874311) (end 149.992966 121.999942) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 149.032378 125.917572) (end 148.910658 125.995605) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 156.379449 130.827718) (end 156.30649 130.833266) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 155.37299 128.247254) (end 155.429316 128.2072) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 142.593857 114.720476) (end 142.648129 114.677826) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 156.726529 128.049019) (end 156.791769 128.074743) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 103.064019 135.894859) (end 103.172873 135.800568) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 123.338336 161.724469) (end 123.280047 161.687101) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 135.39257 154.580673) (end 136.539906 153.993057) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 124.442333 159.104394) (end 124.510507 159.123754) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 140.734008 150.800197) (end 141.665996 149.791715) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 136.103722 124.941866) (end 135.951077 124.458807) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 142.27904 116.574018) (end 142.244448 116.513855) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 125.490749 160.785346) (end 125.474707 160.854852) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 144.415999 122.825317) (end 144.449498 122.680174) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 134.537234 133.624649) (end 134.832881 133.20148) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 148.655673 126.134092) (end 148.522785 126.194169) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 108.69391 116.204368) (end 108.69391 116.204368) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 144.421541 114.720476) (end 144.473669 114.76563) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 124.6425 161.819558) (end 124.57726 161.845281) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 143.218164 114.421604) (end 143.288911 114.40897) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 156.591602 130.789906) (end 156.522096 130.805948) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 156.726529 130.747961) (end 156.659776 130.770547) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 156.30649 127.963714) (end 156.379449 127.969262) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 143.86674 114.437646) (end 143.934915 114.457005) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 144.310943 117.020353) (end 144.252654 117.057721) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 106.248886 135.35127) (end 106.381774 135.411347) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 148.247158 120.564797) (end 148.38655 120.611962) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 156.855407 130.693468) (end 156.791769 130.722238) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 142.212722 115.206215) (end 142.244448 115.14427) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 107.202471 140.236839) (end 107.098283 140.336172) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 153.200217 83.509532) (end 154.950217 63.489532) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 103.780528 135.411347) (end 103.913416 135.35127) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 155.123973 130.312332) (end 155.081324 130.25806) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 138.723097 152.564973) (end 139.75186 151.724638) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 122.654063 160.348921) (end 122.663199 160.277023) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 155.547768 130.661741) (end 155.487605 130.627149) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 148.785027 120.792006) (end 148.910658 120.864242) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 150.173011 124.461426) (end 150.119295 124.597661) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 144.310943 114.637772) (end 144.367269 114.677826) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 123.280047 161.687101) (end 123.223721 161.647047) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 154.841144 129.757532) (end 154.825102 129.688026) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 106.758479 140.603165) (end 106.636759 140.681197) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 150.260602 122.680174) (end 150.294101 122.825317) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 157.652652 129.617278) (end 157.640018 129.688026) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 156.522096 127.991032) (end 156.591602 128.007074) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 142.762744 114.600404) (end 142.822906 114.565812) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 105.538021 141.080949) (end 105.387883 141.100027) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 150.059217 124.73055) (end 149.992966 124.859904) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 150.35505 123.429923) (end 150.351146 123.584303) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 102.316906 139.283254) (end 102.26319 139.147019) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 149.47637 121.308601) (end 149.575704 121.412789) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 156.451348 127.978398) (end 156.522096 127.991032) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 143.288911 117.249155) (end 143.218164 117.236521) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 108.077247 137.961136) (end 108.081151 138.115516) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 125.512519 160.348921) (end 125.518067 160.421881) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 157.556307 129.957699) (end 157.527537 130.021337) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 145.677722 120.942274) (end 145.799442 120.864242) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 144.370539 123.736657) (end 144.358954 123.584303) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 157.640018 129.108955) (end 157.652652 129.179702) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 102.09664 138.422249) (end 102.085055 138.269896) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 118.816354 154.517715) (end 120.10877 155.032104) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 142.822906 114.565812) (end 142.884852 114.534085) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 142.399112 116.742904) (end 142.356463 116.688632) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 144.389617 123.886795) (end 144.370539 123.736657) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 124.157221 161.930587) (end 124.083291 161.932456) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 143.148657 117.220479) (end 143.080483 117.20112) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 102.959831 140.236839) (end 102.860497 140.132651) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 103.403823 135.627867) (end 103.525542 135.549835) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 142.316409 115.025819) (end 142.356463 114.969493) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 106.511128 135.477598) (end 106.636759 135.549835) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 149.149997 125.833931) (end 149.032378 125.917572) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 125.432762 160.989779) (end 125.407038 161.05502) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 143.433769 114.394286) (end 143.507699 114.392417) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 115.731736 97.999892) (end 115.919412 116.110572) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 147.959654 126.368974) (end 147.81192 126.395357) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 107.396096 140.023797) (end 107.301805 140.132651) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 132.976362 120.23514) (end 132.531551 119.898743) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 136.456684 126.927001) (end 136.406857 126.42508) (layer "Edge.Cuts") (width 0.264582))
  (gr_arc (start 93.19 83.52) (mid 99.545005 91.806581) (end 96.824368 101.888826) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 143.288911 114.40897) (end 143.36081 114.399834) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 101.468404 111.418639) (end 91.333932 126.901862) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 142.158228 115.335094) (end 142.183952 115.269854) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 108.065662 137.808782) (end 108.077247 137.961136) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 154.825102 129.688026) (end 154.812468 129.617278) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 145.134396 125.447058) (end 145.040105 125.338204) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 157.661788 129.545379) (end 157.652652 129.617278) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 142.158228 116.323031) (end 142.135642 116.256279) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 124.886535 161.687101) (end 124.828246 161.724469) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 145.677722 125.917572) (end 145.560103 125.833931) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 102.515471 139.671128) (end 102.443235 139.545497) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 144.389617 122.973051) (end 144.415999 122.825317) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 123.864503 161.915903) (end 123.793756 161.903269) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 124.032515 156.064531) (end 125.344111 156.238648) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 130.514348 156.086757) (end 131.770144 155.837026) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 122.892001 161.299055) (end 122.854632 161.240766) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 122.711234 160.923027) (end 122.691875 160.854852) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 104.049651 135.297554) (end 104.189043 135.250389) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 155.487605 128.169832) (end 155.547768 128.135239) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 135.772443 123.983337) (end 135.567706 123.516603) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 146.605304 120.524371) (end 146.750446 120.490872) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 131.770144 155.837026) (end 133.004143 155.502724) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 123.589322 159.14634) (end 123.656075 159.123754) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 122.974704 161.409652) (end 122.932055 161.35538) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 149.759056 121.634973) (end 149.842697 121.752592) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 136.480196 127.935224) (end 136.481093 127.430766) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 144.066908 114.505315) (end 144.130546 114.534085) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 144.942475 115.755133) (end 144.944344 115.829063) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 155.873519 128.007074) (end 155.943025 127.991032) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 123.524082 161.819558) (end 123.460444 161.790788) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 108.046584 137.658644) (end 108.065662 137.808782) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 142.212722 116.45191) (end 142.183952 116.388272) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 133.394041 120.590616) (end 132.976362 120.23514) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 154.812468 129.617278) (end 154.803332 129.545379) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 143.365306 147.522895) (end 144.125538 146.262689) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 143.797234 114.421604) (end 143.86674 114.437646) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 102.593504 136.438185) (end 102.677145 136.320565) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 136.406857 126.42508) (end 136.331497 125.926152) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 156.451348 130.818582) (end 156.379449 130.827718) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 107.568798 139.792847) (end 107.485157 139.910466) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 150.220176 122.537813) (end 150.260602 122.680174) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 154.937583 128.775643) (end 154.969309 128.713698) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 104.331405 135.209963) (end 104.476547 135.176465) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 154.969309 130.083283) (end 154.937583 130.021337) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 144.951044 125.224874) (end 144.867403 125.107254) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 102.115718 137.658644) (end 102.1421 137.510909) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 144.523562 116.844926) (end 144.473669 116.892495) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 144.821427 144.918708) (end 144.821427 144.918708) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 142.116283 116.188104) (end 142.100241 116.118598) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 149.263328 121.114975) (end 149.372182 121.209267) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 157.461219 130.143445) (end 157.42385 130.201734) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 124.083291 159.059165) (end 124.083291 159.059165) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 154.908813 129.957699) (end 154.883089 129.892459) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 104.774419 135.131004) (end 104.926771 135.119419) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 146.32355 126.247885) (end 146.187315 126.194169) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 157.42385 130.201734) (end 157.383796 130.25806) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 144.35505 123.429923) (end 144.358954 123.275543) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 157.09213 130.549726) (end 157.035804 130.58978) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 108.077247 138.269896) (end 108.065662 138.422249) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 155.04127 128.595246) (end 155.081324 128.53892) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 149.669995 121.521642) (end 149.759056 121.634973) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 123.793756 159.088353) (end 123.864503 159.075718) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 116.276044 153.23317) (end 117.537597 153.918092) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 142.762744 117.057721) (end 142.704455 117.020353) (layer "Edge.Cuts") (width 0.126705))
  (gr_arc (start 113.94 59.02) (mid 113.299694 62.090805) (end 110.177774 61.785103) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 157.035804 128.2072) (end 157.09213 128.247254) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 148.785027 126.067841) (end 148.655673 126.134092) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 146.605304 126.335476) (end 146.462942 126.29505) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 105.387883 135.131004) (end 105.538021 135.150082) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 124.009361 161.930587) (end 123.936402 161.925039) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 143.797234 117.236521) (end 143.726487 117.249155) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 145.23373 125.551246) (end 145.134396 125.447058) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 106.248886 140.879762) (end 106.112651 140.933477) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 154.841144 129.039449) (end 154.860503 128.971274) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 155.081324 128.53892) (end 155.123973 128.484648) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 149.149997 121.025915) (end 149.263328 121.114975) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 102.1421 138.720122) (end 102.115718 138.572388) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 146.462942 126.29505) (end 146.32355 126.247885) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 154.797784 129.47242) (end 154.795915 129.39849) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 106.112651 140.933477) (end 105.973259 140.980642) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 104.926771 135.119419) (end 105.081151 135.115516) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 125.146724 159.529841) (end 125.191878 159.581969) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 148.38655 120.611962) (end 148.522785 120.665677) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 102.515471 136.559904) (end 102.593504 136.438185) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 144.78937 124.985535) (end 144.717134 124.859904) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 146.187315 120.665677) (end 146.32355 120.611962) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 102.081151 138.115516) (end 102.085055 137.961136) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 144.130546 117.12404) (end 144.066908 117.15281) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 115.035241 152.462881) (end 116.276044 153.23317) (layer "Edge.Cuts") (width 0.264582))
  (gr_arc (start 91.440001 63.500001) (mid 100.421999 58.415223) (end 110.177774 61.785103) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 149.842697 121.752592) (end 149.92073 121.874311) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 148.910658 125.995605) (end 148.785027 126.067841) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 142.822906 117.092314) (end 142.762744 117.057721) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 155.003902 128.653535) (end 155.04127 128.595246) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 157.461219 128.653535) (end 157.495811 128.713698) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 147.959654 120.490872) (end 148.104796 120.524371) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 145.040105 121.521642) (end 145.134396 121.412789) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 125.474707 160.136769) (end 125.490749 160.206275) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 122.82004 159.811018) (end 122.854632 159.750856) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 102.766206 136.207235) (end 102.860497 136.098381) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 143.654588 114.399834) (end 143.726487 114.40897) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 122.663199 160.714599) (end 122.654063 160.6427) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 123.067428 161.511674) (end 123.019858 161.46178) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 142.704455 117.020353) (end 142.648129 116.980299) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 125.490749 160.206275) (end 125.503383 160.277023) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 124.942861 159.344574) (end 124.997133 159.387224) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 107.899112 137.084013) (end 107.946277 137.223405) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 125.346542 161.180603) (end 125.31195 161.240766) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 110.350437 148.526738) (end 111.472785 149.639154) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 102.443235 139.545497) (end 102.376984 139.416143) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 144.066908 117.15281) (end 144.001668 117.178533) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 154.795915 129.39849) (end 154.797784 129.32456) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 142.316409 116.632307) (end 142.27904 116.574018) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 122.720396 155.805446) (end 124.032515 156.064531) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 143.218164 117.236521) (end 143.148657 117.220479) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 156.013772 130.818582) (end 155.943025 130.805948) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 102.1421 137.510909) (end 102.175599 137.365767) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 107.485157 139.910466) (end 107.396096 140.023797) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 122.932055 159.636241) (end 122.974704 159.581969) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 144.951044 121.634973) (end 145.040105 121.521642) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 125.099154 159.479947) (end 125.146724 159.529841) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 146.32355 120.611962) (end 146.462942 120.564797) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 135.352257 132.317009) (end 135.575757 131.858007) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 124.768083 159.23256) (end 124.828246 159.267152) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 122.654063 160.6427) (end 122.648515 160.569741) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 144.421541 116.93765) (end 144.367269 116.980299) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 144.85717 116.323031) (end 144.831446 116.388272) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 122.82004 161.180603) (end 122.788314 161.118658) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 105.830897 141.021068) (end 105.685755 141.054567) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 149.992966 124.859904) (end 149.92073 124.985535) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 145.799442 120.864242) (end 145.925073 120.792006) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 107.986703 138.865265) (end 107.946277 139.007626) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 104.331405 141.021068) (end 104.189043 140.980642) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 144.650883 122.129296) (end 144.717134 121.999942) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 125.191878 159.581969) (end 125.234527 159.636241) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 143.726487 114.40897) (end 143.797234 114.421604) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 155.943025 127.991032) (end 156.013772 127.978398) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 106.636759 135.549835) (end 106.758479 135.627867) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 144.367269 116.980299) (end 144.310943 117.020353) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 103.172873 135.800568) (end 103.286204 135.711508) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 106.989429 140.430464) (end 106.876098 140.519524) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 103.286204 135.711508) (end 103.403823 135.627867) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 145.799442 125.995605) (end 145.677722 125.917572) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 144.489924 122.537813) (end 144.537089 122.39842) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 123.280047 159.30452) (end 123.338336 159.267152) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 102.316906 136.947778) (end 102.376984 136.814889) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 146.054427 120.725755) (end 146.187315 120.665677) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 123.067428 159.479947) (end 123.117321 159.432378) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 103.525542 140.681197) (end 103.403823 140.603165) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 124.157221 159.061035) (end 124.23018 159.066582) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 125.31195 161.240766) (end 125.274581 161.299055) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 124.083291 159.059165) (end 124.157221 159.061035) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 156.23256 130.835136) (end 156.15863 130.833266) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 108.081151 138.115516) (end 108.077247 138.269896) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 134.832881 133.20148) (end 135.104593 132.765217) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 102.860497 140.132651) (end 102.766206 140.023797) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 149.372182 121.209267) (end 149.47637 121.308601) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 144.449498 124.179672) (end 144.415999 124.03453) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 105.973259 140.980642) (end 105.830897 141.021068) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 124.442333 161.887227) (end 124.372826 161.903269) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 142.94849 117.15281) (end 142.884852 117.12404) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 143.433769 117.263839) (end 143.36081 117.258291) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 154.883089 128.904521) (end 154.908813 128.839281) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 155.738591 128.049019) (end 155.805344 128.026433) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 107.301805 140.132651) (end 107.202471 140.236839) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 144.915157 116.118598) (end 144.899115 116.188104) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 154.795915 129.39849) (end 154.795915 129.39849) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 144.358954 123.275543) (end 144.370539 123.12319) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 147.35505 120.429923) (end 147.35505 120.429923) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 143.080483 117.20112) (end 143.01373 117.178533) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 157.640018 129.688026) (end 157.623976 129.757532) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 106.876098 140.519524) (end 106.758479 140.603165) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 132.059495 98.093734) (end 132.059495 98.093734) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 124.706138 161.790788) (end 124.6425 161.819558) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 136.32682 129.441275) (end 136.402946 128.941628) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 156.522096 130.805948) (end 156.451348 130.818582) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 132.059495 119.582572) (end 132.059495 119.582572) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 105.387883 141.100027) (end 105.23553 141.111612) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 156.23256 127.961845) (end 156.23256 127.961845) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 123.169449 159.387224) (end 123.223721 159.344574) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 107.986703 137.365767) (end 108.020202 137.510909) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 103.064019 140.336172) (end 102.959831 140.236839) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 123.019858 159.529841) (end 123.067428 159.479947) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 104.189043 135.250389) (end 104.331405 135.209963) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 123.864503 159.075718) (end 123.936402 159.066582) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 102.959831 135.994193) (end 103.064019 135.894859) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 108.081151 138.115516) (end 108.081151 138.115516) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 142.100241 116.118598) (end 142.087607 116.047851) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 146.89818 120.46449) (end 147.048318 120.445412) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 144.736357 116.574018) (end 144.698989 116.632307) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 144.370539 123.12319) (end 144.389617 122.973051) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 143.934915 117.20112) (end 143.86674 117.220479) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 122.691875 160.136769) (end 122.711234 160.068595) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 122.759544 161.05502) (end 122.73382 160.989779) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 105.685755 135.176465) (end 105.830897 135.209963) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 142.071053 115.829063) (end 142.072923 115.755133) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 145.446772 125.744871) (end 145.337918 125.65058) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 145.23373 121.308601) (end 145.337918 121.209267) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 123.223721 159.344574) (end 123.280047 159.30452) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 144.77095 116.513855) (end 144.736357 116.574018) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 108.081151 138.115516) (end 108.081151 138.115516) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 142.072923 115.755133) (end 142.078471 115.682173) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 156.791769 128.074743) (end 156.855407 128.103513) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 144.415999 124.03453) (end 144.389617 123.886795) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 157.248424 128.382627) (end 157.295993 128.43252) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 150.351146 123.584303) (end 150.339561 123.736657) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 142.087607 115.610275) (end 142.100241 115.539527) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 142.541729 116.892495) (end 142.491836 116.844926) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 147.35505 126.429923) (end 147.35505 126.429923) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 133.784703 120.964019) (end 133.394041 120.590616) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 107.646831 136.559904) (end 107.719067 136.685535) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 142.356463 116.688632) (end 142.316409 116.632307) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 144.927791 115.610275) (end 144.936927 115.682173) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 157.604617 129.825706) (end 157.582031 129.892459) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 155.318718 128.289903) (end 155.37299 128.247254) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 149.263328 125.744871) (end 149.149997 125.833931) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 146.462942 120.564797) (end 146.605304 120.524371) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 155.429316 128.2072) (end 155.487605 128.169832) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 144.85717 115.335094) (end 144.879756 115.401847) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 148.104796 126.335476) (end 147.959654 126.368974) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 144.899115 115.470021) (end 144.915157 115.539527) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 144.717134 124.859904) (end 144.650883 124.73055) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 157.09213 128.247254) (end 157.146402 128.289903) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 103.286204 140.519524) (end 103.172873 140.430464) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 107.098283 140.336172) (end 106.989429 140.430464) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 102.443235 136.685535) (end 102.515471 136.559904) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 124.009361 159.061035) (end 124.083291 159.059165) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 125.234527 161.35538) (end 125.191878 161.409652) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 156.659776 128.026433) (end 156.726529 128.049019) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 149.372182 125.65058) (end 149.263328 125.744871) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 144.616286 116.742904) (end 144.571132 116.795032) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 144.698989 115.025819) (end 144.736357 115.084108) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 105.973259 135.250389) (end 106.112651 135.297554) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 124.302079 161.915903) (end 124.23018 161.925039) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 149.575704 121.412789) (end 149.669995 121.521642) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 142.135642 116.256279) (end 142.116283 116.188104) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 139.75186 151.724638) (end 140.734008 150.800197) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 124.57726 159.14634) (end 124.6425 159.172063) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 148.104796 120.524371) (end 148.247158 120.564797) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 155.003902 130.143445) (end 154.969309 130.083283) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 142.444266 116.795032) (end 142.399112 116.742904) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 102.766206 140.023797) (end 102.677145 139.910466) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 142.244448 115.14427) (end 142.27904 115.084108) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 144.802676 116.45191) (end 144.77095 116.513855) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 107.719067 139.545497) (end 107.646831 139.671128) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 146.054427 126.134092) (end 145.925073 126.067841) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 125.378268 159.872964) (end 125.407038 159.936602) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 102.115718 138.572388) (end 102.09664 138.422249) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 156.379449 127.969262) (end 156.451348 127.978398) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 125.474707 160.854852) (end 125.455348 160.923027) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 157.661788 129.251601) (end 157.667336 129.32456) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 147.81192 120.46449) (end 147.959654 120.490872) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 149.47637 125.551246) (end 149.372182 125.65058) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 150.059217 122.129296) (end 150.119295 122.262185) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 156.23256 127.961845) (end 156.30649 127.963714) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 134.217767 134.033576) (end 134.537234 133.624649) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 125.099154 161.511674) (end 125.049261 161.559243) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 125.31195 159.750856) (end 125.346542 159.811018) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 133.004143 155.502724) (end 134.2128 155.083918) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 122.854632 161.240766) (end 122.82004 161.180603) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 107.845396 136.947778) (end 107.899112 137.084013) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 106.876098 135.711508) (end 106.989429 135.800568) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 125.512519 160.6427) (end 125.503383 160.714599) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 122.974704 159.581969) (end 123.019858 159.529841) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 143.01373 117.178533) (end 142.94849 117.15281) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 147.200671 126.42602) (end 147.048318 126.414435) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 145.134396 121.412789) (end 145.23373 121.308601) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 142.183952 116.388272) (end 142.158228 116.323031) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 105.081151 135.115516) (end 105.23553 135.119419) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 157.146402 128.289903) (end 157.19853 128.335058) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 146.187315 126.194169) (end 146.054427 126.134092) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 102.376984 136.814889) (end 102.443235 136.685535) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 124.372826 161.903269) (end 124.302079 161.915903) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 157.669206 129.39849) (end 157.669206 129.39849) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 157.604617 128.971274) (end 157.623976 129.039449) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 143.01373 114.479592) (end 143.080483 114.457005) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 148.655673 120.725755) (end 148.785027 120.792006) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 144.001668 114.479592) (end 144.066908 114.505315) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 156.085671 130.827718) (end 156.013772 130.818582) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 143.507699 114.392417) (end 143.581629 114.394286) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 157.495811 128.713698) (end 157.527537 128.775643) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 142.541729 114.76563) (end 142.593857 114.720476) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 91.44 63.5) (end 93.19 83.52) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 107.785318 139.416143) (end 107.719067 139.545497) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 117.537597 153.918092) (end 118.816354 154.517715) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 157.341147 128.484648) (end 157.383796 128.53892) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 102.085055 137.961136) (end 102.09664 137.808782) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 146.750446 126.368974) (end 146.605304 126.335476) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 107.485157 136.320565) (end 107.568798 136.438185) (layer "Edge.Cuts") (width 0.264582))
  (gr_arc (start 149.49 101.87) (mid 146.790647 91.769417) (end 153.200217 83.509532) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 144.473669 114.76563) (end 144.523562 114.813199) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 123.656075 161.867868) (end 123.589322 161.845281) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 103.780528 140.819684) (end 103.651173 140.753433) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 124.997133 159.387224) (end 125.049261 159.432378) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 125.234527 159.636241) (end 125.274581 159.692567) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 155.26659 130.461923) (end 155.216697 130.414354) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 108.69391 116.204368) (end 101.468404 111.418639) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 143.726487 117.249155) (end 143.654588 117.258291) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 146.89818 126.395357) (end 146.750446 126.368974) (layer "Edge.Cuts") (width 0.264582))
  (gr_arc (start 136.212443 61.774635) (mid 133.090522 62.080338) (end 132.450217 59.009532) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 104.476547 135.176465) (end 104.624281 135.150082) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 157.527537 128.775643) (end 157.556307 128.839281) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 155.123973 128.484648) (end 155.169128 128.43252) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 144.915157 115.539527) (end 144.927791 115.610275) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 141.665996 149.791715) (end 142.544277 148.699259) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 123.524082 159.172063) (end 123.589322 159.14634) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 125.407038 159.936602) (end 125.432762 160.001842) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 144.802676 115.206215) (end 144.831446 115.269854) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 106.381774 140.819684) (end 106.248886 140.879762) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 125.519936 160.495811) (end 125.519936 160.495811) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 122.854632 159.750856) (end 122.892001 159.692567) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 123.398498 159.23256) (end 123.460444 159.200833) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 143.86674 117.220479) (end 143.797234 117.236521) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 157.42385 128.595246) (end 157.461219 128.653535) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 157.295993 130.36446) (end 157.248424 130.414354) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 103.913416 135.35127) (end 104.049651 135.297554) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 123.589322 161.845281) (end 123.524082 161.819558) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 154.812468 129.179702) (end 154.825102 129.108955) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 142.087607 116.047851) (end 142.078471 115.975952) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 102.216025 139.007626) (end 102.175599 138.865265) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 157.667336 129.32456) (end 157.669206 129.39849) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 157.341147 130.312332) (end 157.295993 130.36446) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 144.616286 114.915221) (end 144.658935 114.969493) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 124.372826 159.088353) (end 124.442333 159.104394) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 107.202471 135.994193) (end 107.301805 136.098381) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 155.805344 130.770547) (end 155.738591 130.747961) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 157.383796 130.25806) (end 157.341147 130.312332) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 112.916604 138.350059) (end 108.224717 146.044746) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 144.698989 116.632307) (end 144.658935 116.688632) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 132.059495 98.093734) (end 115.731736 97.999892) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 125.146724 161.46178) (end 125.099154 161.511674) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 123.793756 161.903269) (end 123.724249 161.887227) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 150.119295 124.597661) (end 150.059217 124.73055) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 145.925073 120.792006) (end 146.054427 120.725755) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 104.189698 131.593742) (end 112.916604 138.350059) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 122.932055 161.35538) (end 122.892001 161.299055) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 136.23049 125.431364) (end 136.103722 124.941866) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 155.943025 130.805948) (end 155.873519 130.789906) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 154.803332 129.251601) (end 154.812468 129.179702) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 104.926771 141.111612) (end 104.774419 141.100027) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 144.590805 122.262185) (end 144.650883 122.129296) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 147.200671 120.433827) (end 147.35505 120.429923) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 115.919412 116.110572) (end 108.69391 116.204368) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 156.659776 130.770547) (end 156.591602 130.789906) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 107.301805 136.098381) (end 107.396096 136.207235) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 125.274581 159.692567) (end 125.31195 159.750856) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 124.510507 161.867868) (end 124.442333 161.887227) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 144.944344 115.829063) (end 144.944344 115.829063) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 123.656075 159.123754) (end 123.724249 159.104394) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 124.706138 159.200833) (end 124.768083 159.23256) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 155.216697 130.414354) (end 155.169128 130.36446) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 125.432762 160.001842) (end 125.455348 160.068595) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 105.081151 141.115516) (end 105.081151 141.115516) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 144.571132 114.863093) (end 144.616286 114.915221) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 154.969309 128.713698) (end 155.003902 128.653535) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 107.568798 136.438185) (end 107.646831 136.559904) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 125.274581 161.299055) (end 125.234527 161.35538) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 134.485432 121.760017) (end 134.148462 121.354203) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 150.320483 123.886795) (end 150.294101 124.03453) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 135.575757 131.858007) (end 135.774981 131.389357) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 108.046584 138.572388) (end 108.020202 138.720122) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 102.312943 134.127357) (end 104.189698 131.593742) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 156.917353 128.135239) (end 156.977515 128.169832) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 132.531551 119.898743) (end 132.059495 119.582572) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 144.867403 125.107254) (end 144.78937 124.985535) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 143.36081 114.399834) (end 143.433769 114.394286) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 155.873519 130.789906) (end 155.805344 130.770547) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 145.925073 126.067841) (end 145.799442 125.995605) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 104.624281 135.150082) (end 104.774419 135.131004) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 108.224717 146.044746) (end 109.266565 147.328624) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 122.73382 160.989779) (end 122.711234 160.923027) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 142.491836 116.844926) (end 142.444266 116.795032) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 135.774981 131.389357) (end 135.949813 130.912211) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 142.648129 116.980299) (end 142.593857 116.93765) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 149.669995 125.338204) (end 149.575704 125.447058) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 157.19853 130.461923) (end 157.146402 130.507077) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 155.547768 128.135239) (end 155.609713 128.103513) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 142.544277 148.699259) (end 143.365306 147.522895) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 125.503383 160.277023) (end 125.512519 160.348921) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 143.934915 114.457005) (end 144.001668 114.479592) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 147.048318 126.414435) (end 146.89818 126.395357) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 125.049261 161.559243) (end 124.997133 161.604398) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 156.30649 130.833266) (end 156.23256 130.835136) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 144.252654 114.600404) (end 144.310943 114.637772) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 144.658935 114.969493) (end 144.698989 115.025819) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 123.169449 161.604398) (end 123.117321 161.559243) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 144.537089 124.461426) (end 144.489924 124.322034) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 142.648129 114.677826) (end 142.704455 114.637772) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 156.23256 130.835136) (end 156.23256 130.835136) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 157.495811 130.083283) (end 157.461219 130.143445) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 156.15863 130.833266) (end 156.085671 130.827718) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 136.10014 130.427715) (end 136.225847 129.93702) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 103.403823 140.603165) (end 103.286204 140.519524) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 142.078471 115.682173) (end 142.087607 115.610275) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 134.217767 134.033576) (end 134.217767 134.033576) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 142.244448 116.513855) (end 142.212722 116.45191) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 155.487605 130.627149) (end 155.429316 130.58978) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 154.860503 129.825706) (end 154.841144 129.757532) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 125.455348 160.923027) (end 125.432762 160.989779) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 123.936402 161.925039) (end 123.864503 161.915903) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 150.119295 122.262185) (end 150.173011 122.39842) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 150.173011 122.39842) (end 150.220176 122.537813) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 157.582031 128.904521) (end 157.604617 128.971274) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 104.189698 131.593742) (end 104.189698 131.593742) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 147.509429 120.433827) (end 147.661782 120.445412) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 145.337918 121.209267) (end 145.446772 121.114975) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 155.216697 128.382627) (end 155.26659 128.335058) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 123.460444 159.200833) (end 123.524082 159.172063) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 122.675833 160.206275) (end 122.691875 160.136769) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 144.367269 114.677826) (end 144.421541 114.720476) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 113.818733 151.60716) (end 115.035241 152.462881) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 142.593857 116.93765) (end 142.541729 116.892495) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 142.100241 115.539527) (end 142.116283 115.470021) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 156.977515 128.169832) (end 157.035804 128.2072) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 143.507699 117.265708) (end 143.433769 117.263839) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 122.648515 160.421881) (end 122.654063 160.348921) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 102.26319 137.084013) (end 102.316906 136.947778) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 155.169128 128.43252) (end 155.216697 128.382627) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 144.831446 116.388272) (end 144.802676 116.45191) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 124.768083 161.759062) (end 124.706138 161.790788) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 134.2128 155.083918) (end 135.39257 154.580673) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 122.73382 160.001842) (end 122.759544 159.936602) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 125.518067 160.421881) (end 125.519936 160.495811) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 157.667336 129.47242) (end 157.661788 129.545379) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 143.507699 117.265708) (end 143.507699 117.265708) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 125.503383 160.714599) (end 125.490749 160.785346) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 144.899115 116.188104) (end 144.879756 116.256279) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 144.821427 144.918708) (end 134.217767 134.033576) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 149.032378 120.942274) (end 149.149997 121.025915) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 104.189043 140.980642) (end 104.049651 140.933477) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 157.582031 129.892459) (end 157.556307 129.957699) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 144.944344 115.829063) (end 144.942475 115.902993) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 91.333932 126.901862) (end 91.333932 126.901862) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 145.337918 125.65058) (end 145.23373 125.551246) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 122.711234 160.068595) (end 122.73382 160.001842) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 147.35505 120.429923) (end 147.509429 120.433827) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 124.083291 161.932456) (end 124.083291 161.932456) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 148.522785 120.665677) (end 148.655673 120.725755) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 142.116283 115.470021) (end 142.135642 115.401847) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 142.491836 114.813199) (end 142.541729 114.76563) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 105.081151 141.115516) (end 104.926771 141.111612) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 123.398498 161.759062) (end 123.338336 161.724469) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 156.085671 127.969262) (end 156.15863 127.963714) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 102.175599 138.865265) (end 102.1421 138.720122) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 144.537089 122.39842) (end 144.590805 122.262185) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 123.223721 161.647047) (end 123.169449 161.604398) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 124.886535 159.30452) (end 124.942861 159.344574) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 144.867403 121.752592) (end 144.951044 121.634973) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 156.855407 128.103513) (end 156.917353 128.135239) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 155.26659 128.335058) (end 155.318718 128.289903) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 107.719067 136.685535) (end 107.785318 136.814889) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 142.072923 115.902993) (end 142.071053 115.829063) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 156.917353 130.661741) (end 156.855407 130.693468) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 144.658935 116.688632) (end 144.616286 116.742904) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 102.216025 137.223405) (end 102.26319 137.084013) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 143.581629 117.263839) (end 143.507699 117.265708) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 155.805344 128.026433) (end 155.873519 128.007074) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 157.146402 130.507077) (end 157.09213 130.549726) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 107.098283 135.894859) (end 107.202471 135.994193) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 155.673351 128.074743) (end 155.738591 128.049019) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 154.883089 129.892459) (end 154.860503 129.825706) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 124.23018 161.925039) (end 124.157221 161.930587) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 135.079462 122.613943) (end 134.795727 122.180314) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 106.989429 135.800568) (end 107.098283 135.894859) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 124.57726 161.845281) (end 124.510507 161.867868) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 144.35505 123.429923) (end 144.35505 123.429923) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 103.172873 140.430464) (end 103.064019 140.336172) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 157.652652 129.179702) (end 157.661788 129.251601) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 108.065662 138.422249) (end 108.046584 138.572388) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 155.673351 130.722238) (end 155.609713 130.693468) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 143.080483 114.457005) (end 143.148657 114.437646) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 157.527537 130.021337) (end 157.495811 130.083283) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 107.845396 139.283254) (end 107.785318 139.416143) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 155.081324 130.25806) (end 155.04127 130.201734) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 122.646645 160.495811) (end 122.648515 160.421881) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 156.15863 127.963714) (end 156.23256 127.961845) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 150.35505 123.429923) (end 150.35505 123.429923) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 122.788314 161.118658) (end 122.759544 161.05502) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 103.651173 135.477598) (end 103.780528 135.411347) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 123.338336 159.267152) (end 123.398498 159.23256) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 107.785318 136.814889) (end 107.845396 136.947778) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 144.717134 121.999942) (end 144.78937 121.874311) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 108.224717 146.044746) (end 108.224717 146.044746) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 107.899112 139.147019) (end 107.845396 139.283254) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 150.260602 124.179672) (end 150.220176 124.322034) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 142.444266 114.863093) (end 142.491836 114.813199) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 156.791769 130.722238) (end 156.726529 130.747961) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 125.344111 156.238648) (end 126.651637 156.327863) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 102.593504 139.792847) (end 102.515471 139.671128) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 103.913416 140.879762) (end 103.780528 140.819684) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 143.507699 114.392417) (end 143.507699 114.392417) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 105.23553 135.119419) (end 105.387883 135.131004) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 108.020202 138.720122) (end 107.986703 138.865265) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 144.125538 146.262689) (end 144.821427 144.918708) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 156.013772 127.978398) (end 156.085671 127.969262) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 144.77095 115.14427) (end 144.802676 115.206215) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 91.333932 126.901862) (end 102.312943 134.127357) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 155.04127 130.201734) (end 155.003902 130.143445) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 102.677145 139.910466) (end 102.593504 139.792847) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 122.788314 159.872964) (end 122.82004 159.811018) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 102.085055 138.269896) (end 102.081151 138.115516) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 123.724249 161.887227) (end 123.656075 161.867868) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 104.049651 140.933477) (end 103.913416 140.879762) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 148.247158 126.29505) (end 148.104796 126.335476) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 105.081151 135.115516) (end 105.081151 135.115516) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 125.519936 160.495811) (end 125.518067 160.569741) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 125.049261 159.432378) (end 125.099154 159.479947) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 148.910658 120.864242) (end 149.032378 120.942274) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 125.407038 161.05502) (end 125.378268 161.118658) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 143.581629 114.394286) (end 143.654588 114.399834) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 147.661782 120.445412) (end 147.81192 120.46449) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 144.78937 121.874311) (end 144.867403 121.752592) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 123.019858 161.46178) (end 122.974704 161.409652) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 136.225847 129.93702) (end 136.32682 129.441275) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 107.946277 137.223405) (end 107.986703 137.365767) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 155.609713 130.693468) (end 155.547768 130.661741) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 149.759056 125.224874) (end 149.669995 125.338204) (layer "Edge.Cuts") (width 0.264582))
  (gr_arc (start 149.49 101.87) (mid 123.179909 165.454039) (end 96.824368 101.888826) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 104.476547 141.054567) (end 104.331405 141.021068) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 108.020202 137.510909) (end 108.046584 137.658644) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 144.001668 117.178533) (end 143.934915 117.20112) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 147.81192 126.395357) (end 147.661782 126.414435) (layer "Edge.Cuts") (width 0.264582))
  (gr_arc (start 113.94 59.02) (mid 123.192569 54.524426) (end 132.450217 59.009532) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 144.736357 115.084108) (end 144.77095 115.14427) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 144.831446 115.269854) (end 144.85717 115.335094) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 145.040105 125.338204) (end 144.951044 125.224874) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 124.510507 159.123754) (end 124.57726 159.14634) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 105.685755 141.054567) (end 105.538021 141.080949) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 143.148657 114.437646) (end 143.218164 114.421604) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 112.630066 150.66594) (end 113.818733 151.60716) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 124.083291 161.932456) (end 124.009361 161.930587) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 148.522785 126.194169) (end 148.38655 126.247885) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 144.489924 124.322034) (end 144.449498 124.179672) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 142.704455 114.637772) (end 142.762744 114.600404) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 146.750446 120.490872) (end 146.89818 120.46449) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 112.916604 138.350059) (end 112.916604 138.350059) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 127.951549 156.332242) (end 129.240302 156.251851) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 121.411299 155.461325) (end 122.720396 155.805446) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 155.169128 130.36446) (end 155.123973 130.312332) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 157.556307 128.839281) (end 157.582031 128.904521) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 142.94849 114.505315) (end 143.01373 114.479592) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 126.651637 156.327863) (end 127.951549 156.332242) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 136.539906 153.993057) (end 137.651263 153.321134) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 125.346542 159.811018) (end 125.378268 159.872964) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 148.38655 126.247885) (end 148.247158 126.29505) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 144.942475 115.902993) (end 144.936927 115.975952) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 144.473669 116.892495) (end 144.421541 116.93765) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 142.884852 117.12404) (end 142.822906 117.092314) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 120.10877 155.032104) (end 121.411299 155.461325) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 137.651263 153.321134) (end 138.723097 152.564973) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 104.624281 141.080949) (end 104.476547 141.054567) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 154.803332 129.545379) (end 154.797784 129.47242) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 144.944344 115.829063) (end 144.944344 115.829063) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 125.191878 161.409652) (end 125.146724 161.46178) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 135.567706 123.516603) (end 135.33675 123.059755) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 101.468404 111.418639) (end 101.468404 111.418639) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 155.37299 130.549726) (end 155.318718 130.507077) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 147.048318 120.445412) (end 147.200671 120.433827) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 150.220176 124.322034) (end 150.173011 124.461426) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 142.183952 115.269854) (end 142.212722 115.206215) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 144.192491 114.565812) (end 144.252654 114.600404) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 104.774419 141.100027) (end 104.624281 141.080949) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 132.059495 119.582572) (end 132.059495 98.093734) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 156.591602 128.007074) (end 156.659776 128.026433) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 144.590805 124.597661) (end 144.537089 124.461426) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 149.842697 125.107254) (end 149.759056 125.224874) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 144.130546 114.534085) (end 144.192491 114.565812) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 124.942861 161.647047) (end 124.886535 161.687101) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 134.148462 121.354203) (end 133.784703 120.964019) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 103.525542 135.549835) (end 103.651173 135.477598) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 144.879756 116.256279) (end 144.85717 116.323031) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 150.339561 123.736657) (end 150.320483 123.886795) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 122.663199 160.277023) (end 122.675833 160.206275) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 124.23018 159.066582) (end 124.302079 159.075718) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 144.523562 114.813199) (end 144.571132 114.863093) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 143.36081 117.258291) (end 143.288911 117.249155) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 105.23553 141.111612) (end 105.081151 141.115516) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 122.646645 160.495811) (end 122.646645 160.495811) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 157.248424 130.414354) (end 157.19853 130.461923) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 106.381774 135.411347) (end 106.511128 135.477598) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 102.175599 137.365767) (end 102.216025 137.223405) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 122.691875 160.854852) (end 122.675833 160.785346) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 144.936927 115.682173) (end 144.942475 115.755133) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 143.654588 117.258291) (end 143.581629 117.263839) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 150.294101 122.825317) (end 150.320483 122.973051) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 145.446772 121.114975) (end 145.560103 121.025915) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 135.104593 132.765217) (end 135.352257 132.317009) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 157.623976 129.757532) (end 157.604617 129.825706) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 150.320483 122.973051) (end 150.339561 123.12319) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 144.252654 117.057721) (end 144.192491 117.092314) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 157.295993 128.43252) (end 157.341147 128.484648) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 157.669206 129.39849) (end 157.669206 129.39849) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 102.860497 136.098381) (end 102.959831 135.994193) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 123.117321 161.559243) (end 123.067428 161.511674) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 142.078471 115.975952) (end 142.072923 115.902993) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 123.724249 159.104394) (end 123.793756 159.088353) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 142.356463 114.969493) (end 142.399112 114.915221) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 145.560103 125.833931) (end 145.446772 125.744871) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 142.135642 115.401847) (end 142.158228 115.335094) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 149.992966 121.999942) (end 150.059217 122.129296) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 106.112651 135.297554) (end 106.248886 135.35127) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 106.636759 140.681197) (end 106.511128 140.753433) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 105.830897 135.209963) (end 105.973259 135.250389) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 154.797784 129.32456) (end 154.803332 129.251601) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 144.879756 115.401847) (end 144.899115 115.470021) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 107.646831 139.671128) (end 107.568798 139.792847) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 125.378268 161.118658) (end 125.346542 161.180603) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 136.454109 128.439228) (end 136.480196 127.935224) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 123.117321 159.432378) (end 123.169449 159.387224) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 136.331497 125.926152) (end 136.23049 125.431364) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 122.892001 159.692567) (end 122.932055 159.636241) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 135.951077 124.458807) (end 135.772443 123.983337) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 124.6425 159.172063) (end 124.706138 159.200833) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 135.33675 123.059755) (end 135.079462 122.613943) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 125.455348 160.068595) (end 125.474707 160.136769) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 122.675833 160.785346) (end 122.663199 160.714599) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 123.936402 159.066582) (end 124.009361 159.061035) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 105.538021 135.150082) (end 105.685755 135.176465) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 149.575704 125.447058) (end 149.47637 125.551246) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 115.919412 116.110572) (end 115.919412 116.110572) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 155.738591 130.747961) (end 155.673351 130.722238) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 134.795727 122.180314) (end 134.485432 121.760017) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 102.081151 138.115516) (end 102.081151 138.115516) (layer "Edge.Cuts") (width 0.264582))
  (gr_arc (start 136.212443 61.774635) (mid 145.968218 58.404755) (end 154.950216 63.489533) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 142.071053 115.829063) (end 142.071053 115.829063) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 144.449498 122.680174) (end 144.489924 122.537813) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 106.511128 140.753433) (end 106.381774 140.819684) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 142.27904 115.084108) (end 142.316409 115.025819) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 144.358954 123.584303) (end 144.35505 123.429923) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 124.828246 161.724469) (end 124.768083 161.759062) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 155.609713 128.103513) (end 155.673351 128.074743) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 154.825102 129.108955) (end 154.841144 129.039449) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 157.383796 128.53892) (end 157.42385 128.595246) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 157.669206 129.39849) (end 157.667336 129.47242) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 102.312943 134.127357) (end 102.312943 134.127357) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 142.884852 114.534085) (end 142.94849 114.505315) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 144.571132 116.795032) (end 144.523562 116.844926) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 144.927791 116.047851) (end 144.915157 116.118598) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 147.661782 126.414435) (end 147.509429 126.42602) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 157.035804 130.58978) (end 156.977515 130.627149) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 122.759544 159.936602) (end 122.788314 159.872964) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 135.949813 130.912211) (end 136.10014 130.427715) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 149.92073 124.985535) (end 149.842697 125.107254) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 125.519936 160.495811) (end 125.519936 160.495811) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 150.35505 123.429923) (end 150.35505 123.429923) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 102.677145 136.320565) (end 102.766206 136.207235) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 123.460444 161.790788) (end 123.398498 161.759062) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 102.26319 139.147019) (end 102.216025 139.007626) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 157.623976 129.039449) (end 157.640018 129.108955) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 122.648515 160.569741) (end 122.646645 160.495811) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 145.560103 121.025915) (end 145.677722 120.942274) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 150.339561 123.12319) (end 150.351146 123.275543) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 124.302079 159.075718) (end 124.372826 159.088353) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 147.509429 126.42602) (end 147.35505 126.429923) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 144.936927 115.975952) (end 144.927791 116.047851) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 154.937583 130.021337) (end 154.908813 129.957699) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 102.376984 139.416143) (end 102.316906 139.283254) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 144.192491 117.092314) (end 144.130546 117.12404) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 144.650883 124.73055) (end 144.590805 124.597661) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 147.35505 126.429923) (end 147.200671 126.42602) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 155.318718 130.507077) (end 155.26659 130.461923) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 103.651173 140.753433) (end 103.525542 140.681197) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 107.396096 136.207235) (end 107.485157 136.320565) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 136.481093 127.430766) (end 136.456684 126.927001) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 154.908813 128.839281) (end 154.937583 128.775643) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 125.518067 160.569741) (end 125.512519 160.6427) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 106.758479 135.627867) (end 106.876098 135.711508) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 157.19853 128.335058) (end 157.248424 128.382627) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 156.977515 130.627149) (end 156.917353 130.661741) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 107.946277 139.007626) (end 107.899112 139.147019) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 154.860503 128.971274) (end 154.883089 128.904521) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 136.402946 128.941628) (end 136.454109 128.439228) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 150.294101 124.03453) (end 150.260602 124.179672) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 109.266565 147.328624) (end 110.350437 148.526738) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 124.997133 161.604398) (end 124.942861 161.647047) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 142.399112 114.915221) (end 142.444266 114.863093) (layer "Edge.Cuts") (width 0.126705))
  (gr_line (start 150.351146 123.275543) (end 150.35505 123.429923) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 111.472785 149.639154) (end 112.630066 150.66594) (layer "Edge.Cuts") (width 0.264582))
  (gr_line (start 129.240302 156.251851) (end 130.514348 156.086757) (layer "Edge.Cuts") (width 0.264582))
  (gr_text "Move dial \npartway to \nread total " (at 99.5172 151.2824 -35.5) (layer "B.SilkS"))
  (gr_text "Dial 0 to \nsubtract next \nnumber dialed" (at 114.935 158.2928 -27) (layer "B.SilkS"))
  (gr_text "Dial 0\nthree times \nto clear total" (at 131.5466 160.0708 13) (layer "B.SilkS"))
  (gr_text "JLCJLCJLCJLCJLC" (at 114.2238 106.1212 90) (layer "F.SilkS"))
  (zone (net 2) (net_name "GND") (layer "F.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (mode hatch) (thermal_gap 0.508) (thermal_bridge_width 0.508)
      (hatch_thickness 0.3) (hatch_gap 0.5) (hatch_orientation 22.5)
      (hatch_smoothing_level 2) (hatch_smoothing_value 0.1)
      (hatch_border_algorithm hatch_thickness) (hatch_min_hole_area 0.3))
    (polygon
      (pts
        (xy 252.2474 16.891)
        (xy 264.9728 125.8316)
        (xy 240.6904 207.4164)
        (xy 41.8084 213.5124)
        (xy 8.7884 15.4686)
        (xy 168.402 8.636)
        (xy 199.263 5.9436)
      )
    )
  )
  (zone (net 2) (net_name "GND") (layer "B.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (mode hatch) (thermal_gap 0.508) (thermal_bridge_width 0.508)
      (hatch_thickness 0.4) (hatch_gap 0.4) (hatch_orientation 22.5)
      (hatch_smoothing_level 2) (hatch_smoothing_value 0.8)
      (hatch_border_algorithm hatch_thickness) (hatch_min_hole_area 0.3))
    (polygon
      (pts
        (xy 115.316 3.2258)
        (xy 154.7368 8.763)
        (xy 280.6954 18.6182)
        (xy 286.2326 191.0588)
        (xy 103.632 200.914)
        (xy 11.3792 183.8452)
        (xy 16.7894 87.9856)
        (xy 21.9456 24.0792)
      )
    )
  )
)
