# Adafruit_Si5351 [![Build Status](https://github.com/adafruit/Adafruit_Si5351_Library/workflows/Arduino%20Library%20CI/badge.svg)](https://github.com/adafruit/Adafruit_Si5351_Library/actions)[![Documentation](https://github.com/adafruit/ci-arduino/blob/master/assets/doxygen_badge.svg)](http://adafruit.github.io/Adafruit_Si5351_Library/html/index.html)
===============

Driver for Adafruit's Si5351 Clockgen Breakout

Designed specifically to work with the Si5351 breakout in the adafruit shop
  ----> https://www.adafruit.com/products/2045

This chip uses I2C to communicate, 2 pins are required to interface

Adafruit invests time and resources providing this open source code, 
please support Adafruit and open-source hardware by purchasing 
products from Adafruit!

Check out the links above for our tutorials and wiring diagrams 

Written by Limor Fried/Ladyada for Adafruit Industries.  
BSD license, all text above must be included in any redistribution

To download. click the ZIP button on the right, rename the uncompressed folder Adafruit_Si5351. Check that the Adafruit_Si5351 folder contains Adafruit_Si5351.cpp and Adafruit_Si5351.h

Place the Adafruit_Si5351 library folder your arduinosketchfolder/libraries/ folder. You may need to create the libraries subfolder if its your first library. Restart the IDE.
