(kicad_pcb (version 20211014) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "Net-(J2-Pad20)")
  (net 2 "Net-(J2-Pad21)")
  (net 3 "Net-(J2-Pad22)")
  (net 4 "Net-(J2-Pad23)")
  (net 5 "Net-(J2-Pad24)")
  (net 6 "Net-(J2-Pad25)")
  (net 7 "Net-(J2-Pad26)")
  (net 8 "Net-(J2-Pad27)")
  (net 9 "Net-(J2-Pad28)")
  (net 10 "Net-(J1-Pad1)")
  (net 11 "Net-(J1-Pad2)")
  (net 12 "Net-(J1-Pad3)")
  (net 13 "Net-(J1-Pad4)")
  (net 14 "Net-(J1-Pad5)")
  (net 15 "Net-(J1-Pad6)")
  (net 16 "Net-(J1-Pad7)")
  (net 17 "Net-(J1-Pad8)")
  (net 18 "Net-(J1-Pad9)")
  (net 19 "GND")
  (net 20 "Net-(J1-Pad11)")
  (net 21 "Net-(J1-Pad12)")
  (net 22 "Net-(J1-Pad13)")
  (net 23 "Net-(J1-Pad14)")
  (net 24 "Net-(J1-Pad15)")
  (net 25 "Net-(J1-Pad16)")
  (net 26 "Net-(J1-Pad17)")
  (net 27 "Net-(J1-Pad18)")
  (net 28 "Net-(J1-Pad19)")
  (net 29 "+5V")
  (net 30 "Net-(J2-Pad29)")
  (net 31 "Net-(J2-Pad30)")
  (net 32 "Net-(J2-Pad31)")
  (net 33 "Net-(R2-Pad2)")
  (net 34 "Net-(R3-Pad2)")
  (net 35 "Net-(R4-Pad2)")
  (net 36 "Net-(R5-Pad2)")
  (net 37 "Net-(R6-Pad2)")
  (net 38 "Net-(R7-Pad2)")
  (net 39 "Net-(R8-Pad2)")
  (net 40 "Net-(R9-Pad2)")
  (net 41 "Net-(D1-Pad1)")
  (net 42 "Net-(D2-Pad1)")
  (net 43 "Net-(D3-Pad1)")
  (net 44 "Net-(D4-Pad1)")
  (net 45 "Net-(D5-Pad1)")
  (net 46 "Net-(D6-Pad1)")
  (net 47 "Net-(D7-Pad1)")
  (net 48 "Net-(D8-Pad1)")
  (net 49 "Net-(D9-Pad1)")
  (net 50 "Net-(D10-Pad1)")
  (net 51 "Net-(D11-Pad1)")
  (net 52 "Net-(D12-Pad1)")
  (net 53 "Net-(D13-Pad1)")
  (net 54 "Net-(D14-Pad1)")
  (net 55 "Net-(D15-Pad1)")
  (net 56 "Net-(D16-Pad1)")
  (net 57 "Net-(D17-Pad1)")
  (net 58 "Net-(D18-Pad1)")
  (net 59 "Net-(D19-Pad1)")
  (net 60 "Net-(D20-Pad1)")
  (net 61 "Net-(D21-Pad1)")
  (net 62 "Net-(D22-Pad1)")
  (net 63 "Net-(D23-Pad1)")
  (net 64 "Net-(D24-Pad1)")
  (net 65 "Net-(D25-Pad1)")
  (net 66 "Net-(D26-Pad1)")
  (net 67 "Net-(D27-Pad1)")
  (net 68 "Net-(D28-Pad1)")
  (net 69 "Net-(D29-Pad1)")
  (net 70 "Net-(D30-Pad1)")
  (net 71 "Net-(R1-Pad2)")
  (net 72 "Net-(R10-Pad2)")
  (net 73 "Net-(R11-Pad2)")
  (net 74 "Net-(R12-Pad2)")
  (net 75 "Net-(R13-Pad2)")
  (net 76 "Net-(R14-Pad2)")
  (net 77 "Net-(R15-Pad2)")
  (net 78 "Net-(R16-Pad2)")
  (net 79 "Net-(R17-Pad2)")
  (net 80 "Net-(R18-Pad2)")
  (net 81 "Net-(R19-Pad2)")
  (net 82 "Net-(R20-Pad2)")
  (net 83 "Net-(R21-Pad2)")
  (net 84 "Net-(R22-Pad2)")
  (net 85 "Net-(R23-Pad2)")
  (net 86 "Net-(R24-Pad2)")
  (net 87 "Net-(R25-Pad2)")
  (net 88 "Net-(R26-Pad2)")
  (net 89 "Net-(R27-Pad2)")
  (net 90 "Net-(R28-Pad2)")
  (net 91 "Net-(R29-Pad2)")
  (net 92 "Net-(R30-Pad2)")
  (net 93 "Net-(D13-Pad2)")
  (net 94 "Net-(D15-Pad2)")
  (net 95 "Net-(D19-Pad2)")
  (net 96 "Net-(D27-Pad2)")
  (footprint "LED_THT:LED_D5.0mm" (layer "F.Cu")
    (tedit 5995936A)
    (at 46.36 35.56 180)
    (descr "LED, diameter 5.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LL-504BC2E-009.pdf")
    (tags "LED diameter 5.0mm 2 pins")
    (property "Sheetfile" "MultiTester.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "D30" (at -3.932 2.54) (layer "F.SilkS"))
    (fp_text value "LED" (at 1.27 3.96) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.25 0) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 70 "Net-(D30-Pad1)") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 96 "Net-(D27-Pad2)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_THT.3dshapes/LED_D5.0mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 50.165 126.365)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "MultiTester.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R17" (at 5.08 -2.37) (layer "F.SilkS"))
    (fp_text value "1K" (at 5.08 2.37) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 5.08 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 57 "Net-(D17-Pad1)") (pintype "passive"))
    (pad "2" thru_hole oval (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 79 "Net-(R17-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 33.02 98.425 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "MultiTester.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R10" (at 5.08 -2.37) (layer "F.SilkS"))
    (fp_text value "1K" (at 5.08 2.37) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 5.08 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 50 "Net-(D10-Pad1)") (pintype "passive"))
    (pad "2" thru_hole oval (at 10.16 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 72 "Net-(R10-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Disc_D3.4mm_W2.1mm_P2.50mm" (layer "F.Cu")
    (tedit 5AE50EF0)
    (at 70.475 92.08 180)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.4*2.1mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3.4mm width 2.1mm Capacitor")
    (property "Sheetfile" "MultiTester.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C4" (at 4.943 0.132) (layer "F.SilkS"))
    (fp_text value "C" (at 1.25 2.3) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.25 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 29 "+5V") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D3.4mm_W2.1mm_P2.50mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 33.02 119.38 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "MultiTester.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R13" (at 5.08 -2.37) (layer "F.SilkS"))
    (fp_text value "1K" (at 5.08 2.37) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 5.08 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 53 "Net-(D13-Pad1)") (pintype "passive"))
    (pad "2" thru_hole oval (at 10.16 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 75 "Net-(R13-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 50.165 91.44)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "MultiTester.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R22" (at 5.08 -2.37) (layer "F.SilkS"))
    (fp_text value "1K" (at 5.08 2.37) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 5.08 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 62 "Net-(D22-Pad1)") (pintype "passive"))
    (pad "2" thru_hole oval (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 84 "Net-(R22-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_THT:LED_D5.0mm" (layer "F.Cu")
    (tedit 5995936A)
    (at 46.365 112.395 180)
    (descr "LED, diameter 5.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LL-504BC2E-009.pdf")
    (tags "LED diameter 5.0mm 2 pins")
    (property "Sheetfile" "MultiTester.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "D19" (at -3.927 2.159) (layer "F.SilkS"))
    (fp_text value "LED" (at 1.27 3.96) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.25 0) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 59 "Net-(D19-Pad1)") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 95 "Net-(D19-Pad2)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_THT.3dshapes/LED_D5.0mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_DIP:DIP-14_W7.62mm" (layer "F.Cu")
    (tedit 5A02E8C5)
    (at 65.405 27.94)
    (descr "14-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (property "Sheetfile" "MultiTester.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U1" (at -0.381 -2.54) (layer "F.SilkS"))
    (fp_text value "74LS06" (at 3.81 17.57) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 7.62) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "Net-(J1-Pad1)") (pintype "input"))
    (pad "2" thru_hole oval (at 0 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 71 "Net-(R1-Pad2)") (pintype "open_collector"))
    (pad "3" thru_hole oval (at 0 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 "Net-(J1-Pad2)") (pintype "input"))
    (pad "4" thru_hole oval (at 0 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 33 "Net-(R2-Pad2)") (pintype "open_collector"))
    (pad "5" thru_hole oval (at 0 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 "Net-(J1-Pad3)") (pintype "input"))
    (pad "6" thru_hole oval (at 0 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 34 "Net-(R3-Pad2)") (pintype "open_collector"))
    (pad "7" thru_hole oval (at 0 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "8" thru_hole oval (at 7.62 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 35 "Net-(R4-Pad2)") (pintype "open_collector"))
    (pad "9" thru_hole oval (at 7.62 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 "Net-(J1-Pad4)") (pintype "input"))
    (pad "10" thru_hole oval (at 7.62 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 36 "Net-(R5-Pad2)") (pintype "open_collector"))
    (pad "11" thru_hole oval (at 7.62 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 "Net-(J1-Pad5)") (pintype "input"))
    (pad "12" thru_hole oval (at 7.62 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 37 "Net-(R6-Pad2)") (pintype "open_collector"))
    (pad "13" thru_hole oval (at 7.62 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 "Net-(J1-Pad6)") (pintype "input"))
    (pad "14" thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 29 "+5V") (pinfunction "VCC") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-14_W7.62mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_THT:LED_D5.0mm" (layer "F.Cu")
    (tedit 5995936A)
    (at 36.688 119.38)
    (descr "LED, diameter 5.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LL-504BC2E-009.pdf")
    (tags "LED diameter 5.0mm 2 pins")
    (property "Sheetfile" "MultiTester.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "D13" (at -3.668 -2.032) (layer "F.SilkS"))
    (fp_text value "LED" (at 1.27 3.96) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.25 0) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 53 "Net-(D13-Pad1)") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 93 "Net-(D13-Pad2)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_THT.3dshapes/LED_D5.0mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_THT:LED_D5.0mm" (layer "F.Cu")
    (tedit 5995936A)
    (at 46.365 91.44 180)
    (descr "LED, diameter 5.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LL-504BC2E-009.pdf")
    (tags "LED diameter 5.0mm 2 pins")
    (property "Sheetfile" "MultiTester.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "D22" (at -3.927 2.54) (layer "F.SilkS"))
    (fp_text value "LED" (at 1.27 3.96) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.25 0) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 62 "Net-(D22-Pad1)") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 95 "Net-(D19-Pad2)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_THT.3dshapes/LED_D5.0mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Socket:DIP_Socket-20_W4.3_W5.08_W7.62_W10.16_W10.9_3M_220-3342-00-0602J" (layer "F.Cu")
    (tedit 5AF5D4CC)
    (at 136.525 38.735)
    (descr "3M 20-pin zero insertion force socket, through-hole, row spacing 7.62 mm (300 mils), http://multimedia.3m.com/mws/media/494546O/3mtm-dip-sockets-100-2-54-mm-ts0365.pdf")
    (tags "THT DIP DIL ZIF 7.62mm 300mil Socket")
    (property "Sheetfile" "MultiTester.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J1" (at 3.81 -11.56) (layer "F.SilkS"))
    (fp_text value "Conn_01x20_Female" (at 3.81 30.84) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 9.64) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 2 1.44) (drill 1) (layers *.Cu *.Mask)
      (net 10 "Net-(J1-Pad1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54) (size 2 1.44) (drill 1) (layers *.Cu *.Mask)
      (net 11 "Net-(J1-Pad2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 5.08) (size 2 1.44) (drill 1) (layers *.Cu *.Mask)
      (net 12 "Net-(J1-Pad3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 7.62) (size 2 1.44) (drill 1) (layers *.Cu *.Mask)
      (net 13 "Net-(J1-Pad4)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 10.16) (size 2 1.44) (drill 1) (layers *.Cu *.Mask)
      (net 14 "Net-(J1-Pad5)") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 0 12.7) (size 2 1.44) (drill 1) (layers *.Cu *.Mask)
      (net 15 "Net-(J1-Pad6)") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole oval (at 0 15.24) (size 2 1.44) (drill 1) (layers *.Cu *.Mask)
      (net 16 "Net-(J1-Pad7)") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" thru_hole oval (at 0 17.78) (size 2 1.44) (drill 1) (layers *.Cu *.Mask)
      (net 17 "Net-(J1-Pad8)") (pinfunction "Pin_8") (pintype "passive"))
    (pad "9" thru_hole oval (at 0 20.32) (size 2 1.44) (drill 1) (layers *.Cu *.Mask)
      (net 18 "Net-(J1-Pad9)") (pinfunction "Pin_9") (pintype "passive"))
    (pad "10" thru_hole oval (at 0 22.86) (size 2 1.44) (drill 1) (layers *.Cu *.Mask)
      (net 19 "GND") (pinfunction "Pin_10") (pintype "passive"))
    (pad "11" thru_hole oval (at 7.62 22.86) (size 2 1.44) (drill 1) (layers *.Cu *.Mask)
      (net 20 "Net-(J1-Pad11)") (pinfunction "Pin_11") (pintype "passive"))
    (pad "12" thru_hole oval (at 7.62 20.32) (size 2 1.44) (drill 1) (layers *.Cu *.Mask)
      (net 21 "Net-(J1-Pad12)") (pinfunction "Pin_12") (pintype "passive"))
    (pad "13" thru_hole oval (at 7.62 17.78) (size 2 1.44) (drill 1) (layers *.Cu *.Mask)
      (net 22 "Net-(J1-Pad13)") (pinfunction "Pin_13") (pintype "passive"))
    (pad "14" thru_hole oval (at 7.62 15.24) (size 2 1.44) (drill 1) (layers *.Cu *.Mask)
      (net 23 "Net-(J1-Pad14)") (pinfunction "Pin_14") (pintype "passive"))
    (pad "15" thru_hole oval (at 7.62 12.7) (size 2 1.44) (drill 1) (layers *.Cu *.Mask)
      (net 24 "Net-(J1-Pad15)") (pinfunction "Pin_15") (pintype "passive"))
    (pad "16" thru_hole oval (at 7.62 10.16) (size 2 1.44) (drill 1) (layers *.Cu *.Mask)
      (net 25 "Net-(J1-Pad16)") (pinfunction "Pin_16") (pintype "passive"))
    (pad "17" thru_hole oval (at 7.62 7.62) (size 2 1.44) (drill 1) (layers *.Cu *.Mask)
      (net 26 "Net-(J1-Pad17)") (pinfunction "Pin_17") (pintype "passive"))
    (pad "18" thru_hole oval (at 7.62 5.08) (size 2 1.44) (drill 1) (layers *.Cu *.Mask)
      (net 27 "Net-(J1-Pad18)") (pinfunction "Pin_18") (pintype "passive"))
    (pad "19" thru_hole oval (at 7.62 2.54) (size 2 1.44) (drill 1) (layers *.Cu *.Mask)
      (net 28 "Net-(J1-Pad19)") (pinfunction "Pin_19") (pintype "passive"))
    (pad "20" thru_hole oval (at 7.62 0) (size 2 1.44) (drill 1) (layers *.Cu *.Mask)
      (net 29 "+5V") (pinfunction "Pin_20") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Socket.3dshapes/DIP_Socket-20_W4.3_W5.08_W7.62_W10.16_W10.9_3M_220-3342-00-0602J.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 33.02 63.5 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "MultiTester.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R5" (at 5.08 -2.37) (layer "F.SilkS"))
    (fp_text value "1K" (at 5.08 2.37) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 5.08 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 45 "Net-(D5-Pad1)") (pintype "passive"))
    (pad "2" thru_hole oval (at 10.16 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 36 "Net-(R5-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 33.02 77.47 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "MultiTester.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R7" (at 5.08 -2.37) (layer "F.SilkS"))
    (fp_text value "1K" (at 5.08 2.37) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 5.08 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 47 "Net-(D7-Pad1)") (pintype "passive"))
    (pad "2" thru_hole oval (at 10.16 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 38 "Net-(R7-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 50.165 77.47)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "MultiTester.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R24" (at 5.08 -2.37) (layer "F.SilkS"))
    (fp_text value "1K" (at 5.08 2.37) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 5.08 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 64 "Net-(D24-Pad1)") (pintype "passive"))
    (pad "2" thru_hole oval (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 86 "Net-(R24-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 50.165 105.41)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "MultiTester.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R20" (at 5.08 -2.37) (layer "F.SilkS"))
    (fp_text value "1K" (at 5.08 2.37) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 5.08 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 60 "Net-(D20-Pad1)") (pintype "passive"))
    (pad "2" thru_hole oval (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 82 "Net-(R20-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Disc_D3.4mm_W2.1mm_P2.50mm" (layer "F.Cu")
    (tedit 5AE50EF0)
    (at 70.465 116.205 180)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.4*2.1mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3.4mm width 2.1mm Capacitor")
    (property "Sheetfile" "MultiTester.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C2" (at 4.933 -0.127) (layer "F.SilkS"))
    (fp_text value "C" (at 1.25 2.3) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.25 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 29 "+5V") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D3.4mm_W2.1mm_P2.50mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 33.02 133.35 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "MultiTester.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R15" (at 5.08 -2.37) (layer "F.SilkS"))
    (fp_text value "1K" (at 5.08 2.37) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 5.08 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 55 "Net-(D15-Pad1)") (pintype "passive"))
    (pad "2" thru_hole oval (at 10.16 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 77 "Net-(R15-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 24.13 28.575)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "H1" (at 5.334 -0.127) (layer "F.SilkS"))
    (fp_text value "MountingHole_3.2mm_M3" (at 3.81 -6.35) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (footprint "LED_THT:LED_D5.0mm" (layer "F.Cu")
    (tedit 5995936A)
    (at 46.365 98.425 180)
    (descr "LED, diameter 5.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LL-504BC2E-009.pdf")
    (tags "LED diameter 5.0mm 2 pins")
    (property "Sheetfile" "MultiTester.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "D21" (at -3.927 2.413) (layer "F.SilkS"))
    (fp_text value "LED" (at 1.27 3.96) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.25 0) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 61 "Net-(D21-Pad1)") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 95 "Net-(D19-Pad2)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_THT.3dshapes/LED_D5.0mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Socket:DIP_Socket-14_W4.3_W5.08_W7.62_W10.16_W10.9_3M_214-3339-00-0602J" (layer "F.Cu")
    (tedit 5AF5D4CC)
    (at 174.7375 38.31)
    (descr "3M 14-pin zero insertion force socket, through-hole, row spacing 7.62 mm (300 mils), http://multimedia.3m.com/mws/media/494546O/3mtm-dip-sockets-100-2-54-mm-ts0365.pdf")
    (tags "THT DIP DIL ZIF 7.62mm 300mil Socket")
    (property "Sheetfile" "MultiTester.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J5" (at 3.81 -11.56) (layer "F.SilkS"))
    (fp_text value "Conn_01x14_Female" (at 3.81 23.44) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 5.94) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 2 1.44) (drill 1) (layers *.Cu *.Mask)
      (net 10 "Net-(J1-Pad1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54) (size 2 1.44) (drill 1) (layers *.Cu *.Mask)
      (net 11 "Net-(J1-Pad2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 5.08) (size 2 1.44) (drill 1) (layers *.Cu *.Mask)
      (net 12 "Net-(J1-Pad3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 7.62) (size 2 1.44) (drill 1) (layers *.Cu *.Mask)
      (net 13 "Net-(J1-Pad4)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 10.16) (size 2 1.44) (drill 1) (layers *.Cu *.Mask)
      (net 14 "Net-(J1-Pad5)") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 0 12.7) (size 2 1.44) (drill 1) (layers *.Cu *.Mask)
      (net 15 "Net-(J1-Pad6)") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole oval (at 0 15.24) (size 2 1.44) (drill 1) (layers *.Cu *.Mask)
      (net 19 "GND") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" thru_hole oval (at 7.62 15.24) (size 2 1.44) (drill 1) (layers *.Cu *.Mask)
      (net 16 "Net-(J1-Pad7)") (pinfunction "Pin_8") (pintype "passive"))
    (pad "9" thru_hole oval (at 7.62 12.7) (size 2 1.44) (drill 1) (layers *.Cu *.Mask)
      (net 17 "Net-(J1-Pad8)") (pinfunction "Pin_9") (pintype "passive"))
    (pad "10" thru_hole oval (at 7.62 10.16) (size 2 1.44) (drill 1) (layers *.Cu *.Mask)
      (net 18 "Net-(J1-Pad9)") (pinfunction "Pin_10") (pintype "passive"))
    (pad "11" thru_hole oval (at 7.62 7.62) (size 2 1.44) (drill 1) (layers *.Cu *.Mask)
      (net 20 "Net-(J1-Pad11)") (pinfunction "Pin_11") (pintype "passive"))
    (pad "12" thru_hole oval (at 7.62 5.08) (size 2 1.44) (drill 1) (layers *.Cu *.Mask)
      (net 21 "Net-(J1-Pad12)") (pinfunction "Pin_12") (pintype "passive"))
    (pad "13" thru_hole oval (at 7.62 2.54) (size 2 1.44) (drill 1) (layers *.Cu *.Mask)
      (net 22 "Net-(J1-Pad13)") (pinfunction "Pin_13") (pintype "passive"))
    (pad "14" thru_hole oval (at 7.62 0) (size 2 1.44) (drill 1) (layers *.Cu *.Mask)
      (net 29 "+5V") (pinfunction "Pin_14") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Socket.3dshapes/DIP_Socket-14_W4.3_W5.08_W7.62_W10.16_W10.9_3M_214-3339-00-0602J.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 33.02 70.485 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "MultiTester.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R6" (at 5.08 -2.37) (layer "F.SilkS"))
    (fp_text value "1K" (at 5.08 2.37) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 5.08 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 46 "Net-(D6-Pad1)") (pintype "passive"))
    (pad "2" thru_hole oval (at 10.16 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 37 "Net-(R6-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Button_Switch_THT:SW_DIP_SPSTx04_Slide_9.78x12.34mm_W7.62mm_P2.54mm" (layer "F.Cu")
    (tedit 5A4E1404)
    (at 140.97 82.55 180)
    (descr "4x-dip-switch SPST , Slide, row spacing 7.62 mm (300 mils), body size 9.78x12.34mm (see e.g. https://www.ctscorp.com/wp-content/uploads/206-208.pdf)")
    (tags "DIP Switch SPST Slide 7.62mm 300mil")
    (property "Sheetfile" "MultiTester.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "SW1" (at 3.81 -3.42) (layer "F.SilkS"))
    (fp_text value "SW_DIP_x04" (at 3.81 11.04) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 7.27 3.81 90) (layer "F.Fab"))
    (fp_text user "on" (at 5.365 -1.4975) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 93 "Net-(D13-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 94 "Net-(D15-Pad2)") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 5.08 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 95 "Net-(D19-Pad2)") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 7.62 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 96 "Net-(D27-Pad2)") (pintype "passive"))
    (pad "5" thru_hole oval (at 7.62 7.62 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 29 "+5V") (pintype "passive"))
    (pad "6" thru_hole oval (at 7.62 5.08 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 29 "+5V") (pintype "passive"))
    (pad "7" thru_hole oval (at 7.62 2.54 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 29 "+5V") (pintype "passive"))
    (pad "8" thru_hole oval (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 29 "+5V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Button_Switch_THT.3dshapes/SW_DIP_SPSTx04_Slide_9.78x12.34mm_W7.62mm_P2.54mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (footprint "Capacitor_THT:C_Disc_D3.4mm_W2.1mm_P2.50mm" (layer "F.Cu")
    (tedit 5AE50EF0)
    (at 70.485 46.36 180)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.4*2.1mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3.4mm width 2.1mm Capacitor")
    (property "Sheetfile" "MultiTester.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C1" (at 4.953 0.132) (layer "F.SilkS"))
    (fp_text value "C" (at 1.25 2.3) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.25 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 29 "+5V") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D3.4mm_W2.1mm_P2.50mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 93.345 138.43)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "A2" (at 0 -4.2) (layer "F.SilkS"))
    (fp_text value "MountingHole_3.2mm_M3" (at 14.605 0) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (footprint "LED_THT:LED_D5.0mm" (layer "F.Cu")
    (tedit 5995936A)
    (at 46.355 49.53 180)
    (descr "LED, diameter 5.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LL-504BC2E-009.pdf")
    (tags "LED diameter 5.0mm 2 pins")
    (property "Sheetfile" "MultiTester.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "D28" (at -3.937 2.286) (layer "F.SilkS"))
    (fp_text value "LED" (at 1.27 3.96) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.25 0) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 68 "Net-(D28-Pad1)") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 96 "Net-(D27-Pad2)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_THT.3dshapes/LED_D5.0mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_THT:LED_D5.0mm" (layer "F.Cu")
    (tedit 5995936A)
    (at 46.365 105.41 180)
    (descr "LED, diameter 5.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LL-504BC2E-009.pdf")
    (tags "LED diameter 5.0mm 2 pins")
    (property "Sheetfile" "MultiTester.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "D20" (at -3.927 2.286) (layer "F.SilkS"))
    (fp_text value "LED" (at 1.27 3.96) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.25 0) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 60 "Net-(D20-Pad1)") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 95 "Net-(D19-Pad2)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_THT.3dshapes/LED_D5.0mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Disc_D3.4mm_W2.1mm_P2.50mm" (layer "F.Cu")
    (tedit 5AE50EF0)
    (at 70.485 69.215 180)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.4*2.1mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3.4mm width 2.1mm Capacitor")
    (property "Sheetfile" "MultiTester.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C5" (at 4.953 0.127) (layer "F.SilkS"))
    (fp_text value "C" (at 1.25 2.3) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.25 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 29 "+5V") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D3.4mm_W2.1mm_P2.50mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 190.5 28.575)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "H2" (at 0 4.953) (layer "F.SilkS"))
    (fp_text value "MountingHole_3.2mm_M3" (at -5.08 -6.35) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 50.165 112.395)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "MultiTester.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R19" (at 5.08 -2.37) (layer "F.SilkS"))
    (fp_text value "1K" (at 5.08 2.37) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 5.08 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 59 "Net-(D19-Pad1)") (pintype "passive"))
    (pad "2" thru_hole oval (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 81 "Net-(R19-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Disc_D3.4mm_W2.1mm_P2.50mm" (layer "F.Cu")
    (tedit 5AE50EF0)
    (at 70.475 139.7 180)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.4*2.1mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3.4mm width 2.1mm Capacitor")
    (property "Sheetfile" "MultiTester.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C3" (at 1.25 -2.3) (layer "F.SilkS"))
    (fp_text value "C" (at 1.25 2.3) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.25 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 29 "+5V") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D3.4mm_W2.1mm_P2.50mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 169.545 90.17)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "A5" (at 0 4.826) (layer "F.SilkS"))
    (fp_text value "MountingHole_3.2mm_M3" (at -0.635 8.255) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 50.165 35.56)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "MultiTester.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R30" (at 5.08 -2.37) (layer "F.SilkS"))
    (fp_text value "1K" (at 5.08 2.37) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 5.08 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 70 "Net-(D30-Pad1)") (pintype "passive"))
    (pad "2" thru_hole oval (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 92 "Net-(R30-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 33.02 84.455 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "MultiTester.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R8" (at 5.08 -2.37) (layer "F.SilkS"))
    (fp_text value "1K" (at 5.08 2.37) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 5.08 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 48 "Net-(D8-Pad1)") (pintype "passive"))
    (pad "2" thru_hole oval (at 10.16 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 39 "Net-(R8-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Socket:DIP_Socket-32_W11.9_W12.7_W15.24_W17.78_W18.5_3M_232-1285-00-0602J" (layer "F.Cu")
    (tedit 5AF5D4CC)
    (at 83.2775 38.8075)
    (descr "3M 32-pin zero insertion force socket, through-hole, row spacing 15.24 mm (600 mils), http://multimedia.3m.com/mws/media/494546O/3mtm-dip-sockets-100-2-54-mm-ts0365.pdf")
    (tags "THT DIP DIL ZIF 15.24mm 600mil Socket")
    (property "Sheetfile" "MultiTester.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J2" (at 7.62 -11.56) (layer "F.SilkS"))
    (fp_text value "Conn_01x32_Female" (at 7.62 45.94) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 7.62 17.19) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 2 1.44) (drill 1) (layers *.Cu *.Mask)
      (net 10 "Net-(J1-Pad1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54) (size 2 1.44) (drill 1) (layers *.Cu *.Mask)
      (net 11 "Net-(J1-Pad2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 5.08) (size 2 1.44) (drill 1) (layers *.Cu *.Mask)
      (net 12 "Net-(J1-Pad3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 7.62) (size 2 1.44) (drill 1) (layers *.Cu *.Mask)
      (net 13 "Net-(J1-Pad4)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 10.16) (size 2 1.44) (drill 1) (layers *.Cu *.Mask)
      (net 14 "Net-(J1-Pad5)") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 0 12.7) (size 2 1.44) (drill 1) (layers *.Cu *.Mask)
      (net 15 "Net-(J1-Pad6)") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole oval (at 0 15.24) (size 2 1.44) (drill 1) (layers *.Cu *.Mask)
      (net 16 "Net-(J1-Pad7)") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" thru_hole oval (at 0 17.78) (size 2 1.44) (drill 1) (layers *.Cu *.Mask)
      (net 17 "Net-(J1-Pad8)") (pinfunction "Pin_8") (pintype "passive"))
    (pad "9" thru_hole oval (at 0 20.32) (size 2 1.44) (drill 1) (layers *.Cu *.Mask)
      (net 18 "Net-(J1-Pad9)") (pinfunction "Pin_9") (pintype "passive"))
    (pad "10" thru_hole oval (at 0 22.86) (size 2 1.44) (drill 1) (layers *.Cu *.Mask)
      (net 20 "Net-(J1-Pad11)") (pinfunction "Pin_10") (pintype "passive"))
    (pad "11" thru_hole oval (at 0 25.4) (size 2 1.44) (drill 1) (layers *.Cu *.Mask)
      (net 21 "Net-(J1-Pad12)") (pinfunction "Pin_11") (pintype "passive"))
    (pad "12" thru_hole oval (at 0 27.94) (size 2 1.44) (drill 1) (layers *.Cu *.Mask)
      (net 22 "Net-(J1-Pad13)") (pinfunction "Pin_12") (pintype "passive"))
    (pad "13" thru_hole oval (at 0 30.48) (size 2 1.44) (drill 1) (layers *.Cu *.Mask)
      (net 23 "Net-(J1-Pad14)") (pinfunction "Pin_13") (pintype "passive"))
    (pad "14" thru_hole oval (at 0 33.02) (size 2 1.44) (drill 1) (layers *.Cu *.Mask)
      (net 24 "Net-(J1-Pad15)") (pinfunction "Pin_14") (pintype "passive"))
    (pad "15" thru_hole oval (at 0 35.56) (size 2 1.44) (drill 1) (layers *.Cu *.Mask)
      (net 25 "Net-(J1-Pad16)") (pinfunction "Pin_15") (pintype "passive"))
    (pad "16" thru_hole oval (at 0 38.1) (size 2 1.44) (drill 1) (layers *.Cu *.Mask)
      (net 19 "GND") (pinfunction "Pin_16") (pintype "passive"))
    (pad "17" thru_hole oval (at 15.24 38.1) (size 2 1.44) (drill 1) (layers *.Cu *.Mask)
      (net 26 "Net-(J1-Pad17)") (pinfunction "Pin_17") (pintype "passive"))
    (pad "18" thru_hole oval (at 15.24 35.56) (size 2 1.44) (drill 1) (layers *.Cu *.Mask)
      (net 27 "Net-(J1-Pad18)") (pinfunction "Pin_18") (pintype "passive"))
    (pad "19" thru_hole oval (at 15.24 33.02) (size 2 1.44) (drill 1) (layers *.Cu *.Mask)
      (net 28 "Net-(J1-Pad19)") (pinfunction "Pin_19") (pintype "passive"))
    (pad "20" thru_hole oval (at 15.24 30.48) (size 2 1.44) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(J2-Pad20)") (pinfunction "Pin_20") (pintype "passive"))
    (pad "21" thru_hole oval (at 15.24 27.94) (size 2 1.44) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(J2-Pad21)") (pinfunction "Pin_21") (pintype "passive"))
    (pad "22" thru_hole oval (at 15.24 25.4) (size 2 1.44) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(J2-Pad22)") (pinfunction "Pin_22") (pintype "passive"))
    (pad "23" thru_hole oval (at 15.24 22.86) (size 2 1.44) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(J2-Pad23)") (pinfunction "Pin_23") (pintype "passive"))
    (pad "24" thru_hole oval (at 15.24 20.32) (size 2 1.44) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(J2-Pad24)") (pinfunction "Pin_24") (pintype "passive"))
    (pad "25" thru_hole oval (at 15.24 17.78) (size 2 1.44) (drill 1) (layers *.Cu *.Mask)
      (net 6 "Net-(J2-Pad25)") (pinfunction "Pin_25") (pintype "passive"))
    (pad "26" thru_hole oval (at 15.24 15.24) (size 2 1.44) (drill 1) (layers *.Cu *.Mask)
      (net 7 "Net-(J2-Pad26)") (pinfunction "Pin_26") (pintype "passive"))
    (pad "27" thru_hole oval (at 15.24 12.7) (size 2 1.44) (drill 1) (layers *.Cu *.Mask)
      (net 8 "Net-(J2-Pad27)") (pinfunction "Pin_27") (pintype "passive"))
    (pad "28" thru_hole oval (at 15.24 10.16) (size 2 1.44) (drill 1) (layers *.Cu *.Mask)
      (net 9 "Net-(J2-Pad28)") (pinfunction "Pin_28") (pintype "passive"))
    (pad "29" thru_hole oval (at 15.24 7.62) (size 2 1.44) (drill 1) (layers *.Cu *.Mask)
      (net 30 "Net-(J2-Pad29)") (pinfunction "Pin_29") (pintype "passive"))
    (pad "30" thru_hole oval (at 15.24 5.08) (size 2 1.44) (drill 1) (layers *.Cu *.Mask)
      (net 31 "Net-(J2-Pad30)") (pinfunction "Pin_30") (pintype "passive"))
    (pad "31" thru_hole oval (at 15.24 2.54) (size 2 1.44) (drill 1) (layers *.Cu *.Mask)
      (net 32 "Net-(J2-Pad31)") (pinfunction "Pin_31") (pintype "passive"))
    (pad "32" thru_hole oval (at 15.24 0) (size 2 1.44) (drill 1) (layers *.Cu *.Mask)
      (net 29 "+5V") (pinfunction "Pin_32") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Socket.3dshapes/DIP_Socket-32_W11.9_W12.7_W15.24_W17.78_W18.5_3M_232-1285-00-0602J.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 33.02 42.545 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "MultiTester.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R2" (at 5.08 -2.37) (layer "F.SilkS"))
    (fp_text value "1K" (at 5.08 2.37) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 5.08 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 42 "Net-(D2-Pad1)") (pintype "passive"))
    (pad "2" thru_hole oval (at 10.16 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 33 "Net-(R2-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 190.5 80.772)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "H3" (at 0 -4.2) (layer "F.SilkS"))
    (fp_text value "MountingHole_3.2mm_M3" (at 6.35 0 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (footprint "LED_THT:LED_D5.0mm" (layer "F.Cu")
    (tedit 5995936A)
    (at 36.683 98.425)
    (descr "LED, diameter 5.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LL-504BC2E-009.pdf")
    (tags "LED diameter 5.0mm 2 pins")
    (property "Sheetfile" "MultiTester.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "D10" (at -3.663 -2.413) (layer "F.SilkS"))
    (fp_text value "LED" (at 1.27 3.96) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.25 0) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 50 "Net-(D10-Pad1)") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 29 "+5V") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_THT.3dshapes/LED_D5.0mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 175.895 138.43)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "A4" (at 0 -4.2) (layer "F.SilkS"))
    (fp_text value "MountingHole_3.2mm_M3" (at -5.715 -6.985) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 50.165 133.35)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "MultiTester.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R16" (at 5.08 -2.37) (layer "F.SilkS"))
    (fp_text value "1K" (at 5.08 2.37) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 5.08 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 56 "Net-(D16-Pad1)") (pintype "passive"))
    (pad "2" thru_hole oval (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 78 "Net-(R16-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_DIP:DIP-14_W7.62mm" (layer "F.Cu")
    (tedit 5A02E8C5)
    (at 65.415 50.795)
    (descr "14-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (property "Sheetfile" "MultiTester.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U5" (at -0.391 -2.33) (layer "F.SilkS"))
    (fp_text value "74LS06" (at 3.81 17.57) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 7.62) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(J2-Pad26)") (pintype "input"))
    (pad "2" thru_hole oval (at 0 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 87 "Net-(R25-Pad2)") (pintype "open_collector"))
    (pad "3" thru_hole oval (at 0 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 "Net-(J2-Pad27)") (pintype "input"))
    (pad "4" thru_hole oval (at 0 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 88 "Net-(R26-Pad2)") (pintype "open_collector"))
    (pad "5" thru_hole oval (at 0 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 "Net-(J2-Pad28)") (pintype "input"))
    (pad "6" thru_hole oval (at 0 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 89 "Net-(R27-Pad2)") (pintype "open_collector"))
    (pad "7" thru_hole oval (at 0 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "8" thru_hole oval (at 7.62 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 90 "Net-(R28-Pad2)") (pintype "open_collector"))
    (pad "9" thru_hole oval (at 7.62 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 30 "Net-(J2-Pad29)") (pintype "input"))
    (pad "10" thru_hole oval (at 7.62 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 91 "Net-(R29-Pad2)") (pintype "open_collector"))
    (pad "11" thru_hole oval (at 7.62 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 31 "Net-(J2-Pad30)") (pintype "input"))
    (pad "12" thru_hole oval (at 7.62 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 92 "Net-(R30-Pad2)") (pintype "open_collector"))
    (pad "13" thru_hole oval (at 7.62 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 32 "Net-(J2-Pad31)") (pintype "input"))
    (pad "14" thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 29 "+5V") (pinfunction "VCC") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-14_W7.62mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 33.02 112.395 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "MultiTester.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R12" (at 5.08 -2.37) (layer "F.SilkS"))
    (fp_text value "1K" (at 5.08 2.37) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 5.08 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 52 "Net-(D12-Pad1)") (pintype "passive"))
    (pad "2" thru_hole oval (at 10.16 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 74 "Net-(R12-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Socket:DIP_Socket-28_W11.9_W12.7_W15.24_W17.78_W18.5_3M_228-1277-00-0602J" (layer "F.Cu")
    (tedit 5AF5D4CC)
    (at 109.855 38.735)
    (descr "3M 28-pin zero insertion force socket, through-hole, row spacing 15.24 mm (600 mils), http://multimedia.3m.com/mws/media/494546O/3mtm-dip-sockets-100-2-54-mm-ts0365.pdf")
    (tags "THT DIP DIL ZIF 15.24mm 600mil Socket")
    (property "Sheetfile" "MultiTester.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J3" (at 7.62 -11.56) (layer "F.SilkS"))
    (fp_text value "Conn_01x28_Female" (at 7.62 40.84) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 7.62 14.64) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 2 1.44) (drill 1) (layers *.Cu *.Mask)
      (net 10 "Net-(J1-Pad1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54) (size 2 1.44) (drill 1) (layers *.Cu *.Mask)
      (net 11 "Net-(J1-Pad2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 5.08) (size 2 1.44) (drill 1) (layers *.Cu *.Mask)
      (net 12 "Net-(J1-Pad3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 7.62) (size 2 1.44) (drill 1) (layers *.Cu *.Mask)
      (net 13 "Net-(J1-Pad4)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 10.16) (size 2 1.44) (drill 1) (layers *.Cu *.Mask)
      (net 14 "Net-(J1-Pad5)") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 0 12.7) (size 2 1.44) (drill 1) (layers *.Cu *.Mask)
      (net 15 "Net-(J1-Pad6)") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole oval (at 0 15.24) (size 2 1.44) (drill 1) (layers *.Cu *.Mask)
      (net 16 "Net-(J1-Pad7)") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" thru_hole oval (at 0 17.78) (size 2 1.44) (drill 1) (layers *.Cu *.Mask)
      (net 17 "Net-(J1-Pad8)") (pinfunction "Pin_8") (pintype "passive"))
    (pad "9" thru_hole oval (at 0 20.32) (size 2 1.44) (drill 1) (layers *.Cu *.Mask)
      (net 18 "Net-(J1-Pad9)") (pinfunction "Pin_9") (pintype "passive"))
    (pad "10" thru_hole oval (at 0 22.86) (size 2 1.44) (drill 1) (layers *.Cu *.Mask)
      (net 20 "Net-(J1-Pad11)") (pinfunction "Pin_10") (pintype "passive"))
    (pad "11" thru_hole oval (at 0 25.4) (size 2 1.44) (drill 1) (layers *.Cu *.Mask)
      (net 21 "Net-(J1-Pad12)") (pinfunction "Pin_11") (pintype "passive"))
    (pad "12" thru_hole oval (at 0 27.94) (size 2 1.44) (drill 1) (layers *.Cu *.Mask)
      (net 22 "Net-(J1-Pad13)") (pinfunction "Pin_12") (pintype "passive"))
    (pad "13" thru_hole oval (at 0 30.48) (size 2 1.44) (drill 1) (layers *.Cu *.Mask)
      (net 23 "Net-(J1-Pad14)") (pinfunction "Pin_13") (pintype "passive"))
    (pad "14" thru_hole oval (at 0 33.02) (size 2 1.44) (drill 1) (layers *.Cu *.Mask)
      (net 19 "GND") (pinfunction "Pin_14") (pintype "passive"))
    (pad "15" thru_hole oval (at 15.24 33.02) (size 2 1.44) (drill 1) (layers *.Cu *.Mask)
      (net 24 "Net-(J1-Pad15)") (pinfunction "Pin_15") (pintype "passive"))
    (pad "16" thru_hole oval (at 15.24 30.48) (size 2 1.44) (drill 1) (layers *.Cu *.Mask)
      (net 25 "Net-(J1-Pad16)") (pinfunction "Pin_16") (pintype "passive"))
    (pad "17" thru_hole oval (at 15.24 27.94) (size 2 1.44) (drill 1) (layers *.Cu *.Mask)
      (net 26 "Net-(J1-Pad17)") (pinfunction "Pin_17") (pintype "passive"))
    (pad "18" thru_hole oval (at 15.24 25.4) (size 2 1.44) (drill 1) (layers *.Cu *.Mask)
      (net 27 "Net-(J1-Pad18)") (pinfunction "Pin_18") (pintype "passive"))
    (pad "19" thru_hole oval (at 15.24 22.86) (size 2 1.44) (drill 1) (layers *.Cu *.Mask)
      (net 28 "Net-(J1-Pad19)") (pinfunction "Pin_19") (pintype "passive"))
    (pad "20" thru_hole oval (at 15.24 20.32) (size 2 1.44) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(J2-Pad20)") (pinfunction "Pin_20") (pintype "passive"))
    (pad "21" thru_hole oval (at 15.24 17.78) (size 2 1.44) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(J2-Pad21)") (pinfunction "Pin_21") (pintype "passive"))
    (pad "22" thru_hole oval (at 15.24 15.24) (size 2 1.44) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(J2-Pad22)") (pinfunction "Pin_22") (pintype "passive"))
    (pad "23" thru_hole oval (at 15.24 12.7) (size 2 1.44) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(J2-Pad23)") (pinfunction "Pin_23") (pintype "passive"))
    (pad "24" thru_hole oval (at 15.24 10.16) (size 2 1.44) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(J2-Pad24)") (pinfunction "Pin_24") (pintype "passive"))
    (pad "25" thru_hole oval (at 15.24 7.62) (size 2 1.44) (drill 1) (layers *.Cu *.Mask)
      (net 6 "Net-(J2-Pad25)") (pinfunction "Pin_25") (pintype "passive"))
    (pad "26" thru_hole oval (at 15.24 5.08) (size 2 1.44) (drill 1) (layers *.Cu *.Mask)
      (net 7 "Net-(J2-Pad26)") (pinfunction "Pin_26") (pintype "passive"))
    (pad "27" thru_hole oval (at 15.24 2.54) (size 2 1.44) (drill 1) (layers *.Cu *.Mask)
      (net 8 "Net-(J2-Pad27)") (pinfunction "Pin_27") (pintype "passive"))
    (pad "28" thru_hole oval (at 15.24 0) (size 2 1.44) (drill 1) (layers *.Cu *.Mask)
      (net 29 "+5V") (pinfunction "Pin_28") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Socket.3dshapes/DIP_Socket-28_W11.9_W12.7_W15.24_W17.78_W18.5_3M_228-1277-00-0602J.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 33.02 56.515 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "MultiTester.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R4" (at 5.08 -2.37) (layer "F.SilkS"))
    (fp_text value "1K" (at 5.08 2.37) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 5.08 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 44 "Net-(D4-Pad1)") (pintype "passive"))
    (pad "2" thru_hole oval (at 10.16 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 35 "Net-(R4-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Disc_D3.4mm_W2.1mm_P2.50mm" (layer "F.Cu")
    (tedit 5AE50EF0)
    (at 110.236 83.546 90)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.4*2.1mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3.4mm width 2.1mm Capacitor")
    (property "Sheetfile" "MultiTester.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C9" (at 1.25 -2.3 90) (layer "F.SilkS"))
    (fp_text value "C" (at 1.25 2.3 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.25 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 29 "+5V") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.5 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D3.4mm_W2.1mm_P2.50mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_THT:LED_D5.0mm" (layer "F.Cu")
    (tedit 5995936A)
    (at 36.698 77.47)
    (descr "LED, diameter 5.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LL-504BC2E-009.pdf")
    (tags "LED diameter 5.0mm 2 pins")
    (property "Sheetfile" "MultiTester.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "D7" (at -3.17 -2.286) (layer "F.SilkS"))
    (fp_text value "LED" (at 1.27 3.96) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.25 0) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 47 "Net-(D7-Pad1)") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 29 "+5V") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_THT.3dshapes/LED_D5.0mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinSocket_2.54mm:PinSocket_2x17_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 5A19A431)
    (at 187.325 94.615)
    (descr "Through hole straight socket strip, 2x17, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 2x17 2.54mm double row")
    (property "Sheetfile" "MultiTester.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J6" (at -1.27 -2.77) (layer "F.SilkS"))
    (fp_text value "Conn_01x34_Female" (at 3.175 23.241 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at -1.27 20.32 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 "+5V") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at -2.54 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 "+5V") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 "Net-(J1-Pad1)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at -2.54 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 "Net-(J1-Pad2)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 "Net-(J1-Pad3)") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at -2.54 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 "Net-(J1-Pad4)") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 "Net-(J1-Pad5)") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" thru_hole oval (at -2.54 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 "Net-(J1-Pad6)") (pinfunction "Pin_8") (pintype "passive"))
    (pad "9" thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 "Net-(J1-Pad7)") (pinfunction "Pin_9") (pintype "passive"))
    (pad "10" thru_hole oval (at -2.54 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 "Net-(J1-Pad8)") (pinfunction "Pin_10") (pintype "passive"))
    (pad "11" thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 "Net-(J1-Pad9)") (pinfunction "Pin_11") (pintype "passive"))
    (pad "12" thru_hole oval (at -2.54 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 "Net-(J1-Pad11)") (pinfunction "Pin_12") (pintype "passive"))
    (pad "13" thru_hole oval (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 "Net-(J1-Pad12)") (pinfunction "Pin_13") (pintype "passive"))
    (pad "14" thru_hole oval (at -2.54 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 "Net-(J1-Pad13)") (pinfunction "Pin_14") (pintype "passive"))
    (pad "15" thru_hole oval (at 0 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 "Net-(J1-Pad14)") (pinfunction "Pin_15") (pintype "passive"))
    (pad "16" thru_hole oval (at -2.54 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 "Net-(J1-Pad15)") (pinfunction "Pin_16") (pintype "passive"))
    (pad "17" thru_hole oval (at 0 20.32) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 "Net-(J1-Pad16)") (pinfunction "Pin_17") (pintype "passive"))
    (pad "18" thru_hole oval (at -2.54 20.32) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 "Net-(J1-Pad17)") (pinfunction "Pin_18") (pintype "passive"))
    (pad "19" thru_hole oval (at 0 22.86) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 "Net-(J1-Pad18)") (pinfunction "Pin_19") (pintype "passive"))
    (pad "20" thru_hole oval (at -2.54 22.86) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 "Net-(J1-Pad19)") (pinfunction "Pin_20") (pintype "passive"))
    (pad "21" thru_hole oval (at 0 25.4) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(J2-Pad20)") (pinfunction "Pin_21") (pintype "passive"))
    (pad "22" thru_hole oval (at -2.54 25.4) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(J2-Pad21)") (pinfunction "Pin_22") (pintype "passive"))
    (pad "23" thru_hole oval (at 0 27.94) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(J2-Pad22)") (pinfunction "Pin_23") (pintype "passive"))
    (pad "24" thru_hole oval (at -2.54 27.94) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(J2-Pad23)") (pinfunction "Pin_24") (pintype "passive"))
    (pad "25" thru_hole oval (at 0 30.48) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(J2-Pad24)") (pinfunction "Pin_25") (pintype "passive"))
    (pad "26" thru_hole oval (at -2.54 30.48) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 "Net-(J2-Pad25)") (pinfunction "Pin_26") (pintype "passive"))
    (pad "27" thru_hole oval (at 0 33.02) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 "Net-(J2-Pad26)") (pinfunction "Pin_27") (pintype "passive"))
    (pad "28" thru_hole oval (at -2.54 33.02) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 "Net-(J2-Pad27)") (pinfunction "Pin_28") (pintype "passive"))
    (pad "29" thru_hole oval (at 0 35.56) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 "Net-(J2-Pad28)") (pinfunction "Pin_29") (pintype "passive"))
    (pad "30" thru_hole oval (at -2.54 35.56) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 "Net-(J2-Pad29)") (pinfunction "Pin_30") (pintype "passive"))
    (pad "31" thru_hole oval (at 0 38.1) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 "Net-(J2-Pad30)") (pinfunction "Pin_31") (pintype "passive"))
    (pad "32" thru_hole oval (at -2.54 38.1) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 "Net-(J2-Pad31)") (pinfunction "Pin_32") (pintype "passive"))
    (pad "33" thru_hole oval (at 0 40.64) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 "GND") (pinfunction "Pin_33") (pintype "passive"))
    (pad "34" thru_hole oval (at -2.54 40.64) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 "GND") (pinfunction "Pin_34") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_2x17_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_THT:LED_D5.0mm" (layer "F.Cu")
    (tedit 5995936A)
    (at 46.355 63.5 180)
    (descr "LED, diameter 5.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LL-504BC2E-009.pdf")
    (tags "LED diameter 5.0mm 2 pins")
    (property "Sheetfile" "MultiTester.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "D26" (at -3.937 2.54) (layer "F.SilkS"))
    (fp_text value "LED" (at 1.27 3.96) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.25 0) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 66 "Net-(D26-Pad1)") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 95 "Net-(D19-Pad2)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_THT.3dshapes/LED_D5.0mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_THT:LED_D5.0mm" (layer "F.Cu")
    (tedit 5995936A)
    (at 46.365 126.365 180)
    (descr "LED, diameter 5.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LL-504BC2E-009.pdf")
    (tags "LED diameter 5.0mm 2 pins")
    (property "Sheetfile" "MultiTester.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "D17" (at -3.927 2.413) (layer "F.SilkS"))
    (fp_text value "LED" (at 1.27 3.96) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.25 0) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 57 "Net-(D17-Pad1)") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 94 "Net-(D15-Pad2)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_THT.3dshapes/LED_D5.0mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_DIP:DIP-14_W7.62mm" (layer "F.Cu")
    (tedit 5A02E8C5)
    (at 65.395 97.785)
    (descr "14-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (property "Sheetfile" "MultiTester.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U2" (at -0.371 -2.33) (layer "F.SilkS"))
    (fp_text value "74LS06" (at 3.81 17.57) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 7.62) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 "Net-(J1-Pad7)") (pintype "input"))
    (pad "2" thru_hole oval (at 0 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 38 "Net-(R7-Pad2)") (pintype "open_collector"))
    (pad "3" thru_hole oval (at 0 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 "Net-(J1-Pad8)") (pintype "input"))
    (pad "4" thru_hole oval (at 0 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 39 "Net-(R8-Pad2)") (pintype "open_collector"))
    (pad "5" thru_hole oval (at 0 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 "Net-(J1-Pad9)") (pintype "input"))
    (pad "6" thru_hole oval (at 0 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 40 "Net-(R9-Pad2)") (pintype "open_collector"))
    (pad "7" thru_hole oval (at 0 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "8" thru_hole oval (at 7.62 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 72 "Net-(R10-Pad2)") (pintype "open_collector"))
    (pad "9" thru_hole oval (at 7.62 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 "Net-(J1-Pad11)") (pintype "input"))
    (pad "10" thru_hole oval (at 7.62 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 73 "Net-(R11-Pad2)") (pintype "open_collector"))
    (pad "11" thru_hole oval (at 7.62 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 21 "Net-(J1-Pad12)") (pintype "input"))
    (pad "12" thru_hole oval (at 7.62 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 74 "Net-(R12-Pad2)") (pintype "open_collector"))
    (pad "13" thru_hole oval (at 7.62 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 22 "Net-(J1-Pad13)") (pintype "input"))
    (pad "14" thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 29 "+5V") (pinfunction "VCC") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-14_W7.62mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_THT:LED_D5.0mm" (layer "F.Cu")
    (tedit 5995936A)
    (at 36.698 126.365)
    (descr "LED, diameter 5.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LL-504BC2E-009.pdf")
    (tags "LED diameter 5.0mm 2 pins")
    (property "Sheetfile" "MultiTester.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "D14" (at -3.678 -2.413) (layer "F.SilkS"))
    (fp_text value "LED" (at 1.27 3.96) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.25 0) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 54 "Net-(D14-Pad1)") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 93 "Net-(D13-Pad2)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_THT.3dshapes/LED_D5.0mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 33.02 105.41 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "MultiTester.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R11" (at 5.08 -2.37) (layer "F.SilkS"))
    (fp_text value "1K" (at 5.08 2.37) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 5.08 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 51 "Net-(D11-Pad1)") (pintype "passive"))
    (pad "2" thru_hole oval (at 10.16 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 73 "Net-(R11-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_THT:LED_D5.0mm" (layer "F.Cu")
    (tedit 5995936A)
    (at 36.698 133.35)
    (descr "LED, diameter 5.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LL-504BC2E-009.pdf")
    (tags "LED diameter 5.0mm 2 pins")
    (property "Sheetfile" "MultiTester.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "D15" (at -3.678 -2.286) (layer "F.SilkS"))
    (fp_text value "LED" (at 1.27 3.96) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.25 0) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 55 "Net-(D15-Pad1)") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 94 "Net-(D15-Pad2)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_THT.3dshapes/LED_D5.0mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 33.02 126.365 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "MultiTester.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R14" (at 5.08 -2.37) (layer "F.SilkS"))
    (fp_text value "1K" (at 5.08 2.37) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 5.08 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 54 "Net-(D14-Pad1)") (pintype "passive"))
    (pad "2" thru_hole oval (at 10.16 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 76 "Net-(R14-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_THT:LED_D5.0mm" (layer "F.Cu")
    (tedit 5995936A)
    (at 36.698 84.455)
    (descr "LED, diameter 5.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LL-504BC2E-009.pdf")
    (tags "LED diameter 5.0mm 2 pins")
    (property "Sheetfile" "MultiTester.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "D8" (at -3.17 -2.159) (layer "F.SilkS"))
    (fp_text value "LED" (at 1.27 3.96) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.25 0) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 48 "Net-(D8-Pad1)") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 29 "+5V") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_THT.3dshapes/LED_D5.0mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_THT:LED_D5.0mm" (layer "F.Cu")
    (tedit 5995936A)
    (at 36.825 35.56)
    (descr "LED, diameter 5.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LL-504BC2E-009.pdf")
    (tags "LED diameter 5.0mm 2 pins")
    (property "Sheetfile" "MultiTester.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "D1" (at -3.297 -2.54) (layer "F.SilkS"))
    (fp_text value "LED" (at 1.27 3.96) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.25 0) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 41 "Net-(D1-Pad1)") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 29 "+5V") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_THT.3dshapes/LED_D5.0mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Disc_D3.4mm_W2.1mm_P2.50mm" (layer "F.Cu")
    (tedit 5AE50EF0)
    (at 77.216 83.546 90)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.4*2.1mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3.4mm width 2.1mm Capacitor")
    (property "Sheetfile" "MultiTester.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C10" (at 1.25 -2.3 90) (layer "F.SilkS"))
    (fp_text value "C" (at 1.25 2.3 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.25 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 29 "+5V") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.5 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D3.4mm_W2.1mm_P2.50mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 94.615 90.17)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "A1" (at -0.127 4.826) (layer "F.SilkS"))
    (fp_text value "MountingHole_3.2mm_M3" (at 0 8.255) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (footprint "LED_THT:LED_D5.0mm" (layer "F.Cu")
    (tedit 5995936A)
    (at 36.688 112.395)
    (descr "LED, diameter 5.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LL-504BC2E-009.pdf")
    (tags "LED diameter 5.0mm 2 pins")
    (property "Sheetfile" "MultiTester.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "D12" (at -3.668 -2.159) (layer "F.SilkS"))
    (fp_text value "LED" (at 1.27 3.96) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.25 0) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 52 "Net-(D12-Pad1)") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 29 "+5V") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_THT.3dshapes/LED_D5.0mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_THT:LED_D5.0mm" (layer "F.Cu")
    (tedit 5995936A)
    (at 46.365 77.47 180)
    (descr "LED, diameter 5.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LL-504BC2E-009.pdf")
    (tags "LED diameter 5.0mm 2 pins")
    (property "Sheetfile" "MultiTester.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "D24" (at -3.927 2.286) (layer "F.SilkS"))
    (fp_text value "LED" (at 1.27 3.96) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.25 0) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 64 "Net-(D24-Pad1)") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 95 "Net-(D19-Pad2)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_THT.3dshapes/LED_D5.0mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_THT:LED_D5.0mm" (layer "F.Cu")
    (tedit 5995936A)
    (at 46.355 42.545 180)
    (descr "LED, diameter 5.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LL-504BC2E-009.pdf")
    (tags "LED diameter 5.0mm 2 pins")
    (property "Sheetfile" "MultiTester.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "D29" (at -3.937 2.413) (layer "F.SilkS"))
    (fp_text value "LED" (at 1.27 3.96) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.25 0) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 69 "Net-(D29-Pad1)") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 96 "Net-(D27-Pad2)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_THT.3dshapes/LED_D5.0mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 50.165 49.53)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "MultiTester.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R28" (at 5.08 -2.37) (layer "F.SilkS"))
    (fp_text value "1K" (at 5.08 2.37) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 5.08 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 68 "Net-(D28-Pad1)") (pintype "passive"))
    (pad "2" thru_hole oval (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 90 "Net-(R28-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_THT:LED_D5.0mm" (layer "F.Cu")
    (tedit 5995936A)
    (at 36.683 105.41)
    (descr "LED, diameter 5.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LL-504BC2E-009.pdf")
    (tags "LED diameter 5.0mm 2 pins")
    (property "Sheetfile" "MultiTester.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "D11" (at -3.663 -2.286) (layer "F.SilkS"))
    (fp_text value "LED" (at 1.27 3.96) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.25 0) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 51 "Net-(D11-Pad1)") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 29 "+5V") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_THT.3dshapes/LED_D5.0mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 33.02 49.53 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "MultiTester.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R3" (at 5.08 -2.37) (layer "F.SilkS"))
    (fp_text value "1K" (at 5.08 2.37) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 5.08 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 43 "Net-(D3-Pad1)") (pintype "passive"))
    (pad "2" thru_hole oval (at 10.16 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 34 "Net-(R3-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Disc_D3.4mm_W2.1mm_P2.50mm" (layer "F.Cu")
    (tedit 5AE50EF0)
    (at 169.672 62.758 -90)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.4*2.1mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3.4mm width 2.1mm Capacitor")
    (property "Sheetfile" "MultiTester.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C7" (at 1.25 -2.3 90) (layer "F.SilkS"))
    (fp_text value "C" (at 1.25 2.3 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.25 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 29 "+5V") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D3.4mm_W2.1mm_P2.50mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 50.165 119.38)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "MultiTester.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R18" (at 5.08 -2.37) (layer "F.SilkS"))
    (fp_text value "1K" (at 5.08 2.37) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 5.08 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 58 "Net-(D18-Pad1)") (pintype "passive"))
    (pad "2" thru_hole oval (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 80 "Net-(R18-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 50.165 63.5)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "MultiTester.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R26" (at 5.08 -2.37) (layer "F.SilkS"))
    (fp_text value "1K" (at 5.08 2.37) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 5.08 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 66 "Net-(D26-Pad1)") (pintype "passive"))
    (pad "2" thru_hole oval (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 88 "Net-(R26-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_THT:LED_D5.0mm" (layer "F.Cu")
    (tedit 5995936A)
    (at 46.36 133.35 180)
    (descr "LED, diameter 5.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LL-504BC2E-009.pdf")
    (tags "LED diameter 5.0mm 2 pins")
    (property "Sheetfile" "MultiTester.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "D16" (at -3.932 2.286) (layer "F.SilkS"))
    (fp_text value "LED" (at 1.27 3.96) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.25 0) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 56 "Net-(D16-Pad1)") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 94 "Net-(D15-Pad2)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_THT.3dshapes/LED_D5.0mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_THT:LED_D5.0mm" (layer "F.Cu")
    (tedit 5995936A)
    (at 36.825 49.53)
    (descr "LED, diameter 5.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LL-504BC2E-009.pdf")
    (tags "LED diameter 5.0mm 2 pins")
    (property "Sheetfile" "MultiTester.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "D3" (at -3.297 -2.286) (layer "F.SilkS"))
    (fp_text value "LED" (at 1.27 3.96) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.25 0) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 43 "Net-(D3-Pad1)") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 29 "+5V") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_THT.3dshapes/LED_D5.0mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_DIP:DIP-14_W7.62mm" (layer "F.Cu")
    (tedit 5A02E8C5)
    (at 65.405 121.285)
    (descr "14-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (property "Sheetfile" "MultiTester.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U3" (at -0.381 -2.413) (layer "F.SilkS"))
    (fp_text value "74LS06" (at 3.81 17.57) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 7.62) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 "Net-(J1-Pad14)") (pintype "input"))
    (pad "2" thru_hole oval (at 0 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 75 "Net-(R13-Pad2)") (pintype "open_collector"))
    (pad "3" thru_hole oval (at 0 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 24 "Net-(J1-Pad15)") (pintype "input"))
    (pad "4" thru_hole oval (at 0 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 76 "Net-(R14-Pad2)") (pintype "open_collector"))
    (pad "5" thru_hole oval (at 0 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 25 "Net-(J1-Pad16)") (pintype "input"))
    (pad "6" thru_hole oval (at 0 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 77 "Net-(R15-Pad2)") (pintype "open_collector"))
    (pad "7" thru_hole oval (at 0 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "8" thru_hole oval (at 7.62 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 78 "Net-(R16-Pad2)") (pintype "open_collector"))
    (pad "9" thru_hole oval (at 7.62 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 26 "Net-(J1-Pad17)") (pintype "input"))
    (pad "10" thru_hole oval (at 7.62 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 79 "Net-(R17-Pad2)") (pintype "open_collector"))
    (pad "11" thru_hole oval (at 7.62 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 27 "Net-(J1-Pad18)") (pintype "input"))
    (pad "12" thru_hole oval (at 7.62 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 80 "Net-(R18-Pad2)") (pintype "open_collector"))
    (pad "13" thru_hole oval (at 7.62 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 28 "Net-(J1-Pad19)") (pintype "input"))
    (pad "14" thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 29 "+5V") (pinfunction "VCC") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-14_W7.62mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 50.165 98.425)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "MultiTester.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R21" (at 5.08 -2.37) (layer "F.SilkS"))
    (fp_text value "1K" (at 5.08 2.37) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 5.08 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 61 "Net-(D21-Pad1)") (pintype "passive"))
    (pad "2" thru_hole oval (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 83 "Net-(R21-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_DIP:DIP-14_W7.62mm" (layer "F.Cu")
    (tedit 5A02E8C5)
    (at 65.405 73.66)
    (descr "14-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (property "Sheetfile" "MultiTester.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U4" (at -0.381 -2.286) (layer "F.SilkS"))
    (fp_text value "74LS06" (at 3.81 17.57) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 7.62) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "Net-(J2-Pad20)") (pintype "input"))
    (pad "2" thru_hole oval (at 0 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 81 "Net-(R19-Pad2)") (pintype "open_collector"))
    (pad "3" thru_hole oval (at 0 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "Net-(J2-Pad21)") (pintype "input"))
    (pad "4" thru_hole oval (at 0 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 82 "Net-(R20-Pad2)") (pintype "open_collector"))
    (pad "5" thru_hole oval (at 0 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(J2-Pad22)") (pintype "input"))
    (pad "6" thru_hole oval (at 0 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 83 "Net-(R21-Pad2)") (pintype "open_collector"))
    (pad "7" thru_hole oval (at 0 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "8" thru_hole oval (at 7.62 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 84 "Net-(R22-Pad2)") (pintype "open_collector"))
    (pad "9" thru_hole oval (at 7.62 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(J2-Pad23)") (pintype "input"))
    (pad "10" thru_hole oval (at 7.62 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 85 "Net-(R23-Pad2)") (pintype "open_collector"))
    (pad "11" thru_hole oval (at 7.62 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(J2-Pad24)") (pintype "input"))
    (pad "12" thru_hole oval (at 7.62 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 86 "Net-(R24-Pad2)") (pintype "open_collector"))
    (pad "13" thru_hole oval (at 7.62 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(J2-Pad25)") (pintype "input"))
    (pad "14" thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 29 "+5V") (pinfunction "VCC") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-14_W7.62mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 33.02 91.44 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "MultiTester.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R9" (at 5.08 -2.37) (layer "F.SilkS"))
    (fp_text value "1K" (at 5.08 2.37) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 5.08 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 49 "Net-(D9-Pad1)") (pintype "passive"))
    (pad "2" thru_hole oval (at 10.16 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 40 "Net-(R9-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Socket:DIP_Socket-16_W4.3_W5.08_W7.62_W10.16_W10.9_3M_216-3340-00-0602J" (layer "F.Cu")
    (tedit 5C461E8A)
    (at 155.6875 38.43)
    (descr "3M 16-pin zero insertion force socket, through-hole, row spacing 7.62 mm (300 mils), http://multimedia.3m.com/mws/media/494546O/3mtm-dip-sockets-100-2-54-mm-ts0365.pdf")
    (tags "THT DIP DIL ZIF 7.62mm 300mil Socket")
    (property "Sheetfile" "MultiTester.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J4" (at 3.81 -11.56) (layer "F.SilkS"))
    (fp_text value "Conn_01x16_Female" (at 3.81 25.74) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 7.09) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 2 1.44) (drill 1) (layers *.Cu *.Mask)
      (net 10 "Net-(J1-Pad1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54) (size 2 1.44) (drill 1) (layers *.Cu *.Mask)
      (net 11 "Net-(J1-Pad2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 5.08) (size 2 1.44) (drill 1) (layers *.Cu *.Mask)
      (net 12 "Net-(J1-Pad3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 7.62) (size 2 1.44) (drill 1) (layers *.Cu *.Mask)
      (net 13 "Net-(J1-Pad4)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 10.16) (size 2 1.44) (drill 1) (layers *.Cu *.Mask)
      (net 14 "Net-(J1-Pad5)") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 0 12.7) (size 2 1.44) (drill 1) (layers *.Cu *.Mask)
      (net 15 "Net-(J1-Pad6)") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole oval (at 0 15.24) (size 2 1.44) (drill 1) (layers *.Cu *.Mask)
      (net 16 "Net-(J1-Pad7)") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" thru_hole oval (at 0 17.78) (size 2 1.44) (drill 1) (layers *.Cu *.Mask)
      (net 19 "GND") (pinfunction "Pin_8") (pintype "passive"))
    (pad "9" thru_hole oval (at 7.62 17.78) (size 2 1.44) (drill 1) (layers *.Cu *.Mask)
      (net 17 "Net-(J1-Pad8)") (pinfunction "Pin_9") (pintype "passive"))
    (pad "10" thru_hole oval (at 7.62 15.24) (size 2 1.44) (drill 1) (layers *.Cu *.Mask)
      (net 18 "Net-(J1-Pad9)") (pinfunction "Pin_10") (pintype "passive"))
    (pad "11" thru_hole oval (at 7.62 12.7) (size 2 1.44) (drill 1) (layers *.Cu *.Mask)
      (net 20 "Net-(J1-Pad11)") (pinfunction "Pin_11") (pintype "passive"))
    (pad "12" thru_hole oval (at 7.62 10.16) (size 2 1.44) (drill 1) (layers *.Cu *.Mask)
      (net 21 "Net-(J1-Pad12)") (pinfunction "Pin_12") (pintype "passive"))
    (pad "13" thru_hole oval (at 7.62 7.62) (size 2 1.44) (drill 1) (layers *.Cu *.Mask)
      (net 22 "Net-(J1-Pad13)") (pinfunction "Pin_13") (pintype "passive"))
    (pad "14" thru_hole oval (at 7.62 5.08) (size 2 1.44) (drill 1) (layers *.Cu *.Mask)
      (net 23 "Net-(J1-Pad14)") (pinfunction "Pin_14") (pintype "passive"))
    (pad "15" thru_hole oval (at 7.62 2.54) (size 2 1.44) (drill 1) (layers *.Cu *.Mask)
      (net 24 "Net-(J1-Pad15)") (pinfunction "Pin_15") (pintype "passive"))
    (pad "16" thru_hole oval (at 7.62 0) (size 2 1.44) (drill 1) (layers *.Cu *.Mask)
      (net 29 "+5V") (pinfunction "Pin_16") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Socket.3dshapes/DIP_Socket-16_W4.3_W5.08_W7.62_W10.16_W10.9_3M_216-3340-00-0602J.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_THT:LED_D5.0mm" (layer "F.Cu")
    (tedit 5995936A)
    (at 36.698 70.485)
    (descr "LED, diameter 5.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LL-504BC2E-009.pdf")
    (tags "LED diameter 5.0mm 2 pins")
    (property "Sheetfile" "MultiTester.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "D6" (at -3.17 -2.413) (layer "F.SilkS"))
    (fp_text value "LED" (at 1.27 3.96) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.25 0) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 46 "Net-(D6-Pad1)") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 29 "+5V") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_THT.3dshapes/LED_D5.0mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_THT:LED_D5.0mm" (layer "F.Cu")
    (tedit 5995936A)
    (at 46.36 70.485 180)
    (descr "LED, diameter 5.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LL-504BC2E-009.pdf")
    (tags "LED diameter 5.0mm 2 pins")
    (property "Sheetfile" "MultiTester.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "D25" (at -3.932 2.413) (layer "F.SilkS"))
    (fp_text value "LED" (at 1.27 3.96) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.25 0) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 65 "Net-(D25-Pad1)") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 95 "Net-(D19-Pad2)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_THT.3dshapes/LED_D5.0mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Disc_D3.4mm_W2.1mm_P2.50mm" (layer "F.Cu")
    (tedit 5AE50EF0)
    (at 182.88 62.992 -90)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.4*2.1mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3.4mm width 2.1mm Capacitor")
    (property "Sheetfile" "MultiTester.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C6" (at 1.25 -2.3 90) (layer "F.SilkS"))
    (fp_text value "C" (at 1.25 2.3 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.25 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 29 "+5V") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D3.4mm_W2.1mm_P2.50mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_THT:LED_D5.0mm" (layer "F.Cu")
    (tedit 5995936A)
    (at 46.355 56.515 180)
    (descr "LED, diameter 5.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LL-504BC2E-009.pdf")
    (tags "LED diameter 5.0mm 2 pins")
    (property "Sheetfile" "MultiTester.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "D27" (at -3.429 2.159) (layer "F.SilkS"))
    (fp_text value "LED" (at 1.27 3.96) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.25 0) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 67 "Net-(D27-Pad1)") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 96 "Net-(D27-Pad2)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_THT.3dshapes/LED_D5.0mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 33.02 35.56 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "MultiTester.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R1" (at 5.08 -2.37) (layer "F.SilkS"))
    (fp_text value "1K" (at 5.08 2.37) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 5.08 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 41 "Net-(D1-Pad1)") (pintype "passive"))
    (pad "2" thru_hole oval (at 10.16 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 71 "Net-(R1-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Disc_D3.4mm_W2.1mm_P2.50mm" (layer "F.Cu")
    (tedit 5AE50EF0)
    (at 150.368 70.846 90)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.4*2.1mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3.4mm width 2.1mm Capacitor")
    (property "Sheetfile" "MultiTester.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C8" (at 1.25 -2.3 90) (layer "F.SilkS"))
    (fp_text value "C" (at 1.25 2.3 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.25 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 29 "+5V") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.5 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D3.4mm_W2.1mm_P2.50mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_THT:LED_D5.0mm" (layer "F.Cu")
    (tedit 5995936A)
    (at 46.36 119.38 180)
    (descr "LED, diameter 5.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LL-504BC2E-009.pdf")
    (tags "LED diameter 5.0mm 2 pins")
    (property "Sheetfile" "MultiTester.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "D18" (at -3.932 2.54) (layer "F.SilkS"))
    (fp_text value "LED" (at 1.27 3.96) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.25 0) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 58 "Net-(D18-Pad1)") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 94 "Net-(D15-Pad2)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_THT.3dshapes/LED_D5.0mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_THT:LED_D5.0mm" (layer "F.Cu")
    (tedit 5995936A)
    (at 36.698 63.5)
    (descr "LED, diameter 5.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LL-504BC2E-009.pdf")
    (tags "LED diameter 5.0mm 2 pins")
    (property "Sheetfile" "MultiTester.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "D5" (at -3.17 -2.54) (layer "F.SilkS"))
    (fp_text value "LED" (at 1.27 3.96) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.25 0) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 45 "Net-(D5-Pad1)") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 29 "+5V") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_THT.3dshapes/LED_D5.0mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 50.165 70.485)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "MultiTester.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R25" (at 5.08 -2.37) (layer "F.SilkS"))
    (fp_text value "1K" (at 5.08 2.37) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 5.08 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 65 "Net-(D25-Pad1)") (pintype "passive"))
    (pad "2" thru_hole oval (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 87 "Net-(R25-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_THT:LED_D5.0mm" (layer "F.Cu")
    (tedit 5995936A)
    (at 36.825 42.545)
    (descr "LED, diameter 5.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LL-504BC2E-009.pdf")
    (tags "LED diameter 5.0mm 2 pins")
    (property "Sheetfile" "MultiTester.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "D2" (at -3.297 -2.413) (layer "F.SilkS"))
    (fp_text value "LED" (at 1.27 3.96) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.25 0) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 42 "Net-(D2-Pad1)") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 29 "+5V") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_THT.3dshapes/LED_D5.0mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 50.165 84.455)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "MultiTester.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R23" (at 5.08 -2.37) (layer "F.SilkS"))
    (fp_text value "1K" (at 5.08 2.37) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 5.08 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 63 "Net-(D23-Pad1)") (pintype "passive"))
    (pad "2" thru_hole oval (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 85 "Net-(R23-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 23.876 141.224)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "H5" (at 5.08 0) (layer "F.SilkS"))
    (fp_text value "MountingHole_3.2mm_M3" (at 3.81 5.715) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (footprint "LED_THT:LED_D5.0mm" (layer "F.Cu")
    (tedit 5995936A)
    (at 36.825 56.515)
    (descr "LED, diameter 5.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LL-504BC2E-009.pdf")
    (tags "LED diameter 5.0mm 2 pins")
    (property "Sheetfile" "MultiTester.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "D4" (at -3.297 -2.159) (layer "F.SilkS"))
    (fp_text value "LED" (at 1.27 3.96) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.25 0) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 44 "Net-(D4-Pad1)") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 29 "+5V") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_THT.3dshapes/LED_D5.0mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 190.5 141.224)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "H4" (at -4.572 0) (layer "F.SilkS"))
    (fp_text value "MountingHole_3.2mm_M3" (at -4.064 6.096) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 50.165 56.515)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "MultiTester.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R27" (at 5.08 -2.37) (layer "F.SilkS"))
    (fp_text value "1K" (at 5.08 2.37) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 5.08 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 67 "Net-(D27-Pad1)") (pintype "passive"))
    (pad "2" thru_hole oval (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 89 "Net-(R27-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_THT:LED_D5.0mm" (layer "F.Cu")
    (tedit 5995936A)
    (at 36.698 91.44)
    (descr "LED, diameter 5.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LL-504BC2E-009.pdf")
    (tags "LED diameter 5.0mm 2 pins")
    (property "Sheetfile" "MultiTester.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "D9" (at -3.17 -2.54) (layer "F.SilkS"))
    (fp_text value "LED" (at 1.128 3.96) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.25 0) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 49 "Net-(D9-Pad1)") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 29 "+5V") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_THT.3dshapes/LED_D5.0mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 50.165 42.545)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "MultiTester.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R29" (at 5.08 -2.37) (layer "F.SilkS"))
    (fp_text value "1K" (at 5.08 2.37) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 5.08 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 69 "Net-(D29-Pad1)") (pintype "passive"))
    (pad "2" thru_hole oval (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 91 "Net-(R29-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 145.415 133.35)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "A3" (at 0 -4.2) (layer "F.SilkS"))
    (fp_text value "MountingHole_3.2mm_M3" (at 0 4.2) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (footprint "LED_THT:LED_D5.0mm" (layer "F.Cu")
    (tedit 5995936A)
    (at 46.36 84.455 180)
    (descr "LED, diameter 5.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LL-504BC2E-009.pdf")
    (tags "LED diameter 5.0mm 2 pins")
    (property "Sheetfile" "MultiTester.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "D23" (at -3.932 2.159) (layer "F.SilkS"))
    (fp_text value "LED" (at 1.27 3.96) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.25 0) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 63 "Net-(D23-Pad1)") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 95 "Net-(D19-Pad2)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_THT.3dshapes/LED_D5.0mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 195.58 145.796) (end 192.532 145.796) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 18.796 145.796) (end 18.796 23.368) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 195.58 23.368) (end 19.304 23.368) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 18.796 145.796) (end 192.532 145.796) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 195.58 23.368) (end 195.58 145.796) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 18.796 23.368) (end 19.304 23.368) (layer "Edge.Cuts") (width 0.1))
  (gr_text "Chip Tester - 14 to 32 pin DIP" (at 170.18 78.232) (layer "F.SilkS"))
  (gr_text "20 pin and up" (at 148.844 80.264) (layer "F.SilkS"))
  (gr_text "74LS06" (at 71.628 25.4) (layer "F.SilkS"))
  (gr_text "74LS06" (at 71.12 118.872) (layer "F.SilkS"))
  (gr_text "Arduino ATMEGA" (at 150.876 88.9) (layer "F.SilkS"))
  (gr_text "16 pin and up" (at 148.844 82.804) (layer "F.SilkS"))
  (gr_text "74LS06" (at 71.628 95.504) (layer "F.SilkS"))
  (gr_text "24 pin and up" (at 148.844 77.724) (layer "F.SilkS"))
  (gr_text "74LS06" (at 71.374 48.514) (layer "F.SilkS"))
  (gr_text "74LS06" (at 71.628 71.374) (layer "F.SilkS"))
  (gr_text "32 pin" (at 145.796 75.184) (layer "F.SilkS"))
  (dimension (type aligned) (layer "User.1")
    (pts (xy 165.735 86.36) (xy 165.735 88.9))
    (height -3.81)
    (gr_text "2.5400 mm" (at 168.395 87.63 90) (layer "User.1"))
    (format (units 3) (units_format 1) (precision 4))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (dimension (type aligned) (layer "User.1")
    (pts (xy 71.755 126.365) (xy 168.275 126.365))
    (height -5.08)
    (gr_text "96.5200 mm" (at 120.015 120.135) (layer "User.1"))
    (format (units 3) (units_format 1) (precision 4))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (dimension (type aligned) (layer "User.1")
    (pts (xy 71.755 139.7) (xy 71.755 86.36))
    (height -3.81)
    (gr_text "53.3400 mm" (at 66.795 113.03 90) (layer "User.1"))
    (format (units 3) (units_format 1) (precision 4))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (dimension (type aligned) (layer "User.1")
    (pts (xy 88.265 86.36) (xy 88.265 88.9))
    (height -3.81)
    (gr_text "2.5400 mm" (at 90.925 87.63 90) (layer "User.1"))
    (format (units 3) (units_format 1) (precision 4))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (dimension (type aligned) (layer "User.1")
    (pts (xy 173.355 139.7) (xy 71.755 139.7))
    (height -6.35)
    (gr_text "101.6000 mm" (at 122.555 144.9) (layer "User.1"))
    (format (units 3) (units_format 1) (precision 4))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (dimension (type aligned) (layer "User.1")
    (pts (xy 83.185 139.7) (xy 83.185 137.16))
    (height -3.81)
    (gr_text "2.5400 mm" (at 78.225 138.43 90) (layer "User.1"))
    (format (units 3) (units_format 1) (precision 4))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (dimension (type aligned) (layer "User.1")
    (pts (xy 71.755 102.87) (xy 161.925 102.87))
    (height 3.81)
    (gr_text "90.1700 mm" (at 116.84 105.53) (layer "User.1"))
    (format (units 3) (units_format 1) (precision 4))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (dimension (type aligned) (layer "User.1")
    (pts (xy 145.415 139.7) (xy 145.415 132.08))
    (height 3.81)
    (gr_text "7.6200 mm" (at 148.075 135.89 90) (layer "User.1"))
    (format (units 3) (units_format 1) (precision 4))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (dimension (type aligned) (layer "User.1")
    (pts (xy 71.755 90.17) (xy 86.995 90.17))
    (height 3.81)
    (gr_text "15.2400 mm" (at 79.375 92.83) (layer "User.1"))
    (format (units 3) (units_format 1) (precision 4))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (dimension (type aligned) (layer "User.1")
    (pts (xy 173.355 137.16) (xy 173.355 139.7))
    (height -3.81)
    (gr_text "2.5400 mm" (at 176.015 138.43 90) (layer "User.1"))
    (format (units 3) (units_format 1) (precision 4))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (dimension (type aligned) (layer "User.1")
    (pts (xy 71.755 133.985) (xy 85.725 133.985))
    (height -3.81)
    (gr_text "13.9700 mm" (at 78.74 129.025) (layer "User.1"))
    (format (units 3) (units_format 1) (precision 4))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (dimension (type aligned) (layer "User.1")
    (pts (xy 71.755 127) (xy 137.795 127))
    (height -1.905)
    (gr_text "66.0400 mm" (at 104.775 123.945) (layer "User.1"))
    (format (units 3) (units_format 1) (precision 4))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
)
