(kicad_pcb (version 20211014) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010f8_ffffffff)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference false)
      (plotvalue false)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "Gerbers/")
    )
  )
  (net 0 "")
  (net 1 "VCC")
  (net 2 "GND")
  (net 3 "/MA1")
  (net 4 "/MA2")
  (net 5 "/MA3")
  (net 6 "/MA4")
  (net 7 "/RST")
  (net 8 "/StpA")
  (net 9 "/DirA")
  (net 10 "/StpB")
  (net 11 "/DirB")
  (net 12 "/MB1")
  (net 13 "/MB2")
  (net 14 "/MB3")
  (net 15 "/MB4")
  (net 16 "/MC1")
  (net 17 "/MC2")
  (net 18 "/MC3")
  (net 19 "/MC4")
  (net 20 "/StpC")
  (net 21 "/DirC")
  (net 22 "/StpD")
  (net 23 "/DirD")
  (net 24 "/MD1")
  (net 25 "/MD2")
  (net 26 "/MD3")
  (net 27 "/MD4")
  (footprint "SpeedFootprints:R_0603_1608MetricSQ" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 127.77 69.12)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "SpeedoDrive.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R5" (at -0.08 0.05 180) (layer "F.CrtYd"))
    (fp_text value "10K" (at 0 1.43 180) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 180) (layer "F.Fab"))
    (pad "" smd rect (at -0.825 0) (size 0.8 0.95) (layers "F.Paste"))
    (pad "" smd rect (at 0.825 0) (size 0.8 0.95) (layers "F.Paste"))
    (pad "1" smd roundrect (at -0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (net 10 "/StpB") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "SpeedFootprints:C_0805_2012MetricSQ" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 119.21 65.14 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "SpeedoDrive.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C1" (at 0.05 -0.04 90) (layer "F.CrtYd"))
    (fp_text value "6.8uF" (at 0 1.68 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "" smd rect (at 0.95 0 90) (size 1 1.45) (layers "F.Paste"))
    (pad "" smd rect (at -0.95 0 90) (size 1 1.45) (layers "F.Paste"))
    (pad "1" smd roundrect (at -0.95 0 90) (size 1 1.45) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "VCC") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 90) (size 1 1.45) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "SpeedFootprints:C_0805_2012MetricSQ" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 135.83 91.21 -90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "SpeedoDrive.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C2" (at 0.05 -0.04 -90) (layer "F.CrtYd"))
    (fp_text value "4.7uF" (at 0 1.68 -90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 -90) (layer "F.Fab"))
    (pad "" smd rect (at -0.95 0 270) (size 1 1.45) (layers "F.Paste"))
    (pad "" smd rect (at 0.95 0 270) (size 1 1.45) (layers "F.Paste"))
    (pad "1" smd roundrect (at -0.95 0 270) (size 1 1.45) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "VCC") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 270) (size 1 1.45) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "SpeedFootprints:R_0603_1608MetricSQ" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 135.45 65.43 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "SpeedoDrive.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R1" (at -0.08 0.01 90) (layer "F.CrtYd"))
    (fp_text value "10K" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "" smd rect (at -0.825 0 270) (size 0.8 0.95) (layers "F.Paste"))
    (pad "" smd rect (at 0.825 0 270) (size 0.8 0.95) (layers "F.Paste"))
    (pad "1" smd roundrect (at -0.825 0 270) (size 0.8 0.95) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 270) (size 0.8 0.95) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (net 7 "/RST") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "SpeedFootprints:C_0603_1608MetricSQ" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 121.63 68.81 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "SpeedoDrive.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C3" (at -0.06 -0.04) (layer "F.CrtYd"))
    (fp_text value "100nF" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" smd rect (at 0.775 0 180) (size 0.9 0.95) (layers "F.Paste"))
    (pad "" smd rect (at -0.775 0 180) (size 0.9 0.95) (layers "F.Paste"))
    (pad "1" smd roundrect (at -0.775 0 180) (size 0.9 0.95) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "VCC") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0 180) (size 0.9 0.95) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "SpeedFootprints:C_0805_2012MetricSQ" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 119.01 68.59 -90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "SpeedoDrive.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C5" (at 0.08 0 -90) (layer "F.CrtYd"))
    (fp_text value "4.7uF" (at 0 1.68 -90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 -90) (layer "F.Fab"))
    (pad "" smd rect (at -0.95 0 270) (size 1 1.45) (layers "F.Paste"))
    (pad "" smd rect (at 0.95 0 270) (size 1 1.45) (layers "F.Paste"))
    (pad "1" smd roundrect (at -0.95 0 270) (size 1 1.45) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "VCC") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 270) (size 1 1.45) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x05_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 59FED5CC)
    (at 132.63 65.18 -90)
    (descr "Through hole straight pin header, 1x05, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x05 2.54mm single row")
    (property "Sheetfile" "SpeedoDrive.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J1" (at -0.44 3.88 180) (layer "F.CrtYd"))
    (fp_text value "Conn_01x05" (at 0 12.49 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 5.08) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 "/RST") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 "/StpA") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 "/DirA") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 "/StpB") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 "/DirB") (pinfunction "Pin_5") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x05_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "SpeedFootprints:R_0603_1608MetricSQ" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 130.88 69.12 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "SpeedoDrive.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R2" (at -0.04 0.07) (layer "F.CrtYd"))
    (fp_text value "10K" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" smd rect (at -0.825 0 180) (size 0.8 0.95) (layers "F.Paste"))
    (pad "" smd rect (at 0.825 0 180) (size 0.8 0.95) (layers "F.Paste"))
    (pad "1" smd roundrect (at -0.825 0 180) (size 0.8 0.95) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (net 9 "/DirA") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 180) (size 0.8 0.95) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "SpeedFootprints:R_0603_1608MetricSQ" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 130.8 90.8 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "SpeedoDrive.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R8" (at -0.03 -0.02 90) (layer "F.CrtYd"))
    (fp_text value "10K" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "" smd rect (at -0.825 0 270) (size 0.8 0.95) (layers "F.Paste"))
    (pad "" smd rect (at 0.825 0 270) (size 0.8 0.95) (layers "F.Paste"))
    (pad "1" smd roundrect (at -0.825 0 270) (size 0.8 0.95) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (net 23 "/DirD") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 270) (size 0.8 0.95) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_SO:SOIC-28W_7.5x17.9mm_P1.27mm" (layer "F.Cu")
    (tedit 5D9F72B1)
    (at 128.425 79.62)
    (descr "SOIC, 28 Pin (JEDEC MS-013AE, https://www.analog.com/media/en/package-pcb-resources/package/35833120341221rw_28.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (property "Sheetfile" "SpeedoDrive.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U1" (at -0.115 -6.48) (layer "F.CrtYd"))
    (fp_text value "VID6606" (at 0 9.9) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" smd rect (at -4.65 -6.985) (size 2.05 0.6) (layers "F.Paste"))
    (pad "" smd rect (at -4.65 -4.445) (size 2.05 0.6) (layers "F.Paste"))
    (pad "" smd rect (at -4.65 -5.715) (size 2.05 0.6) (layers "F.Paste"))
    (pad "" smd rect (at -4.65 -8.255) (size 2.05 0.6) (layers "F.Paste"))
    (pad "1" smd roundrect (at -4.65 -8.255) (size 2.05 0.6) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "VCC") (pinfunction "Vcc") (pintype "power_in"))
    (pad "2" smd roundrect (at -4.65 -6.985) (size 2.05 0.6) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (net 11 "/DirB") (pinfunction "Dir_B") (pintype "input"))
    (pad "3" smd roundrect (at -4.65 -5.715) (size 2.05 0.6) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (net 10 "/StpB") (pinfunction "Step_B") (pintype "input"))
    (pad "4" smd roundrect (at -4.65 -4.445) (size 2.05 0.6) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "/MA3") (pinfunction "Mot_A3") (pintype "output"))
    (pad "5" smd rect (at -4.65 -3.175) (size 2.05 0.6) (layers "F.Paste")
      (pintype "output"))
    (pad "5" smd roundrect (at -4.65 -3.175) (size 2.05 0.6) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (net 6 "/MA4") (pinfunction "Mot_A4") (pintype "output"))
    (pad "6" smd roundrect (at -4.65 -1.905) (size 2.05 0.6) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "/MA2") (pinfunction "Mot_A2") (pintype "output"))
    (pad "6" smd rect (at -4.65 -1.905) (size 2.05 0.6) (layers "F.Paste")
      (pintype "output"))
    (pad "7" smd rect (at -4.65 -0.635) (size 2.05 0.6) (layers "F.Paste")
      (pintype "output"))
    (pad "7" smd roundrect (at -4.65 -0.635) (size 2.05 0.6) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "/MA1") (pinfunction "Mot_A1") (pintype "output"))
    (pad "8" smd rect (at -4.65 0.635) (size 2.05 0.6) (layers "F.Paste")
      (pintype "output"))
    (pad "8" smd roundrect (at -4.65 0.635) (size 2.05 0.6) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (net 24 "/MD1") (pinfunction "Mot_D1") (pintype "output"))
    (pad "9" smd roundrect (at -4.65 1.905) (size 2.05 0.6) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (net 25 "/MD2") (pinfunction "Mot_D2") (pintype "output"))
    (pad "9" smd rect (at -4.65 1.905) (size 2.05 0.6) (layers "F.Paste")
      (pintype "output"))
    (pad "10" smd rect (at -4.65 3.175) (size 2.05 0.6) (layers "F.Paste")
      (pintype "output"))
    (pad "10" smd roundrect (at -4.65 3.175) (size 2.05 0.6) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (net 27 "/MD4") (pinfunction "Mot_D4") (pintype "output"))
    (pad "11" smd rect (at -4.65 4.445) (size 2.05 0.6) (layers "F.Paste")
      (pintype "output"))
    (pad "11" smd roundrect (at -4.65 4.445) (size 2.05 0.6) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (net 26 "/MD3") (pinfunction "Mot_D3") (pintype "output"))
    (pad "12" smd roundrect (at -4.65 5.715) (size 2.05 0.6) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "Vss") (pintype "power_in"))
    (pad "12" smd rect (at -4.65 5.715) (size 2.05 0.6) (layers "F.Paste")
      (pintype "power_in"))
    (pad "13" smd roundrect (at -4.65 6.985) (size 2.05 0.6) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (net 21 "/DirC") (pinfunction "Dir_C") (pintype "input"))
    (pad "13" smd rect (at -4.65 6.985) (size 2.05 0.6) (layers "F.Paste")
      (pintype "input"))
    (pad "14" smd rect (at -4.65 8.255) (size 2.05 0.6) (layers "F.Paste")
      (pintype "input"))
    (pad "14" smd roundrect (at -4.65 8.255) (size 2.05 0.6) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (net 20 "/StpC") (pinfunction "Step_C") (pintype "input"))
    (pad "15" smd roundrect (at 4.65 8.255) (size 2.05 0.6) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "VCC") (pinfunction "Vcc") (pintype "power_in"))
    (pad "15" smd rect (at 4.65 8.255) (size 2.05 0.6) (layers "F.Paste")
      (pintype "power_in"))
    (pad "16" smd rect (at 4.65 6.985) (size 2.05 0.6) (layers "F.Paste")
      (pintype "input"))
    (pad "16" smd roundrect (at 4.65 6.985) (size 2.05 0.6) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (net 23 "/DirD") (pinfunction "Dir_D") (pintype "input"))
    (pad "17" smd roundrect (at 4.65 5.715) (size 2.05 0.6) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "/StpD") (pinfunction "Step_D") (pintype "input"))
    (pad "17" smd rect (at 4.65 5.715) (size 2.05 0.6) (layers "F.Paste")
      (pintype "input"))
    (pad "18" smd rect (at 4.65 4.445) (size 2.05 0.6) (layers "F.Paste")
      (pintype "output"))
    (pad "18" smd roundrect (at 4.65 4.445) (size 2.05 0.6) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (net 18 "/MC3") (pinfunction "Mot_C3") (pintype "output"))
    (pad "19" smd roundrect (at 4.65 3.175) (size 2.05 0.6) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (net 19 "/MC4") (pinfunction "Mot_C4") (pintype "output"))
    (pad "19" smd rect (at 4.65 3.175) (size 2.05 0.6) (layers "F.Paste")
      (pintype "output"))
    (pad "20" smd rect (at 4.65 1.905) (size 2.05 0.6) (layers "F.Paste")
      (pintype "output"))
    (pad "20" smd roundrect (at 4.65 1.905) (size 2.05 0.6) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (net 17 "/MC2") (pinfunction "Mot_C2") (pintype "output"))
    (pad "21" smd rect (at 4.65 0.635) (size 2.05 0.6) (layers "F.Paste")
      (pintype "output"))
    (pad "21" smd roundrect (at 4.65 0.635) (size 2.05 0.6) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (net 16 "/MC1") (pinfunction "Mot_C1") (pintype "output"))
    (pad "22" smd roundrect (at 4.65 -0.635) (size 2.05 0.6) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (net 12 "/MB1") (pinfunction "Mot_B1") (pintype "output"))
    (pad "22" smd rect (at 4.65 -0.635) (size 2.05 0.6) (layers "F.Paste")
      (pintype "output"))
    (pad "23" smd roundrect (at 4.65 -1.905) (size 2.05 0.6) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (net 13 "/MB2") (pinfunction "Mot_B2") (pintype "output"))
    (pad "23" smd rect (at 4.65 -1.905) (size 2.05 0.6) (layers "F.Paste")
      (pintype "output"))
    (pad "24" smd roundrect (at 4.65 -3.175) (size 2.05 0.6) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (net 15 "/MB4") (pinfunction "Mot_B4") (pintype "output"))
    (pad "24" smd rect (at 4.65 -3.175) (size 2.05 0.6) (layers "F.Paste")
      (pintype "output"))
    (pad "25" smd roundrect (at 4.65 -4.445) (size 2.05 0.6) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (net 14 "/MB3") (pinfunction "Mot_B3") (pintype "output"))
    (pad "25" smd rect (at 4.65 -4.445) (size 2.05 0.6) (layers "F.Paste")
      (pintype "output"))
    (pad "26" smd rect (at 4.65 -5.715) (size 2.05 0.6) (layers "F.Paste")
      (pintype "input"))
    (pad "26" smd roundrect (at 4.65 -5.715) (size 2.05 0.6) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (net 7 "/RST") (pinfunction "Reset") (pintype "input"))
    (pad "27" smd roundrect (at 4.65 -6.985) (size 2.05 0.6) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (net 9 "/DirA") (pinfunction "Dir_A") (pintype "input"))
    (pad "27" smd rect (at 4.65 -6.985) (size 2.05 0.6) (layers "F.Paste")
      (pintype "input"))
    (pad "28" smd roundrect (at 4.65 -8.255) (size 2.05 0.6) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (net 8 "/StpA") (pinfunction "Step_A") (pintype "input"))
    (pad "28" smd rect (at 4.65 -8.255) (size 2.05 0.6) (layers "F.Paste")
      (pintype "input"))
    (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-28W_7.5x17.9mm_P1.27mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "SpeedFootprints:R_0603_1608MetricSQ" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 125.6 90.8 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "SpeedoDrive.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R6" (at -0.02 0.06 270) (layer "F.CrtYd"))
    (fp_text value "10K" (at 0 1.43 270) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 270) (layer "F.Fab"))
    (pad "" smd rect (at 0.825 0 90) (size 0.8 0.95) (layers "F.Paste"))
    (pad "" smd rect (at -0.825 0 90) (size 0.8 0.95) (layers "F.Paste"))
    (pad "1" smd roundrect (at -0.825 0 90) (size 0.8 0.95) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 90) (size 0.8 0.95) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (net 21 "/DirC") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x08_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 59FED5CC)
    (at 119.6 72.26)
    (descr "Through hole straight pin header, 1x08, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x08 2.54mm single row")
    (property "Sheetfile" "SpeedoDrive.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J4" (at -0.15 6.32) (layer "F.CrtYd"))
    (fp_text value "Conn_01x08" (at 0 20.11) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 8.89 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 "/MA4") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 "/MA3") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "/MA2") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "/MA1") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 "/MD1") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 "/MD2") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole oval (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 "/MD3") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" thru_hole oval (at 0 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 "/MD4") (pinfunction "Pin_8") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x08_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "SpeedFootprints:R_0603_1608MetricSQ" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 128.4 90.8 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "SpeedoDrive.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R9" (at -0.01 -0.12 90) (layer "F.CrtYd"))
    (fp_text value "10K" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "" smd rect (at -0.825 0 270) (size 0.8 0.95) (layers "F.Paste"))
    (pad "" smd rect (at 0.825 0 270) (size 0.8 0.95) (layers "F.Paste"))
    (pad "1" smd roundrect (at -0.825 0 270) (size 0.8 0.95) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "/StpD") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 270) (size 0.8 0.95) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "SpeedFootprints:C_0805_2012MetricSQ" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 138.09 91.25 -90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "SpeedoDrive.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C6" (at -0.24 0.05 -90) (layer "F.CrtYd"))
    (fp_text value "6.8uF" (at 0 1.68 -90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 -90) (layer "F.Fab"))
    (pad "" smd rect (at -0.95 0 270) (size 1 1.45) (layers "F.Paste"))
    (pad "" smd rect (at 0.95 0 270) (size 1 1.45) (layers "F.Paste"))
    (pad "1" smd roundrect (at -0.95 0 270) (size 1 1.45) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "VCC") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 270) (size 1 1.45) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "SpeedFootprints:R_0603_1608MetricSQ" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 123.4 90.775 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "SpeedoDrive.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R7" (at 0.025 0 270) (layer "F.CrtYd"))
    (fp_text value "10K" (at 0 1.43 270) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 270) (layer "F.Fab"))
    (pad "" smd rect (at -0.825 0 90) (size 0.8 0.95) (layers "F.Paste"))
    (pad "" smd rect (at 0.825 0 90) (size 0.8 0.95) (layers "F.Paste"))
    (pad "1" smd roundrect (at -0.825 0 90) (size 0.8 0.95) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 90) (size 0.8 0.95) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (net 20 "/StpC") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "SpeedFootprints:R_0603_1608MetricSQ" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 124.73 69.1)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "SpeedoDrive.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R4" (at 0.25 0.01 180) (layer "F.CrtYd"))
    (fp_text value "10K" (at 0 1.43 180) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 180) (layer "F.Fab"))
    (pad "" smd rect (at 0.825 0) (size 0.8 0.95) (layers "F.Paste"))
    (pad "" smd rect (at -0.825 0) (size 0.8 0.95) (layers "F.Paste"))
    (pad "1" smd roundrect (at -0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (net 11 "/DirB") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x06_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 59FED5CC)
    (at 121.32 95.35 90)
    (descr "Through hole straight pin header, 1x06, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x06 2.54mm single row")
    (property "Sheetfile" "SpeedoDrive.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J3" (at -0.1 6.48 180) (layer "F.CrtYd"))
    (fp_text value "Conn_01x06" (at 0 15.03 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 6.35) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 "/StpC") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 "/DirC") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 "/StpD") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 "/DirD") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "VCC") (pinfunction "Pin_6") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x06_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x08_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 59FED5CC)
    (at 137.43 69.72)
    (descr "Through hole straight pin header, 1x08, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x08 2.54mm single row")
    (property "Sheetfile" "SpeedoDrive.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J2" (at -0.1 6.33) (layer "F.CrtYd"))
    (fp_text value "Conn_01x08" (at 0 20.11) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 8.89 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 "/MB4") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 "/MB3") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 "/MB2") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 "/MB1") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 "/MC1") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 "/MC2") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole oval (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 "/MC3") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" thru_hole oval (at 0 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 "/MC4") (pinfunction "Pin_8") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x08_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "SpeedFootprints:C_0603_1608MetricSQ" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 133.39 90.68 -90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "SpeedoDrive.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C4" (at 0.01 0.01 90) (layer "F.CrtYd"))
    (fp_text value "100nF" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "" smd rect (at 0.775 0 270) (size 0.9 0.95) (layers "F.Paste"))
    (pad "" smd rect (at -0.775 0 270) (size 0.9 0.95) (layers "F.Paste"))
    (pad "1" smd roundrect (at -0.775 0 270) (size 0.9 0.95) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "VCC") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0 270) (size 0.9 0.95) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "SpeedFootprints:R_0603_1608MetricSQ" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 134 69.16 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "SpeedoDrive.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R3" (at 0.05 0.05) (layer "F.CrtYd"))
    (fp_text value "10K" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" smd rect (at -0.825 0 180) (size 0.8 0.95) (layers "F.Paste"))
    (pad "" smd rect (at 0.825 0 180) (size 0.8 0.95) (layers "F.Paste"))
    (pad "1" smd roundrect (at -0.825 0 180) (size 0.8 0.95) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 180) (size 0.8 0.95) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (net 8 "/StpA") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_rect (start 117.61 63.04) (end 139.57 97.35) (layer "Edge.Cuts") (width 0.1) (fill none))
  (gr_text "8/22\njkl" (at 125.47 78.37 270) (layer "B.SilkS"))
  (gr_text "SpeedoDrive" (at 133.66 77.56 270) (layer "B.SilkS"))
  (gr_text "For VID6606\nor X12.017" (at 130.4 77.71 270) (layer "B.SilkS"))
  (gr_text "B2" (at 135.07 74.84) (layer "F.SilkS"))
  (gr_text "RST" (at 132.91 67.6) (layer "F.SilkS"))
  (gr_text "SB" (at 124.91 67.55) (layer "F.SilkS"))
  (gr_text "DA" (at 127.54 67.51) (layer "F.SilkS"))
  (gr_text "B1" (at 135.03 77.38) (layer "F.SilkS"))
  (gr_text "SD" (at 126.6 92.97) (layer "F.SilkS"))
  (gr_text "C3" (at 135.03 85) (layer "F.SilkS"))
  (gr_text "SC" (at 121.35 92.92) (layer "F.SilkS"))
  (gr_text "VCC" (at 133.56 92.95) (layer "F.SilkS"))
  (gr_text "B3" (at 135.16 72.26) (layer "F.SilkS"))
  (gr_text "D2" (at 121.94 84.83) (layer "F.SilkS"))
  (gr_text "A3" (at 121.9 74.84) (layer "F.SilkS"))
  (gr_text "A1" (at 121.8 79.74) (layer "F.SilkS"))
  (gr_text "GND" (at 131.43 93.01) (layer "F.SilkS"))
  (gr_text "SpeedoDrive" (at 128.32 80.25 270) (layer "F.SilkS"))
  (gr_text "D1" (at 121.9 82.46) (layer "F.SilkS"))
  (gr_text "DD" (at 128.88 93.02) (layer "F.SilkS"))
  (gr_text "C2" (at 135.12 82.46) (layer "F.SilkS"))
  (gr_text "C1" (at 134.99 79.79) (layer "F.SilkS"))
  (gr_text "C4" (at 135.12 87.54) (layer "F.SilkS"))
  (gr_text "SA" (at 130.12 67.55) (layer "F.SilkS"))
  (gr_text "A4" (at 121.9 72.3) (layer "F.SilkS"))
  (gr_text "DC" (at 123.89 93.01) (layer "F.SilkS"))
  (gr_text "B4" (at 134.95 70.43) (layer "F.SilkS"))
  (gr_text "A2" (at 121.94 77.25) (layer "F.SilkS"))
  (gr_text "DB" (at 122.45 67.38) (layer "F.SilkS"))
  (gr_text "D4" (at 122.03 90.09) (layer "F.SilkS"))
  (gr_text "D3" (at 121.99 87.38) (layer "F.SilkS"))
  (zone (net 2) (net_name "GND") (layer "B.Cu") (hatch edge 0.508)
    (connect_pads thru_hole_only (clearance 0.254))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.254) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 139.42 97.14)
        (xy 117.67 97.14)
        (xy 117.67 63.14)
        (xy 139.42 63.14)
      )
    )
  )
)
