(kicad_pcb (version 20211014) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0)
    (aux_axis_origin 101.6 50.8)
    (grid_origin 101.6 50.8)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "unconnected-(J1-Pad1)")
  (net 2 "unconnected-(J1-Pad2)")
  (net 3 "unconnected-(J1-Pad3)")
  (net 4 "unconnected-(J1-Pad4)")
  (net 5 "/~{RFSH}")
  (net 6 "unconnected-(J1-Pad6)")
  (net 7 "/~{RESET}")
  (net 8 "/~{BUSRQ}")
  (net 9 "/~{INT}")
  (net 10 "/~{NMI}")
  (net 11 "/~{CLK}")
  (net 12 "/~{WAIT}")
  (net 13 "unconnected-(J1-Pad13)")
  (net 14 "unconnected-(J1-Pad14)")
  (net 15 "/~{HALT}")
  (net 16 "unconnected-(J1-Pad16)")
  (net 17 "/D0")
  (net 18 "/~{BUSAK}")
  (net 19 "/D2")
  (net 20 "/D1")
  (net 21 "unconnected-(J1-Pad21)")
  (net 22 "/D3")
  (net 23 "unconnected-(J1-Pad24)")
  (net 24 "unconnected-(J1-Pad25)")
  (net 25 "unconnected-(J1-Pad27)")
  (net 26 "unconnected-(J1-Pad28)")
  (net 27 "/D4")
  (net 28 "unconnected-(J1-Pad30)")
  (net 29 "unconnected-(J1-Pad31)")
  (net 30 "/D5")
  (net 31 "unconnected-(J1-Pad33)")
  (net 32 "unconnected-(J1-Pad34)")
  (net 33 "unconnected-(J1-Pad35)")
  (net 34 "unconnected-(J1-Pad36)")
  (net 35 "unconnected-(J1-Pad37)")
  (net 36 "unconnected-(J1-Pad38)")
  (net 37 "unconnected-(J1-Pad39)")
  (net 38 "unconnected-(J1-Pad40)")
  (net 39 "unconnected-(J1-Pad41)")
  (net 40 "unconnected-(J1-Pad42)")
  (net 41 "unconnected-(J1-Pad43)")
  (net 42 "unconnected-(J1-Pad44)")
  (net 43 "unconnected-(J1-Pad45)")
  (net 44 "unconnected-(J1-Pad46)")
  (net 45 "unconnected-(J1-Pad47)")
  (net 46 "unconnected-(J1-Pad48)")
  (net 47 "unconnected-(J1-Pad49)")
  (net 48 "unconnected-(J1-Pad50)")
  (net 49 "unconnected-(J1-Pad51)")
  (net 50 "unconnected-(J1-Pad52)")
  (net 51 "unconnected-(J1-Pad53)")
  (net 52 "unconnected-(J1-Pad54)")
  (net 53 "+3V3")
  (net 54 "GND")
  (net 55 "+5V")
  (net 56 "unconnected-(J2-Pad1)")
  (net 57 "unconnected-(J2-Pad2)")
  (net 58 "unconnected-(J2-Pad3)")
  (net 59 "unconnected-(J2-Pad4)")
  (net 60 "unconnected-(J2-Pad5)")
  (net 61 "unconnected-(J2-Pad6)")
  (net 62 "unconnected-(J2-Pad7)")
  (net 63 "unconnected-(J2-Pad8)")
  (net 64 "unconnected-(J2-Pad9)")
  (net 65 "unconnected-(J2-Pad10)")
  (net 66 "unconnected-(J2-Pad11)")
  (net 67 "unconnected-(J2-Pad12)")
  (net 68 "unconnected-(J2-Pad13)")
  (net 69 "unconnected-(J2-Pad14)")
  (net 70 "unconnected-(J2-Pad15)")
  (net 71 "unconnected-(J2-Pad16)")
  (net 72 "/A7")
  (net 73 "/A4")
  (net 74 "/A5")
  (net 75 "/A6")
  (net 76 "/A3")
  (net 77 "/A2")
  (net 78 "/A1")
  (net 79 "/A0")
  (net 80 "/~{M1}")
  (net 81 "/~{IORQ}")
  (net 82 "/~{MREQ}")
  (net 83 "unconnected-(J2-Pad28)")
  (net 84 "unconnected-(J2-Pad29)")
  (net 85 "unconnected-(J2-Pad30)")
  (net 86 "unconnected-(J2-Pad31)")
  (net 87 "unconnected-(J2-Pad32)")
  (net 88 "unconnected-(J2-Pad33)")
  (net 89 "unconnected-(J2-Pad34)")
  (net 90 "unconnected-(J2-Pad35)")
  (net 91 "/~{WR}")
  (net 92 "/~{RD}")
  (net 93 "/D7")
  (net 94 "/D6")
  (net 95 "unconnected-(J2-Pad40)")
  (net 96 "unconnected-(J2-Pad41)")
  (net 97 "unconnected-(J2-Pad42)")
  (net 98 "unconnected-(J2-Pad43)")
  (net 99 "unconnected-(J2-Pad44)")
  (net 100 "unconnected-(J2-Pad45)")
  (net 101 "unconnected-(J2-Pad46)")
  (net 102 "/A15")
  (net 103 "/A14")
  (net 104 "/A13")
  (net 105 "/A12")
  (net 106 "/A11")
  (net 107 "/A10")
  (net 108 "/A9")
  (net 109 "/A8")
  (net 110 "unconnected-(J2-Pad55)")
  (net 111 "unconnected-(J2-Pad56)")
  (net 112 "unconnected-(J2-Pad57)")
  (net 113 "unconnected-(J2-Pad58)")
  (net 114 "unconnected-(U1-Pad11)")
  (net 115 "Net-(J1-Pad23)")
  (net 116 "Net-(J1-Pad26)")
  (footprint "Aesthetics:OSHW-LOGO-M" (layer "F.Cu")
    (tedit 200000)
    (at 151.5364 119.0244)
    (descr "OPEN-SOURCE HARDWARE (OSHW) LOGO - MEDIUM - SILKSCREEN")
    (tags "OPEN-SOURCE HARDWARE (OSHW) LOGO - MEDIUM - SILKSCREEN")
    (property "Champ4" "")
    (property "Sheetfile" "stm32f407_z80.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "LOGO1" (at -1.016 -0.508) (layer "F.SilkS") hide)
    (fp_text value "OSHW-LOGOM" (at 15.24 0) (layer "F.SilkS") hide)
  )
  (footprint "Connectors:1X06" (layer "F.Cu")
    (tedit 5963D43D)
    (at 138.938 122.3518 180)
    (descr "PLATED THROUGH HOLE - 6 PIN")
    (tags "PLATED THROUGH HOLE - 6 PIN")
    (property "Champ4" "XXX-00000")
    (property "Sheetfile" "stm32f407_z80.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "J3" (at 0 -1.905 180) (layer "F.SilkS"))
    (fp_text value "6_PIN_SERIAL_TARGET" (at 0 1.905 180) (layer "F.SilkS"))
    (pad "1" thru_hole circle locked (at 0 0 180) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad "2" thru_hole circle locked (at 2.54 0 180) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 115 "Net-(J1-Pad23)") (solder_mask_margin 0.1016))
    (pad "3" thru_hole circle locked (at 5.08 0 180) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 116 "Net-(J1-Pad26)") (solder_mask_margin 0.1016))
    (pad "4" thru_hole circle locked (at 7.62 0 180) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad "5" thru_hole circle locked (at 10.16 0 180) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad "6" thru_hole circle locked (at 12.7 0 180) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 54 "GND") (solder_mask_margin 0.1016))
  )
  (footprint "PHYSNOCT:PHYSNOCT" (layer "F.Cu")
    (tedit 0)
    (at 108.4941 116.6134)
    (property "Sheetfile" "stm32f407_z80.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U2" (at 0 0) (layer "Cmts.User") hide)
    (fp_text value "PHYSNOCT_PHYSNOCT" (at 0 0) (layer "Eco1.User") hide)
  )
  (footprint "Connector_PinSocket_2.54mm:PinSocket_2x29_P2.54mm_Vertical" (layer "B.Cu")
    (tedit 5A19A41F)
    (at 101.6 50.8 180)
    (descr "Through hole straight socket strip, 2x29, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 2x29 2.54mm double row")
    (property "Sheetfile" "stm32f407_z80.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J1" (at -1.27 2.77) (layer "B.SilkS"))
    (fp_text value "Conn_02x29_Odd_Even" (at -12.8778 -68.1736) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at -1.27 -35.56 90) (layer "B.Fab"))
    (pad "1" thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "unconnected-(J1-Pad1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at -2.54 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "unconnected-(J1-Pad2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 -2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "unconnected-(J1-Pad3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at -2.54 -2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "unconnected-(J1-Pad4)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 -5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 "/~{RFSH}") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at -2.54 -5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 "unconnected-(J1-Pad6)") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole oval (at 0 -7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 "/~{RESET}") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" thru_hole oval (at -2.54 -7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 "/~{BUSRQ}") (pinfunction "Pin_8") (pintype "passive"))
    (pad "9" thru_hole oval (at 0 -10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 "/~{INT}") (pinfunction "Pin_9") (pintype "passive"))
    (pad "10" thru_hole oval (at -2.54 -10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 "/~{NMI}") (pinfunction "Pin_10") (pintype "passive"))
    (pad "11" thru_hole oval (at 0 -12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 "/~{CLK}") (pinfunction "Pin_11") (pintype "passive"))
    (pad "12" thru_hole oval (at -2.54 -12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 "/~{WAIT}") (pinfunction "Pin_12") (pintype "passive"))
    (pad "13" thru_hole oval (at 0 -15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 "unconnected-(J1-Pad13)") (pinfunction "Pin_13") (pintype "passive"))
    (pad "14" thru_hole oval (at -2.54 -15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 "unconnected-(J1-Pad14)") (pinfunction "Pin_14") (pintype "passive"))
    (pad "15" thru_hole oval (at 0 -17.78 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 "/~{HALT}") (pinfunction "Pin_15") (pintype "passive"))
    (pad "16" thru_hole oval (at -2.54 -17.78 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 "unconnected-(J1-Pad16)") (pinfunction "Pin_16") (pintype "passive"))
    (pad "17" thru_hole oval (at 0 -20.32 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 "/D0") (pinfunction "Pin_17") (pintype "passive"))
    (pad "18" thru_hole oval (at -2.54 -20.32 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 "/~{BUSAK}") (pinfunction "Pin_18") (pintype "passive"))
    (pad "19" thru_hole oval (at 0 -22.86 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 "/D2") (pinfunction "Pin_19") (pintype "passive"))
    (pad "20" thru_hole oval (at -2.54 -22.86 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 "/D1") (pinfunction "Pin_20") (pintype "passive"))
    (pad "21" thru_hole oval (at 0 -25.4 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 "unconnected-(J1-Pad21)") (pinfunction "Pin_21") (pintype "passive"))
    (pad "22" thru_hole oval (at -2.54 -25.4 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 "/D3") (pinfunction "Pin_22") (pintype "passive"))
    (pad "23" thru_hole oval (at 0 -27.94 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 115 "Net-(J1-Pad23)") (pinfunction "Pin_23") (pintype "passive"))
    (pad "24" thru_hole oval (at -2.54 -27.94 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 "unconnected-(J1-Pad24)") (pinfunction "Pin_24") (pintype "passive"))
    (pad "25" thru_hole oval (at 0 -30.48 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 "unconnected-(J1-Pad25)") (pinfunction "Pin_25") (pintype "passive"))
    (pad "26" thru_hole oval (at -2.54 -30.48 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 116 "Net-(J1-Pad26)") (pinfunction "Pin_26") (pintype "passive"))
    (pad "27" thru_hole oval (at 0 -33.02 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 "unconnected-(J1-Pad27)") (pinfunction "Pin_27") (pintype "passive"))
    (pad "28" thru_hole oval (at -2.54 -33.02 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 "unconnected-(J1-Pad28)") (pinfunction "Pin_28") (pintype "passive"))
    (pad "29" thru_hole oval (at 0 -35.56 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 "/D4") (pinfunction "Pin_29") (pintype "passive"))
    (pad "30" thru_hole oval (at -2.54 -35.56 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 "unconnected-(J1-Pad30)") (pinfunction "Pin_30") (pintype "passive"))
    (pad "31" thru_hole oval (at 0 -38.1 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 "unconnected-(J1-Pad31)") (pinfunction "Pin_31") (pintype "passive"))
    (pad "32" thru_hole oval (at -2.54 -38.1 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 "/D5") (pinfunction "Pin_32") (pintype "passive"))
    (pad "33" thru_hole oval (at 0 -40.64 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 "unconnected-(J1-Pad33)") (pinfunction "Pin_33") (pintype "passive"))
    (pad "34" thru_hole oval (at -2.54 -40.64 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 "unconnected-(J1-Pad34)") (pinfunction "Pin_34") (pintype "passive"))
    (pad "35" thru_hole oval (at 0 -43.18 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 33 "unconnected-(J1-Pad35)") (pinfunction "Pin_35") (pintype "passive"))
    (pad "36" thru_hole oval (at -2.54 -43.18 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 "unconnected-(J1-Pad36)") (pinfunction "Pin_36") (pintype "passive"))
    (pad "37" thru_hole oval (at 0 -45.72 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 35 "unconnected-(J1-Pad37)") (pinfunction "Pin_37") (pintype "passive"))
    (pad "38" thru_hole oval (at -2.54 -45.72 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 36 "unconnected-(J1-Pad38)") (pinfunction "Pin_38") (pintype "passive"))
    (pad "39" thru_hole oval (at 0 -48.26 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 37 "unconnected-(J1-Pad39)") (pinfunction "Pin_39") (pintype "passive"))
    (pad "40" thru_hole oval (at -2.54 -48.26 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 38 "unconnected-(J1-Pad40)") (pinfunction "Pin_40") (pintype "passive"))
    (pad "41" thru_hole oval (at 0 -50.8 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 39 "unconnected-(J1-Pad41)") (pinfunction "Pin_41") (pintype "passive"))
    (pad "42" thru_hole oval (at -2.54 -50.8 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 40 "unconnected-(J1-Pad42)") (pinfunction "Pin_42") (pintype "passive"))
    (pad "43" thru_hole oval (at 0 -53.34 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 41 "unconnected-(J1-Pad43)") (pinfunction "Pin_43") (pintype "passive"))
    (pad "44" thru_hole oval (at -2.54 -53.34 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 42 "unconnected-(J1-Pad44)") (pinfunction "Pin_44") (pintype "passive"))
    (pad "45" thru_hole oval (at 0 -55.88 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 43 "unconnected-(J1-Pad45)") (pinfunction "Pin_45") (pintype "passive"))
    (pad "46" thru_hole oval (at -2.54 -55.88 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 44 "unconnected-(J1-Pad46)") (pinfunction "Pin_46") (pintype "passive"))
    (pad "47" thru_hole oval (at 0 -58.42 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 45 "unconnected-(J1-Pad47)") (pinfunction "Pin_47") (pintype "passive"))
    (pad "48" thru_hole oval (at -2.54 -58.42 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 46 "unconnected-(J1-Pad48)") (pinfunction "Pin_48") (pintype "passive"))
    (pad "49" thru_hole oval (at 0 -60.96 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 47 "unconnected-(J1-Pad49)") (pinfunction "Pin_49") (pintype "passive"))
    (pad "50" thru_hole oval (at -2.54 -60.96 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 48 "unconnected-(J1-Pad50)") (pinfunction "Pin_50") (pintype "passive"))
    (pad "51" thru_hole oval (at 0 -63.5 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 49 "unconnected-(J1-Pad51)") (pinfunction "Pin_51") (pintype "passive"))
    (pad "52" thru_hole oval (at -2.54 -63.5 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 50 "unconnected-(J1-Pad52)") (pinfunction "Pin_52") (pintype "passive"))
    (pad "53" thru_hole oval (at 0 -66.04 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 51 "unconnected-(J1-Pad53)") (pinfunction "Pin_53") (pintype "passive+no_connect"))
    (pad "54" thru_hole oval (at -2.54 -66.04 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 52 "unconnected-(J1-Pad54)") (pinfunction "Pin_54") (pintype "passive+no_connect"))
    (pad "55" thru_hole oval (at 0 -68.58 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 53 "+3V3") (pinfunction "Pin_55") (pintype "passive"))
    (pad "56" thru_hole oval (at -2.54 -68.58 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 54 "GND") (pinfunction "Pin_56") (pintype "passive"))
    (pad "57" thru_hole oval (at 0 -71.12 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 55 "+5V") (pinfunction "Pin_57") (pintype "passive"))
    (pad "58" thru_hole oval (at -2.54 -71.12 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 54 "GND") (pinfunction "Pin_58") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_2x29_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinSocket_2.54mm:PinSocket_2x29_P2.54mm_Vertical" (layer "B.Cu")
    (tedit 5A19A41F)
    (at 161.6202 50.8 180)
    (descr "Through hole straight socket strip, 2x29, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 2x29 2.54mm double row")
    (property "Sheetfile" "stm32f407_z80.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J2" (at -1.27 2.77) (layer "B.SilkS"))
    (fp_text value "Conn_02x29_Odd_Even" (at 11.0236 -71.6534) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at -1.27 -35.56 90) (layer "B.Fab"))
    (pad "1" thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 56 "unconnected-(J2-Pad1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at -2.54 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 57 "unconnected-(J2-Pad2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 -2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 58 "unconnected-(J2-Pad3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at -2.54 -2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 59 "unconnected-(J2-Pad4)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 -5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 60 "unconnected-(J2-Pad5)") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at -2.54 -5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 61 "unconnected-(J2-Pad6)") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole oval (at 0 -7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 62 "unconnected-(J2-Pad7)") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" thru_hole oval (at -2.54 -7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 63 "unconnected-(J2-Pad8)") (pinfunction "Pin_8") (pintype "passive"))
    (pad "9" thru_hole oval (at 0 -10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 64 "unconnected-(J2-Pad9)") (pinfunction "Pin_9") (pintype "passive"))
    (pad "10" thru_hole oval (at -2.54 -10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 65 "unconnected-(J2-Pad10)") (pinfunction "Pin_10") (pintype "passive"))
    (pad "11" thru_hole oval (at 0 -12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 66 "unconnected-(J2-Pad11)") (pinfunction "Pin_11") (pintype "passive"))
    (pad "12" thru_hole oval (at -2.54 -12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 67 "unconnected-(J2-Pad12)") (pinfunction "Pin_12") (pintype "passive"))
    (pad "13" thru_hole oval (at 0 -15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 68 "unconnected-(J2-Pad13)") (pinfunction "Pin_13") (pintype "passive"))
    (pad "14" thru_hole oval (at -2.54 -15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 69 "unconnected-(J2-Pad14)") (pinfunction "Pin_14") (pintype "passive"))
    (pad "15" thru_hole oval (at 0 -17.78 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 70 "unconnected-(J2-Pad15)") (pinfunction "Pin_15") (pintype "passive"))
    (pad "16" thru_hole oval (at -2.54 -17.78 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 71 "unconnected-(J2-Pad16)") (pinfunction "Pin_16") (pintype "passive"))
    (pad "17" thru_hole oval (at 0 -20.32 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 72 "/A7") (pinfunction "Pin_17") (pintype "passive"))
    (pad "18" thru_hole oval (at -2.54 -20.32 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 75 "/A6") (pinfunction "Pin_18") (pintype "passive"))
    (pad "19" thru_hole oval (at 0 -22.86 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 74 "/A5") (pinfunction "Pin_19") (pintype "passive"))
    (pad "20" thru_hole oval (at -2.54 -22.86 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 73 "/A4") (pinfunction "Pin_20") (pintype "passive"))
    (pad "21" thru_hole oval (at 0 -25.4 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 76 "/A3") (pinfunction "Pin_21") (pintype "passive"))
    (pad "22" thru_hole oval (at -2.54 -25.4 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 77 "/A2") (pinfunction "Pin_22") (pintype "passive"))
    (pad "23" thru_hole oval (at 0 -27.94 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 78 "/A1") (pinfunction "Pin_23") (pintype "passive"))
    (pad "24" thru_hole oval (at -2.54 -27.94 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 79 "/A0") (pinfunction "Pin_24") (pintype "passive"))
    (pad "25" thru_hole oval (at 0 -30.48 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 80 "/~{M1}") (pinfunction "Pin_25") (pintype "passive"))
    (pad "26" thru_hole oval (at -2.54 -30.48 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 81 "/~{IORQ}") (pinfunction "Pin_26") (pintype "passive"))
    (pad "27" thru_hole oval (at 0 -33.02 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 82 "/~{MREQ}") (pinfunction "Pin_27") (pintype "passive"))
    (pad "28" thru_hole oval (at -2.54 -33.02 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 83 "unconnected-(J2-Pad28)") (pinfunction "Pin_28") (pintype "passive"))
    (pad "29" thru_hole oval (at 0 -35.56 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 84 "unconnected-(J2-Pad29)") (pinfunction "Pin_29") (pintype "passive"))
    (pad "30" thru_hole oval (at -2.54 -35.56 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 85 "unconnected-(J2-Pad30)") (pinfunction "Pin_30") (pintype "passive"))
    (pad "31" thru_hole oval (at 0 -38.1 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 86 "unconnected-(J2-Pad31)") (pinfunction "Pin_31") (pintype "passive"))
    (pad "32" thru_hole oval (at -2.54 -38.1 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 87 "unconnected-(J2-Pad32)") (pinfunction "Pin_32") (pintype "passive"))
    (pad "33" thru_hole oval (at 0 -40.64 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 88 "unconnected-(J2-Pad33)") (pinfunction "Pin_33") (pintype "passive"))
    (pad "34" thru_hole oval (at -2.54 -40.64 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 89 "unconnected-(J2-Pad34)") (pinfunction "Pin_34") (pintype "passive"))
    (pad "35" thru_hole oval (at 0 -43.18 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 90 "unconnected-(J2-Pad35)") (pinfunction "Pin_35") (pintype "passive"))
    (pad "36" thru_hole oval (at -2.54 -43.18 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 91 "/~{WR}") (pinfunction "Pin_36") (pintype "passive"))
    (pad "37" thru_hole oval (at 0 -45.72 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 92 "/~{RD}") (pinfunction "Pin_37") (pintype "passive"))
    (pad "38" thru_hole oval (at -2.54 -45.72 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 93 "/D7") (pinfunction "Pin_38") (pintype "passive"))
    (pad "39" thru_hole oval (at 0 -48.26 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 94 "/D6") (pinfunction "Pin_39") (pintype "passive"))
    (pad "40" thru_hole oval (at -2.54 -48.26 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 95 "unconnected-(J2-Pad40)") (pinfunction "Pin_40") (pintype "passive"))
    (pad "41" thru_hole oval (at 0 -50.8 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 96 "unconnected-(J2-Pad41)") (pinfunction "Pin_41") (pintype "passive"))
    (pad "42" thru_hole oval (at -2.54 -50.8 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 97 "unconnected-(J2-Pad42)") (pinfunction "Pin_42") (pintype "passive"))
    (pad "43" thru_hole oval (at 0 -53.34 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 98 "unconnected-(J2-Pad43)") (pinfunction "Pin_43") (pintype "passive"))
    (pad "44" thru_hole oval (at -2.54 -53.34 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 99 "unconnected-(J2-Pad44)") (pinfunction "Pin_44") (pintype "passive"))
    (pad "45" thru_hole oval (at 0 -55.88 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 100 "unconnected-(J2-Pad45)") (pinfunction "Pin_45") (pintype "passive"))
    (pad "46" thru_hole oval (at -2.54 -55.88 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 101 "unconnected-(J2-Pad46)") (pinfunction "Pin_46") (pintype "passive"))
    (pad "47" thru_hole oval (at 0 -58.42 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 102 "/A15") (pinfunction "Pin_47") (pintype "passive"))
    (pad "48" thru_hole oval (at -2.54 -58.42 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 103 "/A14") (pinfunction "Pin_48") (pintype "passive"))
    (pad "49" thru_hole oval (at 0 -60.96 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 104 "/A13") (pinfunction "Pin_49") (pintype "passive"))
    (pad "50" thru_hole oval (at -2.54 -60.96 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 105 "/A12") (pinfunction "Pin_50") (pintype "passive"))
    (pad "51" thru_hole oval (at 0 -63.5 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 106 "/A11") (pinfunction "Pin_51") (pintype "passive"))
    (pad "52" thru_hole oval (at -2.54 -63.5 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 107 "/A10") (pinfunction "Pin_52") (pintype "passive"))
    (pad "53" thru_hole oval (at 0 -66.04 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 108 "/A9") (pinfunction "Pin_53") (pintype "passive"))
    (pad "54" thru_hole oval (at -2.54 -66.04 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 109 "/A8") (pinfunction "Pin_54") (pintype "passive"))
    (pad "55" thru_hole oval (at 0 -68.58 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 110 "unconnected-(J2-Pad55)") (pinfunction "Pin_55") (pintype "passive"))
    (pad "56" thru_hole oval (at -2.54 -68.58 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 111 "unconnected-(J2-Pad56)") (pinfunction "Pin_56") (pintype "passive"))
    (pad "57" thru_hole oval (at 0 -71.12 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 112 "unconnected-(J2-Pad57)") (pinfunction "Pin_57") (pintype "passive"))
    (pad "58" thru_hole oval (at -2.54 -71.12 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 113 "unconnected-(J2-Pad58)") (pinfunction "Pin_58") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_2x29_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "digikey-footprints:DIP-40_W15.24mm" (layer "B.Cu")
    (tedit 59C9209A)
    (at 129.54 48.26 180)
    (descr "http://www.ti.com/lit/ds/symlink/tpic6b595.pdf")
    (property "Sheetfile" "stm32f407_z80.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U1" (at -2.54 0) (layer "B.SilkS"))
    (fp_text value "Z80CPU" (at 7.15 -51.43) (layer "B.Fab"))
    (fp_text user "REF**" (at 7.31 -25.74) (layer "B.Fab"))
    (pad "1" thru_hole circle locked (at 0 0 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 106 "/A11") (pinfunction "A11") (pintype "output"))
    (pad "2" thru_hole circle locked (at 0 -2.54 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 105 "/A12") (pinfunction "A12") (pintype "output"))
    (pad "3" thru_hole circle locked (at 0 -5.08 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 104 "/A13") (pinfunction "A13") (pintype "output"))
    (pad "4" thru_hole circle locked (at 0 -7.62 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 103 "/A14") (pinfunction "A14") (pintype "output"))
    (pad "5" thru_hole circle locked (at 0 -10.16 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 102 "/A15") (pinfunction "A15") (pintype "output"))
    (pad "6" thru_hole circle locked (at 0 -12.7 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 11 "/~{CLK}") (pinfunction "~{CLK}") (pintype "input"))
    (pad "7" thru_hole circle locked (at 0 -15.24 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 27 "/D4") (pinfunction "D4") (pintype "bidirectional"))
    (pad "8" thru_hole circle locked (at 0 -17.78 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 22 "/D3") (pinfunction "D3") (pintype "bidirectional"))
    (pad "9" thru_hole circle locked (at 0 -20.32 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 30 "/D5") (pinfunction "D5") (pintype "bidirectional"))
    (pad "10" thru_hole circle locked (at 0 -22.86 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 94 "/D6") (pinfunction "D6") (pintype "bidirectional"))
    (pad "11" thru_hole circle locked (at 0 -25.4 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 114 "unconnected-(U1-Pad11)") (pinfunction "VCC") (pintype "power_in+no_connect"))
    (pad "12" thru_hole circle locked (at 0 -27.94 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 19 "/D2") (pinfunction "D2") (pintype "bidirectional"))
    (pad "13" thru_hole circle locked (at 0 -30.48 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 93 "/D7") (pinfunction "D7") (pintype "bidirectional"))
    (pad "14" thru_hole circle locked (at 0 -33.02 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 17 "/D0") (pinfunction "D0") (pintype "bidirectional"))
    (pad "15" thru_hole circle locked (at 0 -35.56 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 20 "/D1") (pinfunction "D1") (pintype "bidirectional"))
    (pad "16" thru_hole circle locked (at 0 -38.1 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 9 "/~{INT}") (pinfunction "~{INT}") (pintype "input"))
    (pad "17" thru_hole circle locked (at 0 -40.64 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 10 "/~{NMI}") (pinfunction "~{NMI}") (pintype "input"))
    (pad "18" thru_hole circle locked (at 0 -43.18 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 15 "/~{HALT}") (pinfunction "~{HALT}") (pintype "output"))
    (pad "19" thru_hole circle locked (at 0 -45.72 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 82 "/~{MREQ}") (pinfunction "~{MREQ}") (pintype "output"))
    (pad "20" thru_hole circle locked (at 0 -48.26 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 81 "/~{IORQ}") (pinfunction "~{IORQ}") (pintype "output"))
    (pad "21" thru_hole circle locked (at 15.24 -48.26 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 92 "/~{RD}") (pinfunction "~{RD}") (pintype "output"))
    (pad "22" thru_hole circle locked (at 15.24 -45.72 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 91 "/~{WR}") (pinfunction "~{WR}") (pintype "output"))
    (pad "23" thru_hole circle locked (at 15.24 -43.18 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 18 "/~{BUSAK}") (pinfunction "~{BUSACK}") (pintype "output"))
    (pad "24" thru_hole circle locked (at 15.24 -40.64 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 12 "/~{WAIT}") (pinfunction "~{WAIT}") (pintype "input"))
    (pad "25" thru_hole circle locked (at 15.24 -38.1 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 8 "/~{BUSRQ}") (pinfunction "~{BUSRQ}") (pintype "input"))
    (pad "26" thru_hole circle locked (at 15.24 -35.56 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 7 "/~{RESET}") (pinfunction "~{RESET}") (pintype "input"))
    (pad "27" thru_hole circle locked (at 15.24 -33.02 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 80 "/~{M1}") (pinfunction "~{M1}") (pintype "output"))
    (pad "28" thru_hole circle locked (at 15.24 -30.48 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 5 "/~{RFSH}") (pinfunction "~{RFSH}") (pintype "output"))
    (pad "29" thru_hole circle locked (at 15.24 -27.94 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 54 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "30" thru_hole circle locked (at 15.24 -25.4 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 79 "/A0") (pinfunction "A0") (pintype "output"))
    (pad "31" thru_hole circle locked (at 15.24 -22.86 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 78 "/A1") (pinfunction "A1") (pintype "output"))
    (pad "32" thru_hole circle locked (at 15.24 -20.32 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 77 "/A2") (pinfunction "A2") (pintype "output"))
    (pad "33" thru_hole circle locked (at 15.24 -17.78 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 76 "/A3") (pinfunction "A3") (pintype "output"))
    (pad "34" thru_hole circle locked (at 15.24 -15.24 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 73 "/A4") (pinfunction "A4") (pintype "output"))
    (pad "35" thru_hole circle locked (at 15.24 -12.7 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 74 "/A5") (pinfunction "A5") (pintype "output"))
    (pad "36" thru_hole circle locked (at 15.24 -10.16 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 75 "/A6") (pinfunction "A6") (pintype "output"))
    (pad "37" thru_hole circle locked (at 15.24 -7.62 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 72 "/A7") (pinfunction "A7") (pintype "output"))
    (pad "38" thru_hole circle locked (at 15.24 -5.08 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 109 "/A8") (pinfunction "A8") (pintype "output"))
    (pad "39" thru_hole circle locked (at 15.24 -2.54 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 108 "/A9") (pinfunction "A9") (pintype "output"))
    (pad "40" thru_hole circle locked (at 15.24 0 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 107 "/A10") (pinfunction "A10") (pintype "output"))
  )
  (gr_rect (start 99.06 44.704) (end 167.64 124.46) (layer "Edge.Cuts") (width 0.1) (fill none))
  (gr_text "TXO" (at 133.985 118.6434 90) (layer "B.SilkS"))
  (gr_text "GND" (at 122.9868 122.301) (layer "B.SilkS"))
  (gr_text "RXI" (at 136.3472 118.5672 90) (layer "B.SilkS"))
  (gr_text "RXI" (at 136.398 118.5418 90) (layer "F.SilkS"))
  (gr_text "TXO" (at 133.985 118.5672 90) (layer "F.SilkS"))
  (gr_text "Z80 ICE" (at 132.715 107.061) (layer "F.SilkS"))
  (gr_text "GND" (at 123.0122 122.2502) (layer "F.SilkS"))
)
