(kicad_pcb (version 20211014) (generator pcbnew)
  (general
    (thickness 4.69)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (1 "In1.Cu" signal)
    (2 "In2.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "In1.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 2" (type "prepreg") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "In2.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 3" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "ENIG")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x0000020_7ffffff8)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes false)
      (creategerberjobfile true)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference false)
      (plotvalue false)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk true)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "/Vm")
  (net 2 "GND")
  (net 3 "Net-(C3-Pad2)")
  (net 4 "Net-(C7-Pad1)")
  (net 5 "Net-(C7-Pad2)")
  (net 6 "Net-(C8-Pad2)")
  (net 7 "unconnected-(U1-Pad23)")
  (net 8 "unconnected-(U1-Pad24)")
  (net 9 "unconnected-(U1-Pad25)")
  (net 10 "Net-(C9-Pad2)")
  (net 11 "/MB2")
  (net 12 "Net-(C11-Pad2)")
  (net 13 "/MB1")
  (net 14 "/MA1")
  (net 15 "/MA2")
  (net 16 "Net-(C19-Pad2)")
  (net 17 "/CB2")
  (net 18 "/CB1")
  (net 19 "/CA2")
  (net 20 "/CA1")
  (net 21 "/LB")
  (net 22 "/LA")
  (net 23 "/HB2")
  (net 24 "/HB1")
  (net 25 "/LB2")
  (net 26 "/LB1")
  (net 27 "/SRBH")
  (net 28 "/SRBL")
  (net 29 "/HA2")
  (net 30 "/HA1")
  (net 31 "/LA2")
  (net 32 "/LA1")
  (net 33 "/SRAH")
  (net 34 "/SRAL")
  (net 35 "/HB2G")
  (net 36 "/HB1G")
  (net 37 "/LB1G")
  (net 38 "/LB2G")
  (net 39 "/HA1G")
  (net 40 "/HA2G")
  (net 41 "/LA1G")
  (net 42 "/LA2G")
  (net 43 "Net-(U1-Pad13)")
  (net 44 "Net-(U1-Pad14)")
  (net 45 "Net-(U1-Pad15)")
  (net 46 "Net-(U1-Pad16)")
  (net 47 "Net-(U1-Pad17)")
  (net 48 "Net-(U1-Pad18)")
  (net 49 "Net-(R12-Pad2)")
  (net 50 "Net-(U1-Pad26)")
  (net 51 "Net-(U1-Pad27)")
  (footprint "StronStepperFootprints:R_0603_1608MetricRect" (layer "F.Cu")
    (tedit 62395325)
    (at 88.3 78.6 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "StrongStepper.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R12" (at 0 -1.43) (layer "Eco1.User"))
    (fp_text value "10K" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect (at -0.825 0 180) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd rect (at 0.825 0 180) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 49 "Net-(R12-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "StronStepperFootprints:TDSON-8-2EP+5x6mm_P0.65_DUAL" (layer "F.Cu")
    (tedit 6244D870)
    (at 110.05 60.35 90)
    (descr "TDSON-8-2EP_5x6mm_P0.65_DUAL StepUp generated footprint")
    (property "Sheetfile" "StrongStepper.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "Q2" (at 0 -4.1 90) (layer "Eco1.User"))
    (fp_text value "BSC150" (at 0 4.5 90) (layer "Eco1.User"))
    (pad "1" smd rect (at 1.905 -2.825 90) (size 0.65 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 21 "/LB") (pinfunction "S1") (pintype "passive"))
    (pad "2" smd rect (at 0.635 -2.825 90) (size 0.65 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 37 "/LB1G") (pinfunction "G1") (pintype "passive"))
    (pad "3" smd rect (at -0.635 -2.825 90) (size 0.65 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 21 "/LB") (pinfunction "S2") (pintype "passive"))
    (pad "4" smd rect (at -1.905 -2.825 90) (size 0.65 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 38 "/LB2G") (pinfunction "G2") (pintype "passive"))
    (pad "5" smd custom (at -1.337 0 90) (size 0.2 0.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 11 "/MB2") (pinfunction "D2") (pintype "passive") (zone_connect 2)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
            (xy 1.012 -1.575)
            (xy -1.013 -1.575)
            (xy -1.013 3.425)
            (xy -0.312 3.425)
            (xy -0.312 2.925)
            (xy 0.322 2.925)
            (xy 0.322 3.425)
            (xy 1.012 3.425)
          ) (width 0) (fill yes))
      ))
    (pad "8" smd custom (at 1.337 0 90) (size 0.2 0.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 13 "/MB1") (pinfunction "D1") (pintype "passive") (zone_connect 2)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
            (xy -1.012 -1.575)
            (xy 1.013 -1.575)
            (xy 1.013 3.425)
            (xy 0.312 3.425)
            (xy 0.312 2.925)
            (xy -0.323 2.925)
            (xy -0.323 3.425)
            (xy -1.012 3.425)
          ) (width 0) (fill yes))
      ))
    (model "/home/jim/Shared/Projects/Circuits/StrongStepper/TDSON-8-2EP_5x6mm_P0.65_DUAL.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "StronStepperFootprints:TDSON-8-2EP+5x6mm_P0.65_DUAL" (layer "F.Cu")
    (tedit 62340315)
    (at 110.7 75.9 90)
    (descr "TDSON-8-2EP_5x6mm_P0.65_DUAL StepUp generated footprint")
    (property "Sheetfile" "StrongStepper.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "Q4" (at -1.9 -4.1 90) (layer "Eco1.User"))
    (fp_text value "BSC150" (at 0 4.5 90) (layer "Eco1.User"))
    (pad "1" smd rect (at 1.905 -2.825 90) (size 0.65 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 22 "/LA") (pinfunction "S1") (pintype "passive"))
    (pad "2" smd rect (at 0.635 -2.825 90) (size 0.65 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 41 "/LA1G") (pinfunction "G1") (pintype "passive"))
    (pad "3" smd rect (at -0.635 -2.825 90) (size 0.65 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 22 "/LA") (pinfunction "S2") (pintype "passive"))
    (pad "4" smd rect (at -1.905 -2.825 90) (size 0.65 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 42 "/LA2G") (pinfunction "G2") (pintype "passive"))
    (pad "5" smd custom (at -1.337 0 90) (size 0.2 0.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "/MA2") (pinfunction "D2") (pintype "passive") (zone_connect 2)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
            (xy 1.012 -1.575)
            (xy -1.013 -1.575)
            (xy -1.013 3.425)
            (xy -0.312 3.425)
            (xy -0.312 2.925)
            (xy 0.322 2.925)
            (xy 0.322 3.425)
            (xy 1.012 3.425)
          ) (width 0) (fill yes))
      ))
    (pad "8" smd custom (at 1.337 0 90) (size 0.2 0.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 14 "/MA1") (pinfunction "D1") (pintype "passive") (zone_connect 2)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
            (xy -1.012 -1.575)
            (xy 1.013 -1.575)
            (xy 1.013 3.425)
            (xy 0.312 3.425)
            (xy 0.312 2.925)
            (xy -0.323 2.925)
            (xy -0.323 3.425)
            (xy -1.012 3.425)
          ) (width 0) (fill yes))
      ))
    (model "/home/jim/Shared/Projects/Circuits/StrongStepper/TDSON-8-2EP_5x6mm_P0.65_DUAL.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "StronStepperFootprints:PTSA_05_25_4" (layer "F.Cu")
    (tedit 623CE9CB)
    (at 136.95 65.1 90)
    (property "Sheetfile" "StrongStepper.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J2" (at -2 -4.35 90 unlocked) (layer "Eco1.User"))
    (fp_text value "Conn_01x04" (at -1.5 6 90 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at -5 0 90) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 15 "/MA2") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole circle (at -2.5 0.1 90) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 14 "/MA1") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole circle (at 0 0 90) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 11 "/MB2") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole circle (at 2.5 0 90) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 13 "/MB1") (pinfunction "Pin_4") (pintype "passive"))
  )
  (footprint "StronStepperFootprints:R_0603_1608MetricRect" (layer "F.Cu")
    (tedit 62395325)
    (at 92.6 81.4)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "StrongStepper.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R18" (at 0 1.4) (layer "Eco1.User"))
    (fp_text value "47R" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect (at -0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 34 "/SRAL") (pintype "passive"))
    (pad "2" smd rect (at 0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinSocket_1.27mm:PinSocket_1x02_P1.27mm_Vertical" (layer "F.Cu")
    (tedit 624E5899)
    (at 86.85 72)
    (descr "Through hole straight socket strip, 1x02, 1.27mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x02 1.27mm single row")
    (property "Sheetfile" "StrongStepper.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J4" (at -0.05 -1.35) (layer "Eco1.User"))
    (fp_text value "Conn_01x02_Male" (at 0.05 2.7) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0.635 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1 1) (drill 0.7) (layers *.Cu *.Mask)
      (net 50 "Net-(U1-Pad26)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 1.27) (size 1 1) (drill 0.7) (layers *.Cu *.Mask)
      (net 51 "Net-(U1-Pad27)") (pinfunction "Pin_2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinSocket_1.27mm.3dshapes/PinSocket_1x02_P1.27mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "StronStepperFootprints:TQFP-48-1EP_7x7mm_P0.5mm_EP5x5mm_ThermalVias" (layer "F.Cu")
    (tedit 623D41F2)
    (at 91.0556 67.5576 -90)
    (descr "TQFP, 48 Pin (https://www.trinamic.com/fileadmin/assets/Products/ICs_Documents/TMC2100_datasheet_Rev1.08.pdf (page 45)), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "TQFP QFP")
    (property "Sheetfile" "StrongStepper.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U1" (at 0 -5.85 90) (layer "Eco1.User"))
    (fp_text value "TMC5160A-TA" (at 0 5.85 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd rect (at -4.1625 -2.75 270) (size 1.475 0.24) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 24 "/HB1") (pinfunction "HB1") (pintype "output"))
    (pad "2" smd rect (at -4.1625 -2.25 270) (size 1.475 0.24) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 18 "/CB1") (pinfunction "CB1") (pintype "passive"))
    (pad "3" smd rect (at -4.1625 -1.75 270) (size 1.475 0.24) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 6 "Net-(C8-Pad2)") (pinfunction "12VOUT") (pintype "power_out"))
    (pad "4" smd rect (at -4.1625 -1.25 270) (size 1.475 0.24) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "/Vm") (pinfunction "VSA") (pintype "power_in"))
    (pad "5" smd rect (at -4.1625 -0.75 270) (size 1.475 0.24) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 10 "Net-(C9-Pad2)") (pinfunction "5VOUT") (pintype "power_out"))
    (pad "6" smd rect (at -4.1625 -0.25 270) (size 1.475 0.24) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "GNDA") (pintype "power_in"))
    (pad "7" smd rect (at -4.1625 0.25 270) (size 1.475 0.24) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 34 "/SRAL") (pinfunction "SRAL") (pintype "passive"))
    (pad "8" smd rect (at -4.1625 0.75 270) (size 1.475 0.24) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 33 "/SRAH") (pinfunction "SRAH") (pintype "passive"))
    (pad "9" smd rect (at -4.1625 1.25 270) (size 1.475 0.24) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 27 "/SRBH") (pinfunction "SRBH") (pintype "passive"))
    (pad "10" smd rect (at -4.1625 1.75 270) (size 1.475 0.24) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 28 "/SRBL") (pinfunction "SRBL") (pintype "passive"))
    (pad "11" smd rect (at -4.1625 2.25 270) (size 1.475 0.24) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "TST_MODE") (pintype "input"))
    (pad "12" smd rect (at -4.1625 2.75 270) (size 1.475 0.24) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "CLK") (pintype "input"))
    (pad "13" smd rect (at -2.75 4.1625 270) (size 0.24 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 43 "Net-(U1-Pad13)") (pinfunction "~{CS}/CFG3") (pintype "input"))
    (pad "14" smd rect (at -2.25 4.1625 270) (size 0.24 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 44 "Net-(U1-Pad14)") (pinfunction "SCK/CFG2") (pintype "input"))
    (pad "15" smd rect (at -1.75 4.1625 270) (size 0.24 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 45 "Net-(U1-Pad15)") (pinfunction "SDI/CFG1") (pintype "input"))
    (pad "16" smd rect (at -1.25 4.1625 270) (size 0.24 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 46 "Net-(U1-Pad16)") (pinfunction "SDO/CFG0") (pintype "bidirectional"))
    (pad "17" smd rect (at -0.75 4.1625 270) (size 0.24 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 47 "Net-(U1-Pad17)") (pinfunction "REFL/STEP") (pintype "input"))
    (pad "18" smd rect (at -0.25 4.1625 270) (size 0.24 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 48 "Net-(U1-Pad18)") (pinfunction "REFR/DIR") (pintype "input"))
    (pad "19" smd rect (at 0.25 4.1625 270) (size 0.24 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "GNDD") (pintype "power_in"))
    (pad "20" smd rect (at 0.75 4.1625 270) (size 0.24 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 16 "Net-(C19-Pad2)") (pinfunction "VCC_IO") (pintype "power_in"))
    (pad "21" smd rect (at 1.25 4.1625 270) (size 0.24 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 16 "Net-(C19-Pad2)") (pinfunction "SD_MODE") (pintype "input"))
    (pad "22" smd rect (at 1.75 4.1625 270) (size 0.24 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 16 "Net-(C19-Pad2)") (pinfunction "SPI_MODE") (pintype "input"))
    (pad "23" smd rect (at 2.25 4.1625 270) (size 0.24 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 7 "unconnected-(U1-Pad23)") (pinfunction "ENCB/DCEN/CFG4") (pintype "input+no_connect"))
    (pad "24" smd rect (at 2.75 4.1625 270) (size 0.24 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 8 "unconnected-(U1-Pad24)") (pinfunction "ENCA/DCIN/CFG5") (pintype "input+no_connect"))
    (pad "25" smd rect (at 4.1625 2.75 270) (size 1.475 0.24) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "unconnected-(U1-Pad25)") (pinfunction "ENCN/DCO/CFG6") (pintype "bidirectional+no_connect"))
    (pad "26" smd rect (at 4.1625 2.25 270) (size 1.475 0.24) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 50 "Net-(U1-Pad26)") (pinfunction "SWN/DIAG0") (pintype "bidirectional"))
    (pad "27" smd rect (at 4.1625 1.75 270) (size 1.475 0.24) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 51 "Net-(U1-Pad27)") (pinfunction "SWP/DIAG1") (pintype "bidirectional"))
    (pad "28" smd rect (at 4.1625 1.25 270) (size 1.475 0.24) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 49 "Net-(R12-Pad2)") (pinfunction "~{DRV_EN}") (pintype "input"))
    (pad "29" smd rect (at 4.1625 0.75 270) (size 1.475 0.24) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "Net-(C11-Pad2)") (pinfunction "VCC") (pintype "power_in"))
    (pad "30" smd rect (at 4.1625 0.25 270) (size 1.475 0.24) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "GNDD") (pintype "passive"))
    (pad "31" smd rect (at 4.1625 -0.25 270) (size 1.475 0.24) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "Net-(C7-Pad2)") (pinfunction "CPO") (pintype "passive"))
    (pad "32" smd rect (at 4.1625 -0.75 270) (size 1.475 0.24) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "Net-(C7-Pad1)") (pinfunction "CPI") (pintype "passive"))
    (pad "33" smd rect (at 4.1625 -1.25 270) (size 1.475 0.24) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "/Vm") (pinfunction "VS") (pintype "power_in"))
    (pad "34" smd rect (at 4.1625 -1.75 270) (size 1.475 0.24) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "Net-(C3-Pad2)") (pinfunction "VCP") (pintype "passive"))
    (pad "35" smd rect (at 4.1625 -2.25 270) (size 1.475 0.24) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 19 "/CA2") (pinfunction "CA2") (pintype "passive"))
    (pad "36" smd rect (at 4.1625 -2.75 270) (size 1.475 0.24) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 29 "/HA2") (pinfunction "HA2") (pintype "output"))
    (pad "37" smd rect (at 2.75 -4.1625 270) (size 0.24 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "/MA2") (pinfunction "BMA2") (pintype "passive"))
    (pad "38" smd rect (at 2.25 -4.1625 270) (size 0.24 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 31 "/LA2") (pinfunction "LA2") (pintype "output"))
    (pad "39" smd rect (at 1.75 -4.1625 270) (size 0.24 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 32 "/LA1") (pinfunction "LA1") (pintype "output"))
    (pad "40" smd rect (at 1.25 -4.1625 270) (size 0.24 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 14 "/MA1") (pinfunction "BMA1") (pintype "passive"))
    (pad "41" smd rect (at 0.75 -4.1625 270) (size 0.24 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 30 "/HA1") (pinfunction "HA1") (pintype "output"))
    (pad "42" smd rect (at 0.25 -4.1625 270) (size 0.24 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 20 "/CA1") (pinfunction "CA1") (pintype "passive"))
    (pad "43" smd rect (at -0.25 -4.1625 270) (size 0.24 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 17 "/CB2") (pinfunction "CB2") (pintype "passive"))
    (pad "44" smd rect (at -0.75 -4.1625 270) (size 0.24 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 23 "/HB2") (pinfunction "HB2") (pintype "output"))
    (pad "45" smd rect (at -1.25 -4.1625 270) (size 0.24 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 11 "/MB2") (pinfunction "BMB2") (pintype "passive"))
    (pad "46" smd rect (at -1.75 -4.1625 270) (size 0.24 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 25 "/LB2") (pinfunction "LB2") (pintype "output"))
    (pad "47" smd rect (at -2.25 -4.1625 270) (size 0.24 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 26 "/LB1") (pinfunction "LB1") (pintype "output"))
    (pad "48" smd rect (at -2.75 -4.1625 270) (size 0.24 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 13 "/MB1") (pinfunction "BMB1") (pintype "passive"))
    (pad "49" smd rect (at 0 0 270) (size 5 5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "EP") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_QFP.3dshapes/TQFP-48-1EP_7x7mm_P0.5mm_EP5x5mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x10_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 59FED5CC)
    (at 81.2 55.975)
    (descr "Through hole straight pin header, 1x10, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x10 2.54mm single row")
    (property "Sheetfile" "StrongStepper.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J3" (at 0 -2.33) (layer "Eco1.User"))
    (fp_text value "Conn_01x10_Male" (at 0 25.19) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 43 "Net-(U1-Pad13)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 44 "Net-(U1-Pad14)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 45 "Net-(U1-Pad15)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 46 "Net-(U1-Pad16)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 47 "Net-(U1-Pad17)") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole oval (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 48 "Net-(U1-Pad18)") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" thru_hole oval (at 0 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "Pin_8") (pintype "passive"))
    (pad "9" thru_hole oval (at 0 20.32) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 "Net-(C19-Pad2)") (pinfunction "Pin_9") (pintype "passive"))
    (pad "10" thru_hole oval (at 0 22.86) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 49 "Net-(R12-Pad2)") (pinfunction "Pin_10") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x10_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "StronStepperFootprints:C_0603_1608MetricRect" (layer "F.Cu")
    (tedit 623954C9)
    (at 134.05 75 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "StrongStepper.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C15" (at 0 -1.43 90) (layer "Eco1.User"))
    (fp_text value "1.0nF" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at -1.9 0 90) (layer "F.Fab"))
    (pad "1" smd rect (at -0.775 0 90) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd rect (at 0.775 0 90) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 14 "/MA1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "StronStepperFootprints:C_0603_1608MetricRect" (layer "F.Cu")
    (tedit 623954C9)
    (at 97.2 73.2 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "StrongStepper.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C17" (at 0 1.6 90) (layer "Eco1.User"))
    (fp_text value "220nF" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd rect (at -0.775 0 90) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 19 "/CA2") (pintype "passive"))
    (pad "2" smd rect (at 0.775 0 90) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "/MA2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "StronStepperFootprints:C_0603_1608MetricRect" (layer "F.Cu")
    (tedit 623954C9)
    (at 93.3 57.95 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "StrongStepper.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C5" (at -2.3 0.55) (layer "Eco1.User"))
    (fp_text value "100nF" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect (at -0.775 0 180) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd rect (at 0.775 0 180) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "/Vm") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "StronStepperFootprints:R_0603_1608MetricRect" (layer "F.Cu")
    (tedit 62395325)
    (at 93.425 54)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "StrongStepper.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R9" (at -2.425 0.2) (layer "Eco1.User"))
    (fp_text value "47R" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect (at -0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 28 "/SRBL") (pintype "passive"))
    (pad "2" smd rect (at 0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "StronStepperFootprints:C_0603_1608MetricRect" (layer "F.Cu")
    (tedit 623954C9)
    (at 88.75 76)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "StrongStepper.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C11" (at -2.35 -3.2) (layer "Eco1.User"))
    (fp_text value "470nF" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect (at -0.775 0) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd rect (at 0.775 0) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "Net-(C11-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "StronStepperFootprints:R_1206_3216MetricRect" (layer "F.Cu")
    (tedit 623953FC)
    (at 125.45 68.3125 -90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "StrongStepper.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R11" (at 0 -1.82 90) (layer "Eco1.User"))
    (fp_text value "10R" (at 0 1.82 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd rect (at -1.4625 0 270) (size 1.125 1.75) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 29 "/HA2") (pintype "passive"))
    (pad "2" smd rect (at 1.4625 0 270) (size 1.125 1.75) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 40 "/HA2G") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "StronStepperFootprints:R_1206_3216MetricRect" (layer "F.Cu")
    (tedit 623953FC)
    (at 121.7 68.15 -90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "StrongStepper.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R10" (at 0 -1.82 90) (layer "Eco1.User"))
    (fp_text value "10R" (at 0 1.82 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd rect (at -1.4625 0 270) (size 1.125 1.75) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 30 "/HA1") (pintype "passive"))
    (pad "2" smd rect (at 1.4625 0 270) (size 1.125 1.75) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 39 "/HA1G") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "StronStepperFootprints:C_0603_1608MetricRect" (layer "F.Cu")
    (tedit 623954C9)
    (at 138 57.875 -90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "StrongStepper.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C14" (at 0 -1.43 90) (layer "Eco1.User"))
    (fp_text value "1.0nF" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd rect (at -0.775 0 270) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd rect (at 0.775 0 270) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 13 "/MB1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "StronStepperFootprints:R_1206_3216MetricRect" (layer "F.Cu")
    (tedit 623953FC)
    (at 105.15 67.8 90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "StrongStepper.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R5" (at 0 1.65 90) (layer "Eco1.User"))
    (fp_text value "10R" (at 0 1.82 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd rect (at -1.4625 0 90) (size 1.125 1.75) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 25 "/LB2") (pintype "passive"))
    (pad "2" smd rect (at 1.4625 0 90) (size 1.125 1.75) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 38 "/LB2G") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "StronStepperFootprints:R_1206_3216MetricRect" (layer "F.Cu")
    (tedit 623953FC)
    (at 102.05 67.8 90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "StrongStepper.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R4" (at 0.2 1.55 90) (layer "Eco1.User"))
    (fp_text value "10R" (at 0 1.82 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd rect (at -1.4625 0 90) (size 1.125 1.75) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 26 "/LB1") (pintype "passive"))
    (pad "2" smd rect (at 1.4625 0 90) (size 1.125 1.75) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 37 "/LB1G") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "StronStepperFootprints:C_0603_1608MetricRect" (layer "F.Cu")
    (tedit 623954C9)
    (at 90.95 59.525 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "StrongStepper.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C9" (at 0 -1.43 90) (layer "Eco1.User"))
    (fp_text value "2.2uF" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd rect (at -0.775 0 90) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd rect (at 0.775 0 90) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 10 "Net-(C9-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "StronStepperFootprints:R_0603_1608MetricRect" (layer "F.Cu")
    (tedit 62395325)
    (at 92.45 79.6)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "StrongStepper.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R15" (at 2.75 0.2) (layer "Eco1.User"))
    (fp_text value "47R" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect (at -0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 33 "/SRAH") (pintype "passive"))
    (pad "2" smd rect (at 0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 22 "/LA") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "StronStepperFootprints:C_0603_1608MetricRect" (layer "F.Cu")
    (tedit 623954C9)
    (at 93.25 75.1 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "StrongStepper.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C3" (at 0 -1.43 90) (layer "Eco1.User"))
    (fp_text value "100nF" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd rect (at -0.775 0 90) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "/Vm") (pintype "passive"))
    (pad "2" smd rect (at 0.775 0 90) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "Net-(C3-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "StronStepperFootprints:C_0603_1608MetricRect" (layer "F.Cu")
    (tedit 623954C9)
    (at 97.3 61.95 -90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "StrongStepper.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C12" (at 0 -1.43 90) (layer "Eco1.User"))
    (fp_text value "220nF" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd rect (at -0.775 0 270) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 18 "/CB1") (pintype "passive"))
    (pad "2" smd rect (at 0.775 0 270) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 13 "/MB1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "StronStepperFootprints:R_1206_3216MetricRect" (layer "F.Cu")
    (tedit 623953FC)
    (at 108.4 67.5 -90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "StrongStepper.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R13" (at 0 -1.82 90) (layer "Eco1.User"))
    (fp_text value "10R" (at 0 1.82 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd rect (at -1.4625 0 270) (size 1.125 1.75) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 32 "/LA1") (pintype "passive"))
    (pad "2" smd rect (at 1.4625 0 270) (size 1.125 1.75) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 41 "/LA1G") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "StronStepperFootprints:C_0603_1608MetricRect" (layer "F.Cu")
    (tedit 623954C9)
    (at 92.6 77.6)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "StrongStepper.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C4" (at 2.4 0) (layer "Eco1.User"))
    (fp_text value "100nF" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect (at -0.775 0) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd rect (at 0.775 0) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "/Vm") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "StronStepperFootprints:C_0603_1608MetricRect" (layer "F.Cu")
    (tedit 623954C9)
    (at 135.4 57.8 -90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "StrongStepper.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C13" (at 0 -1.43 90) (layer "Eco1.User"))
    (fp_text value "1.0nF" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd rect (at -0.775 0 270) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd rect (at 0.775 0 270) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 11 "/MB2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "StronStepperFootprints:TDSON-8-2EP+5x6mm_P0.65_DUAL" (layer "F.Cu")
    (tedit 62340315)
    (at 123.25 75.95 90)
    (descr "TDSON-8-2EP_5x6mm_P0.65_DUAL StepUp generated footprint")
    (property "Sheetfile" "StrongStepper.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "Q3" (at 0 -4.1 90) (layer "Eco1.User"))
    (fp_text value "BSC150" (at 0 4.5 90) (layer "Eco1.User"))
    (pad "1" smd rect (at 1.905 -2.825 90) (size 0.65 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 14 "/MA1") (pinfunction "S1") (pintype "passive"))
    (pad "2" smd rect (at 0.635 -2.825 90) (size 0.65 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 39 "/HA1G") (pinfunction "G1") (pintype "passive"))
    (pad "3" smd rect (at -0.635 -2.825 90) (size 0.65 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "/MA2") (pinfunction "S2") (pintype "passive"))
    (pad "4" smd rect (at -1.905 -2.825 90) (size 0.65 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 40 "/HA2G") (pinfunction "G2") (pintype "passive"))
    (pad "5" smd custom (at -1.337 0 90) (size 0.2 0.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "/Vm") (pinfunction "D2") (pintype "passive") (zone_connect 2)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
            (xy 1.012 -1.575)
            (xy -1.013 -1.575)
            (xy -1.013 3.425)
            (xy -0.312 3.425)
            (xy -0.312 2.925)
            (xy 0.322 2.925)
            (xy 0.322 3.425)
            (xy 1.012 3.425)
          ) (width 0) (fill yes))
      ))
    (pad "8" smd custom (at 1.337 0 90) (size 0.2 0.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "/Vm") (pinfunction "D1") (pintype "passive") (zone_connect 2)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
            (xy -1.012 -1.575)
            (xy 1.013 -1.575)
            (xy 1.013 3.425)
            (xy 0.312 3.425)
            (xy 0.312 2.925)
            (xy -0.323 2.925)
            (xy -0.323 3.425)
            (xy -1.012 3.425)
          ) (width 0) (fill yes))
      ))
    (model "/home/jim/Shared/Projects/Circuits/StrongStepper/TDSON-8-2EP_5x6mm_P0.65_DUAL.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "StronStepperFootprints:R_0603_1608MetricRect" (layer "F.Cu")
    (tedit 62395325)
    (at 88.75 74.2 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "StrongStepper.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R3" (at 2.15 -1.8) (layer "Eco1.User"))
    (fp_text value "2R2" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect (at -0.825 0 180) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "Net-(C11-Pad2)") (pintype "passive"))
    (pad "2" smd rect (at 0.825 0 180) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 10 "Net-(C9-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "StronStepperFootprints:C_0603_1608MetricRect" (layer "F.Cu")
    (tedit 623954C9)
    (at 99.1 66.2 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "StrongStepper.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C10" (at -0.2 1.3 90) (layer "Eco1.User"))
    (fp_text value "220nF" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd rect (at -0.775 0 90) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 17 "/CB2") (pintype "passive"))
    (pad "2" smd rect (at 0.775 0 90) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 11 "/MB2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "StronStepperFootprints:C_1210_3225MetricRect" (layer "F.Cu")
    (tedit 6239551B)
    (at 85.525 81.925)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "StrongStepper.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C6" (at 0 -2.3) (layer "Eco1.User"))
    (fp_text value "4.7uF" (at 0 2.3) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect (at -1.475 0) (size 1.15 2.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd rect (at 1.475 0) (size 1.15 2.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "/Vm") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "StronStepperFootprints:R_1206_3216MetricRect" (layer "F.Cu")
    (tedit 623953FC)
    (at 111.65 67.8 -90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "StrongStepper.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R14" (at 0 -1.82 90) (layer "Eco1.User"))
    (fp_text value "10R" (at 0 1.82 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd rect (at -1.4625 0 270) (size 1.125 1.75) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 31 "/LA2") (pintype "passive"))
    (pad "2" smd rect (at 1.4625 0 270) (size 1.125 1.75) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 42 "/LA2G") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "StronStepperFootprints:C_0603_1608MetricRect" (layer "F.Cu")
    (tedit 623954C9)
    (at 93.95 59.75 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "StrongStepper.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C8" (at 0 -1.43) (layer "Eco1.User"))
    (fp_text value "2.2uF" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect (at -0.775 0 180) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd rect (at 0.775 0 180) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 6 "Net-(C8-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "StronStepperFootprints:MPT_05_254_2" (layer "F.Cu")
    (tedit 623CF317)
    (at 131.7 56.8)
    (property "Sheetfile" "StrongStepper.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J1" (at -0.95 -4.2 unlocked) (layer "Eco1.User"))
    (fp_text value "Conn_01x02" (at -0.7 4.5 unlocked) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at -2.54 -2.54) (size 1.1 1.1) (drill 1.1) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0 -2.54) (size 1.1 1.1) (drill 1.1) (layers F&B.Cu *.Mask))
    (pad "1" thru_hole circle (at 0 0) (size 1.8 1.8) (drill 1.1) (layers *.Cu *.Mask)
      (net 1 "/Vm") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole circle (at -2.54 0) (size 1.8 1.8) (drill 1.1) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "Pin_2") (pintype "passive"))
  )
  (footprint "StronStepperFootprints:C_0603_1608MetricRect" (layer "F.Cu")
    (tedit 623954C9)
    (at 91.45 74.85 -90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "StrongStepper.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C7" (at 0.10942 -3.35 90) (layer "Eco1.User"))
    (fp_text value "22nF" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd rect (at -0.775 0 270) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "Net-(C7-Pad1)") (pintype "passive"))
    (pad "2" smd rect (at 0.775 0 270) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "Net-(C7-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "StronStepperFootprints:C_0603_1608MetricRect" (layer "F.Cu")
    (tedit 623954C9)
    (at 99.15 69.95 -90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "StrongStepper.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C18" (at 0 -1.43 90) (layer "Eco1.User"))
    (fp_text value "220nF" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd rect (at -0.775 0 270) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 20 "/CA1") (pintype "passive"))
    (pad "2" smd rect (at 0.775 0 270) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 14 "/MA1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "StronStepperFootprints:C_0603_1608MetricRect" (layer "F.Cu")
    (tedit 623954C9)
    (at 137.3 77.625 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "StrongStepper.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C16" (at 0 -1.6 90) (layer "Eco1.User"))
    (fp_text value "1.0nF" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0.1 0 90) (layer "F.Fab"))
    (pad "1" smd rect (at -0.775 0 90) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd rect (at 0.775 0 90) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "/MA2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "StronStepperFootprints:R_0603_1608MetricRect" (layer "F.Cu")
    (tedit 62395325)
    (at 93.425 56.25)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "StrongStepper.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R8" (at -2.825 0.15) (layer "Eco1.User"))
    (fp_text value "47R" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect (at -0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 27 "/SRBH") (pintype "passive"))
    (pad "2" smd rect (at 0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 21 "/LB") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "StronStepperFootprints:R_1206_3216MetricRect" (layer "F.Cu")
    (tedit 623953FC)
    (at 114.8 68.0125 90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "StrongStepper.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R1" (at 0.0125 1.8 90) (layer "Eco1.User"))
    (fp_text value "10R" (at 0 1.82 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd rect (at -1.4625 0 90) (size 1.125 1.75) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 24 "/HB1") (pintype "passive"))
    (pad "2" smd rect (at 1.4625 0 90) (size 1.125 1.75) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 36 "/HB1G") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 86.6 54.6)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 -4.2) (layer "F.SilkS"))
    (fp_text value "MountingHole_3.2mm_M3" (at 0 4.2) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle locked (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (footprint "StronStepperFootprints:TDSON-8-2EP+5x6mm_P0.65_DUAL" (layer "F.Cu")
    (tedit 6244C67F)
    (at 123.4 60.45 90)
    (descr "TDSON-8-2EP_5x6mm_P0.65_DUAL StepUp generated footprint")
    (property "Sheetfile" "StrongStepper.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "Q1" (at 0 -4.1 90) (layer "Eco1.User"))
    (fp_text value "BSC150" (at 0 4.5 90) (layer "Eco1.User"))
    (pad "1" smd rect (at 1.905 -2.825 90) (size 0.65 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 13 "/MB1") (pinfunction "S1") (pintype "passive"))
    (pad "2" smd rect (at 0.635 -2.825 90) (size 0.65 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 36 "/HB1G") (pinfunction "G1") (pintype "passive"))
    (pad "3" smd rect (at -0.635 -2.825 90) (size 0.65 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 11 "/MB2") (pinfunction "S2") (pintype "passive"))
    (pad "4" smd rect (at -1.905 -2.825 90) (size 0.65 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "/HB2G") (pinfunction "G2") (pintype "passive"))
    (pad "5" smd custom (at -1.337 0 90) (size 0.2 0.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "/Vm") (pinfunction "D2") (pintype "passive") (zone_connect 2)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
            (xy 1.012 -1.575)
            (xy -1.013 -1.575)
            (xy -1.013 3.425)
            (xy -0.312 3.425)
            (xy -0.312 2.925)
            (xy 0.322 2.925)
            (xy 0.322 3.425)
            (xy 1.012 3.425)
          ) (width 0) (fill yes))
      ))
    (pad "8" smd custom (at 1.337 0 90) (size 0.2 0.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "/Vm") (pinfunction "D1") (pintype "passive") (zone_connect 2)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
            (xy -1.012 -1.575)
            (xy 1.013 -1.575)
            (xy 1.013 3.425)
            (xy 0.312 3.425)
            (xy 0.312 2.925)
            (xy -0.323 2.925)
            (xy -0.323 3.425)
            (xy -1.012 3.425)
          ) (width 0) (fill yes))
      ))
    (model "/home/jim/Shared/Projects/Circuits/StrongStepper/TDSON-8-2EP_5x6mm_P0.65_DUAL.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "StronStepperFootprints:C_0603_1608MetricRect" (layer "F.Cu")
    (tedit 623954C9)
    (at 84.95 75.375 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "StrongStepper.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C19" (at 0 -1.43 90) (layer "Eco1.User"))
    (fp_text value "100nF" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd rect (at -0.775 0 90) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd rect (at 0.775 0 90) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 16 "Net-(C19-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "StronStepperFootprints:R_1206_3216MetricRect" (layer "F.Cu")
    (tedit 623953FC)
    (at 118.15 68.2 90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "StrongStepper.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R2" (at 0 1.65 90) (layer "Eco1.User"))
    (fp_text value "10R" (at 0 1.82 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd rect (at -1.4625 0 90) (size 1.125 1.75) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 23 "/HB2") (pintype "passive"))
    (pad "2" smd rect (at 1.4625 0 90) (size 1.125 1.75) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "/HB2G") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "StronStepperFootprints:R_2512_6332MetricRect" (layer "B.Cu")
    (tedit 62395456)
    (at 100.4 54.6 180)
    (descr "Resistor SMD 2512 (6332 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "StrongStepper.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R7" (at 0 0) (layer "B.SilkS"))
    (fp_text value "0R10" (at 0 -2.62) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd rect (at -2.9625 0 180) (size 1.225 3.35) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 21 "/LB") (pintype "passive"))
    (pad "2" smd rect (at 2.9625 0 180) (size 1.225 3.35) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_2512_6332Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:CP_Radial_D12.5mm_P5.00mm" (layer "B.Cu")
    (tedit 5AE50EF1)
    (at 123.4 54.2 180)
    (descr "CP, Radial series, Radial, pin pitch=5.00mm, , diameter=12.5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 5.00mm  diameter 12.5mm Electrolytic Capacitor")
    (property "Sheetfile" "StrongStepper.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C2" (at 2.5 7.5) (layer "B.SilkS"))
    (fp_text value "220uF" (at 2.5 -7.5) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 0) (layer "B.Fab"))
    (pad "1" thru_hole rect (at 0 0 180) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 1 "/Vm") (pintype "passive"))
    (pad "2" thru_hole circle (at 5 0 180) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_D12.5mm_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "StronStepperFootprints:R_2512_6332MetricRect" (layer "B.Cu")
    (tedit 62395456)
    (at 100.15 81.9 180)
    (descr "Resistor SMD 2512 (6332 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "StrongStepper.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R16" (at 0 0.1) (layer "B.SilkS"))
    (fp_text value "0R10" (at 0 -2.62) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd rect (at -2.9625 0 180) (size 1.225 3.35) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 22 "/LA") (pintype "passive"))
    (pad "2" smd rect (at 2.9625 0 180) (size 1.225 3.35) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_2512_6332Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "StronStepperFootprints:R_2512_6332MetricRect" (layer "B.Cu")
    (tedit 62395456)
    (at 100.15 77.4 180)
    (descr "Resistor SMD 2512 (6332 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "StrongStepper.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R17" (at 0.35 0) (layer "B.SilkS"))
    (fp_text value "0R10" (at 0 -2.62) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd rect (at -2.9625 0 180) (size 1.225 3.35) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 22 "/LA") (pintype "passive"))
    (pad "2" smd rect (at 2.9625 0 180) (size 1.225 3.35) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_2512_6332Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:CP_Radial_D12.5mm_P5.00mm" (layer "B.Cu")
    (tedit 5AE50EF1)
    (at 123.523959 82 180)
    (descr "CP, Radial series, Radial, pin pitch=5.00mm, , diameter=12.5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 5.00mm  diameter 12.5mm Electrolytic Capacitor")
    (property "Sheetfile" "StrongStepper.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C1" (at 2.5 7.5) (layer "B.SilkS"))
    (fp_text value "220uF" (at 2.5 -7.5) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 0) (layer "B.Fab"))
    (pad "1" thru_hole rect (at 0 0 180) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 1 "/Vm") (pintype "passive"))
    (pad "2" thru_hole circle (at 5 0 180) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_D12.5mm_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "StronStepperFootprints:R_2512_6332MetricRect" (layer "B.Cu")
    (tedit 62395456)
    (at 100.4 58.9 180)
    (descr "Resistor SMD 2512 (6332 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "StrongStepper.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R6" (at 0 0.1) (layer "B.SilkS"))
    (fp_text value "0R10" (at 0 -2.62) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd rect (at -2.9625 0 180) (size 1.225 3.35) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 21 "/LB") (pintype "passive"))
    (pad "2" smd rect (at 2.9625 0 180) (size 1.225 3.35) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_2512_6332Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_rect (start 140.8 52.2) (end 79.2 84.4) (layer "Edge.Cuts") (width 0.1) (fill none))
  (gr_text "DIR" (at 83.6 71.2) (layer "F.SilkS"))
  (gr_text "/CS" (at 81.8 53.8) (layer "F.SilkS"))
  (gr_text "MA1" (at 128.4 67.6) (layer "F.SilkS"))
  (gr_text "SCK" (at 83.6 58.6) (layer "F.SilkS"))
  (gr_text "GND" (at 126.2 54.2) (layer "F.SilkS"))
  (gr_text "MA2" (at 128.4 70) (layer "F.SilkS"))
  (gr_text "/EN" (at 81.2 81.2) (layer "F.SilkS"))
  (gr_text "4/12/22" (at 131.8 80.6) (layer "F.SilkS"))
  (gr_text "MB1" (at 128.4 62.6) (layer "F.SilkS"))
  (gr_text "SDO" (at 83.6 63.4) (layer "F.SilkS"))
  (gr_text "VM" (at 134.4 54.4) (layer "F.SilkS"))
  (gr_text "GND" (at 83.6 73.2) (layer "F.SilkS"))
  (gr_text "SDI" (at 83.6 61) (layer "F.SilkS"))
  (gr_text "jkl" (at 131.6 82.6) (layer "F.SilkS"))
  (gr_text "BEEFY STEPPER" (at 106 54.6) (layer "F.SilkS"))
  (gr_text "MB2" (at 128.4 65.2) (layer "F.SilkS"))
  (gr_text "GND" (at 83.6 66) (layer "F.SilkS"))
  (gr_text "VCC" (at 83.8 77.8) (layer "F.SilkS"))
  (gr_text "STEP" (at 83.8 68.8) (layer "F.SilkS"))
  (zone (net 13) (net_name "/MB1") (layer "F.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.128))
    (min_thickness 0.128) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.254) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 121.2 60.1)
        (xy 108.45 60.05)
        (xy 108.4 55.4)
        (xy 121.15 55.4)
      )
    )
  )
  (zone (net 11) (net_name "/MB2") (layer "F.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.128))
    (min_thickness 0.128) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.254) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 121.2 60.75)
        (xy 121.2 64.75)
        (xy 108.45 64.55)
        (xy 108.45 60.7)
      )
    )
  )
  (zone (net 14) (net_name "/MA1") (layer "F.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.128))
    (min_thickness 0.128) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.254) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 121.15 75.7)
        (xy 109.1 75.55)
        (xy 109.094125 71.295838)
        (xy 121.044125 71.245838)
      )
    )
  )
  (zone (net 15) (net_name "/MA2") (layer "F.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.128))
    (min_thickness 0.128) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.254) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 121.1 80.45)
        (xy 109.1 80.5)
        (xy 109 76.15)
        (xy 121.1 76.15)
      )
    )
  )
  (zone (net 22) (net_name "/LA") (layer "F.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.128))
    (min_thickness 0.128) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.254) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 108.431763 84.070093)
        (xy 101.331763 84.220093)
        (xy 101.3 71.6)
        (xy 108.4 71.6)
      )
    )
  )
  (zone (net 21) (net_name "/LB") (layer "F.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.128))
    (min_thickness 0.128) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.254) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 107.85 64.2)
        (xy 100.65 64.25)
        (xy 100.65 52.4)
        (xy 107.85 52.4)
      )
    )
  )
  (zone (net 1) (net_name "/Vm") (layer "F.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.128))
    (min_thickness 0.128) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.254) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 133.355512 55.363476)
        (xy 133.382826 80.8983)
        (xy 121.686465 80.949152)
        (xy 121.709151 55.314328)
      )
    )
  )
  (zone (net 2) (net_name "GND") (layer "In1.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.128))
    (min_thickness 0.128) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.254) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 140.6 84.2)
        (xy 79.4 84.4)
        (xy 79.4 52.4)
        (xy 140.6 52.4)
      )
    )
  )
  (zone (net 1) (net_name "/Vm") (layer "In2.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.128))
    (min_thickness 0.128) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.254) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 140.6 84.2)
        (xy 79.4 84.2)
        (xy 79.4 52.4)
        (xy 140.6 52.4)
      )
    )
  )
  (zone (net 21) (net_name "/LB") (layer "B.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.128))
    (min_thickness 0.128) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.254) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 107.945914 64.097062)
        (xy 100.495914 64.247062)
        (xy 100.65 52.4)
        (xy 107.85 52.4)
      )
    )
  )
  (zone (net 15) (net_name "/MA2") (layer "B.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.128))
    (min_thickness 0.128) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.254) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 138.7 80.4)
        (xy 109.05 80.5)
        (xy 109.05 76.2)
        (xy 135.65 76.15)
        (xy 135.590333 69.200311)
        (xy 138.690333 69.100311)
      )
    )
  )
  (zone (net 13) (net_name "/MB1") (layer "B.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.128))
    (min_thickness 0.128) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.254) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 139.097016 63.699955)
        (xy 135.547054 63.65272)
        (xy 135.500038 60.252765)
        (xy 108.35 60.05)
        (xy 108.4 55.35)
        (xy 138.8 55.35)
      )
    )
  )
  (zone (net 14) (net_name "/MA1") (layer "B.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.128))
    (min_thickness 0.128) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.254) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 139.004347 68.646725)
        (xy 135.054347 68.746725)
        (xy 135.15 75.7)
        (xy 109.05 75.55)
        (xy 109.122961 71.405338)
        (xy 128.299766 71.401185)
        (xy 128.3 66.549953)
        (xy 139 66.55)
      )
    )
  )
  (zone (net 22) (net_name "/LA") (layer "B.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.128))
    (min_thickness 0.128) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.254) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 108.449688 84.194755)
        (xy 101.299688 84.144755)
        (xy 101.25 71.65)
        (xy 108.45 71.65)
      )
    )
  )
  (zone (net 11) (net_name "/MB2") (layer "B.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.128))
    (min_thickness 0.128) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.254) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 135.1 60.8)
        (xy 135.156951 63.925492)
        (xy 139.106951 64.025492)
        (xy 139.048002 66.245898)
        (xy 128.255397 66.144369)
        (xy 128.257395 64.848471)
        (xy 108.3 64.6)
        (xy 108.4 60.7)
      )
    )
  )
)
