(kicad_pcb (version 20211014) (generator pcbnew)
  (general
    (thickness 0.9)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 0.81) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "+5V")
  (net 2 "GND")
  (net 3 "Net-(D1-Pad2)")
  (net 4 "Net-(D2-Pad2)")
  (net 5 "Net-(D3-Pad2)")
  (net 6 "Net-(D4-Pad2)")
  (net 7 "Net-(D5-Pad2)")
  (net 8 "DIN")
  (net 9 "Net-(D6-Pad2)")
  (net 10 "Net-(D7-Pad2)")
  (net 11 "Net-(D10-Pad4)")
  (net 12 "Net-(D10-Pad2)")
  (net 13 "Net-(D11-Pad2)")
  (net 14 "Net-(D19-Pad2)")
  (net 15 "Net-(D12-Pad2)")
  (net 16 "Net-(D13-Pad2)")
  (net 17 "Net-(D14-Pad2)")
  (net 18 "Net-(D15-Pad2)")
  (net 19 "Net-(D16-Pad2)")
  (net 20 "Net-(D17-Pad2)")
  (net 21 "Net-(D18-Pad2)")
  (net 22 "DOUT")
  (net 23 "Net-(D8-Pad2)")
  (footprint "footprint_lib:XL-0807RGBC-WS2812B" (layer "F.Cu")
    (tedit 0)
    (at 105.7 109.5)
    (property "Sheetfile" "drone_LED_strip.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D6" (at -0.2 -1.6 unlocked) (layer "F.SilkS") hide)
    (fp_text value "WS2812B" (at 10.5 -10 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 10.5 -8.5 unlocked) (layer "F.Fab"))
    (pad "1" smd roundrect (at 0.75 -0.45) (size 0.6 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+5V") (pinfunction "VDD") (pintype "power_in"))
    (pad "2" smd roundrect (at -0.75 -0.45) (size 0.6 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 9 "Net-(D6-Pad2)") (pinfunction "DOUT") (pintype "output"))
    (pad "3" smd roundrect (at -0.75 0.45) (size 0.6 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "VSS") (pintype "power_in"))
    (pad "4" smd roundrect (at 0.75 0.45) (size 0.6 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 7 "Net-(D5-Pad2)") (pinfunction "DIN") (pintype "input"))
  )
  (footprint "footprint_lib:XL-0807RGBC-WS2812B" (layer "F.Cu")
    (tedit 0)
    (at 105.7 111.9 180)
    (property "Sheetfile" "drone_LED_strip.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D15" (at 10.5 -11.5 180 unlocked) (layer "F.SilkS") hide)
    (fp_text value "WS2812B" (at 10.5 -10 180 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 10.5 -8.5 180 unlocked) (layer "F.Fab"))
    (pad "1" smd roundrect (at 0.75 -0.45 180) (size 0.6 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+5V") (pinfunction "VDD") (pintype "power_in"))
    (pad "2" smd roundrect (at -0.75 -0.45 180) (size 0.6 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 18 "Net-(D15-Pad2)") (pinfunction "DOUT") (pintype "output"))
    (pad "3" smd roundrect (at -0.75 0.45 180) (size 0.6 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "VSS") (pintype "power_in"))
    (pad "4" smd roundrect (at 0.75 0.45 180) (size 0.6 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 17 "Net-(D14-Pad2)") (pinfunction "DIN") (pintype "input"))
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 115.2 111.9 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "drone_LED_strip.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C8" (at 0 -1.16 90) (layer "F.SilkS") hide)
    (fp_text value "C" (at 0 1.16 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.48 0 90) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+5V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.48 0 90) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprint_lib:XL-0807RGBC-WS2812B" (layer "F.Cu")
    (tedit 0)
    (at 94.3 109.5)
    (property "Sheetfile" "drone_LED_strip.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D9" (at 10.5 -11.5 unlocked) (layer "F.SilkS") hide)
    (fp_text value "WS2812B" (at 10.5 -10 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 10.5 -8.5 unlocked) (layer "F.Fab"))
    (pad "1" smd roundrect (at 0.75 -0.45) (size 0.6 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+5V") (pinfunction "VDD") (pintype "power_in"))
    (pad "2" smd roundrect (at -0.75 -0.45) (size 0.6 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 11 "Net-(D10-Pad4)") (pinfunction "DOUT") (pintype "output"))
    (pad "3" smd roundrect (at -0.75 0.45) (size 0.6 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "VSS") (pintype "power_in"))
    (pad "4" smd roundrect (at 0.75 0.45) (size 0.6 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 23 "Net-(D8-Pad2)") (pinfunction "DIN") (pintype "input"))
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 96.2 109.5 -90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "drone_LED_strip.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C17" (at 0 -1.16 90) (layer "F.SilkS") hide)
    (fp_text value "C" (at 0 1.16 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.48 0 270) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+5V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.48 0 270) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 111.4 111.9 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "drone_LED_strip.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C18" (at 0 -1.16 90) (layer "F.SilkS") hide)
    (fp_text value "C" (at 0 1.16 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.48 0 90) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+5V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.48 0 90) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_1.00mm:PinHeader_1x04_P1.00mm_Horizontal" (layer "F.Cu")
    (tedit 59FED737)
    (at 129.9 109.2)
    (descr "Through hole angled pin header, 1x04, 1.00mm pitch, 2.0mm pin length, single row")
    (tags "Through hole angled pin header THT 1x04 1.00mm single row")
    (property "Sheetfile" "drone_LED_strip.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J1" (at 1.375 -1.5) (layer "F.SilkS") hide)
    (fp_text value "Conn_01x04" (at 1.375 4.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0.75 1.5 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 "+5V") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 1) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 8 "DIN") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 2) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 22 "DOUT") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 3) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "Pin_4") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_1.00mm.3dshapes/PinHeader_1x04_P1.00mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 92.4 111.9 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "drone_LED_strip.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C13" (at 0 -1.16 90) (layer "F.SilkS") hide)
    (fp_text value "C" (at 0 1.16 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.48 0 90) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+5V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.48 0 90) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprint_lib:XL-0807RGBC-WS2812B" (layer "F.Cu")
    (tedit 0)
    (at 94.3 111.9 180)
    (property "Sheetfile" "drone_LED_strip.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D12" (at 10.5 -11.5 180 unlocked) (layer "F.SilkS") hide)
    (fp_text value "WS2812B" (at 10.5 -10 180 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 10.5 -8.5 180 unlocked) (layer "F.Fab"))
    (pad "1" smd roundrect (at 0.75 -0.45 180) (size 0.6 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+5V") (pinfunction "VDD") (pintype "power_in"))
    (pad "2" smd roundrect (at -0.75 -0.45 180) (size 0.6 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 15 "Net-(D12-Pad2)") (pinfunction "DOUT") (pintype "output"))
    (pad "3" smd roundrect (at -0.75 0.45 180) (size 0.6 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "VSS") (pintype "power_in"))
    (pad "4" smd roundrect (at 0.75 0.45 180) (size 0.6 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 13 "Net-(D11-Pad2)") (pinfunction "DIN") (pintype "input"))
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 103.8 109.5 -90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "drone_LED_strip.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C6" (at 1.9 0.3 90) (layer "F.SilkS") hide)
    (fp_text value "C" (at 0 1.16 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.48 0 270) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+5V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.48 0 270) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 96.2 111.9 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "drone_LED_strip.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C20" (at 0 -1.16 90) (layer "F.SilkS") hide)
    (fp_text value "C" (at 0 1.16 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.48 0 90) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+5V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.48 0 90) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprint_lib:XL-0807RGBC-WS2812B" (layer "F.Cu")
    (tedit 0)
    (at 101.9 109.5)
    (property "Sheetfile" "drone_LED_strip.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D7" (at 10.5 -11.5 unlocked) (layer "F.SilkS") hide)
    (fp_text value "WS2812B" (at 10.5 -10 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 10.5 -8.5 unlocked) (layer "F.Fab"))
    (pad "1" smd roundrect (at 0.75 -0.45) (size 0.6 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+5V") (pinfunction "VDD") (pintype "power_in"))
    (pad "2" smd roundrect (at -0.75 -0.45) (size 0.6 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 10 "Net-(D7-Pad2)") (pinfunction "DOUT") (pintype "output"))
    (pad "3" smd roundrect (at -0.75 0.45) (size 0.6 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "VSS") (pintype "power_in"))
    (pad "4" smd roundrect (at 0.75 0.45) (size 0.6 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 9 "Net-(D6-Pad2)") (pinfunction "DIN") (pintype "input"))
  )
  (footprint "footprint_lib:XL-0807RGBC-WS2812B" (layer "F.Cu")
    (tedit 0)
    (at 124.7 111.9 180)
    (property "Sheetfile" "drone_LED_strip.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D20" (at 10.5 -11.5 180 unlocked) (layer "F.SilkS") hide)
    (fp_text value "WS2812B" (at 10.5 -10 180 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 10.5 -8.5 180 unlocked) (layer "F.Fab"))
    (pad "1" smd roundrect (at 0.75 -0.45 180) (size 0.6 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+5V") (pinfunction "VDD") (pintype "power_in"))
    (pad "2" smd roundrect (at -0.75 -0.45 180) (size 0.6 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "DOUT") (pinfunction "DOUT") (pintype "output"))
    (pad "3" smd roundrect (at -0.75 0.45 180) (size 0.6 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "VSS") (pintype "power_in"))
    (pad "4" smd roundrect (at 0.75 0.45 180) (size 0.6 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 14 "Net-(D19-Pad2)") (pinfunction "DIN") (pintype "input"))
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 115.2 109.5 -90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "drone_LED_strip.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C3" (at 0 -1.16 -90) (layer "F.SilkS") hide)
    (fp_text value "C" (at 0 1.16 -90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 -90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.48 0 270) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+5V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.48 0 270) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 88.6 109.5 -90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "drone_LED_strip.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C12" (at 0 -1.16 90) (layer "F.SilkS") hide)
    (fp_text value "C" (at 0 1.16 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.48 0 270) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+5V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.48 0 270) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprint_lib:XL-0807RGBC-WS2812B" (layer "F.Cu")
    (tedit 0)
    (at 109.5 111.9 180)
    (property "Sheetfile" "drone_LED_strip.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D16" (at 10.5 -11.5 180 unlocked) (layer "F.SilkS") hide)
    (fp_text value "WS2812B" (at 10.5 -10 180 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 10.5 -8.5 180 unlocked) (layer "F.Fab"))
    (pad "1" smd roundrect (at 0.75 -0.45 180) (size 0.6 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+5V") (pinfunction "VDD") (pintype "power_in"))
    (pad "2" smd roundrect (at -0.75 -0.45 180) (size 0.6 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 19 "Net-(D16-Pad2)") (pinfunction "DOUT") (pintype "output"))
    (pad "3" smd roundrect (at -0.75 0.45 180) (size 0.6 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "VSS") (pintype "power_in"))
    (pad "4" smd roundrect (at 0.75 0.45 180) (size 0.6 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 18 "Net-(D15-Pad2)") (pinfunction "DIN") (pintype "input"))
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 103.8 111.9 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "drone_LED_strip.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C15" (at 0 -1.16 90) (layer "F.SilkS") hide)
    (fp_text value "C" (at 0 1.16 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.48 0 90) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+5V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.48 0 90) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprint_lib:XL-0807RGBC-WS2812B" (layer "F.Cu")
    (tedit 0)
    (at 120.9 111.9 180)
    (property "Sheetfile" "drone_LED_strip.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D19" (at 10.5 -11.5 180 unlocked) (layer "F.SilkS") hide)
    (fp_text value "WS2812B" (at 10.5 -10 180 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 10.5 -8.5 180 unlocked) (layer "F.Fab"))
    (pad "1" smd roundrect (at 0.75 -0.45 180) (size 0.6 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+5V") (pinfunction "VDD") (pintype "power_in"))
    (pad "2" smd roundrect (at -0.75 -0.45 180) (size 0.6 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 14 "Net-(D19-Pad2)") (pinfunction "DOUT") (pintype "output"))
    (pad "3" smd roundrect (at -0.75 0.45 180) (size 0.6 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "VSS") (pintype "power_in"))
    (pad "4" smd roundrect (at 0.75 0.45 180) (size 0.6 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 21 "Net-(D18-Pad2)") (pinfunction "DIN") (pintype "input"))
  )
  (footprint "footprint_lib:XL-0807RGBC-WS2812B" (layer "F.Cu")
    (tedit 0)
    (at 117.1 109.5)
    (property "Sheetfile" "drone_LED_strip.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D3" (at -0.2 -1.6 unlocked) (layer "F.SilkS") hide)
    (fp_text value "WS2812B" (at 10.5 -10 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 10.5 -8.5 unlocked) (layer "F.Fab"))
    (pad "1" smd roundrect (at 0.75 -0.45) (size 0.6 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+5V") (pinfunction "VDD") (pintype "power_in"))
    (pad "2" smd roundrect (at -0.75 -0.45) (size 0.6 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "Net-(D3-Pad2)") (pinfunction "DOUT") (pintype "output"))
    (pad "3" smd roundrect (at -0.75 0.45) (size 0.6 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "VSS") (pintype "power_in"))
    (pad "4" smd roundrect (at 0.75 0.45) (size 0.6 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "Net-(D2-Pad2)") (pinfunction "DIN") (pintype "input"))
  )
  (footprint "footprint_lib:XL-0807RGBC-WS2812B" (layer "F.Cu")
    (tedit 0)
    (at 124.7 109.5)
    (property "Sheetfile" "drone_LED_strip.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D1" (at -0.2 -1.6 unlocked) (layer "F.SilkS") hide)
    (fp_text value "WS2812B" (at 10.5 -10 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 10.5 -8.5 unlocked) (layer "F.Fab"))
    (pad "1" smd roundrect (at 0.75 -0.45) (size 0.6 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+5V") (pinfunction "VDD") (pintype "power_in"))
    (pad "2" smd roundrect (at -0.75 -0.45) (size 0.6 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "Net-(D1-Pad2)") (pinfunction "DOUT") (pintype "output"))
    (pad "3" smd roundrect (at -0.75 0.45) (size 0.6 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "VSS") (pintype "power_in"))
    (pad "4" smd roundrect (at 0.75 0.45) (size 0.6 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 8 "DIN") (pinfunction "DIN") (pintype "input"))
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 88.6 111.9 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "drone_LED_strip.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C11" (at 0 -1.16 90) (layer "F.SilkS") hide)
    (fp_text value "C" (at 0 1.16 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.48 0 90) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+5V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.48 0 90) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprint_lib:XL-0807RGBC-WS2812B" (layer "F.Cu")
    (tedit 0)
    (at 109.5 109.5)
    (property "Sheetfile" "drone_LED_strip.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D5" (at -0.2 -1.6 unlocked) (layer "F.SilkS") hide)
    (fp_text value "WS2812B" (at 10.5 -10 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 10.5 -8.5 unlocked) (layer "F.Fab"))
    (pad "1" smd roundrect (at 0.75 -0.45) (size 0.6 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+5V") (pinfunction "VDD") (pintype "power_in"))
    (pad "2" smd roundrect (at -0.75 -0.45) (size 0.6 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 7 "Net-(D5-Pad2)") (pinfunction "DOUT") (pintype "output"))
    (pad "3" smd roundrect (at -0.75 0.45) (size 0.6 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "VSS") (pintype "power_in"))
    (pad "4" smd roundrect (at 0.75 0.45) (size 0.6 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 6 "Net-(D4-Pad2)") (pinfunction "DIN") (pintype "input"))
  )
  (footprint "footprint_lib:XL-0807RGBC-WS2812B" (layer "F.Cu")
    (tedit 0)
    (at 113.3 109.5)
    (property "Sheetfile" "drone_LED_strip.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D4" (at -0.2 -1.6 unlocked) (layer "F.SilkS") hide)
    (fp_text value "WS2812B" (at 10.5 -10 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 10.5 -8.5 unlocked) (layer "F.Fab"))
    (pad "1" smd roundrect (at 0.75 -0.45) (size 0.6 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+5V") (pinfunction "VDD") (pintype "power_in"))
    (pad "2" smd roundrect (at -0.75 -0.45) (size 0.6 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 6 "Net-(D4-Pad2)") (pinfunction "DOUT") (pintype "output"))
    (pad "3" smd roundrect (at -0.75 0.45) (size 0.6 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "VSS") (pintype "power_in"))
    (pad "4" smd roundrect (at 0.75 0.45) (size 0.6 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "Net-(D3-Pad2)") (pinfunction "DIN") (pintype "input"))
  )
  (footprint "footprint_lib:XL-0807RGBC-WS2812B" (layer "F.Cu")
    (tedit 0)
    (at 98.1 111.9 180)
    (property "Sheetfile" "drone_LED_strip.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D13" (at 10.5 -11.5 180 unlocked) (layer "F.SilkS") hide)
    (fp_text value "WS2812B" (at 10.5 -10 180 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 10.5 -8.5 180 unlocked) (layer "F.Fab"))
    (pad "1" smd roundrect (at 0.75 -0.45 180) (size 0.6 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+5V") (pinfunction "VDD") (pintype "power_in"))
    (pad "2" smd roundrect (at -0.75 -0.45 180) (size 0.6 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 16 "Net-(D13-Pad2)") (pinfunction "DOUT") (pintype "output"))
    (pad "3" smd roundrect (at -0.75 0.45 180) (size 0.6 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "VSS") (pintype "power_in"))
    (pad "4" smd roundrect (at 0.75 0.45 180) (size 0.6 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 15 "Net-(D12-Pad2)") (pinfunction "DIN") (pintype "input"))
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 100 111.9 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "drone_LED_strip.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C14" (at 0 -1.16 90) (layer "F.SilkS") hide)
    (fp_text value "C" (at 0 1.16 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.48 0 90) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+5V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.48 0 90) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprint_lib:XL-0807RGBC-WS2812B" (layer "F.Cu")
    (tedit 0)
    (at 90.5 111.9 180)
    (property "Sheetfile" "drone_LED_strip.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D11" (at 10.5 -11.5 180 unlocked) (layer "F.SilkS") hide)
    (fp_text value "WS2812B" (at 10.5 -10 180 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 10.5 -8.5 180 unlocked) (layer "F.Fab"))
    (pad "1" smd roundrect (at 0.75 -0.45 180) (size 0.6 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+5V") (pinfunction "VDD") (pintype "power_in"))
    (pad "2" smd roundrect (at -0.75 -0.45 180) (size 0.6 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 13 "Net-(D11-Pad2)") (pinfunction "DOUT") (pintype "output"))
    (pad "3" smd roundrect (at -0.75 0.45 180) (size 0.6 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "VSS") (pintype "power_in"))
    (pad "4" smd roundrect (at 0.75 0.45 180) (size 0.6 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 12 "Net-(D10-Pad2)") (pinfunction "DIN") (pintype "input"))
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 119 109.5 -90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "drone_LED_strip.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C2" (at 0 -1.16 -90) (layer "F.SilkS") hide)
    (fp_text value "C" (at 0 1.16 -90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 -90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.48 0 270) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+5V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.48 0 270) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprint_lib:XL-0807RGBC-WS2812B" (layer "F.Cu")
    (tedit 0)
    (at 113.3 111.9 180)
    (property "Sheetfile" "drone_LED_strip.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D17" (at 10.5 -11.5 180 unlocked) (layer "F.SilkS") hide)
    (fp_text value "WS2812B" (at 10.5 -10 180 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 10.5 -8.5 180 unlocked) (layer "F.Fab"))
    (pad "1" smd roundrect (at 0.75 -0.45 180) (size 0.6 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+5V") (pinfunction "VDD") (pintype "power_in"))
    (pad "2" smd roundrect (at -0.75 -0.45 180) (size 0.6 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 20 "Net-(D17-Pad2)") (pinfunction "DOUT") (pintype "output"))
    (pad "3" smd roundrect (at -0.75 0.45 180) (size 0.6 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "VSS") (pintype "power_in"))
    (pad "4" smd roundrect (at 0.75 0.45 180) (size 0.6 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 19 "Net-(D16-Pad2)") (pinfunction "DIN") (pintype "input"))
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 92.4 109.5 -90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "drone_LED_strip.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C10" (at 0 -1.16 90) (layer "F.SilkS") hide)
    (fp_text value "C" (at 0 1.16 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.48 0 270) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+5V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.48 0 270) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 122.8 109.5 -90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "drone_LED_strip.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C1" (at 0 -1.16 -90) (layer "F.SilkS") hide)
    (fp_text value "C" (at 0 1.16 -90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 -90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.48 0 270) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+5V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.48 0 270) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprint_lib:XL-0807RGBC-WS2812B" (layer "F.Cu")
    (tedit 0)
    (at 117.1 111.9 180)
    (property "Sheetfile" "drone_LED_strip.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D18" (at 10.5 -11.5 180 unlocked) (layer "F.SilkS") hide)
    (fp_text value "WS2812B" (at 10.5 -10 180 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 10.5 -8.5 180 unlocked) (layer "F.Fab"))
    (pad "1" smd roundrect (at 0.75 -0.45 180) (size 0.6 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+5V") (pinfunction "VDD") (pintype "power_in"))
    (pad "2" smd roundrect (at -0.75 -0.45 180) (size 0.6 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 21 "Net-(D18-Pad2)") (pinfunction "DOUT") (pintype "output"))
    (pad "3" smd roundrect (at -0.75 0.45 180) (size 0.6 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "VSS") (pintype "power_in"))
    (pad "4" smd roundrect (at 0.75 0.45 180) (size 0.6 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 20 "Net-(D17-Pad2)") (pinfunction "DIN") (pintype "input"))
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 119 111.9 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "drone_LED_strip.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C9" (at 0 -1.16 90) (layer "F.SilkS") hide)
    (fp_text value "C" (at 0 1.16 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.48 0 90) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+5V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.48 0 90) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 107.6 111.9 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "drone_LED_strip.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C16" (at 0 -1.16 90) (layer "F.SilkS") hide)
    (fp_text value "C" (at 0 1.16 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.48 0 90) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+5V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.48 0 90) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 122.8 111.9 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "drone_LED_strip.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C19" (at 0 -1.16 90) (layer "F.SilkS") hide)
    (fp_text value "C" (at 0 1.16 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.48 0 90) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+5V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.48 0 90) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprint_lib:XL-0807RGBC-WS2812B" (layer "F.Cu")
    (tedit 0)
    (at 120.9 109.5)
    (property "Sheetfile" "drone_LED_strip.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D2" (at -0.2 -1.6 unlocked) (layer "F.SilkS") hide)
    (fp_text value "WS2812B" (at 10.5 -10 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 10.5 -8.5 unlocked) (layer "F.Fab"))
    (pad "1" smd roundrect (at 0.75 -0.45) (size 0.6 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+5V") (pinfunction "VDD") (pintype "power_in"))
    (pad "2" smd roundrect (at -0.75 -0.45) (size 0.6 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "Net-(D2-Pad2)") (pinfunction "DOUT") (pintype "output"))
    (pad "3" smd roundrect (at -0.75 0.45) (size 0.6 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "VSS") (pintype "power_in"))
    (pad "4" smd roundrect (at 0.75 0.45) (size 0.6 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "Net-(D1-Pad2)") (pinfunction "DIN") (pintype "input"))
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 107.6 109.5 -90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "drone_LED_strip.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C5" (at 0 -1.16 -90) (layer "F.SilkS") hide)
    (fp_text value "C" (at 0 1.16 -90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 -90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.48 0 270) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+5V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.48 0 270) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprint_lib:XL-0807RGBC-WS2812B" (layer "F.Cu")
    (tedit 0)
    (at 101.9 111.9 180)
    (property "Sheetfile" "drone_LED_strip.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D14" (at 10.5 -11.5 180 unlocked) (layer "F.SilkS") hide)
    (fp_text value "WS2812B" (at 10.5 -10 180 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 10.5 -8.5 180 unlocked) (layer "F.Fab"))
    (pad "1" smd roundrect (at 0.75 -0.45 180) (size 0.6 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+5V") (pinfunction "VDD") (pintype "power_in"))
    (pad "2" smd roundrect (at -0.75 -0.45 180) (size 0.6 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 17 "Net-(D14-Pad2)") (pinfunction "DOUT") (pintype "output"))
    (pad "3" smd roundrect (at -0.75 0.45 180) (size 0.6 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "VSS") (pintype "power_in"))
    (pad "4" smd roundrect (at 0.75 0.45 180) (size 0.6 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 16 "Net-(D13-Pad2)") (pinfunction "DIN") (pintype "input"))
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 100 109.5 -90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "drone_LED_strip.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C7" (at 0 -1.16 90) (layer "F.SilkS") hide)
    (fp_text value "C" (at 0 1.16 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.48 0 270) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+5V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.48 0 270) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprint_lib:XL-0807RGBC-WS2812B" (layer "F.Cu")
    (tedit 0)
    (at 98.1 109.5)
    (property "Sheetfile" "drone_LED_strip.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D8" (at 10.5 -11.5 unlocked) (layer "F.SilkS") hide)
    (fp_text value "WS2812B" (at 10.5 -10 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 10.5 -8.5 unlocked) (layer "F.Fab"))
    (pad "1" smd roundrect (at 0.75 -0.45) (size 0.6 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+5V") (pinfunction "VDD") (pintype "power_in"))
    (pad "2" smd roundrect (at -0.75 -0.45) (size 0.6 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 23 "Net-(D8-Pad2)") (pinfunction "DOUT") (pintype "output"))
    (pad "3" smd roundrect (at -0.75 0.45) (size 0.6 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "VSS") (pintype "power_in"))
    (pad "4" smd roundrect (at 0.75 0.45) (size 0.6 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 10 "Net-(D7-Pad2)") (pinfunction "DIN") (pintype "input"))
  )
  (footprint "footprint_lib:XL-0807RGBC-WS2812B" (layer "F.Cu")
    (tedit 0)
    (at 90.5 109.5)
    (property "Sheetfile" "drone_LED_strip.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D10" (at 5.2 -3.5 unlocked) (layer "F.SilkS") hide)
    (fp_text value "WS2812B" (at 10.5 -10 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 10.5 -8.5 unlocked) (layer "F.Fab"))
    (pad "1" smd roundrect (at 0.75 -0.45) (size 0.6 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+5V") (pinfunction "VDD") (pintype "power_in"))
    (pad "2" smd roundrect (at -0.75 -0.45) (size 0.6 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 12 "Net-(D10-Pad2)") (pinfunction "DOUT") (pintype "output"))
    (pad "3" smd roundrect (at -0.75 0.45) (size 0.6 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "VSS") (pintype "power_in"))
    (pad "4" smd roundrect (at 0.75 0.45) (size 0.6 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 11 "Net-(D10-Pad4)") (pinfunction "DIN") (pintype "input"))
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 111.4 109.5 -90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "drone_LED_strip.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C4" (at 0 -1.16 -90) (layer "F.SilkS") hide)
    (fp_text value "C" (at 0 1.16 -90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 -90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.48 0 270) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+5V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.48 0 270) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_arc (start 131.5 112.7) (mid 131.207107 113.407107) (end 130.5 113.7) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 87.5 113.7) (end 130.5 113.7) (layer "Edge.Cuts") (width 0.1))
  (gr_arc (start 130.5 107.7) (mid 131.207107 107.992893) (end 131.5 108.7) (layer "Edge.Cuts") (width 0.1))
  (gr_arc (start 87.5 113.7) (mid 86.792893 113.407107) (end 86.5 112.7) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 131.5 108.7) (end 131.5 112.7) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 130.5 107.7) (end 87.5 107.7) (layer "Edge.Cuts") (width 0.1))
  (gr_arc (start 86.5 108.7) (mid 86.792893 107.992893) (end 87.5 107.7) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 86.5 108.7) (end 86.5 112.7) (layer "Edge.Cuts") (width 0.1))
  (gr_text "DOUT" (at 127.6 111.2) (layer "B.SilkS"))
  (gr_text "DIN" (at 128.1 110.2) (layer "B.SilkS"))
  (gr_text "+5V\n" (at 127.8 109.2) (layer "B.SilkS"))
  (gr_text "Drone LED strip ver.: 1.0\nDesigned by @_cybermouse_" (at 126.1 110.7) (layer "B.SilkS"))
  (gr_text "GND" (at 127.9 112.2) (layer "B.SilkS"))
  (gr_text "DIN" (at 128.1 110.2) (layer "F.SilkS"))
  (gr_text "+5V\n" (at 127.8 109.2) (layer "F.SilkS"))
  (gr_text "DOUT" (at 127.6 111.2) (layer "F.SilkS"))
  (gr_text "GND" (at 127.9 112.2) (layer "F.SilkS"))
  (zone (net 2) (net_name "GND") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.2) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 0.1))
    (polygon
      (pts
        (xy 129.400138 111.8)
        (xy 130.300138 111.8)
        (xy 130.300138 112.6)
        (xy 126.000138 112.6)
        (xy 126.000138 111.8)
        (xy 124.300138 111.8)
        (xy 124.299425 110.0913)
        (xy 129.399425 110.098696)
      )
    )
  )
  (zone (net 1) (net_name "+5V") (layer "F.Cu") (hatch edge 0.508)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.2) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 0.1))
    (polygon
      (pts
        (xy 132.1 114.1)
        (xy 85.4 114.1)
        (xy 85.4 107.2)
        (xy 132.1 107.2)
      )
    )
  )
  (zone (net 2) (net_name "GND") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.2) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 125.8 111.8)
        (xy 88.1 111.8)
        (xy 88.1 109.6)
        (xy 125.8 109.6)
      )
    )
  )
  (zone (net 2) (net_name "GND") (layer "B.Cu") (hatch edge 0.508)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.2) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 0.1))
    (polygon
      (pts
        (xy 132.1 114.1)
        (xy 85.4 114.1)
        (xy 85.4 107.2)
        (xy 132.1 107.2)
      )
    )
  )
)
