<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.1.0">
<drawing>
<board>
<plain>
<circle x="57.677" y="27.413" radius="25" width="0.01" layer="20"/>
<text>9</text>
<text>6</text>
<text>3</text>
<text>1</text>
<text>2</text>
<text>3</text>
<text>4</text>
<text>5</text>
<text>6</text>
<text>7</text>
<text>8</text>
<text>9</text>
<text>10</text>
<text>11</text>
<text>12</text>
<text>Bobricius</text>
<text>CR2032 3V</text>
</plain>
<libraries>
<library name="SmallRoomLabs">
<packages>
<package name="HEADER-2X3-EXTENDED">
</package>
<package name="CHIPLED_0805">
</package>
</packages>
</library>
<library name="microbuilder">
<packages>
<package name="0603">
<description>0603 (1608 Metric)</description>
</package>
<package name="MOUNTINGHOLE_2.0_PLATED">
</package>
</packages>
</library>
<library name="SparkFun">
<packages>
<package name="TQFP32-08">
<description>&lt;B&gt;Thin Plasic Quad Flat Package&lt;/B&gt; Grid 0.8 mm</description>
</package>
<package name="TACTILE-SWITCH-1101NE">
<description>Sparkfun SKU# COM-08229</description>
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="SMT-8585-BUZZER">
</package>
</packages>
</library>
<library name="OSHW">
<packages>
<package name="OSHW_FILLX200_NOTEXT">
</package>
</packages>
</library>
<library name="SparkFun-Electromechanical">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find anything that moves- switches, relays, buttons, potentiometers. Also, anything that goes on a board but isn't electrical in nature- screws, standoffs, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="BATTCON_20MM">
</package>
</packages>
</library>
<library name="es">
<packages>
<package name="KX-327LT">
</package>
</packages>
</library>
<library name="rc-master-smd">
<packages>
<package name="C0603">
<description>&lt;b&gt;SMD CHIP CAP&lt;/b&gt; - 0603</description>
</package>
</packages>
</library>
<library name="led">
<description>&lt;b&gt;LEDs&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;&lt;br&gt;
Extended by Federico Battaglin &lt;author&gt;&amp;lt;federico.rd@fdpinternational.com&amp;gt;&lt;/author&gt; with DUOLED</description>
<packages>
<package name="CHIPLED_0603">
<description>&lt;b&gt;CHIPLED&lt;/b&gt;&lt;p&gt;
Source: http://www.osram.convergy.de/ ... LG_LY Q971.pdf</description>
</package>
</packages>
</library>
<library name="transistor-small-signal">
<packages>
<package name="SOT23">
<description>&lt;b&gt;SOT-23&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U$2" library="SparkFun" package="TQFP32-08" value="AVR-MEGA8-AI"/>
<element name="U$17" library="SmallRoomLabs" package="HEADER-2X3-EXTENDED" value="AVR-ISP6AVRISP-EXTENED"/>
<element name="R12" library="microbuilder" package="0603" value="">
<attribute name="VALUE"/>
</element>
<element name="U$19" library="OSHW" package="OSHW_FILLX200_NOTEXT" value=""/>
<element name="LED1" library="SmallRoomLabs" package="CHIPLED_0805" value="LEDSMD0805"/>
<element name="LED2" library="SmallRoomLabs" package="CHIPLED_0805" value="LEDSMD0805"/>
<element name="LED3" library="SmallRoomLabs" package="CHIPLED_0805" value="LEDSMD0805"/>
<element name="LED4" library="SmallRoomLabs" package="CHIPLED_0805" value="LEDSMD0805"/>
<element name="LED5" library="SmallRoomLabs" package="CHIPLED_0805" value="LEDSMD0805"/>
<element name="LED6" library="SmallRoomLabs" package="CHIPLED_0805" value="LEDSMD0805"/>
<element name="LED7" library="SmallRoomLabs" package="CHIPLED_0805" value="LEDSMD0805"/>
<element name="LED8" library="SmallRoomLabs" package="CHIPLED_0805" value="LEDSMD0805"/>
<element name="LED9" library="SmallRoomLabs" package="CHIPLED_0805" value="LEDSMD0805"/>
<element name="LED10" library="SmallRoomLabs" package="CHIPLED_0805" value="LEDSMD0805"/>
<element name="LED11" library="SmallRoomLabs" package="CHIPLED_0805" value="LEDSMD0805"/>
<element name="LED12" library="SmallRoomLabs" package="CHIPLED_0805" value="LEDSMD0805"/>
<element name="LED13" library="SmallRoomLabs" package="CHIPLED_0805" value="LEDSMD0805"/>
<element name="LED14" library="SmallRoomLabs" package="CHIPLED_0805" value="LEDSMD0805"/>
<element name="LED15" library="SmallRoomLabs" package="CHIPLED_0805" value="LEDSMD0805"/>
<element name="LED16" library="SmallRoomLabs" package="CHIPLED_0805" value="LEDSMD0805"/>
<element name="LED17" library="SmallRoomLabs" package="CHIPLED_0805" value="LEDSMD0805"/>
<element name="LED18" library="SmallRoomLabs" package="CHIPLED_0805" value="LEDSMD0805"/>
<element name="LED19" library="SmallRoomLabs" package="CHIPLED_0805" value="LEDSMD0805"/>
<element name="LED20" library="SmallRoomLabs" package="CHIPLED_0805" value="LEDSMD0805"/>
<element name="LED21" library="SmallRoomLabs" package="CHIPLED_0805" value="LEDSMD0805"/>
<element name="LED22" library="SmallRoomLabs" package="CHIPLED_0805" value="LEDSMD0805"/>
<element name="LED23" library="SmallRoomLabs" package="CHIPLED_0805" value="LEDSMD0805"/>
<element name="LED24" library="SmallRoomLabs" package="CHIPLED_0805" value="LEDSMD0805"/>
<element name="LED25" library="SmallRoomLabs" package="CHIPLED_0805" value="LEDSMD0805"/>
<element name="LED26" library="SmallRoomLabs" package="CHIPLED_0805" value="LEDSMD0805"/>
<element name="LED27" library="SmallRoomLabs" package="CHIPLED_0805" value="LEDSMD0805"/>
<element name="LED28" library="SmallRoomLabs" package="CHIPLED_0805" value="LEDSMD0805"/>
<element name="LED29" library="SmallRoomLabs" package="CHIPLED_0805" value="LEDSMD0805"/>
<element name="LED30" library="SmallRoomLabs" package="CHIPLED_0805" value="LEDSMD0805"/>
<element name="LED31" library="SmallRoomLabs" package="CHIPLED_0805" value="LEDSMD0805"/>
<element name="LED32" library="SmallRoomLabs" package="CHIPLED_0805" value="LEDSMD0805"/>
<element name="LED33" library="SmallRoomLabs" package="CHIPLED_0805" value="LEDSMD0805"/>
<element name="LED34" library="SmallRoomLabs" package="CHIPLED_0805" value="LEDSMD0805"/>
<element name="LED35" library="SmallRoomLabs" package="CHIPLED_0805" value="LEDSMD0805"/>
<element name="LED36" library="SmallRoomLabs" package="CHIPLED_0805" value="LEDSMD0805"/>
<element name="LED37" library="SmallRoomLabs" package="CHIPLED_0805" value="LEDSMD0805"/>
<element name="LED38" library="SmallRoomLabs" package="CHIPLED_0805" value="LEDSMD0805"/>
<element name="LED39" library="SmallRoomLabs" package="CHIPLED_0805" value="LEDSMD0805"/>
<element name="LED40" library="SmallRoomLabs" package="CHIPLED_0805" value="LEDSMD0805"/>
<element name="LED41" library="SmallRoomLabs" package="CHIPLED_0805" value="LEDSMD0805"/>
<element name="LED42" library="SmallRoomLabs" package="CHIPLED_0805" value="LEDSMD0805"/>
<element name="LED43" library="SmallRoomLabs" package="CHIPLED_0805" value="LEDSMD0805"/>
<element name="LED44" library="SmallRoomLabs" package="CHIPLED_0805" value="LEDSMD0805"/>
<element name="LED45" library="SmallRoomLabs" package="CHIPLED_0805" value="LEDSMD0805"/>
<element name="LED46" library="SmallRoomLabs" package="CHIPLED_0805" value="LEDSMD0805"/>
<element name="LED47" library="SmallRoomLabs" package="CHIPLED_0805" value="LEDSMD0805"/>
<element name="LED48" library="SmallRoomLabs" package="CHIPLED_0805" value="LEDSMD0805"/>
<element name="LED49" library="SmallRoomLabs" package="CHIPLED_0805" value="LEDSMD0805"/>
<element name="LED50" library="SmallRoomLabs" package="CHIPLED_0805" value="LEDSMD0805"/>
<element name="LED51" library="SmallRoomLabs" package="CHIPLED_0805" value="LEDSMD0805"/>
<element name="LED52" library="SmallRoomLabs" package="CHIPLED_0805" value="LEDSMD0805"/>
<element name="LED53" library="SmallRoomLabs" package="CHIPLED_0805" value="LEDSMD0805"/>
<element name="LED54" library="SmallRoomLabs" package="CHIPLED_0805" value="LEDSMD0805"/>
<element name="LED55" library="SmallRoomLabs" package="CHIPLED_0805" value="LEDSMD0805"/>
<element name="LED56" library="SmallRoomLabs" package="CHIPLED_0805" value="LEDSMD0805"/>
<element name="LED57" library="SmallRoomLabs" package="CHIPLED_0805" value="LEDSMD0805"/>
<element name="LED58" library="SmallRoomLabs" package="CHIPLED_0805" value="LEDSMD0805"/>
<element name="LED59" library="SmallRoomLabs" package="CHIPLED_0805" value="LEDSMD0805"/>
<element name="LED60" library="SmallRoomLabs" package="CHIPLED_0805" value="LEDSMD0805"/>
<element name="LED61" library="SmallRoomLabs" package="CHIPLED_0805" value="LEDSMD0805"/>
<element name="LED62" library="SmallRoomLabs" package="CHIPLED_0805" value="LEDSMD0805"/>
<element name="LED63" library="SmallRoomLabs" package="CHIPLED_0805" value="LEDSMD0805"/>
<element name="LED64" library="SmallRoomLabs" package="CHIPLED_0805" value="LEDSMD0805"/>
<element name="LED65" library="SmallRoomLabs" package="CHIPLED_0805" value="LEDSMD0805"/>
<element name="LED66" library="SmallRoomLabs" package="CHIPLED_0805" value="LEDSMD0805"/>
<element name="LED67" library="SmallRoomLabs" package="CHIPLED_0805" value="LEDSMD0805"/>
<element name="LED68" library="SmallRoomLabs" package="CHIPLED_0805" value="LEDSMD0805"/>
<element name="LED69" library="SmallRoomLabs" package="CHIPLED_0805" value="LEDSMD0805"/>
<element name="LED70" library="SmallRoomLabs" package="CHIPLED_0805" value="LEDSMD0805"/>
<element name="LED71" library="SmallRoomLabs" package="CHIPLED_0805" value="LEDSMD0805"/>
<element name="LED72" library="SmallRoomLabs" package="CHIPLED_0805" value="LEDSMD0805"/>
<element name="BAT2" library="SparkFun-Electromechanical" package="BATTCON_20MM" value=""/>
<element name="32,768KHZ" library="es" package="KX-327LT" value="32768KHz"/>
<element name="C3" library="rc-master-smd" package="C0603" value="22p"/>
<element name="C6" library="rc-master-smd" package="C0603" value="22p"/>
<element name="U$23" library="microbuilder" package="MOUNTINGHOLE_2.0_PLATED" value="MOUNTINGHOLE2.0"/>
<element name="U$24" library="microbuilder" package="MOUNTINGHOLE_2.0_PLATED" value="MOUNTINGHOLE2.0"/>
<element name="U$25" library="microbuilder" package="MOUNTINGHOLE_2.0_PLATED" value="MOUNTINGHOLE2.0"/>
<element name="U$26" library="microbuilder" package="MOUNTINGHOLE_2.0_PLATED" value="MOUNTINGHOLE2.0"/>
<element name="LED73" library="led" package="CHIPLED_0603" value="">
<attribute name="VALUE"/>
</element>
<element name="LED74" library="led" package="CHIPLED_0603" value="">
<attribute name="VALUE"/>
</element>
<element name="LED75" library="led" package="CHIPLED_0603" value="">
<attribute name="VALUE"/>
</element>
<element name="LED76" library="led" package="CHIPLED_0603" value="">
<attribute name="VALUE"/>
</element>
<element name="LED77" library="led" package="CHIPLED_0603" value="">
<attribute name="VALUE"/>
</element>
<element name="LED78" library="led" package="CHIPLED_0603" value="">
<attribute name="VALUE"/>
</element>
<element name="LED79" library="led" package="CHIPLED_0603" value="">
<attribute name="VALUE"/>
</element>
<element name="LED80" library="led" package="CHIPLED_0603" value="">
<attribute name="VALUE"/>
</element>
<element name="LED81" library="led" package="CHIPLED_0603" value="">
<attribute name="VALUE"/>
</element>
<element name="LED82" library="led" package="CHIPLED_0603" value="">
<attribute name="VALUE"/>
</element>
<element name="LED83" library="led" package="CHIPLED_0603" value="">
<attribute name="VALUE"/>
</element>
<element name="LED84" library="led" package="CHIPLED_0603" value="">
<attribute name="VALUE"/>
</element>
<element name="LED85" library="led" package="CHIPLED_0603" value="">
<attribute name="VALUE"/>
</element>
<element name="LED86" library="led" package="CHIPLED_0603" value="">
<attribute name="VALUE"/>
</element>
<element name="LED87" library="led" package="CHIPLED_0603" value="">
<attribute name="VALUE"/>
</element>
<element name="LED88" library="led" package="CHIPLED_0603" value="">
<attribute name="VALUE"/>
</element>
<element name="LED89" library="led" package="CHIPLED_0603" value="">
<attribute name="VALUE"/>
</element>
<element name="LED90" library="led" package="CHIPLED_0603" value="">
<attribute name="VALUE"/>
</element>
<element name="LED91" library="led" package="CHIPLED_0603" value="">
<attribute name="VALUE"/>
</element>
<element name="LED92" library="led" package="CHIPLED_0603" value="">
<attribute name="VALUE"/>
</element>
<element name="Q4" library="transistor-small-signal" package="SOT23" value="BSS123"/>
<element name="U$6" library="adafruit" package="SMT-8585-BUZZER" value="BUZZER"/>
<element name="D3-BOOT1" library="SparkFun" package="TACTILE-SWITCH-1101NE" value="">
<attribute name="VALUE"/>
</element>
<element name="D3-BOOT2" library="SparkFun" package="TACTILE-SWITCH-1101NE" value="">
<attribute name="VALUE"/>
</element>
<element name="C1" library="rc-master-smd" package="C0603" value="22p"/>
</elements>
<signals>
<signal name="GND">
<contactref element="U$2" pad="5"/>
<contactref element="U$2" pad="3"/>
<contactref element="U$2" pad="21"/>
<contactref element="U$17" pad="6"/>
<contactref element="BAT2" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="C6" pad="1"/>
<contactref element="Q4" pad="2"/>
<contactref element="D3-BOOT1" pad="P$1"/>
<contactref element="D3-BOOT2" pad="P$1"/>
<contactref element="C1" pad="2"/>
</signal>
<signal name="VCC">
<contactref element="U$2" pad="6"/>
<contactref element="U$2" pad="4"/>
<contactref element="U$2" pad="18"/>
<contactref element="U$17" pad="2"/>
<contactref element="R12" pad="2"/>
<contactref element="U$6" pad="+"/>
</signal>
<signal name="CP1">
<contactref element="LED1" pad="C"/>
<contactref element="LED2" pad="C"/>
<contactref element="LED3" pad="C"/>
<contactref element="LED4" pad="C"/>
<contactref element="LED5" pad="C"/>
<contactref element="LED6" pad="C"/>
<contactref element="LED7" pad="C"/>
<contactref element="LED8" pad="C"/>
<contactref element="LED9" pad="A"/>
<contactref element="LED17" pad="A"/>
<contactref element="LED25" pad="A"/>
<contactref element="LED33" pad="A"/>
<contactref element="LED41" pad="A"/>
<contactref element="LED49" pad="A"/>
<contactref element="LED57" pad="A"/>
<contactref element="LED65" pad="A"/>
<contactref element="U$2" pad="30"/>
</signal>
<signal name="CP2">
<contactref element="LED1" pad="A"/>
<contactref element="LED9" pad="C"/>
<contactref element="LED10" pad="C"/>
<contactref element="LED11" pad="C"/>
<contactref element="LED12" pad="C"/>
<contactref element="LED13" pad="C"/>
<contactref element="LED14" pad="C"/>
<contactref element="LED15" pad="C"/>
<contactref element="LED16" pad="C"/>
<contactref element="LED18" pad="A"/>
<contactref element="LED26" pad="A"/>
<contactref element="LED34" pad="A"/>
<contactref element="LED42" pad="A"/>
<contactref element="LED50" pad="A"/>
<contactref element="LED58" pad="A"/>
<contactref element="LED66" pad="A"/>
<contactref element="U$2" pad="31"/>
</signal>
<signal name="CP3">
<contactref element="LED2" pad="A"/>
<contactref element="LED10" pad="A"/>
<contactref element="LED17" pad="C"/>
<contactref element="LED18" pad="C"/>
<contactref element="LED19" pad="C"/>
<contactref element="LED20" pad="C"/>
<contactref element="LED21" pad="C"/>
<contactref element="LED22" pad="C"/>
<contactref element="LED23" pad="C"/>
<contactref element="LED24" pad="C"/>
<contactref element="LED27" pad="A"/>
<contactref element="LED35" pad="A"/>
<contactref element="LED43" pad="A"/>
<contactref element="LED51" pad="A"/>
<contactref element="LED59" pad="A"/>
<contactref element="LED67" pad="A"/>
<contactref element="U$2" pad="28"/>
</signal>
<signal name="CP4">
<contactref element="LED3" pad="A"/>
<contactref element="LED11" pad="A"/>
<contactref element="LED19" pad="A"/>
<contactref element="LED25" pad="C"/>
<contactref element="LED26" pad="C"/>
<contactref element="LED27" pad="C"/>
<contactref element="LED28" pad="C"/>
<contactref element="LED29" pad="C"/>
<contactref element="LED30" pad="C"/>
<contactref element="LED31" pad="C"/>
<contactref element="LED32" pad="C"/>
<contactref element="LED36" pad="A"/>
<contactref element="LED44" pad="A"/>
<contactref element="LED52" pad="A"/>
<contactref element="LED60" pad="A"/>
<contactref element="LED68" pad="A"/>
<contactref element="U$2" pad="14"/>
</signal>
<signal name="CP5">
<contactref element="LED4" pad="A"/>
<contactref element="LED12" pad="A"/>
<contactref element="LED20" pad="A"/>
<contactref element="LED28" pad="A"/>
<contactref element="LED33" pad="C"/>
<contactref element="LED34" pad="C"/>
<contactref element="LED35" pad="C"/>
<contactref element="LED36" pad="C"/>
<contactref element="LED37" pad="C"/>
<contactref element="LED38" pad="C"/>
<contactref element="LED39" pad="C"/>
<contactref element="LED40" pad="C"/>
<contactref element="LED45" pad="A"/>
<contactref element="LED53" pad="A"/>
<contactref element="LED61" pad="A"/>
<contactref element="LED69" pad="A"/>
<contactref element="U$2" pad="2"/>
</signal>
<signal name="CP6">
<contactref element="LED5" pad="A"/>
<contactref element="LED13" pad="A"/>
<contactref element="LED21" pad="A"/>
<contactref element="LED29" pad="A"/>
<contactref element="LED37" pad="A"/>
<contactref element="LED41" pad="C"/>
<contactref element="LED42" pad="C"/>
<contactref element="LED43" pad="C"/>
<contactref element="LED44" pad="C"/>
<contactref element="LED45" pad="C"/>
<contactref element="LED46" pad="C"/>
<contactref element="LED47" pad="C"/>
<contactref element="LED48" pad="C"/>
<contactref element="LED54" pad="A"/>
<contactref element="LED62" pad="A"/>
<contactref element="LED70" pad="A"/>
<contactref element="U$2" pad="9"/>
</signal>
<signal name="CP7">
<contactref element="LED6" pad="A"/>
<contactref element="LED14" pad="A"/>
<contactref element="LED22" pad="A"/>
<contactref element="LED30" pad="A"/>
<contactref element="LED38" pad="A"/>
<contactref element="LED46" pad="A"/>
<contactref element="LED49" pad="C"/>
<contactref element="LED50" pad="C"/>
<contactref element="LED51" pad="C"/>
<contactref element="LED52" pad="C"/>
<contactref element="LED53" pad="C"/>
<contactref element="LED54" pad="C"/>
<contactref element="LED55" pad="C"/>
<contactref element="LED56" pad="C"/>
<contactref element="LED63" pad="A"/>
<contactref element="LED71" pad="A"/>
<contactref element="U$2" pad="10"/>
</signal>
<signal name="CP8">
<contactref element="LED7" pad="A"/>
<contactref element="LED15" pad="A"/>
<contactref element="LED23" pad="A"/>
<contactref element="LED31" pad="A"/>
<contactref element="LED39" pad="A"/>
<contactref element="LED47" pad="A"/>
<contactref element="LED55" pad="A"/>
<contactref element="LED57" pad="C"/>
<contactref element="LED58" pad="C"/>
<contactref element="LED59" pad="C"/>
<contactref element="LED60" pad="C"/>
<contactref element="LED61" pad="C"/>
<contactref element="LED62" pad="C"/>
<contactref element="LED63" pad="C"/>
<contactref element="LED64" pad="C"/>
<contactref element="LED72" pad="A"/>
<contactref element="U$2" pad="11"/>
</signal>
<signal name="CP9">
<contactref element="LED8" pad="A"/>
<contactref element="LED16" pad="A"/>
<contactref element="LED24" pad="A"/>
<contactref element="LED32" pad="A"/>
<contactref element="LED40" pad="A"/>
<contactref element="LED48" pad="A"/>
<contactref element="LED56" pad="A"/>
<contactref element="LED64" pad="A"/>
<contactref element="LED65" pad="C"/>
<contactref element="LED66" pad="C"/>
<contactref element="LED67" pad="C"/>
<contactref element="LED68" pad="C"/>
<contactref element="LED69" pad="C"/>
<contactref element="LED70" pad="C"/>
<contactref element="LED71" pad="C"/>
<contactref element="LED72" pad="C"/>
<contactref element="U$2" pad="12"/>
</signal>
<signal name="A4">
<contactref element="U$2" pad="27"/>
<contactref element="LED89" pad="A"/>
<contactref element="LED90" pad="A"/>
<contactref element="LED91" pad="A"/>
<contactref element="LED92" pad="A"/>
<contactref element="LED73" pad="C"/>
<contactref element="LED77" pad="C"/>
<contactref element="LED81" pad="C"/>
<contactref element="LED85" pad="C"/>
</signal>
<signal name="A0">
<contactref element="U$2" pad="23"/>
<contactref element="LED73" pad="A"/>
<contactref element="LED74" pad="A"/>
<contactref element="LED75" pad="A"/>
<contactref element="LED76" pad="A"/>
<contactref element="LED92" pad="C"/>
<contactref element="LED88" pad="C"/>
<contactref element="LED84" pad="C"/>
<contactref element="LED80" pad="C"/>
</signal>
<signal name="SCK">
<contactref element="U$2" pad="17"/>
<contactref element="U$17" pad="3"/>
</signal>
<signal name="MISO">
<contactref element="U$17" pad="1"/>
<contactref element="U$2" pad="16"/>
</signal>
<signal name="MOSI">
<contactref element="U$2" pad="15"/>
<contactref element="U$17" pad="4"/>
</signal>
<signal name="RESET">
<contactref element="R12" pad="1"/>
<contactref element="U$2" pad="29"/>
<contactref element="U$17" pad="5"/>
</signal>
<signal name="V+">
<contactref element="BAT2" pad="1"/>
<contactref element="C1" pad="1"/>
</signal>
<signal name="PB6">
<contactref element="32,768KHZ" pad="4"/>
<contactref element="C3" pad="1"/>
<contactref element="U$2" pad="7"/>
</signal>
<signal name="PB7">
<contactref element="32,768KHZ" pad="1"/>
<contactref element="C6" pad="2"/>
<contactref element="U$2" pad="8"/>
</signal>
<signal name="D3">
<contactref element="U$2" pad="1"/>
<contactref element="D3-BOOT1" pad="P$2"/>
</signal>
<signal name="OUT">
<contactref element="Q4" pad="3"/>
<contactref element="U$6" pad="-"/>
</signal>
<signal name="A3">
<contactref element="U$2" pad="26"/>
<contactref element="LED85" pad="A"/>
<contactref element="LED86" pad="A"/>
<contactref element="LED87" pad="A"/>
<contactref element="LED88" pad="A"/>
<contactref element="LED89" pad="C"/>
<contactref element="LED74" pad="C"/>
<contactref element="LED78" pad="C"/>
<contactref element="LED82" pad="C"/>
</signal>
<signal name="A1">
<contactref element="U$2" pad="24"/>
<contactref element="LED77" pad="A"/>
<contactref element="LED78" pad="A"/>
<contactref element="LED79" pad="A"/>
<contactref element="LED80" pad="A"/>
<contactref element="LED91" pad="C"/>
<contactref element="LED87" pad="C"/>
<contactref element="LED83" pad="C"/>
<contactref element="LED76" pad="C"/>
</signal>
<signal name="A2">
<contactref element="U$2" pad="25"/>
<contactref element="LED81" pad="A"/>
<contactref element="LED82" pad="A"/>
<contactref element="LED83" pad="A"/>
<contactref element="LED84" pad="A"/>
<contactref element="LED90" pad="C"/>
<contactref element="LED86" pad="C"/>
<contactref element="LED75" pad="C"/>
<contactref element="LED79" pad="C"/>
</signal>
<signal name="D2">
<contactref element="U$2" pad="32"/>
<contactref element="D3-BOOT2" pad="P$2"/>
</signal>
<signal name="D9">
<contactref element="U$2" pad="13"/>
<contactref element="Q4" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
