<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<schematic>
<libraries>
<library name="microbuilder">
<description>&lt;h2&gt;&lt;b&gt;microBuilder.eu&lt;/b&gt; Eagle Footprint Library&lt;/h2&gt;

&lt;p&gt;Footprints for common components used in our projects and products.  This is the same library that we use internally, and it is regularly updated.  The newest version can always be found at &lt;b&gt;www.microBuilder.eu&lt;/b&gt;.  If you find this library useful, please feel free to purchase something from our online store. Please also note that all holes are optimised for metric drill bits!&lt;/p&gt;

&lt;h3&gt;Obligatory Warning&lt;/h3&gt;
&lt;p&gt;While it probably goes without saying, there are no guarantees that the footprints or schematic symbols in this library are flawless, and we make no promises of fitness for production, prototyping or any other purpose. These libraries are provided for information puposes only, and are used at your own discretion.  While we make every effort to produce accurate footprints, and many of the items found in this library have be proven in production, we can't make any promises of suitability for a specific purpose. If you do find any errors, though, please feel free to contact us at www.microbuilder.eu to let us know about it so that we can update the library accordingly!&lt;/p&gt;

&lt;h3&gt;License&lt;/h3&gt;
&lt;p&gt;This work is placed in the public domain, and may be freely used for commercial and non-commercial work with the following conditions:&lt;/p&gt;
&lt;p&gt;THIS SOFTWARE IS PROVIDED ''AS IS'' AND ANY EXPRESS OR IMPLIED WARRANTIES, INCLUDING, BUT NOT LIMITED TO, THE IMPLIED WARRANTIES OF MERCHANTABILITY AND FITNESS FOR A PARTICULAR PURPOSE ARE DISCLAIMED.  IN NO EVENT SHALL THE INSTITUTE OR CONTRIBUTORS BE LIABLE FOR ANY DIRECT, INDIRECT, INCIDENTAL, SPECIAL, EXEMPLARY, OR CONSEQUENTIAL DAMAGES (INCLUDING,  BUT NOT LIMITED TO, PROCUREMENT OF SUBSTITUTE GOODS OR SERVICES; LOSS OF USE, DATA, OR PROFITS; OR BUSINESS INTERRUPTION) HOWEVER CAUSED AND ON ANY THEORY OF LIABILITY, WHETHER IN CONTRACT, STRICT LIABILITY, OR TORT (INCLUDING NEGLIGENCE OR OTHERWISE) ARISING IN ANY WAY OUT OF THE USE OF THIS SOFTWARE, EVEN IF ADVISED OF THE POSSIBILITY OF SUCH DAMAGE.
&lt;/p&gt;</description>
<packages>
<package name="RFM69HCW">
</package>
<package name="RFMHCW_SMT">
</package>
<package name="_0402">
<description>&lt;b&gt; 0402&lt;/b&gt;</description>
</package>
<package name="_0402MP">
<description>&lt;b&gt;0402 MicroPitch&lt;p&gt;</description>
</package>
<package name="_0603">
<description>&lt;b&gt;0603&lt;/b&gt;</description>
</package>
<package name="_0603MP">
<description>&lt;b&gt;0603 MicroPitch&lt;/b&gt;</description>
</package>
<package name="_0805">
<description>&lt;b&gt;0805&lt;/b&gt;</description>
</package>
<package name="_0805MP">
<description>&lt;b&gt;0805 MicroPitch&lt;/b&gt;</description>
</package>
<package name="0603">
<description>0603 (1608 Metric)</description>
</package>
<package name="0603@1">
<description>0603 (1608 Metric)</description>
</package>
<package name="1X01_OVAL">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X01_ROUND">
</package>
<package name="1X01_2MM">
</package>
<package name="1X01_2MM_OVAL">
</package>
<package name="1X01_SMD_MASKHELD_2X2MM">
</package>
<package name="1X01_SMD_MASKHELD_1X2MM">
</package>
<package name="SOLDERJUMPER_REFLOW">
<description>&lt;b&gt;Solder Jumper&lt;/b&gt; - Reflow</description>
</package>
<package name="SOLDERJUMPER_WAVE">
<description>&lt;b&gt;Solder Jumper&lt;/b&gt; - Wave</description>
</package>
<package name="SOLDERJUMPER_CLOSEDWIRE">
</package>
<package name="SOLDERJUMPER_REFLOW_NOPASTE">
</package>
<package name="SOLDERJUMPER_ARROW_NOPASTE">
</package>
<package name="USB_C_CUSB31-CFM2AX-01-X">
</package>
<package name="SMA90_DIP">
<description>SMA DIP Connector 90° 50 Ohm</description>
</package>
<package name="SMA_EDGELAUNCH">
</package>
<package name="SMA_EDGELAUNCH_UFL">
</package>
<package name="0805@1">
<description>0805 (2012 Metric)</description>
</package>
<package name="1206@1">
<description>1206 (3216 Metric)</description>
</package>
<package name="0402@1">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="0603-MINI">
<description>0603-Mini
&lt;p&gt;Mini footprint for dense boards&lt;/p&gt;</description>
</package>
<package name="0805_NOTHERMALS">
</package>
<package name="USB_A-SMT">
<description>4UConnector: 10017</description>
</package>
<package name="USB_HOST-PTH">
</package>
<package name="USBA_PCB">
</package>
<package name="USB_A-THM">
</package>
<package name="SOIC8_150MIL">
<description>&lt;b&gt;Small Outline IC - 150mil Wide&lt;/b&gt;</description>
</package>
<package name="SOIC8_208MIL">
<description>&lt;b&gt;Small Outline IC - 208mil Wide&lt;/b&gt;</description>
</package>
<package name="USON8">
</package>
<package name="APA102">
</package>
<package name="APA102_2020">
</package>
<package name="0805">
<description>0805 (2012 Metric)</description>
</package>
<package name="1206">
<description>1206 (3216 Metric)</description>
</package>
<package name="0402">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="0603-MINI@2">
<description>0603-Mini
&lt;p&gt;Mini footprint for dense boards&lt;/p&gt;</description>
</package>
<package name="2012">
</package>
<package name="0805_NOTHERMALS@2">
</package>
<package name="2512">
<description>&lt;b&gt;RESISTOR 2512 (Metric 6432)&lt;/b&gt;</description>
</package>
<package name="TQFN48_7MM">
</package>
<package name="SOT23-5">
<description>&lt;b&gt;Small Outline Transistor&lt;/b&gt; - 5 Pin</description>
</package>
</packages>
<symbols>
<symbol name="RFM69HCW">
<pin name="MISO" direction="out"/>
<pin name="DIO0"/>
<pin name="DIO2"/>
<pin name="DIO1"/>
<pin name="DIO5"/>
<pin name="RESET" direction="in"/>
<pin name="GND@3" direction="pwr"/>
<pin name="ANT"/>
<pin name="GND@1" direction="pwr"/>
<pin name="DIO3"/>
<pin name="MOSI" direction="in"/>
<pin name="SCK" direction="in"/>
<pin name="NSS" direction="in"/>
<pin name="DIO4"/>
<pin name="VDD" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
</symbol>
<symbol name="3.3V">
<pin name="3.3V" direction="sup"/>
</symbol>
<symbol name="GND">
<pin name="GND" direction="sup"/>
</symbol>
<symbol name="CAPACITOR">
<pin name="P$1" direction="pas"/>
<pin name="P$2" direction="pas"/>
</symbol>
<symbol name="PINHD1">
<pin name="1" direction="pas" function="dot"/>
</symbol>
<symbol name="RESISTOR">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="VBUS">
<pin name="VBUS" direction="sup"/>
</symbol>
<symbol name="SOLDERJUMPER">
<pin name="2" direction="pas"/>
<pin name="1" direction="pas"/>
</symbol>
<symbol name="USB_C">
<pin name="D+"/>
<pin name="D-"/>
<pin name="VBUS" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="CC1"/>
<pin name="SBU1"/>
<pin name="CC2"/>
<pin name="SBU2"/>
</symbol>
<symbol name="SMACONNECTOR">
<pin name="ANT"/>
<pin name="GND1" direction="pwr"/>
<pin name="GND2" direction="pwr"/>
<pin name="GND3" direction="pwr"/>
<pin name="GND4" direction="pwr"/>
</symbol>
<symbol name="USB_NOID">
<pin name="D+"/>
<pin name="D-"/>
<pin name="VBUS" direction="pwr"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="M25P16">
<pin name="SCK"/>
<pin name="MOSI"/>
<pin name="MISO"/>
<pin name="SSEL"/>
<pin name="WP#/IO2"/>
<pin name="HOLD#/IO3"/>
<pin name="VCC"/>
<pin name="VSS"/>
</symbol>
<symbol name="APA102">
<pin name="VDD" direction="pwr"/>
<pin name="DI" direction="in"/>
<pin name="GND" direction="pwr"/>
<pin name="DO" direction="out"/>
<pin name="CKI" direction="in"/>
<pin name="CKO" direction="out"/>
</symbol>
<symbol name="ATSAMD51G">
<pin name="GND" direction="pwr"/>
<pin name="VDDA" direction="pwr"/>
<pin name="PA16/I2C/I0/SERCOM1.0+3.1"/>
<pin name="PA17/I2C/I1/SERCOM1.1+3.0"/>
<pin name="PA18/I2/SERCOM1+3.2"/>
<pin name="PA19/I3/SERCOM1+3.3"/>
<pin name="PA22/I2C/I6/SERCOM3.0+5.1/I2SDI"/>
<pin name="PA23/I2C/I7/SERCOM3.1+5.0/SOF/I2SFS1"/>
<pin name="PA24/I8/SERCOM3+5.2/D-"/>
<pin name="PA25/I9/SERCOM3+5.3/D+"/>
<pin name="PA27/I11"/>
<pin name="PA30/I14/SECOM1.2/SWCLK"/>
<pin name="PA31/I15/SECOM1.3/SWDIO"/>
<pin name="PA09/I2C/I9/AIN9/SERCOM0.1+2.0/I2SFS0"/>
<pin name="PA08/I2C/AIN8/SERCOM0.0+2.1/I2SMCK"/>
<pin name="PA15/I15/SERCOM2+4.3"/>
<pin name="PA11/I11/AIN11/SERCOM0+2.3/I2SDO"/>
<pin name="PA14/I14/SERCOM2+4.2"/>
<pin name="PA10/I10/AIN10/SERCOM0+2.2/I2SCK"/>
<pin name="/RESET" function="dot"/>
<pin name="PA06/I6/VREFC/AIN6/SERCOM0.2"/>
<pin name="PA00/EINT0/SERCOM1.0"/>
<pin name="PA01/EINT1/SERCOM1.1"/>
<pin name="PA02/EINT2/AIN0/VOUT0"/>
<pin name="PA03/I3/VREFA/AIN1"/>
<pin name="PA04/I4/VREFB/AIN4/SERCOM0.0"/>
<pin name="PA05/I5/AIN5/VOUT1/SERCOM0.1"/>
<pin name="PA07/I7/AIN7/SERCOM0.3"/>
<pin name="VSW" direction="pwr"/>
<pin name="GNDA" direction="pwr"/>
<pin name="VDDIO" direction="pwr"/>
<pin name="VDDCORE" direction="pwr"/>
<pin name="PB08/I8/AIN2/SERCOM4.0"/>
<pin name="PB09/I9/AIN3/SERCOM4.1"/>
<pin name="PB10/I10/SERCOM4.2/I2SDI"/>
<pin name="PB11/I11/SERCOM4.3/I2SFS1"/>
<pin name="PA12/I12/I2C/SERCOM2.0+4.1"/>
<pin name="PA13/I13/I2C/SERCOM2.1+4.0"/>
<pin name="PA20/I4/SERCOM3+5.2/I2SFS0"/>
<pin name="PA21/I5/SERCOM3+5.3/I2SDO"/>
<pin name="PB22/I6/SERCOM1+5.2"/>
<pin name="PB23/I7/SERCOM1+5.3"/>
<pin name="PB02/I2/AIN14/SERCOM5.0"/>
<pin name="PB03/I3/AIN15/SERCOM5.1"/>
</symbol>
<symbol name="THERMAL-SLUG">
<pin name="TP" direction="pwr"/>
</symbol>
<symbol name="VREG_SOT23-5">
<pin name="IN" direction="pwr"/>
<pin name="OUT" direction="sup"/>
<pin name="EN" direction="in"/>
<pin name="GND" direction="pwr"/>
<pin name="P4"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="RFM69HCW" prefix="U" uservalue="yes">
<description>&lt;p&gt;&lt;b&gt;RFM69HCW - ISM Band RF Transceiver&lt;/b&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="RFM69HCW"/>
</gates>
<devices>
<device name="" package="RFM69HCW">
<connects>
<connect gate="G$1" pin="ANT" pad="1 1P"/>
<connect gate="G$1" pin="DIO0" pad="6 6P"/>
<connect gate="G$1" pin="DIO1" pad="7 7P"/>
<connect gate="G$1" pin="DIO2" pad="8 8P"/>
<connect gate="G$1" pin="DIO3" pad="3 3P"/>
<connect gate="G$1" pin="DIO4" pad="4 4P"/>
<connect gate="G$1" pin="DIO5" pad="15 15P"/>
<connect gate="G$1" pin="GND@1" pad="2 2P"/>
<connect gate="G$1" pin="GND@2" pad="9 9P"/>
<connect gate="G$1" pin="GND@3" pad="16 16P"/>
<connect gate="G$1" pin="MISO" pad="10 10P"/>
<connect gate="G$1" pin="MOSI" pad="11 11P"/>
<connect gate="G$1" pin="NSS" pad="13 13P"/>
<connect gate="G$1" pin="RESET" pad="14 14P"/>
<connect gate="G$1" pin="SCK" pad="12 12P"/>
<connect gate="G$1" pin="VDD" pad="5 5P"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_SMT" package="RFMHCW_SMT">
<connects>
<connect gate="G$1" pin="ANT" pad="1P"/>
<connect gate="G$1" pin="DIO0" pad="6P"/>
<connect gate="G$1" pin="DIO1" pad="7P"/>
<connect gate="G$1" pin="DIO2" pad="8P"/>
<connect gate="G$1" pin="DIO3" pad="3P"/>
<connect gate="G$1" pin="DIO4" pad="4P"/>
<connect gate="G$1" pin="DIO5" pad="15P"/>
<connect gate="G$1" pin="GND@1" pad="2P"/>
<connect gate="G$1" pin="GND@2" pad="9P"/>
<connect gate="G$1" pin="GND@3" pad="16P"/>
<connect gate="G$1" pin="MISO" pad="10P"/>
<connect gate="G$1" pin="MOSI" pad="11P"/>
<connect gate="G$1" pin="NSS" pad="13P"/>
<connect gate="G$1" pin="RESET" pad="14P"/>
<connect gate="G$1" pin="SCK" pad="12P"/>
<connect gate="G$1" pin="VDD" pad="5P"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="3.3V">
<description>&lt;b&gt;3.3V Supply&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="3.3V"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="GND">
<description>&lt;b&gt;GND&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="GND"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CAP_CERAMIC" prefix="C" uservalue="yes">
<description>&lt;p&gt;&lt;b&gt;Ceramic Capacitors&lt;/b&gt;&lt;/p&gt;
&lt;b&gt;0402&lt;/b&gt; - 0402 Surface Mount Capacitors
&lt;ul&gt;
&lt;li&gt;16pF 50V 5% [Digikey: 445-4899-2-ND]&lt;/li&gt;
&lt;li&gt;18pF 50V 5% [Digikey: 490-1281-2-ND]&lt;/li&gt;
&lt;li&gt;22pF 50V 5% [Digikey: 490-1283-2-ND]&lt;/li&gt;
&lt;li&gt;68pF 50V 5% [Digikey: 490-1289-2-ND]&lt;/li&gt;
&lt;li&gt;0.1uF 10V 10% [Digikey: 490-1318-2-ND]&lt;/li&gt;
&lt;li&gt;1.0uF 6.3V 10% [Digikey: 490-1320-2-ND]&lt;/li&gt;
&lt;/ul&gt;
&lt;b&gt;0603&lt;/b&gt; - 0603 Surface Mount Capacitors
&lt;ul&gt;
&lt;li&gt;16 pF 50V 5% [Digikey: 445-5051-2-ND]&lt;/li&gt;
&lt;li&gt;22 pF 50V [Digikey: PCC220ACVTR-ND]&lt;/li&gt;
&lt;li&gt;33 pF 50V 5% [Digikey: 490-1415-1-ND]&lt;/li&gt;
&lt;li&gt;56pF 50V 5% [Digikey: 490-1421-1-ND]&lt;/li&gt;
&lt;li&gt;220pF 50V 5% [Digikey: 445-1285-1-ND]&lt;/li&gt;
&lt;li&gt;680 pF 50V &lt;/li&gt;
&lt;li&gt;2200 pF 50V 5% C0G [Digikey: 445-1297-1-ND]&lt;/li&gt;
&lt;li&gt;5600 pF 100V 5% X7R [Digikey: 478-3711-1-ND]&lt;/li&gt;
&lt;li&gt;0.1 µF 25V 10% [Digikey: PCC2277TR-ND]&lt;/li&gt;
&lt;li&gt;0.22 µF 16V 10% X7R [Digikey: 445-1318-1-ND]&lt;/li&gt;
&lt;li&gt;1.0 µF 25V 10% [Digikey: 445-5146-2-ND]&lt;/li&gt;
&lt;/ul&gt;
&lt;b&gt;0603&lt;/b&gt; - RF Specific
&lt;ul&gt;
&lt;li&gt;3pF 250V +/-0.1pF RF [Digikey: 712-1347-1-ND]&lt;/li&gt;
&lt;li&gt;18 pF 250V 5%  [Digikey: 478-3505-1-ND or 712-1322-1-ND]&lt;/li&gt;
&lt;li&gt;56 pF 250V 5% C0G RF [Digikey: 490-4867-1-ND]&lt;/li&gt;
&lt;li&gt;68 pF 250V RF [Digikey: 490-4868-1-ND]&lt;/li&gt;
&lt;/ul&gt;
&lt;b&gt;0805&lt;/b&gt; - 0805 Surface Mount Capacitors
&lt;ul&gt;
&lt;li&gt;220 pF 250V 2% &lt;strong&gt;RF&lt;/strong&gt; Ceramic Capacitor [Digikey: 712-1398-1-ND]&lt;/li&gt;
&lt;li&gt;1000 pF 50V 2% NP0 Ceramic Capacitor [Digikey: 478-3760-1-ND]&lt;/li&gt;
&lt;li&gt;0.1 µF 25V 10% Ceramic Capacitor [Digikey: PCC1828TR-ND]&lt;/li&gt;
&lt;li&gt;1.0 µF 16V 10% Ceramic Capacitor[Digikey: 490-1691-2-ND]&lt;/li&gt;
&lt;li&gt;10.0 µF 10V 10% Ceramic Capacitor[Digikey: 709-1228-1-ND]&lt;/li&gt;
&lt;li&gt;10.0 uF 16V 10% Ceramic Capacitor [Digikey: 478-5165-2-ND]&lt;/li&gt;
&lt;li&gt;47 uF 6.3V 20% Ceramic Capacitor [Digikey: 587-1779-1-ND or 399-5506-1-ND]&lt;/li&gt;
&lt;/ul&gt;
&lt;/ul&gt;&lt;b&gt;1206&lt;/b&gt; - 1206 Surface Mount Capacitors
&lt;ul&gt;
&lt;li&gt;47uF 10V 20% Ceramic Capacitor [Digikey: 490-5528-1-ND or 399-5508-1-ND or 445-6010-1-ND]&lt;/li&gt;
&lt;li&gt;100uF 6.3V -20%, +80% Y5V Ceramic Capacitor (Digikey: 490-4512-1-ND, Mouser: 81-GRM31CF50J107ZE1L)&lt;/li&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="CAPACITOR"/>
</gates>
<devices>
<device name="0805" package="0805@1">
<connects>
<connect gate="G$1" pin="P$1" pad="1"/>
<connect gate="G$1" pin="P$2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="1206" package="1206@1">
<connects>
<connect gate="G$1" pin="P$1" pad="1"/>
<connect gate="G$1" pin="P$2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0603" package="0603@1">
<connects>
<connect gate="G$1" pin="P$1" pad="1"/>
<connect gate="G$1" pin="P$2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0402" package="0402@1">
<connects>
<connect gate="G$1" pin="P$1" pad="1"/>
<connect gate="G$1" pin="P$2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0603MINI" package="0603-MINI">
<connects>
<connect gate="G$1" pin="P$1" pad="1"/>
<connect gate="G$1" pin="P$2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0805-NOTHERMALS" package="0805_NOTHERMALS">
<connects>
<connect gate="G$1" pin="P$1" pad="1"/>
<connect gate="G$1" pin="P$2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_0402" package="_0402">
<connects>
<connect gate="G$1" pin="P$1" pad="1"/>
<connect gate="G$1" pin="P$2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_0402MP" package="_0402MP">
<connects>
<connect gate="G$1" pin="P$1" pad="1"/>
<connect gate="G$1" pin="P$2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_0603" package="_0603">
<connects>
<connect gate="G$1" pin="P$1" pad="1"/>
<connect gate="G$1" pin="P$2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_0603MP" package="_0603MP">
<connects>
<connect gate="G$1" pin="P$1" pad="1"/>
<connect gate="G$1" pin="P$2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_0805" package="_0805">
<connects>
<connect gate="G$1" pin="P$1" pad="1"/>
<connect gate="G$1" pin="P$2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_0805MP" package="_0805MP">
<connects>
<connect gate="G$1" pin="P$1" pad="1"/>
<connect gate="G$1" pin="P$2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="HEADER-1X1" prefix="JP" uservalue="yes">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="PINHD1"/>
</gates>
<devices>
<device name="" package="1X01_OVAL">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="ROUND" package="1X01_ROUND">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="2MM" package="1X01_2MM">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="2MM_OVAL" package="1X01_2MM_OVAL">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-SMD_MASKHELD_2X2MM" package="1X01_SMD_MASKHELD_2X2MM">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-SMD-MASKHELD_1X2MM" package="1X01_SMD_MASKHELD_1X2MM">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RESISTOR" prefix="R" uservalue="yes">
<description>&lt;p&gt;&lt;b&gt;Resistors&lt;/b&gt;&lt;/p&gt;
&lt;b&gt;0402&lt;/b&gt; - 0402 Surface Mount Package
&lt;ul&gt;
&lt;li&gt;22 Ohm 1% 1/16W [Digikey: 311-22.0LRTR-ND]&lt;/li&gt;
&lt;li&gt;33 Ohm 5% 1/16W&lt;/li&gt;
&lt;li&gt;1.0K 5% 1/16W&lt;/li&gt;
&lt;li&gt;1.5K 5% 1/16W&lt;/li&gt;
&lt;li&gt;2.0K 1% 1/16W&lt;/li&gt;
&lt;li&gt;10.0K 1% 1/16W [Digikey: 311-10.0KLRTR-ND]&lt;/li&gt;
&lt;li&gt;10.0K 5% 1/16W [Digikey: RMCF0402JT10K0TR-ND]&lt;/li&gt;
&lt;li&gt;12.1K 1% 1/16W [Digikey: 311-22.0LRTR-ND]&lt;/li&gt;
&lt;li&gt;100.0K 5% 1/16W&lt;/li&gt;
&lt;/ul&gt;
&lt;b&gt;0603&lt;/b&gt; - 0603 Surface Mount Package&lt;br&gt;
&lt;ul&gt;
&lt;li&gt;0 Ohm 1/10 Watt 1% Resistor&lt;/li&gt;
&lt;li&gt;15 Ohm 1/10 Watt 1% Resistor&lt;/li&gt;
&lt;li&gt;33 Ohm 1/10 Watt 1% Resistor&lt;/li&gt;
&lt;li&gt;49.9 Ohm 1/10 Watt 1% Resistor&lt;/li&gt;
&lt;li&gt;100 Ohm 1/10 Watt 1% Resistor&lt;/li&gt;
&lt;li&gt;150 Ohm 1/10 Watt 1% Resistor&lt;/li&gt;
&lt;li&gt;240 Ohm 1/10 Watt 1% Resistor&lt;/li&gt;
&lt;li&gt;390 Ohm 1/10 Watt 1% Resistor&lt;/li&gt;
&lt;li&gt;560 Ohm 1/10 Watt 1% Resistor&lt;/li&gt;
&lt;li&gt;680 Ohm 1/10 Watt 1% Resistor&lt;/li&gt;
&lt;li&gt;750 Ohm 1/10 Watt 1% Resistor&lt;/li&gt;
&lt;li&gt;1.0K Ohm 1/10 Watt 1% Resistor&lt;/li&gt;
&lt;li&gt;1.5K Ohm 1/10 Watt 1% Resistor&lt;/li&gt;
&lt;li&gt;2.0K Ohm 1/10 Watt 1% Resistor&lt;/li&gt;
&lt;li&gt;2.2K Ohm 1/10 Watt 1% Resistor&lt;/li&gt;
&lt;li&gt;3.3K Ohm 1/10 Watt 1% Resistor&lt;/li&gt;
&lt;li&gt;4.7K Ohm 1/10 Watt 1% Resistor&lt;/li&gt;
&lt;li&gt;10.0K Ohm 1/10 Watt 1% Resistor&lt;/li&gt;
&lt;li&gt;12.0K Ohm 1/10 Watt 1% Resistor&lt;/li&gt;
&lt;li&gt;12.1K Ohm 1/10 Watt 1% Resistor&lt;/li&gt;
&lt;li&gt;20.0K Ohm 1/10 Watt 1% Resistor&lt;/li&gt;
&lt;li&gt;33.0K Ohm 1/10 Watt 1% Resistor&lt;/li&gt;
&lt;li&gt;100.0K Ohm 1/10 Watt 1% Resistor&lt;/li&gt;
&lt;/ul&gt;
&lt;b&gt;0805&lt;/b&gt; - 0805 Surface Mount Package
&lt;ul&gt;
&lt;li&gt;0 Ohm 1/8 Watt 1% Resistor&lt;/li&gt;
&lt;li&gt;33 Ohm 1/8 Watt 1% Resistor&lt;/li&gt;
&lt;li&gt;100 Ohm 1/8 Watt 1% Resistor&lt;/li&gt;
&lt;li&gt;150 Ohm 1/8 Watt 1% Resistor&lt;/li&gt;
&lt;li&gt;200 Ohm 1/8 Watt 1% Resistor&lt;/li&gt;
&lt;li&gt;240 Ohm 1/8 Watt 1% Resistor&lt;/li&gt;
&lt;li&gt;330 Ohm 1/8 Watt 1% Resistor&lt;/li&gt;
&lt;li&gt;390 Ohm 1/8 Watt 1% Resistor&lt;/li&gt;
&lt;li&gt;470 Ohm 1/8 Watt 1% Resistor&lt;/li&gt;
&lt;li&gt;1.0K Ohm 1/8 Watt 1% Resistor&lt;/li&gt;
&lt;li&gt;1.5K Ohm 1/8 Watt 1% Resistor&lt;/li&gt;
&lt;li&gt;2.0K Ohm 1/8 Watt 1% Resistor&lt;/li&gt;
&lt;li&gt;4.7K Ohm 1/8 Watt 1% Resistor&lt;/li&gt;
&lt;li&gt;5.1K Ohm 1/8 Watt 1% Resistor&lt;/li&gt;
&lt;li&gt;5.6K Ohm 1/8 Watt 1% Resistor&lt;/li&gt;
&lt;li&gt;10.0K Ohm 1/8 Watt 1% Resistor&lt;/li&gt;
&lt;li&gt;22.0K Ohm 1/8 Watt 1% Resistor&lt;/li&gt;
&lt;li&gt;33.0K Ohm 1/8 Watt 1% Resistor&lt;/li&gt;
&lt;li&gt;100K Ohm 1/8 Watt 1% Resistor&lt;/li&gt;
&lt;/ul&gt;
&lt;b&gt;1206&lt;/b&gt; - 1206 Surface Mount Package&lt;br/&gt;
&lt;br/&gt;
&lt;b&gt;2012&lt;/b&gt; - 2010 Surface Mount Package&lt;br/&gt;
&lt;ul&gt;&lt;li&gt;0.11 Ohm 1/2 Watt 1% Resistor - Digikey: RHM.11UCT-ND&lt;/li&gt;&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="RESISTOR"/>
</gates>
<devices>
<device name="0805" package="0805">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="1206" package="1206">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0603" package="0603">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0402" package="0402">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0603MINI" package="0603-MINI@2">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="2012" package="2012">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0805_NOTHERMALS" package="0805_NOTHERMALS@2">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="2512" package="2512">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="VBUS">
<description>&lt;p&gt;VBUS Supply Symbole&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="VBUS"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SOLDERJUMPER" prefix="SJ" uservalue="yes">
<description>&lt;p&gt;&lt;b&gt;SMD Solder JUMPER&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;Solder the two pads together to create a connection, or remove the solder to break it.&lt;/p&gt;
&lt;b&gt;REFLOW&lt;/b&gt; - Use this footprint for solder paste and reflow ovens.&lt;br/&gt;
&lt;b&gt;WAVE&lt;/b&gt; - Use this footprint for hand-soldering (larger pads).
&lt;p&gt;&lt;b&gt;CLOSED&lt;/b&gt; - Has a trace between the two pads to ensure it is closed by default.  The trace needs to be cut to disable the jumper, and can be closed again by creating a solder bridge between the two pads.&lt;/p&gt;</description>
<gates>
<gate name="1" symbol="SOLDERJUMPER"/>
</gates>
<devices>
<device name="REFLOW" package="SOLDERJUMPER_REFLOW">
<connects>
<connect gate="1" pin="1" pad="1"/>
<connect gate="1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="WAVE" package="SOLDERJUMPER_WAVE">
<connects>
<connect gate="1" pin="1" pad="1"/>
<connect gate="1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="CLOSED" package="SOLDERJUMPER_CLOSEDWIRE">
<connects>
<connect gate="1" pin="1" pad="1"/>
<connect gate="1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="REFLOW_NOPASTE" package="SOLDERJUMPER_REFLOW_NOPASTE">
<connects>
<connect gate="1" pin="1" pad="1"/>
<connect gate="1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="" package="SOLDERJUMPER_ARROW_NOPASTE">
<connects>
<connect gate="1" pin="1" pad="1"/>
<connect gate="1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="BOM" value="EXCLUDE"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="USB_C" prefix="X" uservalue="yes">
<description>&lt;p&gt;&lt;b&gt;USB Type-C USB 2.0&lt;/b&gt; Connector&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="USB_C"/>
</gates>
<devices>
<device name="" package="USB_C_CUSB31-CFM2AX-01-X">
<connects>
<connect gate="G$1" pin="CC1" pad="A5"/>
<connect gate="G$1" pin="CC2" pad="B5"/>
<connect gate="G$1" pin="D+" pad="A6 B6"/>
<connect gate="G$1" pin="D-" pad="A7 B7"/>
<connect gate="G$1" pin="GND" pad="A1B12 B1A12"/>
<connect gate="G$1" pin="SBU1" pad="A8"/>
<connect gate="G$1" pin="SBU2" pad="B8"/>
<connect gate="G$1" pin="VBUS" pad="A4B9 B4A9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SMACONNECTOR" prefix="X" uservalue="yes">
<description>&lt;b&gt;SMA Connector&lt;/b&gt;
&lt;p&gt;90° DIP SMA Connector, 50 Ohm (4UConnector: 07259)&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="SMACONNECTOR"/>
</gates>
<devices>
<device name="" package="SMA90_DIP">
<connects>
<connect gate="G$1" pin="ANT" pad="ANTENNA"/>
<connect gate="G$1" pin="GND1" pad="GND1"/>
<connect gate="G$1" pin="GND2" pad="GND2"/>
<connect gate="G$1" pin="GND3" pad="GND3"/>
<connect gate="G$1" pin="GND4" pad="GND4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_EDGE" package="SMA_EDGELAUNCH">
<connects>
<connect gate="G$1" pin="ANT" pad="P"/>
<connect gate="G$1" pin="GND1" pad="GND@4"/>
<connect gate="G$1" pin="GND2" pad="GND@3"/>
<connect gate="G$1" pin="GND3" pad="GND@2"/>
<connect gate="G$1" pin="GND4" pad="GND@1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_EDGE_UFL" package="SMA_EDGELAUNCH_UFL">
<connects>
<connect gate="G$1" pin="ANT" pad="P"/>
<connect gate="G$1" pin="GND1" pad="GND@1"/>
<connect gate="G$1" pin="GND2" pad="GND@2"/>
<connect gate="G$1" pin="GND3" pad="GND@3"/>
<connect gate="G$1" pin="GND4" pad="GND@4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="USB_TYPEA" prefix="X" uservalue="yes">
<description>&lt;b&gt;USB - Type A Connectors&lt;/b&gt;
&lt;p&gt;Male types stick out and are inserted into a PC or matching females parts (these are the connectors used on USB Memory Sticks, etc.).  Female parts are generally used for USB Host and accept a male-type connector.&lt;/p&gt;
&lt;ul&gt;
&lt;li&gt;&lt;b&gt;SMT&lt;/b&gt; - 4UCON: 10017&lt;/li&gt;
&lt;li&gt;&lt;b&gt;PTHFML&lt;/b&gt; - Digikey: 609-1045-ND, 4UCon: 05241&lt;/li&gt;
&lt;li&gt;&lt;b&gt;PCB&lt;/b&gt; - Use 2.0mm thick PCBs with this footprint&lt;/li&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="USB_NOID"/>
</gates>
<devices>
<device name="" package="USB_A-SMT">
<connects>
<connect gate="G$1" pin="D+" pad="D+"/>
<connect gate="G$1" pin="D-" pad="D-"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="VBUS" pad="VBUS"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PTHFML" package="USB_HOST-PTH">
<connects>
<connect gate="G$1" pin="D+" pad="D+"/>
<connect gate="G$1" pin="D-" pad="D-"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="VBUS" pad="VBUS"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PCB" package="USBA_PCB">
<connects>
<connect gate="G$1" pin="D+" pad="USB_PLUS"/>
<connect gate="G$1" pin="D-" pad="USB_NEG"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="VBUS" pad="VCC"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_CLIENTTHM" package="USB_A-THM">
<connects>
<connect gate="G$1" pin="D+" pad="D+"/>
<connect gate="G$1" pin="D-" pad="D-"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="VBUS" pad="VBUS"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SPIFLASH_8PIN" prefix="U" uservalue="yes">
<description>&lt;b&gt;SOIC8 SPI Flash&lt;/b&gt;
&lt;p&gt;Be careful with the size since SOIC8 flash comes in several 'widths'&lt;/p&gt;
&lt;p&gt;&lt;b&gt;SOIC8 150 mil&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;&lt;b&gt;M25P16&lt;/b&gt; - 16Mbit (2Mbit x 8) Serial Flash (75MHz SPI Bus), Supply: 2.7-3.6V &lt;br/&gt;&lt;b&gt;Digikey: &lt;/b&gt; SOIC8 - M25P16-VMN6P-ND&lt;/li&gt;
&lt;/ul&gt;
&lt;/p&gt;

&lt;p&gt;&lt;b&gt;SOIC8 208 mil&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;&lt;b&gt;W25Q16BVSSIG&lt;/b&gt; - 16Mbit (2Mbit x 8) Serial Flash (104MHz SPI Bus), Supply: 2.7-3.6V &lt;br/&gt;&lt;b&gt;Digikey: &lt;/b&gt; SOIC8 - W25Q16BVSSIG-ND&lt;/li&gt;
&lt;/ul&gt;
&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="M25P16"/>
</gates>
<devices>
<device name="" package="SOIC8_150MIL">
<connects>
<connect gate="G$1" pin="HOLD#/IO3" pad="7"/>
<connect gate="G$1" pin="MISO" pad="2"/>
<connect gate="G$1" pin="MOSI" pad="5"/>
<connect gate="G$1" pin="SCK" pad="6"/>
<connect gate="G$1" pin="SSEL" pad="1"/>
<connect gate="G$1" pin="VCC" pad="8"/>
<connect gate="G$1" pin="VSS" pad="4"/>
<connect gate="G$1" pin="WP#/IO2" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="208MIL" package="SOIC8_208MIL">
<connects>
<connect gate="G$1" pin="HOLD#/IO3" pad="7"/>
<connect gate="G$1" pin="MISO" pad="2"/>
<connect gate="G$1" pin="MOSI" pad="5"/>
<connect gate="G$1" pin="SCK" pad="6"/>
<connect gate="G$1" pin="SSEL" pad="1"/>
<connect gate="G$1" pin="VCC" pad="8"/>
<connect gate="G$1" pin="VSS" pad="4"/>
<connect gate="G$1" pin="WP#/IO2" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="UX" package="USON8">
<connects>
<connect gate="G$1" pin="HOLD#/IO3" pad="7"/>
<connect gate="G$1" pin="MISO" pad="2"/>
<connect gate="G$1" pin="MOSI" pad="5"/>
<connect gate="G$1" pin="SCK" pad="6"/>
<connect gate="G$1" pin="SSEL" pad="1"/>
<connect gate="G$1" pin="VCC" pad="8"/>
<connect gate="G$1" pin="VSS" pad="4"/>
<connect gate="G$1" pin="WP#/IO2" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="APA102" uservalue="yes">
<description>&lt;p&gt;&lt;b&gt;APA102/DotStar Pixels&lt;/b&gt;&lt;/p&gt;

&lt;p&gt;
&lt;ul&gt;
&lt;li&gt;VCC: 5V DC&lt;/li&gt;
&lt;li&gt;Refresh Rate: 400Hz&lt;/li&gt;
&lt;/ul&gt;
&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="APA102"/>
</gates>
<devices>
<device name="" package="APA102">
<connects>
<connect gate="G$1" pin="CKI" pad="2"/>
<connect gate="G$1" pin="CKO" pad="5"/>
<connect gate="G$1" pin="DI" pad="1"/>
<connect gate="G$1" pin="DO" pad="6"/>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="VDD" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="2020" package="APA102_2020">
<connects>
<connect gate="G$1" pin="CKI" pad="5"/>
<connect gate="G$1" pin="CKO" pad="2"/>
<connect gate="G$1" pin="DI" pad="6"/>
<connect gate="G$1" pin="DO" pad="1"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="VDD" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATSAMD51G">
<gates>
<gate name="G$1" symbol="ATSAMD51G"/>
<gate name="G$3" symbol="THERMAL-SLUG"/>
</gates>
<devices>
<device name="_TQFN48" package="TQFN48_7MM">
<connects>
<connect gate="G$1" pin="/RESET" pad="40"/>
<connect gate="G$1" pin="GND" pad="18 35 42"/>
<connect gate="G$1" pin="GNDA" pad="5"/>
<connect gate="G$1" pin="PA00/EINT0/SERCOM1.0" pad="1"/>
<connect gate="G$1" pin="PA01/EINT1/SERCOM1.1" pad="2"/>
<connect gate="G$1" pin="PA02/EINT2/AIN0/VOUT0" pad="3"/>
<connect gate="G$1" pin="PA03/I3/VREFA/AIN1" pad="4"/>
<connect gate="G$1" pin="PA04/I4/VREFB/AIN4/SERCOM0.0" pad="9"/>
<connect gate="G$1" pin="PA05/I5/AIN5/VOUT1/SERCOM0.1" pad="10"/>
<connect gate="G$1" pin="PA06/I6/VREFC/AIN6/SERCOM0.2" pad="11"/>
<connect gate="G$1" pin="PA07/I7/AIN7/SERCOM0.3" pad="12"/>
<connect gate="G$1" pin="PA08/I2C/AIN8/SERCOM0.0+2.1/I2SMCK" pad="13"/>
<connect gate="G$1" pin="PA09/I2C/I9/AIN9/SERCOM0.1+2.0/I2SFS0" pad="14"/>
<connect gate="G$1" pin="PA10/I10/AIN10/SERCOM0+2.2/I2SCK" pad="15"/>
<connect gate="G$1" pin="PA11/I11/AIN11/SERCOM0+2.3/I2SDO" pad="16"/>
<connect gate="G$1" pin="PA12/I12/I2C/SERCOM2.0+4.1" pad="21"/>
<connect gate="G$1" pin="PA13/I13/I2C/SERCOM2.1+4.0" pad="22"/>
<connect gate="G$1" pin="PA14/I14/SERCOM2+4.2" pad="23"/>
<connect gate="G$1" pin="PA15/I15/SERCOM2+4.3" pad="24"/>
<connect gate="G$1" pin="PA16/I2C/I0/SERCOM1.0+3.1" pad="25"/>
<connect gate="G$1" pin="PA17/I2C/I1/SERCOM1.1+3.0" pad="26"/>
<connect gate="G$1" pin="PA18/I2/SERCOM1+3.2" pad="27"/>
<connect gate="G$1" pin="PA19/I3/SERCOM1+3.3" pad="28"/>
<connect gate="G$1" pin="PA20/I4/SERCOM3+5.2/I2SFS0" pad="29"/>
<connect gate="G$1" pin="PA21/I5/SERCOM3+5.3/I2SDO" pad="30"/>
<connect gate="G$1" pin="PA22/I2C/I6/SERCOM3.0+5.1/I2SDI" pad="31"/>
<connect gate="G$1" pin="PA23/I2C/I7/SERCOM3.1+5.0/SOF/I2SFS1" pad="32"/>
<connect gate="G$1" pin="PA24/I8/SERCOM3+5.2/D-" pad="33"/>
<connect gate="G$1" pin="PA25/I9/SERCOM3+5.3/D+" pad="34"/>
<connect gate="G$1" pin="PA27/I11" pad="39"/>
<connect gate="G$1" pin="PA30/I14/SECOM1.2/SWCLK" pad="45"/>
<connect gate="G$1" pin="PA31/I15/SECOM1.3/SWDIO" pad="46"/>
<connect gate="G$1" pin="PB02/I2/AIN14/SERCOM5.0" pad="47"/>
<connect gate="G$1" pin="PB03/I3/AIN15/SERCOM5.1" pad="48"/>
<connect gate="G$1" pin="PB08/I8/AIN2/SERCOM4.0" pad="7"/>
<connect gate="G$1" pin="PB09/I9/AIN3/SERCOM4.1" pad="8"/>
<connect gate="G$1" pin="PB10/I10/SERCOM4.2/I2SDI" pad="19"/>
<connect gate="G$1" pin="PB11/I11/SERCOM4.3/I2SFS1" pad="20"/>
<connect gate="G$1" pin="PB22/I6/SERCOM1+5.2" pad="37"/>
<connect gate="G$1" pin="PB23/I7/SERCOM1+5.3" pad="38"/>
<connect gate="G$1" pin="VDDA" pad="6"/>
<connect gate="G$1" pin="VDDCORE" pad="41"/>
<connect gate="G$1" pin="VDDIO" pad="17 36 44"/>
<connect gate="G$1" pin="VSW" pad="43"/>
<connect gate="G$3" pin="TP" pad="THERMAL"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="VREG_SOT23-5" prefix="U" uservalue="yes">
<description>&lt;p&gt;&lt;b&gt;SOT23-5 Fixed Voltage Regulators&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;&lt;/p&gt;
&lt;table width="700"&gt;
&lt;tr bgcolor="#EEEEEE" &gt;
&lt;td&gt;&lt;b&gt;Part&lt;/b&gt;&lt;/td&gt;
&lt;td&gt;&lt;b&gt;Current Out&lt;/b&gt;&lt;/td&gt;
&lt;td&gt;&lt;b&gt;V Out&lt;/b&gt;&lt;/td&gt;
&lt;td&gt;&lt;b&gt;V In&lt;/b&gt;&lt;/td&gt;
&lt;td&gt;&lt;b&gt;V Dropout&lt;/b&gt;&lt;/td&gt;
&lt;td&gt;&lt;b&gt;θJA (°C/W)&lt;/b&gt;&lt;/td&gt;
&lt;td&gt;&lt;b&gt;TJ (°C)&lt;/b&gt;&lt;/td&gt;
&lt;td&gt;&lt;b&gt;Digikey Part No.&lt;/b&gt;&lt;/td&gt;
&lt;/tr&gt;
&lt;tr&gt;
  &lt;td&gt;ADP121&lt;/td&gt;
  &lt;td&gt;150mA&lt;/td&gt;
  &lt;td&gt;&lt;b&gt;3.3V&lt;/b&gt;&lt;/td&gt;
  &lt;td&gt;3.4-5.5V&lt;/td&gt;
  &lt;td&gt;0.09V @ 150mA&lt;/td&gt;
  &lt;td&gt;--&lt;/td&gt;
  &lt;td&gt;--&lt;/td&gt;
  &lt;td&gt;ADP121-AUJZ33R7CT-ND&lt;/td&gt;
&lt;/tr&gt;
&lt;tr&gt;
  &lt;td&gt;ADP121&lt;/td&gt;
  &lt;td&gt;150mA&lt;/td&gt;
  &lt;td&gt;&lt;b&gt;3.0V&lt;/b&gt;&lt;/td&gt;
  &lt;td&gt;3.1-5.5V&lt;/td&gt;
  &lt;td&gt;0.09V @ 150mA&lt;/td&gt;
  &lt;td&gt;--&lt;/td&gt;
  &lt;td&gt;--&lt;/td&gt;
  &lt;td&gt;ADP121-AUJZ30R7CT-ND&lt;/td&gt;
&lt;/tr&gt;
&lt;tr&gt;
  &lt;td&gt;ADP122&lt;/td&gt;
  &lt;td&gt;&lt;strong&gt;300mA&lt;/strong&gt;&lt;/td&gt;
  &lt;td&gt;&lt;b&gt;3.3V&lt;/b&gt;&lt;/td&gt;
  &lt;td&gt;3.4-5.5V&lt;/td&gt;
  &lt;td&gt;0.085V @ 300mA&lt;/td&gt;
  &lt;td&gt;--&lt;/td&gt;
  &lt;td&gt;--&lt;/td&gt;
  &lt;td&gt;ADP122AUJZ-3.3-R7CT-ND&lt;/td&gt;
&lt;/tr&gt;
&lt;tr&gt;
  &lt;td&gt;ADP1712&lt;/td&gt;
  &lt;td&gt;&lt;strong&gt;300mA&lt;/strong&gt;&lt;/td&gt;
  &lt;td&gt;&lt;b&gt;3.3V&lt;/b&gt;&lt;/td&gt;
  &lt;td&gt;3.5-5.5V&lt;/td&gt;
  &lt;td&gt;0.17V @ 300mA&lt;/td&gt;
  &lt;td&gt;--&lt;/td&gt;
  &lt;td&gt;--&lt;/td&gt;
  &lt;td&gt;ADP1712AUJZ-3.3-R7TR-ND&lt;/td&gt;
&lt;/tr&gt;
&lt;tr&gt;
  &lt;td&gt;AP7311 (&lt;b&gt;Low Cost&lt;/b&gt;)&lt;/td&gt;
  &lt;td&gt;150mA&lt;/td&gt;
  &lt;td&gt;&lt;b&gt;3.3V&lt;/b&gt;&lt;/td&gt;
  &lt;td&gt;3.5-6V&lt;/td&gt;
  &lt;td&gt;0.15V @ 150mA&lt;/td&gt;
  &lt;td&gt;--&lt;/td&gt;
  &lt;td&gt;--&lt;/td&gt;
  &lt;td&gt;AP7311-33WG-7DICT-ND&lt;/td&gt;
&lt;/tr&gt;

&lt;tr&gt;
  &lt;td&gt;LD39015M18R&lt;/td&gt;
  &lt;td&gt;150mA&lt;/td&gt;
  &lt;td&gt;&lt;b&gt;1.8V&lt;/b&gt;&lt;/td&gt;
  &lt;td&gt;1.9V-5.5V&lt;/td&gt;
  &lt;td&gt;0.08V @ 100mA&lt;/td&gt;
  &lt;td&gt;--&lt;/td&gt;
  &lt;td&gt;--&lt;/td&gt;
  &lt;td&gt;497-6977-1-ND&lt;/td&gt;
&lt;/tr&gt;

&lt;tr&gt;
  &lt;td&gt;LP2985A-33DBVR&lt;/td&gt;
  &lt;td&gt;150mA&lt;/td&gt;
  &lt;td&gt;&lt;b&gt;3.3V&lt;/b&gt;&lt;/td&gt;
  &lt;td&gt;3.3-16V&lt;/td&gt;
  &lt;td&gt;0.28V @ 150mA&lt;/td&gt;
  &lt;td&gt;206&lt;/td&gt;
  &lt;td&gt;150&lt;/td&gt;
  &lt;td&gt;296-18479-1-ND&lt;/td&gt;
&lt;/tr&gt;

&lt;tr&gt;
  &lt;td&gt;MCP1824T-3302E/OT&lt;/td&gt;
  &lt;td&gt;&lt;b&gt;300mA&lt;/b&gt;&lt;/td&gt;
  &lt;td&gt;&lt;b&gt;3.3V&lt;/b&gt;&lt;/td&gt;
  &lt;td&gt;3.5V-6V&lt;/td&gt;
  &lt;td&gt;0.2V @ 300mA&lt;/td&gt;
  &lt;td&gt;--&lt;/td&gt;
  &lt;td&gt;--&lt;/td&gt;
  &lt;td&gt;MCP1824T-3302E/OTCT-ND&lt;/td&gt;
&lt;/tr&gt;

&lt;tr&gt;
  &lt;td&gt;MIC5205-2.5YM5 TR&lt;/td&gt;
  &lt;td&gt;150mA&lt;/td&gt;
  &lt;td&gt;&lt;b&gt;2.5V&lt;/b&gt;&lt;/td&gt;
  &lt;td&gt;2.7-16V&lt;/td&gt;
  &lt;td&gt;0.165V @ 150mA&lt;/td&gt;
  &lt;td&gt;--&lt;/td&gt;
  &lt;td&gt;--&lt;/td&gt;
  &lt;td&gt;576-1257-2-ND&lt;/td&gt;
&lt;/tr&gt;
&lt;tr&gt;
  &lt;td&gt;MIC5205-3.0YM5 TR&lt;/td&gt;
  &lt;td&gt;150mA&lt;/td&gt;
  &lt;td&gt;&lt;b&gt;3.0V&lt;/b&gt;&lt;/td&gt;
  &lt;td&gt;3.2V-16V&lt;/td&gt;
  &lt;td&gt;0.165V @ 150mA&lt;/td&gt;
  &lt;td&gt;--&lt;/td&gt;
  &lt;td&gt;--&lt;/td&gt;
  &lt;td&gt;576-1258-2-ND&lt;/td&gt;
&lt;/tr&gt;
&lt;tr&gt;
  &lt;td&gt;MIC5205-3.3YM5 TR&lt;/td&gt;
  &lt;td&gt;150mA&lt;/td&gt;
  &lt;td&gt;&lt;b&gt;3.3V&lt;/b&gt;&lt;/td&gt;
  &lt;td&gt;3.5V-16V&lt;/td&gt;
  &lt;td&gt;0.165V @ 150mA&lt;/td&gt;
  &lt;td&gt;--&lt;/td&gt;
  &lt;td&gt;--&lt;/td&gt;
  &lt;td&gt;576-1259-2-ND&lt;/td&gt;
&lt;/tr&gt;
&lt;tr&gt;
  &lt;td&gt;TPS780330220&lt;/td&gt;
  &lt;td&gt;150mA&lt;/td&gt;
  &lt;td&gt;&lt;b&gt;3.3V+2.2V&lt;/b&gt;&lt;/td&gt;
  &lt;td&gt;3.6-5.5V&lt;/td&gt;
  &lt;td&gt;250mV Max&lt;/td&gt;
  &lt;td&gt;--&lt;/td&gt;
  &lt;td&gt;--&lt;/td&gt;
  &lt;td&gt;296-23332-1-ND&lt;/td&gt;
&lt;/tr&gt;
&lt;tr&gt;
  &lt;td&gt;TDA3663/N1,135&lt;/td&gt;
  &lt;td&gt;100mA&lt;/td&gt;
  &lt;td&gt;&lt;b&gt;3.3V&lt;/b&gt;&lt;/td&gt;
  &lt;td&gt;3.5-&lt;b&gt;45V&lt;/b&gt;&lt;/td&gt;
  &lt;td&gt;0.18V @ 50mA&lt;/td&gt;
  &lt;td&gt;--&lt;/td&gt;
  &lt;td&gt;--&lt;/td&gt;
  &lt;td&gt;568-5343-1-ND&lt;/td&gt;
&lt;/tr&gt;
&lt;tr&gt;
  &lt;td&gt;&lt;/td&gt;
  &lt;td&gt;&lt;/td&gt;
  &lt;td&gt;&lt;/td&gt;
  &lt;td&gt;&lt;/td&gt;
  &lt;td&gt;&lt;/td&gt;
  &lt;td&gt;&lt;/td&gt;
  &lt;td&gt;&lt;/td&gt;
  &lt;td&gt;&lt;/td&gt;
&lt;/tr&gt;
&lt;tr&gt;
  &lt;td&gt;&lt;/td&gt;
  &lt;td&gt;&lt;/td&gt;
  &lt;td&gt;&lt;/td&gt;
  &lt;td&gt;&lt;/td&gt;
  &lt;td&gt;&lt;/td&gt;
  &lt;td&gt;&lt;/td&gt;
  &lt;td&gt;&lt;/td&gt;
  &lt;td&gt;&lt;/td&gt;
&lt;/tr&gt;

&lt;/table&gt;
&lt;p&gt;Max operating temp can be calculated using θJA, TJ (max junction temperature), and power in watts.  Set the "Maximum Ambient Temperature" until it reaches TJ ("Max Junction Temperature"), which is the absolute limit for safe use of the regulator: &lt;a href="http://www.daycounter.com/Calculators/Heat-Sink-Temperature-Calculator.phtml"&gt;Heat Sink Temperature Calculator&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;For example, With 12V source into a 3.3V LP2985 and a 30mA load, we are dissipating (12V-3.3V) * 0.03A = 0.261W.  With a θJA of 206 °C/W, a TJ of 150°C, and 261mW we can safely use the chip without a heat sink up to 75°C (=147.1°C Junction Temperature).&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="VREG_SOT23-5"/>
</gates>
<devices>
<device name="" package="SOT23-5">
<connects>
<connect gate="G$1" pin="EN" pad="3"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="IN" pad="1"/>
<connect gate="G$1" pin="OUT" pad="5"/>
<connect gate="G$1" pin="P4" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
<library name="frames">
<description>&lt;b&gt;Frames for Sheet and Layout&lt;/b&gt;</description>
<packages>
</packages>
<symbols>
<symbol name="FRAME_A_L">
</symbol>
<symbol name="DOCFIELD">
</symbol>
</symbols>
<devicesets>
<deviceset name="FRAME_A_L" prefix="FRAME" uservalue="yes">
<description>&lt;b&gt;FRAME&lt;/b&gt; A Size , 8 1/2 x 11 INCH, Landscape&lt;p&gt;</description>
<gates>
<gate name="G$1" symbol="FRAME_A_L"/>
<gate name="G$2" symbol="DOCFIELD"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
<library name="supply1">
<packages>
</packages>
<symbols>
<symbol name="GND">
<pin name="GND" direction="sup"/>
</symbol>
<symbol name="+3V3">
<pin name="+3V3" direction="sup"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="GND" prefix="GND">
<description>&lt;b&gt;SUPPLY SYMBOL&lt;/b&gt;</description>
<gates>
<gate name="1" symbol="GND"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="+3V3" prefix="+3V3">
<description>&lt;b&gt;SUPPLY SYMBOL&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="+3V3"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
<library name="testpad">
<description>&lt;b&gt;Test Pins/Pads&lt;/b&gt;&lt;p&gt;
Cream on SMD OFF.&lt;br&gt;
new: Attribute TP_SIGNAL_NAME&lt;br&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="B1,27">
<description>&lt;b&gt;TEST PAD&lt;/b&gt;</description>
</package>
<package name="B2,54">
<description>&lt;b&gt;TEST PAD&lt;/b&gt;</description>
</package>
<package name="P1-13">
<description>&lt;b&gt;TEST PAD&lt;/b&gt;</description>
</package>
<package name="P1-13Y">
<description>&lt;b&gt;TEST PAD&lt;/b&gt;</description>
</package>
<package name="P1-17">
<description>&lt;b&gt;TEST PAD&lt;/b&gt;</description>
</package>
<package name="P1-17Y">
<description>&lt;b&gt;TEST PAD&lt;/b&gt;</description>
</package>
<package name="P1-20">
<description>&lt;b&gt;TEST PAD&lt;/b&gt;</description>
</package>
<package name="P1-20Y">
<description>&lt;b&gt;TEST PAD&lt;/b&gt;</description>
</package>
<package name="TP06R">
<description>&lt;b&gt;TEST PAD&lt;/b&gt;</description>
</package>
<package name="TP06SQ">
<description>&lt;b&gt;TEST PAD&lt;/b&gt;</description>
</package>
<package name="TP07R">
<description>&lt;b&gt;TEST PAD&lt;/b&gt;</description>
</package>
<package name="TP07SQ">
<description>&lt;b&gt;TEST PAD&lt;/b&gt;</description>
</package>
<package name="TP08R">
<description>&lt;b&gt;TEST PAD&lt;/b&gt;</description>
</package>
<package name="TP08SQ">
<description>&lt;b&gt;TEST PAD&lt;/b&gt;</description>
</package>
<package name="TP09R">
<description>&lt;b&gt;TEST PAD&lt;/b&gt;</description>
</package>
<package name="TP09SQ">
<description>&lt;b&gt;TEST PAD&lt;/b&gt;</description>
</package>
<package name="TP10R">
<description>&lt;b&gt;TEST PAD&lt;/b&gt;</description>
</package>
<package name="TP10SQ">
<description>&lt;b&gt;TEST PAD&lt;/b&gt;</description>
</package>
<package name="TP11R">
<description>&lt;b&gt;TEST PAD&lt;/b&gt;</description>
</package>
<package name="TP11SQ">
<description>&lt;b&gt;TEST PAD&lt;/b&gt;</description>
</package>
<package name="TP12SQ">
<description>&lt;b&gt;TEST PAD&lt;/b&gt;</description>
</package>
<package name="TP12R">
<description>&lt;b&gt;TEST PAD&lt;/b&gt;</description>
</package>
<package name="TP13R">
<description>&lt;b&gt;TEST PAD&lt;/b&gt;</description>
</package>
<package name="TP14R">
<description>&lt;b&gt;TEST PAD&lt;/b&gt;</description>
</package>
<package name="TP15R">
<description>&lt;b&gt;TEST PAD&lt;/b&gt;</description>
</package>
<package name="TP16R">
<description>&lt;b&gt;TEST PAD&lt;/b&gt;</description>
</package>
<package name="TP17R">
<description>&lt;b&gt;TEST PAD&lt;/b&gt;</description>
</package>
<package name="TP18R">
<description>&lt;b&gt;TEST PAD&lt;/b&gt;</description>
</package>
<package name="TP19R">
<description>&lt;b&gt;TEST PAD&lt;/b&gt;</description>
</package>
<package name="TP20R">
<description>&lt;b&gt;TEST PAD&lt;/b&gt;</description>
</package>
<package name="TP13SQ">
<description>&lt;b&gt;TEST PAD&lt;/b&gt;</description>
</package>
<package name="TP14SQ">
<description>&lt;b&gt;TEST PAD&lt;/b&gt;</description>
</package>
<package name="TP15SQ">
<description>&lt;b&gt;TEST PAD&lt;/b&gt;</description>
</package>
<package name="TP16SQ">
<description>&lt;b&gt;TEST PAD&lt;/b&gt;</description>
</package>
<package name="TP17SQ">
<description>&lt;b&gt;TEST PAD&lt;/b&gt;</description>
</package>
<package name="TP18SQ">
<description>&lt;b&gt;TEST PAD&lt;/b&gt;</description>
</package>
<package name="TP19SQ">
<description>&lt;b&gt;TEST PAD&lt;/b&gt;</description>
</package>
<package name="TP20SQ">
<description>&lt;b&gt;TEST PAD&lt;/b&gt;</description>
</package>
</packages>
<symbols>
<symbol name="TP">
<pin name="TP" direction="in"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="TP" prefix="TP">
<description>&lt;b&gt;Test pad&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="TP"/>
</gates>
<devices>
<device name="B1,27" package="B1,27">
<connects>
<connect gate="G$1" pin="TP" pad="TP"/>
</connects>
<technologies>
<technology name="">
<attribute name="TP_SIGNAL_NAME" value=""/>
</technology>
</technologies>
</device>
<device name="B2,54" package="B2,54">
<connects>
<connect gate="G$1" pin="TP" pad="TP"/>
</connects>
<technologies>
<technology name="">
<attribute name="TP_SIGNAL_NAME" value=""/>
</technology>
</technologies>
</device>
<device name="PAD1-13" package="P1-13">
<connects>
<connect gate="G$1" pin="TP" pad="TP"/>
</connects>
<technologies>
<technology name="">
<attribute name="TP_SIGNAL_NAME" value=""/>
</technology>
</technologies>
</device>
<device name="PAD1-13Y" package="P1-13Y">
<connects>
<connect gate="G$1" pin="TP" pad="TP"/>
</connects>
<technologies>
<technology name="">
<attribute name="TP_SIGNAL_NAME" value=""/>
</technology>
</technologies>
</device>
<device name="PAD1-17" package="P1-17">
<connects>
<connect gate="G$1" pin="TP" pad="TP"/>
</connects>
<technologies>
<technology name="">
<attribute name="TP_SIGNAL_NAME" value=""/>
</technology>
</technologies>
</device>
<device name="PAD1-17Y" package="P1-17Y">
<connects>
<connect gate="G$1" pin="TP" pad="TP"/>
</connects>
<technologies>
<technology name="">
<attribute name="TP_SIGNAL_NAME" value=""/>
</technology>
</technologies>
</device>
<device name="PAD1-20" package="P1-20">
<connects>
<connect gate="G$1" pin="TP" pad="TP"/>
</connects>
<technologies>
<technology name="">
<attribute name="TP_SIGNAL_NAME" value=""/>
</technology>
</technologies>
</device>
<device name="PAD1-20Y" package="P1-20Y">
<connects>
<connect gate="G$1" pin="TP" pad="TP"/>
</connects>
<technologies>
<technology name="">
<attribute name="TP_SIGNAL_NAME" value=""/>
</technology>
</technologies>
</device>
<device name="TP06R" package="TP06R">
<connects>
<connect gate="G$1" pin="TP" pad="TP"/>
</connects>
<technologies>
<technology name="">
<attribute name="TP_SIGNAL_NAME" value=""/>
</technology>
</technologies>
</device>
<device name="TP06SQ" package="TP06SQ">
<connects>
<connect gate="G$1" pin="TP" pad="TP"/>
</connects>
<technologies>
<technology name="">
<attribute name="TP_SIGNAL_NAME" value=""/>
</technology>
</technologies>
</device>
<device name="TP07R" package="TP07R">
<connects>
<connect gate="G$1" pin="TP" pad="TP"/>
</connects>
<technologies>
<technology name="">
<attribute name="TP_SIGNAL_NAME" value=""/>
</technology>
</technologies>
</device>
<device name="TP07SQ" package="TP07SQ">
<connects>
<connect gate="G$1" pin="TP" pad="TP"/>
</connects>
<technologies>
<technology name="">
<attribute name="TP_SIGNAL_NAME" value=""/>
</technology>
</technologies>
</device>
<device name="TP08R" package="TP08R">
<connects>
<connect gate="G$1" pin="TP" pad="TP"/>
</connects>
<technologies>
<technology name="">
<attribute name="TP_SIGNAL_NAME" value=""/>
</technology>
</technologies>
</device>
<device name="TP08SQ" package="TP08SQ">
<connects>
<connect gate="G$1" pin="TP" pad="TP"/>
</connects>
<technologies>
<technology name="">
<attribute name="TP_SIGNAL_NAME" value=""/>
</technology>
</technologies>
</device>
<device name="TP09R" package="TP09R">
<connects>
<connect gate="G$1" pin="TP" pad="TP"/>
</connects>
<technologies>
<technology name="">
<attribute name="TP_SIGNAL_NAME" value=""/>
</technology>
</technologies>
</device>
<device name="TP09SQ" package="TP09SQ">
<connects>
<connect gate="G$1" pin="TP" pad="TP"/>
</connects>
<technologies>
<technology name="">
<attribute name="TP_SIGNAL_NAME" value=""/>
</technology>
</technologies>
</device>
<device name="TP10R" package="TP10R">
<connects>
<connect gate="G$1" pin="TP" pad="TP"/>
</connects>
<technologies>
<technology name="">
<attribute name="TP_SIGNAL_NAME" value=""/>
</technology>
</technologies>
</device>
<device name="TP10SQ" package="TP10SQ">
<connects>
<connect gate="G$1" pin="TP" pad="TP"/>
</connects>
<technologies>
<technology name="">
<attribute name="TP_SIGNAL_NAME" value=""/>
</technology>
</technologies>
</device>
<device name="TP11R" package="TP11R">
<connects>
<connect gate="G$1" pin="TP" pad="TP"/>
</connects>
<technologies>
<technology name="">
<attribute name="TP_SIGNAL_NAME" value=""/>
</technology>
</technologies>
</device>
<device name="TP11SQ" package="TP11SQ">
<connects>
<connect gate="G$1" pin="TP" pad="TP"/>
</connects>
<technologies>
<technology name="">
<attribute name="TP_SIGNAL_NAME" value=""/>
</technology>
</technologies>
</device>
<device name="TP12SQ" package="TP12SQ">
<connects>
<connect gate="G$1" pin="TP" pad="TP"/>
</connects>
<technologies>
<technology name="">
<attribute name="TP_SIGNAL_NAME" value=""/>
</technology>
</technologies>
</device>
<device name="TP12R" package="TP12R">
<connects>
<connect gate="G$1" pin="TP" pad="TP"/>
</connects>
<technologies>
<technology name="">
<attribute name="TP_SIGNAL_NAME" value=""/>
</technology>
</technologies>
</device>
<device name="TP13R" package="TP13R">
<connects>
<connect gate="G$1" pin="TP" pad="TP"/>
</connects>
<technologies>
<technology name="">
<attribute name="TP_SIGNAL_NAME" value=""/>
</technology>
</technologies>
</device>
<device name="TP14R" package="TP14R">
<connects>
<connect gate="G$1" pin="TP" pad="TP"/>
</connects>
<technologies>
<technology name="">
<attribute name="TP_SIGNAL_NAME" value=""/>
</technology>
</technologies>
</device>
<device name="TP15R" package="TP15R">
<connects>
<connect gate="G$1" pin="TP" pad="TP"/>
</connects>
<technologies>
<technology name="">
<attribute name="TP_SIGNAL_NAME" value=""/>
</technology>
</technologies>
</device>
<device name="TP16R" package="TP16R">
<connects>
<connect gate="G$1" pin="TP" pad="TP"/>
</connects>
<technologies>
<technology name="">
<attribute name="TP_SIGNAL_NAME" value=""/>
</technology>
</technologies>
</device>
<device name="TP17R" package="TP17R">
<connects>
<connect gate="G$1" pin="TP" pad="TP"/>
</connects>
<technologies>
<technology name="">
<attribute name="TP_SIGNAL_NAME" value=""/>
</technology>
</technologies>
</device>
<device name="TP18R" package="TP18R">
<connects>
<connect gate="G$1" pin="TP" pad="TP"/>
</connects>
<technologies>
<technology name="">
<attribute name="TP_SIGNAL_NAME" value=""/>
</technology>
</technologies>
</device>
<device name="TP19R" package="TP19R">
<connects>
<connect gate="G$1" pin="TP" pad="TP"/>
</connects>
<technologies>
<technology name="">
<attribute name="TP_SIGNAL_NAME" value=""/>
</technology>
</technologies>
</device>
<device name="TP20R" package="TP20R">
<connects>
<connect gate="G$1" pin="TP" pad="TP"/>
</connects>
<technologies>
<technology name="">
<attribute name="TP_SIGNAL_NAME" value=""/>
</technology>
</technologies>
</device>
<device name="TP13SQ" package="TP13SQ">
<connects>
<connect gate="G$1" pin="TP" pad="TP"/>
</connects>
<technologies>
<technology name="">
<attribute name="TP_SIGNAL_NAME" value=""/>
</technology>
</technologies>
</device>
<device name="TP14SQ" package="TP14SQ">
<connects>
<connect gate="G$1" pin="TP" pad="TP"/>
</connects>
<technologies>
<technology name="">
<attribute name="TP_SIGNAL_NAME" value=""/>
</technology>
</technologies>
</device>
<device name="TP15SQ" package="TP15SQ">
<connects>
<connect gate="G$1" pin="TP" pad="TP"/>
</connects>
<technologies>
<technology name="">
<attribute name="TP_SIGNAL_NAME" value=""/>
</technology>
</technologies>
</device>
<device name="TP16SQ" package="TP16SQ">
<connects>
<connect gate="G$1" pin="TP" pad="TP"/>
</connects>
<technologies>
<technology name="">
<attribute name="TP_SIGNAL_NAME" value=""/>
</technology>
</technologies>
</device>
<device name="TP17SQ" package="TP17SQ">
<connects>
<connect gate="G$1" pin="TP" pad="TP"/>
</connects>
<technologies>
<technology name="">
<attribute name="TP_SIGNAL_NAME" value=""/>
</technology>
</technologies>
</device>
<device name="TP18SQ" package="TP18SQ">
<connects>
<connect gate="G$1" pin="TP" pad="TP"/>
</connects>
<technologies>
<technology name="">
<attribute name="TP_SIGNAL_NAME" value=""/>
</technology>
</technologies>
</device>
<device name="TP19SQ" package="TP19SQ">
<connects>
<connect gate="G$1" pin="TP" pad="TP"/>
</connects>
<technologies>
<technology name="">
<attribute name="TP_SIGNAL_NAME" value=""/>
</technology>
</technologies>
</device>
<device name="TP20SQ" package="TP20SQ">
<connects>
<connect gate="G$1" pin="TP" pad="TP"/>
</connects>
<technologies>
<technology name="">
<attribute name="TP_SIGNAL_NAME" value=""/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
<library name="USB_Type_C_12P">
<packages>
<package name="USB_TYPE_C_12P">
</package>
</packages>
<symbols>
<symbol name="USB_TYPE_C_12P">
<pin name="VBUS_A" direction="pwr"/>
<pin name="CC"/>
<pin name="D+"/>
<pin name="D-"/>
<pin name="RX2-"/>
<pin name="RX2+"/>
<pin name="GNDA" direction="pwr"/>
<pin name="VBUS_B" direction="pwr"/>
<pin name="VCONN"/>
<pin name="TX2-"/>
<pin name="TX2+"/>
<pin name="GNDB" direction="pwr"/>
<pin name="SHIELD1" direction="pas"/>
<pin name="SHIELD2" direction="pas"/>
<pin name="SHIELD3" direction="pas"/>
<pin name="SHIELD4" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="USB_TYPE_C_12P" prefix="J">
<description>USB-C (USB TYPE-C) USB 2.0</description>
<gates>
<gate name="G$1" symbol="USB_TYPE_C_12P"/>
</gates>
<devices>
<device name="USB_TYPE_C_12P" package="USB_TYPE_C_12P">
<connects>
<connect gate="G$1" pin="CC" pad="A5"/>
<connect gate="G$1" pin="D+" pad="A6"/>
<connect gate="G$1" pin="D-" pad="A7"/>
<connect gate="G$1" pin="GNDA" pad="A1"/>
<connect gate="G$1" pin="GNDB" pad="B12"/>
<connect gate="G$1" pin="RX2+" pad="A11"/>
<connect gate="G$1" pin="RX2-" pad="A10"/>
<connect gate="G$1" pin="SHIELD1" pad="S1 S2"/>
<connect gate="G$1" pin="SHIELD2" pad="S3 S4"/>
<connect gate="G$1" pin="SHIELD3" pad="S5"/>
<connect gate="G$1" pin="SHIELD4" pad="S6"/>
<connect gate="G$1" pin="TX2+" pad="B2"/>
<connect gate="G$1" pin="TX2-" pad="B3"/>
<connect gate="G$1" pin="VBUS_A" pad="A4"/>
<connect gate="G$1" pin="VBUS_B" pad="B9"/>
<connect gate="G$1" pin="VCONN" pad="B5"/>
</connects>
<technologies>
<technology name="">
<attribute name="AVAILABILITY" value="In Stock"/>
<attribute name="DESCRIPTION" value=" USB-C (USB TYPE-C) USB 2.0"/>
<attribute name="MP" value="USB_Type_C_12P"/>
<attribute name="PACKAGE" value="None"/>
<attribute name="PRICE" value="None"/>
<attribute name="PURCHASE-URL" value="adafruit.com"/>
<attribute name="XFL" value="xflconn"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<parts>
<part name="U1" library="microbuilder" deviceset="RFM69HCW" device="_SMT" value="RFM98-W"/>
<part name="U$4" library="microbuilder" deviceset="GND" device=""/>
<part name="+3V3" library="microbuilder" deviceset="3.3V" device=""/>
<part name="C1" library="microbuilder" deviceset="CAP_CERAMIC" device="0603" value="10uF"/>
<part name="U$6" library="microbuilder" deviceset="GND" device=""/>
<part name="ANTENNA" library="microbuilder" deviceset="HEADER-1X1" device="ROUND"/>
<part name="FRAME1" library="frames" deviceset="FRAME_A_L" device=""/>
<part name="C6" library="microbuilder" deviceset="CAP_CERAMIC" device="0603" value="10µF"/>
<part name="U$27" library="microbuilder" deviceset="GND" device=""/>
<part name="U$30" library="microbuilder" deviceset="GND" device=""/>
<part name="GND7" library="supply1" deviceset="GND" device=""/>
<part name="U$3" library="microbuilder" deviceset="VBUS" device=""/>
<part name="GND8" library="supply1" deviceset="GND" device=""/>
<part name="+3V7" library="supply1" deviceset="+3V3" device=""/>
<part name="+3V8" library="supply1" deviceset="+3V3" device=""/>
<part name="P3V" library="testpad" deviceset="TP" device="TP20R"/>
<part name="PGND" library="testpad" deviceset="TP" device="TP20R"/>
<part name="PCLK" library="testpad" deviceset="TP" device="TP20R"/>
<part name="PIO" library="testpad" deviceset="TP" device="TP20R" value="TPTP20R"/>
<part name="PI3V" library="testpad" deviceset="TP" device="PAD1-13"/>
<part name="PIGND" library="testpad" deviceset="TP" device="PAD1-13"/>
<part name="PICLK" library="testpad" deviceset="TP" device="PAD1-13"/>
<part name="PIIO" library="testpad" deviceset="TP" device="PAD1-13"/>
<part name="+3V1" library="supply1" deviceset="+3V3" device=""/>
<part name="U$5" library="microbuilder" deviceset="GND" device=""/>
<part name="RESET" library="microbuilder" deviceset="SOLDERJUMPER" device=""/>
<part name="USB_C2" library="microbuilder" deviceset="USB_C" device=""/>
<part name="U$17" library="microbuilder" deviceset="VBUS" device=""/>
<part name="U$18" library="microbuilder" deviceset="GND" device=""/>
<part name="X3" library="microbuilder" deviceset="SMACONNECTOR" device="_EDGE_UFL" value="SMA con"/>
<part name="U$8" library="microbuilder" deviceset="GND" device=""/>
<part name="U$9" library="microbuilder" deviceset="GND" device=""/>
<part name="R1" library="microbuilder" deviceset="RESISTOR" device="0603" value="100k"/>
<part name="R2" library="microbuilder" deviceset="RESISTOR" device="0603" value="5.1k"/>
<part name="R3" library="microbuilder" deviceset="RESISTOR" device="0603" value="5.1k"/>
<part name="R4" library="microbuilder" deviceset="RESISTOR" device="0603" value="100k"/>
<part name="USB_A" library="microbuilder" deviceset="USB_TYPEA" device="PTHFML" value="USB_A_FEMALE"/>
<part name="U4" library="microbuilder" deviceset="SPIFLASH_8PIN" device="UX" value="GD25x16"/>
<part name="L2" library="microbuilder" deviceset="APA102" device="2020" value="RGB"/>
<part name="+3V5" library="supply1" deviceset="+3V3" device=""/>
<part name="U$10" library="microbuilder" deviceset="GND" device=""/>
<part name="U$12" library="microbuilder" deviceset="GND" device=""/>
<part name="+3V10" library="supply1" deviceset="+3V3" device=""/>
<part name="U$13" library="microbuilder" deviceset="GND" device=""/>
<part name="IC2" library="microbuilder" deviceset="ATSAMD51G" device="_TQFN48"/>
<part name="U$16" library="microbuilder" deviceset="GND" device=""/>
<part name="+3V11" library="supply1" deviceset="+3V3" device=""/>
<part name="+3V6" library="supply1" deviceset="+3V3" device=""/>
<part name="U$7" library="microbuilder" deviceset="GND" device=""/>
<part name="R6" library="microbuilder" deviceset="RESISTOR" device="0805" value="2.2K"/>
<part name="R7" library="microbuilder" deviceset="RESISTOR" device="0805" value="10K"/>
<part name="C2" library="microbuilder" deviceset="CAP_CERAMIC" device="0603" value="1µF"/>
<part name="C3" library="microbuilder" deviceset="CAP_CERAMIC" device="0603" value="10µF"/>
<part name="U$28" library="microbuilder" deviceset="GND" device=""/>
<part name="U$29" library="microbuilder" deviceset="GND" device=""/>
<part name="+3V4" library="supply1" deviceset="+3V3" device=""/>
<part name="U3" library="microbuilder" deviceset="VREG_SOT23-5" device="" value="AP2112K-3.3"/>
<part name="U$11" library="microbuilder" deviceset="GND" device=""/>
<part name="C4" library="microbuilder" deviceset="CAP_CERAMIC" device="0603" value="10µF"/>
<part name="C5" library="microbuilder" deviceset="CAP_CERAMIC" device="0603" value="1µF"/>
<part name="C7" library="microbuilder" deviceset="CAP_CERAMIC" device="0603" value="1µF"/>
<part name="U$14" library="microbuilder" deviceset="VBUS" device=""/>
<part name="U$15" library="microbuilder" deviceset="GND" device=""/>
<part name="USB_C" library="USB_Type_C_12P" deviceset="USB_TYPE_C_12P" device="USB_TYPE_C_12P"/>
<part name="U$19" library="microbuilder" deviceset="GND" device=""/>
<part name="U$20" library="microbuilder" deviceset="GND" device=""/>
<part name="U$21" library="microbuilder" deviceset="VBUS" device=""/>
<part name="U$22" library="microbuilder" deviceset="VBUS" device=""/>
</parts>
<sheets>
<sheet>
<plain>
<text>Terminals</text>
<text>RFM98-W</text>
<text>POWER</text>
<text>RESET</text>
<text>Flash</text>
<text>RGB LED</text>
<text>LoRa module
interrupts DIO0 to DIO5 not used</text>
<text>emergency reset, usually a button
not used, could be activated if needed</text>
<text>flash memory for circuitpython libraries</text>
<text>for flashing purpose</text>
<text>SERCOM0: (avail on A1, A4, A5, D2)
SERCOM1: SPI
SERCOM2: I2C
SERCOM3: UART
SERCOM4: (NEOPIX DMA MOSI)
SERCOM5: (avail on D10-D13)</text>
<text>PCCDEN1</text>
<text>PCCDEN2</text>
<text>PCCD0</text>
<text>PCCD1</text>
<text>PCCD2</text>
<text>PCCD3</text>
<text>PCCD4</text>
<text>PCCD5</text>
<text>PCCD6</text>
<text>PCCD7</text>
<text>PCCLK</text>
<text>ATSAMD51G</text>
<text>USB C Plug (male)</text>
</plain>
<busses>
</busses>
<nets>
<net name="GND">
<segment>
<pinref part="U1" gate="G$1" pin="GND@3"/>
<pinref part="U$4" gate="G$1" pin="GND"/>
<pinref part="U1" gate="G$1" pin="GND@2"/>
</segment>
<segment>
<pinref part="C1" gate="G$1" pin="P$2"/>
<pinref part="U$6" gate="G$1" pin="GND"/>
<pinref part="U1" gate="G$1" pin="GND@1"/>
</segment>
<segment>
<pinref part="C6" gate="G$1" pin="P$2"/>
<pinref part="U$27" gate="G$1" pin="GND"/>
</segment>
<segment>
<pinref part="GND7" gate="1" pin="GND"/>
<pinref part="RESET" gate="1" pin="2"/>
</segment>
<segment>
<pinref part="U$30" gate="G$1" pin="GND"/>
<pinref part="U3" gate="G$1" pin="GND"/>
</segment>
<segment>
<pinref part="PIGND" gate="G$1" pin="TP"/>
<pinref part="U$5" gate="G$1" pin="GND"/>
<pinref part="PGND" gate="G$1" pin="TP"/>
</segment>
<segment>
<pinref part="U$18" gate="G$1" pin="GND"/>
<pinref part="USB_C2" gate="G$1" pin="GND"/>
<pinref part="R2" gate="G$1" pin="1"/>
<pinref part="R3" gate="G$1" pin="1"/>
</segment>
<segment>
<pinref part="X3" gate="G$1" pin="GND1"/>
<pinref part="X3" gate="G$1" pin="GND2"/>
<pinref part="U$8" gate="G$1" pin="GND"/>
</segment>
<segment>
<pinref part="X3" gate="G$1" pin="GND3"/>
<pinref part="X3" gate="G$1" pin="GND4"/>
<pinref part="U$9" gate="G$1" pin="GND"/>
</segment>
<segment>
<pinref part="U4" gate="G$1" pin="VSS"/>
<pinref part="GND8" gate="1" pin="GND"/>
</segment>
<segment>
<pinref part="L2" gate="G$1" pin="GND"/>
<pinref part="U$10" gate="G$1" pin="GND"/>
</segment>
<segment>
<pinref part="U$12" gate="G$1" pin="GND"/>
<pinref part="IC2" gate="G$1" pin="GND"/>
<pinref part="IC2" gate="G$1" pin="GNDA"/>
</segment>
<segment>
<pinref part="IC2" gate="G$3" pin="TP"/>
<pinref part="U$16" gate="G$1" pin="GND"/>
</segment>
<segment>
<pinref part="U$7" gate="G$1" pin="GND"/>
<pinref part="C2" gate="G$1" pin="P$2"/>
</segment>
<segment>
<pinref part="U$13" gate="G$1" pin="GND"/>
<pinref part="C3" gate="G$1" pin="P$2"/>
</segment>
<segment>
<pinref part="U$28" gate="G$1" pin="GND"/>
<pinref part="C5" gate="G$1" pin="P$2"/>
</segment>
<segment>
<pinref part="U$29" gate="G$1" pin="GND"/>
<pinref part="C4" gate="G$1" pin="P$2"/>
</segment>
<segment>
<pinref part="U$11" gate="G$1" pin="GND"/>
<pinref part="C7" gate="G$1" pin="P$2"/>
</segment>
<segment>
<pinref part="USB_A" gate="G$1" pin="GND"/>
<pinref part="U$15" gate="G$1" pin="GND"/>
</segment>
<segment>
<pinref part="U$20" gate="G$1" pin="GND"/>
<pinref part="USB_C" gate="G$1" pin="SHIELD1"/>
<pinref part="USB_C" gate="G$1" pin="SHIELD3"/>
<pinref part="USB_C" gate="G$1" pin="GNDA"/>
</segment>
<segment>
<pinref part="USB_C" gate="G$1" pin="SHIELD4"/>
<pinref part="U$19" gate="G$1" pin="GND"/>
<pinref part="USB_C" gate="G$1" pin="SHIELD2"/>
<pinref part="USB_C" gate="G$1" pin="GNDB"/>
</segment>
</net>
<net name="RST_3V">
<segment>
<pinref part="U1" gate="G$1" pin="RESET"/>
</segment>
<segment>
<pinref part="IC2" gate="G$1" pin="PB09/I9/AIN3/SERCOM4.1"/>
</segment>
</net>
<net name="CS_3V">
<segment>
<pinref part="U1" gate="G$1" pin="NSS"/>
</segment>
<segment>
<pinref part="IC2" gate="G$1" pin="PA04/I4/VREFB/AIN4/SERCOM0.0"/>
</segment>
</net>
<net name="N$1">
<segment>
<pinref part="U1" gate="G$1" pin="ANT"/>
<pinref part="ANTENNA" gate="G$1" pin="1"/>
<pinref part="X3" gate="G$1" pin="ANT"/>
</segment>
</net>
<net name="DIO3">
<segment>
<pinref part="U1" gate="G$1" pin="DIO3"/>
</segment>
</net>
<net name="DIO0">
<segment>
<pinref part="U1" gate="G$1" pin="DIO0"/>
</segment>
</net>
<net name="DIO2">
<segment>
<pinref part="U1" gate="G$1" pin="DIO2"/>
</segment>
</net>
<net name="DIO1">
<segment>
<pinref part="U1" gate="G$1" pin="DIO1"/>
</segment>
</net>
<net name="DIO5">
<segment>
<pinref part="U1" gate="G$1" pin="DIO5"/>
</segment>
</net>
<net name="DIO4">
<segment>
<pinref part="U1" gate="G$1" pin="DIO4"/>
</segment>
</net>
<net name="+3V3">
<segment>
<pinref part="U1" gate="G$1" pin="VDD"/>
<pinref part="C1" gate="G$1" pin="P$1"/>
<pinref part="+3V3" gate="G$1" pin="3.3V"/>
</segment>
<segment>
<pinref part="+3V7" gate="G$1" pin="+3V3"/>
<pinref part="U4" gate="G$1" pin="VCC"/>
</segment>
<segment>
<pinref part="P3V" gate="G$1" pin="TP"/>
<pinref part="PI3V" gate="G$1" pin="TP"/>
<pinref part="+3V1" gate="G$1" pin="+3V3"/>
</segment>
<segment>
<pinref part="+3V8" gate="G$1" pin="+3V3"/>
<pinref part="R4" gate="G$1" pin="2"/>
</segment>
<segment>
<pinref part="L2" gate="G$1" pin="VDD"/>
<pinref part="+3V5" gate="G$1" pin="+3V3"/>
</segment>
<segment>
<pinref part="+3V10" gate="G$1" pin="+3V3"/>
<pinref part="IC2" gate="G$1" pin="VDDA"/>
<pinref part="IC2" gate="G$1" pin="VDDIO"/>
</segment>
<segment>
<pinref part="+3V11" gate="G$1" pin="+3V3"/>
<pinref part="R7" gate="G$1" pin="1"/>
</segment>
<segment>
<pinref part="+3V6" gate="G$1" pin="+3V3"/>
<pinref part="R6" gate="G$1" pin="1"/>
</segment>
<segment>
<pinref part="+3V4" gate="G$1" pin="+3V3"/>
<pinref part="U3" gate="G$1" pin="OUT"/>
<pinref part="C4" gate="G$1" pin="P$1"/>
<pinref part="C5" gate="G$1" pin="P$1"/>
<pinref part="C7" gate="G$1" pin="P$1"/>
</segment>
</net>
<net name="VBUS">
<segment>
<pinref part="U$3" gate="G$1" pin="VBUS"/>
<pinref part="C6" gate="G$1" pin="P$1"/>
<pinref part="R1" gate="G$1" pin="2"/>
<pinref part="U3" gate="G$1" pin="IN"/>
</segment>
<segment>
<pinref part="USB_C2" gate="G$1" pin="VBUS"/>
<pinref part="U$17" gate="G$1" pin="VBUS"/>
</segment>
<segment>
<pinref part="USB_A" gate="G$1" pin="VBUS"/>
<pinref part="U$14" gate="G$1" pin="VBUS"/>
</segment>
<segment>
<pinref part="USB_C" gate="G$1" pin="VBUS_A"/>
<pinref part="U$21" gate="G$1" pin="VBUS"/>
</segment>
<segment>
<pinref part="USB_C" gate="G$1" pin="VBUS_B"/>
<pinref part="U$22" gate="G$1" pin="VBUS"/>
</segment>
</net>
<net name="!RESET">
<segment>
<pinref part="RESET" gate="1" pin="1"/>
</segment>
<segment>
<pinref part="IC2" gate="G$1" pin="/RESET"/>
<pinref part="R7" gate="G$1" pin="2"/>
<pinref part="C2" gate="G$1" pin="P$1"/>
</segment>
</net>
<net name="EN">
<segment>
<pinref part="R1" gate="G$1" pin="1"/>
<pinref part="U3" gate="G$1" pin="EN"/>
</segment>
</net>
<net name="MOSI">
<segment>
<pinref part="U1" gate="G$1" pin="MOSI"/>
</segment>
<segment>
<pinref part="IC2" gate="G$1" pin="PA00/EINT0/SERCOM1.0"/>
</segment>
</net>
<net name="MISO">
<segment>
<pinref part="U1" gate="G$1" pin="MISO"/>
</segment>
<segment>
<pinref part="IC2" gate="G$1" pin="PB23/I7/SERCOM1+5.3"/>
</segment>
</net>
<net name="SCK">
<segment>
<pinref part="U1" gate="G$1" pin="SCK"/>
</segment>
<segment>
<pinref part="IC2" gate="G$1" pin="PA01/EINT1/SERCOM1.1"/>
</segment>
</net>
<net name="D+">
<segment>
<pinref part="USB_C2" gate="G$1" pin="D+"/>
</segment>
<segment>
<pinref part="USB_C" gate="G$1" pin="D+"/>
</segment>
<segment>
<pinref part="IC2" gate="G$1" pin="PA25/I9/SERCOM3+5.3/D+"/>
</segment>
<segment>
<pinref part="USB_A" gate="G$1" pin="D+"/>
</segment>
</net>
<net name="D-">
<segment>
<pinref part="USB_C2" gate="G$1" pin="D-"/>
</segment>
<segment>
<pinref part="USB_C" gate="G$1" pin="D-"/>
</segment>
<segment>
<pinref part="IC2" gate="G$1" pin="PA24/I8/SERCOM3+5.2/D-"/>
</segment>
<segment>
<pinref part="USB_A" gate="G$1" pin="D-"/>
</segment>
</net>
<net name="SWCLK">
<segment>
<pinref part="PCLK" gate="G$1" pin="TP"/>
<pinref part="PICLK" gate="G$1" pin="TP"/>
</segment>
<segment>
<pinref part="IC2" gate="G$1" pin="PA30/I14/SECOM1.2/SWCLK"/>
<pinref part="R6" gate="G$1" pin="2"/>
</segment>
</net>
<net name="SWDIO">
<segment>
<pinref part="PIO" gate="G$1" pin="TP"/>
<pinref part="PIIO" gate="G$1" pin="TP"/>
</segment>
<segment>
<pinref part="IC2" gate="G$1" pin="PA31/I15/SECOM1.3/SWDIO"/>
</segment>
</net>
<net name="QSPI_DATA[0]">
<segment>
<pinref part="U4" gate="G$1" pin="MOSI"/>
</segment>
<segment>
<pinref part="IC2" gate="G$1" pin="PA08/I2C/AIN8/SERCOM0.0+2.1/I2SMCK"/>
</segment>
</net>
<net name="QSPI_DATA[1]">
<segment>
<pinref part="U4" gate="G$1" pin="MISO"/>
</segment>
<segment>
<pinref part="IC2" gate="G$1" pin="PA09/I2C/I9/AIN9/SERCOM0.1+2.0/I2SFS0"/>
</segment>
</net>
<net name="QSPI_SCK">
<segment>
<pinref part="U4" gate="G$1" pin="SCK"/>
</segment>
<segment>
<pinref part="IC2" gate="G$1" pin="PB10/I10/SERCOM4.2/I2SDI"/>
</segment>
</net>
<net name="QSPI_CS">
<segment>
<pinref part="R4" gate="G$1" pin="1"/>
<pinref part="U4" gate="G$1" pin="SSEL"/>
</segment>
<segment>
<pinref part="IC2" gate="G$1" pin="PB11/I11/SERCOM4.3/I2SFS1"/>
</segment>
</net>
<net name="QSPI_DATA[2]">
<segment>
<pinref part="U4" gate="G$1" pin="WP#/IO2"/>
</segment>
<segment>
<pinref part="IC2" gate="G$1" pin="PA10/I10/AIN10/SERCOM0+2.2/I2SCK"/>
</segment>
</net>
<net name="QSPI_DATA[3]">
<segment>
<pinref part="U4" gate="G$1" pin="HOLD#/IO3"/>
</segment>
<segment>
<pinref part="IC2" gate="G$1" pin="PA11/I11/AIN11/SERCOM0+2.3/I2SDO"/>
</segment>
</net>
<net name="CC1">
<segment>
<pinref part="USB_C2" gate="G$1" pin="CC1"/>
<pinref part="R3" gate="G$1" pin="2"/>
</segment>
<segment>
<pinref part="USB_C" gate="G$1" pin="CC"/>
</segment>
</net>
<net name="N$10">
<segment>
<pinref part="USB_C2" gate="G$1" pin="CC2"/>
<pinref part="R2" gate="G$1" pin="2"/>
</segment>
</net>
<net name="DOTSTAR_DATA">
<segment>
<pinref part="L2" gate="G$1" pin="DI"/>
</segment>
<segment>
<pinref part="IC2" gate="G$1" pin="PB03/I3/AIN15/SERCOM5.1"/>
</segment>
</net>
<net name="DOTSTAR_CLK">
<segment>
<pinref part="L2" gate="G$1" pin="CKI"/>
</segment>
<segment>
<pinref part="IC2" gate="G$1" pin="PB02/I2/AIN14/SERCOM5.0"/>
</segment>
</net>
<net name="SCL">
<segment>
<pinref part="IC2" gate="G$1" pin="PA13/I13/I2C/SERCOM2.1+4.0"/>
</segment>
</net>
<net name="SDA">
<segment>
<pinref part="IC2" gate="G$1" pin="PA12/I12/I2C/SERCOM2.0+4.1"/>
</segment>
</net>
<net name="A5">
<segment>
<pinref part="IC2" gate="G$1" pin="PA06/I6/VREFC/AIN6/SERCOM0.2"/>
</segment>
</net>
<net name="A2">
<segment>
<pinref part="IC2" gate="G$1" pin="PB08/I8/AIN2/SERCOM4.0"/>
</segment>
</net>
<net name="A1">
<segment>
<pinref part="IC2" gate="G$1" pin="PA05/I5/AIN5/VOUT1/SERCOM0.1"/>
</segment>
</net>
<net name="D11">
<segment>
<pinref part="IC2" gate="G$1" pin="PA21/I5/SERCOM3+5.3/I2SDO"/>
</segment>
</net>
<net name="D12">
<segment>
<pinref part="IC2" gate="G$1" pin="PA23/I2C/I7/SERCOM3.1+5.0/SOF/I2SFS1"/>
</segment>
</net>
<net name="AREF">
<segment>
<pinref part="IC2" gate="G$1" pin="PA03/I3/VREFA/AIN1"/>
</segment>
</net>
<net name="D13">
<segment>
<pinref part="IC2" gate="G$1" pin="PA22/I2C/I6/SERCOM3.0+5.1/I2SDI"/>
</segment>
</net>
<net name="A0">
<segment>
<pinref part="IC2" gate="G$1" pin="PA02/EINT2/AIN0/VOUT0"/>
</segment>
</net>
<net name="D9">
<segment>
<pinref part="IC2" gate="G$1" pin="PA19/I3/SERCOM1+3.3"/>
</segment>
</net>
<net name="D7">
<segment>
<pinref part="IC2" gate="G$1" pin="PA18/I2/SERCOM1+3.2"/>
</segment>
</net>
<net name="D5">
<segment>
<pinref part="IC2" gate="G$1" pin="PA15/I15/SERCOM2+4.3"/>
</segment>
</net>
<net name="D4">
<segment>
<pinref part="IC2" gate="G$1" pin="PA14/I14/SERCOM2+4.2"/>
</segment>
</net>
<net name="TX_D1">
<segment>
<pinref part="IC2" gate="G$1" pin="PA17/I2C/I1/SERCOM1.1+3.0"/>
</segment>
</net>
<net name="RX_D0">
<segment>
<pinref part="IC2" gate="G$1" pin="PA16/I2C/I0/SERCOM1.0+3.1"/>
</segment>
</net>
<net name="D10">
<segment>
<pinref part="IC2" gate="G$1" pin="PA20/I4/SERCOM3+5.2/I2SFS0"/>
</segment>
</net>
<net name="D3">
<segment>
<pinref part="IC2" gate="G$1" pin="PB22/I6/SERCOM1+5.2"/>
</segment>
</net>
<net name="D2">
<segment>
<pinref part="IC2" gate="G$1" pin="PA07/I7/AIN7/SERCOM0.3"/>
</segment>
</net>
<net name="VDDCORE1">
<segment>
<pinref part="IC2" gate="G$1" pin="VDDCORE"/>
<pinref part="C3" gate="G$1" pin="P$1"/>
</segment>
</net>
</nets>
</sheet>
</sheets>
</schematic>
</drawing>
</eagle>
