(kicad_pcb (version 20211014) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "gerbers/")
    )
  )
  (net 0 "")
  (net 1 "+5V")
  (net 2 "GND")
  (net 3 "unconnected-(J1-Pad4)")
  (net 4 "Net-(J1-Pad5)")
  (net 5 "Net-(J2-Pad1)")
  (net 6 "+3V3")
  (net 7 "unconnected-(J2-Pad4)")
  (net 8 "/rx")
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x06_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 59FED5CC)
    (at 128.75 62.75 90)
    (descr "Through hole straight pin header, 1x06, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x06 2.54mm single row")
    (property "Sheetfile" "p1-interface.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J2" (at -2.65 13.25 180) (layer "F.SilkS"))
    (fp_text value "Conn_01x06" (at 0 15.03 90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 6.35) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(J2-Pad1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 "+3V3") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 "+3V3") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 "unconnected-(J2-Pad4)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 "/rx") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "Pin_6") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x06_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_RJ:RJ12_Amphenol_54601" (layer "F.Cu")
    (tedit 5AE2E32D)
    (at 132.03 72.53)
    (descr "RJ12 connector  https://cdn.amphenol-icc.com/media/wysiwyg/files/drawing/c-bmj-0082.pdf")
    (tags "RJ12 connector")
    (property "PN" " 54601-906WPLF")
    (property "Sheetfile" "p1-interface.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J1" (at -1.67 -2.16) (layer "F.SilkS") hide)
    (fp_text value "P1 Connector" (at 3.54 18.3) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 3.16 7.76) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 8.25 8.89) (size 3.25 3.25) (drill 3.25) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -1.91 8.89) (size 3.25 3.25) (drill 3.25) (layers *.Cu *.Mask))
    (pad "1" thru_hole rect (at 0 0) (size 1.52 1.52) (drill 0.76) (layers *.Cu *.Mask)
      (net 1 "+5V") (pintype "passive"))
    (pad "2" thru_hole circle (at 1.27 2.54) (size 1.52 1.52) (drill 0.76) (layers *.Cu *.Mask)
      (net 1 "+5V") (pintype "passive"))
    (pad "3" thru_hole circle (at 2.54 0) (size 1.52 1.52) (drill 0.76) (layers *.Cu *.Mask)
      (net 2 "GND") (pintype "passive"))
    (pad "4" thru_hole circle (at 3.81 2.54) (size 1.52 1.52) (drill 0.76) (layers *.Cu *.Mask)
      (net 3 "unconnected-(J1-Pad4)") (pintype "passive+no_connect"))
    (pad "5" thru_hole circle (at 5.08 0) (size 1.52 1.52) (drill 0.76) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad5)") (pintype "passive"))
    (pad "6" thru_hole circle (at 6.35 2.54) (size 1.52 1.52) (drill 0.76) (layers *.Cu *.Mask)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_RJ.3dshapes/RJ12_Amphenol_54601.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23" (layer "F.Cu")
    (tedit 5FA16958)
    (at 139.7 68.6 180)
    (descr "SOT, 3 Pin (https://www.jedec.org/system/files/docs/to-236h.pdf variant AB), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "Sheetfile" "p1-interface.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "Q1" (at -3 -1.4 180) (layer "F.SilkS"))
    (fp_text value "BC847" (at 0 2.4 180) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 180) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9375 -0.95 180) (size 1.475 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "Net-(J1-Pad5)") (pinfunction "B") (pintype "input"))
    (pad "2" smd roundrect (at -0.9375 0.95 180) (size 1.475 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "E") (pintype "passive"))
    (pad "3" smd roundrect (at 0.9375 0 180) (size 1.475 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 8 "/rx") (pinfunction "C") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 134.58 69.53 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "p1-interface.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R1" (at -0.32 1.63) (layer "F.SilkS"))
    (fp_text value "4k7" (at 0 1.65) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1 0 180) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2083333333)
      (net 4 "Net-(J1-Pad5)") (pintype "passive"))
    (pad "2" smd roundrect (at 1 0 180) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2083333333)
      (net 1 "+5V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 59FED5CC)
    (at 128.75 66.6 90)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (property "Sheetfile" "p1-interface.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J3" (at 0.3 5.15 180) (layer "F.SilkS"))
    (fp_text value "Conn_01x02" (at 0 4.87 90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 1.27) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(J2-Pad1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "+5V") (pinfunction "Pin_2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 128.85 69.55 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "p1-interface.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R2" (at -2.85 -0.05 90) (layer "F.SilkS"))
    (fp_text value "10k" (at 0 1.65) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1 0 180) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2083333333)
      (net 8 "/rx") (pintype "passive"))
    (pad "2" smd roundrect (at 1 0 180) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2083333333)
      (net 6 "+3V3") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 126.35 90.1) (end 144.3 90.05) (layer "Edge.Cuts") (width 0.05))
  (gr_line (start 144.3 60.55) (end 126.3 60.55) (layer "Edge.Cuts") (width 0.05))
  (gr_line (start 144.3 90.05) (end 144.3 60.55) (layer "Edge.Cuts") (width 0.05))
  (gr_line (start 126.3 60.55) (end 126.35 90.1) (layer "Edge.Cuts") (width 0.05))
  (gr_text "www.grodansparadis.com" (at 127.4 80.15 -90) (layer "F.SilkS"))
  (gr_text "p1-interface, rev B" (at 143.45 79.75 270) (layer "F.SilkS"))
  (dimension (type aligned) (layer "F.Cu")
    (pts (xy 126.35 89.861162) (xy 144.3 89.861162))
    (height 5.238838)
    (gr_text "17,9500 mm" (at 135.325 93.3) (layer "F.Cu"))
    (format (units 3) (units_format 1) (precision 4))
    (style (thickness 0.2) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (dimension (type aligned) (layer "F.Cu")
    (pts (xy 126.549926 90) (xy 126.549926 60.55))
    (height -5.899926)
    (gr_text "29,4500 mm" (at 118.85 75.275 90) (layer "F.Cu"))
    (format (units 3) (units_format 1) (precision 4))
    (style (thickness 0.2) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (zone (net 2) (net_name "GND") (layer "F.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 145 90.45)
        (xy 125.25 90.35)
        (xy 125.4 59.95)
        (xy 125.4 60.05)
        (xy 145.1 59.95)
      )
    )
  )
  (zone (net 2) (net_name "GND") (layer "B.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 146.049779 90.845737)
        (xy 124.349779 90.795737)
        (xy 123.849779 61.245737)
        (xy 124.299779 59.545737)
        (xy 145.849779 59.445737)
      )
    )
  )
)
