(kicad_pcb (version 20211014) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "LASK4-GERBER/")
    )
  )
  (net 0 "")
  (net 1 "GND")
  (net 2 "/Down")
  (net 3 "+3.3V")
  (net 4 "/GPIO_2_ADC1_1")
  (net 5 "/GPIO_3_ADC1_2")
  (net 6 "/GPIO_4_ADC1_3")
  (net 7 "/GPIO_5_ADC1_4")
  (net 8 "/BatGND")
  (net 9 "/BatV3-7")
  (net 10 "+5V")
  (net 11 "/SCL33")
  (net 12 "/SDA34")
  (net 13 "/Select")
  (net 14 "/Start")
  (net 15 "unconnected-(U1-Pad1)")
  (net 16 "unconnected-(U2-Pad1)")
  (net 17 "unconnected-(U4-Pad1)")
  (net 18 "unconnected-(U6-Pad0)")
  (net 19 "unconnected-(U6-Pad1)")
  (net 20 "unconnected-(U6-Pad6)")
  (net 21 "/Up")
  (net 22 "unconnected-(U6-Pad11)")
  (net 23 "unconnected-(U6-Pad12)")
  (net 24 "unconnected-(U6-Pad13)")
  (net 25 "unconnected-(U6-Pad14)")
  (net 26 "unconnected-(U6-Pad15)")
  (net 27 "unconnected-(U6-Pad16)")
  (net 28 "unconnected-(U6-Pad17)")
  (net 29 "unconnected-(U6-Pad18)")
  (net 30 "unconnected-(U6-Pad21)")
  (net 31 "unconnected-(U6-Pad35)")
  (net 32 "unconnected-(U6-Pad36)")
  (net 33 "unconnected-(U6-Pad37)")
  (net 34 "unconnected-(U6-Pad38)")
  (net 35 "unconnected-(U6-Pad39)")
  (net 36 "unconnected-(U6-Pad40)")
  (net 37 "unconnected-(U3-Pad1)")
  (net 38 "/BatterPowered")
  (net 39 "/ChargingMode")
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 59FED5CC)
    (at 193.04 113.03 -90)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (property "Sheetfile" "LASK4.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "Switch1" (at 0 -2.33 90) (layer "F.SilkS") hide)
    (fp_text value "SW_SPDT" (at 0 7.41 90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 2.54) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 38 "/BatterPowered") (pinfunction "A") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 "+5V") (pinfunction "B") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 39 "/ChargingMode") (pinfunction "C") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_2.2mm_M2_DIN965_Pad" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 168.91 76.2)
    (descr "Mounting Hole 2.2mm, M2, DIN965")
    (tags "mounting hole 2.2mm m2 din965")
    (property "Sheetfile" "LASK4.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "H5" (at 0 -2.9) (layer "F.SilkS"))
    (fp_text value "MountingHole_Pad" (at 0 2.9) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 3.8 3.8) (drill 2.2) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "1") (pintype "input"))
  )
  (footprint "Connector_PinHeader_2.00mm:PinHeader_1x03_P2.00mm_Vertical" (layer "F.Cu")
    (tedit 59FED667)
    (at 196.755 79.375 90)
    (descr "Through hole straight pin header, 1x03, 2.00mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.00mm single row")
    (property "Sheetfile" "LASK4.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "H4" (at 0 -2.06 90) (layer "F.SilkS"))
    (fp_text value "Hall-49E" (at 0 6.06 90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 2) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "+3.3V") (pinfunction "VCC") (pintype "input"))
    (pad "2" thru_hole oval (at 0 2 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "GND") (pintype "input"))
    (pad "3" thru_hole oval (at 0 4 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "/GPIO_5_ADC1_4") (pinfunction "Vout") (pintype "output"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.00mm.3dshapes/PinHeader_1x03_P2.00mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Button_Switch_THT:SW_PUSH_6mm" (layer "F.Cu")
    (tedit 5A02FE31)
    (at 192.89 95.94)
    (descr "https://www.omron.com/ecb/products/pdf/en-b3f.pdf")
    (tags "tact sw push 6mm")
    (property "Sheetfile" "LASK4.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "Select1" (at 3.25 -2) (layer "F.SilkS"))
    (fp_text value "SW_Push" (at 3.75 6.7) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 3.25 2.25) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "1") (pintype "passive"))
    (pad "1" thru_hole circle (at 6.5 0 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at 6.5 4.5 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 13 "/Select") (pinfunction "2") (pintype "passive"))
    (pad "2" thru_hole circle (at 0 4.5 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 13 "/Select") (pinfunction "2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Button_Switch_THT.3dshapes/SW_PUSH_6mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 59FED5CC)
    (at 163.83 91.44 180)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (property "Sheetfile" "LASK4.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "S1" (at 0 -2.33) (layer "F.SilkS"))
    (fp_text value "SSD1306" (at -8.255 3.81) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 3.81 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "GND") (pintype "input"))
    (pad "2" thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 "+5V") (pinfunction "VCC") (pintype "input"))
    (pad "3" thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 "/SCL33") (pinfunction "SCL") (pintype "input"))
    (pad "4" thru_hole oval (at 0 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 "/SDA34") (pinfunction "SDA") (pintype "input"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x04_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.00mm:PinHeader_1x03_P2.00mm_Vertical" (layer "F.Cu")
    (tedit 59FED667)
    (at 156.115 79.375 90)
    (descr "Through hole straight pin header, 1x03, 2.00mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.00mm single row")
    (property "Sheetfile" "LASK4.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "H2" (at 0 6.445 90) (layer "F.SilkS"))
    (fp_text value "Hall-49E" (at 0 6.06 90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 2) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "+3.3V") (pinfunction "VCC") (pintype "input"))
    (pad "2" thru_hole oval (at 0 2 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "GND") (pintype "input"))
    (pad "3" thru_hole oval (at 0 4 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "/GPIO_3_ADC1_2") (pinfunction "Vout") (pintype "output"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.00mm.3dshapes/PinHeader_1x03_P2.00mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.00mm:PinHeader_1x03_P2.00mm_Vertical" (layer "F.Cu")
    (tedit 59FED667)
    (at 176.435 79.375 90)
    (descr "Through hole straight pin header, 1x03, 2.00mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.00mm single row")
    (property "Sheetfile" "LASK4.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "H3" (at 0 -2.06 90) (layer "F.SilkS"))
    (fp_text value "Hall-49E" (at 0 6.06 90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 2) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "+3.3V") (pinfunction "VCC") (pintype "input"))
    (pad "2" thru_hole oval (at 0 2 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "GND") (pintype "input"))
    (pad "3" thru_hole oval (at 0 4 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "/GPIO_4_ADC1_3") (pinfunction "Vout") (pintype "output"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.00mm.3dshapes/PinHeader_1x03_P2.00mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Button_Switch_THT:SW_PUSH_6mm" (layer "F.Cu")
    (tedit 5A02FE31)
    (at 181.46 95.94)
    (descr "https://www.omron.com/ecb/products/pdf/en-b3f.pdf")
    (tags "tact sw push 6mm")
    (property "Sheetfile" "LASK4.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "Up1" (at 3.25 -2) (layer "F.SilkS"))
    (fp_text value "SW_Push" (at 3.75 6.7) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 3.25 2.25) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 6.5 0 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "1") (pintype "passive"))
    (pad "1" thru_hole circle (at 0 0 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at 6.5 4.5 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 21 "/Up") (pinfunction "2") (pintype "passive"))
    (pad "2" thru_hole circle (at 0 4.5 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 21 "/Up") (pinfunction "2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Button_Switch_THT.3dshapes/SW_PUSH_6mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23W" (layer "F.Cu")
    (tedit 5A02FF57)
    (at 137.668 75.876 90)
    (descr "SOT-23W http://www.allegromicro.com/~/media/Files/Datasheets/A112x-Datasheet.ashx?la=en&hash=7BC461E058CC246E0BAB62433B2F1ECA104CA9D3")
    (tags "SOT-23W")
    (property "Sheetfile" "LASK4.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U1" (at 0 -2.5 90) (layer "F.SilkS"))
    (fp_text value "A1101ELHL" (at 0 2.5 90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect (at -1.2 -0.95 90) (size 1 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "unconnected-(U1-Pad1)") (pinfunction "VCC") (pintype "power_in"))
    (pad "2" smd rect (at -1.2 0.95 90) (size 1 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "/GPIO_2_ADC1_1") (pinfunction "VOUT") (pintype "open_collector"))
    (pad "3" smd rect (at 1.2 0 90) (size 1 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "GND") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23W.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Button_Switch_THT:SW_PUSH_6mm" (layer "F.Cu")
    (tedit 5A02FE31)
    (at 181.46 104.775)
    (descr "https://www.omron.com/ecb/products/pdf/en-b3f.pdf")
    (tags "tact sw push 6mm")
    (property "Sheetfile" "LASK4.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "Down1" (at 3.25 -2) (layer "F.SilkS"))
    (fp_text value "SW_Push" (at 1.42 6.985) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 3.25 2.25) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 6.5 0 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "1") (pintype "passive"))
    (pad "1" thru_hole circle (at 0 0 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at 0 4.5 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 2 "/Down") (pinfunction "2") (pintype "passive"))
    (pad "2" thru_hole circle (at 6.5 4.5 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 2 "/Down") (pinfunction "2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Button_Switch_THT.3dshapes/SW_PUSH_6mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23W" (layer "F.Cu")
    (tedit 5A02FF57)
    (at 158.115 75.876 90)
    (descr "SOT-23W http://www.allegromicro.com/~/media/Files/Datasheets/A112x-Datasheet.ashx?la=en&hash=7BC461E058CC246E0BAB62433B2F1ECA104CA9D3")
    (tags "SOT-23W")
    (property "Sheetfile" "LASK4.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U2" (at 0 -2.5 90) (layer "F.SilkS"))
    (fp_text value "A1101ELHL" (at 0 2.5 90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect (at -1.2 -0.95 90) (size 1 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 16 "unconnected-(U2-Pad1)") (pinfunction "VCC") (pintype "power_in"))
    (pad "2" smd rect (at -1.2 0.95 90) (size 1 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "/GPIO_3_ADC1_2") (pinfunction "VOUT") (pintype "open_collector"))
    (pad "3" smd rect (at 1.2 0 90) (size 1 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "GND") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23W.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_2.2mm_M2_DIN965_Pad" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 147.32 76.2)
    (descr "Mounting Hole 2.2mm, M2, DIN965")
    (tags "mounting hole 2.2mm m2 din965")
    (property "Sheetfile" "LASK4.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "H7" (at 0 -2.9) (layer "F.SilkS"))
    (fp_text value "MountingHole_Pad" (at 0 2.9) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 3.8 3.8) (drill 2.2) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "1") (pintype "input"))
  )
  (footprint "MountingHole:MountingHole_2.2mm_M2_DIN965_Pad" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 189.23 76.2)
    (descr "Mounting Hole 2.2mm, M2, DIN965")
    (tags "mounting hole 2.2mm m2 din965")
    (property "Sheetfile" "LASK4.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "H6" (at 0 -2.9) (layer "F.SilkS"))
    (fp_text value "MountingHole_Pad" (at 0 2.9) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 3.8 3.8) (drill 2.2) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "1") (pintype "input"))
  )
  (footprint "Package_TO_SOT_SMD:SOT-23W" (layer "F.Cu")
    (tedit 5A02FF57)
    (at 198.755 75.876 90)
    (descr "SOT-23W http://www.allegromicro.com/~/media/Files/Datasheets/A112x-Datasheet.ashx?la=en&hash=7BC461E058CC246E0BAB62433B2F1ECA104CA9D3")
    (tags "SOT-23W")
    (property "Sheetfile" "LASK4.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U4" (at 0 -2.5 90) (layer "F.SilkS"))
    (fp_text value "A1101ELHL" (at 0 2.5 90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect (at -1.2 -0.95 90) (size 1 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 17 "unconnected-(U4-Pad1)") (pinfunction "VCC") (pintype "power_in"))
    (pad "2" smd rect (at -1.2 0.95 90) (size 1 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 7 "/GPIO_5_ADC1_4") (pinfunction "VOUT") (pintype "open_collector"))
    (pad "3" smd rect (at 1.2 0 90) (size 1 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "GND") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23W.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23W" (layer "F.Cu")
    (tedit 5A02FF57)
    (at 178.435 75.876 90)
    (descr "SOT-23W http://www.allegromicro.com/~/media/Files/Datasheets/A112x-Datasheet.ashx?la=en&hash=7BC461E058CC246E0BAB62433B2F1ECA104CA9D3")
    (tags "SOT-23W")
    (property "Sheetfile" "LASK4.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U3" (at 0 -2.5 90) (layer "F.SilkS"))
    (fp_text value "A1101ELHL" (at 0 2.5 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 180) (layer "F.Fab"))
    (pad "1" smd rect (at -1.2 -0.95 90) (size 1 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 37 "unconnected-(U3-Pad1)") (pinfunction "VCC") (pintype "power_in"))
    (pad "2" smd rect (at -1.2 0.95 90) (size 1 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 6 "/GPIO_4_ADC1_3") (pinfunction "VOUT") (pintype "open_collector"))
    (pad "3" smd rect (at 1.2 0 90) (size 1 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "GND") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23W.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Button_Switch_THT:SW_PUSH_6mm" (layer "F.Cu")
    (tedit 5A02FE31)
    (at 192.89 104.775)
    (descr "https://www.omron.com/ecb/products/pdf/en-b3f.pdf")
    (tags "tact sw push 6mm")
    (property "Sheetfile" "LASK4.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "Start1" (at 3.25 -2) (layer "F.SilkS"))
    (fp_text value "SW_Push" (at 3.75 6.7) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 3.25 2.25) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 6.5 0 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "1") (pintype "passive"))
    (pad "1" thru_hole circle (at 0 0 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at 6.5 4.5 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 14 "/Start") (pinfunction "2") (pintype "passive"))
    (pad "2" thru_hole circle (at 0 4.5 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 14 "/Start") (pinfunction "2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Button_Switch_THT.3dshapes/SW_PUSH_6mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.00mm:PinHeader_1x03_P2.00mm_Vertical" (layer "F.Cu")
    (tedit 59FED667)
    (at 135.7 79.375 90)
    (descr "Through hole straight pin header, 1x03, 2.00mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.00mm single row")
    (property "Sheetfile" "LASK4.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "H1" (at 0 6.54 90) (layer "F.SilkS"))
    (fp_text value "Hall-49E" (at 0 6.06 90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 2) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "+3.3V") (pinfunction "VCC") (pintype "input"))
    (pad "2" thru_hole oval (at 0 2 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "GND") (pintype "input"))
    (pad "3" thru_hole oval (at 0 4 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "/GPIO_2_ADC1_1") (pinfunction "Vout") (pintype "output"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.00mm.3dshapes/PinHeader_1x03_P2.00mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x06_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 59FED5CC)
    (at 177.165 96.52 -90)
    (descr "Through hole straight pin header, 1x06, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x06 2.54mm single row")
    (property "Sheetfile" "LASK4.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U5" (at 0 -2.33 90) (layer "F.SilkS"))
    (fp_text value "Charge37lion" (at 10.16 5.715) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 6.35) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 39 "/ChargingMode") (pinfunction "VIN") (pintype "input"))
    (pad "2" thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "IN-GND") (pintype "input"))
    (pad "3" thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 "/BatGND") (pinfunction "BAT-GND") (pintype "input"))
    (pad "4" thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 "/BatV3-7") (pinfunction "BAT+") (pintype "input"))
    (pad "5" thru_hole oval (at 0 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 "/BatGND") (pinfunction "OUT-GND") (pintype "input"))
    (pad "6" thru_hole oval (at 0 12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 38 "/BatterPowered") (pinfunction "OUT-5V") (pintype "input"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x06_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "00OpenMuscleFootprint:ESP32-S2-Mini" (layer "F.Cu")
    (tedit 0)
    (at 148.59 81.28)
    (property "Sheetfile" "LASK4.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U6" (at 0 -0.5 unlocked) (layer "F.SilkS") hide)
    (fp_text value "EPS32-S2-Mini" (at -1.27 6.35 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.5 unlocked) (layer "F.Fab") hide)
    (pad "0" thru_hole circle (at -12.7 11.43) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 18 "unconnected-(U6-Pad0)") (pinfunction "EN") (pintype "input"))
    (pad "1" thru_hole circle (at -10.16 11.43) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 19 "unconnected-(U6-Pad1)") (pinfunction "ADC1_0") (pintype "input"))
    (pad "2" thru_hole circle (at -10.16 13.97) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 4 "/GPIO_2_ADC1_1") (pinfunction "ADC1_1") (pintype "input"))
    (pad "3" thru_hole circle (at -12.7 13.97) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 5 "/GPIO_3_ADC1_2") (pinfunction "ADC1_2") (pintype "input"))
    (pad "4" thru_hole circle (at -10.16 16.51) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 6 "/GPIO_4_ADC1_3") (pinfunction "ADC1_3") (pintype "input"))
    (pad "5" thru_hole circle (at -12.7 16.51) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 7 "/GPIO_5_ADC1_4") (pinfunction "ADC1_4") (pintype "input"))
    (pad "6" thru_hole circle (at -10.16 19.05) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 20 "unconnected-(U6-Pad6)") (pinfunction "ADC1_5") (pintype "input"))
    (pad "7" thru_hole circle (at -12.7 19.05) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 14 "/Start") (pinfunction "ADC1_6") (pintype "input"))
    (pad "8" thru_hole circle (at -10.16 21.59) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 13 "/Select") (pinfunction "ADC1_7") (pintype "input"))
    (pad "9" thru_hole circle (at -12.7 21.59) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 2 "/Down") (pinfunction "ADC1_8") (pintype "input"))
    (pad "10" thru_hole circle (at -10.16 24.13) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 21 "/Up") (pinfunction "ADC1_9") (pintype "input"))
    (pad "11" thru_hole circle (at -12.7 24.13) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 22 "unconnected-(U6-Pad11)") (pinfunction "ADC2_0") (pintype "input"))
    (pad "12" thru_hole circle (at -12.7 26.67) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 23 "unconnected-(U6-Pad12)") (pinfunction "ADC2_1") (pintype "input"))
    (pad "13" thru_hole circle (at -10.16 26.67) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 24 "unconnected-(U6-Pad13)") (pinfunction "ADC2_2") (pintype "input"))
    (pad "14" thru_hole circle (at -10.16 29.21) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 25 "unconnected-(U6-Pad14)") (pinfunction "ADC2_3") (pintype "input"))
    (pad "15" thru_hole circle (at 7.62 29.21) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 26 "unconnected-(U6-Pad15)") (pinfunction "ADC2_4") (pintype "input"))
    (pad "16" thru_hole circle (at 10.16 24.13) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 27 "unconnected-(U6-Pad16)") (pinfunction "ADC2_5") (pintype "input"))
    (pad "17" thru_hole circle (at 7.62 24.13) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 28 "unconnected-(U6-Pad17)") (pinfunction "ADC2_6") (pintype "input"))
    (pad "18" thru_hole circle (at 10.16 21.59) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 29 "unconnected-(U6-Pad18)") (pinfunction "ADC2_7") (pintype "input"))
    (pad "21" thru_hole circle (at 7.62 21.59) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 30 "unconnected-(U6-Pad21)") (pinfunction "21") (pintype "input"))
    (pad "33" thru_hole circle (at 10.16 19.05) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 11 "/SCL33") (pinfunction "FSPI_HD_io4") (pintype "input"))
    (pad "34" thru_hole circle (at 7.62 19.05) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 12 "/SDA34") (pinfunction "FSPI_SCO_dqs") (pintype "input"))
    (pad "35" thru_hole circle (at 10.16 16.51) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 31 "unconnected-(U6-Pad35)") (pinfunction "FSPI_D_io6") (pintype "input"))
    (pad "36" thru_hole circle (at 7.62 16.51) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 32 "unconnected-(U6-Pad36)") (pinfunction "FSPI_CLK_io7") (pintype "input"))
    (pad "37" thru_hole circle (at 10.16 13.97) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 33 "unconnected-(U6-Pad37)") (pinfunction "FSPI_Q") (pintype "input"))
    (pad "38" thru_hole circle (at 7.62 13.97) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 34 "unconnected-(U6-Pad38)") (pinfunction "FSPI_WP") (pintype "input"))
    (pad "39" thru_hole circle (at 10.16 11.43) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 35 "unconnected-(U6-Pad39)") (pinfunction "CLK3") (pintype "input"))
    (pad "40" thru_hole circle (at 7.62 11.43) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 36 "unconnected-(U6-Pad40)") (pinfunction "CLK2") (pintype "input"))
    (pad "129" thru_hole circle (at 7.62 26.67) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "GND") (pintype "input"))
    (pad "130" thru_hole circle (at 10.16 26.67) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "GND") (pintype "input"))
    (pad "133" thru_hole circle (at -12.7 29.21) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 3 "+3.3V") (pinfunction "3.3V") (pintype "input"))
    (pad "150" thru_hole circle (at 10.16 29.21) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 10 "+5V") (pinfunction "VBUS") (pintype "input"))
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical" (layer "B.Cu")
    (tedit 59FED5CC)
    (at 197.485 87.63 180)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (property "Sheetfile" "LASK4.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J1" (at 0 2.33) (layer "B.SilkS"))
    (fp_text value "Conn_01x02" (at 0 -4.87) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -1.27 90) (layer "B.Fab"))
    (pad "1" thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 "/BatGND") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 -2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 "/BatV3-7") (pinfunction "Pin_2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 136.525 72.39) (end 200.025 72.39) (layer "Edge.Cuts") (width 0.1))
  (gr_arc (start 133.985 74.93) (mid 134.728949 73.133949) (end 136.525 72.39) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 133.985 112.395) (end 133.985 74.93) (layer "Edge.Cuts") (width 0.1))
  (gr_arc (start 136.525 114.935) (mid 134.728949 114.191051) (end 133.985 112.395) (layer "Edge.Cuts") (width 0.1))
  (gr_arc (start 200.025 72.39) (mid 201.821051 73.133949) (end 202.565 74.93) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 202.565 74.93) (end 202.565 112.395) (layer "Edge.Cuts") (width 0.1))
  (gr_arc (start 202.565 112.395) (mid 201.821051 114.191051) (end 200.025 114.935) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 200.025 114.935) (end 136.525 114.935) (layer "Edge.Cuts") (width 0.1))
)
