(kicad_sch (version 20211123) (generator eeschema)
  (paper "A4")
  (lib_symbols
    (symbol "Connector_Generic:Conn_01x02" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
      (property "Reference" "J" (id 0) (at 0 2.54 0))
      (property "Value" "Conn_01x02" (id 1) (at 0 -5.08 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "~" (id 3) (at 0 0 0))
      (property "ki_keywords" "connector" (id 4) (at 0 0 0))
      (property "ki_description" "Generic connector, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "Connector*:*_1x??_*" (id 6) (at 0 0 0))
      (symbol "Conn_01x02_1_1"
        (rectangle (start -1.27 -2.413) (end 0 -2.667)
          (fill (type none))
        )
        (rectangle (start -1.27 0.127) (end 0 -0.127)
          (fill (type none))
        )
        (rectangle (start -1.27 1.27) (end 1.27 -3.81)
          (fill (type background))
        )
        (pin passive line (at -5.08 0 0) (length 3.81)
          (name "Pin_1")
          (number "1")
        )
        (pin passive line (at -5.08 -2.54 0) (length 3.81)
          (name "Pin_2")
          (number "2")
        )
      )
    )
    (symbol "Mechanical:MountingHole_Pad" (pin_numbers hide) (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
      (property "Reference" "H" (id 0) (at 0 6.35 0))
      (property "Value" "MountingHole_Pad" (id 1) (at 0 4.445 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "~" (id 3) (at 0 0 0))
      (property "ki_keywords" "mounting hole" (id 4) (at 0 0 0))
      (property "ki_description" "Mounting Hole with connection" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "MountingHole*Pad*" (id 6) (at 0 0 0))
      (symbol "MountingHole_Pad_0_1"
        (circle (center 0 1.27) (radius 1.27)
          (fill (type none))
        )
      )
      (symbol "MountingHole_Pad_1_1"
        (pin input line (at 0 -2.54 90) (length 2.54)
          (name "1")
          (number "1")
        )
      )
    )
    (symbol "OpenMuscleLibrary:Charge37lion" (in_bom yes) (on_board yes)
      (property "Reference" "U" (id 0) (at 0 0 0))
      (property "Value" "Charge37lion" (id 1) (at 0 0 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "" (id 3) (at 0 0 0))
      (symbol "Charge37lion_1_1"
        (pin input line (at 2.54 -16.51 180) (length 2.54)
          (name "VIN")
          (number "1")
        )
        (pin input line (at 2.54 -13.97 180) (length 2.54)
          (name "IN-GND")
          (number "2")
        )
        (pin input line (at 2.54 -11.43 180) (length 2.54)
          (name "BAT-GND")
          (number "3")
        )
        (pin input line (at 2.54 -8.89 180) (length 2.54)
          (name "BAT+")
          (number "4")
        )
        (pin input line (at 2.54 -6.35 180) (length 2.54)
          (name "OUT-GND")
          (number "5")
        )
        (pin input line (at 2.54 -3.81 180) (length 2.54)
          (name "OUT-5V")
          (number "6")
        )
      )
    )
    (symbol "OpenMuscleLibrary:EPS32-S2-Mini" (in_bom yes) (on_board yes)
      (property "Reference" "U" (id 0) (at 0 17.78 0))
      (property "Value" "EPS32-S2-Mini" (id 1) (at 0 20.32 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "" (id 3) (at 0 0 0))
      (symbol "EPS32-S2-Mini_0_1"
        (rectangle (start -12.7 16.51) (end 10.16 -26.67)
          (fill (type none))
        )
      )
      (symbol "EPS32-S2-Mini_1_1"
        (pin input line (at -15.24 13.97 0) (length 2.54)
          (name "EN")
          (number "0")
        )
        (pin input line (at -15.24 11.43 0) (length 2.54)
          (name "ADC1_0")
          (number "1")
        )
        (pin input line (at -15.24 -11.43 0) (length 2.54)
          (name "ADC1_9")
          (number "10")
        )
        (pin input line (at -15.24 -13.97 0) (length 2.54)
          (name "ADC2_0")
          (number "11")
        )
        (pin input line (at -15.24 -16.51 0) (length 2.54)
          (name "ADC2_1")
          (number "12")
        )
        (pin input line (at 12.7 -21.59 180) (length 2.54)
          (name "GND")
          (number "129")
        )
        (pin input line (at -15.24 -19.05 0) (length 2.54)
          (name "ADC2_2")
          (number "13")
        )
        (pin input line (at 12.7 -19.05 180) (length 2.54)
          (name "GND")
          (number "130")
        )
        (pin input line (at -15.24 -24.13 0) (length 2.54)
          (name "3.3V")
          (number "133")
        )
        (pin input line (at -15.24 -21.59 0) (length 2.54)
          (name "ADC2_3")
          (number "14")
        )
        (pin input line (at 12.7 -16.51 180) (length 2.54)
          (name "ADC2_4")
          (number "15")
        )
        (pin input line (at 12.7 -24.13 180) (length 2.54)
          (name "VBUS")
          (number "150")
        )
        (pin input line (at 12.7 -13.97 180) (length 2.54)
          (name "ADC2_5")
          (number "16")
        )
        (pin input line (at 12.7 -11.43 180) (length 2.54)
          (name "ADC2_6")
          (number "17")
        )
        (pin input line (at 12.7 -8.89 180) (length 2.54)
          (name "ADC2_7")
          (number "18")
        )
        (pin input line (at -15.24 8.89 0) (length 2.54)
          (name "ADC1_1")
          (number "2")
        )
        (pin input line (at 12.7 -6.35 180) (length 2.54)
          (name "21")
          (number "21")
        )
        (pin input line (at -15.24 6.35 0) (length 2.54)
          (name "ADC1_2")
          (number "3")
        )
        (pin input line (at 12.7 -3.81 180) (length 2.54)
          (name "FSPI_HD_io4")
          (number "33")
        )
        (pin input line (at 12.7 -1.27 180) (length 2.54)
          (name "FSPI_SCO_dqs")
          (number "34")
        )
        (pin input line (at 12.7 1.27 180) (length 2.54)
          (name "FSPI_D_io6")
          (number "35")
        )
        (pin input line (at 12.7 3.81 180) (length 2.54)
          (name "FSPI_CLK_io7")
          (number "36")
        )
        (pin input line (at 12.7 6.35 180) (length 2.54)
          (name "FSPI_Q")
          (number "37")
        )
        (pin input line (at 12.7 8.89 180) (length 2.54)
          (name "FSPI_WP")
          (number "38")
        )
        (pin input line (at 12.7 11.43 180) (length 2.54)
          (name "CLK3")
          (number "39")
        )
        (pin input line (at -15.24 3.81 0) (length 2.54)
          (name "ADC1_3")
          (number "4")
        )
        (pin input line (at 12.7 13.97 180) (length 2.54)
          (name "CLK2")
          (number "40")
        )
        (pin input line (at -15.24 1.27 0) (length 2.54)
          (name "ADC1_4")
          (number "5")
        )
        (pin input line (at -15.24 -1.27 0) (length 2.54)
          (name "ADC1_5")
          (number "6")
        )
        (pin input line (at -15.24 -3.81 0) (length 2.54)
          (name "ADC1_6")
          (number "7")
        )
        (pin input line (at -15.24 -6.35 0) (length 2.54)
          (name "ADC1_7")
          (number "8")
        )
        (pin input line (at -15.24 -8.89 0) (length 2.54)
          (name "ADC1_8")
          (number "9")
        )
      )
    )
    (symbol "OpenMuscleLibrary:Hall-49E" (in_bom yes) (on_board yes)
      (property "Reference" "H" (id 0) (at -1.27 5.08 0))
      (property "Value" "Hall-49E" (id 1) (at 2.54 7.62 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "" (id 3) (at 0 0 0))
      (symbol "Hall-49E_0_1"
        (rectangle (start -2.54 3.81) (end 2.54 -2.54)
          (fill (type none))
        )
      )
      (symbol "Hall-49E_1_1"
        (pin input line (at 2.54 -2.54 0) (length 2.54)
          (name "VCC")
          (number "1")
        )
        (pin input line (at 2.54 0 0) (length 2.54)
          (name "GND")
          (number "2")
        )
        (pin output line (at 2.54 2.54 0) (length 2.54)
          (name "Vout")
          (number "3")
        )
      )
    )
    (symbol "OpenMuscleLibrary:SSD1306" (in_bom yes) (on_board yes)
      (property "Reference" "S" (id 0) (at 0 0 0))
      (property "Value" "SSD1306" (id 1) (at 0 0 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "" (id 3) (at 0 0 0))
      (symbol "SSD1306_1_1"
        (pin input line (at 1.27 -11.43 180) (length 2.54)
          (name "GND")
          (number "1")
        )
        (pin input line (at 1.27 -8.89 180) (length 2.54)
          (name "VCC")
          (number "2")
        )
        (pin input line (at 1.27 -6.35 180) (length 2.54)
          (name "SCL")
          (number "3")
        )
        (pin input line (at 1.27 -3.81 180) (length 2.54)
          (name "SDA")
          (number "4")
        )
      )
    )
    (symbol "Sensor_Magnetic:A1101ELHL" (in_bom yes) (on_board yes)
      (property "Reference" "U" (id 0) (at 0 11.43 0))
      (property "Value" "A1101ELHL" (id 1) (at 0 8.89 0))
      (property "Footprint" "Package_TO_SOT_SMD:SOT-23W" (id 2) (at 0 -8.89 0))
      (property "Datasheet" "https://www.allegromicro.com/-/media/files/datasheets/a110x-datasheet.ashx" (id 3) (at 0 16.51 0))
      (property "ki_keywords" "hall switch" (id 4) (at 0 0 0))
      (property "ki_description" "Hall effect switch, unipolar, Bop=100G, Brp=45G, -40C to +85C, SOT-23W" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "SOT?23*" (id 6) (at 0 0 0))
      (symbol "A1101ELHL_0_1"
        (rectangle (start -5.08 7.62) (end 5.08 -7.62)
          (fill (type background))
        )
      )
      (symbol "A1101ELHL_1_1"
        (pin power_in line (at -2.54 10.16 270) (length 2.54)
          (name "VCC")
          (number "1")
        )
        (pin open_collector line (at 7.62 0 180) (length 2.54)
          (name "VOUT")
          (number "2")
        )
        (pin power_in line (at -2.54 -10.16 90) (length 2.54)
          (name "GND")
          (number "3")
        )
      )
    )
    (symbol "Switch:SW_Push" (pin_numbers hide) (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
      (property "Reference" "SW" (id 0) (at 1.27 2.54 0))
      (property "Value" "SW_Push" (id 1) (at 0 -1.524 0))
      (property "Footprint" "" (id 2) (at 0 5.08 0))
      (property "Datasheet" "~" (id 3) (at 0 5.08 0))
      (property "ki_keywords" "switch normally-open pushbutton push-button" (id 4) (at 0 0 0))
      (property "ki_description" "Push button switch, generic, two pins" (id 5) (at 0 0 0))
      (symbol "SW_Push_0_1"
        (circle (center -2.032 0) (radius 0.508)
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 1.27)
            (xy 0 3.048)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 2.54 1.27)
            (xy -2.54 1.27)
          )
          (fill (type none))
        )
        (circle (center 2.032 0) (radius 0.508)
          (fill (type none))
        )
        (pin passive line (at -5.08 0 0) (length 2.54)
          (name "1")
          (number "1")
        )
        (pin passive line (at 5.08 0 180) (length 2.54)
          (name "2")
          (number "2")
        )
      )
    )
    (symbol "Switch:SW_SPDT" (pin_names (offset 0) hide) (in_bom yes) (on_board yes)
      (property "Reference" "SW" (id 0) (at 0 4.318 0))
      (property "Value" "SW_SPDT" (id 1) (at 0 -5.08 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "~" (id 3) (at 0 0 0))
      (property "ki_keywords" "switch single-pole double-throw spdt ON-ON" (id 4) (at 0 0 0))
      (property "ki_description" "Switch, single pole double throw" (id 5) (at 0 0 0))
      (symbol "SW_SPDT_0_0"
        (circle (center -2.032 0) (radius 0.508)
          (fill (type none))
        )
        (circle (center 2.032 -2.54) (radius 0.508)
          (fill (type none))
        )
      )
      (symbol "SW_SPDT_0_1"
        (polyline
          (pts
            (xy -1.524 0.254)
            (xy 1.651 2.286)
          )
          (fill (type none))
        )
        (circle (center 2.032 2.54) (radius 0.508)
          (fill (type none))
        )
      )
      (symbol "SW_SPDT_1_1"
        (pin passive line (at 5.08 2.54 180) (length 2.54)
          (name "A")
          (number "1")
        )
        (pin passive line (at -5.08 0 0) (length 2.54)
          (name "B")
          (number "2")
        )
        (pin passive line (at 5.08 -2.54 180) (length 2.54)
          (name "C")
          (number "3")
        )
      )
    )
    (symbol "power:+3.3V" (power) (pin_names (offset 0)) (in_bom yes) (on_board yes)
      (property "Reference" "#PWR" (id 0) (at 0 -3.81 0))
      (property "Value" "+3.3V" (id 1) (at 0 3.556 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "" (id 3) (at 0 0 0))
      (property "ki_keywords" "power-flag" (id 4) (at 0 0 0))
      (property "ki_description" "Power symbol creates a global label with name \"+3.3V\"" (id 5) (at 0 0 0))
      (symbol "+3.3V_0_1"
        (polyline
          (pts
            (xy -0.762 1.27)
            (xy 0 2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 0)
            (xy 0 2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 2.54)
            (xy 0.762 1.27)
          )
          (fill (type none))
        )
      )
      (symbol "+3.3V_1_1"
        (pin power_in line (at 0 0 90) (length 0) hide
          (name "+3.3V")
          (number "1")
        )
      )
    )
    (symbol "power:+5V" (power) (pin_names (offset 0)) (in_bom yes) (on_board yes)
      (property "Reference" "#PWR" (id 0) (at 0 -3.81 0))
      (property "Value" "+5V" (id 1) (at 0 3.556 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "" (id 3) (at 0 0 0))
      (property "ki_keywords" "power-flag" (id 4) (at 0 0 0))
      (property "ki_description" "Power symbol creates a global label with name \"+5V\"" (id 5) (at 0 0 0))
      (symbol "+5V_0_1"
        (polyline
          (pts
            (xy -0.762 1.27)
            (xy 0 2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 0)
            (xy 0 2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 2.54)
            (xy 0.762 1.27)
          )
          (fill (type none))
        )
      )
      (symbol "+5V_1_1"
        (pin power_in line (at 0 0 90) (length 0) hide
          (name "+5V")
          (number "1")
        )
      )
    )
    (symbol "power:GND" (power) (pin_names (offset 0)) (in_bom yes) (on_board yes)
      (property "Reference" "#PWR" (id 0) (at 0 -6.35 0))
      (property "Value" "GND" (id 1) (at 0 -3.81 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "" (id 3) (at 0 0 0))
      (property "ki_keywords" "power-flag" (id 4) (at 0 0 0))
      (property "ki_description" "Power symbol creates a global label with name \"GND\" , ground" (id 5) (at 0 0 0))
      (symbol "GND_0_1"
        (polyline
          (pts
            (xy 0 0)
            (xy 0 -1.27)
            (xy 1.27 -1.27)
            (xy 0 -2.54)
            (xy -1.27 -1.27)
            (xy 0 -1.27)
          )
          (fill (type none))
        )
      )
      (symbol "GND_1_1"
        (pin power_in line (at 0 0 270) (length 0) hide
          (name "GND")
          (number "1")
        )
      )
    )
  )
  (junction (at 158.75 78.74) (diameter 0) (color 0 0 0 0))
  (junction (at 73.66 53.34) (diameter 0) (color 0 0 0 0))
  (junction (at 125.73 78.74) (diameter 0) (color 0 0 0 0))
  (junction (at 156.21 78.74) (diameter 0) (color 0 0 0 0))
  (junction (at 248.92 97.79) (diameter 0) (color 0 0 0 0))
  (junction (at 69.85 78.74) (diameter 0) (color 0 0 0 0))
  (junction (at 85.09 78.74) (diameter 0) (color 0 0 0 0))
  (junction (at 107.95 53.34) (diameter 0) (color 0 0 0 0))
  (junction (at 121.92 78.74) (diameter 0) (color 0 0 0 0))
  (junction (at 163.83 78.74) (diameter 0) (color 0 0 0 0))
  (junction (at 105.41 78.74) (diameter 0) (color 0 0 0 0))
  (junction (at 138.43 78.74) (diameter 0) (color 0 0 0 0))
  (junction (at 142.24 53.34) (diameter 0) (color 0 0 0 0))
  (junction (at 93.98 78.74) (diameter 0) (color 0 0 0 0))
  (wire (pts (xy 107.95 45.72) (xy 121.92 45.72)))
  (wire (pts (xy 85.09 45.72) (xy 85.09 78.74)))
  (wire (pts (xy 199.39 72.39) (xy 217.17 72.39)))
  (wire (pts (xy 142.24 48.26) (xy 142.24 53.34)))
  (wire (pts (xy 63.5 53.34) (xy 73.66 53.34)))
  (wire (pts (xy 168.91 106.68) (xy 176.53 106.68)))
  (wire (pts (xy 208.28 100.33) (xy 217.17 100.33)))
  (wire (pts (xy 208.28 87.63) (xy 217.17 87.63)))
  (wire (pts (xy 142.24 45.72) (xy 156.21 45.72)))
  (wire (pts (xy 199.39 69.85) (xy 217.17 69.85)))
  (wire (pts (xy 156.21 78.74) (xy 158.75 78.74)))
  (wire (pts (xy 250.19 77.47) (xy 245.11 77.47)))
  (wire (pts (xy 148.59 58.42) (xy 149.86 58.42)))
  (wire (pts (xy 105.41 78.74) (xy 121.92 78.74)))
  (wire (pts (xy 73.66 48.26) (xy 73.66 53.34)))
  (wire (pts (xy 93.98 48.26) (xy 93.98 78.74)))
  (wire (pts (xy 97.79 109.22) (xy 99.06 109.22)))
  (wire (pts (xy 73.66 45.72) (xy 85.09 45.72)))
  (wire (pts (xy 184.15 43.18) (xy 184.15 58.42)))
  (wire (pts (xy 115.57 58.42) (xy 114.3 58.42)))
  (wire (pts (xy 163.83 78.74) (xy 172.72 78.74)))
  (wire (pts (xy 114.3 43.18) (xy 114.3 58.42)))
  (wire (pts (xy 125.73 48.26) (xy 125.73 78.74)))
  (wire (pts (xy 69.85 78.74) (xy 85.09 78.74)))
  (wire (pts (xy 138.43 111.76) (xy 153.67 111.76)))
  (wire (pts (xy 245.11 95.25) (xy 248.92 95.25)))
  (wire (pts (xy 156.21 45.72) (xy 156.21 78.74)))
  (wire (pts (xy 142.24 43.18) (xy 149.86 43.18)))
  (wire (pts (xy 107.95 48.26) (xy 107.95 53.34)))
  (wire (pts (xy 248.92 95.25) (xy 248.92 97.79)))
  (wire (pts (xy 146.05 93.98) (xy 151.13 93.98)))
  (wire (pts (xy 73.66 53.34) (xy 107.95 53.34)))
  (wire (pts (xy 125.73 78.74) (xy 138.43 78.74)))
  (wire (pts (xy 175.26 43.18) (xy 184.15 43.18)))
  (wire (pts (xy 182.88 69.85) (xy 182.88 58.42)))
  (wire (pts (xy 248.92 97.79) (xy 251.46 96.52)))
  (wire (pts (xy 121.92 78.74) (xy 125.73 78.74)))
  (wire (pts (xy 121.92 45.72) (xy 121.92 78.74)))
  (wire (pts (xy 73.66 43.18) (xy 80.01 43.18)))
  (wire (pts (xy 158.75 48.26) (xy 158.75 78.74)))
  (wire (pts (xy 85.09 78.74) (xy 93.98 78.74)))
  (wire (pts (xy 208.28 85.09) (xy 217.17 85.09)))
  (wire (pts (xy 115.57 68.58) (xy 115.57 58.42)))
  (wire (pts (xy 168.91 109.22) (xy 176.53 109.22)))
  (wire (pts (xy 250.19 80.01) (xy 245.11 80.01)))
  (wire (pts (xy 80.01 43.18) (xy 80.01 68.58)))
  (wire (pts (xy 138.43 109.22) (xy 146.05 109.22)))
  (wire (pts (xy 149.86 43.18) (xy 149.86 58.42)))
  (wire (pts (xy 142.24 53.34) (xy 175.26 53.34)))
  (wire (pts (xy 107.95 43.18) (xy 114.3 43.18)))
  (wire (pts (xy 138.43 114.3) (xy 138.43 119.38)))
  (wire (pts (xy 158.75 78.74) (xy 163.83 78.74)))
  (wire (pts (xy 97.79 106.68) (xy 99.06 106.68)))
  (wire (pts (xy 146.05 101.6) (xy 138.43 101.6)))
  (wire (pts (xy 245.11 100.33) (xy 259.08 100.33)))
  (wire (pts (xy 208.28 80.01) (xy 217.17 80.01)))
  (wire (pts (xy 182.88 58.42) (xy 184.15 58.42)))
  (wire (pts (xy 217.17 67.31) (xy 199.39 67.31)))
  (wire (pts (xy 138.43 78.74) (xy 156.21 78.74)))
  (wire (pts (xy 163.83 45.72) (xy 163.83 78.74)))
  (wire (pts (xy 138.43 106.68) (xy 146.05 106.68)))
  (wire (pts (xy 168.91 114.3) (xy 185.42 114.3)))
  (wire (pts (xy 148.59 68.58) (xy 148.59 58.42)))
  (wire (pts (xy 245.11 97.79) (xy 248.92 97.79)))
  (wire (pts (xy 208.28 82.55) (xy 217.17 82.55)))
  (wire (pts (xy 168.91 111.76) (xy 185.42 111.76)))
  (wire (pts (xy 138.43 104.14) (xy 146.05 104.14)))
  (wire (pts (xy 175.26 45.72) (xy 163.83 45.72)))
  (wire (pts (xy 172.72 78.74) (xy 172.72 80.01)))
  (wire (pts (xy 107.95 53.34) (xy 142.24 53.34)))
  (wire (pts (xy 93.98 78.74) (xy 105.41 78.74)))
  (wire (pts (xy 175.26 53.34) (xy 175.26 48.26)))
  (wire (pts (xy 199.39 74.93) (xy 217.17 74.93)))
  (label "SDA34" (at 250.19 77.47 0))
  (label "ChargingMode" (at 161.29 96.52 0))
  (label "SDA34" (at 176.53 106.68 0))
  (label "GPIO_5_ADC1_4" (at 199.39 74.93 0))
  (label "BatV3-7" (at 99.06 106.68 0))
  (label "GPIO_2_ADC1_1" (at 199.39 67.31 0))
  (label "GPIO_4_ADC1_3" (at 199.39 72.39 0))
  (label "Down" (at 208.28 85.09 0))
  (label "SCL33" (at 250.19 80.01 0))
  (label "SCL33" (at 176.53 109.22 0))
  (label "BatGND" (at 99.06 109.22 0))
  (label "GPIO_4_ADC1_3" (at 149.86 58.42 0))
  (label "GPIO_2_ADC1_1" (at 80.01 58.42 0))
  (label "GPIO_3_ADC1_2" (at 114.3 58.42 0))
  (label "GPIO_5_ADC1_4" (at 184.15 58.42 0))
  (label "Start" (at 208.28 80.01 0))
  (label "Up" (at 208.28 87.63 0))
  (label "Up" (at 101.6 135.89 0))
  (label "GPIO_3_ADC1_2" (at 199.39 69.85 0))
  (label "Start" (at 157.48 135.89 0))
  (label "BatV3-7" (at 146.05 106.68 0))
  (label "BatGND" (at 146.05 104.14 0))
  (label "BatterPowered" (at 146.05 101.6 0))
  (label "Down" (at 119.38 135.89 0))
  (label "ChargingMode" (at 138.43 119.38 0))
  (label "Select" (at 138.43 135.89 0))
  (label "BatGND" (at 146.05 109.22 0))
  (label "Select" (at 208.28 82.55 0))
  (label "BatterPowered" (at 161.29 91.44 0))
  (symbol (lib_id "OpenMuscleLibrary:EPS32-S2-Mini") (at 232.41 76.2 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "U6" (id 0) (at 231.14 54.61 0))
    (property "Value" "EPS32-S2-Mini" (id 1) (at 231.14 57.15 0))
    (property "Footprint" "00OpenMuscleFootprint:ESP32-S2-Mini" (id 2) (at 232.41 76.2 0))
    (property "Datasheet" "" (id 3) (at 232.41 76.2 0))
    (pin "0")
    (pin "1")
    (pin "10")
    (pin "11")
    (pin "12")
    (pin "129")
    (pin "13")
    (pin "130")
    (pin "133")
    (pin "14")
    (pin "15")
    (pin "150")
    (pin "16")
    (pin "17")
    (pin "18")
    (pin "2")
    (pin "21")
    (pin "3")
    (pin "33")
    (pin "34")
    (pin "35")
    (pin "36")
    (pin "37")
    (pin "38")
    (pin "39")
    (pin "4")
    (pin "40")
    (pin "5")
    (pin "6")
    (pin "7")
    (pin "8")
    (pin "9")
  )
  (symbol (lib_id "OpenMuscleLibrary:Hall-49E") (at 71.12 45.72 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "H1" (id 0) (at 69.85 38.1 0))
    (property "Value" "Hall-49E" (id 1) (at 67.31 39.37 0))
    (property "Footprint" "Connector_PinHeader_2.00mm:PinHeader_1x03_P2.00mm_Vertical" (id 2) (at 71.12 45.72 0))
    (property "Datasheet" "" (id 3) (at 71.12 45.72 0))
    (pin "1")
    (pin "2")
    (pin "3")
  )
  (symbol (lib_id "power:+5V") (at 146.05 93.98 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR0103" (id 0) (at 146.05 97.79 0))
    (property "Value" "+5V" (id 1) (at 146.05 87.63 0))
    (property "Footprint" "" (id 2) (at 146.05 93.98 0))
    (property "Datasheet" "" (id 3) (at 146.05 93.98 0))
    (pin "1")
  )
  (symbol (lib_id "OpenMuscleLibrary:Charge37lion") (at 135.89 97.79 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "U5" (id 0) (at 135.89 96.52 0))
    (property "Value" "Charge37lion" (id 1) (at 135.89 99.06 0))
    (property "Footprint" "Connector_PinHeader_2.54mm:PinHeader_1x06_P2.54mm_Vertical" (id 2) (at 135.89 97.79 0))
    (property "Datasheet" "" (id 3) (at 135.89 97.79 0))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
    (pin "6")
  )
  (symbol (lib_id "power:GND") (at 185.42 114.3 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "#PWR0105" (id 0) (at 185.42 120.65 0))
    (property "Value" "GND" (id 1) (at 185.42 119.38 0))
    (property "Footprint" "" (id 2) (at 185.42 114.3 0))
    (property "Datasheet" "" (id 3) (at 185.42 114.3 0))
    (pin "1")
  )
  (symbol (lib_id "Switch:SW_Push") (at 96.52 135.89 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "Up1" (id 0) (at 96.52 128.27 0))
    (property "Value" "SW_Push" (id 1) (at 96.52 130.81 0))
    (property "Footprint" "Button_Switch_THT:SW_PUSH_6mm" (id 2) (at 96.52 130.81 0))
    (property "Datasheet" "~" (id 3) (at 96.52 130.81 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Sensor_Magnetic:A1101ELHL") (at 72.39 68.58 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "U1" (id 0) (at 66.04 67.3099 0))
    (property "Value" "A1101ELHL" (id 1) (at 66.04 69.8499 0))
    (property "Footprint" "Package_TO_SOT_SMD:SOT-23W" (id 2) (at 72.39 77.47 0))
    (property "Datasheet" "https://www.allegromicro.com/-/media/files/datasheets/a110x-datasheet.ashx" (id 3) (at 72.39 52.07 0))
    (pin "1")
    (pin "2")
    (pin "3")
  )
  (symbol (lib_id "power:+5V") (at 185.42 111.76 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "#PWR0106" (id 0) (at 185.42 115.57 0))
    (property "Value" "+5V" (id 1) (at 185.42 106.68 0))
    (property "Footprint" "" (id 2) (at 185.42 111.76 0))
    (property "Datasheet" "" (id 3) (at 185.42 111.76 0))
    (pin "1")
  )
  (symbol (lib_id "Sensor_Magnetic:A1101ELHL") (at 140.97 68.58 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "U3" (id 0) (at 134.62 67.3099 0))
    (property "Value" "A1101ELHL" (id 1) (at 134.62 69.8499 0))
    (property "Footprint" "Package_TO_SOT_SMD:SOT-23W" (id 2) (at 140.97 77.47 0))
    (property "Datasheet" "https://www.allegromicro.com/-/media/files/datasheets/a110x-datasheet.ashx" (id 3) (at 140.97 52.07 0))
    (pin "1")
    (pin "2")
    (pin "3")
  )
  (symbol (lib_id "Switch:SW_Push") (at 133.35 135.89 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "Select1" (id 0) (at 133.35 128.27 0))
    (property "Value" "SW_Push" (id 1) (at 133.35 130.81 0))
    (property "Footprint" "Button_Switch_THT:SW_PUSH_6mm" (id 2) (at 133.35 130.81 0))
    (property "Datasheet" "~" (id 3) (at 133.35 130.81 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "power:GND") (at 109.22 135.89 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "#PWR0112" (id 0) (at 109.22 142.24 0))
    (property "Value" "GND" (id 1) (at 109.22 140.97 0))
    (property "Footprint" "" (id 2) (at 109.22 135.89 0))
    (property "Datasheet" "" (id 3) (at 109.22 135.89 0))
    (pin "1")
  )
  (symbol (lib_id "Connector_Generic:Conn_01x02") (at 92.71 109.22 180) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "J1" (id 0) (at 92.71 100.33 0))
    (property "Value" "Conn_01x02" (id 1) (at 92.71 102.87 0))
    (property "Footprint" "Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical" (id 2) (at 92.71 109.22 0))
    (property "Datasheet" "~" (id 3) (at 92.71 109.22 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Switch:SW_Push") (at 114.3 135.89 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "Down1" (id 0) (at 114.3 128.27 0))
    (property "Value" "SW_Push" (id 1) (at 114.3 130.81 0))
    (property "Footprint" "Button_Switch_THT:SW_PUSH_6mm" (id 2) (at 114.3 130.81 0))
    (property "Datasheet" "~" (id 3) (at 114.3 130.81 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Mechanical:MountingHole_Pad") (at 158.75 45.72 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "H7" (id 0) (at 154.94 27.94 0))
    (property "Value" "MountingHole_Pad" (id 1) (at 154.94 30.48 0))
    (property "Footprint" "MountingHole:MountingHole_2.2mm_M2_DIN965_Pad" (id 2) (at 158.75 45.72 0))
    (property "Datasheet" "~" (id 3) (at 158.75 45.72 0))
    (pin "1")
  )
  (symbol (lib_id "power:GND") (at 91.44 135.89 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "#PWR0110" (id 0) (at 91.44 142.24 0))
    (property "Value" "GND" (id 1) (at 91.44 140.97 0))
    (property "Footprint" "" (id 2) (at 91.44 135.89 0))
    (property "Datasheet" "" (id 3) (at 91.44 135.89 0))
    (pin "1")
  )
  (symbol (lib_id "Switch:SW_Push") (at 152.4 135.89 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "Start1" (id 0) (at 152.4 128.27 0))
    (property "Value" "SW_Push" (id 1) (at 152.4 130.81 0))
    (property "Footprint" "Button_Switch_THT:SW_PUSH_6mm" (id 2) (at 152.4 130.81 0))
    (property "Datasheet" "~" (id 3) (at 152.4 130.81 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "power:GND") (at 147.32 135.89 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "#PWR0111" (id 0) (at 147.32 142.24 0))
    (property "Value" "GND" (id 1) (at 147.32 140.97 0))
    (property "Footprint" "" (id 2) (at 147.32 135.89 0))
    (property "Datasheet" "" (id 3) (at 147.32 135.89 0))
    (pin "1")
  )
  (symbol (lib_id "Sensor_Magnetic:A1101ELHL") (at 175.26 69.85 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "U4" (id 0) (at 168.91 68.5799 0))
    (property "Value" "A1101ELHL" (id 1) (at 168.91 71.1199 0))
    (property "Footprint" "Package_TO_SOT_SMD:SOT-23W" (id 2) (at 175.26 78.74 0))
    (property "Datasheet" "https://www.allegromicro.com/-/media/files/datasheets/a110x-datasheet.ashx" (id 3) (at 175.26 53.34 0))
    (pin "1")
    (pin "2")
    (pin "3")
  )
  (symbol (lib_id "OpenMuscleLibrary:Hall-49E") (at 105.41 45.72 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "H2" (id 0) (at 105.41 38.1 0))
    (property "Value" "Hall-49E" (id 1) (at 102.87 40.64 0))
    (property "Footprint" "Connector_PinHeader_2.00mm:PinHeader_1x03_P2.00mm_Vertical" (id 2) (at 105.41 45.72 0))
    (property "Datasheet" "" (id 3) (at 105.41 45.72 0))
    (pin "1")
    (pin "2")
    (pin "3")
  )
  (symbol (lib_id "power:+3.3V") (at 63.5 53.34 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "#PWR0102" (id 0) (at 63.5 57.15 0))
    (property "Value" "+3.3V" (id 1) (at 63.5 48.26 0))
    (property "Footprint" "" (id 2) (at 63.5 53.34 0))
    (property "Datasheet" "" (id 3) (at 63.5 53.34 0))
    (pin "1")
  )
  (symbol (lib_id "power:GND") (at 69.85 78.74 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "#PWR0101" (id 0) (at 69.85 85.09 0))
    (property "Value" "GND" (id 1) (at 69.85 83.82 0))
    (property "Footprint" "" (id 2) (at 69.85 78.74 0))
    (property "Datasheet" "" (id 3) (at 69.85 78.74 0))
    (pin "1")
  )
  (symbol (lib_id "Mechanical:MountingHole_Pad") (at 93.98 45.72 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "H5" (id 0) (at 87.63 31.75 0))
    (property "Value" "MountingHole_Pad" (id 1) (at 87.63 34.29 0))
    (property "Footprint" "MountingHole:MountingHole_2.2mm_M2_DIN965_Pad" (id 2) (at 93.98 45.72 0))
    (property "Datasheet" "~" (id 3) (at 93.98 45.72 0))
    (pin "1")
  )
  (symbol (lib_id "power:GND") (at 251.46 96.52 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR0108" (id 0) (at 251.46 102.87 0))
    (property "Value" "GND" (id 1) (at 251.46 95.25 0))
    (property "Footprint" "" (id 2) (at 251.46 96.52 0))
    (property "Datasheet" "" (id 3) (at 251.46 96.52 0))
    (pin "1")
  )
  (symbol (lib_id "OpenMuscleLibrary:Hall-49E") (at 172.72 45.72 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "H4" (id 0) (at 172.72 35.56 0))
    (property "Value" "Hall-49E" (id 1) (at 170.18 39.37 0))
    (property "Footprint" "Connector_PinHeader_2.00mm:PinHeader_1x03_P2.00mm_Vertical" (id 2) (at 172.72 45.72 0))
    (property "Datasheet" "" (id 3) (at 172.72 45.72 0))
    (pin "1")
    (pin "2")
    (pin "3")
  )
  (symbol (lib_id "Mechanical:MountingHole_Pad") (at 125.73 45.72 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "H6" (id 0) (at 120.65 30.48 0))
    (property "Value" "MountingHole_Pad" (id 1) (at 120.65 33.02 0))
    (property "Footprint" "MountingHole:MountingHole_2.2mm_M2_DIN965_Pad" (id 2) (at 125.73 45.72 0))
    (property "Datasheet" "~" (id 3) (at 125.73 45.72 0))
    (pin "1")
  )
  (symbol (lib_id "power:+5V") (at 259.08 100.33 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "#PWR0109" (id 0) (at 259.08 104.14 0))
    (property "Value" "+5V" (id 1) (at 259.08 95.25 0))
    (property "Footprint" "" (id 2) (at 259.08 100.33 0))
    (property "Datasheet" "" (id 3) (at 259.08 100.33 0))
    (pin "1")
  )
  (symbol (lib_id "Sensor_Magnetic:A1101ELHL") (at 107.95 68.58 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "U2" (id 0) (at 101.6 67.3099 0))
    (property "Value" "A1101ELHL" (id 1) (at 101.6 69.8499 0))
    (property "Footprint" "Package_TO_SOT_SMD:SOT-23W" (id 2) (at 107.95 77.47 0))
    (property "Datasheet" "https://www.allegromicro.com/-/media/files/datasheets/a110x-datasheet.ashx" (id 3) (at 107.95 52.07 0))
    (pin "1")
    (pin "2")
    (pin "3")
  )
  (symbol (lib_id "Switch:SW_SPDT") (at 156.21 93.98 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "Switch1" (id 0) (at 156.21 86.36 0))
    (property "Value" "SW_SPDT" (id 1) (at 156.21 88.9 0))
    (property "Footprint" "Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical" (id 2) (at 156.21 93.98 0))
    (property "Datasheet" "~" (id 3) (at 156.21 93.98 0))
    (pin "1")
    (pin "2")
    (pin "3")
  )
  (symbol (lib_id "OpenMuscleLibrary:Hall-49E") (at 139.7 45.72 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "H3" (id 0) (at 140.97 36.83 0))
    (property "Value" "Hall-49E" (id 1) (at 137.16 39.37 0))
    (property "Footprint" "Connector_PinHeader_2.00mm:PinHeader_1x03_P2.00mm_Vertical" (id 2) (at 139.7 45.72 0))
    (property "Datasheet" "" (id 3) (at 139.7 45.72 0))
    (pin "1")
    (pin "2")
    (pin "3")
  )
  (symbol (lib_id "OpenMuscleLibrary:SSD1306") (at 167.64 102.87 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "S1" (id 0) (at 166.37 101.6 0))
    (property "Value" "SSD1306" (id 1) (at 166.37 104.14 0))
    (property "Footprint" "Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical" (id 2) (at 167.64 102.87 0))
    (property "Datasheet" "" (id 3) (at 167.64 102.87 0))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
  )
  (symbol (lib_id "power:+3.3V") (at 208.28 100.33 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "#PWR0107" (id 0) (at 208.28 104.14 0))
    (property "Value" "+3.3V" (id 1) (at 208.28 95.25 0))
    (property "Footprint" "" (id 2) (at 208.28 100.33 0))
    (property "Datasheet" "" (id 3) (at 208.28 100.33 0))
    (pin "1")
  )
  (symbol (lib_id "power:GND") (at 128.27 135.89 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "#PWR0113" (id 0) (at 128.27 142.24 0))
    (property "Value" "GND" (id 1) (at 128.27 140.97 0))
    (property "Footprint" "" (id 2) (at 128.27 135.89 0))
    (property "Datasheet" "" (id 3) (at 128.27 135.89 0))
    (pin "1")
  )
  (symbol (lib_id "power:GND") (at 153.67 111.76 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "#PWR0104" (id 0) (at 153.67 118.11 0))
    (property "Value" "GND" (id 1) (at 153.67 116.84 0))
    (property "Footprint" "" (id 2) (at 153.67 111.76 0))
    (property "Datasheet" "" (id 3) (at 153.67 111.76 0))
    (pin "1")
  )
  (sheet_instances
    (path (page "1"))
  )
  (symbol_instances
    (path
      (reference "#PWR0101") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR0102") (unit 1) (value "+3.3V") (footprint "")
    )
    (path
      (reference "#PWR0103") (unit 1) (value "+5V") (footprint "")
    )
    (path
      (reference "#PWR0104") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR0105") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR0106") (unit 1) (value "+5V") (footprint "")
    )
    (path
      (reference "#PWR0107") (unit 1) (value "+3.3V") (footprint "")
    )
    (path
      (reference "#PWR0108") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR0109") (unit 1) (value "+5V") (footprint "")
    )
    (path
      (reference "#PWR0110") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR0111") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR0112") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR0113") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "Down1") (unit 1) (value "SW_Push") (footprint "Button_Switch_THT:SW_PUSH_6mm")
    )
    (path
      (reference "H1") (unit 1) (value "Hall-49E") (footprint "Connector_PinHeader_2.00mm:PinHeader_1x03_P2.00mm_Vertical")
    )
    (path
      (reference "H2") (unit 1) (value "Hall-49E") (footprint "Connector_PinHeader_2.00mm:PinHeader_1x03_P2.00mm_Vertical")
    )
    (path
      (reference "H3") (unit 1) (value "Hall-49E") (footprint "Connector_PinHeader_2.00mm:PinHeader_1x03_P2.00mm_Vertical")
    )
    (path
      (reference "H4") (unit 1) (value "Hall-49E") (footprint "Connector_PinHeader_2.00mm:PinHeader_1x03_P2.00mm_Vertical")
    )
    (path
      (reference "H5") (unit 1) (value "MountingHole_Pad") (footprint "MountingHole:MountingHole_2.2mm_M2_DIN965_Pad")
    )
    (path
      (reference "H6") (unit 1) (value "MountingHole_Pad") (footprint "MountingHole:MountingHole_2.2mm_M2_DIN965_Pad")
    )
    (path
      (reference "H7") (unit 1) (value "MountingHole_Pad") (footprint "MountingHole:MountingHole_2.2mm_M2_DIN965_Pad")
    )
    (path
      (reference "J1") (unit 1) (value "Conn_01x02") (footprint "Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical")
    )
    (path
      (reference "S1") (unit 1) (value "SSD1306") (footprint "Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical")
    )
    (path
      (reference "Select1") (unit 1) (value "SW_Push") (footprint "Button_Switch_THT:SW_PUSH_6mm")
    )
    (path
      (reference "Start1") (unit 1) (value "SW_Push") (footprint "Button_Switch_THT:SW_PUSH_6mm")
    )
    (path
      (reference "Switch1") (unit 1) (value "SW_SPDT") (footprint "Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical")
    )
    (path
      (reference "U1") (unit 1) (value "A1101ELHL") (footprint "Package_TO_SOT_SMD:SOT-23W")
    )
    (path
      (reference "U2") (unit 1) (value "A1101ELHL") (footprint "Package_TO_SOT_SMD:SOT-23W")
    )
    (path
      (reference "U3") (unit 1) (value "A1101ELHL") (footprint "Package_TO_SOT_SMD:SOT-23W")
    )
    (path
      (reference "U4") (unit 1) (value "A1101ELHL") (footprint "Package_TO_SOT_SMD:SOT-23W")
    )
    (path
      (reference "U5") (unit 1) (value "Charge37lion") (footprint "Connector_PinHeader_2.54mm:PinHeader_1x06_P2.54mm_Vertical")
    )
    (path
      (reference "U6") (unit 1) (value "EPS32-S2-Mini") (footprint "00OpenMuscleFootprint:ESP32-S2-Mini")
    )
    (path
      (reference "Up1") (unit 1) (value "SW_Push") (footprint "Button_Switch_THT:SW_PUSH_6mm")
    )
  )
)
