(kicad_pcb (version 20221018) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0)
    (grid_origin 152.4 101.6)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (plot_on_all_layers_selection 0x0000000_00000000)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (dashed_line_dash_ratio 12.000000)
      (dashed_line_gap_ratio 3.000000)
      (svgprecision 4)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "Net-(U1A-+)")
  (net 2 "/-sin_var_freq")
  (net 3 "Net-(U2A-+)")
  (net 4 "GND")
  (net 5 "VSS")
  (net 6 "Net-(U2C--)")
  (net 7 "/cos_fixed_freq")
  (net 8 "Net-(U1B-+)")
  (net 9 "/cos_var_freq")
  (net 10 "Net-(U2B-+)")
  (net 11 "Net-(U1D--)")
  (net 12 "VDD")
  (net 13 "Net-(U2D--)")
  (net 14 "Net-(U1C--)")
  (net 15 "Net-(D4-K)")
  (net 16 "Net-(BT1-+)")
  (net 17 "Net-(SW1A-B)")
  (net 18 "Net-(BT2--)")
  (net 19 "Net-(SW1B-B)")
  (net 20 "Net-(U1A--)")
  (net 21 "Net-(U2A--)")
  (net 22 "Net-(R3-Pad2)")
  (net 23 "Net-(U1B--)")
  (net 24 "Net-(U2B--)")
  (net 25 "Net-(R9-Pad2)")
  (net 26 "Net-(D1-A)")
  (net 27 "/sin_fixed_freq")
  (net 28 "/+sin_var_freq")
  (net 29 "/Channel 1, X")
  (net 30 "/Channel 2, Y")
  (net 31 "unconnected-(SW1A-A-Pad1)")
  (net 32 "unconnected-(SW1B-A-Pad4)")
  (net 33 "Net-(D2-A)")
  (net 34 "Net-(D2-K)")
  (net 35 "Net-(C15-Pad2)")
  (net 36 "Net-(C16-Pad2)")
  (net 37 "/+{slash}- sin var freq")
  (net 38 "/X, mixer out")
  (net 39 "unconnected-(SW2A-A-Pad1)")
  (net 40 "/Y, mixer out")
  (net 41 "unconnected-(SW2A-B-Pad2)")
  (net 42 "unconnected-(SW2A-C-Pad3)")
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "F.Cu")
    (at 156.840275 89.121899 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Dielectric" "X7R")
    (property "MPN" "GCJ188R71H104KA12D ")
    (property "Sheetfile" "opamp-spiro.kicad_sch")
    (property "Sheetname" "")
    (property "Voltage" "50V")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C13" (at 4.412899 0.233325 90) (layer "F.SilkS"))
    (fp_text value "0.1u" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.8625 0 90) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "VSS") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8625 0 90) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Global_MWS_Library:Pot-dual-Bourns-PTV112-4420A-B" (layer "F.Cu")
    (at 163.4 126.8)
    (property "MPN" "PTV112-4420A-B103")
    (property "Shaft" "6mm, flatted D to 4.5mm")
    (property "Sheetfile" "opamp-spiro.kicad_sch")
    (property "Sheetname" "")
    (property "Tol" "20%")
    (property "ki_description" "Dual potentiometer, separate units")
    (property "ki_keywords" "resistor variable")
    (attr through_hole)
    (fp_text reference "RV1" (at -7.4 -16.8 90 unlocked) (layer "F.SilkS"))
    (fp_text value "10k" (at 1 5 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 7 unlocked) (layer "F.Fab"))
    (pad "" thru_hole oval (at -6.8 -11) (size 3.2 3.4) (drill oval 2.1 2.3) (layers "*.Cu" "*.Mask"))
    (pad "" thru_hole oval (at 6.8 -11) (size 3.2 3.4) (drill oval 2.1 2.3) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle (at -3 0) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 4 "GND") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at -5 0) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 4 "GND") (pinfunction "2") (pintype "passive"))
    (pad "3" thru_hole circle (at 5 0) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 25 "Net-(R9-Pad2)") (pinfunction "3") (pintype "passive"))
    (pad "4" thru_hole circle (at -1 0) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 4 "GND") (pinfunction "4") (pintype "passive"))
    (pad "5" thru_hole circle (at 1 0) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 4 "GND") (pinfunction "5") (pintype "passive"))
    (pad "6" thru_hole circle (at 3 0) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 22 "Net-(R3-Pad2)") (pinfunction "6") (pintype "passive"))
    (model "${MY3DMOD}/PTV112-4420A-B503--3DModel-STEP-269445.STEP"
      (offset (xyz 0 11 -1.2))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (footprint "TestPoint:TestPoint_THTPad_2.0x2.0mm_Drill1.0mm" (layer "F.Cu")
    (at 139.065 105.8418)
    (descr "THT rectangular pad as test Point, square 2.0mm_Drill1.0mm  side length, hole diameter 1.0mm")
    (tags "test point THT pad rectangle square")
    (property "Sheetfile" "opamp-spiro.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "test point")
    (property "ki_keywords" "test point tp")
    (attr exclude_from_pos_files)
    (fp_text reference "TP6" (at 2.9464 0.1778) (layer "F.SilkS") hide)
    (fp_text value "TestPoint" (at 0 2.05) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -2) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 27 "/sin_fixed_freq") (pinfunction "1") (pintype "passive"))
  )
  (footprint "Global_MWS_Library:MountingHole_No4_Isolated" (layer "F.Cu")
    (at 127 127 90)
    (descr "Mounting Hole #4 isolated")
    (tags "Mounting Hole #4 isolated")
    (property "Sheetfile" "opamp-spiro.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole without connection")
    (property "ki_keywords" "mounting hole")
    (attr exclude_from_pos_files)
    (fp_text reference "H1" (at 0 -6 90) (layer "F.SilkS") hide)
    (fp_text value "#4" (at 0 7.2 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 3 90) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0 90) (size 3.175 3.175) (drill 3.175) (layers "F&B.Cu" "*.Mask"))
    (zone (net 0) (net_name "") (layers "*.Cu" "*.SilkS") (hatch edge 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.254) (filled_areas_thickness no)
      (keepout (tracks not_allowed) (vias not_allowed) (pads allowed) (copperpour not_allowed) (footprints not_allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 127 122.2327)
          (xy 126.576214 122.251573)
          (xy 126.155784 122.308044)
          (xy 125.742038 122.401665)
          (xy 125.338252 122.531696)
          (xy 124.947624 122.697105)
          (xy 124.573247 122.896585)
          (xy 124.218084 123.128554)
          (xy 123.884948 123.391177)
          (xy 123.576477 123.682375)
          (xy 123.295112 123.999841)
          (xy 123.043082 124.341062)
          (xy 122.822383 124.703336)
          (xy 122.634762 125.083794)
          (xy 122.481704 125.479425)
          (xy 122.364421 125.887096)
          (xy 122.283842 126.303578)
          (xy 122.240605 126.725575)
          (xy 122.235052 127.149745)
          (xy 122.267228 127.572728)
          (xy 122.336877 127.991177)
          (xy 122.443448 128.401778)
          (xy 122.586097 128.80128)
          (xy 122.763695 129.18652)
          (xy 122.974835 129.554447)
          (xy 123.217847 129.902148)
          (xy 123.490804 130.226871)
          (xy 123.791547 130.526043)
          (xy 124.117695 130.797297)
          (xy 124.466664 131.038484)
          (xy 124.835691 131.247695)
          (xy 125.221855 131.423274)
          (xy 125.622099 131.563829)
          (xy 126.033252 131.668249)
          (xy 126.45206 131.735706)
          (xy 126.875207 131.765666)
          (xy 127.299341 131.757893)
          (xy 127.721106 131.712447)
          (xy 128.137161 131.629688)
          (xy 128.544212 131.510273)
          (xy 128.939036 131.355145)
          (xy 129.318507 131.165534)
          (xy 129.67962 130.942941)
          (xy 130.019517 130.689128)
          (xy 130.335505 130.406106)
          (xy 130.625083 130.096114)
          (xy 130.885959 129.761607)
          (xy 131.116066 129.405235)
          (xy 131.313582 129.029818)
          (xy 131.476944 128.638329)
          (xy 131.604858 128.233868)
          (xy 131.696312 127.819638)
          (xy 131.75058 127.398917)
          (xy 131.767235 126.975039)
          (xy 131.746143 126.551357)
          (xy 131.687471 126.131229)
          (xy 131.591685 125.717979)
          (xy 131.459542 125.314879)
          (xy 131.29209 124.925123)
          (xy 131.090653 124.551795)
          (xy 130.856827 124.197851)
          (xy 130.592463 123.866095)
          (xy 130.299654 123.559152)
          (xy 129.980719 123.279454)
          (xy 129.638184 123.029215)
          (xy 129.274759 122.810415)
          (xy 128.893323 122.624788)
          (xy 128.496896 122.473804)
          (xy 128.088617 122.358657)
          (xy 127.671718 122.28026)
          (xy 127.249501 122.239233)
        )
      )
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "F.Cu")
    (at 157.043475 100.274399 -90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Dielectric" "X7R")
    (property "MPN" "GCJ188R71H104KA12D ")
    (property "Sheetfile" "opamp-spiro.kicad_sch")
    (property "Sheetname" "")
    (property "Voltage" "50V")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C14" (at 4.119601 -0.258725 90) (layer "F.SilkS"))
    (fp_text value "0.1u" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.8625 0 270) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 12 "VDD") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8625 0 270) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TestPoint:TestPoint_THTPad_2.0x2.0mm_Drill1.0mm" (layer "F.Cu")
    (at 146.8 88.4)
    (descr "THT rectangular pad as test Point, square 2.0mm_Drill1.0mm  side length, hole diameter 1.0mm")
    (tags "test point THT pad rectangle square")
    (property "Sheetfile" "opamp-spiro.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "test point")
    (property "ki_keywords" "test point tp")
    (attr exclude_from_pos_files)
    (fp_text reference "TP9" (at 0 -1.998) (layer "F.SilkS") hide)
    (fp_text value "TestPoint" (at 0 2.05) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -2) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 4 "GND") (pinfunction "1") (pintype "passive"))
  )
  (footprint "TestPoint:TestPoint_THTPad_2.0x2.0mm_Drill1.0mm" (layer "F.Cu")
    (at 127.846825 98.060799)
    (descr "THT rectangular pad as test Point, square 2.0mm_Drill1.0mm  side length, hole diameter 1.0mm")
    (tags "test point THT pad rectangle square")
    (property "Sheetfile" "opamp-spiro.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "test point")
    (property "ki_keywords" "test point tp")
    (attr exclude_from_pos_files)
    (fp_text reference "TP1" (at -2.8194 0) (layer "F.SilkS") hide)
    (fp_text value "TestPoint" (at 0 2.05) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -2) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 7 "/cos_fixed_freq") (pinfunction "1") (pintype "passive"))
  )
  (footprint "TestPoint:TestPoint_THTPad_2.0x2.0mm_Drill1.0mm" (layer "F.Cu")
    (at 127.6 113.8 90)
    (descr "THT rectangular pad as test Point, square 2.0mm_Drill1.0mm  side length, hole diameter 1.0mm")
    (tags "test point THT pad rectangle square")
    (property "Sheetfile" "opamp-spiro.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "test point")
    (property "ki_keywords" "test point tp")
    (attr exclude_from_pos_files)
    (fp_text reference "TP5" (at 0 2.5 90) (layer "F.SilkS") hide)
    (fp_text value "TestPoint" (at 0 2.05 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -2 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 4 "GND") (pinfunction "1") (pintype "passive"))
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (at 141.955875 93.539599 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "MPN" "ERJ-3EKF1002V")
    (property "Sheetfile" "opamp-spiro.kicad_sch")
    (property "Sheetname" "")
    (property "Tol" "1%")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R15" (at -3.1223 -0.0508) (layer "F.SilkS"))
    (fp_text value "10k" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 180) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 27 "/sin_fixed_freq") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 14 "Net-(U1C--)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TestPoint:TestPoint_THTPad_2.0x2.0mm_Drill1.0mm" (layer "F.Cu")
    (at 176.15 95.1)
    (descr "THT rectangular pad as test Point, square 2.0mm_Drill1.0mm  side length, hole diameter 1.0mm")
    (tags "test point THT pad rectangle square")
    (property "Sheetfile" "opamp-spiro.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "test point")
    (property "ki_keywords" "test point tp")
    (attr exclude_from_pos_files)
    (fp_text reference "TP3" (at -0.26 2.34) (layer "F.SilkS"))
    (fp_text value "TestPoint" (at 0 2.05) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -2) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 12 "VDD") (pinfunction "1") (pintype "passive"))
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (at 154.261182 85.8012 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "MPN" "ERJ-3EKF1002V")
    (property "Sheetfile" "opamp-spiro.kicad_sch")
    (property "Sheetname" "")
    (property "Tol" "1%")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R27" (at -3.2012 -0.938818 -90) (layer "F.SilkS"))
    (fp_text value "10k" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 270) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 13 "Net-(U2D--)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TestPoint:TestPoint_THTPad_2.0x2.0mm_Drill1.0mm" (layer "F.Cu")
    (at 166.62 106.76)
    (descr "THT rectangular pad as test Point, square 2.0mm_Drill1.0mm  side length, hole diameter 1.0mm")
    (tags "test point THT pad rectangle square")
    (property "Sheetfile" "opamp-spiro.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "test point")
    (property "ki_keywords" "test point tp")
    (attr exclude_from_pos_files)
    (fp_text reference "TP7" (at 0 -1.998) (layer "F.SilkS") hide)
    (fp_text value "TestPoint" (at 0 2.05) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -2) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 28 "/+sin_var_freq") (pinfunction "1") (pintype "passive"))
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (at 131.299582 85.4456 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "MPN" "ERJ-3EKF1001V")
    (property "Sheetfile" "opamp-spiro.kicad_sch")
    (property "Sheetname" "")
    (property "Tol" "1%")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R23" (at 3.2004 0.196218 90) (layer "F.SilkS"))
    (fp_text value "1k" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 90) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 35 "Net-(C15-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 29 "/Channel 1, X") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "F.Cu")
    (at 166.8272 97.3328 -90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Dielectric" "X7R")
    (property "MPN" "GRM188Z71A106KA73D ")
    (property "Sheetfile" "opamp-spiro.kicad_sch")
    (property "Sheetname" "")
    (property "Voltage" "10V")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C9" (at 0.0254 1.4732 90) (layer "F.SilkS"))
    (fp_text value "10u" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.8625 0 270) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 12 "VDD") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8625 0 270) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "F.Cu")
    (at 132.188582 89.7636 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Dielectric" "NP0")
    (property "MPN" "GCM1885C2A101JA16D ")
    (property "Sheetfile" "opamp-spiro.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C15" (at 3.258182 0) (layer "F.SilkS"))
    (fp_text value "100p" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.8625 0 180) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 11 "Net-(U1D--)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8625 0 180) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 35 "Net-(C15-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (at 134.933425 100.016599 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "MPN" "ERJ-3EKF2202V")
    (property "Sheetfile" "opamp-spiro.kicad_sch")
    (property "Sheetname" "")
    (property "Tol" "1%")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R4" (at -2.6162 -0.0254 90) (layer "F.SilkS"))
    (fp_text value "22k" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 90) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "Net-(U1A-+)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Global_MWS_Library:logo_for_pcb_15mm" (layer "F.Cu")
    (at 123.6 113.4 90)
    (property "Sheetfile" "opamp-spiro.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "SYM1" (at 2.8 3.7 90) (layer "F.SilkS") hide)
    (fp_text value "MWS_Logo" (at -3.1 3.8 90) (layer "F.SilkS") hide)
  )
  (footprint "TestPoint:TestPoint_THTPad_2.0x2.0mm_Drill1.0mm" (layer "F.Cu")
    (at 148.495382 103.378)
    (descr "THT rectangular pad as test Point, square 2.0mm_Drill1.0mm  side length, hole diameter 1.0mm")
    (tags "test point THT pad rectangle square")
    (property "Sheetfile" "opamp-spiro.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "test point")
    (property "ki_keywords" "test point tp")
    (attr exclude_from_pos_files)
    (fp_text reference "TP2" (at -2.267582 0.0254 90) (layer "F.SilkS") hide)
    (fp_text value "TestPoint" (at 0 2.05) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -2) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 9 "/cos_var_freq") (pinfunction "1") (pintype "passive"))
  )
  (footprint "Package_SO:SOIC-14_3.9x8.7mm_P1.27mm" (layer "F.Cu")
    (at 135.592182 94.5388 90)
    (descr "SOIC, 14 Pin (JEDEC MS-012AB, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_14.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (property "MPN" "MCP6004-I/SL ")
    (property "Sheetfile" "opamp-spiro.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "1MHz, Low-Power Op Amp, DIP-14/SOIC-14/TSSOP-14")
    (property "ki_keywords" "quad opamp")
    (attr smd)
    (fp_text reference "U1" (at 3.1496 -5.696582 180) (layer "F.SilkS"))
    (fp_text value "MCP6004" (at 0 5.28 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.475 -3.81 90) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 7 "/cos_fixed_freq") (pintype "output"))
    (pad "2" smd roundrect (at -2.475 -2.54 90) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 20 "Net-(U1A--)") (pinfunction "-") (pintype "input"))
    (pad "3" smd roundrect (at -2.475 -1.27 90) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "Net-(U1A-+)") (pinfunction "+") (pintype "input"))
    (pad "4" smd roundrect (at -2.475 0 90) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 12 "VDD") (pinfunction "V+") (pintype "power_in"))
    (pad "5" smd roundrect (at -2.475 1.27 90) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 8 "Net-(U1B-+)") (pinfunction "+") (pintype "input"))
    (pad "6" smd roundrect (at -2.475 2.54 90) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 23 "Net-(U1B--)") (pinfunction "-") (pintype "input"))
    (pad "7" smd roundrect (at -2.475 3.81 90) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 27 "/sin_fixed_freq") (pintype "output"))
    (pad "8" smd roundrect (at 2.475 3.81 90) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 33 "Net-(D2-A)") (pintype "output"))
    (pad "9" smd roundrect (at 2.475 2.54 90) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 14 "Net-(U1C--)") (pinfunction "-") (pintype "input"))
    (pad "10" smd roundrect (at 2.475 1.27 90) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "GND") (pinfunction "+") (pintype "input"))
    (pad "11" smd roundrect (at 2.475 0 90) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "VSS") (pinfunction "V-") (pintype "power_in"))
    (pad "12" smd roundrect (at 2.475 -1.27 90) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 38 "/X, mixer out") (pinfunction "+") (pintype "input"))
    (pad "13" smd roundrect (at 2.475 -2.54 90) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 11 "Net-(U1D--)") (pinfunction "-") (pintype "input"))
    (pad "14" smd roundrect (at 2.475 -3.81 90) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 35 "Net-(C15-Pad2)") (pintype "output"))
    (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-14_3.9x8.7mm_P1.27mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Global_MWS_Library:MountingHole_No4_Isolated" (layer "F.Cu")
    (at 177.8 127)
    (descr "Mounting Hole #4 isolated")
    (tags "Mounting Hole #4 isolated")
    (property "Sheetfile" "opamp-spiro.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole without connection")
    (property "ki_keywords" "mounting hole")
    (attr exclude_from_pos_files)
    (fp_text reference "H2" (at 0 -6) (layer "F.SilkS") hide)
    (fp_text value "#4" (at 0 7.2) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 3) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 3.175 3.175) (drill 3.175) (layers "F&B.Cu" "*.Mask"))
    (zone (net 0) (net_name "") (layers "*.Cu" "*.SilkS") (hatch edge 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.254) (filled_areas_thickness no)
      (keepout (tracks not_allowed) (vias not_allowed) (pads allowed) (copperpour not_allowed) (footprints not_allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 182.5673 127)
          (xy 182.548427 126.576214)
          (xy 182.491956 126.155784)
          (xy 182.398335 125.742038)
          (xy 182.268304 125.338252)
          (xy 182.102895 124.947624)
          (xy 181.903415 124.573247)
          (xy 181.671446 124.218084)
          (xy 181.408823 123.884948)
          (xy 181.117625 123.576477)
          (xy 180.800159 123.295112)
          (xy 180.458938 123.043082)
          (xy 180.096664 122.822383)
          (xy 179.716206 122.634762)
          (xy 179.320575 122.481704)
          (xy 178.912904 122.364421)
          (xy 178.496422 122.283842)
          (xy 178.074425 122.240605)
          (xy 177.650255 122.235052)
          (xy 177.227272 122.267228)
          (xy 176.808823 122.336877)
          (xy 176.398222 122.443448)
          (xy 175.99872 122.586097)
          (xy 175.61348 122.763695)
          (xy 175.245553 122.974835)
          (xy 174.897852 123.217847)
          (xy 174.573129 123.490804)
          (xy 174.273957 123.791547)
          (xy 174.002703 124.117695)
          (xy 173.761516 124.466664)
          (xy 173.552305 124.835691)
          (xy 173.376726 125.221855)
          (xy 173.236171 125.622099)
          (xy 173.131751 126.033252)
          (xy 173.064294 126.45206)
          (xy 173.034334 126.875207)
          (xy 173.042107 127.299341)
          (xy 173.087553 127.721106)
          (xy 173.170312 128.137161)
          (xy 173.289727 128.544212)
          (xy 173.444855 128.939036)
          (xy 173.634466 129.318507)
          (xy 173.857059 129.67962)
          (xy 174.110872 130.019517)
          (xy 174.393894 130.335505)
          (xy 174.703886 130.625083)
          (xy 175.038393 130.885959)
          (xy 175.394765 131.116066)
          (xy 175.770182 131.313582)
          (xy 176.161671 131.476944)
          (xy 176.566132 131.604858)
          (xy 176.980362 131.696312)
          (xy 177.401083 131.75058)
          (xy 177.824961 131.767235)
          (xy 178.248643 131.746143)
          (xy 178.668771 131.687471)
          (xy 179.082021 131.591685)
          (xy 179.485121 131.459542)
          (xy 179.874877 131.29209)
          (xy 180.248205 131.090653)
          (xy 180.602149 130.856827)
          (xy 180.933905 130.592463)
          (xy 181.240848 130.299654)
          (xy 181.520546 129.980719)
          (xy 181.770785 129.638184)
          (xy 181.989585 129.274759)
          (xy 182.175212 128.893323)
          (xy 182.326196 128.496896)
          (xy 182.441343 128.088617)
          (xy 182.51974 127.671718)
          (xy 182.560767 127.249501)
        )
      )
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (at 149.118675 96.237699 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "MPN" "ERJ-3EKF1002V")
    (property "Sheetfile" "opamp-spiro.kicad_sch")
    (property "Sheetname" "")
    (property "Tol" "1%")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R8" (at 0 -1.43 90) (layer "F.SilkS"))
    (fp_text value "10k" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 90) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 9 "/cos_var_freq") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 24 "Net-(U2B--)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "F.Cu")
    (at 160.294675 88.309099)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Dielectric" "NP0")
    (property "MPN" "GCM1885C2A101JA16D ")
    (property "Sheetfile" "opamp-spiro.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C8" (at -2.174675 0.040901 270) (layer "F.SilkS"))
    (fp_text value "100p" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.8625 0) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 6 "Net-(U2C--)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8625 0) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "/-sin_var_freq") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TestPoint:TestPoint_THTPad_2.0x2.0mm_Drill1.0mm" (layer "F.Cu")
    (at 124 101.8)
    (descr "THT rectangular pad as test Point, square 2.0mm_Drill1.0mm  side length, hole diameter 1.0mm")
    (tags "test point THT pad rectangle square")
    (property "Sheetfile" "opamp-spiro.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "test point")
    (property "ki_keywords" "test point tp")
    (attr exclude_from_pos_files)
    (fp_text reference "TP13" (at 0 -1.998) (layer "F.SilkS") hide)
    (fp_text value "TestPoint" (at 0 2.05) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -2) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 38 "/X, mixer out") (pinfunction "1") (pintype "passive"))
  )
  (footprint "TestPoint:TestPoint_THTPad_2.0x2.0mm_Drill1.0mm" (layer "F.Cu")
    (at 171.958 88.0364)
    (descr "THT rectangular pad as test Point, square 2.0mm_Drill1.0mm  side length, hole diameter 1.0mm")
    (tags "test point THT pad rectangle square")
    (property "Sheetfile" "opamp-spiro.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "test point")
    (property "ki_keywords" "test point tp")
    (attr exclude_from_pos_files)
    (fp_text reference "TP19" (at 0 -1.998) (layer "F.SilkS"))
    (fp_text value "TestPoint" (at 0 2.05) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -2) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 19 "Net-(SW1B-B)") (pinfunction "1") (pintype "passive"))
  )
  (footprint "TestPoint:TestPoint_THTPad_2.0x2.0mm_Drill1.0mm" (layer "F.Cu")
    (at 135.6 79.4766)
    (descr "THT rectangular pad as test Point, square 2.0mm_Drill1.0mm  side length, hole diameter 1.0mm")
    (tags "test point THT pad rectangle square")
    (property "Sheetfile" "opamp-spiro.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "test point")
    (property "ki_keywords" "test point tp")
    (attr exclude_from_pos_files)
    (fp_text reference "TP17" (at 0 -1.998) (layer "F.SilkS") hide)
    (fp_text value "Chan 1, X" (at 0 2.05) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -2) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 29 "/Channel 1, X") (pinfunction "1") (pintype "passive"))
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "F.Cu")
    (at 153.448382 89.8906 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Dielectric" "NP0")
    (property "MPN" "GCM1885C2A101JA16D ")
    (property "Sheetfile" "opamp-spiro.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C16" (at 3.232782 0.0508) (layer "F.SilkS"))
    (fp_text value "100p" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.8625 0 180) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 13 "Net-(U2D--)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8625 0 180) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 36 "Net-(C16-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (at 139.048225 86.376799 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "MPN" "ERJ-3EKF1002V")
    (property "Sheetfile" "opamp-spiro.kicad_sch")
    (property "Sheetname" "")
    (property "Tol" "1%")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R18" (at 0.0254 1.397) (layer "F.SilkS"))
    (fp_text value "10k" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 180) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 34 "Net-(D2-K)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 14 "Net-(U1C--)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "F.Cu")
    (at 135.568425 89.018399 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Dielectric" "X7R")
    (property "MPN" "GCJ188R71H104KA12D ")
    (property "Sheetfile" "opamp-spiro.kicad_sch")
    (property "Sheetname" "")
    (property "Voltage" "50V")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C10" (at 4.1656 0.127 90) (layer "F.SilkS"))
    (fp_text value "0.1u" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.8625 0 90) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "VSS") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8625 0 90) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_SOD-523" (layer "F.Cu")
    (at 162.936275 87.433199 90)
    (descr "http://www.diodes.com/datasheets/ap02001.pdf p.144")
    (tags "Diode SOD523")
    (property "MPN" "1N914BWT ")
    (property "Sheetfile" "opamp-spiro.kicad_sch")
    (property "Sheetname" "")
    (property "Sim.Device" "D")
    (property "Sim.Pins" "1=K 2=A")
    (property "ki_description" "75V 0.15A Fast switching Diode, SOD-523")
    (property "ki_keywords" "diode")
    (attr smd)
    (fp_text reference "D5" (at 2.343199 -0.046075 90) (layer "F.SilkS"))
    (fp_text value "1N914WT" (at 0 1.4 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -1.3 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.7 0 270) (size 0.6 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "/-sin_var_freq") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7 0 270) (size 0.6 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 15 "Net-(D4-K)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SOD-523.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Global_MWS_Library:MountingHole_No4_Isolated" (layer "F.Cu")
    (at 127 76.2)
    (descr "Mounting Hole #4 isolated")
    (tags "Mounting Hole #4 isolated")
    (property "Sheetfile" "opamp-spiro.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole without connection")
    (property "ki_keywords" "mounting hole")
    (attr exclude_from_pos_files)
    (fp_text reference "H4" (at 0 -6) (layer "F.SilkS") hide)
    (fp_text value "#4" (at 0 7.2) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 3) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 3.175 3.175) (drill 3.175) (layers "F&B.Cu" "*.Mask"))
    (zone (net 0) (net_name "") (layers "*.Cu" "*.SilkS") (hatch edge 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.254) (filled_areas_thickness no)
      (keepout (tracks not_allowed) (vias not_allowed) (pads allowed) (copperpour not_allowed) (footprints not_allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 131.7673 76.2)
          (xy 131.748427 75.776214)
          (xy 131.691956 75.355784)
          (xy 131.598335 74.942038)
          (xy 131.468304 74.538252)
          (xy 131.302895 74.147624)
          (xy 131.103415 73.773247)
          (xy 130.871446 73.418084)
          (xy 130.608823 73.084948)
          (xy 130.317625 72.776477)
          (xy 130.000159 72.495112)
          (xy 129.658938 72.243082)
          (xy 129.296664 72.022383)
          (xy 128.916206 71.834762)
          (xy 128.520575 71.681704)
          (xy 128.112904 71.564421)
          (xy 127.696422 71.483842)
          (xy 127.274425 71.440605)
          (xy 126.850255 71.435052)
          (xy 126.427272 71.467228)
          (xy 126.008823 71.536877)
          (xy 125.598222 71.643448)
          (xy 125.19872 71.786097)
          (xy 124.81348 71.963695)
          (xy 124.445553 72.174835)
          (xy 124.097852 72.417847)
          (xy 123.773129 72.690804)
          (xy 123.473957 72.991547)
          (xy 123.202703 73.317695)
          (xy 122.961516 73.666664)
          (xy 122.752305 74.035691)
          (xy 122.576726 74.421855)
          (xy 122.436171 74.822099)
          (xy 122.331751 75.233252)
          (xy 122.264294 75.65206)
          (xy 122.234334 76.075207)
          (xy 122.242107 76.499341)
          (xy 122.287553 76.921106)
          (xy 122.370312 77.337161)
          (xy 122.489727 77.744212)
          (xy 122.644855 78.139036)
          (xy 122.834466 78.518507)
          (xy 123.057059 78.87962)
          (xy 123.310872 79.219517)
          (xy 123.593894 79.535505)
          (xy 123.903886 79.825083)
          (xy 124.238393 80.085959)
          (xy 124.594765 80.316066)
          (xy 124.970182 80.513582)
          (xy 125.361671 80.676944)
          (xy 125.766132 80.804858)
          (xy 126.180362 80.896312)
          (xy 126.601083 80.95058)
          (xy 127.024961 80.967235)
          (xy 127.448643 80.946143)
          (xy 127.868771 80.887471)
          (xy 128.282021 80.791685)
          (xy 128.685121 80.659542)
          (xy 129.074877 80.49209)
          (xy 129.448205 80.290653)
          (xy 129.802149 80.056827)
          (xy 130.133905 79.792463)
          (xy 130.440848 79.499654)
          (xy 130.720546 79.180719)
          (xy 130.970785 78.838184)
          (xy 131.189585 78.474759)
          (xy 131.375212 78.093323)
          (xy 131.526196 77.696896)
          (xy 131.641343 77.288617)
          (xy 131.71974 76.871718)
          (xy 131.760767 76.449501)
        )
      )
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (at 149.093275 99.639399 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "MPN" "ERJ-3EKF1002V")
    (property "Sheetfile" "opamp-spiro.kicad_sch")
    (property "Sheetname" "")
    (property "Tol" "1%")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R6" (at 0.045999 -1.570075 90) (layer "F.SilkS"))
    (fp_text value "10k" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 90) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 21 "Net-(U2A--)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 9 "/cos_var_freq") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Global_MWS_Library:Switch_pushbtn_DPDT_Latching_TL2201EEYA" (layer "F.Cu")
    (at 178.562 88.9)
    (property "Datasheet-2" "https://configured-product-images.s3.amazonaws.com/2D/specs/P010350.pdf")
    (property "MPN" "TL2201EEYA")
    (property "Sheetfile" "opamp-spiro.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Switch, dual pole double throw, separate symbols")
    (property "ki_keywords" "switch dual-pole double-throw DPDT spdt ON-ON")
    (attr through_hole)
    (fp_text reference "SW1" (at -6.112 2.06 90) (layer "F.SilkS"))
    (fp_text value "SW_DPDT_x2" (at 3.805 6.135) (layer "F.Fab"))
    (pad "1" thru_hole rect (at -2.45 2.7) (size 1.308 1.308) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 31 "unconnected-(SW1A-A-Pad1)") (pinfunction "A") (pintype "passive+no_connect"))
    (pad "2" thru_hole circle (at 0.05 2.7) (size 1.308 1.308) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 17 "Net-(SW1A-B)") (pinfunction "B") (pintype "passive"))
    (pad "3" thru_hole circle (at 2.55 2.7) (size 1.308 1.308) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 12 "VDD") (pinfunction "C") (pintype "passive"))
    (pad "4" thru_hole circle (at -2.45 -2.7) (size 1.308 1.308) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 32 "unconnected-(SW1B-A-Pad4)") (pinfunction "A") (pintype "passive+no_connect"))
    (pad "5" thru_hole circle (at 0.05 -2.7) (size 1.308 1.308) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 19 "Net-(SW1B-B)") (pinfunction "B") (pintype "passive"))
    (pad "6" thru_hole circle (at 2.55 -2.7) (size 1.308 1.308) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 5 "VSS") (pinfunction "C") (pintype "passive"))
    (model "$MY3DMOD/TL2201EEYA--3DModel-STEP-418109.STEP"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "F.Cu")
    (at 169.52 83.4969 -90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Dielectric" "X7R")
    (property "MPN" "GRM188Z71A106KA73D ")
    (property "Sheetfile" "opamp-spiro.kicad_sch")
    (property "Sheetname" "")
    (property "Voltage" "10V")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C4" (at -3.9949 0.0258 90) (layer "F.SilkS"))
    (fp_text value "10u" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.8625 0 270) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8625 0 270) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "VSS") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (at 166.7256 92.6338 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "MPN" "ERJ-3EKF1001V")
    (property "Sheetfile" "opamp-spiro.kicad_sch")
    (property "Sheetname" "")
    (property "Tol" "1%")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R11" (at -0.0254 1.4478 -90) (layer "F.SilkS"))
    (fp_text value "1k" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 270) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 26 "Net-(D1-A)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 12 "VDD") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "F.Cu")
    (at 136.533625 100.016599 -90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Dielectric" "X7R")
    (property "MPN" "GCJ188R71H104KA12D ")
    (property "Sheetfile" "opamp-spiro.kicad_sch")
    (property "Sheetname" "")
    (property "Voltage" "50V")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C11" (at 1.634201 -1.515375 90) (layer "F.SilkS"))
    (fp_text value "0.1u" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.8625 0 270) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 12 "VDD") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8625 0 270) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_SOD-523" (layer "F.Cu")
    (at 164.460275 87.433199 -90)
    (descr "http://www.diodes.com/datasheets/ap02001.pdf p.144")
    (tags "Diode SOD523")
    (property "MPN" "1N914BWT ")
    (property "Sheetfile" "opamp-spiro.kicad_sch")
    (property "Sheetname" "")
    (property "Sim.Device" "D")
    (property "Sim.Pins" "1=K 2=A")
    (property "ki_description" "75V 0.15A Fast switching Diode, SOD-523")
    (property "ki_keywords" "diode")
    (attr smd)
    (fp_text reference "D4" (at -2.343199 -0.030125 90) (layer "F.SilkS"))
    (fp_text value "1N914WT" (at 0 1.4 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -1.3 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.7 0 90) (size 0.6 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 15 "Net-(D4-K)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7 0 90) (size 0.6 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "/-sin_var_freq") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SOD-523.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (at 152.447975 100.096599)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "MPN" "ERJ-3EKF1002V")
    (property "Sheetfile" "opamp-spiro.kicad_sch")
    (property "Sheetname" "")
    (property "Tol" "1%")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R2" (at 0.002825 -1.239799) (layer "F.SilkS"))
    (fp_text value "10k" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "/-sin_var_freq") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 21 "Net-(U2A--)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (at 152.508582 85.7758 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "MPN" "ERJ-3EKF1001V")
    (property "Sheetfile" "opamp-spiro.kicad_sch")
    (property "Sheetname" "")
    (property "Tol" "1%")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R29" (at 0 -1.43 90) (layer "F.SilkS"))
    (fp_text value "1k" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 90) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 36 "Net-(C16-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 30 "/Channel 2, Y") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TestPoint:TestPoint_THTPad_2.0x2.0mm_Drill1.0mm" (layer "F.Cu")
    (at 167.5892 101.8794)
    (descr "THT rectangular pad as test Point, square 2.0mm_Drill1.0mm  side length, hole diameter 1.0mm")
    (tags "test point THT pad rectangle square")
    (property "Sheetfile" "opamp-spiro.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "test point")
    (property "ki_keywords" "test point tp")
    (attr exclude_from_pos_files)
    (fp_text reference "TP12" (at -3.429 -1.016) (layer "F.SilkS"))
    (fp_text value "TestPoint" (at 0 2.05) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -2) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 16 "Net-(BT1-+)") (pinfunction "1") (pintype "passive"))
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (at 130.209025 97.908399 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "MPN" "ERJ-3EKF1002V")
    (property "Sheetfile" "opamp-spiro.kicad_sch")
    (property "Sheetname" "")
    (property "Tol" "1%")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R5" (at -2.6162 0.0508 90) (layer "F.SilkS"))
    (fp_text value "10k" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 90) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 20 "Net-(U1A--)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 7 "/cos_fixed_freq") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "F.Cu")
    (at 152.649275 101.950799)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "MPN" "C0805C473K3GECAUTO")
    (property "Sheetfile" "opamp-spiro.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C2" (at -1.479275 1.749201) (layer "F.SilkS"))
    (fp_text value "47n" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.0375 0) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 2 "/-sin_var_freq") (pintype "passive"))
    (pad "2" smd roundrect (at 1.0375 0) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 3 "Net-(U2A-+)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Global_MWS_Library:MountingHole_No4_Isolated" (layer "F.Cu")
    (at 177.8 76.2)
    (descr "Mounting Hole #4 isolated")
    (tags "Mounting Hole #4 isolated")
    (property "Sheetfile" "opamp-spiro.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole without connection")
    (property "ki_keywords" "mounting hole")
    (attr exclude_from_pos_files)
    (fp_text reference "H3" (at 0 -6) (layer "F.SilkS") hide)
    (fp_text value "#4" (at 0 7.2) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 3) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 3.175 3.175) (drill 3.175) (layers "F&B.Cu" "*.Mask"))
    (zone (net 0) (net_name "") (layers "*.Cu" "*.SilkS") (hatch edge 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.254) (filled_areas_thickness no)
      (keepout (tracks not_allowed) (vias not_allowed) (pads allowed) (copperpour not_allowed) (footprints not_allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 182.5673 76.2)
          (xy 182.548427 75.776214)
          (xy 182.491956 75.355784)
          (xy 182.398335 74.942038)
          (xy 182.268304 74.538252)
          (xy 182.102895 74.147624)
          (xy 181.903415 73.773247)
          (xy 181.671446 73.418084)
          (xy 181.408823 73.084948)
          (xy 181.117625 72.776477)
          (xy 180.800159 72.495112)
          (xy 180.458938 72.243082)
          (xy 180.096664 72.022383)
          (xy 179.716206 71.834762)
          (xy 179.320575 71.681704)
          (xy 178.912904 71.564421)
          (xy 178.496422 71.483842)
          (xy 178.074425 71.440605)
          (xy 177.650255 71.435052)
          (xy 177.227272 71.467228)
          (xy 176.808823 71.536877)
          (xy 176.398222 71.643448)
          (xy 175.99872 71.786097)
          (xy 175.61348 71.963695)
          (xy 175.245553 72.174835)
          (xy 174.897852 72.417847)
          (xy 174.573129 72.690804)
          (xy 174.273957 72.991547)
          (xy 174.002703 73.317695)
          (xy 173.761516 73.666664)
          (xy 173.552305 74.035691)
          (xy 173.376726 74.421855)
          (xy 173.236171 74.822099)
          (xy 173.131751 75.233252)
          (xy 173.064294 75.65206)
          (xy 173.034334 76.075207)
          (xy 173.042107 76.499341)
          (xy 173.087553 76.921106)
          (xy 173.170312 77.337161)
          (xy 173.289727 77.744212)
          (xy 173.444855 78.139036)
          (xy 173.634466 78.518507)
          (xy 173.857059 78.87962)
          (xy 174.110872 79.219517)
          (xy 174.393894 79.535505)
          (xy 174.703886 79.825083)
          (xy 175.038393 80.085959)
          (xy 175.394765 80.316066)
          (xy 175.770182 80.513582)
          (xy 176.161671 80.676944)
          (xy 176.566132 80.804858)
          (xy 176.980362 80.896312)
          (xy 177.401083 80.95058)
          (xy 177.824961 80.967235)
          (xy 178.248643 80.946143)
          (xy 178.668771 80.887471)
          (xy 179.082021 80.791685)
          (xy 179.485121 80.659542)
          (xy 179.874877 80.49209)
          (xy 180.248205 80.290653)
          (xy 180.602149 80.056827)
          (xy 180.933905 79.792463)
          (xy 181.240848 79.499654)
          (xy 181.520546 79.180719)
          (xy 181.770785 78.838184)
          (xy 181.989585 78.474759)
          (xy 182.175212 78.093323)
          (xy 182.326196 77.696896)
          (xy 182.441343 77.288617)
          (xy 182.51974 76.871718)
          (xy 182.560767 76.449501)
        )
      )
    )
  )
  (footprint "TestPoint:TestPoint_THTPad_2.0x2.0mm_Drill1.0mm" (layer "F.Cu")
    (at 153.88 105.49)
    (descr "THT rectangular pad as test Point, square 2.0mm_Drill1.0mm  side length, hole diameter 1.0mm")
    (tags "test point THT pad rectangle square")
    (property "Sheetfile" "opamp-spiro.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "test point")
    (property "ki_keywords" "test point tp")
    (attr exclude_from_pos_files)
    (fp_text reference "TP11" (at 0 -1.998) (layer "F.SilkS") hide)
    (fp_text value "TestPoint" (at 0 2.05) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -2) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 2 "/-sin_var_freq") (pinfunction "1") (pintype "passive"))
  )
  (footprint "TestPoint:TestPoint_THTPad_2.0x2.0mm_Drill1.0mm" (layer "F.Cu")
    (at 181.5592 95.1992)
    (descr "THT rectangular pad as test Point, square 2.0mm_Drill1.0mm  side length, hole diameter 1.0mm")
    (tags "test point THT pad rectangle square")
    (property "Sheetfile" "opamp-spiro.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "test point")
    (property "ki_keywords" "test point tp")
    (attr exclude_from_pos_files)
    (fp_text reference "TP15" (at 0.0208 2.3708) (layer "F.SilkS"))
    (fp_text value "TestPoint" (at 0 2.05) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -2) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 17 "Net-(SW1A-B)") (pinfunction "1") (pintype "passive"))
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (at 160.294675 86.734299 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "MPN" "ERJ-3EKF1002V")
    (property "Sheetfile" "opamp-spiro.kicad_sch")
    (property "Sheetname" "")
    (property "Tol" "1%")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R19" (at 0 1.568099) (layer "F.SilkS"))
    (fp_text value "10k" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 180) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 15 "Net-(D4-K)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 6 "Net-(U2C--)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TestPoint:TestPoint_THTPad_2.0x2.0mm_Drill1.0mm" (layer "F.Cu")
    (at 172.1866 82.296)
    (descr "THT rectangular pad as test Point, square 2.0mm_Drill1.0mm  side length, hole diameter 1.0mm")
    (tags "test point THT pad rectangle square")
    (property "Sheetfile" "opamp-spiro.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "test point")
    (property "ki_keywords" "test point tp")
    (attr exclude_from_pos_files)
    (fp_text reference "TP4" (at 2.921 0.1778) (layer "F.SilkS") hide)
    (fp_text value "TestPoint" (at 0 2.05) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -2) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 5 "VSS") (pinfunction "1") (pintype "passive"))
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (at 162.529875 93.340199 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "MPN" "ERJ-3EKF1002V")
    (property "Sheetfile" "opamp-spiro.kicad_sch")
    (property "Sheetname" "")
    (property "Tol" "1%")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R17" (at 0 -1.43 90) (layer "F.SilkS"))
    (fp_text value "10k" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 270) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 28 "/+sin_var_freq") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 6 "Net-(U2C--)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (at 161.361475 100.299799 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "MPN" "ERJ-3EKF1002V")
    (property "Sheetfile" "opamp-spiro.kicad_sch")
    (property "Sheetname" "")
    (property "Tol" "1%")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R13" (at -3.205201 0.004725 90) (layer "F.SilkS"))
    (fp_text value "10k" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 90) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 24 "Net-(U2B--)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 28 "/+sin_var_freq") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "F.Cu")
    (at 128.810382 95.393799)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "MPN" "GRM1885C1H103JA01J ")
    (property "Sheetfile" "opamp-spiro.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C5" (at -2.5654 -0.0254) (layer "F.SilkS"))
    (fp_text value "10n" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.8625 0) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 7 "/cos_fixed_freq") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8625 0) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 8 "Net-(U1B-+)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (at 141.905075 91.913999 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "MPN" "ERJ-3EKF1003V")
    (property "Sheetfile" "opamp-spiro.kicad_sch")
    (property "Sheetname" "")
    (property "Tol" "1%")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R14" (at -3.1223 -0.0254) (layer "F.SilkS"))
    (fp_text value "100k" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 180) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 27 "/sin_fixed_freq") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 14 "Net-(U1C--)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "F.Cu")
    (at 138.997425 88.027799)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Dielectric" "NP0")
    (property "MPN" "GCM1885C2A101JA16D ")
    (property "Sheetfile" "opamp-spiro.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C7" (at -2.027425 -0.017799 90) (layer "F.SilkS"))
    (fp_text value "100p" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.8625 0) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 14 "Net-(U1C--)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8625 0) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 33 "Net-(D2-A)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (at 132.188582 88.0618 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "MPN" "ERJ-3EKF1002V")
    (property "Sheetfile" "opamp-spiro.kicad_sch")
    (property "Sheetname" "")
    (property "Tol" "1%")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R25" (at 3.283582 -0.127) (layer "F.SilkS"))
    (fp_text value "10k" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 180) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 11 "Net-(U1D--)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 35 "Net-(C15-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (at 153.422982 88.2904 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "MPN" "ERJ-3EKF1002V")
    (property "Sheetfile" "opamp-spiro.kicad_sch")
    (property "Sheetname" "")
    (property "Tol" "1%")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R28" (at 3.207382 -0.0254) (layer "F.SilkS"))
    (fp_text value "10k" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 180) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 13 "Net-(U2D--)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 36 "Net-(C16-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (at 131.783825 100.018499 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "MPN" "ERJ-3EKF1002V")
    (property "Sheetfile" "opamp-spiro.kicad_sch")
    (property "Sheetname" "")
    (property "Tol" "1%")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R1" (at -2.5635 0 90) (layer "F.SilkS"))
    (fp_text value "10k" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 90) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 33 "Net-(D2-A)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 20 "Net-(U1A--)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_SOD-523" (layer "F.Cu")
    (at 141.713582 87.0712 90)
    (descr "http://www.diodes.com/datasheets/ap02001.pdf p.144")
    (tags "Diode SOD523")
    (property "MPN" "1N914BWT ")
    (property "Sheetfile" "opamp-spiro.kicad_sch")
    (property "Sheetname" "")
    (property "Sim.Device" "D")
    (property "Sim.Pins" "1=K 2=A")
    (property "ki_description" "75V 0.15A Fast switching Diode, SOD-523")
    (property "ki_keywords" "diode")
    (attr smd)
    (fp_text reference "D3" (at 2.221 0.0762 90) (layer "F.SilkS"))
    (fp_text value "1N914WT" (at 0 1.4 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -1.3 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.7 0 270) (size 0.6 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 33 "Net-(D2-A)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7 0 270) (size 0.6 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 34 "Net-(D2-K)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SOD-523.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "F.Cu")
    (at 133.358625 100.020399 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "MPN" "GRM1885C1H103JA01J ")
    (property "Sheetfile" "opamp-spiro.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C1" (at -2.6378 -0.0254 90) (layer "F.SilkS"))
    (fp_text value "10n" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.8625 0 90) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 33 "Net-(D2-A)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8625 0 90) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "Net-(U1A-+)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_SOD-523" (layer "F.Cu")
    (at 143.237582 87.0712 -90)
    (descr "http://www.diodes.com/datasheets/ap02001.pdf p.144")
    (tags "Diode SOD523")
    (property "MPN" "1N914BWT ")
    (property "Sheetfile" "opamp-spiro.kicad_sch")
    (property "Sheetname" "")
    (property "Sim.Device" "D")
    (property "Sim.Pins" "1=K 2=A")
    (property "ki_description" "75V 0.15A Fast switching Diode, SOD-523")
    (property "ki_keywords" "diode")
    (attr smd)
    (fp_text reference "D2" (at -2.2718 -0.1016 90) (layer "F.SilkS"))
    (fp_text value "1N914WT" (at 0 1.4 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -1.3 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.7 0 90) (size 0.6 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 34 "Net-(D2-K)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7 0 90) (size 0.6 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 33 "Net-(D2-A)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SOD-523.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "F.Cu")
    (at 169.0624 87.6554 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "MPN" "ERJ-P06F10R0V")
    (property "Power" "0.5W")
    (property "Sheetfile" "opamp-spiro.kicad_sch")
    (property "Sheetname" "")
    (property "Tol" "1%")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R24" (at 1.8034 -2.4384 180) (layer "F.SilkS"))
    (fp_text value "10" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1 0 90) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 18 "Net-(BT2--)") (pintype "passive"))
    (pad "2" smd roundrect (at 1 0 90) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 19 "Net-(SW1B-B)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "F.Cu")
    (at 170.3324 101.9048 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "MPN" "ERJ-P06F10R0V")
    (property "Power" "0.5W")
    (property "Sheetfile" "opamp-spiro.kicad_sch")
    (property "Sheetname" "")
    (property "Tol" "1%")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R22" (at -0.0762 1.778 90) (layer "F.SilkS"))
    (fp_text value "10" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1 0 90) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 16 "Net-(BT1-+)") (pintype "passive"))
    (pad "2" smd roundrect (at 1 0 90) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 17 "Net-(SW1A-B)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_SOD-523" (layer "F.Cu")
    (at 165.0746 78.8162 90)
    (descr "http://www.diodes.com/datasheets/ap02001.pdf p.144")
    (tags "Diode SOD523")
    (property "MPN" "STS521033B950 ")
    (property "Sheetfile" "opamp-spiro.kicad_sch")
    (property "Sheetname" "")
    (property "Voltage" "")
    (property "ki_description" "Bidirectional transient-voltage-suppression diode")
    (property "ki_keywords" "diode TVS thyrector")
    (attr smd)
    (fp_text reference "D11" (at 2.794 0.0762 90) (layer "F.SilkS"))
    (fp_text value "3V3" (at 0 1.4 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -1.3 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.7 0 270) (size 0.6 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 30 "/Channel 2, Y") (pinfunction "A1") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7 0 270) (size 0.6 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "GND") (pinfunction "A2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SOD-523.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TestPoint:TestPoint_THTPad_2.0x2.0mm_Drill1.0mm" (layer "F.Cu")
    (at 178.94 119.75)
    (descr "THT rectangular pad as test Point, square 2.0mm_Drill1.0mm  side length, hole diameter 1.0mm")
    (tags "test point THT pad rectangle square")
    (property "Sheetfile" "opamp-spiro.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "test point")
    (property "ki_keywords" "test point tp")
    (attr exclude_from_pos_files)
    (fp_text reference "TP8" (at 0 -1.998) (layer "F.SilkS") hide)
    (fp_text value "TestPoint" (at 0 2.05) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -2) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 4 "GND") (pinfunction "1") (pintype "passive"))
  )
  (footprint "Global_MWS_Library:Pot-dual-Bourns-PTV112-4420A-B" (layer "F.Cu")
    (at 141.224 127)
    (property "MPN" "PTV112-4420A-B103")
    (property "Sheetfile" "opamp-spiro.kicad_sch")
    (property "Sheetname" "")
    (property "Tol" "20%")
    (property "ki_description" "Dual potentiometer, separate units")
    (property "ki_keywords" "resistor variable")
    (attr through_hole)
    (fp_text reference "RV2" (at -7.493 -16.6624 90 unlocked) (layer "F.SilkS"))
    (fp_text value "10k" (at 0.492 1.438 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at -0.508 3.438 unlocked) (layer "F.Fab"))
    (pad "" thru_hole oval (at -6.8 -11) (size 3.2 3.4) (drill oval 2.1 2.3) (layers "*.Cu" "*.Mask"))
    (pad "" thru_hole oval (at 6.8 -11) (size 3.2 3.4) (drill oval 2.1 2.3) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle (at -3 0) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 9 "/cos_var_freq") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at -5 0) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 38 "/X, mixer out") (pinfunction "2") (pintype "passive"))
    (pad "3" thru_hole circle (at 5 0) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 7 "/cos_fixed_freq") (pinfunction "3") (pintype "passive"))
    (pad "4" thru_hole circle (at -1 0) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 37 "/+{slash}- sin var freq") (pinfunction "4") (pintype "passive"))
    (pad "5" thru_hole circle (at 1 0) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 40 "/Y, mixer out") (pinfunction "5") (pintype "passive"))
    (pad "6" thru_hole circle (at 3 0) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 27 "/sin_fixed_freq") (pinfunction "6") (pintype "passive"))
    (model "${MY3DMOD}/PTV112-4420A-B503--3DModel-STEP-269445.STEP"
      (offset (xyz 0 11 -1.2))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (footprint "TestPoint:TestPoint_THTPad_2.0x2.0mm_Drill1.0mm" (layer "F.Cu")
    (at 144.9324 105.8164)
    (descr "THT rectangular pad as test Point, square 2.0mm_Drill1.0mm  side length, hole diameter 1.0mm")
    (tags "test point THT pad rectangle square")
    (property "Sheetfile" "opamp-spiro.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "test point")
    (property "ki_keywords" "test point tp")
    (attr exclude_from_pos_files)
    (fp_text reference "TP14" (at 0 -1.998) (layer "F.SilkS") hide)
    (fp_text value "TestPoint" (at 0 2.05) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -2) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 40 "/Y, mixer out") (pinfunction "1") (pintype "passive"))
  )
  (footprint "TestPoint:TestPoint_THTPad_2.0x2.0mm_Drill1.0mm" (layer "F.Cu")
    (at 125.65 85.35)
    (descr "THT rectangular pad as test Point, square 2.0mm_Drill1.0mm  side length, hole diameter 1.0mm")
    (tags "test point THT pad rectangle square")
    (property "Sheetfile" "opamp-spiro.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "test point")
    (property "ki_keywords" "test point tp")
    (attr exclude_from_pos_files)
    (fp_text reference "TP10" (at 0 -1.998) (layer "F.SilkS") hide)
    (fp_text value "TestPoint" (at 0 2.05) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -2) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 4 "GND") (pinfunction "1") (pintype "passive"))
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "F.Cu")
    (at 168.5544 97.3074 -90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Dielectric" "X7R")
    (property "MPN" "GRM188Z71A106KA73D ")
    (property "Sheetfile" "opamp-spiro.kicad_sch")
    (property "Sheetname" "")
    (property "Voltage" "10V")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C3" (at -2.2606 0.0508 -180) (layer "F.SilkS"))
    (fp_text value "10u" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.8625 0 270) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 12 "VDD") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8625 0 270) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "F.Cu")
    (at 151.049075 96.417499 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "MPN" "C0805C473K3GECAUTO")
    (property "Sheetfile" "opamp-spiro.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C6" (at 2.589899 0.030125 180) (layer "F.SilkS"))
    (fp_text value "47n" (at 0 1.68 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.0375 0 90) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 9 "/cos_var_freq") (pintype "passive"))
    (pad "2" smd roundrect (at 1.0375 0 90) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 10 "Net-(U2B-+)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Global_MWS_Library:Switch_pushbtn_DPDT_Latching_TL2201EEYA" (layer "F.Cu")
    (at 178.562 104.14)
    (property "Datasheet-2" "https://configured-product-images.s3.amazonaws.com/2D/specs/P010350.pdf")
    (property "MPN" "TL2201EEYA")
    (property "Sheetfile" "opamp-spiro.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Switch, dual pole double throw, separate symbols")
    (property "ki_keywords" "switch dual-pole double-throw DPDT spdt ON-ON")
    (attr through_hole)
    (fp_text reference "SW2" (at -3.429 -5.3086) (layer "F.SilkS"))
    (fp_text value "SW_DPDT_x2" (at 3.805 6.135) (layer "F.Fab"))
    (pad "1" thru_hole rect (at -2.45 2.7) (size 1.308 1.308) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 39 "unconnected-(SW2A-A-Pad1)") (pinfunction "A") (pintype "passive+no_connect"))
    (pad "2" thru_hole circle (at 0.05 2.7) (size 1.308 1.308) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 41 "unconnected-(SW2A-B-Pad2)") (pinfunction "B") (pintype "passive+no_connect"))
    (pad "3" thru_hole circle (at 2.55 2.7) (size 1.308 1.308) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 42 "unconnected-(SW2A-C-Pad3)") (pinfunction "C") (pintype "passive+no_connect"))
    (pad "4" thru_hole circle (at -2.45 -2.7) (size 1.308 1.308) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 2 "/-sin_var_freq") (pinfunction "A") (pintype "passive"))
    (pad "5" thru_hole circle (at 0.05 -2.7) (size 1.308 1.308) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 37 "/+{slash}- sin var freq") (pinfunction "B") (pintype "passive"))
    (pad "6" thru_hole circle (at 2.55 -2.7) (size 1.308 1.308) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 28 "/+sin_var_freq") (pinfunction "C") (pintype "passive"))
    (model "$MY3DMOD/TL2201EEYA--3DModel-STEP-418109.STEP"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (footprint "TestPoint:TestPoint_THTPad_2.0x2.0mm_Drill1.0mm" (layer "F.Cu")
    (at 171.0944 93.9546)
    (descr "THT rectangular pad as test Point, square 2.0mm_Drill1.0mm  side length, hole diameter 1.0mm")
    (tags "test point THT pad rectangle square")
    (property "Sheetfile" "opamp-spiro.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "test point")
    (property "ki_keywords" "test point tp")
    (attr exclude_from_pos_files)
    (fp_text reference "TP18" (at 0.1256 2.2754 180) (layer "F.SilkS"))
    (fp_text value "TestPoint" (at 0 2.05) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -2) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 18 "Net-(BT2--)") (pinfunction "1") (pintype "passive"))
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (at 139.148182 99.2378 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "MPN" "ERJ-3EKF2202V")
    (property "Sheetfile" "opamp-spiro.kicad_sch")
    (property "Sheetname" "")
    (property "Tol" "1%")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R10" (at -3.168018 -0.0254) (layer "F.SilkS"))
    (fp_text value "22k" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 180) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 8 "Net-(U1B-+)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (at 160.294675 89.909299)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "MPN" "ERJ-3EKF1002V")
    (property "Sheetfile" "opamp-spiro.kicad_sch")
    (property "Sheetname" "")
    (property "Tol" "1%")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R21" (at 3.052725 0.006701) (layer "F.SilkS"))
    (fp_text value "10k" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 6 "Net-(U2C--)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "/-sin_var_freq") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (at 155.468675 100.274399 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "MPN" "ERJ-3EKF2201V")
    (property "Sheetfile" "opamp-spiro.kicad_sch")
    (property "Sheetname" "")
    (property "Tol" "1%")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R3" (at 2.697201 -0.004725 90) (layer "F.SilkS"))
    (fp_text value "2.2k" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 270) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "Net-(U2A-+)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "Net-(R3-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_SOD-523" (layer "F.Cu")
    (at 139.8016 78.8416 90)
    (descr "http://www.diodes.com/datasheets/ap02001.pdf p.144")
    (tags "Diode SOD523")
    (property "MPN" "STS521033B950 ")
    (property "Sheetfile" "opamp-spiro.kicad_sch")
    (property "Sheetname" "")
    (property "Voltage" "")
    (property "ki_description" "Bidirectional transient-voltage-suppression diode")
    (property "ki_keywords" "diode TVS thyrector")
    (attr smd)
    (fp_text reference "D10" (at 0.0254 -1.3716 90) (layer "F.SilkS"))
    (fp_text value "3V3" (at 0 1.4 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -1.3 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.7 0 270) (size 0.6 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 29 "/Channel 1, X") (pinfunction "A1") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7 0 270) (size 0.6 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "GND") (pinfunction "A2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SOD-523.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (at 141.029425 96.587599 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "MPN" "ERJ-3EKF1002V")
    (property "Sheetfile" "opamp-spiro.kicad_sch")
    (property "Sheetname" "")
    (property "Tol" "1%")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R12" (at -0.067599 -1.667775 90) (layer "F.SilkS"))
    (fp_text value "10k" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 270) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 23 "Net-(U1B--)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 27 "/sin_fixed_freq") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (at 162.555275 96.794599 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "MPN" "ERJ-3EKF1003V")
    (property "Sheetfile" "opamp-spiro.kicad_sch")
    (property "Sheetname" "")
    (property "Tol" "1%")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R16" (at 0.045999 1.477925 90) (layer "F.SilkS"))
    (fp_text value "100k" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 90) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 28 "/+sin_var_freq") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 6 "Net-(U2C--)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (at 133.102982 85.471 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "MPN" "ERJ-3EKF1002V")
    (property "Sheetfile" "opamp-spiro.kicad_sch")
    (property "Sheetname" "")
    (property "Tol" "1%")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R26" (at -3.1496 0.032382 90) (layer "F.SilkS"))
    (fp_text value "10k" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 270) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 11 "Net-(U1D--)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (at 128.810382 93.818999)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "MPN" "ERJ-3EKF1002V")
    (property "Sheetfile" "opamp-spiro.kicad_sch")
    (property "Sheetname" "")
    (property "Tol" "1%")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R7" (at -2.75655 0.1524) (layer "F.SilkS"))
    (fp_text value "10k" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 7 "/cos_fixed_freq") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 23 "Net-(U1B--)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_SO:SOIC-14_3.9x8.7mm_P1.27mm" (layer "F.Cu")
    (at 156.840275 94.597099 90)
    (descr "SOIC, 14 Pin (JEDEC MS-012AB, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_14.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (property "MPN" "MCP6004-I/SL ")
    (property "Sheetfile" "opamp-spiro.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "1MHz, Low-Power Op Amp, DIP-14/SOIC-14/TSSOP-14")
    (property "ki_keywords" "quad opamp")
    (attr smd)
    (fp_text reference "U2" (at 2.903099 -5.888075 180) (layer "F.SilkS"))
    (fp_text value "MCP6004" (at 0 5.28 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.475 -3.81 90) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 9 "/cos_var_freq") (pintype "output"))
    (pad "2" smd roundrect (at -2.475 -2.54 90) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 21 "Net-(U2A--)") (pinfunction "-") (pintype "input"))
    (pad "3" smd roundrect (at -2.475 -1.27 90) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "Net-(U2A-+)") (pinfunction "+") (pintype "input"))
    (pad "4" smd roundrect (at -2.475 0 90) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 12 "VDD") (pinfunction "V+") (pintype "power_in"))
    (pad "5" smd roundrect (at -2.475 1.27 90) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 10 "Net-(U2B-+)") (pinfunction "+") (pintype "input"))
    (pad "6" smd roundrect (at -2.475 2.54 90) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 24 "Net-(U2B--)") (pinfunction "-") (pintype "input"))
    (pad "7" smd roundrect (at -2.475 3.81 90) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 28 "/+sin_var_freq") (pintype "output"))
    (pad "8" smd roundrect (at 2.475 3.81 90) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "/-sin_var_freq") (pintype "output"))
    (pad "9" smd roundrect (at 2.475 2.54 90) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 6 "Net-(U2C--)") (pinfunction "-") (pintype "input"))
    (pad "10" smd roundrect (at 2.475 1.27 90) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "GND") (pinfunction "+") (pintype "input"))
    (pad "11" smd roundrect (at 2.475 0 90) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "VSS") (pinfunction "V-") (pintype "power_in"))
    (pad "12" smd roundrect (at 2.475 -1.27 90) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 40 "/Y, mixer out") (pinfunction "+") (pintype "input"))
    (pad "13" smd roundrect (at 2.475 -2.54 90) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 13 "Net-(U2D--)") (pinfunction "-") (pintype "input"))
    (pad "14" smd roundrect (at 2.475 -3.81 90) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 36 "Net-(C16-Pad2)") (pintype "output"))
    (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-14_3.9x8.7mm_P1.27mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (at 139.022825 89.678799)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "MPN" "ERJ-3EKF1002V")
    (property "Sheetfile" "opamp-spiro.kicad_sch")
    (property "Sheetname" "")
    (property "Tol" "1%")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R20" (at 3.090175 0.059401) (layer "F.SilkS"))
    (fp_text value "10k" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 14 "Net-(U1C--)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 33 "Net-(D2-A)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "F.Cu")
    (at 167.7924 83.4655 -90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Dielectric" "X7R")
    (property "MPN" "GRM188Z71A106KA73D ")
    (property "Sheetfile" "opamp-spiro.kicad_sch")
    (property "Sheetname" "")
    (property "Voltage" "10V")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C12" (at -4.4461 -0.127 90) (layer "F.SilkS"))
    (fp_text value "10u" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.8625 0 270) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8625 0 270) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "VSS") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TestPoint:TestPoint_THTPad_2.0x2.0mm_Drill1.0mm" (layer "F.Cu")
    (at 162.4 79.5274)
    (descr "THT rectangular pad as test Point, square 2.0mm_Drill1.0mm  side length, hole diameter 1.0mm")
    (tags "test point THT pad rectangle square")
    (property "Sheetfile" "opamp-spiro.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "test point")
    (property "ki_keywords" "test point tp")
    (attr exclude_from_pos_files)
    (fp_text reference "TP16" (at 0 -1.998) (layer "F.SilkS") hide)
    (fp_text value "Chan 2, Y" (at 0 2.05) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -2) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 30 "/Channel 2, Y") (pinfunction "1") (pintype "passive"))
  )
  (footprint "LED_SMD:LED_0603_1608Metric" (layer "F.Cu")
    (at 166.7256 88.9 -90)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "LED")
    (property "MPN" "150060GS75000 ")
    (property "Sheetfile" "opamp-spiro.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Light emitting diode")
    (property "ki_keywords" "LED diode")
    (attr smd)
    (fp_text reference "D1" (at 0.5842 1.4224 90) (layer "F.SilkS"))
    (fp_text value "Green" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "VSS") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 26 "Net-(D1-A)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (at 159.380275 100.274399 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "MPN" "ERJ-3EKF2201V")
    (property "Sheetfile" "opamp-spiro.kicad_sch")
    (property "Sheetname" "")
    (property "Tol" "1%")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R9" (at 2.798801 -0.157125 90) (layer "F.SilkS"))
    (fp_text value "2.2k" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 270) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 10 "Net-(U2B-+)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 25 "Net-(R9-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Global_MWS_Library:BNC-RA-Molex-73100-0105" (layer "B.Cu")
    (at 165.1 74.5236 180)
    (property "MPN" "73100-0105")
    (property "Sheetfile" "opamp-spiro.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "coaxial connector (BNC, SMA, SMB, SMC, Cinch/RCA, LEMO, ...)")
    (property "ki_keywords" "BNC SMA SMB SMC LEMO coaxial connector CINCH RCA")
    (attr through_hole)
    (fp_text reference "J3" (at 7.2898 0.1778 unlocked) (layer "B.SilkS"))
    (fp_text value "BNC" (at 0 4.6 unlocked) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0.0508 2.8448 unlocked) (layer "B.Fab"))
    (pad "1" thru_hole circle (at 0 -7.8 180) (size 2 2) (drill 0.92) (layers "*.Cu" "*.Mask")
      (net 30 "/Channel 2, Y") (pinfunction "In") (pintype "passive"))
    (pad "2" thru_hole circle (at -3.8 0 180) (size 3.5 3.5) (drill 1.8) (layers "*.Cu" "*.Mask")
      (net 4 "GND") (pinfunction "Ext") (pintype "passive"))
    (pad "2" thru_hole circle (at 3.8 0 180) (size 3.5 3.5) (drill 1.8) (layers "*.Cu" "*.Mask")
      (net 4 "GND") (pinfunction "Ext") (pintype "passive"))
    (model "$MY3DMOD/BNC-RA-PCB-mount-Molex-73100-0105.stp"
      (offset (xyz 0 4.8 3.1))
      (scale (xyz 1 1 1))
      (rotate (xyz 90 180 0))
    )
  )
  (footprint "Global_MWS_Library:BNC-RA-Molex-73100-0105" (layer "B.Cu")
    (at 139.7 74.5236 180)
    (property "MPN" "73100-0105")
    (property "Sheetfile" "opamp-spiro.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "coaxial connector (BNC, SMA, SMB, SMC, Cinch/RCA, LEMO, ...)")
    (property "ki_keywords" "BNC SMA SMB SMC LEMO coaxial connector CINCH RCA")
    (attr through_hole)
    (fp_text reference "J2" (at -7.0358 0.0508 unlocked) (layer "B.SilkS"))
    (fp_text value "BNC" (at -0.1778 2.2352 unlocked) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at -0.2032 0.0254 unlocked) (layer "B.Fab"))
    (pad "1" thru_hole circle (at 0 -7.8 180) (size 2 2) (drill 0.92) (layers "*.Cu" "*.Mask")
      (net 29 "/Channel 1, X") (pinfunction "In") (pintype "passive"))
    (pad "2" thru_hole circle (at -3.8 0 180) (size 3.5 3.5) (drill 1.8) (layers "*.Cu" "*.Mask")
      (net 4 "GND") (pinfunction "Ext") (pintype "passive"))
    (pad "2" thru_hole circle (at 3.8 0 180) (size 3.5 3.5) (drill 1.8) (layers "*.Cu" "*.Mask")
      (net 4 "GND") (pinfunction "Ext") (pintype "passive"))
    (model "$MY3DMOD/BNC-RA-PCB-mount-Molex-73100-0105.stp"
      (offset (xyz 0 4.8 3.1))
      (scale (xyz 1 1 1))
      (rotate (xyz 90 180 0))
    )
  )
  (footprint "Global_MWS_Library:BatteryHolder_Keystone_2466_1xAAA_small_silkscreen" (layer "B.Cu")
    (at 125.5522 90.9574)
    (descr "1xAAA Battery Holder, Keystone, Plastic Case, http://www.keyelco.com/product-pdf.cfm?p=1031")
    (tags "AAA battery holder Keystone")
    (property "MPN" "2466")
    (property "Sheetfile" "opamp-spiro.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Single-cell battery")
    (property "ki_keywords" "battery cell")
    (attr through_hole)
    (fp_text reference "BT2" (at 23.0978 -7.8574 180) (layer "B.SilkS"))
    (fp_text value "1V5 (AAA)" (at 22 0 180) (layer "B.Fab"))
    (fp_text user "-" (at 48.26 0 180) (layer "B.SilkS"))
    (fp_text user "+" (at -3.81 0 180) (layer "B.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0 180) (layer "B.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 2 2) (drill 1.02) (layers "*.Cu" "*.Mask")
      (net 4 "GND") (pinfunction "+") (pintype "passive"))
    (pad "2" thru_hole circle (at 44.7 0) (size 2 2) (drill 1.02) (layers "*.Cu" "*.Mask")
      (net 18 "Net-(BT2--)") (pinfunction "-") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Battery.3dshapes/BatteryHolder_Keystone_2466_1xAAA.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Global_MWS_Library:BatteryHolder_Keystone_2466_1xAAA_small_silkscreen" (layer "B.Cu")
    (at 170.1038 105.156 180)
    (descr "1xAAA Battery Holder, Keystone, Plastic Case, http://www.keyelco.com/product-pdf.cfm?p=1031")
    (tags "AAA battery holder Keystone")
    (property "MPN" "2466")
    (property "Sheetfile" "opamp-spiro.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Single-cell battery")
    (property "ki_keywords" "battery cell")
    (attr through_hole)
    (fp_text reference "BT1" (at 21.9538 -7.944) (layer "B.SilkS"))
    (fp_text value "1V5 (AAA)" (at 22 0) (layer "B.Fab"))
    (fp_text user "-" (at 48.26 0) (layer "B.SilkS"))
    (fp_text user "+" (at -3.81 0) (layer "B.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" thru_hole rect (at 0 0 180) (size 2 2) (drill 1.02) (layers "*.Cu" "*.Mask")
      (net 16 "Net-(BT1-+)") (pinfunction "+") (pintype "passive"))
    (pad "2" thru_hole circle (at 44.7 0 180) (size 2 2) (drill 1.02) (layers "*.Cu" "*.Mask")
      (net 4 "GND") (pinfunction "-") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Battery.3dshapes/BatteryHolder_Keystone_2466_1xAAA.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 127 69.85) (end 177.8 69.85)
    (layer "Edge.Cuts"))
  (gr_arc (start 177.8 69.85) (mid 182.290128 71.709872) (end 184.15 76.2)
    (layer "Edge.Cuts"))
  (gr_arc (start 120.65 76.2) (mid 122.509872 71.709872) (end 127 69.85)
    (layer "Edge.Cuts"))
  (gr_line (start 177.8 133.35) (end 127 133.35)
    (layer "Edge.Cuts"))
  (gr_arc (start 127 133.35) (mid 122.509872 131.490128) (end 120.65 127)
    (layer "Edge.Cuts"))
  (gr_line (start 120.65 127) (end 120.65 76.2)
    (layer "Edge.Cuts"))
  (gr_line (start 184.15 76.2) (end 184.15 127)
    (layer "Edge.Cuts"))
  (gr_arc (start 184.15 127) (mid 182.290128 131.490128) (end 177.8 133.35)
    (layer "Edge.Cuts"))
  (gr_text "-sin, \n var" (at 151.33 109.23) (layer "F.SilkS"))
  (gr_text "X" (at 128.2 103) (layer "F.SilkS"))
  (gr_text "Mix\nout" (at 126 103) (layer "F.SilkS"))
  (gr_text "MIXING" (at 136.31 131.8) (layer "F.SilkS" knockout))
  (gr_text "FREQUENCY" (at 155.78 131.6) (layer "F.SilkS" knockout))
  (gr_text "Y" (at 144.526 108.6104) (layer "F.SilkS"))
  (gr_text "POWER" (at 174.44 84.07) (layer "F.SilkS" knockout))
  (gr_text "HYPO/\nEPI" (at 178.5 113.5) (layer "F.SilkS" knockout))
  (gr_text "sine,\nfixed" (at 133.477 107.2134) (layer "F.SilkS"))
  (gr_text "VCC" (at 174.33 96.43 90) (layer "F.SilkS"))
  (gr_text "cos,\nfixed" (at 122.5296 99.568) (layer "F.SilkS"))
  (gr_text "sin,\nvar" (at 162.6362 107.9754) (layer "F.SilkS"))
  (gr_text "X" (at 138.6 73.8) (layer "F.SilkS" knockout))
  (gr_text "X" (at 132.8 80) (layer "F.SilkS"))
  (gr_text "VSS" (at 170.7642 80.4926) (layer "F.SilkS"))
  (gr_text "Y" (at 162 77.8) (layer "F.SilkS"))
  (gr_text "Mix out" (at 142.875 104.4194) (layer "F.SilkS"))
  (gr_text "Y" (at 164 73.8) (layer "F.SilkS" knockout))
  (gr_text "Op Art" (at 152.4 73.4) (layer "F.SilkS"))
  (gr_text "cos,\nvar" (at 147.2438 107.2642) (layer "F.SilkS"))
  (zone (net 16) (net_name "Net-(BT1-+)") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30020)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 169.420235 102.40437)
        (xy 169.670232 101.971356)
        (xy 168.5892 101.024533)
        (xy 167.588334 101.878901)
        (xy 168.5892 102.8794)
      )
    )
  )
  (zone (net 10) (net_name "Net-(U2B-+)") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30215)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 158.13803 95.676909)
        (xy 157.850841 95.955336)
        (xy 157.810275 96.247099)
        (xy 158.110971 97.072816)
        (xy 158.323177 96.112191)
      )
    )
  )
  (zone (net 9) (net_name "/cos_var_freq") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30051)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 149.949938 97.139896)
        (xy 149.667096 97.422738)
        (xy 150.388471 97.956065)
        (xy 151.049782 97.455706)
        (xy 150.478404 96.886529)
      )
    )
  )
  (zone (net 34) (net_name "Net-(D2-K)") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30221)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 142.363582 86.5712)
        (xy 142.363582 86.1712)
        (xy 141.970985 86.082618)
        (xy 141.712582 86.3712)
        (xy 141.970985 86.659782)
      )
    )
  )
  (zone (net 27) (net_name "/sin_fixed_freq") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30087)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 140.153314 96.790999)
        (xy 140.153314 97.190999)
        (xy 140.559581 97.776023)
        (xy 141.030425 97.500099)
        (xy 141.136752 97.012599)
      )
    )
  )
  (zone (net 24) (net_name "Net-(U2B--)") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30063)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 160.756576 100.324557)
        (xy 160.473733 100.6074)
        (xy 160.886475 101.40905)
        (xy 161.362182 101.213006)
        (xy 161.545726 100.724799)
      )
    )
  )
  (zone (net 10) (net_name "Net-(U2B-+)") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30203)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 157.910314 98.34997)
        (xy 158.310236 98.342152)
        (xy 158.398857 97.954502)
        (xy 158.110256 97.0711)
        (xy 157.821693 97.954502)
      )
    )
  )
  (zone (net 18) (net_name "Net-(BT2--)") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30035)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 170.62473 92.398283)
        (xy 170.978283 92.04473)
        (xy 171.17608 91.340083)
        (xy 170.251493 90.956693)
        (xy 169.545093 91.664507)
      )
    )
  )
  (zone (net 5) (net_name "VSS") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30125)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 168.7424 84.578)
        (xy 168.7424 84.078)
        (xy 168.187269 83.853)
        (xy 167.7914 84.328)
        (xy 168.187269 84.803)
      )
    )
  )
  (zone (net 7) (net_name "/cos_fixed_freq") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30002)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 129.41251 99.909327)
        (xy 129.695353 99.626484)
        (xy 128.846825 97.646585)
        (xy 127.846118 98.060092)
        (xy 127.432612 99.060799)
      )
    )
  )
  (zone (net 4) (net_name "GND") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30096)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 135.841173 87.143399)
        (xy 135.341173 87.143399)
        (xy 135.111504 87.765012)
        (xy 135.568425 88.156899)
        (xy 136.025346 87.765012)
      )
    )
  )
  (zone (net 16) (net_name "Net-(BT1-+)") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30046)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 169.8538 104.1048)
        (xy 170.3538 104.1048)
        (xy 170.830602 103.495212)
        (xy 170.3324 102.9038)
        (xy 169.65143 103.350471)
      )
    )
  )
  (zone (net 12) (net_name "VDD") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30213)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 135.497645 98.400961)
        (xy 135.780487 98.118119)
        (xy 135.880764 97.896203)
        (xy 135.591475 97.013093)
        (xy 135.326269 97.93013)
      )
    )
  )
  (zone (net 24) (net_name "Net-(U2B--)") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30209)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 159.548071 95.793321)
        (xy 159.15576 95.871365)
        (xy 159.091693 96.189696)
        (xy 159.38047 97.073079)
        (xy 159.659911 96.176308)
      )
    )
  )
  (zone (net 14) (net_name "Net-(U1C--)") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30199)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 138.335725 90.7888)
        (xy 137.935725 90.7888)
        (xy 137.8436 91.181397)
        (xy 138.132182 92.0648)
        (xy 138.420764 91.181397)
      )
    )
  )
  (zone (net 9) (net_name "/cos_var_freq") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30153)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 149.318675 97.764399)
        (xy 148.918675 97.764399)
        (xy 148.636354 98.386012)
        (xy 149.093275 98.727899)
        (xy 149.550196 98.386012)
      )
    )
  )
  (zone (net 33) (net_name "Net-(D2-A)") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30143)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 140.135325 88.728799)
        (xy 139.735325 88.728799)
        (xy 139.465904 89.350412)
        (xy 139.935325 89.679799)
        (xy 140.404746 89.350412)
      )
    )
  )
  (zone (net 28) (net_name "/+sin_var_freq") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30015)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 166.424 108.76)
        (xy 166.824 108.76)
        (xy 167.62 107.76)
        (xy 166.62 106.759)
        (xy 165.621999 107.76)
      )
    )
  )
  (zone (net 2) (net_name "/-sin_var_freq") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30084)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 164.35 105.01)
        (xy 164.35 104.61)
        (xy 163.541342 104.34806)
        (xy 163.349 104.81)
        (xy 163.541342 105.27194)
      )
    )
  )
  (zone (net 4) (net_name "GND") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30120)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 135.583625 100.679099)
        (xy 135.583625 101.179099)
        (xy 136.168544 101.374002)
        (xy 136.534625 100.879099)
        (xy 136.118733 100.425308)
      )
    )
  )
  (zone (net 33) (net_name "Net-(D2-A)") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30223)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 141.063582 87.5712)
        (xy 141.063582 87.9712)
        (xy 141.456179 88.059782)
        (xy 141.714582 87.7712)
        (xy 141.456179 87.482618)
      )
    )
  )
  (zone (net 38) (net_name "/X, mixer out") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30013)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 126 102)
        (xy 126 101.6)
        (xy 125 100.8)
        (xy 123.999 101.8)
        (xy 125 102.8)
      )
    )
  )
  (zone (net 28) (net_name "/+sin_var_freq") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30042)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 180.328526 100.373683)
        (xy 180.045683 100.656526)
        (xy 180.507783 101.690275)
        (xy 181.112707 101.440707)
        (xy 181.362275 100.835783)
      )
    )
  )
  (zone (net 8) (net_name "Net-(U1B-+)") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30177)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 137.080892 98.342353)
        (xy 137.363735 98.05951)
        (xy 137.162182 96.970857)
        (xy 136.861475 97.013093)
        (xy 136.844336 97.9888)
      )
    )
  )
  (zone (net 28) (net_name "/+sin_var_freq") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30062)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 163.443017 97.1022)
        (xy 163.160174 96.819357)
        (xy 162.371024 97.219599)
        (xy 162.554568 97.707806)
        (xy 163.030275 97.903851)
      )
    )
  )
  (zone (net 5) (net_name "VSS") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30202)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 157.040275 90.847099)
        (xy 156.640275 90.847099)
        (xy 156.551693 91.239696)
        (xy 156.840275 92.123099)
        (xy 157.128857 91.239696)
      )
    )
  )
  (zone (net 19) (net_name "Net-(SW1B-B)") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30041)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 177.510328 86.948119)
        (xy 177.863881 87.301672)
        (xy 178.862275 86.804217)
        (xy 178.612707 86.199293)
        (xy 178.007783 85.949725)
      )
    )
  )
  (zone (net 23) (net_name "Net-(U1B--)") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30181)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 130.489014 94.063254)
        (xy 130.767522 93.776144)
        (xy 130.093406 93.38188)
        (xy 129.722165 93.818303)
        (xy 130.063769 94.27592)
      )
    )
  )
  (zone (net 3) (net_name "Net-(U2A-+)") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30101)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 155.820275 98.399399)
        (xy 155.320275 98.399399)
        (xy 155.029967 98.993753)
        (xy 155.468675 99.362899)
        (xy 155.943675 99.111899)
      )
    )
  )
  (zone (net 11) (net_name "Net-(U1D--)") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30118)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 132.802182 89.0118)
        (xy 133.302182 89.0118)
        (xy 133.558877 88.407585)
        (xy 133.101082 88.0608)
        (xy 132.631661 88.390187)
      )
    )
  )
  (zone (net 27) (net_name "/sin_fixed_freq") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30025)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 140.848182 105.858618)
        (xy 141.248182 105.858618)
        (xy 140.065 104.849743)
        (xy 139.065 105.8408)
        (xy 140.065 106.8418)
      )
    )
  )
  (zone (net 5) (net_name "VSS") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30026)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 171.616718 83.88973)
        (xy 171.97027 84.243282)
        (xy 172.989228 83.296)
        (xy 172.187307 82.295293)
        (xy 171.1866 83.296)
      )
    )
  )
  (zone (net 2) (net_name "/-sin_var_freq") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30129)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 162.169675 88.48)
        (xy 162.169675 88.08)
        (xy 161.548062 87.852178)
        (xy 161.156175 88.309099)
        (xy 161.548062 88.76602)
      )
    )
  )
  (zone (net 9) (net_name "/cos_var_freq") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30208)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 151.81 131.1)
        (xy 151.81 131.5)
        (xy 152.456927 131.669552)
        (xy 152.611 131.3)
        (xy 152.456927 130.930448)
      )
    )
  )
  (zone (net 4) (net_name "GND") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30110)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 134.052982 84.788403)
        (xy 134.052982 84.288403)
        (xy 133.431369 84.089079)
        (xy 133.101982 84.5585)
        (xy 133.43334 85.026603)
      )
    )
  )
  (zone (net 4) (net_name "GND") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30069)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 168.8044 98.6696)
        (xy 168.3044 98.6696)
        (xy 168.09246 99.478258)
        (xy 168.5544 99.6706)
        (xy 169.01634 99.478258)
      )
    )
  )
  (zone (net 27) (net_name "/sin_fixed_freq") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30178)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 142.075816 97.532808)
        (xy 141.792974 97.249966)
        (xy 141.357812 97.030678)
        (xy 141.028718 97.500806)
        (xy 141.412656 97.932874)
      )
    )
  )
  (zone (net 5) (net_name "VSS") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30128)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 156.640275 90.996899)
        (xy 157.040275 90.996899)
        (xy 157.297196 90.375286)
        (xy 156.840275 89.983399)
        (xy 156.383354 90.375286)
      )
    )
  )
  (zone (net 17) (net_name "Net-(SW1A-B)") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30039)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 178.362 92.908)
        (xy 178.862 92.908)
        (xy 179.216217 91.850275)
        (xy 178.612 91.599)
        (xy 178.007783 91.850275)
      )
    )
  )
  (zone (net 2) (net_name "/-sin_var_freq") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30044)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 152.405259 103.02707)
        (xy 152.682505 102.738742)
        (xy 152.199275 101.70747)
        (xy 151.611055 101.950106)
        (xy 151.505906 102.675799)
      )
    )
  )
  (zone (net 40) (net_name "/Y, mixer out") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30214)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 155.376076 93.248622)
        (xy 155.762446 93.352148)
        (xy 155.858857 93.004502)
        (xy 155.570533 92.121134)
        (xy 155.281693 93.004502)
      )
    )
  )
  (zone (net 10) (net_name "Net-(U2B-+)") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30047)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 152.361575 95.579999)
        (xy 152.361575 95.179999)
        (xy 151.619746 94.811529)
        (xy 151.048075 95.379999)
        (xy 151.619746 95.948469)
      )
    )
  )
  (zone (net 12) (net_name "VDD") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30076)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 164.6642 101.223848)
        (xy 164.1642 101.223848)
        (xy 163.95903 102.031159)
        (xy 164.42097 102.223501)
        (xy 164.88291 102.031159)
      )
    )
  )
  (zone (net 7) (net_name "/cos_fixed_freq") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30166)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 127.646825 94.768999)
        (xy 128.046825 94.768999)
        (xy 128.354884 94.165972)
        (xy 127.897882 93.817999)
        (xy 127.428461 94.147386)
      )
    )
  )
  (zone (net 6) (net_name "Net-(U2C--)") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30137)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 159.180275 87.684299)
        (xy 159.580275 87.684299)
        (xy 159.851596 87.062686)
        (xy 159.382175 86.733299)
        (xy 158.912754 87.062686)
      )
    )
  )
  (zone (net 38) (net_name "/X, mixer out") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30212)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 134.113955 93.198104)
        (xy 134.460359 93.398112)
        (xy 134.596801 92.967099)
        (xy 134.322682 92.062934)
        (xy 134.0336 92.946203)
      )
    )
  )
  (zone (net 12) (net_name "VDD") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30054)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 158.492 101.255136)
        (xy 157.992 101.255136)
        (xy 157.868367 102.23)
        (xy 158.368367 102.231)
        (xy 158.830307 102.038658)
      )
    )
  )
  (zone (net 30) (net_name "/Channel 2, Y") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30021)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 163.261324 81.6134)
        (xy 163.261324 82.0134)
        (xy 164.392893 83.030707)
        (xy 165.101 82.3236)
        (xy 165.1 81.3236)
      )
    )
  )
  (zone (net 28) (net_name "/+sin_var_freq") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30155)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 162.355275 98.669599)
        (xy 162.755275 98.669599)
        (xy 163.012196 98.047986)
        (xy 162.555275 97.706099)
        (xy 162.098354 98.047986)
      )
    )
  )
  (zone (net 36) (net_name "Net-(C16-Pad2)") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30107)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 152.260482 89.2404)
        (xy 152.760482 89.2404)
        (xy 152.979903 88.618787)
        (xy 152.510482 88.2894)
        (xy 152.041061 88.618787)
      )
    )
  )
  (zone (net 16) (net_name "Net-(BT1-+)") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30037)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 169.323308 101.795845)
        (xy 169.131972 102.257786)
        (xy 169.6324 103.114645)
        (xy 170.333323 102.905182)
        (xy 170.54216 102.3048)
      )
    )
  )
  (zone (net 5) (net_name "VSS") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30058)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 156.215349 89.07663)
        (xy 155.932506 89.359473)
        (xy 156.365275 90.181151)
        (xy 156.840982 89.985106)
        (xy 156.974527 89.446899)
      )
    )
  )
  (zone (net 2) (net_name "/-sin_var_freq") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30229)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 163.810275 87.933199)
        (xy 163.810275 88.333199)
        (xy 164.202872 88.421781)
        (xy 164.461275 88.133199)
        (xy 164.202872 87.844617)
      )
    )
  )
  (zone (net 27) (net_name "/sin_fixed_freq") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30103)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 143.108225 92.589599)
        (xy 142.608225 92.589599)
        (xy 142.398954 93.211212)
        (xy 142.868375 93.540599)
        (xy 143.337796 93.211212)
      )
    )
  )
  (zone (net 13) (net_name "Net-(U2D--)") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30194)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 154.511182 90.847099)
        (xy 154.011182 90.847099)
        (xy 154.000275 91.297099)
        (xy 154.300275 92.123099)
        (xy 154.572605 91.215374)
      )
    )
  )
  (zone (net 36) (net_name "Net-(C16-Pad2)") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30106)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 152.758582 87.3404)
        (xy 152.258582 87.3404)
        (xy 152.041061 87.962013)
        (xy 152.510482 88.2914)
        (xy 152.979903 87.962013)
      )
    )
  )
  (zone (net 7) (net_name "/cos_fixed_freq") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30235)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 131.182182 96.795899)
        (xy 131.182182 97.195899)
        (xy 131.482182 97.304967)
        (xy 131.783182 97.0138)
        (xy 131.482182 96.704701)
      )
    )
  )
  (zone (net 9) (net_name "/cos_var_freq") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30099)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 148.267 99.270387)
        (xy 148.555336 99.547625)
        (xy 149.277505 99.214399)
        (xy 149.093968 98.726179)
        (xy 148.618275 98.530126)
      )
    )
  )
  (zone (net 35) (net_name "Net-(C15-Pad2)") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30183)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 132.032182 90.7888)
        (xy 131.532182 90.7888)
        (xy 131.482182 91.2388)
        (xy 131.782182 92.0648)
        (xy 132.082181 91.2388)
      )
    )
  )
  (zone (net 12) (net_name "VDD") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30078)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 155.256445 107.2428)
        (xy 155.256445 107.7428)
        (xy 156.060051 107.92934)
        (xy 156.252393 107.4674)
        (xy 156.060051 107.00546)
      )
    )
  )
  (zone (net 7) (net_name "/cos_fixed_freq") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30144)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 131.159025 97.195899)
        (xy 131.159025 96.795899)
        (xy 130.537412 96.526478)
        (xy 130.208025 96.995899)
        (xy 130.537412 97.46532)
      )
    )
  )
  (zone (net 2) (net_name "/-sin_var_freq") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30185)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 161.971552 90.187611)
        (xy 162.254393 89.90477)
        (xy 161.601556 89.488121)
        (xy 161.206468 89.908592)
        (xy 161.548062 90.36622)
      )
    )
  )
  (zone (net 36) (net_name "Net-(C16-Pad2)") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30119)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 152.760482 88.9406)
        (xy 152.260482 88.9406)
        (xy 152.081492 89.539716)
        (xy 152.585882 89.8916)
        (xy 153.028823 89.46846)
      )
    )
  )
  (zone (net 22) (net_name "Net-(R3-Pad2)") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30205)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 155.274443 102.004102)
        (xy 155.666757 101.926074)
        (xy 155.925596 101.527786)
        (xy 155.46848 101.185919)
        (xy 155.011754 101.527786)
      )
    )
  )
  (zone (net 17) (net_name "Net-(SW1A-B)") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30004)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 179.750069 96.41)
        (xy 179.750069 96.91)
        (xy 181.913376 96.1992)
        (xy 181.5602 95.1992)
        (xy 180.5592 94.722002)
      )
    )
  )
  (zone (net 3) (net_name "Net-(U2A-+)") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30182)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 155.320275 98.347099)
        (xy 155.820275 98.347099)
        (xy 155.870275 97.897099)
        (xy 155.570275 97.071099)
        (xy 155.270275 97.897099)
      )
    )
  )
  (zone (net 29) (net_name "/Channel 1, X") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30018)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 140.0016 80.343809)
        (xy 139.6016 80.343809)
        (xy 138.77612 81.940917)
        (xy 139.7 82.3246)
        (xy 140.62388 81.940917)
      )
    )
  )
  (zone (net 12) (net_name "VDD") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30126)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 167.7772 96.7203)
        (xy 167.7772 96.2203)
        (xy 167.222069 95.9953)
        (xy 166.8262 96.4703)
        (xy 167.222069 96.9453)
      )
    )
  )
  (zone (net 35) (net_name "Net-(C15-Pad2)") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30105)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 131.026082 89.0118)
        (xy 131.526082 89.0118)
        (xy 131.745503 88.390187)
        (xy 131.276082 88.0608)
        (xy 130.806661 88.390187)
      )
    )
  )
  (zone (net 35) (net_name "Net-(C15-Pad2)") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30117)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 131.049582 87.3206)
        (xy 131.549582 87.3206)
        (xy 131.756503 86.698987)
        (xy 131.299582 86.3571)
        (xy 130.842661 86.698987)
      )
    )
  )
  (zone (net 4) (net_name "GND") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30135)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 139.860682 100.1878)
        (xy 140.260682 100.1878)
        (xy 140.530103 99.566187)
        (xy 140.060682 99.2368)
        (xy 139.591261 99.566187)
      )
    )
  )
  (zone (net 4) (net_name "GND") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30071)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 167.5424 82.2292)
        (xy 168.0424 82.2292)
        (xy 168.25434 81.420542)
        (xy 167.7924 81.2282)
        (xy 167.33046 81.420542)
      )
    )
  )
  (zone (net 30) (net_name "/Channel 2, Y") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30160)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 152.708582 83.9008)
        (xy 152.308582 83.9008)
        (xy 152.051661 84.522413)
        (xy 152.508582 84.8643)
        (xy 152.965503 84.522413)
      )
    )
  )
  (zone (net 4) (net_name "GND") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30197)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 158.310275 90.847099)
        (xy 157.910275 90.847099)
        (xy 157.821693 91.239696)
        (xy 158.110275 92.123099)
        (xy 158.398857 91.239696)
      )
    )
  )
  (zone (net 5) (net_name "VSS") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30170)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 167.567529 85.220637)
        (xy 167.937081 85.373705)
        (xy 168.249321 84.718887)
        (xy 167.792782 84.327077)
        (xy 167.335479 84.718887)
      )
    )
  )
  (zone (net 15) (net_name "Net-(D4-K)") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30161)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 162.169675 86.934299)
        (xy 162.169675 86.534299)
        (xy 161.548062 86.277378)
        (xy 161.206175 86.734299)
        (xy 161.548062 87.19122)
      )
    )
  )
  (zone (net 4) (net_name "GND") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30210)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 157.318875 101.594099)
        (xy 156.818875 101.594099)
        (xy 156.606935 102.058658)
        (xy 157.068875 102.251)
        (xy 157.530815 102.058658)
      )
    )
  )
  (zone (net 5) (net_name "VSS") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30192)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 135.818425 90.7888)
        (xy 135.318425 90.7888)
        (xy 135.292182 91.2388)
        (xy 135.592182 92.0648)
        (xy 135.875643 91.173734)
      )
    )
  )
  (zone (net 15) (net_name "Net-(D4-K)") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30227)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 163.810275 86.533199)
        (xy 163.810275 86.933199)
        (xy 164.202872 87.021781)
        (xy 164.461275 86.733199)
        (xy 164.202872 86.444617)
      )
    )
  )
  (zone (net 4) (net_name "GND") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30089)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 156.818875 102.149399)
        (xy 157.318875 102.149399)
        (xy 157.500396 101.527786)
        (xy 157.043475 101.135899)
        (xy 156.586554 101.527786)
      )
    )
  )
  (zone (net 7) (net_name "/cos_fixed_freq") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30138)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 129.259025 96.795899)
        (xy 129.259025 97.195899)
        (xy 129.880638 97.46532)
        (xy 130.210025 96.995899)
        (xy 129.880638 96.526478)
      )
    )
  )
  (zone (net 4) (net_name "GND") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30193)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 137.088425 90.7888)
        (xy 136.588425 90.7888)
        (xy 136.562182 91.2388)
        (xy 136.862182 92.0648)
        (xy 137.145643 91.173734)
      )
    )
  )
  (zone (net 5) (net_name "VSS") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30068)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 154.626182 83.4858)
        (xy 154.626182 82.9858)
        (xy 153.817524 82.77386)
        (xy 153.625182 83.2358)
        (xy 153.817524 83.69774)
      )
    )
  )
  (zone (net 16) (net_name "Net-(BT1-+)") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30007)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 170.3538 103.156)
        (xy 169.8538 103.156)
        (xy 169.1038 104.156)
        (xy 170.1038 105.157)
        (xy 171.1038 104.156)
      )
    )
  )
  (zone (net 4) (net_name "GND") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30070)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 133.3914 84.288403)
        (xy 133.3914 84.788403)
        (xy 134.200058 85.000343)
        (xy 134.3924 84.538403)
        (xy 134.200058 84.076463)
      )
    )
  )
  (zone (net 23) (net_name "Net-(U1B--)") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30198)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 138.332182 95.7388)
        (xy 137.932182 95.7388)
        (xy 137.8436 96.131397)
        (xy 138.132182 97.0148)
        (xy 138.420764 96.131397)
      )
    )
  )
  (zone (net 8) (net_name "Net-(U1B-+)") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30211)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 136.970974 95.672395)
        (xy 136.624565 95.872395)
        (xy 136.562182 96.1888)
        (xy 136.862682 97.014666)
        (xy 137.114255 96.080066)
      )
    )
  )
  (zone (net 12) (net_name "VDD") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30133)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 166.951 95.4578)
        (xy 166.551 95.4578)
        (xy 166.370279 96.079413)
        (xy 166.8272 96.4713)
        (xy 167.272802 96.062474)
      )
    )
  )
  (zone (net 12) (net_name "VDD") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30003)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 174.381112 96.476521)
        (xy 174.631108 96.909535)
        (xy 176.555328 96.1)
        (xy 176.150866 95.099501)
        (xy 175.15 94.676829)
      )
    )
  )
  (zone (net 6) (net_name "Net-(U2C--)") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30201)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 159.580275 90.847099)
        (xy 159.180275 90.847099)
        (xy 159.091693 91.239696)
        (xy 159.380275 92.123099)
        (xy 159.668857 91.239696)
      )
    )
  )
  (zone (net 24) (net_name "Net-(U2B--)") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30061)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 150.006417 94.7203)
        (xy 149.723574 94.437457)
        (xy 148.934424 94.837699)
        (xy 149.117968 95.325906)
        (xy 149.593675 95.521951)
      )
    )
  )
  (zone (net 33) (net_name "Net-(D2-A)") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30086)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 139.0302 103.051)
        (xy 139.0302 103.451)
        (xy 139.838858 103.71294)
        (xy 140.0312 103.251)
        (xy 139.838858 102.78906)
      )
    )
  )
  (zone (net 9) (net_name "/cos_var_freq") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30022)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 148.318275 101.378)
        (xy 147.918275 101.378)
        (xy 147.495382 102.378)
        (xy 148.495382 103.379)
        (xy 149.324338 102.378)
      )
    )
  )
  (zone (net 30) (net_name "/Channel 2, Y") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30016)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 164.4 79.7162)
        (xy 164.4 79.3162)
        (xy 163.4 78.5274)
        (xy 162.399 79.5274)
        (xy 163.399999 80.521812)
      )
    )
  )
  (zone (net 33) (net_name "Net-(D2-A)") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30147)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 139.735325 88.977799)
        (xy 140.135325 88.977799)
        (xy 140.364314 88.378682)
        (xy 139.859925 88.026799)
        (xy 139.416983 88.449938)
      )
    )
  )
  (zone (net 4) (net_name "GND") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30102)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 155.211182 85.1387)
        (xy 155.211182 84.6387)
        (xy 154.589569 84.419279)
        (xy 154.260182 84.8887)
        (xy 154.589569 85.358121)
      )
    )
  )
  (zone (net 9) (net_name "/cos_var_freq") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30148)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 148.918675 98.112699)
        (xy 149.318675 98.112699)
        (xy 149.575596 97.491086)
        (xy 149.118675 97.149199)
        (xy 148.661754 97.491086)
      )
    )
  )
  (zone (net 6) (net_name "Net-(U2C--)") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30146)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 161.610211 94.052481)
        (xy 161.557995 94.449057)
        (xy 162.201488 94.72212)
        (xy 162.530866 94.252829)
        (xy 162.201488 93.783278)
      )
    )
  )
  (zone (net 35) (net_name "Net-(C15-Pad2)") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30111)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 131.549582 87.1118)
        (xy 131.049582 87.1118)
        (xy 130.809169 87.729659)
        (xy 131.276082 88.0628)
        (xy 131.745503 87.733413)
      )
    )
  )
  (zone (net 25) (net_name "Net-(R9-Pad2)") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30150)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 159.180275 102.149399)
        (xy 159.580275 102.149399)
        (xy 159.837196 101.527786)
        (xy 159.380275 101.185899)
        (xy 158.923354 101.527786)
      )
    )
  )
  (zone (net 12) (net_name "VDD") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30053)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 157.633046 100.355023)
        (xy 157.986599 100.00147)
        (xy 157.518475 99.215147)
        (xy 157.042768 99.411192)
        (xy 156.909224 99.949399)
      )
    )
  )
  (zone (net 11) (net_name "Net-(U1D--)") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30108)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 133.352982 87.1118)
        (xy 132.852982 87.1118)
        (xy 132.631661 87.733413)
        (xy 133.101082 88.0628)
        (xy 133.570503 87.733413)
      )
    )
  )
  (zone (net 33) (net_name "Net-(D2-A)") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30055)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 133.967559 101.814602)
        (xy 134.250402 101.531759)
        (xy 133.833625 100.693349)
        (xy 133.357918 100.882192)
        (xy 133.213941 101.420399)
      )
    )
  )
  (zone (net 4) (net_name "GND") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30088)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 140.260682 99.564663)
        (xy 139.860682 99.564663)
        (xy 139.56826 100.367258)
        (xy 140.0302 100.5596)
        (xy 140.49214 100.367258)
      )
    )
  )
  (zone (net 5) (net_name "VSS") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30122)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 168.57 84.078)
        (xy 168.57 84.578)
        (xy 169.110394 84.821101)
        (xy 169.521 84.3594)
        (xy 169.14414 83.871698)
      )
    )
  )
  (zone (net 18) (net_name "Net-(BT2--)") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30050)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 168.969763 89.965196)
        (xy 169.385499 89.687416)
        (xy 169.713331 89.146027)
        (xy 169.061845 88.654569)
        (xy 168.516391 89.236144)
      )
    )
  )
  (zone (net 4) (net_name "GND") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30077)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 136.783625 101.255136)
        (xy 136.283625 101.255136)
        (xy 136.08846 102.060457)
        (xy 136.5504 102.252799)
        (xy 137.01234 102.060457)
      )
    )
  )
  (zone (net 20) (net_name "Net-(U1A--)") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30190)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 131.049093 99.305999)
        (xy 131.049093 98.905999)
        (xy 130.661248 98.472981)
        (xy 130.208025 98.820899)
        (xy 130.446525 99.308399)
      )
    )
  )
  (zone (net 2) (net_name "/-sin_var_freq") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30236)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 162.174298 88.062861)
        (xy 162.457139 88.345702)
        (xy 162.678872 88.421781)
        (xy 162.936982 88.132492)
        (xy 162.650454 87.863605)
      )
    )
  )
  (zone (net 1) (net_name "Net-(U1A-+)") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30109)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 134.499414 98.324602)
        (xy 134.099462 98.330768)
        (xy 134.458425 99.274211)
        (xy 134.93344 99.105098)
        (xy 135.147987 98.616599)
      )
    )
  )
  (zone (net 36) (net_name "Net-(C16-Pad2)") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30081)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 152.766582 90.799446)
        (xy 153.266582 90.799446)
        (xy 153.123382 89.91488)
        (xy 152.585882 89.8896)
        (xy 152.285655 90.365555)
      )
    )
  )
  (zone (net 8) (net_name "Net-(U1B-+)") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30066)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 137.644871 98.340646)
        (xy 137.362028 98.623489)
        (xy 137.748182 99.417252)
        (xy 138.236389 99.238507)
        (xy 138.43686 98.7628)
      )
    )
  )
  (zone (net 5) (net_name "VSS") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30040)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 180.363881 85.098328)
        (xy 180.010328 85.451881)
        (xy 180.507783 86.450275)
        (xy 181.112707 86.200707)
        (xy 181.362275 85.595783)
      )
    )
  )
  (zone (net 5) (net_name "VSS") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30124)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 170.47 84.6094)
        (xy 170.47 84.1094)
        (xy 169.914869 83.8844)
        (xy 169.519 84.3594)
        (xy 169.914869 84.8344)
      )
    )
  )
  (zone (net 14) (net_name "Net-(U1C--)") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30165)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 141.192575 92.589599)
        (xy 140.792575 92.589599)
        (xy 140.573954 93.211212)
        (xy 141.043375 93.540599)
        (xy 141.500472 93.192767)
      )
    )
  )
  (zone (net 1) (net_name "Net-(U1A-+)") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30167)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 133.983425 98.957899)
        (xy 133.983425 99.357899)
        (xy 134.605038 99.57352)
        (xy 134.934425 99.104099)
        (xy 134.584934 98.64811)
      )
    )
  )
  (zone (net 5) (net_name "VSS") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30164)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 134.760311 89.629591)
        (xy 134.510317 90.062605)
        (xy 135.157875 90.341187)
        (xy 135.569291 89.881398)
        (xy 135.194516 89.391894)
      )
    )
  )
  (zone (net 33) (net_name "Net-(D2-A)") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30142)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 132.733825 101.130999)
        (xy 132.733825 100.730999)
        (xy 132.112212 100.461578)
        (xy 131.782825 100.930999)
        (xy 132.112212 101.40042)
      )
    )
  )
  (zone (net 14) (net_name "Net-(U1C--)") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30145)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 140.792575 92.863999)
        (xy 141.192575 92.863999)
        (xy 141.461996 92.242386)
        (xy 140.992575 91.912999)
        (xy 140.523154 92.242386)
      )
    )
  )
  (zone (net 21) (net_name "Net-(U2A--)") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30064)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 149.981017 99.947)
        (xy 149.698174 99.664157)
        (xy 148.909024 100.064399)
        (xy 149.092568 100.552606)
        (xy 149.568275 100.74865)
      )
    )
  )
  (zone (net 5) (net_name "VSS") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30010)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 174.1866 82.546)
        (xy 174.1866 82.046)
        (xy 173.1866 81.296)
        (xy 172.1856 82.296)
        (xy 173.1866 83.296)
      )
    )
  )
  (zone (net 33) (net_name "Net-(D2-A)") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30179)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 139.680272 90.44031)
        (xy 139.963114 90.723152)
        (xy 140.365804 90.065467)
        (xy 139.936032 89.678092)
        (xy 139.465904 90.007186)
      )
    )
  )
  (zone (net 12) (net_name "VDD") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30156)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 166.551 94.5088)
        (xy 166.951 94.5088)
        (xy 167.182521 93.887187)
        (xy 166.7256 93.5453)
        (xy 166.268679 93.887187)
      )
    )
  )
  (zone (net 37) (net_name "/+{slash}- sin var freq") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30045)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 177.619813 102.209922)
        (xy 177.966225 102.409918)
        (xy 178.862275 102.044217)
        (xy 178.612499 101.439134)
        (xy 178.007783 101.189725)
      )
    )
  )
  (zone (net 38) (net_name "/X, mixer out") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30032)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 135.16334 125.656497)
        (xy 134.880497 125.93934)
        (xy 135.438702 127.325281)
        (xy 136.224707 127.000707)
        (xy 136.549281 126.214702)
      )
    )
  )
  (zone (net 7) (net_name "/cos_fixed_freq") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30031)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 145.16334 125.656497)
        (xy 144.880497 125.93934)
        (xy 145.438702 127.325281)
        (xy 146.224707 127.000707)
        (xy 146.549281 126.214702)
      )
    )
  )
  (zone (net 9) (net_name "/cos_var_freq") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30237)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 152.495029 96.880283)
        (xy 152.598552 97.266653)
        (xy 152.730275 97.372853)
        (xy 153.03124 97.071841)
        (xy 152.730275 96.77285)
      )
    )
  )
  (zone (net 36) (net_name "Net-(C16-Pad2)") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30189)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 153.266582 90.847099)
        (xy 152.766582 90.847099)
        (xy 152.730275 91.297099)
        (xy 153.030275 92.123099)
        (xy 153.320924 91.250088)
      )
    )
  )
  (zone (net 6) (net_name "Net-(U2C--)") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30152)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 162.755275 94.919599)
        (xy 162.355275 94.919599)
        (xy 162.098354 95.541212)
        (xy 162.555275 95.883099)
        (xy 163.012196 95.541212)
      )
    )
  )
  (zone (net 4) (net_name "GND") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30001)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 140.759997 75.227964)
        (xy 141.039318 75.514283)
        (xy 142.459822 75.914173)
        (xy 143.500715 74.522902)
        (xy 141.827161 74.016829)
      )
    )
  )
  (zone (net 9) (net_name "/cos_var_freq") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30191)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 149.812651 97.568294)
        (xy 150.095494 97.285451)
        (xy 149.568335 96.798445)
        (xy 149.117968 97.149492)
        (xy 149.356175 97.637699)
      )
    )
  )
  (zone (net 33) (net_name "Net-(D2-A)") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30218)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 142.363582 87.9712)
        (xy 142.363582 87.5712)
        (xy 141.970985 87.482618)
        (xy 141.712582 87.7712)
        (xy 141.970985 88.059782)
      )
    )
  )
  (zone (net 4) (net_name "GND") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30094)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 168.0424 81.5905)
        (xy 167.5424 81.5905)
        (xy 167.335479 82.212113)
        (xy 167.7924 82.604)
        (xy 168.249321 82.212113)
      )
    )
  )
  (zone (net 27) (net_name "/sin_fixed_freq") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30154)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 140.848182 98.462599)
        (xy 141.248182 98.462599)
        (xy 141.486346 97.840986)
        (xy 141.029425 97.499099)
        (xy 140.572504 97.840986)
      )
    )
  )
  (zone (net 15) (net_name "Net-(D4-K)") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30226)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 163.586275 86.933199)
        (xy 163.586275 86.533199)
        (xy 163.193678 86.444617)
        (xy 162.935275 86.733199)
        (xy 163.193678 87.021781)
      )
    )
  )
  (zone (net 35) (net_name "Net-(C15-Pad2)") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30082)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 131.532182 90.658457)
        (xy 132.032182 90.658457)
        (xy 131.863582 89.771403)
        (xy 131.326082 89.7626)
        (xy 131.035406 90.2386)
      )
    )
  )
  (zone (net 34) (net_name "Net-(D2-K)") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30222)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 142.587582 86.1712)
        (xy 142.587582 86.5712)
        (xy 142.980179 86.659782)
        (xy 143.238582 86.3712)
        (xy 142.980179 86.082618)
      )
    )
  )
  (zone (net 27) (net_name "/sin_fixed_freq") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30113)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 142.608225 92.863999)
        (xy 143.108225 92.863999)
        (xy 143.286996 92.242386)
        (xy 142.817575 91.912999)
        (xy 142.356771 92.255283)
      )
    )
  )
  (zone (net 6) (net_name "Net-(U2C--)") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30180)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 159.727383 93.376289)
        (xy 160.010226 93.093446)
        (xy 159.680275 92.060002)
        (xy 159.379568 92.121392)
        (xy 159.480592 93.097099)
      )
    )
  )
  (zone (net 33) (net_name "Net-(D2-A)") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30159)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 140.897825 89.878799)
        (xy 140.897825 89.478799)
        (xy 140.276212 89.221878)
        (xy 139.934325 89.678799)
        (xy 140.276212 90.13572)
      )
    )
  )
  (zone (net 12) (net_name "VDD") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30052)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 137.123196 100.097223)
        (xy 137.476749 99.74367)
        (xy 137.008625 98.957347)
        (xy 136.532918 99.153392)
        (xy 136.399374 99.691599)
      )
    )
  )
  (zone (net 25) (net_name "Net-(R9-Pad2)") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30027)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 168.6 125.1)
        (xy 168.2 125.1)
        (xy 167.614702 126.474719)
        (xy 168.4 126.801)
        (xy 169.185298 126.474719)
      )
    )
  )
  (zone (net 6) (net_name "Net-(U2C--)") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30149)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 162.355275 95.215199)
        (xy 162.755275 95.215199)
        (xy 162.986796 94.593586)
        (xy 162.529875 94.251699)
        (xy 162.072954 94.593586)
      )
    )
  )
  (zone (net 19) (net_name "Net-(SW1B-B)") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30036)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 169.876718 87.823271)
        (xy 170.230271 87.469718)
        (xy 169.7624 86.506872)
        (xy 169.061693 86.654693)
        (xy 168.813872 87.2554)
      )
    )
  )
  (zone (net 4) (net_name "GND") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30093)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 136.283625 101.891599)
        (xy 136.783625 101.891599)
        (xy 136.990546 101.269986)
        (xy 136.533625 100.878099)
        (xy 136.076704 101.269986)
      )
    )
  )
  (zone (net 4) (net_name "GND") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30131)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 157.091075 87.246899)
        (xy 156.691075 87.246899)
        (xy 156.3844 87.866946)
        (xy 156.840275 88.260399)
        (xy 157.297196 87.868512)
      )
    )
  )
  (zone (net 9) (net_name "/cos_var_freq") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30196)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 148.962329 108.905172)
        (xy 149.245172 108.622329)
        (xy 148.979552 107.996927)
        (xy 148.609293 108.149293)
        (xy 148.327157 108.432843)
      )
    )
  )
  (zone (net 4) (net_name "GND") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30095)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 168.3044 99.1824)
        (xy 168.8044 99.1824)
        (xy 169.011321 98.560787)
        (xy 168.5544 98.1689)
        (xy 168.097479 98.560787)
      )
    )
  )
  (zone (net 5) (net_name "VSS") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30092)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 135.318425 90.893399)
        (xy 135.818425 90.893399)
        (xy 136.025346 90.271786)
        (xy 135.568425 89.879899)
        (xy 135.111504 90.271786)
      )
    )
  )
  (zone (net 28) (net_name "/+sin_var_freq") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30176)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 162.412154 99.430361)
        (xy 162.129313 99.14752)
        (xy 161.689862 98.917878)
        (xy 161.360768 99.388006)
        (xy 161.737662 99.824781)
      )
    )
  )
  (zone (net 15) (net_name "Net-(D4-K)") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30225)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 162.286275 86.534299)
        (xy 162.286275 86.934299)
        (xy 162.678872 87.021781)
        (xy 162.937275 86.733199)
        (xy 162.678872 86.444617)
      )
    )
  )
  (zone (net 2) (net_name "/-sin_var_freq") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30162)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 161.007175 89.259099)
        (xy 161.407175 89.259099)
        (xy 161.652078 88.674179)
        (xy 161.157175 88.308099)
        (xy 160.703384 88.72399)
      )
    )
  )
  (zone (net 34) (net_name "Net-(D2-K)") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30220)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 141.063582 86.176799)
        (xy 141.063582 86.576799)
        (xy 141.456179 86.659782)
        (xy 141.714582 86.3712)
        (xy 141.456179 86.082618)
      )
    )
  )
  (zone (net 13) (net_name "Net-(U2D--)") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30114)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 154.011182 87.6762)
        (xy 154.511182 87.6762)
        (xy 154.718103 87.054587)
        (xy 154.261182 86.7127)
        (xy 153.804261 87.054587)
      )
    )
  )
  (zone (net 40) (net_name "/Y, mixer out") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30023)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 143.0864 105.6164)
        (xy 143.0864 106.0164)
        (xy 143.9324 106.8164)
        (xy 144.9334 105.8164)
        (xy 143.9324 104.8164)
      )
    )
  )
  (zone (net 30) (net_name "/Channel 2, Y") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30230)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 164.8746 80.1162)
        (xy 165.2746 80.1162)
        (xy 165.3746 79.776319)
        (xy 165.0746 79.5152)
        (xy 164.7746 79.776319)
      )
    )
  )
  (zone (net 23) (net_name "Net-(U1B--)") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30097)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 140.485842 94.848729)
        (xy 140.208596 95.137057)
        (xy 140.554425 95.871828)
        (xy 141.030145 95.675792)
        (xy 141.213697 95.187599)
      )
    )
  )
  (zone (net 27) (net_name "/sin_fixed_freq") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30136)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 142.668375 94.489599)
        (xy 143.068375 94.489599)
        (xy 143.337796 93.867986)
        (xy 142.868375 93.538599)
        (xy 142.398954 93.867986)
      )
    )
  )
  (zone (net 40) (net_name "/Y, mixer out") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30030)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 143.28466 128.343503)
        (xy 143.567503 128.06066)
        (xy 143.009298 126.674719)
        (xy 142.223293 126.999293)
        (xy 141.898719 127.785298)
      )
    )
  )
  (zone (net 28) (net_name "/+sin_var_freq") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30186)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 160.924687 98.342408)
        (xy 161.212477 98.064604)
        (xy 160.950275 97.019519)
        (xy 160.649581 97.07138)
        (xy 160.690809 98.047099)
      )
    )
  )
  (zone (net 5) (net_name "VSS") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30188)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 166.9256 87.2375)
        (xy 166.5256 87.2375)
        (xy 166.2881 87.778835)
        (xy 166.7256 88.1135)
        (xy 167.1631 87.778835)
      )
    )
  )
  (zone (net 4) (net_name "GND") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30073)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 135.341173 87.805947)
        (xy 135.841173 87.805947)
        (xy 136.053113 86.997289)
        (xy 135.591173 86.804947)
        (xy 135.129233 86.997289)
      )
    )
  )
  (zone (net 17) (net_name "Net-(SW1A-B)") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30049)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 171.763535 100.971388)
        (xy 171.409982 100.617835)
        (xy 170.878071 100.32383)
        (xy 170.331693 100.905507)
        (xy 170.923262 101.455574)
      )
    )
  )
  (zone (net 34) (net_name "Net-(D2-K)") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30157)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 140.923225 86.576799)
        (xy 140.923225 86.176799)
        (xy 140.301612 85.919878)
        (xy 139.959725 86.376799)
        (xy 140.301612 86.83372)
      )
    )
  )
  (zone (net 5) (net_name "VSS") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30057)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 166.884631 84.952926)
        (xy 167.167474 85.235769)
        (xy 167.926652 84.8655)
        (xy 167.793107 84.327293)
        (xy 167.3174 84.131248)
      )
    )
  )
  (zone (net 33) (net_name "Net-(D2-A)") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30100)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 142.139125 102.271817)
        (xy 141.739125 102.271817)
        (xy 141.581842 103.059658)
        (xy 142.043782 103.252)
        (xy 142.505722 103.059658)
      )
    )
  )
  (zone (net 12) (net_name "VDD") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30024)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 175.158 93.838)
        (xy 174.658 93.838)
        (xy 175.15 95.510311)
        (xy 176.15 95.101)
        (xy 176.56815 94.1)
      )
    )
  )
  (zone (net 20) (net_name "Net-(U1A--)") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30174)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 131.009104 98.882837)
        (xy 130.726263 99.165678)
        (xy 131.418444 99.550702)
        (xy 131.784532 99.106706)
        (xy 131.455438 98.636578)
      )
    )
  )
  (zone (net 11) (net_name "Net-(U1D--)") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30115)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 132.852982 87.346)
        (xy 133.352982 87.346)
        (xy 133.559903 86.724387)
        (xy 133.102982 86.3825)
        (xy 132.646061 86.724387)
      )
    )
  )
  (zone (net 9) (net_name "/cos_var_freq") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30033)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 139.28466 128.343503)
        (xy 139.567503 128.06066)
        (xy 139.009298 126.674719)
        (xy 138.223293 126.999293)
        (xy 137.898719 127.785298)
      )
    )
  )
  (zone (net 4) (net_name "GND") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30090)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 166.5772 99.2078)
        (xy 167.0772 99.2078)
        (xy 167.284121 98.586187)
        (xy 166.8272 98.1943)
        (xy 166.370279 98.586187)
      )
    )
  )
  (zone (net 2) (net_name "/-sin_var_freq") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30169)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 160.799777 104.742248)
        (xy 160.516934 104.459405)
        (xy 159.922424 104.314461)
        (xy 159.730375 104.777108)
        (xy 159.922424 105.238341)
      )
    )
  )
  (zone (net 12) (net_name "VDD") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30171)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 165.703089 96.299958)
        (xy 166.056642 96.653511)
        (xy 166.421762 96.938238)
        (xy 166.827907 96.469593)
        (xy 166.428911 95.997584)
      )
    )
  )
  (zone (net 4) (net_name "GND") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30085)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 156.691075 87.886699)
        (xy 157.091075 87.886699)
        (xy 157.353015 87.078041)
        (xy 156.891075 86.885699)
        (xy 156.429135 87.078041)
      )
    )
  )
  (zone (net 1) (net_name "Net-(U1A-+)") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30204)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 134.098449 98.265078)
        (xy 134.498401 98.258906)
        (xy 134.605275 97.904417)
        (xy 134.322167 97.012801)
        (xy 134.022182 97.8388)
      )
    )
  )
  (zone (net 29) (net_name "/Channel 1, X") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30006)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 137.7 82.0736)
        (xy 137.7 82.5736)
        (xy 139.317317 83.24748)
        (xy 139.701 82.3236)
        (xy 139.317317 81.39972)
      )
    )
  )
  (zone (net 37) (net_name "/+{slash}- sin var freq") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30034)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 141.28466 128.343503)
        (xy 141.567503 128.06066)
        (xy 141.009298 126.674719)
        (xy 140.223293 126.999293)
        (xy 139.898719 127.785298)
      )
    )
  )
  (zone (net 27) (net_name "/sin_fixed_freq") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30234)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 140.002182 97.190999)
        (xy 140.002182 96.790999)
        (xy 139.702182 96.702165)
        (xy 139.401182 97.0138)
        (xy 139.702182 97.302596)
      )
    )
  )
  (zone (net 2) (net_name "/-sin_var_freq") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30139)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 151.335475 101.046599)
        (xy 151.735475 101.046599)
        (xy 152.004896 100.424986)
        (xy 151.535475 100.095599)
        (xy 151.066054 100.424986)
      )
    )
  )
  (zone (net 14) (net_name "Net-(U1C--)") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30141)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 137.935725 87.326799)
        (xy 138.335725 87.326799)
        (xy 138.605146 86.705186)
        (xy 138.135725 86.375799)
        (xy 137.666304 86.705186)
      )
    )
  )
  (zone (net 30) (net_name "/Channel 2, Y") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30017)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 165.2746 80.328652)
        (xy 164.8746 80.328652)
        (xy 164.17612 81.940917)
        (xy 165.1 82.3246)
        (xy 166.02388 81.940917)
      )
    )
  )
  (zone (net 33) (net_name "Net-(D2-A)") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30163)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 132.408625 100.730999)
        (xy 132.408625 101.130999)
        (xy 132.992458 101.377077)
        (xy 133.359625 100.882899)
        (xy 132.944274 100.428299)
      )
    )
  )
  (zone (net 29) (net_name "/Channel 1, X") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30012)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 137.6 79.6766)
        (xy 137.6 79.2766)
        (xy 136.6 78.4766)
        (xy 135.599 79.4766)
        (xy 136.6 80.4766)
      )
    )
  )
  (zone (net 2) (net_name "/-sin_var_freq") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30083)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 156.119992 103.640785)
        (xy 155.832117 103.918503)
        (xy 155.732975 104.727653)
        (xy 156.233669 104.728372)
        (xy 156.694915 104.536311)
      )
    )
  )
  (zone (net 4) (net_name "GND") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30091)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 169.7696 81.6219)
        (xy 169.2696 81.6219)
        (xy 169.063079 82.243513)
        (xy 169.52 82.6354)
        (xy 169.976921 82.243513)
      )
    )
  )
  (zone (net 4) (net_name "GND") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30059)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 157.465201 89.167168)
        (xy 157.748044 88.884325)
        (xy 157.315275 88.062647)
        (xy 156.839568 88.258692)
        (xy 156.706024 88.796899)
      )
    )
  )
  (zone (net 5) (net_name "VSS") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30132)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 150.716666 83.631733)
        (xy 151.028414 84.022644)
        (xy 151.700424 83.67234)
        (xy 151.509863 83.209777)
        (xy 151.047142 83.019058)
      )
    )
  )
  (zone (net 12) (net_name "VDD") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30112)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 160.150528 106.703025)
        (xy 159.796975 106.349472)
        (xy 159.43106 107.301458)
        (xy 159.892293 107.493507)
        (xy 160.35494 107.301458)
      )
    )
  )
  (zone (net 1) (net_name "Net-(U1A-+)") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30168)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 134.308625 99.357899)
        (xy 134.308625 98.957899)
        (xy 133.753494 98.682899)
        (xy 133.357625 99.157899)
        (xy 133.753494 99.632899)
      )
    )
  )
  (zone (net 2) (net_name "/-sin_var_freq") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30043)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 175.092441 102.254716)
        (xy 175.375284 102.537559)
        (xy 176.362275 102.044217)
        (xy 176.112707 101.439293)
        (xy 175.507783 101.189725)
      )
    )
  )
  (zone (net 9) (net_name "/cos_var_freq") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30207)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 152.8 128.3)
        (xy 152.4 128.3)
        (xy 152.230448 128.946927)
        (xy 152.6 129.101)
        (xy 152.969552 128.946927)
      )
    )
  )
  (zone (net 22) (net_name "Net-(R3-Pad2)") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30028)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 166.6 125.1)
        (xy 166.2 125.1)
        (xy 165.614702 126.474719)
        (xy 166.4 126.801)
        (xy 167.185298 126.474719)
      )
    )
  )
  (zone (net 27) (net_name "/sin_fixed_freq") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30029)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 145.28466 128.343503)
        (xy 145.567503 128.06066)
        (xy 145.009298 126.674719)
        (xy 144.223293 126.999293)
        (xy 143.898719 127.785298)
      )
    )
  )
  (zone (net 33) (net_name "Net-(D2-A)") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30216)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 139.686864 90.999403)
        (xy 139.404021 90.71656)
        (xy 139.214887 91.096218)
        (xy 139.401475 92.064507)
        (xy 139.702182 91.2388)
      )
    )
  )
  (zone (net 4) (net_name "GND") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30074)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 169.2696 82.2038)
        (xy 169.7696 82.2038)
        (xy 169.98154 81.395142)
        (xy 169.5196 81.2028)
        (xy 169.05766 81.395142)
      )
    )
  )
  (zone (net 11) (net_name "Net-(U1D--)") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30184)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 133.302182 90.7888)
        (xy 132.802182 90.7888)
        (xy 132.752182 91.2388)
        (xy 133.052182 92.0648)
        (xy 133.352181 91.238799)
      )
    )
  )
  (zone (net 2) (net_name "/-sin_var_freq") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30011)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 154.08 103.49)
        (xy 153.68 103.49)
        (xy 152.88 104.49)
        (xy 153.88 105.491)
        (xy 154.88 104.49)
      )
    )
  )
  (zone (net 4) (net_name "GND") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30079)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 154.675959 84.6387)
        (xy 154.675959 85.1387)
        (xy 155.477487 85.314797)
        (xy 155.669829 84.852857)
        (xy 155.477487 84.390917)
      )
    )
  )
  (zone (net 12) (net_name "VDD") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30080)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 139.273674 101.540596)
        (xy 138.920122 101.894148)
        (xy 139.838858 102.36674)
        (xy 140.030907 101.905507)
        (xy 140.0302 101.4048)
      )
    )
  )
  (zone (net 35) (net_name "Net-(C15-Pad2)") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30121)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 131.526082 88.8136)
        (xy 131.026082 88.8136)
        (xy 130.831178 89.398519)
        (xy 131.326082 89.7646)
        (xy 131.779872 89.348708)
      )
    )
  )
  (zone (net 12) (net_name "VDD") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30123)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 167.6044 96.2203)
        (xy 167.6044 96.7203)
        (xy 168.174991 96.930229)
        (xy 168.5554 96.4449)
        (xy 168.146496 95.980651)
      )
    )
  )
  (zone (net 2) (net_name "/-sin_var_freq") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30228)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 163.586275 88.333199)
        (xy 163.586275 87.933199)
        (xy 163.193678 87.844617)
        (xy 162.935275 88.133199)
        (xy 163.193678 88.421781)
      )
    )
  )
  (zone (net 12) (net_name "VDD") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30038)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 180.975485 90.181932)
        (xy 180.621932 90.535485)
        (xy 180.458 91.6)
        (xy 181.112707 91.600707)
        (xy 181.716217 91.349725)
      )
    )
  )
  (zone (net 26) (net_name "Net-(D1-A)") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30187)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 166.5256 90.5625)
        (xy 166.9256 90.5625)
        (xy 167.1631 90.021164)
        (xy 166.7256 89.6865)
        (xy 166.2881 90.021164)
      )
    )
  )
  (zone (net 4) (net_name "GND") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30232)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 140.00245 77.565072)
        (xy 139.604966 77.520292)
        (xy 139.502454 77.880909)
        (xy 139.801489 78.142593)
        (xy 140.102454 77.882051)
      )
    )
  )
  (zone (net 29) (net_name "/Channel 1, X") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30134)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 131.567966 83.603296)
        (xy 131.068034 83.595132)
        (xy 130.842661 84.192213)
        (xy 131.299566 84.534099)
        (xy 131.756503 84.192213)
      )
    )
  )
  (zone (net 2) (net_name "/-sin_var_freq") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30140)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 161.407175 88.959299)
        (xy 161.007175 88.959299)
        (xy 160.737754 89.580912)
        (xy 161.207175 89.910299)
        (xy 161.676596 89.580912)
      )
    )
  )
  (zone (net 3) (net_name "Net-(U2A-+)") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30065)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 154.60776 99.988871)
        (xy 154.890603 100.271714)
        (xy 155.662963 99.849399)
        (xy 155.469382 99.361192)
        (xy 154.993675 99.174267)
      )
    )
  )
  (zone (net 4) (net_name "GND") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30072)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 167.0772 98.6442)
        (xy 166.5772 98.6442)
        (xy 166.36526 99.452858)
        (xy 166.8272 99.6452)
        (xy 167.28914 99.452858)
      )
    )
  )
  (zone (net 4) (net_name "GND") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30000)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 163.724808 75.60765)
        (xy 164.00765 75.324808)
        (xy 162.985831 74.077299)
        (xy 161.299293 74.522893)
        (xy 162.284119 75.9502)
      )
    )
  )
  (zone (net 17) (net_name "Net-(SW1A-B)") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30009)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 179.5592 94.9492)
        (xy 179.5592 95.4492)
        (xy 180.5592 96.1992)
        (xy 181.5602 95.1992)
        (xy 180.5592 94.1992)
      )
    )
  )
  (zone (net 2) (net_name "/-sin_var_freq") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30200)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 160.850275 90.847099)
        (xy 160.450275 90.847099)
        (xy 160.361693 91.239696)
        (xy 160.650275 92.123099)
        (xy 160.938857 91.239696)
      )
    )
  )
  (zone (net 7) (net_name "/cos_fixed_freq") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30014)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 128.046825 96.060799)
        (xy 127.646825 96.060799)
        (xy 126.846825 97.060799)
        (xy 127.846825 98.061799)
        (xy 128.846825 97.060799)
      )
    )
  )
  (zone (net 4) (net_name "GND") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30172)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 136.307717 88.436324)
        (xy 136.655407 88.077004)
        (xy 135.998702 87.725136)
        (xy 135.567707 88.155204)
        (xy 135.904074 88.670467)
      )
    )
  )
  (zone (net 21) (net_name "Net-(U2A--)") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30098)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 152.817265 99.270592)
        (xy 152.539471 99.558392)
        (xy 152.872975 100.280831)
        (xy 153.361194 100.097293)
        (xy 153.557246 99.621599)
      )
    )
  )
  (zone (net 7) (net_name "/cos_fixed_freq") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30005)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 129.819943 97.195899)
        (xy 129.819943 96.795899)
        (xy 127.593308 97.060799)
        (xy 127.845825 98.060799)
        (xy 128.846825 98.657044)
      )
    )
  )
  (zone (net 29) (net_name "/Channel 1, X") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30217)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 139.1516 79.2766)
        (xy 139.1516 79.6766)
        (xy 139.521516 79.815026)
        (xy 139.8026 79.5416)
        (xy 139.6016 79.2416)
      )
    )
  )
  (zone (net 12) (net_name "VDD") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30195)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 156.607809 98.414593)
        (xy 157.069841 98.223477)
        (xy 157.128857 97.954502)
        (xy 156.839893 97.071175)
        (xy 156.540275 97.897099)
      )
    )
  )
  (zone (net 29) (net_name "/Channel 1, X") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30231)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 139.6016 80.1416)
        (xy 140.0016 80.1416)
        (xy 140.1016 79.801719)
        (xy 139.8016 79.5406)
        (xy 139.5016 79.801719)
      )
    )
  )
  (zone (net 28) (net_name "/+sin_var_freq") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30060)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 163.134774 93.315441)
        (xy 163.417617 93.032598)
        (xy 163.004875 92.230947)
        (xy 162.529168 92.426992)
        (xy 162.345623 92.915199)
      )
    )
  )
  (zone (net 4) (net_name "GND") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30233)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 165.246401 77.506062)
        (xy 164.848916 77.550842)
        (xy 164.762965 77.868467)
        (xy 165.074711 78.117193)
        (xy 165.362663 77.848104)
      )
    )
  )
  (zone (net 36) (net_name "Net-(C16-Pad2)") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30116)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 152.258582 87.6508)
        (xy 152.758582 87.6508)
        (xy 152.965503 87.029187)
        (xy 152.508582 86.6873)
        (xy 152.051661 87.029187)
      )
    )
  )
  (zone (net 5) (net_name "VSS") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30127)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 166.8424 84.078)
        (xy 166.8424 84.578)
        (xy 167.397531 84.803)
        (xy 167.7934 84.328)
        (xy 167.397531 83.853)
      )
    )
  )
  (zone (net 21) (net_name "Net-(U2A--)") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30206)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 154.100295 98.325587)
        (xy 154.500255 98.331157)
        (xy 154.588857 97.954502)
        (xy 154.300288 97.0711)
        (xy 154.011693 97.954502)
      )
    )
  )
  (zone (net 12) (net_name "VDD") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30056)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 135.908699 98.24633)
        (xy 135.625856 98.529173)
        (xy 136.058625 99.350851)
        (xy 136.534332 99.154806)
        (xy 136.667877 98.616599)
      )
    )
  )
  (zone (net 19) (net_name "Net-(SW1B-B)") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30008)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 173.958 88.2864)
        (xy 173.958 87.7864)
        (xy 172.958 87.0364)
        (xy 171.957 88.0364)
        (xy 172.958 89.0364)
      )
    )
  )
  (zone (net 4) (net_name "GND") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30104)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 135.883425 101.179099)
        (xy 135.883425 100.679099)
        (xy 135.261812 100.459678)
        (xy 134.932425 100.929099)
        (xy 135.261812 101.39852)
      )
    )
  )
  (zone (net 18) (net_name "Net-(BT2--)") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30019)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 169.313982 89.447612)
        (xy 168.81405 89.455826)
        (xy 169.32832 91.340083)
        (xy 170.252216 90.958399)
        (xy 170.634883 90.03352)
      )
    )
  )
  (zone (net 20) (net_name "Net-(U1A--)") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30175)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 132.465952 98.031205)
        (xy 132.748795 98.314048)
        (xy 132.999386 97.9888)
        (xy 133.052889 97.013093)
        (xy 132.752182 96.959283)
      )
    )
  )
  (zone (net 33) (net_name "Net-(D2-A)") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30219)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 142.587582 87.5712)
        (xy 142.587582 87.9712)
        (xy 142.980179 88.059782)
        (xy 143.238582 87.7712)
        (xy 142.980179 87.482618)
      )
    )
  )
  (zone (net 30) (net_name "/Channel 2, Y") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30224)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 164.4246 79.3162)
        (xy 164.4246 79.7162)
        (xy 164.817197 79.804782)
        (xy 165.0756 79.5162)
        (xy 164.817197 79.227618)
      )
    )
  )
  (zone (net 26) (net_name "Net-(D1-A)") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30151)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 166.9256 90.7588)
        (xy 166.5256 90.7588)
        (xy 166.268679 91.380413)
        (xy 166.7256 91.7223)
        (xy 167.182521 91.380413)
      )
    )
  )
  (zone (net 20) (net_name "Net-(U1A--)") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30067)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 132.608218 98.454625)
        (xy 132.325375 98.171782)
        (xy 131.576765 98.618499)
        (xy 131.783118 99.106706)
        (xy 132.258825 99.282291)
      )
    )
  )
  (zone (net 2) (net_name "/-sin_var_freq") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30048)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 151.735475 100.638299)
        (xy 151.335475 100.638299)
        (xy 151.043305 101.380128)
        (xy 151.611775 101.951799)
        (xy 152.165801 101.358511)
      )
    )
  )
  (zone (net 10) (net_name "Net-(U2B-+)") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30173)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 158.600842 98.966562)
        (xy 158.323013 99.254329)
        (xy 158.945284 99.735607)
        (xy 159.380994 99.362593)
        (xy 159.142775 98.874399)
      )
    )
  )
  (zone (net 14) (net_name "Net-(U1C--)") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30158)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 140.080875 93.339599)
        (xy 140.080875 93.739599)
        (xy 140.702488 93.99652)
        (xy 141.044375 93.539599)
        (xy 140.702488 93.082678)
      )
    )
  )
  (zone (net 12) (net_name "VDD") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30075)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 144.564211 102.763283)
        (xy 144.917765 102.409729)
        (xy 144.495822 101.688058)
        (xy 144.033175 101.878693)
        (xy 143.84254 102.34134)
      )
    )
  )
  (zone (net 8) (net_name "Net-(U1B-+)") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30130)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 130.685382 95.593799)
        (xy 130.685382 95.193799)
        (xy 130.063769 94.936878)
        (xy 129.671882 95.393799)
        (xy 130.063769 95.85072)
      )
    )
  )
  (zone (net 12) (net_name "VDD") (layer "B.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30002)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 163.438613 102.0612)
        (xy 163.438613 102.5612)
        (xy 164.42097 102.722501)
        (xy 164.42197 102.222501)
        (xy 164.229628 101.760561)
      )
    )
  )
  (zone (net 9) (net_name "/cos_var_freq") (layer "B.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30017)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 152.8 130.501989)
        (xy 152.4 130.501989)
        (xy 152.240448 131.146927)
        (xy 152.61 131.301)
        (xy 152.979552 131.146927)
      )
    )
  )
  (zone (net 33) (net_name "Net-(D2-A)") (layer "B.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30007)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 141.043782 103.051)
        (xy 141.043782 103.451)
        (xy 141.85244 103.71294)
        (xy 142.044782 103.251)
        (xy 141.85244 102.78906)
      )
    )
  )
  (zone (net 2) (net_name "/-sin_var_freq") (layer "B.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30013)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 162.356683 104.576401)
        (xy 162.356683 104.976401)
        (xy 163.158658 105.27194)
        (xy 163.351 104.81)
        (xy 163.158658 104.34806)
      )
    )
  )
  (zone (net 4) (net_name "GND") (layer "B.Cu") (hatch edge 0.5)
    (connect_pads (clearance 0.5))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 120.65 133.35)
        (xy 120.65 69.85)
        (xy 184.15 69.85)
        (xy 184.15 133.35)
      )
    )
  )
  (zone (net 33) (net_name "Net-(D2-A)") (layer "B.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30011)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 141.0302 103.451)
        (xy 141.0302 103.051)
        (xy 140.221542 102.78906)
        (xy 140.0292 103.251)
        (xy 140.221542 103.71294)
      )
    )
  )
  (zone (net 9) (net_name "/cos_var_freq") (layer "B.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30000)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 148.295382 105.378)
        (xy 148.695382 105.378)
        (xy 149.495382 104.378)
        (xy 148.495382 103.377)
        (xy 147.495382 104.378)
      )
    )
  )
  (zone (net 5) (net_name "VSS") (layer "B.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30006)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 152.631234 82.9604)
        (xy 152.631234 83.4604)
        (xy 153.43484 83.69774)
        (xy 153.627182 83.2358)
        (xy 153.43484 82.77386)
      )
    )
  )
  (zone (net 9) (net_name "/cos_var_freq") (layer "B.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30015)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 148.695382 107.372799)
        (xy 148.295382 107.372799)
        (xy 148.21 108.15)
        (xy 148.61 108.151)
        (xy 148.979552 107.996927)
      )
    )
  )
  (zone (net 2) (net_name "/-sin_var_freq") (layer "B.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30008)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 157.232975 104.927653)
        (xy 157.232975 104.527653)
        (xy 156.424317 104.265713)
        (xy 156.231975 104.727653)
        (xy 156.424317 105.189593)
      )
    )
  )
  (zone (net 12) (net_name "VDD") (layer "B.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30003)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 141.0302 102.1548)
        (xy 141.0302 101.6548)
        (xy 140.221542 101.44286)
        (xy 140.0292 101.9048)
        (xy 140.221542 102.36674)
      )
    )
  )
  (zone (net 12) (net_name "VDD") (layer "B.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30010)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 157.251393 107.6674)
        (xy 157.251393 107.2674)
        (xy 156.442735 107.00546)
        (xy 156.250393 107.4674)
        (xy 156.442735 107.92934)
      )
    )
  )
  (zone (net 12) (net_name "VDD") (layer "B.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30012)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 158.898052 107.2674)
        (xy 158.898052 107.6674)
        (xy 159.701658 107.95474)
        (xy 159.894 107.4928)
        (xy 159.701658 107.03086)
      )
    )
  )
  (zone (net 2) (net_name "/-sin_var_freq") (layer "B.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30014)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 158.740779 104.527653)
        (xy 158.740779 104.927653)
        (xy 159.53974 105.238341)
        (xy 159.732082 104.776401)
        (xy 159.53974 104.314461)
      )
    )
  )
  (zone (net 12) (net_name "VDD") (layer "B.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30001)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 159.352215 102.5612)
        (xy 159.352215 102.0612)
        (xy 158.559709 101.76806)
        (xy 158.367367 102.23)
        (xy 158.368367 102.73)
      )
    )
  )
  (zone (net 9) (net_name "/cos_var_freq") (layer "B.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30016)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 152.4 129.9)
        (xy 152.8 129.9)
        (xy 152.969552 129.253073)
        (xy 152.6 129.099)
        (xy 152.230448 129.253073)
      )
    )
  )
  (zone (net 2) (net_name "/-sin_var_freq") (layer "B.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30009)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 160.731082 104.976401)
        (xy 160.731082 104.576401)
        (xy 159.922424 104.314461)
        (xy 159.730082 104.776401)
        (xy 159.922424 105.238341)
      )
    )
  )
  (zone (net 5) (net_name "VSS") (layer "B.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30004)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 152.509082 83.4604)
        (xy 152.509082 82.9604)
        (xy 151.700424 82.74846)
        (xy 151.508082 83.2104)
        (xy 151.700424 83.67234)
      )
    )
  )
  (zone (net 12) (net_name "VDD") (layer "B.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30005)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 143.038934 101.6548)
        (xy 143.038934 102.1548)
        (xy 143.84254 102.34134)
        (xy 144.034882 101.8794)
        (xy 143.84254 101.41746)
      )
    )
  )
)
