(kicad_sch
	(version 20231120)
	(generator "eeschema")
	(generator_version "8.0")
	(paper "A4")
	(title_block
		(title "CNC3040 Control Box")
	)
	(lib_symbols
		(symbol "Analog_Switch:TS3A24159DGSR"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "U"
				(at -3.81 7.62 0)
			)
			(property "Value" "TS3A24159DGSR"
				(at -3.81 5.715 0)
			)
			(property "Footprint" "Package_SO:TSSOP-10_3x3mm_P0.5mm"
				(at 1.27 -11.43 0)
			)
			(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ts3a24159.pdf"
				(at 1.27 -13.335 0)
			)
			(property "Description" "Dual SPDT 0.3Ω Bidirectional Analog Switch, TSSOP-10"
				(at 0 0 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(property "ki_keywords" "switch analog SPDT"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "*SSOP*3x3mm*P0.5mm*"
				(at 0 0 0)
			)
			(symbol "TS3A24159DGSR_1_1"
				(rectangle
					(start -3.81 4.445)
					(end 3.81 -4.445)
					(fill
						(type background)
					)
				)
				(circle
					(center -2.159 0)
					(radius 0.508)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -5.08 0) (xy -2.794 0)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -1.651 0.127) (xy 2.54 1.905)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -5.08) (xy 0 -4.572)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -4.318) (xy 0 -4.064)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -3.81) (xy 0 -3.556)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -3.302) (xy 0 -3.048)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -2.794) (xy 0 -2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -2.286) (xy 0 -2.032)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -1.778) (xy 0 -1.524)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -1.27) (xy 0 -1.016)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -0.762) (xy 0 -0.508)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -0.254) (xy 0 0)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 0.254) (xy 0 0.508)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 5.08 -2.54) (xy 2.794 -2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 5.08 2.54) (xy 2.794 2.54)
					)
					(fill
						(type none)
					)
				)
				(circle
					(center 2.159 -2.54)
					(radius 0.508)
					(fill
						(type none)
					)
				)
				(circle
					(center 2.159 2.54)
					(radius 0.508)
					(fill
						(type none)
					)
				)
				(pin passive line
					(at 7.62 -2.54 180)
					(length 2.54)
					(name "~")
					(number "2")
				)
				(pin passive line
					(at -7.62 0 0)
					(length 2.54)
					(name "~")
					(number "3")
				)
				(pin input line
					(at 0 -7.62 90)
					(length 2.54)
					(name "~")
					(number "4")
				)
				(pin passive line
					(at 7.62 2.54 180)
					(length 2.54)
					(name "~")
					(number "5")
				)
			)
			(symbol "TS3A24159DGSR_2_1"
				(rectangle
					(start -3.81 4.445)
					(end 3.81 -4.445)
					(fill
						(type background)
					)
				)
				(circle
					(center -2.159 0)
					(radius 0.508)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -5.08 0) (xy -2.794 0)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -1.651 0.127) (xy 2.54 1.905)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -5.08) (xy 0 -4.572)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -4.318) (xy 0 -4.064)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -3.81) (xy 0 -3.556)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -3.302) (xy 0 -3.048)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -2.794) (xy 0 -2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -2.286) (xy 0 -2.032)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -1.778) (xy 0 -1.524)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -1.27) (xy 0 -1.016)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -0.762) (xy 0 -0.508)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -0.254) (xy 0 0)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 0.254) (xy 0 0.508)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 5.08 -2.54) (xy 2.794 -2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 5.08 2.54) (xy 2.794 2.54)
					)
					(fill
						(type none)
					)
				)
				(circle
					(center 2.159 -2.54)
					(radius 0.508)
					(fill
						(type none)
					)
				)
				(circle
					(center 2.159 2.54)
					(radius 0.508)
					(fill
						(type none)
					)
				)
				(pin passive line
					(at 7.62 -2.54 180)
					(length 2.54)
					(name "~")
					(number "10")
				)
				(pin passive line
					(at 7.62 2.54 180)
					(length 2.54)
					(name "~")
					(number "7")
				)
				(pin input line
					(at 0 -7.62 90)
					(length 2.54)
					(name "~")
					(number "8")
				)
				(pin passive line
					(at -7.62 0 0)
					(length 2.54)
					(name "~")
					(number "9")
				)
			)
			(symbol "TS3A24159DGSR_3_1"
				(rectangle
					(start -3.81 10.16)
					(end 3.81 -10.16)
					(fill
						(type background)
					)
				)
				(pin power_in line
					(at 0 12.7 270)
					(length 2.54)
					(name "VCC")
					(number "1")
				)
				(pin power_in line
					(at 0 -12.7 90)
					(length 2.54)
					(name "GND")
					(number "6")
				)
			)
		)
		(symbol "Connector:Conn_01x01_Pin"
			(pin_names
				(offset 1.016) hide)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "J"
				(at 0 2.54 0)
			)
			(property "Value" "Conn_01x01_Pin"
				(at 0 -2.54 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" "~"
				(at 0 0 0)
			)
			(property "Description" "Generic connector, single row, 01x01, script generated"
				(at 0 0 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(property "ki_keywords" "connector"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "Connector*:*_1x??_*"
				(at 0 0 0)
			)
			(symbol "Conn_01x01_Pin_1_1"
				(polyline
					(pts
						(xy 1.27 0) (xy 0.8636 0)
					)
					(fill
						(type none)
					)
				)
				(rectangle
					(start 0.8636 0.127)
					(end 0 -0.127)
					(fill
						(type outline)
					)
				)
				(pin passive line
					(at 5.08 0 180)
					(length 3.81)
					(name "Pin_1")
					(number "1")
				)
			)
		)
		(symbol "Connector:Conn_01x02_Pin"
			(pin_names
				(offset 1.016) hide)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "J"
				(at 0 2.54 0)
			)
			(property "Value" "Conn_01x02_Pin"
				(at 0 -5.08 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" "~"
				(at 0 0 0)
			)
			(property "Description" "Generic connector, single row, 01x02, script generated"
				(at 0 0 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(property "ki_keywords" "connector"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "Connector*:*_1x??_*"
				(at 0 0 0)
			)
			(symbol "Conn_01x02_Pin_1_1"
				(polyline
					(pts
						(xy 1.27 -2.54) (xy 0.8636 -2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.27 0) (xy 0.8636 0)
					)
					(fill
						(type none)
					)
				)
				(rectangle
					(start 0.8636 -2.413)
					(end 0 -2.667)
					(fill
						(type outline)
					)
				)
				(rectangle
					(start 0.8636 0.127)
					(end 0 -0.127)
					(fill
						(type outline)
					)
				)
				(pin passive line
					(at 5.08 0 180)
					(length 3.81)
					(name "Pin_1")
					(number "1")
				)
				(pin passive line
					(at 5.08 -2.54 180)
					(length 3.81)
					(name "Pin_2")
					(number "2")
				)
			)
		)
		(symbol "Connector:Conn_01x03_Pin"
			(pin_names
				(offset 1.016) hide)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "J"
				(at 0 5.08 0)
			)
			(property "Value" "Conn_01x03_Pin"
				(at 0 -5.08 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" "~"
				(at 0 0 0)
			)
			(property "Description" "Generic connector, single row, 01x03, script generated"
				(at 0 0 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(property "ki_keywords" "connector"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "Connector*:*_1x??_*"
				(at 0 0 0)
			)
			(symbol "Conn_01x03_Pin_1_1"
				(polyline
					(pts
						(xy 1.27 -2.54) (xy 0.8636 -2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.27 0) (xy 0.8636 0)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.27 2.54) (xy 0.8636 2.54)
					)
					(fill
						(type none)
					)
				)
				(rectangle
					(start 0.8636 -2.413)
					(end 0 -2.667)
					(fill
						(type outline)
					)
				)
				(rectangle
					(start 0.8636 0.127)
					(end 0 -0.127)
					(fill
						(type outline)
					)
				)
				(rectangle
					(start 0.8636 2.667)
					(end 0 2.413)
					(fill
						(type outline)
					)
				)
				(pin passive line
					(at 5.08 2.54 180)
					(length 3.81)
					(name "Pin_1")
					(number "1")
				)
				(pin passive line
					(at 5.08 0 180)
					(length 3.81)
					(name "Pin_2")
					(number "2")
				)
				(pin passive line
					(at 5.08 -2.54 180)
					(length 3.81)
					(name "Pin_3")
					(number "3")
				)
			)
		)
		(symbol "Connector:Conn_01x04_Pin"
			(pin_names
				(offset 1.016) hide)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "J"
				(at 0 5.08 0)
			)
			(property "Value" "Conn_01x04_Pin"
				(at 0 -7.62 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" "~"
				(at 0 0 0)
			)
			(property "Description" "Generic connector, single row, 01x04, script generated"
				(at 0 0 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(property "ki_keywords" "connector"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "Connector*:*_1x??_*"
				(at 0 0 0)
			)
			(symbol "Conn_01x04_Pin_1_1"
				(polyline
					(pts
						(xy 1.27 -5.08) (xy 0.8636 -5.08)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.27 -2.54) (xy 0.8636 -2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.27 0) (xy 0.8636 0)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.27 2.54) (xy 0.8636 2.54)
					)
					(fill
						(type none)
					)
				)
				(rectangle
					(start 0.8636 -4.953)
					(end 0 -5.207)
					(fill
						(type outline)
					)
				)
				(rectangle
					(start 0.8636 -2.413)
					(end 0 -2.667)
					(fill
						(type outline)
					)
				)
				(rectangle
					(start 0.8636 0.127)
					(end 0 -0.127)
					(fill
						(type outline)
					)
				)
				(rectangle
					(start 0.8636 2.667)
					(end 0 2.413)
					(fill
						(type outline)
					)
				)
				(pin passive line
					(at 5.08 2.54 180)
					(length 3.81)
					(name "Pin_1")
					(number "1")
				)
				(pin passive line
					(at 5.08 0 180)
					(length 3.81)
					(name "Pin_2")
					(number "2")
				)
				(pin passive line
					(at 5.08 -2.54 180)
					(length 3.81)
					(name "Pin_3")
					(number "3")
				)
				(pin passive line
					(at 5.08 -5.08 180)
					(length 3.81)
					(name "Pin_4")
					(number "4")
				)
			)
		)
		(symbol "Connector:DE9_Plug"
			(pin_names
				(offset 1.016) hide)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "J"
				(at 0 13.97 0)
			)
			(property "Value" "DE9_Plug"
				(at 0 -14.605 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" " ~"
				(at 0 0 0)
			)
			(property "Description" "9-pin male plug pin D-SUB connector"
				(at 0 0 0)
			)
			(property "ki_keywords" "connector male plug D-SUB DB9"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "DSUB*Male*"
				(at 0 0 0)
			)
			(symbol "DE9_Plug_0_1"
				(circle
					(center -1.778 -10.16)
					(radius 0.762)
					(fill
						(type outline)
					)
				)
				(circle
					(center -1.778 -5.08)
					(radius 0.762)
					(fill
						(type outline)
					)
				)
				(circle
					(center -1.778 0)
					(radius 0.762)
					(fill
						(type outline)
					)
				)
				(circle
					(center -1.778 5.08)
					(radius 0.762)
					(fill
						(type outline)
					)
				)
				(circle
					(center -1.778 10.16)
					(radius 0.762)
					(fill
						(type outline)
					)
				)
				(polyline
					(pts
						(xy -3.81 -10.16) (xy -2.54 -10.16)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -3.81 -7.62) (xy 0.508 -7.62)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -3.81 -5.08) (xy -2.54 -5.08)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -3.81 -2.54) (xy 0.508 -2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -3.81 0) (xy -2.54 0)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -3.81 2.54) (xy 0.508 2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -3.81 5.08) (xy -2.54 5.08)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -3.81 7.62) (xy 0.508 7.62)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -3.81 10.16) (xy -2.54 10.16)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -3.81 -13.335) (xy -3.81 13.335) (xy 3.81 9.525) (xy 3.81 -9.525) (xy -3.81 -13.335)
					)
					(fill
						(type background)
					)
				)
				(circle
					(center 1.27 -7.62)
					(radius 0.762)
					(fill
						(type outline)
					)
				)
				(circle
					(center 1.27 -2.54)
					(radius 0.762)
					(fill
						(type outline)
					)
				)
				(circle
					(center 1.27 2.54)
					(radius 0.762)
					(fill
						(type outline)
					)
				)
				(circle
					(center 1.27 7.62)
					(radius 0.762)
					(fill
						(type outline)
					)
				)
			)
			(symbol "DE9_Plug_1_1"
				(pin passive line
					(at -7.62 -10.16 0)
					(length 3.81)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at -7.62 -5.08 0)
					(length 3.81)
					(name "2")
					(number "2")
				)
				(pin passive line
					(at -7.62 0 0)
					(length 3.81)
					(name "3")
					(number "3")
				)
				(pin passive line
					(at -7.62 5.08 0)
					(length 3.81)
					(name "4")
					(number "4")
				)
				(pin passive line
					(at -7.62 10.16 0)
					(length 3.81)
					(name "5")
					(number "5")
				)
				(pin passive line
					(at -7.62 -7.62 0)
					(length 3.81)
					(name "6")
					(number "6")
				)
				(pin passive line
					(at -7.62 -2.54 0)
					(length 3.81)
					(name "7")
					(number "7")
				)
				(pin passive line
					(at -7.62 2.54 0)
					(length 3.81)
					(name "8")
					(number "8")
				)
				(pin passive line
					(at -7.62 7.62 0)
					(length 3.81)
					(name "9")
					(number "9")
				)
			)
		)
		(symbol "Device:LED"
			(pin_numbers hide)
			(pin_names
				(offset 1.016) hide)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "D"
				(at 0 2.54 0)
			)
			(property "Value" "LED"
				(at 0 -2.54 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" "~"
				(at 0 0 0)
			)
			(property "Description" "Light emitting diode"
				(at 0 0 0)
			)
			(property "ki_keywords" "LED diode"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "LED* LED_SMD:* LED_THT:*"
				(at 0 0 0)
			)
			(symbol "LED_0_1"
				(polyline
					(pts
						(xy -1.27 -1.27) (xy -1.27 1.27)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -1.27 0) (xy 1.27 0)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.27 -1.27) (xy 1.27 1.27) (xy -1.27 0) (xy 1.27 -1.27)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -3.048 -0.762) (xy -4.572 -2.286) (xy -3.81 -2.286) (xy -4.572 -2.286) (xy -4.572 -1.524)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -1.778 -0.762) (xy -3.302 -2.286) (xy -2.54 -2.286) (xy -3.302 -2.286) (xy -3.302 -1.524)
					)
					(fill
						(type none)
					)
				)
			)
			(symbol "LED_1_1"
				(pin passive line
					(at -3.81 0 0)
					(length 2.54)
					(name "K")
					(number "1")
				)
				(pin passive line
					(at 3.81 0 180)
					(length 2.54)
					(name "A")
					(number "2")
				)
			)
		)
		(symbol "Device:R_Potentiometer"
			(pin_names
				(offset 1.016) hide)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "RV"
				(at -4.445 0 90)
			)
			(property "Value" "R_Potentiometer"
				(at -2.54 0 90)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" "~"
				(at 0 0 0)
			)
			(property "Description" "Potentiometer"
				(at 0 0 0)
			)
			(property "ki_keywords" "resistor variable"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "Potentiometer*"
				(at 0 0 0)
			)
			(symbol "R_Potentiometer_0_1"
				(polyline
					(pts
						(xy 2.54 0) (xy 1.524 0)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.143 0) (xy 2.286 0.508) (xy 2.286 -0.508) (xy 1.143 0)
					)
					(fill
						(type outline)
					)
				)
				(rectangle
					(start 1.016 2.54)
					(end -1.016 -2.54)
					(fill
						(type none)
					)
				)
			)
			(symbol "R_Potentiometer_1_1"
				(pin passive line
					(at 0 3.81 270)
					(length 1.27)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 3.81 0 180)
					(length 1.27)
					(name "2")
					(number "2")
				)
				(pin passive line
					(at 0 -3.81 90)
					(length 1.27)
					(name "3")
					(number "3")
				)
			)
		)
		(symbol "Device:R_US"
			(pin_numbers hide)
			(pin_names
				(offset 0)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "R"
				(at 2.54 0 90)
			)
			(property "Value" "R_US"
				(at -2.54 0 90)
			)
			(property "Footprint" ""
				(at 1.016 -0.254 90)
			)
			(property "Datasheet" "~"
				(at 0 0 0)
			)
			(property "Description" "Resistor, US symbol"
				(at 0 0 0)
			)
			(property "ki_keywords" "R res resistor"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "R_*"
				(at 0 0 0)
			)
			(symbol "R_US_0_1"
				(polyline
					(pts
						(xy 0 -2.286) (xy 0 -2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 2.286) (xy 0 2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -0.762) (xy 1.016 -1.143) (xy 0 -1.524) (xy -1.016 -1.905) (xy 0 -2.286)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 0.762) (xy 1.016 0.381) (xy 0 0) (xy -1.016 -0.381) (xy 0 -0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 2.286) (xy 1.016 1.905) (xy 0 1.524) (xy -1.016 1.143) (xy 0 0.762)
					)
					(fill
						(type none)
					)
				)
			)
			(symbol "R_US_1_1"
				(pin passive line
					(at 0 3.81 270)
					(length 1.27)
					(name "~")
					(number "1")
				)
				(pin passive line
					(at 0 -3.81 90)
					(length 1.27)
					(name "~")
					(number "2")
				)
			)
		)
		(symbol "Device:RotaryEncoder_Switch"
			(pin_names
				(offset 0.254) hide)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "SW"
				(at 0 6.604 0)
			)
			(property "Value" "RotaryEncoder_Switch"
				(at 0 -6.604 0)
			)
			(property "Footprint" ""
				(at -3.81 4.064 0)
			)
			(property "Datasheet" "~"
				(at 0 6.604 0)
			)
			(property "Description" "Rotary encoder, dual channel, incremental quadrate outputs, with switch"
				(at 0 0 0)
			)
			(property "ki_keywords" "rotary switch encoder switch push button"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "RotaryEncoder*Switch*"
				(at 0 0 0)
			)
			(symbol "RotaryEncoder_Switch_0_1"
				(rectangle
					(start -5.08 5.08)
					(end 5.08 -5.08)
					(fill
						(type background)
					)
				)
				(circle
					(center -3.81 0)
					(radius 0.254)
					(fill
						(type outline)
					)
				)
				(circle
					(center -0.381 0)
					(radius 1.905)
					(fill
						(type none)
					)
				)
				(arc
					(start -0.381 2.667)
					(mid -3.0988 -0.0635)
					(end -0.381 -2.794)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -0.635 -1.778) (xy -0.635 1.778)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -0.381 -1.778) (xy -0.381 1.778)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -0.127 1.778) (xy -0.127 -1.778)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 3.81 0) (xy 3.429 0)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 3.81 1.016) (xy 3.81 -1.016)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -5.08 -2.54) (xy -3.81 -2.54) (xy -3.81 -2.032)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -5.08 2.54) (xy -3.81 2.54) (xy -3.81 2.032)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0.254 -3.048) (xy -0.508 -2.794) (xy 0.127 -2.413)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0.254 2.921) (xy -0.508 2.667) (xy 0.127 2.286)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 5.08 -2.54) (xy 4.318 -2.54) (xy 4.318 -1.016)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 5.08 2.54) (xy 4.318 2.54) (xy 4.318 1.016)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -5.08 0) (xy -3.81 0) (xy -3.81 -1.016) (xy -3.302 -2.032)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -4.318 0) (xy -3.81 0) (xy -3.81 1.016) (xy -3.302 2.032)
					)
					(fill
						(type none)
					)
				)
				(circle
					(center 4.318 -1.016)
					(radius 0.127)
					(fill
						(type none)
					)
				)
				(circle
					(center 4.318 1.016)
					(radius 0.127)
					(fill
						(type none)
					)
				)
			)
			(symbol "RotaryEncoder_Switch_1_1"
				(pin passive line
					(at -7.62 2.54 0)
					(length 2.54)
					(name "A")
					(number "A")
				)
				(pin passive line
					(at -7.62 -2.54 0)
					(length 2.54)
					(name "B")
					(number "B")
				)
				(pin passive line
					(at -7.62 0 0)
					(length 2.54)
					(name "C")
					(number "C")
				)
				(pin passive line
					(at 7.62 2.54 180)
					(length 2.54)
					(name "S1")
					(number "S1")
				)
				(pin passive line
					(at 7.62 -2.54 180)
					(length 2.54)
					(name "S2")
					(number "S2")
				)
			)
		)
		(symbol "Isolator:ACPL-214-500E"
			(pin_names
				(offset 1.016)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "U"
				(at -5.08 5.08 0)
			)
			(property "Value" "ACPL-214-500E"
				(at 0 5.08 0)
			)
			(property "Footprint" "Package_SO:SOP-4_4.4x2.6mm_P1.27mm"
				(at -21.59 -5.08 0)
			)
			(property "Datasheet" "https://docs.broadcom.com/doc/AV02-0469EN"
				(at 0.635 0 0)
			)
			(property "Description" "AC/DC Phototransistor Optocoupler, Vce 80V, CTR 20-400%, SOP-4"
				(at 0 0 0)
			)
			(property "ki_keywords" "npn ac dc ac-dc acdc phototransistor optocoupler optoisolator"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "SOP*4*4.4x2.6mm*P1.27mm*"
				(at 0 0 0)
			)
			(symbol "ACPL-214-500E_0_1"
				(rectangle
					(start -5.08 3.81)
					(end 5.08 -3.81)
					(fill
						(type background)
					)
				)
				(circle
					(center -3.175 -2.54)
					(radius 0.127)
					(fill
						(type none)
					)
				)
				(circle
					(center -3.175 2.54)
					(radius 0.127)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -3.81 0.635) (xy -2.54 0.635)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -3.175 -0.635) (xy -3.175 -2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -3.175 -0.635) (xy -3.175 2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -1.905 -0.635) (xy -0.635 -0.635)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 2.54 0.635) (xy 4.445 2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 4.445 -2.54) (xy 2.54 -0.635)
					)
					(fill
						(type outline)
					)
				)
				(polyline
					(pts
						(xy 4.445 -2.54) (xy 5.08 -2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 4.445 2.54) (xy 5.08 2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -5.08 2.54) (xy -1.27 2.54) (xy -1.27 -0.635)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -1.27 -0.635) (xy -1.27 -2.54) (xy -5.08 -2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 2.54 1.905) (xy 2.54 -1.905) (xy 2.54 -1.905)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -3.175 0.635) (xy -3.81 -0.635) (xy -2.54 -0.635) (xy -3.175 0.635)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -1.27 -0.635) (xy -1.905 0.635) (xy -0.635 0.635) (xy -1.27 -0.635)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0.127 -0.508) (xy 1.397 -0.508) (xy 1.016 -0.635) (xy 1.016 -0.381) (xy 1.397 -0.508)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0.127 0.508) (xy 1.397 0.508) (xy 1.016 0.381) (xy 1.016 0.635) (xy 1.397 0.508)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 3.048 -1.651) (xy 3.556 -1.143) (xy 4.064 -2.159) (xy 3.048 -1.651) (xy 3.048 -1.651)
					)
					(fill
						(type outline)
					)
				)
			)
			(symbol "ACPL-214-500E_1_1"
				(pin passive line
					(at -7.62 2.54 0)
					(length 2.54)
					(name "~")
					(number "1")
				)
				(pin passive line
					(at -7.62 -2.54 0)
					(length 2.54)
					(name "~")
					(number "2")
				)
				(pin passive line
					(at 7.62 -2.54 180)
					(length 2.54)
					(name "~")
					(number "3")
				)
				(pin passive line
					(at 7.62 2.54 180)
					(length 2.54)
					(name "~")
					(number "4")
				)
			)
		)
		(symbol "MCU_Module:Arduino_UNO_R3"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "A"
				(at -10.16 23.495 0)
			)
			(property "Value" "Arduino_UNO_R3"
				(at 5.08 -26.67 0)
			)
			(property "Footprint" "Module:Arduino_UNO_R3"
				(at 0 0 0)
			)
			(property "Datasheet" "https://www.arduino.cc/en/Main/arduinoBoardUno"
				(at 0 0 0)
			)
			(property "Description" "Arduino UNO Microcontroller Module, release 3"
				(at 0 0 0)
			)
			(property "ki_keywords" "Arduino UNO R3 Microcontroller Module Atmel AVR USB"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "Arduino*UNO*R3*"
				(at 0 0 0)
			)
			(symbol "Arduino_UNO_R3_0_1"
				(rectangle
					(start -10.16 22.86)
					(end 10.16 -25.4)
					(fill
						(type background)
					)
				)
			)
			(symbol "Arduino_UNO_R3_1_1"
				(pin no_connect line
					(at -10.16 -20.32 0)
					(length 2.54) hide
					(name "NC")
					(number "1")
				)
				(pin bidirectional line
					(at 12.7 -2.54 180)
					(length 2.54)
					(name "A1")
					(number "10")
				)
				(pin bidirectional line
					(at 12.7 -5.08 180)
					(length 2.54)
					(name "A2")
					(number "11")
				)
				(pin bidirectional line
					(at 12.7 -7.62 180)
					(length 2.54)
					(name "A3")
					(number "12")
				)
				(pin bidirectional line
					(at 12.7 -10.16 180)
					(length 2.54)
					(name "SDA/A4")
					(number "13")
				)
				(pin bidirectional line
					(at 12.7 -12.7 180)
					(length 2.54)
					(name "SCL/A5")
					(number "14")
				)
				(pin bidirectional line
					(at -12.7 15.24 0)
					(length 2.54)
					(name "D0/RX")
					(number "15")
				)
				(pin bidirectional line
					(at -12.7 12.7 0)
					(length 2.54)
					(name "D1/TX")
					(number "16")
				)
				(pin bidirectional line
					(at -12.7 10.16 0)
					(length 2.54)
					(name "D2")
					(number "17")
				)
				(pin bidirectional line
					(at -12.7 7.62 0)
					(length 2.54)
					(name "D3")
					(number "18")
				)
				(pin bidirectional line
					(at -12.7 5.08 0)
					(length 2.54)
					(name "D4")
					(number "19")
				)
				(pin output line
					(at 12.7 10.16 180)
					(length 2.54)
					(name "IOREF")
					(number "2")
				)
				(pin bidirectional line
					(at -12.7 2.54 0)
					(length 2.54)
					(name "D5")
					(number "20")
				)
				(pin bidirectional line
					(at -12.7 0 0)
					(length 2.54)
					(name "D6")
					(number "21")
				)
				(pin bidirectional line
					(at -12.7 -2.54 0)
					(length 2.54)
					(name "D7")
					(number "22")
				)
				(pin bidirectional line
					(at -12.7 -5.08 0)
					(length 2.54)
					(name "D8")
					(number "23")
				)
				(pin bidirectional line
					(at -12.7 -7.62 0)
					(length 2.54)
					(name "D9")
					(number "24")
				)
				(pin bidirectional line
					(at -12.7 -10.16 0)
					(length 2.54)
					(name "D10")
					(number "25")
				)
				(pin bidirectional line
					(at -12.7 -12.7 0)
					(length 2.54)
					(name "D11")
					(number "26")
				)
				(pin bidirectional line
					(at -12.7 -15.24 0)
					(length 2.54)
					(name "D12")
					(number "27")
				)
				(pin bidirectional line
					(at -12.7 -17.78 0)
					(length 2.54)
					(name "D13")
					(number "28")
				)
				(pin power_in line
					(at -2.54 -27.94 90)
					(length 2.54)
					(name "GND")
					(number "29")
				)
				(pin input line
					(at 12.7 15.24 180)
					(length 2.54)
					(name "~{RESET}")
					(number "3")
				)
				(pin input line
					(at 12.7 5.08 180)
					(length 2.54)
					(name "AREF")
					(number "30")
				)
				(pin bidirectional line
					(at 12.7 -17.78 180)
					(length 2.54)
					(name "SDA/A4")
					(number "31")
				)
				(pin bidirectional line
					(at 12.7 -20.32 180)
					(length 2.54)
					(name "SCL/A5")
					(number "32")
				)
				(pin power_out line
					(at 2.54 25.4 270)
					(length 2.54)
					(name "3V3")
					(number "4")
				)
				(pin power_out line
					(at 5.08 25.4 270)
					(length 2.54)
					(name "+5V")
					(number "5")
				)
				(pin power_in line
					(at 0 -27.94 90)
					(length 2.54)
					(name "GND")
					(number "6")
				)
				(pin power_in line
					(at 2.54 -27.94 90)
					(length 2.54)
					(name "GND")
					(number "7")
				)
				(pin power_in line
					(at -2.54 25.4 270)
					(length 2.54)
					(name "VIN")
					(number "8")
				)
				(pin bidirectional line
					(at 12.7 0 180)
					(length 2.54)
					(name "A0")
					(number "9")
				)
			)
		)
		(symbol "Switch:SW_Push"
			(pin_numbers hide)
			(pin_names
				(offset 1.016) hide)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "SW"
				(at 1.27 2.54 0)
			)
			(property "Value" "SW_Push"
				(at 0 -1.524 0)
			)
			(property "Footprint" ""
				(at 0 5.08 0)
			)
			(property "Datasheet" "~"
				(at 0 5.08 0)
			)
			(property "Description" "Push button switch, generic, two pins"
				(at 0 0 0)
			)
			(property "ki_keywords" "switch normally-open pushbutton push-button"
				(at 0 0 0)
			)
			(symbol "SW_Push_0_1"
				(circle
					(center -2.032 0)
					(radius 0.508)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 1.27) (xy 0 3.048)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 2.54 1.27) (xy -2.54 1.27)
					)
					(fill
						(type none)
					)
				)
				(circle
					(center 2.032 0)
					(radius 0.508)
					(fill
						(type none)
					)
				)
				(pin passive line
					(at -5.08 0 0)
					(length 2.54)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 5.08 0 180)
					(length 2.54)
					(name "2")
					(number "2")
				)
			)
		)
		(symbol "power:+5C"
			(power)
			(pin_numbers hide)
			(pin_names
				(offset 0) hide)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "#PWR"
				(at 0 -3.81 0)
			)
			(property "Value" "+5C"
				(at 0 3.556 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" "Power symbol creates a global label with name \"+5C\""
				(at 0 0 0)
			)
			(property "ki_keywords" "global power"
				(at 0 0 0)
			)
			(symbol "+5C_0_1"
				(polyline
					(pts
						(xy -0.762 1.27) (xy 0 2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 0) (xy 0 2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 2.54) (xy 0.762 1.27)
					)
					(fill
						(type none)
					)
				)
			)
			(symbol "+5C_1_1"
				(pin power_in line
					(at 0 0 90)
					(length 0)
					(name "~")
					(number "1")
				)
			)
		)
		(symbol "power:GND"
			(power)
			(pin_numbers hide)
			(pin_names
				(offset 0) hide)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "#PWR"
				(at 0 -6.35 0)
			)
			(property "Value" "GND"
				(at 0 -3.81 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
				(at 0 0 0)
			)
			(property "ki_keywords" "global power"
				(at 0 0 0)
			)
			(symbol "GND_0_1"
				(polyline
					(pts
						(xy 0 0) (xy 0 -1.27) (xy 1.27 -1.27) (xy 0 -2.54) (xy -1.27 -1.27) (xy 0 -1.27)
					)
					(fill
						(type none)
					)
				)
			)
			(symbol "GND_1_1"
				(pin power_in line
					(at 0 0 270)
					(length 0)
					(name "~")
					(number "1")
				)
			)
		)
	)
	(junction
		(at 80.01 66.04)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 73.66 123.19)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 237.49 115.57)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 241.3 71.12)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 252.73 148.59)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 107.95 120.65)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 262.89 50.8)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 62.23 123.19)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 259.08 127)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 129.54 85.09)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 229.87 50.8)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 39.37 66.04)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 129.54 71.12)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 30.48 82.55)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 231.14 71.12)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 250.19 60.96)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 87.63 120.65)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 97.79 120.65)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 43.18 123.19)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 100.33 123.19)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 260.35 71.12)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 250.19 71.12)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 224.79 115.57)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 250.19 50.8)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 116.84 123.19)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 74.93 68.58)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 45.72 120.65)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 64.77 120.65)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 266.7 71.12)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 72.39 120.65)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 236.22 148.59)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 237.49 106.68)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 72.39 113.03)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 63.5 107.95)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 237.49 50.8)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 66.04 68.58)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 63.5 66.04)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 40.64 68.58)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 30.48 66.04)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 139.7 71.12)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 275.59 71.12)
		(diameter 0)
		(color 0 0 0 0)
	)
	(wire
		(pts
			(xy 68.58 69.85) (xy 68.58 74.93)
		)
	)
	(wire
		(pts
			(xy 227.33 115.57) (xy 224.79 115.57)
		)
	)
	(wire
		(pts
			(xy 113.03 140.97) (xy 113.03 147.32)
		)
	)
	(wire
		(pts
			(xy 78.74 127) (xy 83.82 127)
		)
	)
	(wire
		(pts
			(xy 59.69 107.95) (xy 59.69 147.32)
		)
	)
	(wire
		(pts
			(xy 110.49 163.83) (xy 110.49 175.26)
		)
	)
	(wire
		(pts
			(xy 62.23 123.19) (xy 62.23 147.32)
		)
	)
	(wire
		(pts
			(xy 107.95 120.65) (xy 129.54 120.65)
		)
	)
	(wire
		(pts
			(xy 248.92 148.59) (xy 252.73 148.59)
		)
	)
	(wire
		(pts
			(xy 271.78 105.41) (xy 259.08 105.41)
		)
	)
	(wire
		(pts
			(xy 63.5 57.15) (xy 63.5 58.42)
		)
	)
	(wire
		(pts
			(xy 237.49 36.83) (xy 237.49 50.8)
		)
	)
	(wire
		(pts
			(xy 127 142.24) (xy 132.08 142.24)
		)
	)
	(wire
		(pts
			(xy 262.89 50.8) (xy 262.89 95.25)
		)
	)
	(wire
		(pts
			(xy 146.05 45.72) (xy 129.54 45.72)
		)
	)
	(wire
		(pts
			(xy 40.64 147.32) (xy 40.64 105.41)
		)
	)
	(wire
		(pts
			(xy 127 147.32) (xy 127 142.24)
		)
	)
	(wire
		(pts
			(xy 40.64 105.41) (xy 60.96 105.41)
		)
	)
	(wire
		(pts
			(xy 35.56 68.58) (xy 40.64 68.58)
		)
	)
	(wire
		(pts
			(xy 95.25 105.41) (xy 68.58 105.41)
		)
	)
	(wire
		(pts
			(xy 262.89 137.16) (xy 252.73 137.16)
		)
	)
	(wire
		(pts
			(xy 246.38 60.96) (xy 250.19 60.96)
		)
	)
	(wire
		(pts
			(xy 129.54 45.72) (xy 129.54 66.04)
		)
	)
	(wire
		(pts
			(xy 77.47 25.4) (xy 77.47 36.83)
		)
	)
	(wire
		(pts
			(xy 76.2 101.6) (xy 76.2 100.33)
		)
	)
	(wire
		(pts
			(xy 30.48 123.19) (xy 43.18 123.19)
		)
	)
	(wire
		(pts
			(xy 68.58 105.41) (xy 68.58 100.33)
		)
	)
	(wire
		(pts
			(xy 227.33 74.93) (xy 229.87 74.93)
		)
	)
	(wire
		(pts
			(xy 255.27 101.6) (xy 266.7 101.6)
		)
	)
	(wire
		(pts
			(xy 87.63 120.65) (xy 97.79 120.65)
		)
	)
	(wire
		(pts
			(xy 143.51 55.88) (xy 157.48 55.88)
		)
	)
	(wire
		(pts
			(xy 97.79 120.65) (xy 107.95 120.65)
		)
	)
	(wire
		(pts
			(xy 64.77 107.95) (xy 64.77 113.03)
		)
	)
	(wire
		(pts
			(xy 73.66 123.19) (xy 100.33 123.19)
		)
	)
	(wire
		(pts
			(xy 142.24 34.29) (xy 142.24 66.04)
		)
	)
	(wire
		(pts
			(xy 250.19 58.42) (xy 250.19 60.96)
		)
	)
	(wire
		(pts
			(xy 139.7 71.12) (xy 157.48 71.12)
		)
	)
	(wire
		(pts
			(xy 39.37 59.69) (xy 39.37 66.04)
		)
	)
	(wire
		(pts
			(xy 110.49 147.32) (xy 110.49 143.51)
		)
	)
	(wire
		(pts
			(xy 257.81 90.17) (xy 260.35 90.17)
		)
	)
	(wire
		(pts
			(xy 129.54 85.09) (xy 96.52 85.09)
		)
	)
	(wire
		(pts
			(xy 237.49 127) (xy 259.08 127)
		)
	)
	(wire
		(pts
			(xy 60.96 105.41) (xy 60.96 100.33)
		)
	)
	(wire
		(pts
			(xy 77.47 57.15) (xy 77.47 69.85)
		)
	)
	(wire
		(pts
			(xy 252.73 148.59) (xy 255.27 148.59)
		)
	)
	(wire
		(pts
			(xy 96.52 72.39) (xy 73.66 72.39)
		)
	)
	(wire
		(pts
			(xy 144.78 60.96) (xy 144.78 170.18)
		)
	)
	(wire
		(pts
			(xy 275.59 71.12) (xy 275.59 33.02)
		)
	)
	(wire
		(pts
			(xy 110.49 140.97) (xy 113.03 140.97)
		)
	)
	(wire
		(pts
			(xy 189.23 71.12) (xy 231.14 71.12)
		)
	)
	(wire
		(pts
			(xy 147.32 63.5) (xy 157.48 63.5)
		)
	)
	(wire
		(pts
			(xy 59.69 163.83) (xy 59.69 176.53)
		)
	)
	(wire
		(pts
			(xy 259.08 60.96) (xy 250.19 60.96)
		)
	)
	(wire
		(pts
			(xy 110.49 116.84) (xy 110.49 140.97)
		)
	)
	(wire
		(pts
			(xy 250.19 71.12) (xy 260.35 71.12)
		)
	)
	(wire
		(pts
			(xy 96.52 35.56) (xy 147.32 35.56)
		)
	)
	(wire
		(pts
			(xy 266.7 71.12) (xy 275.59 71.12)
		)
	)
	(wire
		(pts
			(xy 66.04 113.03) (xy 72.39 113.03)
		)
	)
	(wire
		(pts
			(xy 237.49 50.8) (xy 250.19 50.8)
		)
	)
	(wire
		(pts
			(xy 71.12 106.68) (xy 71.12 100.33)
		)
	)
	(wire
		(pts
			(xy 189.23 63.5) (xy 246.38 63.5)
		)
	)
	(wire
		(pts
			(xy 36.83 120.65) (xy 45.72 120.65)
		)
	)
	(wire
		(pts
			(xy 142.24 66.04) (xy 157.48 66.04)
		)
	)
	(wire
		(pts
			(xy 71.12 71.12) (xy 88.9 71.12)
		)
	)
	(wire
		(pts
			(xy 189.23 50.8) (xy 229.87 50.8)
		)
	)
	(wire
		(pts
			(xy 30.48 82.55) (xy 30.48 123.19)
		)
	)
	(wire
		(pts
			(xy 45.72 147.32) (xy 45.72 120.65)
		)
	)
	(wire
		(pts
			(xy 224.79 55.88) (xy 224.79 90.17)
		)
	)
	(wire
		(pts
			(xy 106.68 116.84) (xy 110.49 116.84)
		)
	)
	(wire
		(pts
			(xy 147.32 35.56) (xy 147.32 63.5)
		)
	)
	(wire
		(pts
			(xy 110.49 175.26) (xy 149.86 175.26)
		)
	)
	(wire
		(pts
			(xy 106.68 102.87) (xy 73.66 102.87)
		)
	)
	(wire
		(pts
			(xy 78.74 147.32) (xy 78.74 127)
		)
	)
	(wire
		(pts
			(xy 80.01 66.04) (xy 129.54 66.04)
		)
	)
	(wire
		(pts
			(xy 274.32 50.8) (xy 274.32 38.1)
		)
	)
	(wire
		(pts
			(xy 96.52 57.15) (xy 96.52 72.39)
		)
	)
	(wire
		(pts
			(xy 251.46 49.53) (xy 259.08 49.53)
		)
	)
	(wire
		(pts
			(xy 92.71 106.68) (xy 71.12 106.68)
		)
	)
	(wire
		(pts
			(xy 35.56 71.12) (xy 35.56 68.58)
		)
	)
	(wire
		(pts
			(xy 236.22 148.59) (xy 241.3 148.59)
		)
	)
	(wire
		(pts
			(xy 134.62 147.32) (xy 134.62 132.08)
		)
	)
	(wire
		(pts
			(xy 261.62 118.11) (xy 261.62 115.57)
		)
	)
	(wire
		(pts
			(xy 275.59 118.11) (xy 261.62 118.11)
		)
	)
	(wire
		(pts
			(xy 116.84 137.16) (xy 114.3 137.16)
		)
	)
	(wire
		(pts
			(xy 250.19 50.8) (xy 262.89 50.8)
		)
	)
	(wire
		(pts
			(xy 259.08 127) (xy 273.05 127)
		)
	)
	(wire
		(pts
			(xy 129.54 68.58) (xy 129.54 71.12)
		)
	)
	(wire
		(pts
			(xy 259.08 134.62) (xy 240.03 134.62)
		)
	)
	(wire
		(pts
			(xy 246.38 63.5) (xy 246.38 60.96)
		)
	)
	(wire
		(pts
			(xy 40.64 168.91) (xy 143.51 168.91)
		)
	)
	(wire
		(pts
			(xy 260.35 71.12) (xy 260.35 90.17)
		)
	)
	(wire
		(pts
			(xy 157.48 53.34) (xy 139.7 53.34)
		)
	)
	(wire
		(pts
			(xy 38.1 104.14) (xy 58.42 104.14)
		)
	)
	(wire
		(pts
			(xy 241.3 71.12) (xy 250.19 71.12)
		)
	)
	(wire
		(pts
			(xy 157.48 50.8) (xy 146.05 50.8)
		)
	)
	(wire
		(pts
			(xy 74.93 68.58) (xy 129.54 68.58)
		)
	)
	(wire
		(pts
			(xy 73.66 102.87) (xy 73.66 100.33)
		)
	)
	(wire
		(pts
			(xy 66.04 57.15) (xy 66.04 68.58)
		)
	)
	(wire
		(pts
			(xy 43.18 123.19) (xy 62.23 123.19)
		)
	)
	(wire
		(pts
			(xy 96.52 36.83) (xy 96.52 35.56)
		)
	)
	(wire
		(pts
			(xy 114.3 137.16) (xy 114.3 116.84)
		)
	)
	(wire
		(pts
			(xy 231.14 85.09) (xy 231.14 106.68)
		)
	)
	(wire
		(pts
			(xy 27.94 59.69) (xy 39.37 59.69)
		)
	)
	(wire
		(pts
			(xy 63.5 66.04) (xy 80.01 66.04)
		)
	)
	(wire
		(pts
			(xy 229.87 50.8) (xy 237.49 50.8)
		)
	)
	(wire
		(pts
			(xy 107.95 143.51) (xy 107.95 120.65)
		)
	)
	(wire
		(pts
			(xy 73.66 21.59) (xy 73.66 36.83)
		)
	)
	(wire
		(pts
			(xy 252.73 137.16) (xy 252.73 148.59)
		)
	)
	(wire
		(pts
			(xy 45.72 120.65) (xy 64.77 120.65)
		)
	)
	(wire
		(pts
			(xy 189.23 60.96) (xy 223.52 60.96)
		)
	)
	(wire
		(pts
			(xy 236.22 144.78) (xy 236.22 148.59)
		)
	)
	(wire
		(pts
			(xy 266.7 38.1) (xy 274.32 38.1)
		)
	)
	(wire
		(pts
			(xy 72.39 113.03) (xy 76.2 113.03)
		)
	)
	(wire
		(pts
			(xy 40.64 163.83) (xy 40.64 168.91)
		)
	)
	(wire
		(pts
			(xy 251.46 35.56) (xy 251.46 49.53)
		)
	)
	(wire
		(pts
			(xy 80.01 36.83) (xy 81.28 36.83)
		)
	)
	(wire
		(pts
			(xy 73.66 72.39) (xy 73.66 74.93)
		)
	)
	(wire
		(pts
			(xy 231.14 71.12) (xy 241.3 71.12)
		)
	)
	(wire
		(pts
			(xy 39.37 66.04) (xy 63.5 66.04)
		)
	)
	(wire
		(pts
			(xy 30.48 66.04) (xy 39.37 66.04)
		)
	)
	(wire
		(pts
			(xy 240.03 58.42) (xy 240.03 101.6)
		)
	)
	(wire
		(pts
			(xy 100.33 123.19) (xy 100.33 147.32)
		)
	)
	(wire
		(pts
			(xy 129.54 71.12) (xy 129.54 85.09)
		)
	)
	(wire
		(pts
			(xy 129.54 71.12) (xy 139.7 71.12)
		)
	)
	(wire
		(pts
			(xy 59.69 107.95) (xy 63.5 107.95)
		)
	)
	(wire
		(pts
			(xy 43.18 123.19) (xy 43.18 147.32)
		)
	)
	(wire
		(pts
			(xy 224.79 99.06) (xy 227.33 99.06)
		)
	)
	(wire
		(pts
			(xy 129.54 147.32) (xy 134.62 147.32)
		)
	)
	(wire
		(pts
			(xy 237.49 137.16) (xy 240.03 137.16)
		)
	)
	(wire
		(pts
			(xy 224.79 115.57) (xy 224.79 99.06)
		)
	)
	(wire
		(pts
			(xy 63.5 100.33) (xy 63.5 107.95)
		)
	)
	(wire
		(pts
			(xy 229.87 74.93) (xy 229.87 50.8)
		)
	)
	(wire
		(pts
			(xy 143.51 55.88) (xy 143.51 168.91)
		)
	)
	(wire
		(pts
			(xy 88.9 34.29) (xy 142.24 34.29)
		)
	)
	(wire
		(pts
			(xy 224.79 148.59) (xy 228.6 148.59)
		)
	)
	(wire
		(pts
			(xy 73.66 123.19) (xy 73.66 147.32)
		)
	)
	(wire
		(pts
			(xy 151.13 68.58) (xy 157.48 68.58)
		)
	)
	(wire
		(pts
			(xy 71.12 71.12) (xy 71.12 74.93)
		)
	)
	(wire
		(pts
			(xy 83.82 127) (xy 83.82 116.84)
		)
	)
	(wire
		(pts
			(xy 106.68 109.22) (xy 106.68 102.87)
		)
	)
	(wire
		(pts
			(xy 129.54 85.09) (xy 129.54 120.65)
		)
	)
	(wire
		(pts
			(xy 146.05 50.8) (xy 146.05 45.72)
		)
	)
	(wire
		(pts
			(xy 110.49 143.51) (xy 107.95 143.51)
		)
	)
	(wire
		(pts
			(xy 237.49 115.57) (xy 237.49 127)
		)
	)
	(wire
		(pts
			(xy 259.08 127) (xy 259.08 134.62)
		)
	)
	(wire
		(pts
			(xy 271.78 115.57) (xy 271.78 105.41)
		)
	)
	(wire
		(pts
			(xy 97.79 120.65) (xy 97.79 147.32)
		)
	)
	(wire
		(pts
			(xy 231.14 106.68) (xy 237.49 106.68)
		)
	)
	(wire
		(pts
			(xy 88.9 36.83) (xy 88.9 34.29)
		)
	)
	(wire
		(pts
			(xy 223.52 95.25) (xy 242.57 95.25)
		)
	)
	(wire
		(pts
			(xy 189.23 68.58) (xy 227.33 68.58)
		)
	)
	(wire
		(pts
			(xy 149.86 175.26) (xy 149.86 58.42)
		)
	)
	(wire
		(pts
			(xy 30.48 82.55) (xy 43.18 82.55)
		)
	)
	(wire
		(pts
			(xy 116.84 123.19) (xy 116.84 132.08)
		)
	)
	(wire
		(pts
			(xy 114.3 109.22) (xy 114.3 101.6)
		)
	)
	(wire
		(pts
			(xy 259.08 105.41) (xy 259.08 127)
		)
	)
	(wire
		(pts
			(xy 275.59 33.02) (xy 266.7 33.02)
		)
	)
	(wire
		(pts
			(xy 273.05 137.16) (xy 273.05 127)
		)
	)
	(wire
		(pts
			(xy 66.04 68.58) (xy 74.93 68.58)
		)
	)
	(wire
		(pts
			(xy 189.23 58.42) (xy 240.03 58.42)
		)
	)
	(wire
		(pts
			(xy 224.79 90.17) (xy 242.57 90.17)
		)
	)
	(wire
		(pts
			(xy 240.03 134.62) (xy 240.03 137.16)
		)
	)
	(wire
		(pts
			(xy 223.52 60.96) (xy 223.52 95.25)
		)
	)
	(wire
		(pts
			(xy 62.23 123.19) (xy 73.66 123.19)
		)
	)
	(wire
		(pts
			(xy 66.04 100.33) (xy 66.04 113.03)
		)
	)
	(wire
		(pts
			(xy 224.79 115.57) (xy 224.79 148.59)
		)
	)
	(wire
		(pts
			(xy 189.23 53.34) (xy 241.3 53.34)
		)
	)
	(wire
		(pts
			(xy 40.64 68.58) (xy 66.04 68.58)
		)
	)
	(wire
		(pts
			(xy 257.81 95.25) (xy 262.89 95.25)
		)
	)
	(wire
		(pts
			(xy 132.08 132.08) (xy 134.62 132.08)
		)
	)
	(wire
		(pts
			(xy 64.77 120.65) (xy 72.39 120.65)
		)
	)
	(wire
		(pts
			(xy 116.84 123.19) (xy 130.81 123.19)
		)
	)
	(wire
		(pts
			(xy 59.69 176.53) (xy 151.13 176.53)
		)
	)
	(wire
		(pts
			(xy 259.08 49.53) (xy 259.08 60.96)
		)
	)
	(wire
		(pts
			(xy 262.89 50.8) (xy 274.32 50.8)
		)
	)
	(wire
		(pts
			(xy 114.3 101.6) (xy 76.2 101.6)
		)
	)
	(wire
		(pts
			(xy 241.3 53.34) (xy 241.3 71.12)
		)
	)
	(wire
		(pts
			(xy 255.27 121.92) (xy 255.27 101.6)
		)
	)
	(wire
		(pts
			(xy 40.64 68.58) (xy 40.64 57.15)
		)
	)
	(wire
		(pts
			(xy 74.93 57.15) (xy 74.93 68.58)
		)
	)
	(wire
		(pts
			(xy 80.01 57.15) (xy 80.01 66.04)
		)
	)
	(wire
		(pts
			(xy 95.25 147.32) (xy 95.25 105.41)
		)
	)
	(wire
		(pts
			(xy 77.47 69.85) (xy 68.58 69.85)
		)
	)
	(wire
		(pts
			(xy 262.89 148.59) (xy 275.59 148.59)
		)
	)
	(wire
		(pts
			(xy 189.23 55.88) (xy 224.79 55.88)
		)
	)
	(wire
		(pts
			(xy 139.7 53.34) (xy 139.7 71.12)
		)
	)
	(wire
		(pts
			(xy 76.2 147.32) (xy 76.2 113.03)
		)
	)
	(wire
		(pts
			(xy 227.33 144.78) (xy 236.22 144.78)
		)
	)
	(wire
		(pts
			(xy 227.33 68.58) (xy 227.33 36.83)
		)
	)
	(wire
		(pts
			(xy 88.9 57.15) (xy 88.9 71.12)
		)
	)
	(wire
		(pts
			(xy 38.1 163.83) (xy 38.1 170.18)
		)
	)
	(wire
		(pts
			(xy 73.66 36.83) (xy 74.93 36.83)
		)
	)
	(wire
		(pts
			(xy 151.13 68.58) (xy 151.13 176.53)
		)
	)
	(wire
		(pts
			(xy 237.49 66.04) (xy 237.49 106.68)
		)
	)
	(wire
		(pts
			(xy 227.33 137.16) (xy 227.33 144.78)
		)
	)
	(wire
		(pts
			(xy 266.7 101.6) (xy 266.7 71.12)
		)
	)
	(wire
		(pts
			(xy 72.39 120.65) (xy 87.63 120.65)
		)
	)
	(wire
		(pts
			(xy 38.1 170.18) (xy 144.78 170.18)
		)
	)
	(wire
		(pts
			(xy 231.14 71.12) (xy 231.14 77.47)
		)
	)
	(wire
		(pts
			(xy 132.08 142.24) (xy 132.08 137.16)
		)
	)
	(wire
		(pts
			(xy 240.03 101.6) (xy 247.65 101.6)
		)
	)
	(wire
		(pts
			(xy 58.42 100.33) (xy 58.42 104.14)
		)
	)
	(wire
		(pts
			(xy 275.59 148.59) (xy 275.59 118.11)
		)
	)
	(wire
		(pts
			(xy 144.78 60.96) (xy 157.48 60.96)
		)
	)
	(wire
		(pts
			(xy 100.33 123.19) (xy 116.84 123.19)
		)
	)
	(wire
		(pts
			(xy 250.19 60.96) (xy 250.19 63.5)
		)
	)
	(wire
		(pts
			(xy 260.35 71.12) (xy 266.7 71.12)
		)
	)
	(wire
		(pts
			(xy 189.23 66.04) (xy 237.49 66.04)
		)
	)
	(wire
		(pts
			(xy 227.33 99.06) (xy 227.33 74.93)
		)
	)
	(wire
		(pts
			(xy 149.86 58.42) (xy 157.48 58.42)
		)
	)
	(wire
		(pts
			(xy 30.48 66.04) (xy 30.48 82.55)
		)
	)
	(wire
		(pts
			(xy 237.49 106.68) (xy 237.49 115.57)
		)
	)
	(wire
		(pts
			(xy 247.65 101.6) (xy 247.65 121.92)
		)
	)
	(wire
		(pts
			(xy 92.71 147.32) (xy 92.71 106.68)
		)
	)
	(wire
		(pts
			(xy 81.28 21.59) (xy 81.28 36.83)
		)
	)
	(wire
		(pts
			(xy 27.94 57.15) (xy 40.64 57.15)
		)
	)
	(wire
		(pts
			(xy 38.1 147.32) (xy 38.1 104.14)
		)
	)
	(wire
		(pts
			(xy 64.77 107.95) (xy 63.5 107.95)
		)
	)
	(rectangle
		(start 186.69 97.79)
		(end 186.69 97.79)
		(fill
			(type none)
		)
	)
	(rectangle
		(start 21.59 49.53)
		(end 138.43 153.67)
		(fill
			(type none)
		)
	)
	(rectangle
		(start 220.98 24.13)
		(end 280.67 154.94)
		(fill
			(type none)
		)
	)
	(text "Control Arduino Carrier Board\n"
		(exclude_from_sim no)
		(at 122.682 51.816 0)
	)
	(text "5       +5V\n    9   GND\n4       Rotary2\n    8   Active-LED\n3       Rotary1\n    7   speed selector\n2       Buttons B1 - B4\n    6   B5 (Stop-button)\n1       GND"
		(exclude_from_sim no)
		(at 156.718 84.836 0)
	)
	(text "Hand-Unit"
		(exclude_from_sim no)
		(at 274.32 27.178 0)
	)
	(symbol
		(lib_id "Device:R_US")
		(at 63.5 62.23 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "R1"
			(at 66.04 60.9599 0)
		)
		(property "Value" "100"
			(at 66.04 63.4999 0)
		)
		(property "Footprint" ""
			(at 64.516 62.484 90)
		)
		(property "Datasheet" "~"
			(at 63.5 62.23 0)
		)
		(property "Description" "Resistor, US symbol"
			(at 63.5 62.23 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "breakout_board"
				(path
					(reference "R1")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Connector:Conn_01x04_Pin")
		(at 40.64 152.4 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "J2"
			(at 33.02 151.765 0)
		)
		(property "Value" "Rotary Encoder"
			(at 40.64 155.956 90)
		)
		(property "Footprint" ""
			(at 40.64 152.4 0)
		)
		(property "Datasheet" "~"
			(at 40.64 152.4 0)
		)
		(property "Description" "Generic connector, single row, 01x04, script generated"
			(at 40.64 152.4 0)
		)
		(pin "4")
		(pin "1")
		(pin "2")
		(pin "3")
		(instances
			(project "breakout_board"
				(path
					(reference "J2")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Connector:Conn_01x04_Pin")
		(at 95.25 152.4 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "J1"
			(at 87.63 151.765 0)
		)
		(property "Value" "4Digit  display"
			(at 95.504 155.956 90)
		)
		(property "Footprint" ""
			(at 95.25 152.4 0)
		)
		(property "Datasheet" "~"
			(at 95.25 152.4 0)
		)
		(property "Description" "Generic connector, single row, 01x04, script generated"
			(at 95.25 152.4 0)
		)
		(pin "4")
		(pin "1")
		(pin "2")
		(pin "3")
		(instances
			(project "breakout_board"
				(path
					(reference "J1")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Analog_Switch:TS3A24159DGSR")
		(at 259.08 35.56 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "U1"
			(at 259.08 26.67 0)
		)
		(property "Value" "TS3A24159DGSR"
			(at 259.08 29.21 0)
		)
		(property "Footprint" "Package_SO:TSSOP-10_3x3mm_P0.5mm"
			(at 260.35 46.99 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ts3a24159.pdf"
			(at 260.35 48.895 0)
		)
		(property "Description" "Dual SPDT 0.3Ω Bidirectional Analog Switch, TSSOP-10"
			(at 259.08 35.56 0)
		)
		(pin "5")
		(pin "8")
		(pin "3")
		(pin "1")
		(pin "6")
		(pin "10")
		(pin "2")
		(pin "4")
		(pin "9")
		(pin "7")
		(instances
			(project "breakout_board"
				(path
					(reference "U1")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Connector:Conn_01x02_Pin")
		(at 110.49 158.75 90)
		(mirror x)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "J18"
			(at 114.3 160.6551 90)
		)
		(property "Value" "~"
			(at 105.918 154.94 90)
		)
		(property "Footprint" ""
			(at 110.49 158.75 0)
		)
		(property "Datasheet" "~"
			(at 110.49 158.75 0)
		)
		(property "Description" "Generic connector, single row, 01x02, script generated"
			(at 110.49 158.75 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "breakout_board"
				(path
					(reference "J18")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Connector:Conn_01x04_Pin")
		(at 95.25 158.75 90)
		(mirror x)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "J17"
			(at 87.63 159.385 0)
		)
		(property "Value" "~"
			(at 95.504 155.194 90)
		)
		(property "Footprint" ""
			(at 95.25 158.75 0)
		)
		(property "Datasheet" "~"
			(at 95.25 158.75 0)
		)
		(property "Description" "Generic connector, single row, 01x04, script generated"
			(at 95.25 158.75 0)
		)
		(pin "4")
		(pin "1")
		(pin "2")
		(pin "3")
		(instances
			(project "breakout_board"
				(path
					(reference "J17")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Connector:DE9_Plug")
		(at 165.1 60.96 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "J12"
			(at 170.18 59.6899 0)
		)
		(property "Value" "Handunit"
			(at 169.418 49.53 0)
		)
		(property "Footprint" ""
			(at 165.1 60.96 0)
		)
		(property "Datasheet" " ~"
			(at 165.1 60.96 0)
		)
		(property "Description" "9-pin male plug pin D-SUB connector"
			(at 165.1 60.96 0)
		)
		(pin "3")
		(pin "7")
		(pin "5")
		(pin "9")
		(pin "2")
		(pin "1")
		(pin "4")
		(pin "6")
		(pin "8")
		(instances
			(project "breakout_board"
				(path
					(reference "J12")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Connector:Conn_01x02_Pin")
		(at 66.04 41.91 270)
		(mirror x)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "J20"
			(at 62.23 40.0049 90)
		)
		(property "Value" "~"
			(at 70.612 49.276 90)
		)
		(property "Footprint" ""
			(at 66.04 41.91 0)
		)
		(property "Datasheet" "~"
			(at 66.04 41.91 0)
		)
		(property "Description" "Generic connector, single row, 01x02, script generated"
			(at 66.04 41.91 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "breakout_board"
				(path
					(reference "J20")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Connector:Conn_01x03_Pin")
		(at 77.47 52.07 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "J9"
			(at 85.09 52.705 0)
		)
		(property "Value" "Spindle Speed Pot"
			(at 77.47 48.26 90)
		)
		(property "Footprint" ""
			(at 77.47 52.07 0)
		)
		(property "Datasheet" "~"
			(at 77.47 52.07 0)
		)
		(property "Description" "Generic connector, single row, 01x03, script generated"
			(at 77.47 52.07 0)
		)
		(pin "1")
		(pin "2")
		(pin "3")
		(instances
			(project "breakout_board"
				(path
					(reference "J9")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:R_US")
		(at 250.19 54.61 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "R2"
			(at 252.73 53.3399 0)
		)
		(property "Value" "1K"
			(at 252.73 55.8799 0)
		)
		(property "Footprint" ""
			(at 251.206 54.864 90)
		)
		(property "Datasheet" "~"
			(at 250.19 54.61 0)
		)
		(property "Description" "Resistor, US symbol"
			(at 250.19 54.61 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "breakout_board"
				(path
					(reference "R2")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 275.59 71.12 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR03"
			(at 275.59 77.47 0)
		)
		(property "Value" "GND"
			(at 275.59 76.2 0)
		)
		(property "Footprint" ""
			(at 275.59 71.12 0)
		)
		(property "Datasheet" ""
			(at 275.59 71.12 0)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 275.59 71.12 0)
		)
		(pin "1")
		(instances
			(project "breakout_board"
				(path
					(reference "#PWR03")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 35.56 71.12 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR02"
			(at 35.56 77.47 0)
		)
		(property "Value" "GND"
			(at 35.56 76.2 0)
		)
		(property "Footprint" ""
			(at 35.56 71.12 0)
		)
		(property "Datasheet" ""
			(at 35.56 71.12 0)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 35.56 71.12 0)
		)
		(pin "1")
		(instances
			(project "breakout_board"
				(path
					(reference "#PWR02")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Connector:Conn_01x02_Pin")
		(at 127 152.4 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "J6"
			(at 130.81 150.4949 90)
		)
		(property "Value" "Speed PWM"
			(at 122.428 156.21 90)
		)
		(property "Footprint" ""
			(at 127 152.4 0)
		)
		(property "Datasheet" "~"
			(at 127 152.4 0)
		)
		(property "Description" "Generic connector, single row, 01x02, script generated"
			(at 127 152.4 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "breakout_board"
				(path
					(reference "J6")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Switch:SW_Push")
		(at 232.41 137.16 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "SW4"
			(at 232.41 129.54 0)
		)
		(property "Value" "SW_Push"
			(at 232.41 132.08 0)
		)
		(property "Footprint" ""
			(at 232.41 132.08 0)
		)
		(property "Datasheet" "~"
			(at 232.41 132.08 0)
		)
		(property "Description" "Push button switch, generic, two pins"
			(at 232.41 137.16 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "breakout_board"
				(path
					(reference "SW4")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Connector:Conn_01x03_Pin")
		(at 76.2 158.75 90)
		(mirror x)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "J16"
			(at 68.58 159.385 0)
		)
		(property "Value" "~"
			(at 76.2 155.194 90)
		)
		(property "Footprint" ""
			(at 76.2 158.75 0)
		)
		(property "Datasheet" "~"
			(at 76.2 158.75 0)
		)
		(property "Description" "Generic connector, single row, 01x03, script generated"
			(at 76.2 158.75 0)
		)
		(pin "1")
		(pin "2")
		(pin "3")
		(instances
			(project "breakout_board"
				(path
					(reference "J16")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:R_US")
		(at 114.3 113.03 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "R7"
			(at 116.84 111.7599 0)
		)
		(property "Value" "100"
			(at 116.84 114.2999 0)
		)
		(property "Footprint" ""
			(at 115.316 113.284 90)
		)
		(property "Datasheet" "~"
			(at 114.3 113.03 0)
		)
		(property "Description" "Resistor, US symbol"
			(at 114.3 113.03 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "breakout_board"
				(path
					(reference "R7")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Connector:Conn_01x02_Pin")
		(at 59.69 158.75 90)
		(mirror x)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "J15"
			(at 63.5 160.6551 90)
		)
		(property "Value" "~"
			(at 55.118 154.94 90)
		)
		(property "Footprint" ""
			(at 59.69 158.75 0)
		)
		(property "Datasheet" "~"
			(at 59.69 158.75 0)
		)
		(property "Description" "Generic connector, single row, 01x02, script generated"
			(at 59.69 158.75 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "breakout_board"
				(path
					(reference "J15")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:R_Potentiometer")
		(at 87.63 116.84 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "RV3"
			(at 88.9001 114.3 0)
		)
		(property "Value" "500, Speed Sensor LED adjust"
			(at 72.898 109.474 90)
		)
		(property "Footprint" ""
			(at 87.63 116.84 0)
		)
		(property "Datasheet" "~"
			(at 87.63 116.84 0)
		)
		(property "Description" "Potentiometer"
			(at 87.63 116.84 0)
		)
		(pin "3")
		(pin "2")
		(pin "1")
		(instances
			(project "breakout_board"
				(path
					(reference "RV3")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Connector:Conn_01x01_Pin")
		(at 88.9 41.91 270)
		(mirror x)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "J22"
			(at 90.17 42.5451 90)
		)
		(property "Value" "~"
			(at 80.264 49.022 90)
		)
		(property "Footprint" ""
			(at 88.9 41.91 0)
		)
		(property "Datasheet" "~"
			(at 88.9 41.91 0)
		)
		(property "Description" "Generic connector, single row, 01x01, script generated"
			(at 88.9 41.91 0)
		)
		(pin "1")
		(instances
			(project "breakout_board"
				(path
					(reference "J22")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:R_US")
		(at 231.14 81.28 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "R11"
			(at 233.68 80.0099 0)
		)
		(property "Value" "5K"
			(at 233.68 82.5499 0)
		)
		(property "Footprint" ""
			(at 230.124 81.026 90)
		)
		(property "Datasheet" "~"
			(at 231.14 81.28 0)
		)
		(property "Description" "Resistor, US symbol"
			(at 231.14 81.28 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "breakout_board"
				(path
					(reference "R11")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:LED")
		(at 251.46 121.92 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "D1"
			(at 253.0475 114.3 0)
		)
		(property "Value" "Active-LED"
			(at 251.714 123.952 0)
		)
		(property "Footprint" ""
			(at 251.46 121.92 0)
		)
		(property "Datasheet" "~"
			(at 251.46 121.92 0)
		)
		(property "Description" "Light emitting diode"
			(at 251.46 121.92 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "breakout_board"
				(path
					(reference "D1")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:R_US")
		(at 250.19 67.31 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "R3"
			(at 252.73 66.0399 0)
		)
		(property "Value" "1K"
			(at 252.73 68.5799 0)
		)
		(property "Footprint" ""
			(at 251.206 67.564 90)
		)
		(property "Datasheet" "~"
			(at 250.19 67.31 0)
		)
		(property "Description" "Resistor, US symbol"
			(at 250.19 67.31 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "breakout_board"
				(path
					(reference "R3")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Connector:Conn_01x02_Pin")
		(at 110.49 152.4 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "J5"
			(at 114.3 150.4949 90)
		)
		(property "Value" "Active LED"
			(at 105.918 156.21 90)
		)
		(property "Footprint" ""
			(at 110.49 152.4 0)
		)
		(property "Datasheet" "~"
			(at 110.49 152.4 0)
		)
		(property "Description" "Generic connector, single row, 01x02, script generated"
			(at 110.49 152.4 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "breakout_board"
				(path
					(reference "J5")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:RotaryEncoder_Switch")
		(at 250.19 92.71 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "SW2"
			(at 250.19 82.55 0)
		)
		(property "Value" "4-Pin Rotary Encoder"
			(at 250.19 85.09 0)
		)
		(property "Footprint" ""
			(at 246.38 88.646 0)
		)
		(property "Datasheet" "~"
			(at 250.19 86.106 0)
		)
		(property "Description" "Rotary encoder, dual channel, incremental quadrate outputs, with switch"
			(at 250.19 92.71 0)
		)
		(pin "C")
		(pin "A")
		(pin "S1")
		(pin "B")
		(pin "S2")
		(instances
			(project "breakout_board"
				(path
					(reference "SW2")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:R_Potentiometer")
		(at 77.47 21.59 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "RV1"
			(at 77.47 15.24 90)
		)
		(property "Value" "Spindle Speed Pot"
			(at 77.47 17.78 90)
		)
		(property "Footprint" ""
			(at 77.47 21.59 0)
		)
		(property "Datasheet" "~"
			(at 77.47 21.59 0)
		)
		(property "Description" "Potentiometer"
			(at 77.47 21.59 0)
		)
		(pin "1")
		(pin "3")
		(pin "2")
		(instances
			(project "breakout_board"
				(path
					(reference "RV1")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Connector:Conn_01x01_Pin")
		(at 96.52 41.91 270)
		(mirror x)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "J23"
			(at 97.79 42.5451 90)
		)
		(property "Value" "~"
			(at 87.884 46.482 90)
		)
		(property "Footprint" ""
			(at 96.52 41.91 0)
		)
		(property "Datasheet" "~"
			(at 96.52 41.91 0)
		)
		(property "Description" "Generic connector, single row, 01x01, script generated"
			(at 96.52 41.91 0)
		)
		(pin "1")
		(instances
			(project "breakout_board"
				(path
					(reference "J23")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Connector:Conn_01x04_Pin")
		(at 40.64 158.75 90)
		(mirror x)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "J14"
			(at 33.02 159.385 0)
		)
		(property "Value" "~"
			(at 40.64 155.194 90)
		)
		(property "Footprint" ""
			(at 40.64 158.75 0)
		)
		(property "Datasheet" "~"
			(at 40.64 158.75 0)
		)
		(property "Description" "Generic connector, single row, 01x04, script generated"
			(at 40.64 158.75 0)
		)
		(pin "4")
		(pin "1")
		(pin "2")
		(pin "3")
		(instances
			(project "breakout_board"
				(path
					(reference "J14")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:R_US")
		(at 232.41 148.59 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "R8"
			(at 232.41 142.24 90)
		)
		(property "Value" "2K"
			(at 232.41 144.78 90)
		)
		(property "Footprint" ""
			(at 232.664 147.574 90)
		)
		(property "Datasheet" "~"
			(at 232.41 148.59 0)
		)
		(property "Description" "Resistor, US symbol"
			(at 232.41 148.59 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "breakout_board"
				(path
					(reference "R8")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Connector:Conn_01x02_Pin")
		(at 66.04 52.07 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "J8"
			(at 62.23 53.9751 90)
		)
		(property "Value" "Power LED"
			(at 70.612 44.704 90)
		)
		(property "Footprint" ""
			(at 66.04 52.07 0)
		)
		(property "Datasheet" "~"
			(at 66.04 52.07 0)
		)
		(property "Description" "Generic connector, single row, 01x02, script generated"
			(at 66.04 52.07 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "breakout_board"
				(path
					(reference "J8")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Switch:SW_Push")
		(at 232.41 115.57 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "SW3"
			(at 232.41 107.95 0)
		)
		(property "Value" "SW_Push"
			(at 232.41 110.49 0)
		)
		(property "Footprint" ""
			(at 232.41 110.49 0)
		)
		(property "Datasheet" "~"
			(at 232.41 110.49 0)
		)
		(property "Description" "Push button switch, generic, two pins"
			(at 232.41 115.57 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "breakout_board"
				(path
					(reference "SW3")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Connector:Conn_01x02_Pin")
		(at 127 158.75 90)
		(mirror x)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "J19"
			(at 130.81 160.6551 90)
		)
		(property "Value" "~"
			(at 122.428 154.94 90)
		)
		(property "Footprint" ""
			(at 127 158.75 0)
		)
		(property "Datasheet" "~"
			(at 127 158.75 0)
		)
		(property "Description" "Generic connector, single row, 01x02, script generated"
			(at 127 158.75 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "breakout_board"
				(path
					(reference "J19")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:+5C")
		(at 30.48 66.04 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR01"
			(at 30.48 69.85 0)
		)
		(property "Value" "+5C"
			(at 30.48 60.96 0)
		)
		(property "Footprint" ""
			(at 30.48 66.04 0)
		)
		(property "Datasheet" ""
			(at 30.48 66.04 0)
		)
		(property "Description" "Power symbol creates a global label with name \"+5C\""
			(at 30.48 66.04 0)
		)
		(pin "1")
		(instances
			(project "breakout_board"
				(path
					(reference "#PWR01")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:R_US")
		(at 64.77 116.84 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "R4"
			(at 67.31 115.5699 0)
		)
		(property "Value" "10K"
			(at 67.31 118.1099 0)
		)
		(property "Footprint" ""
			(at 65.786 117.094 90)
		)
		(property "Datasheet" "~"
			(at 64.77 116.84 0)
		)
		(property "Description" "Resistor, US symbol"
			(at 64.77 116.84 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "breakout_board"
				(path
					(reference "R4")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Connector:Conn_01x02_Pin")
		(at 59.69 152.4 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "J4"
			(at 63.5 150.4949 90)
		)
		(property "Value" "Stop Button"
			(at 55.118 156.21 90)
		)
		(property "Footprint" ""
			(at 59.69 152.4 0)
		)
		(property "Datasheet" "~"
			(at 59.69 152.4 0)
		)
		(property "Description" "Generic connector, single row, 01x02, script generated"
			(at 59.69 152.4 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "breakout_board"
				(path
					(reference "J4")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Switch:SW_Push")
		(at 267.97 137.16 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "SW6"
			(at 267.97 129.54 0)
		)
		(property "Value" "SW_Push"
			(at 267.97 132.08 0)
		)
		(property "Footprint" ""
			(at 267.97 132.08 0)
		)
		(property "Datasheet" "~"
			(at 267.97 132.08 0)
		)
		(property "Description" "Push button switch, generic, two pins"
			(at 267.97 137.16 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "breakout_board"
				(path
					(reference "SW6")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Connector:DE9_Plug")
		(at 181.61 60.96 0)
		(mirror y)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "J13"
			(at 181.61 43.18 0)
		)
		(property "Value" "Cable"
			(at 173.228 52.324 0)
		)
		(property "Footprint" ""
			(at 181.61 60.96 0)
		)
		(property "Datasheet" " ~"
			(at 181.61 60.96 0)
		)
		(property "Description" "9-pin male plug pin D-SUB connector"
			(at 181.61 60.96 0)
		)
		(pin "3")
		(pin "7")
		(pin "5")
		(pin "9")
		(pin "2")
		(pin "1")
		(pin "4")
		(pin "6")
		(pin "8")
		(instances
			(project "breakout_board"
				(path
					(reference "J13")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:R_US")
		(at 106.68 113.03 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "R6"
			(at 109.22 111.7599 0)
		)
		(property "Value" "100"
			(at 109.22 114.2999 0)
		)
		(property "Footprint" ""
			(at 107.696 113.284 90)
		)
		(property "Datasheet" "~"
			(at 106.68 113.03 0)
		)
		(property "Description" "Resistor, US symbol"
			(at 106.68 113.03 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "breakout_board"
				(path
					(reference "R6")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Isolator:ACPL-214-500E")
		(at 124.46 134.62 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "U2"
			(at 124.46 125.73 0)
		)
		(property "Value" "ACPL-214-500E"
			(at 124.46 128.27 0)
		)
		(property "Footprint" "Package_SO:SOP-4_4.4x2.6mm_P1.27mm"
			(at 102.87 139.7 0)
		)
		(property "Datasheet" "https://docs.broadcom.com/doc/AV02-0469EN"
			(at 125.095 134.62 0)
		)
		(property "Description" "AC/DC Phototransistor Optocoupler, Vce 80V, CTR 20-400%, SOP-4"
			(at 124.46 134.62 0)
		)
		(pin "2")
		(pin "1")
		(pin "3")
		(pin "4")
		(instances
			(project "breakout_board"
				(path
					(reference "U2")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "MCU_Module:Arduino_UNO_R3")
		(at 68.58 87.63 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "A1"
			(at 40.64 80.3559 0)
		)
		(property "Value" "Control Arduino"
			(at 61.468 87.884 90)
		)
		(property "Footprint" "Module:Arduino_UNO_R3"
			(at 68.58 87.63 0)
		)
		(property "Datasheet" "https://www.arduino.cc/en/Main/arduinoBoardUno"
			(at 68.58 87.63 0)
		)
		(property "Description" "Arduino UNO Microcontroller Module, release 3"
			(at 68.58 87.63 0)
		)
		(pin "1")
		(pin "15")
		(pin "2")
		(pin "8")
		(pin "29")
		(pin "9")
		(pin "32")
		(pin "4")
		(pin "31")
		(pin "23")
		(pin "12")
		(pin "18")
		(pin "13")
		(pin "16")
		(pin "19")
		(pin "21")
		(pin "14")
		(pin "22")
		(pin "3")
		(pin "24")
		(pin "27")
		(pin "11")
		(pin "28")
		(pin "5")
		(pin "7")
		(pin "26")
		(pin "25")
		(pin "20")
		(pin "10")
		(pin "17")
		(pin "30")
		(pin "6")
		(instances
			(project "breakout_board"
				(path
					(reference "A1")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Connector:Conn_01x03_Pin")
		(at 76.2 152.4 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "J3"
			(at 68.58 151.765 0)
		)
		(property "Value" "Speed Sensor"
			(at 76.2 155.956 90)
		)
		(property "Footprint" ""
			(at 76.2 152.4 0)
		)
		(property "Datasheet" "~"
			(at 76.2 152.4 0)
		)
		(property "Description" "Generic connector, single row, 01x03, script generated"
			(at 76.2 152.4 0)
		)
		(pin "1")
		(pin "2")
		(pin "3")
		(instances
			(project "breakout_board"
				(path
					(reference "J3")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:R_US")
		(at 72.39 116.84 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "R5"
			(at 74.93 115.5699 0)
		)
		(property "Value" "10K"
			(at 74.93 118.1099 0)
		)
		(property "Footprint" ""
			(at 73.406 117.094 90)
		)
		(property "Datasheet" "~"
			(at 72.39 116.84 0)
		)
		(property "Description" "Resistor, US symbol"
			(at 72.39 116.84 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "breakout_board"
				(path
					(reference "R5")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:R_US")
		(at 259.08 148.59 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "R10"
			(at 259.08 142.24 90)
		)
		(property "Value" "2K"
			(at 259.08 144.78 90)
		)
		(property "Footprint" ""
			(at 259.334 147.574 90)
		)
		(property "Datasheet" "~"
			(at 259.08 148.59 0)
		)
		(property "Description" "Resistor, US symbol"
			(at 259.08 148.59 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "breakout_board"
				(path
					(reference "R10")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Switch:SW_Push")
		(at 266.7 115.57 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "SW5"
			(at 266.7 107.95 0)
		)
		(property "Value" "SW_Push"
			(at 266.7 110.49 0)
		)
		(property "Footprint" ""
			(at 266.7 110.49 0)
		)
		(property "Datasheet" "~"
			(at 266.7 110.49 0)
		)
		(property "Description" "Push button switch, generic, two pins"
			(at 266.7 115.57 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "breakout_board"
				(path
					(reference "SW5")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Connector:Conn_01x01_Pin")
		(at 96.52 52.07 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "J11"
			(at 97.79 51.4349 90)
		)
		(property "Value" "Handunit-Speedswitch"
			(at 87.884 47.498 90)
		)
		(property "Footprint" ""
			(at 96.52 52.07 0)
		)
		(property "Datasheet" "~"
			(at 96.52 52.07 0)
		)
		(property "Description" "Generic connector, single row, 01x01, script generated"
			(at 96.52 52.07 0)
		)
		(pin "1")
		(instances
			(project "breakout_board"
				(path
					(reference "J11")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Switch:SW_Push")
		(at 232.41 36.83 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "SW1"
			(at 232.41 29.21 0)
		)
		(property "Value" "SW_Push"
			(at 232.41 31.75 0)
		)
		(property "Footprint" ""
			(at 232.41 31.75 0)
		)
		(property "Datasheet" "~"
			(at 232.41 31.75 0)
		)
		(property "Description" "Push button switch, generic, two pins"
			(at 232.41 36.83 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "breakout_board"
				(path
					(reference "SW1")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Connector:Conn_01x02_Pin")
		(at 22.86 57.15 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "J7"
			(at 24.7651 60.96 90)
		)
		(property "Value" "5V Power In"
			(at 19.05 52.578 90)
		)
		(property "Footprint" ""
			(at 22.86 57.15 0)
		)
		(property "Datasheet" "~"
			(at 22.86 57.15 0)
		)
		(property "Description" "Generic connector, single row, 01x02, script generated"
			(at 22.86 57.15 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "breakout_board"
				(path
					(reference "J7")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Connector:Conn_01x01_Pin")
		(at 88.9 52.07 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "J10"
			(at 90.17 51.4349 90)
		)
		(property "Value" "Handunit-Buttons"
			(at 80.264 44.958 90)
		)
		(property "Footprint" ""
			(at 88.9 52.07 0)
		)
		(property "Datasheet" "~"
			(at 88.9 52.07 0)
		)
		(property "Description" "Generic connector, single row, 01x01, script generated"
			(at 88.9 52.07 0)
		)
		(pin "1")
		(instances
			(project "breakout_board"
				(path
					(reference "J10")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:R_US")
		(at 245.11 148.59 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "R9"
			(at 245.11 142.24 90)
		)
		(property "Value" "2K"
			(at 245.11 144.78 90)
		)
		(property "Footprint" ""
			(at 245.364 147.574 90)
		)
		(property "Datasheet" "~"
			(at 245.11 148.59 0)
		)
		(property "Description" "Resistor, US symbol"
			(at 245.11 148.59 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "breakout_board"
				(path
					(reference "R9")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Connector:Conn_01x03_Pin")
		(at 77.47 41.91 270)
		(mirror x)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "J21"
			(at 85.09 41.275 0)
		)
		(property "Value" "~"
			(at 77.47 45.72 90)
		)
		(property "Footprint" ""
			(at 77.47 41.91 0)
		)
		(property "Datasheet" "~"
			(at 77.47 41.91 0)
		)
		(property "Description" "Generic connector, single row, 01x03, script generated"
			(at 77.47 41.91 0)
		)
		(pin "1")
		(pin "2")
		(pin "3")
		(instances
			(project "breakout_board"
				(path
					(reference "J21")
					(unit 1)
				)
			)
		)
	)
	(sheet_instances
		(path
			(page "1")
		)
	)
)
