(kicad_pcb (version 20221018) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A5")
  (title_block
    (title "7-Seg")
    (date "2023-09-11")
    (rev "1")
    (comment 1 "© 2023. This work is licensed under a CC BY-NC-SA 4.0 License")
  )
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0)
    (grid_origin 106.15 70.39)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (plot_on_all_layers_selection 0x0000000_00000000)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (dashed_line_dash_ratio 12.000000)
      (dashed_line_gap_ratio 3.000000)
      (svgprecision 4)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "Net-(J1-Pin_1)")
  (net 2 "VCC")
  (net 3 "Net-(J1-Pin_3)")
  (net 4 "Net-(J1-Pin_4)")
  (net 5 "Net-(J1-Pin_5)")
  (net 6 "Net-(J1-Pin_6)")
  (net 7 "Net-(J1-Pin_7)")
  (net 8 "GND")
  (net 9 "Net-(U1-OUT0)")
  (net 10 "Net-(U1-OUT1)")
  (net 11 "Net-(U1-OUT2)")
  (net 12 "Net-(U1-OUT3)")
  (net 13 "Net-(U1-OUT4)")
  (net 14 "Net-(U1-OUT5)")
  (net 15 "Net-(U1-OUT6)")
  (net 16 "Net-(U1-OUT7)")
  (net 17 "Net-(U1-R-EXT)")
  (net 18 "unconnected-(J1-Pin_8-Pad8)")
  (footprint "Fuse:Fuse_0603_1608Metric" (layer "F.Cu")
    (at 96.25 62.39)
    (descr "Fuse SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "fuse")
    (property "Sheetfile" "bottom-board-single-7-seg.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resettable fuse, polymeric positive temperature coefficient, small symbol")
    (property "ki_keywords" "resettable fuse PTC PPTC polyfuse polyswitch")
    (attr smd)
    (fp_text reference "F1" (at -2.3 -0.1) (layer "F.SilkS"))
    (fp_text value "Polyfuse_Small" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "Net-(J1-Pin_1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "VCC") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Fuse.3dshapes/Fuse_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Global_MWS:PinHeader_1x07_P2.54mm_Vertical_center_origin" (layer "F.Cu")
    (at 104.15 58.89 90)
    (descr "Through hole straight pin header, 1x07, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x07 2.54mm single row")
    (property "Sheetfile" "bottom-board-single-7-seg.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x07, script generated")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J3" (at 0 -9.95 90) (layer "F.SilkS"))
    (fp_text value "Conn_01x07_Pin" (at 0 9.95 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 -7.62 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 1 "Net-(J1-Pin_1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 -5.08 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 8 "GND") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 -2.54 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 3 "Net-(J1-Pin_3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 0 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 4 "Net-(J1-Pin_4)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 5 "Net-(J1-Pin_5)") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 6 "Net-(J1-Pin_6)") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 7 "Net-(J1-Pin_7)") (pinfunction "Pin_7") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x07_P2.54mm_Vertical.wrl"
      (offset (xyz 0 7.62 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Global_MWS:JST_BM08B-SRSS-TB(LF)(SN)" (layer "F.Cu")
    (at 118.325 70.39 -90)
    (property "Sheetfile" "bottom-board-single-7-seg.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x08, script generated")
    (property "ki_keywords" "connector")
    (attr smd)
    (fp_text reference "J1" (at -6.75 0.775 90) (layer "F.SilkS"))
    (fp_text value "Conn_01x08_Pin" (at 10.225 5.185 90) (layer "F.Fab"))
    (pad "1" smd rect (at -3.5 2.525 270) (size 0.6 1.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "Net-(J1-Pin_1)") (pinfunction "Pin_1") (pintype "passive") (solder_mask_margin 0.102))
    (pad "2" smd rect (at -2.5 2.525 270) (size 0.6 1.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 8 "GND") (pinfunction "Pin_2") (pintype "passive") (solder_mask_margin 0.102))
    (pad "3" smd rect (at -1.5 2.525 270) (size 0.6 1.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "Net-(J1-Pin_3)") (pinfunction "Pin_3") (pintype "passive") (solder_mask_margin 0.102))
    (pad "4" smd rect (at -0.5 2.525 270) (size 0.6 1.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "Net-(J1-Pin_4)") (pinfunction "Pin_4") (pintype "passive") (solder_mask_margin 0.102))
    (pad "5" smd rect (at 0.5 2.525 270) (size 0.6 1.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "Net-(J1-Pin_5)") (pinfunction "Pin_5") (pintype "passive") (solder_mask_margin 0.102))
    (pad "6" smd rect (at 1.5 2.525 270) (size 0.6 1.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 6 "Net-(J1-Pin_6)") (pinfunction "Pin_6") (pintype "passive") (solder_mask_margin 0.102))
    (pad "7" smd rect (at 2.5 2.525 270) (size 0.6 1.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 7 "Net-(J1-Pin_7)") (pinfunction "Pin_7") (pintype "passive") (solder_mask_margin 0.102))
    (pad "8" smd rect (at 3.5 2.525 270) (size 0.6 1.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 18 "unconnected-(J1-Pin_8-Pad8)") (pinfunction "Pin_8") (pintype "passive+no_connect") (solder_mask_margin 0.102))
    (pad "S1" smd rect (at -4.8 0 270) (size 1.2 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (solder_mask_margin 0.102))
    (pad "S2" smd rect (at 4.8 0 270) (size 1.2 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (solder_mask_margin 0.102))
    (model "$MY3DMOD/BM08B-SRSS-TB_LF__SN_.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 180))
    )
  )
  (footprint "Global_MWS:disp-7seg-single-liteon-lts-4301JS" (layer "F.Cu")
    (at 106.15 70.39)
    (property "Sheetfile" "bottom-board-single-7-seg.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U2" (at -0.55 -7.6 unlocked) (layer "F.SilkS"))
    (fp_text value "~" (at 0 7.62 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 9.5 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole roundrect (at -3.81 -5.08) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.25)
      (net 15 "Net-(U1-OUT6)") (pinfunction "G") (pintype "input"))
    (pad "2" thru_hole circle (at -3.81 -2.54) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 14 "Net-(U1-OUT5)") (pinfunction "F") (pintype "input"))
    (pad "3" thru_hole circle (at -3.81 0) (size 1.7 1.7) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 2 "VCC") (pinfunction "CA") (pintype "input"))
    (pad "4" thru_hole circle (at -3.81 2.54) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 13 "Net-(U1-OUT4)") (pinfunction "E") (pintype "input"))
    (pad "5" thru_hole circle (at -3.81 5.08) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 12 "Net-(U1-OUT3)") (pinfunction "D") (pintype "input"))
    (pad "6" thru_hole circle (at 3.81 5.08) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 16 "Net-(U1-OUT7)") (pinfunction "DP") (pintype "input"))
    (pad "7" thru_hole circle (at 3.81 2.54) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 11 "Net-(U1-OUT2)") (pinfunction "C") (pintype "input"))
    (pad "8" thru_hole circle (at 3.81 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 2 "VCC") (pinfunction "CA") (pintype "input"))
    (pad "9" thru_hole circle (at 3.81 -2.54) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 10 "Net-(U1-OUT1)") (pinfunction "B") (pintype "input"))
    (pad "10" thru_hole circle (at 3.81 -5.08) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 9 "Net-(U1-OUT0)") (pinfunction "A") (pintype "input"))
    (model "${MY3DMOD}/LTS-4301JS.stp"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_SO:SOIC-16_3.9x9.9mm_P1.27mm" (layer "F.Cu")
    (at 96.625 70.135)
    (descr "SOIC, 16 Pin (JEDEC MS-012AC, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_16.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (property "Sheetfile" "bottom-board-single-7-seg.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "8-bit constant current LED sink driver, HTSSOP-16")
    (property "ki_keywords" "Shift Register LED driver 8 bit")
    (attr smd)
    (fp_text reference "U1" (at 0.1 6.03) (layer "F.SilkS"))
    (fp_text value "STP08CP05XT" (at 0 5.9) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.475 -4.445) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 8 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "2" smd roundrect (at -2.475 -3.175) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "Net-(J1-Pin_3)") (pinfunction "SDI") (pintype "input"))
    (pad "3" smd roundrect (at -2.475 -1.905) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "Net-(J1-Pin_4)") (pinfunction "CLK") (pintype "input"))
    (pad "4" smd roundrect (at -2.475 -0.635) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "Net-(J1-Pin_5)") (pinfunction "LE") (pintype "input"))
    (pad "5" smd roundrect (at -2.475 0.635) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 9 "Net-(U1-OUT0)") (pinfunction "OUT0") (pintype "output"))
    (pad "6" smd roundrect (at -2.475 1.905) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 10 "Net-(U1-OUT1)") (pinfunction "OUT1") (pintype "output"))
    (pad "7" smd roundrect (at -2.475 3.175) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 11 "Net-(U1-OUT2)") (pinfunction "OUT2") (pintype "output"))
    (pad "8" smd roundrect (at -2.475 4.445) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 12 "Net-(U1-OUT3)") (pinfunction "OUT3") (pintype "output"))
    (pad "9" smd roundrect (at 2.475 4.445) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 13 "Net-(U1-OUT4)") (pinfunction "OUT4") (pintype "output"))
    (pad "10" smd roundrect (at 2.475 3.175) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 14 "Net-(U1-OUT5)") (pinfunction "OUT5") (pintype "output"))
    (pad "11" smd roundrect (at 2.475 1.905) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 15 "Net-(U1-OUT6)") (pinfunction "OUT6") (pintype "output"))
    (pad "12" smd roundrect (at 2.475 0.635) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 16 "Net-(U1-OUT7)") (pinfunction "OUT7") (pintype "output"))
    (pad "13" smd roundrect (at 2.475 -0.635) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 6 "Net-(J1-Pin_6)") (pinfunction "~{OE}") (pintype "input"))
    (pad "14" smd roundrect (at 2.475 -1.905) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 7 "Net-(J1-Pin_7)") (pinfunction "SDO") (pintype "output"))
    (pad "15" smd roundrect (at 2.475 -3.175) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 17 "Net-(U1-R-EXT)") (pinfunction "R-EXT") (pintype "passive"))
    (pad "16" smd roundrect (at 2.475 -4.445) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "VCC") (pinfunction "VDD") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-16_3.9x9.9mm_P1.27mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (at 96.275 63.94)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "bottom-board-single-7-seg.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C1" (at -2.525 0) (layer "F.SilkS"))
    (fp_text value "1u" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.775 0) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 8 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "VCC") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Global_MWS:logo_for_pcb_10mm" (layer "F.Cu")
    (at 140.075 109.95)
    (property "Sheetfile" "bottom-board-single-7-seg.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "SYM1" (at -1.275 2.775) (layer "F.SilkS") hide)
    (fp_text value "MWS_Logo" (at 4.4 2.75) (layer "F.SilkS") hide)
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (at 98.85 63.115 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "bottom-board-single-7-seg.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, small US symbol")
    (property "ki_keywords" "r resistor")
    (attr smd)
    (fp_text reference "R10" (at -0.3 1.45 90) (layer "F.SilkS"))
    (fp_text value "R_Small_US" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 90) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 17 "Net-(U1-R-EXT)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 90) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 8 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_2.7mm_M2.5" (layer "F.Cu")
    (at 117.65 81.89)
    (descr "Mounting Hole 2.7mm, no annular, M2.5")
    (tags "mounting hole 2.7mm no annular m2.5")
    (property "Sheetfile" "bottom-board-single-7-seg.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole without connection")
    (property "ki_keywords" "mounting hole")
    (attr exclude_from_pos_files)
    (fp_text reference "H1" (at 0 -3.7) (layer "F.SilkS") hide)
    (fp_text value "MountingHole" (at 0 3.7) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -3.7) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 2.7 2.7) (drill 2.7) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Global_MWS:logo_for_pcb_10mm" (layer "B.Cu")
    (at 140.075 109.95 180)
    (property "Sheetfile" "bottom-board-single-7-seg.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "SYM2" (at -1.275 -2.775) (layer "B.SilkS") hide)
    (fp_text value "MWS_Logo" (at 4.4 -2.75) (layer "B.SilkS") hide)
  )
  (gr_line (start 119.425 84.665) (end 98.15 84.665)
    (layer "Edge.Cuts"))
  (gr_line (start 91.875 78.14) (end 91.875 57.115)
    (layer "Edge.Cuts"))
  (gr_arc (start 102.65 56.115) (mid 101.65 57.115) (end 100.65 56.115)
    (layer "Edge.Cuts"))
  (gr_arc (start 115.9 62.39) (mid 114.485786 61.804214) (end 113.9 60.39)
    (layer "Edge.Cuts"))
  (gr_line (start 120.425 62.39) (end 120.425 83.665)
    (layer "Edge.Cuts"))
  (gr_arc (start 120.425 83.665) (mid 120.132107 84.372107) (end 119.425 84.665)
    (layer "Edge.Cuts"))
  (gr_arc (start 96.15 78.14) (mid 97.564214 78.725786) (end 98.15 80.14)
    (layer "Edge.Cuts"))
  (gr_line (start 113.9 56.115) (end 113.9 60.39)
    (layer "Edge.Cuts"))
  (gr_line (start 92.875 56.115) (end 93.65 56.115)
    (layer "Edge.Cuts"))
  (gr_line (start 96.15 78.14) (end 91.875 78.14)
    (layer "Edge.Cuts"))
  (gr_line (start 98.15 84.665) (end 98.15 80.14)
    (layer "Edge.Cuts"))
  (gr_line (start 102.65 56.115) (end 113.9 56.115)
    (layer "Edge.Cuts"))
  (gr_line (start 100.65 56.115) (end 100.65 54.715)
    (layer "Edge.Cuts"))
  (gr_line (start 115.9 62.39) (end 120.425 62.39)
    (layer "Edge.Cuts"))
  (gr_arc (start 95.65 56.115) (mid 94.65 57.115) (end 93.65 56.115)
    (layer "Edge.Cuts"))
  (gr_line (start 95.65 54.715) (end 95.65 56.115)
    (layer "Edge.Cuts"))
  (gr_arc (start 91.875 57.115) (mid 92.167893 56.407893) (end 92.875 56.115)
    (layer "Edge.Cuts"))
  (gr_line (start 100.65 54.715) (end 95.65 54.715)
    (layer "Edge.Cuts"))
  (gr_text "PN: 1760003" (at 144.675 113.025) (layer "B.SilkS"))
  (gr_text "© Milky Way Systems, 2023" (at 152.6 93.025 90) (layer "B.SilkS"))
  (gr_text "PN: 1760003" (at 134.575 113.025) (layer "F.SilkS"))
  (gr_text "© Milky Way Systems, 2023" (at 146.725 105.95 90) (layer "F.SilkS"))
  (zone (net 15) (net_name "Net-(U1-OUT6)") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30047)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 100.507439 72.159737)
        (xy 100.224598 71.876896)
        (xy 99.982403 71.751418)
        (xy 99.099293 72.040707)
        (xy 99.987687 72.32505)
      )
    )
  )
  (zone (net 10) (net_name "Net-(U1-OUT1)") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30032)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 95.425 72.24)
        (xy 95.425 71.84)
        (xy 95.032403 71.751418)
        (xy 94.149 72.04)
        (xy 95.032403 72.328582)
      )
    )
  )
  (zone (net 2) (net_name "VCC") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30038)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 103.35 62.715)
        (xy 103.35 63.115)
        (xy 103.996927 63.284552)
        (xy 104.151 62.915)
        (xy 103.996927 62.545448)
      )
    )
  )
  (zone (net 11) (net_name "Net-(U1-OUT2)") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30008)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 108.970051 71.657209)
        (xy 108.687209 71.940051)
        (xy 109.220896 73.236147)
        (xy 109.960707 72.930707)
        (xy 110.266147 72.190896)
      )
    )
  )
  (zone (net 3) (net_name "Net-(J1-Pin_3)") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30022)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 92.875 66.71)
        (xy 92.875 67.21)
        (xy 93.325 67.26)
        (xy 94.151 66.96)
        (xy 93.325 66.66)
      )
    )
  )
  (zone (net 2) (net_name "VCC") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30016)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 96.7875 63.3025)
        (xy 97.2875 63.3025)
        (xy 97.458349 62.729962)
        (xy 97.0375 62.389)
        (xy 96.616651 62.729962)
      )
    )
  )
  (zone (net 13) (net_name "Net-(U1-OUT4)") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30011)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 100.84036 73.391798)
        (xy 101.123202 73.67464)
        (xy 102.34 73.73)
        (xy 102.340707 72.929293)
        (xy 101.774315 72.364315)
      )
    )
  )
  (zone (net 8) (net_name "GND") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30024)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 93.875 64.833093)
        (xy 94.375 64.833093)
        (xy 94.579552 64.203073)
        (xy 94.21 64.049)
        (xy 93.81 64.05)
      )
    )
  )
  (zone (net 8) (net_name "GND") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30017)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 99.362883 63.085726)
        (xy 99.645726 62.802883)
        (xy 99.325 62.199314)
        (xy 98.849293 62.289293)
        (xy 98.684315 62.69)
      )
    )
  )
  (zone (net 15) (net_name "Net-(U1-OUT6)") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30052)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 99.98561 71.84)
        (xy 99.98561 72.24)
        (xy 100.656364 72.127971)
        (xy 100.657364 71.727971)
        (xy 100.373521 71.445128)
      )
    )
  )
  (zone (net 15) (net_name "Net-(U1-OUT6)") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30036)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 104.725 70.94)
        (xy 104.325 70.94)
        (xy 104.155448 71.586927)
        (xy 104.525 71.741)
        (xy 104.894552 71.586927)
      )
    )
  )
  (zone (net 3) (net_name "Net-(J1-Pin_3)") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30023)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 93.546022 67.21)
        (xy 93.546022 66.71)
        (xy 92.903073 66.570448)
        (xy 92.749 66.94)
        (xy 92.75 67.34)
      )
    )
  )
  (zone (net 7) (net_name "Net-(J1-Pin_7)") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30049)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 114.725 72.69)
        (xy 114.725 73.09)
        (xy 115.025 73.19)
        (xy 115.801 72.89)
        (xy 115.025 72.59)
      )
    )
  )
  (zone (net 5) (net_name "Net-(J1-Pin_5)") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30040)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 93.575 69.69)
        (xy 93.575 69.29)
        (xy 92.928073 69.120448)
        (xy 92.774 69.49)
        (xy 92.928073 69.859552)
      )
    )
  )
  (zone (net 2) (net_name "VCC") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30019)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 97.2375 61.4775)
        (xy 96.8375 61.4775)
        (xy 96.616651 62.050038)
        (xy 97.0375 62.391)
        (xy 97.458349 62.050038)
      )
    )
  )
  (zone (net 5) (net_name "Net-(J1-Pin_5)") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30033)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 92.875 69.29)
        (xy 92.875 69.69)
        (xy 93.267597 69.788582)
        (xy 94.151 69.5)
        (xy 93.267597 69.211418)
      )
    )
  )
  (zone (net 14) (net_name "Net-(U1-OUT5)") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30053)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 100.466629 73.331213)
        (xy 100.183787 73.048371)
        (xy 99.925 73.01)
        (xy 99.099293 73.310707)
        (xy 100.063653 73.517045)
      )
    )
  )
  (zone (net 9) (net_name "Net-(U1-OUT0)") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30030)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 95.425 70.97)
        (xy 95.425 70.57)
        (xy 95.032403 70.481418)
        (xy 94.149 70.77)
        (xy 95.032403 71.058582)
      )
    )
  )
  (zone (net 8) (net_name "GND") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30002)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 98.82 60.59)
        (xy 99.32 60.59)
        (xy 99.855298 59.215281)
        (xy 99.07 58.889)
        (xy 98.284702 59.215281)
      )
    )
  )
  (zone (net 12) (net_name "Net-(U1-OUT3)") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30057)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 93.95 75.18)
        (xy 94.35 75.18)
        (xy 94.45 74.88)
        (xy 94.15 74.579)
        (xy 93.85 74.88)
      )
    )
  )
  (zone (net 8) (net_name "GND") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30048)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 114.725 67.69)
        (xy 114.725 68.09)
        (xy 115.025 68.19)
        (xy 115.801 67.89)
        (xy 115.025 67.59)
      )
    )
  )
  (zone (net 4) (net_name "Net-(J1-Pin_4)") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30003)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 105.21066 60.233503)
        (xy 105.493503 59.95066)
        (xy 104.935298 58.564719)
        (xy 104.149293 58.889293)
        (xy 103.824719 59.675298)
      )
    )
  )
  (zone (net 7) (net_name "Net-(J1-Pin_7)") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30029)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 100.375 68.43)
        (xy 100.375 68.03)
        (xy 99.982403 67.941418)
        (xy 99.099 68.23)
        (xy 99.982403 68.518582)
      )
    )
  )
  (zone (net 7) (net_name "Net-(J1-Pin_7)") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30046)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 99.852984 68.03)
        (xy 99.852984 68.43)
        (xy 100.496927 68.584552)
        (xy 100.651 68.215)
        (xy 100.496927 67.845448)
      )
    )
  )
  (zone (net 4) (net_name "Net-(J1-Pin_4)") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30028)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 92.875 68.04)
        (xy 92.875 68.44)
        (xy 93.267597 68.518582)
        (xy 94.151 68.23)
        (xy 93.267597 67.941418)
      )
    )
  )
  (zone (net 4) (net_name "Net-(J1-Pin_4)") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30042)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 93.525 68.44)
        (xy 93.525 68.04)
        (xy 92.878073 67.870448)
        (xy 92.724 68.24)
        (xy 92.878073 68.609552)
      )
    )
  )
  (zone (net 8) (net_name "GND") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30056)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 94.375 65.09)
        (xy 93.875 65.09)
        (xy 93.83722 65.39)
        (xy 94.15 65.691)
        (xy 94.437739 65.39)
      )
    )
  )
  (zone (net 5) (net_name "Net-(J1-Pin_5)") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30034)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 113.65 75.085099)
        (xy 113.25 75.085099)
        (xy 113.225 75.84)
        (xy 113.625 75.841)
        (xy 113.994552 75.686927)
      )
    )
  )
  (zone (net 6) (net_name "Net-(J1-Pin_6)") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30054)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 114.725 71.765)
        (xy 114.725 72.165)
        (xy 115.025 72.19)
        (xy 115.801 71.89)
        (xy 115.025 71.643361)
      )
    )
  )
  (zone (net 2) (net_name "VCC") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30039)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 96.8375 62.1275)
        (xy 97.2375 62.1275)
        (xy 97.407052 61.480573)
        (xy 97.0375 61.3265)
        (xy 96.667948 61.480573)
      )
    )
  )
  (zone (net 1) (net_name "Net-(J1-Pin_1)") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30015)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 95.7125 61.4775)
        (xy 95.2125 61.4775)
        (xy 95.041651 62.050038)
        (xy 95.4625 62.391)
        (xy 95.883349 62.050038)
      )
    )
  )
  (zone (net 16) (net_name "Net-(U1-OUT7)") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30010)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 108.970051 74.197209)
        (xy 108.687209 74.480051)
        (xy 109.220896 75.776147)
        (xy 109.960707 75.470707)
        (xy 110.266147 74.730896)
      )
    )
  )
  (zone (net 10) (net_name "Net-(U1-OUT1)") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30007)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 108.970051 66.577209)
        (xy 108.687209 66.860051)
        (xy 109.220896 68.156147)
        (xy 109.960707 67.850707)
        (xy 110.266147 67.110896)
      )
    )
  )
  (zone (net 2) (net_name "VCC") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30021)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 97.825 65.44)
        (xy 97.825 65.94)
        (xy 98.275 65.99)
        (xy 99.101 65.69)
        (xy 98.275 65.39)
      )
    )
  )
  (zone (net 2) (net_name "VCC") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30014)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 97.2875 63.015)
        (xy 96.7875 63.015)
        (xy 96.617127 63.603896)
        (xy 97.05 63.941)
        (xy 97.482873 63.603896)
      )
    )
  )
  (zone (net 2) (net_name "VCC") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30044)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 100.154264 62.034607)
        (xy 100.437107 61.751764)
        (xy 100.099552 61.174427)
        (xy 99.729293 61.326793)
        (xy 99.576927 61.697052)
      )
    )
  )
  (zone (net 1) (net_name "Net-(J1-Pin_1)") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30058)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 116 66.29)
        (xy 115.6 66.29)
        (xy 115.5 66.59)
        (xy 115.8 66.891)
        (xy 116.1 66.59)
      )
    )
  )
  (zone (net 15) (net_name "Net-(U1-OUT6)") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30001)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 103.447107 66.699949)
        (xy 103.729949 66.417107)
        (xy 103.14 64.97863)
        (xy 102.339293 65.309293)
        (xy 102.00863 66.11)
      )
    )
  )
  (zone (net 8) (net_name "GND") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30041)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 114.975 68.09)
        (xy 114.975 67.69)
        (xy 114.328073 67.520448)
        (xy 114.174 67.89)
        (xy 114.328073 68.259552)
      )
    )
  )
  (zone (net 8) (net_name "GND") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30012)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 94.6 63.69)
        (xy 94.6 64.19)
        (xy 95.177113 64.39)
        (xy 95.501 63.94)
        (xy 95.177113 63.49)
      )
    )
  )
  (zone (net 8) (net_name "GND") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30035)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 99.075 61.49)
        (xy 98.575 61.49)
        (xy 98.439005 61.944953)
        (xy 98.85 62.291)
        (xy 99.238933 61.930212)
      )
    )
  )
  (zone (net 3) (net_name "Net-(J1-Pin_3)") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30004)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 102.907767 57.798781)
        (xy 102.624924 57.515938)
        (xy 101.284719 58.104702)
        (xy 101.609293 58.890707)
        (xy 102.395298 59.215281)
      )
    )
  )
  (zone (net 2) (net_name "VCC") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30013)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 96.8 64.865)
        (xy 97.3 64.865)
        (xy 97.482873 64.276104)
        (xy 97.05 63.939)
        (xy 96.617127 64.276104)
      )
    )
  )
  (zone (net 1) (net_name "Net-(J1-Pin_1)") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30005)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 96.172912 60.338535)
        (xy 96.526465 60.692088)
        (xy 97.291252 59.74)
        (xy 96.530707 58.889293)
        (xy 95.68 59.74)
      )
    )
  )
  (zone (net 6) (net_name "Net-(J1-Pin_6)") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30031)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 100.375 69.7)
        (xy 100.375 69.3)
        (xy 99.982403 69.211418)
        (xy 99.099 69.5)
        (xy 99.982403 69.788582)
      )
    )
  )
  (zone (net 6) (net_name "Net-(J1-Pin_6)") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30027)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 99.892502 69.3)
        (xy 99.892502 69.7)
        (xy 100.521427 69.960052)
        (xy 100.6755 69.5905)
        (xy 100.6745 69.1905)
      )
    )
  )
  (zone (net 3) (net_name "Net-(J1-Pin_3)") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30055)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 116.957842 68.89)
        (xy 116.675 68.607158)
        (xy 116.575 68.59)
        (xy 115.799293 68.890707)
        (xy 116.575 69.085228)
      )
    )
  )
  (zone (net 8) (net_name "GND") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30025)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 94.98812 64.19)
        (xy 94.98812 63.69)
        (xy 94.21 63.65)
        (xy 94.209 64.05)
        (xy 94.363073 64.419552)
      )
    )
  )
  (zone (net 9) (net_name "Net-(U1-OUT0)") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30006)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 110.949949 66.582791)
        (xy 111.232791 66.299949)
        (xy 110.699104 65.003853)
        (xy 109.959293 65.309293)
        (xy 109.653853 66.049104)
      )
    )
  )
  (zone (net 6) (net_name "Net-(J1-Pin_6)") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30037)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 115.15 72.165)
        (xy 115.15 71.765)
        (xy 114.503073 71.595448)
        (xy 114.349 71.965)
        (xy 114.503073 72.334552)
      )
    )
  )
  (zone (net 4) (net_name "Net-(J1-Pin_4)") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30050)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 114.725 69.69)
        (xy 114.725 70.09)
        (xy 115.025 70.19)
        (xy 115.801 69.89)
        (xy 115.025 69.59)
      )
    )
  )
  (zone (net 8) (net_name "GND") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30043)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 106.467893 63.414264)
        (xy 106.750736 63.697107)
        (xy 107.328073 63.359552)
        (xy 107.175707 62.989293)
        (xy 106.805448 62.836927)
      )
    )
  )
  (zone (net 17) (net_name "Net-(U1-R-EXT)") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30018)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 99.431066 64.551091)
        (xy 99.784619 64.197538)
        (xy 99.325 63.750996)
        (xy 98.849293 63.939293)
        (xy 98.743967 64.34)
      )
    )
  )
  (zone (net 12) (net_name "Net-(U1-OUT3)") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30045)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 94.35 74.682323)
        (xy 93.95 74.682323)
        (xy 93.794642 75.326427)
        (xy 94.164194 75.4805)
        (xy 94.533746 75.326427)
      )
    )
  )
  (zone (net 1) (net_name "Net-(J1-Pin_1)") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30000)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 98.056031 57.82)
        (xy 98.056031 57.42)
        (xy 96.221727 58.04)
        (xy 96.529 58.89)
        (xy 97.379999 59.287793)
      )
    )
  )
  (zone (net 17) (net_name "Net-(U1-R-EXT)") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30020)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 100.375 67.21)
        (xy 100.375 66.71)
        (xy 99.925 66.66)
        (xy 99.099 66.96)
        (xy 99.925 67.26)
      )
    )
  )
  (zone (net 7) (net_name "Net-(J1-Pin_7)") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30026)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 115.082922 73.09)
        (xy 115.082922 72.69)
        (xy 114.297467 72.563121)
        (xy 114.296467 72.963121)
        (xy 114.45054 73.332673)
      )
    )
  )
  (zone (net 14) (net_name "Net-(U1-OUT5)") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30009)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 103.329949 69.122791)
        (xy 103.612791 68.839949)
        (xy 103.079104 67.543853)
        (xy 102.339293 67.849293)
        (xy 102.033853 68.589104)
      )
    )
  )
  (zone (net 5) (net_name "Net-(J1-Pin_5)") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30051)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 114.725 70.69)
        (xy 114.725 71.09)
        (xy 115.025 71.19)
        (xy 115.801 70.89)
        (xy 115.025 70.59)
      )
    )
  )
  (zone (net 7) (net_name "Net-(J1-Pin_7)") (layer "B.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30018)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 100.85 67.415)
        (xy 100.45 67.415)
        (xy 100.280448 68.061927)
        (xy 100.65 68.216)
        (xy 101.019552 68.061927)
      )
    )
  )
  (zone (net 3) (net_name "Net-(J1-Pin_3)") (layer "B.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30015)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 93.55 67.14)
        (xy 93.55 66.74)
        (xy 92.903073 66.570448)
        (xy 92.749 66.94)
        (xy 92.903073 67.309552)
      )
    )
  )
  (zone (net 2) (net_name "VCC") (layer "B.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30001)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 104.04 70.59)
        (xy 104.04 70.19)
        (xy 102.665281 69.604702)
        (xy 102.339 70.39)
        (xy 102.665281 71.175298)
      )
    )
  )
  (zone (net 6) (net_name "Net-(J1-Pin_6)") (layer "B.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30022)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 99.967393 70.014764)
        (xy 100.250236 70.297607)
        (xy 100.827573 69.960052)
        (xy 100.675207 69.589793)
        (xy 100.304948 69.437427)
      )
    )
  )
  (zone (net 2) (net_name "VCC") (layer "B.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30017)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 98.93 61.1275)
        (xy 98.93 61.5275)
        (xy 99.576927 61.697052)
        (xy 99.731 61.3275)
        (xy 99.576927 60.957948)
      )
    )
  )
  (zone (net 4) (net_name "Net-(J1-Pin_4)") (layer "B.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30012)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 93.525 68.44)
        (xy 93.525 68.04)
        (xy 92.878073 67.870448)
        (xy 92.724 68.24)
        (xy 92.878073 68.609552)
      )
    )
  )
  (zone (net 7) (net_name "Net-(J1-Pin_7)") (layer "B.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30010)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 115.074202 72.655011)
        (xy 114.79136 72.372169)
        (xy 114.144394 72.593569)
        (xy 114.29676 72.963828)
        (xy 114.58031 73.245964)
      )
    )
  )
  (zone (net 8) (net_name "GND") (layer "B.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30000)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 97.691142 59.915305)
        (xy 98.044695 60.268858)
        (xy 99.395281 59.675298)
        (xy 99.070707 58.889293)
        (xy 98.284702 58.564719)
      )
    )
  )
  (zone (net 2) (net_name "VCC") (layer "B.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30027)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 103.925 63.710027)
        (xy 104.325 63.710027)
        (xy 104.519552 63.068073)
        (xy 104.15 62.914)
        (xy 103.780448 63.068073)
      )
    )
  )
  (zone (net 2) (net_name "VCC") (layer "B.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30016)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 97.8375 61.5275)
        (xy 97.8375 61.1275)
        (xy 97.190573 60.957948)
        (xy 97.0365 61.3275)
        (xy 97.190573 61.697052)
      )
    )
  )
  (zone (net 15) (net_name "Net-(U1-OUT6)") (layer "B.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30019)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 101.456364 71.927971)
        (xy 101.456364 71.527971)
        (xy 100.809437 71.358419)
        (xy 100.655364 71.727971)
        (xy 100.809437 72.097523)
      )
    )
  )
  (zone (net 5) (net_name "Net-(J1-Pin_5)") (layer "B.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30021)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 112.917893 76.264264)
        (xy 113.200736 76.547107)
        (xy 113.778073 76.209552)
        (xy 113.625707 75.839293)
        (xy 113.255448 75.686927)
      )
    )
  )
  (zone (net 8) (net_name "GND") (layer "B.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30011)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 113.375 67.69)
        (xy 113.375 68.09)
        (xy 114.021927 68.259552)
        (xy 114.176 67.89)
        (xy 114.021927 67.520448)
      )
    )
  )
  (zone (net 6) (net_name "Net-(J1-Pin_6)") (layer "B.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30004)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 107.886497 59.95066)
        (xy 108.16934 60.233503)
        (xy 109.555281 59.675298)
        (xy 109.230707 58.889293)
        (xy 108.444702 58.564719)
      )
    )
  )
  (zone (net 6) (net_name "Net-(J1-Pin_6)") (layer "B.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30026)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 113.554973 71.79)
        (xy 113.554973 72.19)
        (xy 114.196927 72.334552)
        (xy 114.351 71.965)
        (xy 114.196927 71.595448)
      )
    )
  )
  (zone (net 8) (net_name "GND") (layer "B.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30009)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 94.46 63.25)
        (xy 93.96 63.25)
        (xy 93.81 64.05)
        (xy 94.21 64.051)
        (xy 94.61 64.05)
      )
    )
  )
  (zone (net 4) (net_name "Net-(J1-Pin_4)") (layer "B.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30002)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 102.806497 59.95066)
        (xy 103.08934 60.233503)
        (xy 104.475281 59.675298)
        (xy 104.150707 58.889293)
        (xy 103.364702 58.564719)
      )
    )
  )
  (zone (net 15) (net_name "Net-(U1-OUT6)") (layer "B.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30025)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 103.727393 71.527971)
        (xy 103.727393 71.927971)
        (xy 104.371927 72.109552)
        (xy 104.526 71.74)
        (xy 104.371927 71.370448)
      )
    )
  )
  (zone (net 8) (net_name "GND") (layer "B.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30020)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 106.975 63.79)
        (xy 107.375 63.79)
        (xy 107.544552 63.143073)
        (xy 107.175 62.989)
        (xy 106.805448 63.143073)
      )
    )
  )
  (zone (net 5) (net_name "Net-(J1-Pin_5)") (layer "B.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30014)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 93.575 69.69)
        (xy 93.575 69.29)
        (xy 92.928073 69.120448)
        (xy 92.774 69.49)
        (xy 92.928073 69.859552)
      )
    )
  )
  (zone (net 2) (net_name "VCC") (layer "B.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30007)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 108.36 70.19)
        (xy 108.36 70.59)
        (xy 109.653853 71.129104)
        (xy 109.961 70.39)
        (xy 109.653853 69.650896)
      )
    )
  )
  (zone (net 7) (net_name "Net-(J1-Pin_7)") (layer "B.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30005)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 110.426497 59.95066)
        (xy 110.70934 60.233503)
        (xy 112.095281 59.675298)
        (xy 111.770707 58.889293)
        (xy 110.984702 58.564719)
      )
    )
  )
  (zone (net 12) (net_name "Net-(U1-OUT3)") (layer "B.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30008)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 100.74 75.27)
        (xy 100.74 75.67)
        (xy 102.033853 76.209104)
        (xy 102.341 75.47)
        (xy 102.033853 74.730896)
      )
    )
  )
  (zone (net 12) (net_name "Net-(U1-OUT3)") (layer "B.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30024)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 94.962304 75.67)
        (xy 94.962304 75.27)
        (xy 94.317267 75.109948)
        (xy 94.163194 75.4795)
        (xy 94.317267 75.849052)
      )
    )
  )
  (zone (net 6) (net_name "Net-(J1-Pin_6)") (layer "B.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30023)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 100.250236 68.883393)
        (xy 99.967393 69.166236)
        (xy 100.304948 69.743573)
        (xy 100.675207 69.591207)
        (xy 100.827573 69.220948)
      )
    )
  )
  (zone (net 5) (net_name "Net-(J1-Pin_5)") (layer "B.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30013)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 92.575 70.29)
        (xy 92.975 70.29)
        (xy 93.144552 69.643073)
        (xy 92.775 69.489)
        (xy 92.405448 69.643073)
      )
    )
  )
  (zone (net 5) (net_name "Net-(J1-Pin_5)") (layer "B.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30003)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 105.346497 59.95066)
        (xy 105.62934 60.233503)
        (xy 107.015281 59.675298)
        (xy 106.690707 58.889293)
        (xy 105.904702 58.564719)
      )
    )
  )
  (zone (net 3) (net_name "Net-(J1-Pin_3)") (layer "B.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30006)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 101.46071 60.44532)
        (xy 101.743551 60.728161)
        (xy 102.395298 59.215281)
        (xy 101.610707 58.889293)
        (xy 100.824702 59.215281)
      )
    )
  )
)
