(kicad_pcb (version 20221018) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "USLetter")
  (title_block
    (title "Haunted Keyboard")
    (date "2023-10-19")
    (rev "v1")
    (company "Jack And Steph's Workshop")
  )
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (plot_on_all_layers_selection 0x0000000_00000000)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (dashed_line_dash_ratio 12.000000)
      (dashed_line_gap_ratio 3.000000)
      (svgprecision 4)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "gerbers/")
    )
  )
  (net 0 "")
  (net 1 "Net-(D1-A)")
  (net 2 "Net-(D2-A)")
  (net 3 "Net-(D3-A)")
  (net 4 "Net-(D4-A)")
  (net 5 "Net-(D5-A)")
  (net 6 "Net-(D6-A)")
  (net 7 "Net-(D7-A)")
  (net 8 "Net-(D8-A)")
  (net 9 "Net-(D9-A)")
  (net 10 "Net-(D10-A)")
  (net 11 "Net-(D11-A)")
  (net 12 "Net-(D12-A)")
  (net 13 "Net-(D13-A)")
  (net 14 "Net-(D14-A)")
  (net 15 "Net-(D15-A)")
  (net 16 "Net-(D16-A)")
  (net 17 "Net-(D17-A)")
  (net 18 "Net-(D18-A)")
  (net 19 "Net-(D19-A)")
  (net 20 "Net-(D20-A)")
  (net 21 "Net-(D21-A)")
  (net 22 "Net-(D22-A)")
  (net 23 "Net-(D23-A)")
  (net 24 "Net-(D24-A)")
  (net 25 "Net-(D25-A)")
  (net 26 "Net-(D26-A)")
  (net 27 "Net-(D27-A)")
  (net 28 "Net-(D28-A)")
  (net 29 "Net-(D29-A)")
  (net 30 "Net-(D30-A)")
  (net 31 "Net-(D31-A)")
  (net 32 "Net-(D32-A)")
  (net 33 "Net-(D33-A)")
  (net 34 "Net-(D34-A)")
  (net 35 "Net-(D35-A)")
  (net 36 "Net-(D36-A)")
  (net 37 "Net-(D37-A)")
  (net 38 "Net-(D38-A)")
  (net 39 "Net-(D39-A)")
  (net 40 "Net-(D40-A)")
  (net 41 "Net-(D41-A)")
  (net 42 "Net-(D42-A)")
  (net 43 "Net-(D43-A)")
  (net 44 "Net-(D44-A)")
  (net 45 "Net-(D45-A)")
  (net 46 "Net-(D46-A)")
  (net 47 "unconnected-(J1-Pin_4-Pad4)")
  (net 48 "unconnected-(J1-Pin_5-Pad5)")
  (net 49 "unconnected-(J1-Pin_6-Pad6)")
  (net 50 "unconnected-(J1-Pin_7-Pad7)")
  (net 51 "unconnected-(J1-Pin_8-Pad8)")
  (net 52 "unconnected-(J2-Pin_3-Pad3)")
  (net 53 "unconnected-(J2-Pin_4-Pad4)")
  (net 54 "unconnected-(J2-Pin_5-Pad5)")
  (net 55 "unconnected-(J2-Pin_7-Pad7)")
  (net 56 "unconnected-(J2-Pin_8-Pad8)")
  (net 57 "unconnected-(J2-Pin_11-Pad11)")
  (net 58 "unconnected-(J2-Pin_13-Pad13)")
  (net 59 "ROW0")
  (net 60 "ROW1")
  (net 61 "ROW2")
  (net 62 "ROW3")
  (net 63 "COL0")
  (net 64 "COL1")
  (net 65 "COL2")
  (net 66 "COL3")
  (net 67 "COL4")
  (net 68 "COL5")
  (net 69 "COL6")
  (net 70 "COL7")
  (net 71 "COL8")
  (net 72 "COL9")
  (net 73 "COL10")
  (net 74 "COL11")
  (net 75 "unconnected-(J1-Pin_18-Pad18)")
  (net 76 "unconnected-(J1-Pin_1-Pad1)")
  (net 77 "unconnected-(J1-Pin_2-Pad2)")
  (net 78 "unconnected-(J1-Pin_3-Pad3)")
  (net 79 "unconnected-(J1-Pin_13-Pad13)")
  (net 80 "unconnected-(D52-DOUT-Pad4)")
  (net 81 "Net-(D47-DOUT)")
  (net 82 "VDD")
  (net 83 "Net-(D48-DOUT)")
  (net 84 "Net-(D49-DOUT)")
  (net 85 "Net-(D50-DOUT)")
  (net 86 "Net-(D51-DOUT)")
  (net 87 "VSS")
  (net 88 "DIN")
  (net 89 "unconnected-(J2-Pin_6-Pad6)")
  (net 90 "unconnected-(J2-Pin_9-Pad9)")
  (net 91 "unconnected-(J1-Pin_9-Pad9)")
  (net 92 "Net-(D47-DIN)")
  (net 93 "unconnected-(J2-Pin_1-Pad1)")
  (footprint "kiswitch:SW_Cherry_MX_Plate_1.00u" (layer "F.Cu")
    (at 98.96625 87.74725)
    (descr "Cherry MX keyswitch Plate Mount Keycap 1.00u")
    (tags "Cherry MX Keyboard Keyswitch Switch Plate Cutout Keycap 1.00u")
    (property "Sheetfile" "demokeyboard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Push button switch, normally open, two pins, 45° tilted")
    (property "ki_keywords" "switch normally-open pushbutton push-button")
    (attr through_hole)
    (fp_text reference "MX28" (at 0 -8) (layer "F.SilkS"))
    (fp_text value "MX_SW_solder" (at 0 8) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 4 4) (drill 4) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle (at -3.81 -2.54) (size 2.5 2.5) (drill 1.5) (layers "*.Cu" "*.Mask")
      (net 66 "COL3") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 -5.08) (size 2.5 2.5) (drill 1.5) (layers "*.Cu" "*.Mask")
      (net 28 "Net-(D28-A)") (pinfunction "2") (pintype "passive"))
    (model "${KICAD6_3RD_PARTY}/3dmodels/com_github_perigoso_keyswitch-kicad-library/3d-library.3dshapes/SW_Cherry_MX_Plate.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "kiswitch:SW_Cherry_MX_Plate_1.00u" (layer "F.Cu")
    (at 213.26625 87.74725)
    (descr "Cherry MX keyswitch Plate Mount Keycap 1.00u")
    (tags "Cherry MX Keyboard Keyswitch Switch Plate Cutout Keycap 1.00u")
    (property "Sheetfile" "demokeyboard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Push button switch, normally open, two pins, 45° tilted")
    (property "ki_keywords" "switch normally-open pushbutton push-button")
    (attr through_hole)
    (fp_text reference "MX34" (at 0 -8) (layer "F.SilkS"))
    (fp_text value "MX_SW_solder" (at 0 8) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 4 4) (drill 4) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle (at -3.81 -2.54) (size 2.5 2.5) (drill 1.5) (layers "*.Cu" "*.Mask")
      (net 72 "COL9") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 -5.08) (size 2.5 2.5) (drill 1.5) (layers "*.Cu" "*.Mask")
      (net 34 "Net-(D34-A)") (pinfunction "2") (pintype "passive"))
    (model "${KICAD6_3RD_PARTY}/3dmodels/com_github_perigoso_keyswitch-kicad-library/3d-library.3dshapes/SW_Cherry_MX_Plate.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "kiswitch:SW_Cherry_MX_Plate_1.00u" (layer "F.Cu")
    (at 198.97875 49.64725)
    (descr "Cherry MX keyswitch Plate Mount Keycap 1.00u")
    (tags "Cherry MX Keyboard Keyswitch Switch Plate Cutout Keycap 1.00u")
    (property "Sheetfile" "demokeyboard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Push button switch, normally open, two pins, 45° tilted")
    (property "ki_keywords" "switch normally-open pushbutton push-button")
    (attr through_hole)
    (fp_text reference "MX10" (at 0 -8) (layer "F.SilkS"))
    (fp_text value "MX_SW_solder" (at 0 8) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 4 4) (drill 4) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle (at -3.81 -2.54) (size 2.5 2.5) (drill 1.5) (layers "*.Cu" "*.Mask")
      (net 72 "COL9") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 -5.08) (size 2.5 2.5) (drill 1.5) (layers "*.Cu" "*.Mask")
      (net 10 "Net-(D10-A)") (pinfunction "2") (pintype "passive"))
    (model "${KICAD6_3RD_PARTY}/3dmodels/com_github_perigoso_keyswitch-kicad-library/3d-library.3dshapes/SW_Cherry_MX_Plate.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "kiswitch:SW_Cherry_MX_Plate_1.25u" (layer "F.Cu")
    (at 53.7225 106.79725)
    (descr "Cherry MX keyswitch Plate Mount Keycap 1.25u")
    (tags "Cherry MX Keyboard Keyswitch Switch Plate Cutout Keycap 1.25u")
    (property "Sheetfile" "demokeyboard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Push button switch, normally open, two pins, 45° tilted")
    (property "ki_keywords" "switch normally-open pushbutton push-button")
    (attr through_hole)
    (fp_text reference "MX38" (at 0 -8) (layer "F.SilkS"))
    (fp_text value "MX_SW_solder" (at 0 8) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 4 4) (drill 4) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle (at -3.81 -2.54) (size 2.5 2.5) (drill 1.5) (layers "*.Cu" "*.Mask")
      (net 64 "COL1") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 -5.08) (size 2.5 2.5) (drill 1.5) (layers "*.Cu" "*.Mask")
      (net 38 "Net-(D38-A)") (pinfunction "2") (pintype "passive"))
    (model "${KICAD6_3RD_PARTY}/3dmodels/com_github_perigoso_keyswitch-kicad-library/3d-library.3dshapes/SW_Cherry_MX_Plate.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "PCM_marbastlib-mx:STAB_MX_P_2u" (layer "F.Cu")
    (at 146.59125 106.79725 180)
    (descr "Footprint for Cherry Clip/Screw in type stabilizers, 2u")
    (property "Sheetfile" "demokeyboard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Cherry MX-style stabilizer")
    (property "ki_keywords" "cherry mx stabilizer stab")
    (attr through_hole exclude_from_pos_files)
    (fp_text reference "S2" (at 0 0) (layer "F.SilkS") hide)
    (fp_text value "MX_stab" (at 0 8.128) (layer "F.Fab"))
    (pad "" thru_hole circle (at -11.90625 -6.985 180) (size 4 4) (drill 3.048) (layers "*.Cu" "B.Mask"))
    (pad "" np_thru_hole circle (at -11.90625 8.255 180) (size 3.9878 3.9878) (drill 3.9878) (layers "*.Cu" "*.Mask"))
    (pad "" thru_hole circle (at 11.90625 -6.985 180) (size 4 4) (drill 3.048) (layers "*.Cu" "B.Mask"))
    (pad "" np_thru_hole circle (at 11.90625 8.255 180) (size 3.9878 3.9878) (drill 3.9878) (layers "*.Cu" "*.Mask"))
  )
  (footprint "kiswitch:SW_Cherry_MX_Plate_1.00u" (layer "F.Cu")
    (at 122.77875 49.64725)
    (descr "Cherry MX keyswitch Plate Mount Keycap 1.00u")
    (tags "Cherry MX Keyboard Keyswitch Switch Plate Cutout Keycap 1.00u")
    (property "Sheetfile" "demokeyboard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Push button switch, normally open, two pins, 45° tilted")
    (property "ki_keywords" "switch normally-open pushbutton push-button")
    (attr through_hole)
    (fp_text reference "MX6" (at 0 -8) (layer "F.SilkS"))
    (fp_text value "MX_SW_solder" (at 0 8) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 4 4) (drill 4) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle (at -3.81 -2.54) (size 2.5 2.5) (drill 1.5) (layers "*.Cu" "*.Mask")
      (net 68 "COL5") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 -5.08) (size 2.5 2.5) (drill 1.5) (layers "*.Cu" "*.Mask")
      (net 6 "Net-(D6-A)") (pinfunction "2") (pintype "passive"))
    (model "${KICAD6_3RD_PARTY}/3dmodels/com_github_perigoso_keyswitch-kicad-library/3d-library.3dshapes/SW_Cherry_MX_Plate.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "kiswitch:SW_Cherry_MX_Plate_1.00u" (layer "F.Cu")
    (at 151.35375 68.69725)
    (descr "Cherry MX keyswitch Plate Mount Keycap 1.00u")
    (tags "Cherry MX Keyboard Keyswitch Switch Plate Cutout Keycap 1.00u")
    (property "Sheetfile" "demokeyboard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Push button switch, normally open, two pins, 45° tilted")
    (property "ki_keywords" "switch normally-open pushbutton push-button")
    (attr through_hole)
    (fp_text reference "MX19" (at 0 -8) (layer "F.SilkS"))
    (fp_text value "MX_SW_solder" (at 0 8) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 4 4) (drill 4) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle (at -3.81 -2.54) (size 2.5 2.5) (drill 1.5) (layers "*.Cu" "*.Mask")
      (net 69 "COL6") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 -5.08) (size 2.5 2.5) (drill 1.5) (layers "*.Cu" "*.Mask")
      (net 19 "Net-(D19-A)") (pinfunction "2") (pintype "passive"))
    (model "${KICAD6_3RD_PARTY}/3dmodels/com_github_perigoso_keyswitch-kicad-library/3d-library.3dshapes/SW_Cherry_MX_Plate.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "kiswitch:SW_Cherry_MX_Plate_1.00u" (layer "F.Cu")
    (at 46.57875 49.64725)
    (descr "Cherry MX keyswitch Plate Mount Keycap 1.00u")
    (tags "Cherry MX Keyboard Keyswitch Switch Plate Cutout Keycap 1.00u")
    (property "Sheetfile" "demokeyboard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Push button switch, normally open, two pins, 45° tilted")
    (property "ki_keywords" "switch normally-open pushbutton push-button")
    (attr through_hole)
    (fp_text reference "MX2" (at 0 -8) (layer "F.SilkS"))
    (fp_text value "MX_SW_solder" (at 0 8) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 4 4) (drill 4) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle (at -3.81 -2.54) (size 2.5 2.5) (drill 1.5) (layers "*.Cu" "*.Mask")
      (net 64 "COL1") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 -5.08) (size 2.5 2.5) (drill 1.5) (layers "*.Cu" "*.Mask")
      (net 2 "Net-(D2-A)") (pinfunction "2") (pintype "passive"))
    (model "${KICAD6_3RD_PARTY}/3dmodels/com_github_perigoso_keyswitch-kicad-library/3d-library.3dshapes/SW_Cherry_MX_Plate.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "kiswitch:SW_Cherry_MX_Plate_1.00u" (layer "F.Cu")
    (at 108.49125 106.79725)
    (descr "Cherry MX keyswitch Plate Mount Keycap 1.00u")
    (tags "Cherry MX Keyboard Keyswitch Switch Plate Cutout Keycap 1.00u")
    (property "Sheetfile" "demokeyboard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Push button switch, normally open, two pins, 45° tilted")
    (property "ki_keywords" "switch normally-open pushbutton push-button")
    (attr through_hole)
    (fp_text reference "MX40" (at 0 -8) (layer "F.SilkS"))
    (fp_text value "MX_SW_solder" (at 0 8) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 4 4) (drill 4) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle (at -3.81 -2.54) (size 2.5 2.5) (drill 1.5) (layers "*.Cu" "*.Mask")
      (net 66 "COL3") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 -5.08) (size 2.5 2.5) (drill 1.5) (layers "*.Cu" "*.Mask")
      (net 40 "Net-(D40-A)") (pinfunction "2") (pintype "passive"))
    (model "${KICAD6_3RD_PARTY}/3dmodels/com_github_perigoso_keyswitch-kicad-library/3d-library.3dshapes/SW_Cherry_MX_Plate.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3" (layer "F.Cu")
    (at 43.6675 74.42525)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (property "Sheetfile" "demokeyboard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole without connection")
    (property "ki_keywords" "mounting hole")
    (attr exclude_from_pos_files)
    (fp_text reference "H1" (at 0 -4.2) (layer "F.SilkS"))
    (fp_text value "MountingHole" (at 0 4.2) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at -1.7815 -4.654) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers "*.Cu" "*.Mask"))
  )
  (footprint "kiswitch:SW_Cherry_MX_Plate_1.00u" (layer "F.Cu")
    (at 170.40375 68.69725)
    (descr "Cherry MX keyswitch Plate Mount Keycap 1.00u")
    (tags "Cherry MX Keyboard Keyswitch Switch Plate Cutout Keycap 1.00u")
    (property "Sheetfile" "demokeyboard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Push button switch, normally open, two pins, 45° tilted")
    (property "ki_keywords" "switch normally-open pushbutton push-button")
    (attr through_hole)
    (fp_text reference "MX20" (at 0 -8) (layer "F.SilkS"))
    (fp_text value "MX_SW_solder" (at 0 8) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 4 4) (drill 4) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle (at -3.81 -2.54) (size 2.5 2.5) (drill 1.5) (layers "*.Cu" "*.Mask")
      (net 70 "COL7") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 -5.08) (size 2.5 2.5) (drill 1.5) (layers "*.Cu" "*.Mask")
      (net 20 "Net-(D20-A)") (pinfunction "2") (pintype "passive"))
    (model "${KICAD6_3RD_PARTY}/3dmodels/com_github_perigoso_keyswitch-kicad-library/3d-library.3dshapes/SW_Cherry_MX_Plate.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "kiswitch:SW_Cherry_MX_Plate_1.25u" (layer "F.Cu")
    (at 248.985 68.69725)
    (descr "Cherry MX keyswitch Plate Mount Keycap 1.25u")
    (tags "Cherry MX Keyboard Keyswitch Switch Plate Cutout Keycap 1.25u")
    (property "Sheetfile" "demokeyboard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Push button switch, normally open, two pins, 45° tilted")
    (property "ki_keywords" "switch normally-open pushbutton push-button")
    (attr through_hole)
    (fp_text reference "MX24" (at 0 -8) (layer "F.SilkS"))
    (fp_text value "MX_SW_solder" (at 0 8) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 4 4) (drill 4) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle (at -3.81 -2.54) (size 2.5 2.5) (drill 1.5) (layers "*.Cu" "*.Mask")
      (net 74 "COL11") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 -5.08) (size 2.5 2.5) (drill 1.5) (layers "*.Cu" "*.Mask")
      (net 24 "Net-(D24-A)") (pinfunction "2") (pintype "passive"))
    (model "${KICAD6_3RD_PARTY}/3dmodels/com_github_perigoso_keyswitch-kicad-library/3d-library.3dshapes/SW_Cherry_MX_Plate.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "kiswitch:SW_Cherry_MX_Plate_1.25u" (layer "F.Cu")
    (at 77.535 106.79725)
    (descr "Cherry MX keyswitch Plate Mount Keycap 1.25u")
    (tags "Cherry MX Keyboard Keyswitch Switch Plate Cutout Keycap 1.25u")
    (property "Sheetfile" "demokeyboard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Push button switch, normally open, two pins, 45° tilted")
    (property "ki_keywords" "switch normally-open pushbutton push-button")
    (attr through_hole)
    (fp_text reference "MX39" (at 0 -8) (layer "F.SilkS"))
    (fp_text value "MX_SW_solder" (at 0 8) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 4 4) (drill 4) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle (at -3.81 -2.54) (size 2.5 2.5) (drill 1.5) (layers "*.Cu" "*.Mask")
      (net 65 "COL2") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 -5.08) (size 2.5 2.5) (drill 1.5) (layers "*.Cu" "*.Mask")
      (net 39 "Net-(D39-A)") (pinfunction "2") (pintype "passive"))
    (model "${KICAD6_3RD_PARTY}/3dmodels/com_github_perigoso_keyswitch-kicad-library/3d-library.3dshapes/SW_Cherry_MX_Plate.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "kiswitch:SW_Cherry_MX_Plate_1.00u" (layer "F.Cu")
    (at 118.01625 87.74725)
    (descr "Cherry MX keyswitch Plate Mount Keycap 1.00u")
    (tags "Cherry MX Keyboard Keyswitch Switch Plate Cutout Keycap 1.00u")
    (property "Sheetfile" "demokeyboard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Push button switch, normally open, two pins, 45° tilted")
    (property "ki_keywords" "switch normally-open pushbutton push-button")
    (attr through_hole)
    (fp_text reference "MX29" (at 0 -8) (layer "F.SilkS"))
    (fp_text value "MX_SW_solder" (at 0 8) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 4 4) (drill 4) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle (at -3.81 -2.54) (size 2.5 2.5) (drill 1.5) (layers "*.Cu" "*.Mask")
      (net 67 "COL4") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 -5.08) (size 2.5 2.5) (drill 1.5) (layers "*.Cu" "*.Mask")
      (net 29 "Net-(D29-A)") (pinfunction "2") (pintype "passive"))
    (model "${KICAD6_3RD_PARTY}/3dmodels/com_github_perigoso_keyswitch-kicad-library/3d-library.3dshapes/SW_Cherry_MX_Plate.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "kiswitch:SW_Cherry_MX_Plate_1.00u" (layer "F.Cu")
    (at 189.45375 68.69725)
    (descr "Cherry MX keyswitch Plate Mount Keycap 1.00u")
    (tags "Cherry MX Keyboard Keyswitch Switch Plate Cutout Keycap 1.00u")
    (property "Sheetfile" "demokeyboard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Push button switch, normally open, two pins, 45° tilted")
    (property "ki_keywords" "switch normally-open pushbutton push-button")
    (attr through_hole)
    (fp_text reference "MX21" (at 0 -8) (layer "F.SilkS"))
    (fp_text value "MX_SW_solder" (at 0 8) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 4 4) (drill 4) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle (at -3.81 -2.54) (size 2.5 2.5) (drill 1.5) (layers "*.Cu" "*.Mask")
      (net 71 "COL8") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 -5.08) (size 2.5 2.5) (drill 1.5) (layers "*.Cu" "*.Mask")
      (net 21 "Net-(D21-A)") (pinfunction "2") (pintype "passive"))
    (model "${KICAD6_3RD_PARTY}/3dmodels/com_github_perigoso_keyswitch-kicad-library/3d-library.3dshapes/SW_Cherry_MX_Plate.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "kiswitch:SW_Cherry_MX_Plate_1.00u" (layer "F.Cu")
    (at 156.11625 87.74725)
    (descr "Cherry MX keyswitch Plate Mount Keycap 1.00u")
    (tags "Cherry MX Keyboard Keyswitch Switch Plate Cutout Keycap 1.00u")
    (property "Sheetfile" "demokeyboard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Push button switch, normally open, two pins, 45° tilted")
    (property "ki_keywords" "switch normally-open pushbutton push-button")
    (attr through_hole)
    (fp_text reference "MX31" (at 0 -8) (layer "F.SilkS"))
    (fp_text value "MX_SW_solder" (at 0 8) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 4 4) (drill 4) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle (at -3.81 -2.54) (size 2.5 2.5) (drill 1.5) (layers "*.Cu" "*.Mask")
      (net 69 "COL6") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 -5.08) (size 2.5 2.5) (drill 1.5) (layers "*.Cu" "*.Mask")
      (net 31 "Net-(D31-A)") (pinfunction "2") (pintype "passive"))
    (model "${KICAD6_3RD_PARTY}/3dmodels/com_github_perigoso_keyswitch-kicad-library/3d-library.3dshapes/SW_Cherry_MX_Plate.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "kiswitch:SW_Cherry_MX_Plate_1.00u" (layer "F.Cu")
    (at 227.55375 68.69725)
    (descr "Cherry MX keyswitch Plate Mount Keycap 1.00u")
    (tags "Cherry MX Keyboard Keyswitch Switch Plate Cutout Keycap 1.00u")
    (property "Sheetfile" "demokeyboard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Push button switch, normally open, two pins, 45° tilted")
    (property "ki_keywords" "switch normally-open pushbutton push-button")
    (attr through_hole)
    (fp_text reference "MX23" (at 0 -8) (layer "F.SilkS"))
    (fp_text value "MX_SW_solder" (at 0 8) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 4 4) (drill 4) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle (at -3.81 -2.54) (size 2.5 2.5) (drill 1.5) (layers "*.Cu" "*.Mask")
      (net 73 "COL10") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 -5.08) (size 2.5 2.5) (drill 1.5) (layers "*.Cu" "*.Mask")
      (net 23 "Net-(D23-A)") (pinfunction "2") (pintype "passive"))
    (model "${KICAD6_3RD_PARTY}/3dmodels/com_github_perigoso_keyswitch-kicad-library/3d-library.3dshapes/SW_Cherry_MX_Plate.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "kiswitch:SW_Cherry_MX_Plate_1.00u" (layer "F.Cu")
    (at 60.86625 87.74725)
    (descr "Cherry MX keyswitch Plate Mount Keycap 1.00u")
    (tags "Cherry MX Keyboard Keyswitch Switch Plate Cutout Keycap 1.00u")
    (property "Sheetfile" "demokeyboard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Push button switch, normally open, two pins, 45° tilted")
    (property "ki_keywords" "switch normally-open pushbutton push-button")
    (attr through_hole)
    (fp_text reference "MX26" (at 0 -8) (layer "F.SilkS"))
    (fp_text value "MX_SW_solder" (at 0 8) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 4 4) (drill 4) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle (at -3.81 -2.54) (size 2.5 2.5) (drill 1.5) (layers "*.Cu" "*.Mask")
      (net 64 "COL1") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 -5.08) (size 2.5 2.5) (drill 1.5) (layers "*.Cu" "*.Mask")
      (net 26 "Net-(D26-A)") (pinfunction "2") (pintype "passive"))
    (model "${KICAD6_3RD_PARTY}/3dmodels/com_github_perigoso_keyswitch-kicad-library/3d-library.3dshapes/SW_Cherry_MX_Plate.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "kiswitch:SW_Cherry_MX_Plate_1.00u" (layer "F.Cu")
    (at 27.52875 49.64725)
    (descr "Cherry MX keyswitch Plate Mount Keycap 1.00u")
    (tags "Cherry MX Keyboard Keyswitch Switch Plate Cutout Keycap 1.00u")
    (property "Sheetfile" "demokeyboard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Push button switch, normally open, two pins, 45° tilted")
    (property "ki_keywords" "switch normally-open pushbutton push-button")
    (attr through_hole)
    (fp_text reference "MX1" (at 0 -8) (layer "F.SilkS"))
    (fp_text value "MX_SW_solder" (at 0 8) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 4 4) (drill 4) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle (at -3.81 -2.54) (size 2.5 2.5) (drill 1.5) (layers "*.Cu" "*.Mask")
      (net 63 "COL0") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 -5.08) (size 2.5 2.5) (drill 1.5) (layers "*.Cu" "*.Mask")
      (net 1 "Net-(D1-A)") (pinfunction "2") (pintype "passive"))
    (model "${KICAD6_3RD_PARTY}/3dmodels/com_github_perigoso_keyswitch-kicad-library/3d-library.3dshapes/SW_Cherry_MX_Plate.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "kiswitch:SW_Cherry_MX_Plate_1.00u" (layer "F.Cu")
    (at 232.31625 106.79725)
    (descr "Cherry MX keyswitch Plate Mount Keycap 1.00u")
    (tags "Cherry MX Keyboard Keyswitch Switch Plate Cutout Keycap 1.00u")
    (property "Sheetfile" "demokeyboard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Push button switch, normally open, two pins, 45° tilted")
    (property "ki_keywords" "switch normally-open pushbutton push-button")
    (attr through_hole)
    (fp_text reference "MX45" (at 0 -8) (layer "F.SilkS"))
    (fp_text value "MX_SW_solder" (at 0 8) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 4 4) (drill 4) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle (at -3.81 -2.54) (size 2.5 2.5) (drill 1.5) (layers "*.Cu" "*.Mask")
      (net 73 "COL10") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 -5.08) (size 2.5 2.5) (drill 1.5) (layers "*.Cu" "*.Mask")
      (net 45 "Net-(D45-A)") (pinfunction "2") (pintype "passive"))
    (model "${KICAD6_3RD_PARTY}/3dmodels/com_github_perigoso_keyswitch-kicad-library/3d-library.3dshapes/SW_Cherry_MX_Plate.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "kiswitch:SW_Cherry_MX_Plate_1.00u" (layer "F.Cu")
    (at 251.36625 87.74725)
    (descr "Cherry MX keyswitch Plate Mount Keycap 1.00u")
    (tags "Cherry MX Keyboard Keyswitch Switch Plate Cutout Keycap 1.00u")
    (property "Sheetfile" "demokeyboard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Push button switch, normally open, two pins, 45° tilted")
    (property "ki_keywords" "switch normally-open pushbutton push-button")
    (attr through_hole)
    (fp_text reference "MX36" (at 0 -8) (layer "F.SilkS"))
    (fp_text value "MX_SW_solder" (at 0 8) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 4 4) (drill 4) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle (at -3.81 -2.54) (size 2.5 2.5) (drill 1.5) (layers "*.Cu" "*.Mask")
      (net 74 "COL11") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 -5.08) (size 2.5 2.5) (drill 1.5) (layers "*.Cu" "*.Mask")
      (net 36 "Net-(D36-A)") (pinfunction "2") (pintype "passive"))
    (model "${KICAD6_3RD_PARTY}/3dmodels/com_github_perigoso_keyswitch-kicad-library/3d-library.3dshapes/SW_Cherry_MX_Plate.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "kiswitch:SW_Cherry_MX_Plate_1.00u" (layer "F.Cu")
    (at 94.20375 68.69725)
    (descr "Cherry MX keyswitch Plate Mount Keycap 1.00u")
    (tags "Cherry MX Keyboard Keyswitch Switch Plate Cutout Keycap 1.00u")
    (property "Sheetfile" "demokeyboard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Push button switch, normally open, two pins, 45° tilted")
    (property "ki_keywords" "switch normally-open pushbutton push-button")
    (attr through_hole)
    (fp_text reference "MX16" (at 0 -8) (layer "F.SilkS"))
    (fp_text value "MX_SW_solder" (at 0 8) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 4 4) (drill 4) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle (at -3.81 -2.54) (size 2.5 2.5) (drill 1.5) (layers "*.Cu" "*.Mask")
      (net 66 "COL3") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 -5.08) (size 2.5 2.5) (drill 1.5) (layers "*.Cu" "*.Mask")
      (net 16 "Net-(D16-A)") (pinfunction "2") (pintype "passive"))
    (model "${KICAD6_3RD_PARTY}/3dmodels/com_github_perigoso_keyswitch-kicad-library/3d-library.3dshapes/SW_Cherry_MX_Plate.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "kiswitch:SW_Cherry_MX_Plate_1.00u" (layer "F.Cu")
    (at 103.72875 49.64725)
    (descr "Cherry MX keyswitch Plate Mount Keycap 1.00u")
    (tags "Cherry MX Keyboard Keyswitch Switch Plate Cutout Keycap 1.00u")
    (property "Sheetfile" "demokeyboard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Push button switch, normally open, two pins, 45° tilted")
    (property "ki_keywords" "switch normally-open pushbutton push-button")
    (attr through_hole)
    (fp_text reference "MX5" (at 0 -8) (layer "F.SilkS"))
    (fp_text value "MX_SW_solder" (at 0 8) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 4 4) (drill 4) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle (at -3.81 -2.54) (size 2.5 2.5) (drill 1.5) (layers "*.Cu" "*.Mask")
      (net 67 "COL4") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 -5.08) (size 2.5 2.5) (drill 1.5) (layers "*.Cu" "*.Mask")
      (net 5 "Net-(D5-A)") (pinfunction "2") (pintype "passive"))
    (model "${KICAD6_3RD_PARTY}/3dmodels/com_github_perigoso_keyswitch-kicad-library/3d-library.3dshapes/SW_Cherry_MX_Plate.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "kiswitch:SW_Cherry_MX_Plate_1.00u" (layer "F.Cu")
    (at 113.25375 68.69725)
    (descr "Cherry MX keyswitch Plate Mount Keycap 1.00u")
    (tags "Cherry MX Keyboard Keyswitch Switch Plate Cutout Keycap 1.00u")
    (property "Sheetfile" "demokeyboard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Push button switch, normally open, two pins, 45° tilted")
    (property "ki_keywords" "switch normally-open pushbutton push-button")
    (attr through_hole)
    (fp_text reference "MX17" (at 0 -8) (layer "F.SilkS"))
    (fp_text value "MX_SW_solder" (at 0 8) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 4 4) (drill 4) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle (at -3.81 -2.54) (size 2.5 2.5) (drill 1.5) (layers "*.Cu" "*.Mask")
      (net 67 "COL4") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 -5.08) (size 2.5 2.5) (drill 1.5) (layers "*.Cu" "*.Mask")
      (net 17 "Net-(D17-A)") (pinfunction "2") (pintype "passive"))
    (model "${KICAD6_3RD_PARTY}/3dmodels/com_github_perigoso_keyswitch-kicad-library/3d-library.3dshapes/SW_Cherry_MX_Plate.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "kiswitch:SW_Cherry_MX_Plate_1.00u" (layer "F.Cu")
    (at 194.21625 106.79725)
    (descr "Cherry MX keyswitch Plate Mount Keycap 1.00u")
    (tags "Cherry MX Keyboard Keyswitch Switch Plate Cutout Keycap 1.00u")
    (property "Sheetfile" "demokeyboard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Push button switch, normally open, two pins, 45° tilted")
    (property "ki_keywords" "switch normally-open pushbutton push-button")
    (attr through_hole)
    (fp_text reference "MX43" (at 0 -8) (layer "F.SilkS"))
    (fp_text value "MX_SW_solder" (at 0 8) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 4 4) (drill 4) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle (at -3.81 -2.54) (size 2.5 2.5) (drill 1.5) (layers "*.Cu" "*.Mask")
      (net 71 "COL8") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 -5.08) (size 2.5 2.5) (drill 1.5) (layers "*.Cu" "*.Mask")
      (net 43 "Net-(D43-A)") (pinfunction "2") (pintype "passive"))
    (model "${KICAD6_3RD_PARTY}/3dmodels/com_github_perigoso_keyswitch-kicad-library/3d-library.3dshapes/SW_Cherry_MX_Plate.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "kiswitch:SW_Cherry_MX_Plate_1.00u" (layer "F.Cu")
    (at 56.10375 68.69725)
    (descr "Cherry MX keyswitch Plate Mount Keycap 1.00u")
    (tags "Cherry MX Keyboard Keyswitch Switch Plate Cutout Keycap 1.00u")
    (property "Sheetfile" "demokeyboard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Push button switch, normally open, two pins, 45° tilted")
    (property "ki_keywords" "switch normally-open pushbutton push-button")
    (attr through_hole)
    (fp_text reference "MX14" (at 0 -8) (layer "F.SilkS"))
    (fp_text value "MX_SW_solder" (at 0 8) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 4 4) (drill 4) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle (at -3.81 -2.54) (size 2.5 2.5) (drill 1.5) (layers "*.Cu" "*.Mask")
      (net 64 "COL1") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 -5.08) (size 2.5 2.5) (drill 1.5) (layers "*.Cu" "*.Mask")
      (net 14 "Net-(D14-A)") (pinfunction "2") (pintype "passive"))
    (model "${KICAD6_3RD_PARTY}/3dmodels/com_github_perigoso_keyswitch-kicad-library/3d-library.3dshapes/SW_Cherry_MX_Plate.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "kiswitch:SW_Cherry_MX_Plate_1.25u" (layer "F.Cu")
    (at 29.91 106.79725)
    (descr "Cherry MX keyswitch Plate Mount Keycap 1.25u")
    (tags "Cherry MX Keyboard Keyswitch Switch Plate Cutout Keycap 1.25u")
    (property "Sheetfile" "demokeyboard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Push button switch, normally open, two pins, 45° tilted")
    (property "ki_keywords" "switch normally-open pushbutton push-button")
    (attr through_hole)
    (fp_text reference "MX37" (at 0 -8) (layer "F.SilkS"))
    (fp_text value "MX_SW_solder" (at 0 8) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 4 4) (drill 4) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle (at -3.81 -2.54) (size 2.5 2.5) (drill 1.5) (layers "*.Cu" "*.Mask")
      (net 63 "COL0") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 -5.08) (size 2.5 2.5) (drill 1.5) (layers "*.Cu" "*.Mask")
      (net 37 "Net-(D37-A)") (pinfunction "2") (pintype "passive"))
    (model "${KICAD6_3RD_PARTY}/3dmodels/com_github_perigoso_keyswitch-kicad-library/3d-library.3dshapes/SW_Cherry_MX_Plate.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "kiswitch:SW_Cherry_MX_Plate_1.00u" (layer "F.Cu")
    (at 137.06625 87.74725)
    (descr "Cherry MX keyswitch Plate Mount Keycap 1.00u")
    (tags "Cherry MX Keyboard Keyswitch Switch Plate Cutout Keycap 1.00u")
    (property "Sheetfile" "demokeyboard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Push button switch, normally open, two pins, 45° tilted")
    (property "ki_keywords" "switch normally-open pushbutton push-button")
    (attr through_hole)
    (fp_text reference "MX30" (at 0 -8) (layer "F.SilkS"))
    (fp_text value "MX_SW_solder" (at 0 8) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 4 4) (drill 4) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle (at -3.81 -2.54) (size 2.5 2.5) (drill 1.5) (layers "*.Cu" "*.Mask")
      (net 68 "COL5") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 -5.08) (size 2.5 2.5) (drill 1.5) (layers "*.Cu" "*.Mask")
      (net 30 "Net-(D30-A)") (pinfunction "2") (pintype "passive"))
    (model "${KICAD6_3RD_PARTY}/3dmodels/com_github_perigoso_keyswitch-kicad-library/3d-library.3dshapes/SW_Cherry_MX_Plate.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "kiswitch:SW_Cherry_MX_Plate_1.00u" (layer "F.Cu")
    (at 141.82875 49.64725)
    (descr "Cherry MX keyswitch Plate Mount Keycap 1.00u")
    (tags "Cherry MX Keyboard Keyswitch Switch Plate Cutout Keycap 1.00u")
    (property "Sheetfile" "demokeyboard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Push button switch, normally open, two pins, 45° tilted")
    (property "ki_keywords" "switch normally-open pushbutton push-button")
    (attr through_hole)
    (fp_text reference "MX7" (at 0 -8) (layer "F.SilkS"))
    (fp_text value "MX_SW_solder" (at 0 8) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 4 4) (drill 4) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle (at -3.81 -2.54) (size 2.5 2.5) (drill 1.5) (layers "*.Cu" "*.Mask")
      (net 69 "COL6") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 -5.08) (size 2.5 2.5) (drill 1.5) (layers "*.Cu" "*.Mask")
      (net 7 "Net-(D7-A)") (pinfunction "2") (pintype "passive"))
    (model "${KICAD6_3RD_PARTY}/3dmodels/com_github_perigoso_keyswitch-kicad-library/3d-library.3dshapes/SW_Cherry_MX_Plate.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "PCM_marbastlib-mx:STAB_MX_P_2u" (layer "F.Cu")
    (at 108.49125 106.79725 180)
    (descr "Footprint for Cherry Clip/Screw in type stabilizers, 2u")
    (property "Sheetfile" "demokeyboard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Cherry MX-style stabilizer")
    (property "ki_keywords" "cherry mx stabilizer stab")
    (attr through_hole exclude_from_pos_files)
    (fp_text reference "S1" (at 0 0) (layer "F.SilkS") hide)
    (fp_text value "MX_stab" (at 0 8.128) (layer "F.Fab"))
    (pad "" thru_hole circle (at -11.90625 -6.985 180) (size 4 4) (drill 3.048) (layers "*.Cu" "B.Mask"))
    (pad "" np_thru_hole circle (at -11.90625 8.255 180) (size 3.9878 3.9878) (drill 3.9878) (layers "*.Cu" "*.Mask"))
    (pad "" thru_hole circle (at 11.90625 -6.985 180) (size 4 4) (drill 3.048) (layers "*.Cu" "B.Mask"))
    (pad "" np_thru_hole circle (at 11.90625 8.255 180) (size 3.9878 3.9878) (drill 3.9878) (layers "*.Cu" "*.Mask"))
  )
  (footprint "kiswitch:SW_Cherry_MX_Plate_1.00u" (layer "F.Cu")
    (at 218.02875 49.64725)
    (descr "Cherry MX keyswitch Plate Mount Keycap 1.00u")
    (tags "Cherry MX Keyboard Keyswitch Switch Plate Cutout Keycap 1.00u")
    (property "Sheetfile" "demokeyboard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Push button switch, normally open, two pins, 45° tilted")
    (property "ki_keywords" "switch normally-open pushbutton push-button")
    (attr through_hole)
    (fp_text reference "MX11" (at 0 -8) (layer "F.SilkS"))
    (fp_text value "MX_SW_solder" (at 0 8) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 4 4) (drill 4) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle (at -3.81 -2.54) (size 2.5 2.5) (drill 1.5) (layers "*.Cu" "*.Mask")
      (net 73 "COL10") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 -5.08) (size 2.5 2.5) (drill 1.5) (layers "*.Cu" "*.Mask")
      (net 11 "Net-(D11-A)") (pinfunction "2") (pintype "passive"))
    (model "${KICAD6_3RD_PARTY}/3dmodels/com_github_perigoso_keyswitch-kicad-library/3d-library.3dshapes/SW_Cherry_MX_Plate.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "kiswitch:SW_Cherry_MX_Plate_1.00u" (layer "F.Cu")
    (at 132.30375 68.69725)
    (descr "Cherry MX keyswitch Plate Mount Keycap 1.00u")
    (tags "Cherry MX Keyboard Keyswitch Switch Plate Cutout Keycap 1.00u")
    (property "Sheetfile" "demokeyboard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Push button switch, normally open, two pins, 45° tilted")
    (property "ki_keywords" "switch normally-open pushbutton push-button")
    (attr through_hole)
    (fp_text reference "MX18" (at 0 -8) (layer "F.SilkS"))
    (fp_text value "MX_SW_solder" (at 0 8) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 4 4) (drill 4) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle (at -3.81 -2.54) (size 2.5 2.5) (drill 1.5) (layers "*.Cu" "*.Mask")
      (net 68 "COL5") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 -5.08) (size 2.5 2.5) (drill 1.5) (layers "*.Cu" "*.Mask")
      (net 18 "Net-(D18-A)") (pinfunction "2") (pintype "passive"))
    (model "${KICAD6_3RD_PARTY}/3dmodels/com_github_perigoso_keyswitch-kicad-library/3d-library.3dshapes/SW_Cherry_MX_Plate.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3" (layer "F.Cu")
    (at 41.6315 103.43825)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (property "Sheetfile" "demokeyboard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole without connection")
    (property "ki_keywords" "mounting hole")
    (attr exclude_from_pos_files)
    (fp_text reference "H3" (at 0 -4.2) (layer "F.SilkS"))
    (fp_text value "MountingHole" (at 0 4.2) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers "*.Cu" "*.Mask"))
  )
  (footprint "kiswitch:SW_Cherry_MX_Plate_1.00u" (layer "F.Cu")
    (at 179.92875 49.64725)
    (descr "Cherry MX keyswitch Plate Mount Keycap 1.00u")
    (tags "Cherry MX Keyboard Keyswitch Switch Plate Cutout Keycap 1.00u")
    (property "Sheetfile" "demokeyboard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Push button switch, normally open, two pins, 45° tilted")
    (property "ki_keywords" "switch normally-open pushbutton push-button")
    (attr through_hole)
    (fp_text reference "MX9" (at 0 -8) (layer "F.SilkS"))
    (fp_text value "MX_SW_solder" (at 0 8) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 4 4) (drill 4) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle (at -3.81 -2.54) (size 2.5 2.5) (drill 1.5) (layers "*.Cu" "*.Mask")
      (net 71 "COL8") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 -5.08) (size 2.5 2.5) (drill 1.5) (layers "*.Cu" "*.Mask")
      (net 9 "Net-(D9-A)") (pinfunction "2") (pintype "passive"))
    (model "${KICAD6_3RD_PARTY}/3dmodels/com_github_perigoso_keyswitch-kicad-library/3d-library.3dshapes/SW_Cherry_MX_Plate.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "kiswitch:SW_Cherry_MX_Plate_1.00u" (layer "F.Cu")
    (at 175.16625 106.79725)
    (descr "Cherry MX keyswitch Plate Mount Keycap 1.00u")
    (tags "Cherry MX Keyboard Keyswitch Switch Plate Cutout Keycap 1.00u")
    (property "Sheetfile" "demokeyboard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Push button switch, normally open, two pins, 45° tilted")
    (property "ki_keywords" "switch normally-open pushbutton push-button")
    (attr through_hole)
    (fp_text reference "MX42" (at 0 -8) (layer "F.SilkS"))
    (fp_text value "MX_SW_solder" (at 0 8) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 4 4) (drill 4) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle (at -3.81 -2.54) (size 2.5 2.5) (drill 1.5) (layers "*.Cu" "*.Mask")
      (net 70 "COL7") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 -5.08) (size 2.5 2.5) (drill 1.5) (layers "*.Cu" "*.Mask")
      (net 42 "Net-(D42-A)") (pinfunction "2") (pintype "passive"))
    (model "${KICAD6_3RD_PARTY}/3dmodels/com_github_perigoso_keyswitch-kicad-library/3d-library.3dshapes/SW_Cherry_MX_Plate.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "kiswitch:SW_Cherry_MX_Plate_1.00u" (layer "F.Cu")
    (at 251.36625 106.79725)
    (descr "Cherry MX keyswitch Plate Mount Keycap 1.00u")
    (tags "Cherry MX Keyboard Keyswitch Switch Plate Cutout Keycap 1.00u")
    (property "Sheetfile" "demokeyboard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Push button switch, normally open, two pins, 45° tilted")
    (property "ki_keywords" "switch normally-open pushbutton push-button")
    (attr through_hole)
    (fp_text reference "MX46" (at 0 -8) (layer "F.SilkS"))
    (fp_text value "MX_SW_solder" (at 0 8) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 4 4) (drill 4) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle (at -3.81 -2.54) (size 2.5 2.5) (drill 1.5) (layers "*.Cu" "*.Mask")
      (net 74 "COL11") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 -5.08) (size 2.5 2.5) (drill 1.5) (layers "*.Cu" "*.Mask")
      (net 46 "Net-(D46-A)") (pinfunction "2") (pintype "passive"))
    (model "${KICAD6_3RD_PARTY}/3dmodels/com_github_perigoso_keyswitch-kicad-library/3d-library.3dshapes/SW_Cherry_MX_Plate.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "kiswitch:SW_Cherry_MX_Plate_1.00u" (layer "F.Cu")
    (at 146.59125 106.79725)
    (descr "Cherry MX keyswitch Plate Mount Keycap 1.00u")
    (tags "Cherry MX Keyboard Keyswitch Switch Plate Cutout Keycap 1.00u")
    (property "Sheetfile" "demokeyboard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Push button switch, normally open, two pins, 45° tilted")
    (property "ki_keywords" "switch normally-open pushbutton push-button")
    (attr through_hole)
    (fp_text reference "MX41" (at 0 -8) (layer "F.SilkS"))
    (fp_text value "MX_SW_solder" (at 0 8) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 4 4) (drill 4) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle (at -3.81 -2.54) (size 2.5 2.5) (drill 1.5) (layers "*.Cu" "*.Mask")
      (net 68 "COL5") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 -5.08) (size 2.5 2.5) (drill 1.5) (layers "*.Cu" "*.Mask")
      (net 41 "Net-(D41-A)") (pinfunction "2") (pintype "passive"))
    (model "${KICAD6_3RD_PARTY}/3dmodels/com_github_perigoso_keyswitch-kicad-library/3d-library.3dshapes/SW_Cherry_MX_Plate.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "kiswitch:SW_Cherry_MX_Plate_1.75u" (layer "F.Cu")
    (at 244.2225 49.64725)
    (descr "Cherry MX keyswitch Plate Mount Keycap 1.75u")
    (tags "Cherry MX Keyboard Keyswitch Switch Plate Cutout Keycap 1.75u")
    (property "Sheetfile" "demokeyboard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Push button switch, normally open, two pins, 45° tilted")
    (property "ki_keywords" "switch normally-open pushbutton push-button")
    (attr through_hole)
    (fp_text reference "MX12" (at 0 -8) (layer "F.SilkS"))
    (fp_text value "MX_SW_solder" (at 0 8) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 4 4) (drill 4) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle (at -3.81 -2.54) (size 2.5 2.5) (drill 1.5) (layers "*.Cu" "*.Mask")
      (net 74 "COL11") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 -5.08) (size 2.5 2.5) (drill 1.5) (layers "*.Cu" "*.Mask")
      (net 12 "Net-(D12-A)") (pinfunction "2") (pintype "passive"))
    (model "${KICAD6_3RD_PARTY}/3dmodels/com_github_perigoso_keyswitch-kicad-library/3d-library.3dshapes/SW_Cherry_MX_Plate.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "kiswitch:SW_Cherry_MX_Plate_1.00u" (layer "F.Cu")
    (at 160.87875 49.64725)
    (descr "Cherry MX keyswitch Plate Mount Keycap 1.00u")
    (tags "Cherry MX Keyboard Keyswitch Switch Plate Cutout Keycap 1.00u")
    (property "Sheetfile" "demokeyboard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Push button switch, normally open, two pins, 45° tilted")
    (property "ki_keywords" "switch normally-open pushbutton push-button")
    (attr through_hole)
    (fp_text reference "MX8" (at 0 -8) (layer "F.SilkS"))
    (fp_text value "MX_SW_solder" (at 0 8) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 4 4) (drill 4) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle (at -3.81 -2.54) (size 2.5 2.5) (drill 1.5) (layers "*.Cu" "*.Mask")
      (net 70 "COL7") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 -5.08) (size 2.5 2.5) (drill 1.5) (layers "*.Cu" "*.Mask")
      (net 8 "Net-(D8-A)") (pinfunction "2") (pintype "passive"))
    (model "${KICAD6_3RD_PARTY}/3dmodels/com_github_perigoso_keyswitch-kicad-library/3d-library.3dshapes/SW_Cherry_MX_Plate.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "kiswitch:SW_Cherry_MX_Plate_1.00u" (layer "F.Cu")
    (at 65.62875 49.64725)
    (descr "Cherry MX keyswitch Plate Mount Keycap 1.00u")
    (tags "Cherry MX Keyboard Keyswitch Switch Plate Cutout Keycap 1.00u")
    (property "Sheetfile" "demokeyboard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Push button switch, normally open, two pins, 45° tilted")
    (property "ki_keywords" "switch normally-open pushbutton push-button")
    (attr through_hole)
    (fp_text reference "MX3" (at 0 -8) (layer "F.SilkS"))
    (fp_text value "MX_SW_solder" (at 0 8) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 4 4) (drill 4) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle (at -3.81 -2.54) (size 2.5 2.5) (drill 1.5) (layers "*.Cu" "*.Mask")
      (net 65 "COL2") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 -5.08) (size 2.5 2.5) (drill 1.5) (layers "*.Cu" "*.Mask")
      (net 3 "Net-(D3-A)") (pinfunction "2") (pintype "passive"))
    (model "${KICAD6_3RD_PARTY}/3dmodels/com_github_perigoso_keyswitch-kicad-library/3d-library.3dshapes/SW_Cherry_MX_Plate.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3" (layer "F.Cu")
    (at 164.3005 103.69275)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (property "Sheetfile" "demokeyboard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole without connection")
    (property "ki_keywords" "mounting hole")
    (attr exclude_from_pos_files)
    (fp_text reference "H4" (at 0 -4.2) (layer "F.SilkS"))
    (fp_text value "MountingHole" (at 0 4.2) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers "*.Cu" "*.Mask"))
  )
  (footprint "kiswitch:SW_Cherry_MX_Plate_1.00u" (layer "F.Cu")
    (at 79.91625 87.74725)
    (descr "Cherry MX keyswitch Plate Mount Keycap 1.00u")
    (tags "Cherry MX Keyboard Keyswitch Switch Plate Cutout Keycap 1.00u")
    (property "Sheetfile" "demokeyboard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Push button switch, normally open, two pins, 45° tilted")
    (property "ki_keywords" "switch normally-open pushbutton push-button")
    (attr through_hole)
    (fp_text reference "MX27" (at 0 -8) (layer "F.SilkS"))
    (fp_text value "MX_SW_solder" (at 0 8) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 4 4) (drill 4) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle (at -3.81 -2.54) (size 2.5 2.5) (drill 1.5) (layers "*.Cu" "*.Mask")
      (net 65 "COL2") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 -5.08) (size 2.5 2.5) (drill 1.5) (layers "*.Cu" "*.Mask")
      (net 27 "Net-(D27-A)") (pinfunction "2") (pintype "passive"))
    (model "${KICAD6_3RD_PARTY}/3dmodels/com_github_perigoso_keyswitch-kicad-library/3d-library.3dshapes/SW_Cherry_MX_Plate.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "kiswitch:SW_Cherry_MX_Plate_1.00u" (layer "F.Cu")
    (at 232.31625 87.74725)
    (descr "Cherry MX keyswitch Plate Mount Keycap 1.00u")
    (tags "Cherry MX Keyboard Keyswitch Switch Plate Cutout Keycap 1.00u")
    (property "Sheetfile" "demokeyboard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Push button switch, normally open, two pins, 45° tilted")
    (property "ki_keywords" "switch normally-open pushbutton push-button")
    (attr through_hole)
    (fp_text reference "MX35" (at 0 -8) (layer "F.SilkS"))
    (fp_text value "MX_SW_solder" (at 0 8) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 4 4) (drill 4) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle (at -3.81 -2.54) (size 2.5 2.5) (drill 1.5) (layers "*.Cu" "*.Mask")
      (net 73 "COL10") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 -5.08) (size 2.5 2.5) (drill 1.5) (layers "*.Cu" "*.Mask")
      (net 35 "Net-(D35-A)") (pinfunction "2") (pintype "passive"))
    (model "${KICAD6_3RD_PARTY}/3dmodels/com_github_perigoso_keyswitch-kicad-library/3d-library.3dshapes/SW_Cherry_MX_Plate.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "kiswitch:SW_Cherry_MX_Plate_1.00u" (layer "F.Cu")
    (at 84.67875 49.64725)
    (descr "Cherry MX keyswitch Plate Mount Keycap 1.00u")
    (tags "Cherry MX Keyboard Keyswitch Switch Plate Cutout Keycap 1.00u")
    (property "Sheetfile" "demokeyboard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Push button switch, normally open, two pins, 45° tilted")
    (property "ki_keywords" "switch normally-open pushbutton push-button")
    (attr through_hole)
    (fp_text reference "MX4" (at 0 -8) (layer "F.SilkS"))
    (fp_text value "MX_SW_solder" (at 0 8) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 4 4) (drill 4) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle (at -3.81 -2.54) (size 2.5 2.5) (drill 1.5) (layers "*.Cu" "*.Mask")
      (net 66 "COL3") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 -5.08) (size 2.5 2.5) (drill 1.5) (layers "*.Cu" "*.Mask")
      (net 4 "Net-(D4-A)") (pinfunction "2") (pintype "passive"))
    (model "${KICAD6_3RD_PARTY}/3dmodels/com_github_perigoso_keyswitch-kicad-library/3d-library.3dshapes/SW_Cherry_MX_Plate.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3" (layer "F.Cu")
    (at 231.9975 48.97525)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (property "Sheetfile" "demokeyboard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole without connection")
    (property "ki_keywords" "mounting hole")
    (attr exclude_from_pos_files)
    (fp_text reference "H2" (at 0 -4.2) (layer "F.SilkS"))
    (fp_text value "MountingHole" (at 0 4.2) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers "*.Cu" "*.Mask"))
  )
  (footprint "kiswitch:SW_Cherry_MX_Plate_1.00u" (layer "F.Cu")
    (at 75.15375 68.69725)
    (descr "Cherry MX keyswitch Plate Mount Keycap 1.00u")
    (tags "Cherry MX Keyboard Keyswitch Switch Plate Cutout Keycap 1.00u")
    (property "Sheetfile" "demokeyboard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Push button switch, normally open, two pins, 45° tilted")
    (property "ki_keywords" "switch normally-open pushbutton push-button")
    (attr through_hole)
    (fp_text reference "MX15" (at 0 -8) (layer "F.SilkS"))
    (fp_text value "MX_SW_solder" (at 0 8) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 4 4) (drill 4) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle (at -3.81 -2.54) (size 2.5 2.5) (drill 1.5) (layers "*.Cu" "*.Mask")
      (net 65 "COL2") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 -5.08) (size 2.5 2.5) (drill 1.5) (layers "*.Cu" "*.Mask")
      (net 15 "Net-(D15-A)") (pinfunction "2") (pintype "passive"))
    (model "${KICAD6_3RD_PARTY}/3dmodels/com_github_perigoso_keyswitch-kicad-library/3d-library.3dshapes/SW_Cherry_MX_Plate.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "kiswitch:SW_Cherry_MX_Plate_1.75u" (layer "F.Cu")
    (at 34.6725 87.74725)
    (descr "Cherry MX keyswitch Plate Mount Keycap 1.75u")
    (tags "Cherry MX Keyboard Keyswitch Switch Plate Cutout Keycap 1.75u")
    (property "Sheetfile" "demokeyboard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Push button switch, normally open, two pins, 45° tilted")
    (property "ki_keywords" "switch normally-open pushbutton push-button")
    (attr through_hole)
    (fp_text reference "MX25" (at 0 -8) (layer "F.SilkS"))
    (fp_text value "MX_SW_solder" (at 0 8) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 4 4) (drill 4) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle (at -3.81 -2.54) (size 2.5 2.5) (drill 1.5) (layers "*.Cu" "*.Mask")
      (net 63 "COL0") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 -5.08) (size 2.5 2.5) (drill 1.5) (layers "*.Cu" "*.Mask")
      (net 25 "Net-(D25-A)") (pinfunction "2") (pintype "passive"))
    (model "${KICAD6_3RD_PARTY}/3dmodels/com_github_perigoso_keyswitch-kicad-library/3d-library.3dshapes/SW_Cherry_MX_Plate.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "kiswitch:SW_Cherry_MX_Plate_1.00u" (layer "F.Cu")
    (at 175.16625 87.74725)
    (descr "Cherry MX keyswitch Plate Mount Keycap 1.00u")
    (tags "Cherry MX Keyboard Keyswitch Switch Plate Cutout Keycap 1.00u")
    (property "Sheetfile" "demokeyboard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Push button switch, normally open, two pins, 45° tilted")
    (property "ki_keywords" "switch normally-open pushbutton push-button")
    (attr through_hole)
    (fp_text reference "MX32" (at 0 -8) (layer "F.SilkS"))
    (fp_text value "MX_SW_solder" (at 0 8) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 4 4) (drill 4) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle (at -3.81 -2.54) (size 2.5 2.5) (drill 1.5) (layers "*.Cu" "*.Mask")
      (net 70 "COL7") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 -5.08) (size 2.5 2.5) (drill 1.5) (layers "*.Cu" "*.Mask")
      (net 32 "Net-(D32-A)") (pinfunction "2") (pintype "passive"))
    (model "${KICAD6_3RD_PARTY}/3dmodels/com_github_perigoso_keyswitch-kicad-library/3d-library.3dshapes/SW_Cherry_MX_Plate.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "kiswitch:SW_Cherry_MX_Plate_1.00u" (layer "F.Cu")
    (at 194.21625 87.74725)
    (descr "Cherry MX keyswitch Plate Mount Keycap 1.00u")
    (tags "Cherry MX Keyboard Keyswitch Switch Plate Cutout Keycap 1.00u")
    (property "Sheetfile" "demokeyboard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Push button switch, normally open, two pins, 45° tilted")
    (property "ki_keywords" "switch normally-open pushbutton push-button")
    (attr through_hole)
    (fp_text reference "MX33" (at 0 -8) (layer "F.SilkS"))
    (fp_text value "MX_SW_solder" (at 0 8) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 4 4) (drill 4) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle (at -3.81 -2.54) (size 2.5 2.5) (drill 1.5) (layers "*.Cu" "*.Mask")
      (net 71 "COL8") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 -5.08) (size 2.5 2.5) (drill 1.5) (layers "*.Cu" "*.Mask")
      (net 33 "Net-(D33-A)") (pinfunction "2") (pintype "passive"))
    (model "${KICAD6_3RD_PARTY}/3dmodels/com_github_perigoso_keyswitch-kicad-library/3d-library.3dshapes/SW_Cherry_MX_Plate.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "kiswitch:SW_Cherry_MX_Plate_1.50u" (layer "F.Cu")
    (at 32.29125 68.69725)
    (descr "Cherry MX keyswitch Plate Mount Keycap 1.50u")
    (tags "Cherry MX Keyboard Keyswitch Switch Plate Cutout Keycap 1.50u")
    (property "Sheetfile" "demokeyboard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Push button switch, normally open, two pins, 45° tilted")
    (property "ki_keywords" "switch normally-open pushbutton push-button")
    (attr through_hole)
    (fp_text reference "MX13" (at 0 -8) (layer "F.SilkS"))
    (fp_text value "MX_SW_solder" (at 0 8) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 4 4) (drill 4) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle (at -3.81 -2.54) (size 2.5 2.5) (drill 1.5) (layers "*.Cu" "*.Mask")
      (net 63 "COL0") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 -5.08) (size 2.5 2.5) (drill 1.5) (layers "*.Cu" "*.Mask")
      (net 13 "Net-(D13-A)") (pinfunction "2") (pintype "passive"))
    (model "${KICAD6_3RD_PARTY}/3dmodels/com_github_perigoso_keyswitch-kicad-library/3d-library.3dshapes/SW_Cherry_MX_Plate.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "kiswitch:SW_Cherry_MX_Plate_1.00u" (layer "F.Cu")
    (at 213.26625 106.79725)
    (descr "Cherry MX keyswitch Plate Mount Keycap 1.00u")
    (tags "Cherry MX Keyboard Keyswitch Switch Plate Cutout Keycap 1.00u")
    (property "Sheetfile" "demokeyboard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Push button switch, normally open, two pins, 45° tilted")
    (property "ki_keywords" "switch normally-open pushbutton push-button")
    (attr through_hole)
    (fp_text reference "MX44" (at 0 -8) (layer "F.SilkS"))
    (fp_text value "MX_SW_solder" (at 0 8) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 4 4) (drill 4) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle (at -3.81 -2.54) (size 2.5 2.5) (drill 1.5) (layers "*.Cu" "*.Mask")
      (net 72 "COL9") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 -5.08) (size 2.5 2.5) (drill 1.5) (layers "*.Cu" "*.Mask")
      (net 44 "Net-(D44-A)") (pinfunction "2") (pintype "passive"))
    (model "${KICAD6_3RD_PARTY}/3dmodels/com_github_perigoso_keyswitch-kicad-library/3d-library.3dshapes/SW_Cherry_MX_Plate.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "kiswitch:SW_Cherry_MX_Plate_1.00u" (layer "F.Cu")
    (at 208.50375 68.69725)
    (descr "Cherry MX keyswitch Plate Mount Keycap 1.00u")
    (tags "Cherry MX Keyboard Keyswitch Switch Plate Cutout Keycap 1.00u")
    (property "Sheetfile" "demokeyboard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Push button switch, normally open, two pins, 45° tilted")
    (property "ki_keywords" "switch normally-open pushbutton push-button")
    (attr through_hole)
    (fp_text reference "MX22" (at 0 -8) (layer "F.SilkS"))
    (fp_text value "MX_SW_solder" (at 0 8) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 4 4) (drill 4) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle (at -3.81 -2.54) (size 2.5 2.5) (drill 1.5) (layers "*.Cu" "*.Mask")
      (net 72 "COL9") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 -5.08) (size 2.5 2.5) (drill 1.5) (layers "*.Cu" "*.Mask")
      (net 22 "Net-(D22-A)") (pinfunction "2") (pintype "passive"))
    (model "${KICAD6_3RD_PARTY}/3dmodels/com_github_perigoso_keyswitch-kicad-library/3d-library.3dshapes/SW_Cherry_MX_Plate.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_SOD-123" (layer "B.Cu")
    (at 37.8475 88.541 90)
    (descr "SOD-123")
    (tags "SOD-123")
    (property "LCSC" "C81598")
    (property "Sheetfile" "demokeyboard.kicad_sch")
    (property "Sheetname" "")
    (property "Sim.Device" "D")
    (property "Sim.Pins" "1=K 2=A")
    (property "ki_description" "Diode, small symbol")
    (property "ki_keywords" "diode")
    (attr smd)
    (fp_text reference "D25" (at 0 2 90) (layer "B.SilkS"))
    (fp_text value "D_Small" (at 0 -2.1 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1.65 0 90) (size 0.9 1.2) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 61 "ROW2") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 1.65 0 90) (size 0.9 1.2) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 25 "Net-(D25-A)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SOD-123.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "B.Cu")
    (at 47.485 83.33275)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "LCSC" "C108463")
    (property "Sheetfile" "demokeyboard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C1" (at 0 1.43 180) (layer "B.SilkS"))
    (fp_text value "C_Small" (at 0 -1.43 180) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 180) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.775 0) (size 0.9 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 87 "VSS") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0) (size 0.9 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 82 "VDD") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_SOD-123" (layer "B.Cu")
    (at 87.85375 50.5035 90)
    (descr "SOD-123")
    (tags "SOD-123")
    (property "LCSC" "C81598")
    (property "Sheetfile" "demokeyboard.kicad_sch")
    (property "Sheetname" "")
    (property "Sim.Device" "D")
    (property "Sim.Pins" "1=K 2=A")
    (property "ki_description" "Diode, small symbol")
    (property "ki_keywords" "diode")
    (attr smd)
    (fp_text reference "D4" (at 0 2 90) (layer "B.SilkS"))
    (fp_text value "D_Small" (at 0 -2.1 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1.65 0 90) (size 0.9 1.2) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 59 "ROW0") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 1.65 0 90) (size 0.9 1.2) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 4 "Net-(D4-A)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SOD-123.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "B.Cu")
    (at 39.5955 53.30175)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "LCSC" "C4184")
    (property "Sheetfile" "demokeyboard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, small symbol")
    (property "ki_keywords" "R resistor")
    (attr smd)
    (fp_text reference "R1" (at 0 1.43) (layer "B.SilkS"))
    (fp_text value "R_Small" (at 0 -1.43) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.825 0) (size 0.8 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 88 "DIN") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0) (size 0.8 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 92 "Net-(D47-DIN)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_SOD-123" (layer "B.Cu")
    (at 154.52875 69.5535 90)
    (descr "SOD-123")
    (tags "SOD-123")
    (property "LCSC" "C81598")
    (property "Sheetfile" "demokeyboard.kicad_sch")
    (property "Sheetname" "")
    (property "Sim.Device" "D")
    (property "Sim.Pins" "1=K 2=A")
    (property "ki_description" "Diode, small symbol")
    (property "ki_keywords" "diode")
    (attr smd)
    (fp_text reference "D19" (at 0 2 90) (layer "B.SilkS"))
    (fp_text value "D_Small" (at 0 -2.1 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1.65 0 90) (size 0.9 1.2) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 60 "ROW1") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 1.65 0 90) (size 0.9 1.2) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 19 "Net-(D19-A)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SOD-123.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "1655:LED_1655" (layer "B.Cu")
    (at 238.2225 63.14725)
    (property "Availability" "In Stock")
    (property "Check_prices" "https://www.snapeda.com/parts/1655/Adafruit+Industries+LLC/view-part/?ref=eda")
    (property "Description" "\nAddressable Lighting Neopixel 10 LED Discrete Serial (Shift Register) Red, Green, Blue (RGB) 5.00mm L x 5.00mm W\n")
    (property "MANUFACTURER" "Adafruit Industries")
    (property "MAXIMUM_PACKAGE_HEIGHT" "1.6 mm")
    (property "MF" "Adafruit")
    (property "MP" "1655")
    (property "PARTREV" "01")
    (property "Package" "Adafruit")
    (property "Price" "None")
    (property "STANDARD" "Manufacturer recommendations")
    (property "Sheetfile" "demokeyboard.kicad_sch")
    (property "Sheetname" "")
    (property "SnapEDA_Link" "https://www.snapeda.com/parts/1655/Adafruit+Industries+LLC/view-part/?ref=snap")
    (attr smd)
    (fp_text reference "D49" (at -0.325 3.635) (layer "B.SilkS"))
    (fp_text value "1655" (at 1.58 -3.635) (layer "B.Fab"))
    (pad "1" smd rect (at -2.45 1.6 270) (size 1 1.5) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 87 "VSS") (pinfunction "VSS") (pintype "power_in") (solder_mask_margin 0.102))
    (pad "2" smd rect (at -2.45 -1.6 270) (size 1 1.5) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 83 "Net-(D48-DOUT)") (pinfunction "DIN") (pintype "input") (solder_mask_margin 0.102))
    (pad "3" smd rect (at 2.45 -1.6 270) (size 1 1.5) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 82 "VDD") (pinfunction "VDD") (pintype "power_in") (solder_mask_margin 0.102))
    (pad "4" smd rect (at 2.45 1.6 270) (size 1 1.5) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 84 "Net-(D49-DOUT)") (pinfunction "DOUT") (pintype "output") (solder_mask_margin 0.102))
  )
  (footprint "Diode_SMD:D_SOD-123" (layer "B.Cu")
    (at 173.57875 69.5535 90)
    (descr "SOD-123")
    (tags "SOD-123")
    (property "LCSC" "C81598")
    (property "Sheetfile" "demokeyboard.kicad_sch")
    (property "Sheetname" "")
    (property "Sim.Device" "D")
    (property "Sim.Pins" "1=K 2=A")
    (property "ki_description" "Diode, small symbol")
    (property "ki_keywords" "diode")
    (attr smd)
    (fp_text reference "D20" (at 0 2 90) (layer "B.SilkS"))
    (fp_text value "D_Small" (at 0 -2.1 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1.65 0 90) (size 0.9 1.2) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 60 "ROW1") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 1.65 0 90) (size 0.9 1.2) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 20 "Net-(D20-A)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SOD-123.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "1655:LED_1655" (layer "B.Cu")
    (at 237.2225 96.14725 180)
    (property "Availability" "In Stock")
    (property "Check_prices" "https://www.snapeda.com/parts/1655/Adafruit+Industries+LLC/view-part/?ref=eda")
    (property "Description" "\nAddressable Lighting Neopixel 10 LED Discrete Serial (Shift Register) Red, Green, Blue (RGB) 5.00mm L x 5.00mm W\n")
    (property "MANUFACTURER" "Adafruit Industries")
    (property "MAXIMUM_PACKAGE_HEIGHT" "1.6 mm")
    (property "MF" "Adafruit")
    (property "MP" "1655")
    (property "PARTREV" "01")
    (property "Package" "Adafruit")
    (property "Price" "None")
    (property "STANDARD" "Manufacturer recommendations")
    (property "Sheetfile" "demokeyboard.kicad_sch")
    (property "Sheetname" "")
    (property "SnapEDA_Link" "https://www.snapeda.com/parts/1655/Adafruit+Industries+LLC/view-part/?ref=snap")
    (attr smd)
    (fp_text reference "D50" (at -0.325 3.635) (layer "B.SilkS"))
    (fp_text value "1655" (at 1.58 -3.635) (layer "B.Fab"))
    (pad "1" smd rect (at -2.45 1.6 90) (size 1 1.5) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 87 "VSS") (pinfunction "VSS") (pintype "power_in") (solder_mask_margin 0.102))
    (pad "2" smd rect (at -2.45 -1.6 90) (size 1 1.5) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 84 "Net-(D49-DOUT)") (pinfunction "DIN") (pintype "input") (solder_mask_margin 0.102))
    (pad "3" smd rect (at 2.45 -1.6 90) (size 1 1.5) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 82 "VDD") (pinfunction "VDD") (pintype "power_in") (solder_mask_margin 0.102))
    (pad "4" smd rect (at 2.45 1.6 90) (size 1 1.5) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 85 "Net-(D50-DOUT)") (pinfunction "DOUT") (pintype "output") (solder_mask_margin 0.102))
  )
  (footprint "Diode_SMD:D_SOD-123" (layer "B.Cu")
    (at 49.75375 50.5035 90)
    (descr "SOD-123")
    (tags "SOD-123")
    (property "LCSC" "C81598")
    (property "Sheetfile" "demokeyboard.kicad_sch")
    (property "Sheetname" "")
    (property "Sim.Device" "D")
    (property "Sim.Pins" "1=K 2=A")
    (property "ki_description" "Diode, small symbol")
    (property "ki_keywords" "diode")
    (attr smd)
    (fp_text reference "D2" (at 0 2 90) (layer "B.SilkS"))
    (fp_text value "D_Small" (at 0 -2.1 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1.65 0 90) (size 0.9 1.2) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 59 "ROW0") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 1.65 0 90) (size 0.9 1.2) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "Net-(D2-A)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SOD-123.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_SOD-123" (layer "B.Cu")
    (at 33.085 107.6535 90)
    (descr "SOD-123")
    (tags "SOD-123")
    (property "LCSC" "C81598")
    (property "Sheetfile" "demokeyboard.kicad_sch")
    (property "Sheetname" "")
    (property "Sim.Device" "D")
    (property "Sim.Pins" "1=K 2=A")
    (property "ki_description" "Diode, small symbol")
    (property "ki_keywords" "diode")
    (attr smd)
    (fp_text reference "D37" (at 0 2 90) (layer "B.SilkS"))
    (fp_text value "D_Small" (at 0 -2.1 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1.65 0 90) (size 0.9 1.2) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 62 "ROW3") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 1.65 0 90) (size 0.9 1.2) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 37 "Net-(D37-A)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SOD-123.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_SOD-123" (layer "B.Cu")
    (at 202.15375 50.441 90)
    (descr "SOD-123")
    (tags "SOD-123")
    (property "LCSC" "C81598")
    (property "Sheetfile" "demokeyboard.kicad_sch")
    (property "Sheetname" "")
    (property "Sim.Device" "D")
    (property "Sim.Pins" "1=K 2=A")
    (property "ki_description" "Diode, small symbol")
    (property "ki_keywords" "diode")
    (attr smd)
    (fp_text reference "D10" (at 0 2 90) (layer "B.SilkS"))
    (fp_text value "D_Small" (at 0 -2.1 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1.65 0 90) (size 0.9 1.2) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 59 "ROW0") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 1.65 0 90) (size 0.9 1.2) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 10 "Net-(D10-A)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SOD-123.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_SOD-123" (layer "B.Cu")
    (at 221.20375 50.5035 90)
    (descr "SOD-123")
    (tags "SOD-123")
    (property "LCSC" "C81598")
    (property "Sheetfile" "demokeyboard.kicad_sch")
    (property "Sheetname" "")
    (property "Sim.Device" "D")
    (property "Sim.Pins" "1=K 2=A")
    (property "ki_description" "Diode, small symbol")
    (property "ki_keywords" "diode")
    (attr smd)
    (fp_text reference "D11" (at 0 2 90) (layer "B.SilkS"))
    (fp_text value "D_Small" (at 0 -2.1 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1.65 0 90) (size 0.9 1.2) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 59 "ROW0") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 1.65 0 90) (size 0.9 1.2) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 11 "Net-(D11-A)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SOD-123.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_SOD-123" (layer "B.Cu")
    (at 216.44125 88.6035 90)
    (descr "SOD-123")
    (tags "SOD-123")
    (property "LCSC" "C81598")
    (property "Sheetfile" "demokeyboard.kicad_sch")
    (property "Sheetname" "")
    (property "Sim.Device" "D")
    (property "Sim.Pins" "1=K 2=A")
    (property "ki_description" "Diode, small symbol")
    (property "ki_keywords" "diode")
    (attr smd)
    (fp_text reference "D34" (at 0 2 90) (layer "B.SilkS"))
    (fp_text value "D_Small" (at 0 -2.1 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1.65 0 90) (size 0.9 1.2) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 61 "ROW2") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 1.65 0 90) (size 0.9 1.2) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 34 "Net-(D34-A)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SOD-123.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_SOD-123" (layer "B.Cu")
    (at 125.95375 50.5035 90)
    (descr "SOD-123")
    (tags "SOD-123")
    (property "LCSC" "C81598")
    (property "Sheetfile" "demokeyboard.kicad_sch")
    (property "Sheetname" "")
    (property "Sim.Device" "D")
    (property "Sim.Pins" "1=K 2=A")
    (property "ki_description" "Diode, small symbol")
    (property "ki_keywords" "diode")
    (attr smd)
    (fp_text reference "D6" (at 0 2 90) (layer "B.SilkS"))
    (fp_text value "D_Small" (at 0 -2.1 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1.65 0 90) (size 0.9 1.2) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 59 "ROW0") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 1.65 0 90) (size 0.9 1.2) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 6 "Net-(D6-A)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SOD-123.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_SOD-123" (layer "B.Cu")
    (at 150.0485 107.6535 90)
    (descr "SOD-123")
    (tags "SOD-123")
    (property "LCSC" "C81598")
    (property "Sheetfile" "demokeyboard.kicad_sch")
    (property "Sheetname" "")
    (property "Sim.Device" "D")
    (property "Sim.Pins" "1=K 2=A")
    (property "ki_description" "Diode, small symbol")
    (property "ki_keywords" "diode")
    (attr smd)
    (fp_text reference "D41" (at 0 2 90) (layer "B.SilkS"))
    (fp_text value "D_Small" (at 0 -2.1 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1.65 0 90) (size 0.9 1.2) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 62 "ROW3") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 1.65 0 90) (size 0.9 1.2) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 41 "Net-(D41-A)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SOD-123.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_SOD-123" (layer "B.Cu")
    (at 252.16 69.5535 90)
    (descr "SOD-123")
    (tags "SOD-123")
    (property "LCSC" "C81598")
    (property "Sheetfile" "demokeyboard.kicad_sch")
    (property "Sheetname" "")
    (property "Sim.Device" "D")
    (property "Sim.Pins" "1=K 2=A")
    (property "ki_description" "Diode, small symbol")
    (property "ki_keywords" "diode")
    (attr smd)
    (fp_text reference "D24" (at 0 2 90) (layer "B.SilkS"))
    (fp_text value "D_Small" (at 0 -2.1 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1.65 0 90) (size 0.9 1.2) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 60 "ROW1") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 1.65 0 90) (size 0.9 1.2) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 24 "Net-(D24-A)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SOD-123.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_SOD-123" (layer "B.Cu")
    (at 254.54125 107.6535 90)
    (descr "SOD-123")
    (tags "SOD-123")
    (property "LCSC" "C81598")
    (property "Sheetfile" "demokeyboard.kicad_sch")
    (property "Sheetname" "")
    (property "Sim.Device" "D")
    (property "Sim.Pins" "1=K 2=A")
    (property "ki_description" "Diode, small symbol")
    (property "ki_keywords" "diode")
    (attr smd)
    (fp_text reference "D46" (at 0 2 90) (layer "B.SilkS"))
    (fp_text value "D_Small" (at 0 -2.1 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1.65 0 90) (size 0.9 1.2) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 62 "ROW3") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 1.65 0 90) (size 0.9 1.2) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 46 "Net-(D46-A)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SOD-123.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_SOD-123" (layer "B.Cu")
    (at 197.39125 88.6035 90)
    (descr "SOD-123")
    (tags "SOD-123")
    (property "LCSC" "C81598")
    (property "Sheetfile" "demokeyboard.kicad_sch")
    (property "Sheetname" "")
    (property "Sim.Device" "D")
    (property "Sim.Pins" "1=K 2=A")
    (property "ki_description" "Diode, small symbol")
    (property "ki_keywords" "diode")
    (attr smd)
    (fp_text reference "D33" (at 0 2 90) (layer "B.SilkS"))
    (fp_text value "D_Small" (at 0 -2.1 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1.65 0 90) (size 0.9 1.2) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 61 "ROW2") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 1.65 0 90) (size 0.9 1.2) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 33 "Net-(D33-A)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SOD-123.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_SOD-123" (layer "B.Cu")
    (at 59.27875 69.491 90)
    (descr "SOD-123")
    (tags "SOD-123")
    (property "LCSC" "C81598")
    (property "Sheetfile" "demokeyboard.kicad_sch")
    (property "Sheetname" "")
    (property "Sim.Device" "D")
    (property "Sim.Pins" "1=K 2=A")
    (property "ki_description" "Diode, small symbol")
    (property "ki_keywords" "diode")
    (attr smd)
    (fp_text reference "D14" (at 0 2 90) (layer "B.SilkS"))
    (fp_text value "D_Small" (at 0 -2.1 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1.65 0 90) (size 0.9 1.2) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 60 "ROW1") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 1.65 0 90) (size 0.9 1.2) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 14 "Net-(D14-A)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SOD-123.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_SOD-123" (layer "B.Cu")
    (at 116.42875 69.5535 90)
    (descr "SOD-123")
    (tags "SOD-123")
    (property "LCSC" "C81598")
    (property "Sheetfile" "demokeyboard.kicad_sch")
    (property "Sheetname" "")
    (property "Sim.Device" "D")
    (property "Sim.Pins" "1=K 2=A")
    (property "ki_description" "Diode, small symbol")
    (property "ki_keywords" "diode")
    (attr smd)
    (fp_text reference "D17" (at 0 2 90) (layer "B.SilkS"))
    (fp_text value "D_Small" (at 0 -2.1 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1.65 0 90) (size 0.9 1.2) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 60 "ROW1") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 1.65 0 90) (size 0.9 1.2) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 17 "Net-(D17-A)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SOD-123.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_SOD-123" (layer "B.Cu")
    (at 102.457 88.541 90)
    (descr "SOD-123")
    (tags "SOD-123")
    (property "LCSC" "C81598")
    (property "Sheetfile" "demokeyboard.kicad_sch")
    (property "Sheetname" "")
    (property "Sim.Device" "D")
    (property "Sim.Pins" "1=K 2=A")
    (property "ki_description" "Diode, small symbol")
    (property "ki_keywords" "diode")
    (attr smd)
    (fp_text reference "D28" (at 0 2 90) (layer "B.SilkS"))
    (fp_text value "D_Small" (at 0 -2.1 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1.65 0 90) (size 0.9 1.2) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 61 "ROW2") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 1.65 0 90) (size 0.9 1.2) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 28 "Net-(D28-A)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SOD-123.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_SOD-123" (layer "B.Cu")
    (at 145.00375 50.5035 90)
    (descr "SOD-123")
    (tags "SOD-123")
    (property "LCSC" "C81598")
    (property "Sheetfile" "demokeyboard.kicad_sch")
    (property "Sheetname" "")
    (property "Sim.Device" "D")
    (property "Sim.Pins" "1=K 2=A")
    (property "ki_description" "Diode, small symbol")
    (property "ki_keywords" "diode")
    (attr smd)
    (fp_text reference "D7" (at 0 2 90) (layer "B.SilkS"))
    (fp_text value "D_Small" (at 0 -2.1 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1.65 0 90) (size 0.9 1.2) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 59 "ROW0") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 1.65 0 90) (size 0.9 1.2) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 7 "Net-(D7-A)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SOD-123.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_SOD-123" (layer "B.Cu")
    (at 35.46625 69.5535 90)
    (descr "SOD-123")
    (tags "SOD-123")
    (property "LCSC" "C81598")
    (property "Sheetfile" "demokeyboard.kicad_sch")
    (property "Sheetname" "")
    (property "Sim.Device" "D")
    (property "Sim.Pins" "1=K 2=A")
    (property "ki_description" "Diode, small symbol")
    (property "ki_keywords" "diode")
    (attr smd)
    (fp_text reference "D13" (at 0 2 90) (layer "B.SilkS"))
    (fp_text value "D_Small" (at 0 -2.1 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1.65 0 90) (size 0.9 1.2) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 60 "ROW1") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 1.65 0 90) (size 0.9 1.2) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 13 "Net-(D13-A)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SOD-123.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_SOD-123" (layer "B.Cu")
    (at 68.80375 50.5035 90)
    (descr "SOD-123")
    (tags "SOD-123")
    (property "LCSC" "C81598")
    (property "Sheetfile" "demokeyboard.kicad_sch")
    (property "Sheetname" "")
    (property "Sim.Device" "D")
    (property "Sim.Pins" "1=K 2=A")
    (property "ki_description" "Diode, small symbol")
    (property "ki_keywords" "diode")
    (attr smd)
    (fp_text reference "D3" (at 0 2 90) (layer "B.SilkS"))
    (fp_text value "D_Small" (at 0 -2.1 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1.65 0 90) (size 0.9 1.2) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 59 "ROW0") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 1.65 0 90) (size 0.9 1.2) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 3 "Net-(D3-A)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SOD-123.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_SOD-123" (layer "B.Cu")
    (at 254.54125 88.6035 90)
    (descr "SOD-123")
    (tags "SOD-123")
    (property "LCSC" "C81598")
    (property "Sheetfile" "demokeyboard.kicad_sch")
    (property "Sheetname" "")
    (property "Sim.Device" "D")
    (property "Sim.Pins" "1=K 2=A")
    (property "ki_description" "Diode, small symbol")
    (property "ki_keywords" "diode")
    (attr smd)
    (fp_text reference "D36" (at 0 2 90) (layer "B.SilkS"))
    (fp_text value "D_Small" (at 0 -2.1 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1.65 0 90) (size 0.9 1.2) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 61 "ROW2") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 1.65 0 90) (size 0.9 1.2) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 36 "Net-(D36-A)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SOD-123.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_SOD-123" (layer "B.Cu")
    (at 183.10375 50.5035 90)
    (descr "SOD-123")
    (tags "SOD-123")
    (property "LCSC" "C81598")
    (property "Sheetfile" "demokeyboard.kicad_sch")
    (property "Sheetname" "")
    (property "Sim.Device" "D")
    (property "Sim.Pins" "1=K 2=A")
    (property "ki_description" "Diode, small symbol")
    (property "ki_keywords" "diode")
    (attr smd)
    (fp_text reference "D9" (at 0 2 90) (layer "B.SilkS"))
    (fp_text value "D_Small" (at 0 -2.1 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1.65 0 90) (size 0.9 1.2) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 59 "ROW0") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 1.65 0 90) (size 0.9 1.2) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 9 "Net-(D9-A)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SOD-123.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_SOD-123" (layer "B.Cu")
    (at 80.71 107.591 90)
    (descr "SOD-123")
    (tags "SOD-123")
    (property "LCSC" "C81598")
    (property "Sheetfile" "demokeyboard.kicad_sch")
    (property "Sheetname" "")
    (property "Sim.Device" "D")
    (property "Sim.Pins" "1=K 2=A")
    (property "ki_description" "Diode, small symbol")
    (property "ki_keywords" "diode")
    (attr smd)
    (fp_text reference "D39" (at 0 2 90) (layer "B.SilkS"))
    (fp_text value "D_Small" (at 0 -2.1 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1.65 0 90) (size 0.9 1.2) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 62 "ROW3") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 1.65 0 90) (size 0.9 1.2) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 39 "Net-(D39-A)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SOD-123.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_SOD-123" (layer "B.Cu")
    (at 30.70375 50.5035 90)
    (descr "SOD-123")
    (tags "SOD-123")
    (property "LCSC" "C81598")
    (property "Sheetfile" "demokeyboard.kicad_sch")
    (property "Sheetname" "")
    (property "Sim.Device" "D")
    (property "Sim.Pins" "1=K 2=A")
    (property "ki_description" "Diode, small symbol")
    (property "ki_keywords" "diode")
    (attr smd)
    (fp_text reference "D1" (at 0 2 270) (layer "B.SilkS"))
    (fp_text value "D_Small" (at 0 -2.1 270) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2 270) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1.65 0 90) (size 0.9 1.2) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 59 "ROW0") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 1.65 0 90) (size 0.9 1.2) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 1 "Net-(D1-A)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SOD-123.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_SOD-123" (layer "B.Cu")
    (at 111.66625 107.6535 90)
    (descr "SOD-123")
    (tags "SOD-123")
    (property "LCSC" "C81598")
    (property "Sheetfile" "demokeyboard.kicad_sch")
    (property "Sheetname" "")
    (property "Sim.Device" "D")
    (property "Sim.Pins" "1=K 2=A")
    (property "ki_description" "Diode, small symbol")
    (property "ki_keywords" "diode")
    (attr smd)
    (fp_text reference "D40" (at 0 2 90) (layer "B.SilkS"))
    (fp_text value "D_Small" (at 0 -2.1 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1.65 0 90) (size 0.9 1.2) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 62 "ROW3") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 1.65 0 90) (size 0.9 1.2) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 40 "Net-(D40-A)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SOD-123.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_SOD-123" (layer "B.Cu")
    (at 197.39125 107.6535 90)
    (descr "SOD-123")
    (tags "SOD-123")
    (property "LCSC" "C81598")
    (property "Sheetfile" "demokeyboard.kicad_sch")
    (property "Sheetname" "")
    (property "Sim.Device" "D")
    (property "Sim.Pins" "1=K 2=A")
    (property "ki_description" "Diode, small symbol")
    (property "ki_keywords" "diode")
    (attr smd)
    (fp_text reference "D43" (at 0 2 90) (layer "B.SilkS"))
    (fp_text value "D_Small" (at 0 -2.1 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1.65 0 90) (size 0.9 1.2) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 62 "ROW3") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 1.65 0 90) (size 0.9 1.2) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 43 "Net-(D43-A)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SOD-123.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_SOD-123" (layer "B.Cu")
    (at 192.62875 69.491 90)
    (descr "SOD-123")
    (tags "SOD-123")
    (property "LCSC" "C81598")
    (property "Sheetfile" "demokeyboard.kicad_sch")
    (property "Sheetname" "")
    (property "Sim.Device" "D")
    (property "Sim.Pins" "1=K 2=A")
    (property "ki_description" "Diode, small symbol")
    (property "ki_keywords" "diode")
    (attr smd)
    (fp_text reference "D21" (at 0 2 90) (layer "B.SilkS"))
    (fp_text value "D_Small" (at 0 -2.1 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1.65 0 90) (size 0.9 1.2) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 60 "ROW1") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 1.65 0 90) (size 0.9 1.2) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 21 "Net-(D21-A)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SOD-123.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinSocket_2.54mm:PinSocket_1x20_P2.54mm_Vertical" (layer "B.Cu")
    (at 68.854803 58.49754 90)
    (descr "Through hole straight socket strip, 1x20, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x20 2.54mm single row")
    (property "Sheetfile" "demokeyboard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x20, script generated")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J1" (at 0 2.77 90) (layer "B.SilkS"))
    (fp_text value "Conn_01x20_Pin" (at 0 -51.03 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -24.13) (layer "B.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 76 "unconnected-(J1-Pin_1-Pad1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 -2.54 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 77 "unconnected-(J1-Pin_2-Pad2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 -5.08 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 78 "unconnected-(J1-Pin_3-Pad3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 -7.62 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 47 "unconnected-(J1-Pin_4-Pad4)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 -10.16 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 48 "unconnected-(J1-Pin_5-Pad5)") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 0 -12.7 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 49 "unconnected-(J1-Pin_6-Pad6)") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole oval (at 0 -15.24 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 50 "unconnected-(J1-Pin_7-Pad7)") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" thru_hole oval (at 0 -17.78 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 51 "unconnected-(J1-Pin_8-Pad8)") (pinfunction "Pin_8") (pintype "passive"))
    (pad "9" thru_hole oval (at 0 -20.32 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 91 "unconnected-(J1-Pin_9-Pad9)") (pinfunction "Pin_9") (pintype "passive"))
    (pad "10" thru_hole oval (at 0 -22.86 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 74 "COL11") (pinfunction "Pin_10") (pintype "passive"))
    (pad "11" thru_hole oval (at 0 -25.4 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 73 "COL10") (pinfunction "Pin_11") (pintype "passive"))
    (pad "12" thru_hole oval (at 0 -27.94 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 72 "COL9") (pinfunction "Pin_12") (pintype "passive"))
    (pad "13" thru_hole oval (at 0 -30.48 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 79 "unconnected-(J1-Pin_13-Pad13)") (pinfunction "Pin_13") (pintype "passive"))
    (pad "14" thru_hole oval (at 0 -33.02 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 71 "COL8") (pinfunction "Pin_14") (pintype "passive"))
    (pad "15" thru_hole oval (at 0 -35.56 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 70 "COL7") (pinfunction "Pin_15") (pintype "passive"))
    (pad "16" thru_hole oval (at 0 -38.1 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 60 "ROW1") (pinfunction "Pin_16") (pintype "passive"))
    (pad "17" thru_hole oval (at 0 -40.64 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 61 "ROW2") (pinfunction "Pin_17") (pintype "passive"))
    (pad "18" thru_hole oval (at 0 -43.18 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 75 "unconnected-(J1-Pin_18-Pad18)") (pinfunction "Pin_18") (pintype "passive"))
    (pad "19" thru_hole oval (at 0 -45.72 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 62 "ROW3") (pinfunction "Pin_19") (pintype "passive"))
    (pad "20" thru_hole oval (at 0 -48.26 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 59 "ROW0") (pinfunction "Pin_20") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x20_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinSocket_2.54mm:PinSocket_1x20_P2.54mm_Vertical" (layer "B.Cu")
    (at 68.838545 40.718005 90)
    (descr "Through hole straight socket strip, 1x20, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x20 2.54mm single row")
    (property "Sheetfile" "demokeyboard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x20, script generated")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J2" (at 0 2.77 90) (layer "B.SilkS"))
    (fp_text value "Conn_01x20_Pin" (at 0 -51.03 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -24.13) (layer "B.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 93 "unconnected-(J2-Pin_1-Pad1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 -2.54 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 82 "VDD") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 -5.08 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 52 "unconnected-(J2-Pin_3-Pad3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 -7.62 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 53 "unconnected-(J2-Pin_4-Pad4)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 -10.16 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 54 "unconnected-(J2-Pin_5-Pad5)") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 0 -12.7 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 89 "unconnected-(J2-Pin_6-Pad6)") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole oval (at 0 -15.24 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 55 "unconnected-(J2-Pin_7-Pad7)") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" thru_hole oval (at 0 -17.78 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 56 "unconnected-(J2-Pin_8-Pad8)") (pinfunction "Pin_8") (pintype "passive"))
    (pad "9" thru_hole oval (at 0 -20.32 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 90 "unconnected-(J2-Pin_9-Pad9)") (pinfunction "Pin_9") (pintype "passive"))
    (pad "10" thru_hole oval (at 0 -22.86 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 88 "DIN") (pinfunction "Pin_10") (pintype "passive"))
    (pad "11" thru_hole oval (at 0 -25.4 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 57 "unconnected-(J2-Pin_11-Pad11)") (pinfunction "Pin_11") (pintype "passive"))
    (pad "12" thru_hole oval (at 0 -27.94 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 69 "COL6") (pinfunction "Pin_12") (pintype "passive"))
    (pad "13" thru_hole oval (at 0 -30.48 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 58 "unconnected-(J2-Pin_13-Pad13)") (pinfunction "Pin_13") (pintype "passive"))
    (pad "14" thru_hole oval (at 0 -33.02 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 68 "COL5") (pinfunction "Pin_14") (pintype "passive"))
    (pad "15" thru_hole oval (at 0 -35.56 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 67 "COL4") (pinfunction "Pin_15") (pintype "passive"))
    (pad "16" thru_hole oval (at 0 -38.1 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 66 "COL3") (pinfunction "Pin_16") (pintype "passive"))
    (pad "17" thru_hole oval (at 0 -40.64 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 65 "COL2") (pinfunction "Pin_17") (pintype "passive"))
    (pad "18" thru_hole oval (at 0 -43.18 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 87 "VSS") (pinfunction "Pin_18") (pintype "passive"))
    (pad "19" thru_hole oval (at 0 -45.72 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 64 "COL1") (pinfunction "Pin_19") (pintype "passive"))
    (pad "20" thru_hole oval (at 0 -48.26 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 63 "COL0") (pinfunction "Pin_20") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x20_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_SOD-123" (layer "B.Cu")
    (at 64.04125 88.6035 90)
    (descr "SOD-123")
    (tags "SOD-123")
    (property "LCSC" "C81598")
    (property "Sheetfile" "demokeyboard.kicad_sch")
    (property "Sheetname" "")
    (property "Sim.Device" "D")
    (property "Sim.Pins" "1=K 2=A")
    (property "ki_description" "Diode, small symbol")
    (property "ki_keywords" "diode")
    (attr smd)
    (fp_text reference "D26" (at 0 2 90) (layer "B.SilkS"))
    (fp_text value "D_Small" (at 0 -2.1 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1.65 0 90) (size 0.9 1.2) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 61 "ROW2") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 1.65 0 90) (size 0.9 1.2) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 26 "Net-(D26-A)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SOD-123.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_SOD-123" (layer "B.Cu")
    (at 140.24125 88.541 90)
    (descr "SOD-123")
    (tags "SOD-123")
    (property "LCSC" "C81598")
    (property "Sheetfile" "demokeyboard.kicad_sch")
    (property "Sheetname" "")
    (property "Sim.Device" "D")
    (property "Sim.Pins" "1=K 2=A")
    (property "ki_description" "Diode, small symbol")
    (property "ki_keywords" "diode")
    (attr smd)
    (fp_text reference "D30" (at 0 2 90) (layer "B.SilkS"))
    (fp_text value "D_Small" (at 0 -2.1 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1.65 0 90) (size 0.9 1.2) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 61 "ROW2") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 1.65 0 90) (size 0.9 1.2) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 30 "Net-(D30-A)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SOD-123.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_SOD-123" (layer "B.Cu")
    (at 56.8975 107.6535 90)
    (descr "SOD-123")
    (tags "SOD-123")
    (property "LCSC" "C81598")
    (property "Sheetfile" "demokeyboard.kicad_sch")
    (property "Sheetname" "")
    (property "Sim.Device" "D")
    (property "Sim.Pins" "1=K 2=A")
    (property "ki_description" "Diode, small symbol")
    (property "ki_keywords" "diode")
    (attr smd)
    (fp_text reference "D38" (at 0 2 90) (layer "B.SilkS"))
    (fp_text value "D_Small" (at 0 -2.1 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1.65 0 90) (size 0.9 1.2) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 62 "ROW3") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 1.65 0 90) (size 0.9 1.2) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 38 "Net-(D38-A)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SOD-123.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_SOD-123" (layer "B.Cu")
    (at 135.47875 69.5535 90)
    (descr "SOD-123")
    (tags "SOD-123")
    (property "LCSC" "C81598")
    (property "Sheetfile" "demokeyboard.kicad_sch")
    (property "Sheetname" "")
    (property "Sim.Device" "D")
    (property "Sim.Pins" "1=K 2=A")
    (property "ki_description" "Diode, small symbol")
    (property "ki_keywords" "diode")
    (attr smd)
    (fp_text reference "D18" (at 0 2 90) (layer "B.SilkS"))
    (fp_text value "D_Small" (at 0 -2.1 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1.65 0 90) (size 0.9 1.2) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 60 "ROW1") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 1.65 0 90) (size 0.9 1.2) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 18 "Net-(D18-A)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SOD-123.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "1655:LED_1655" (layer "B.Cu")
    (at 127.7725 97.74725 180)
    (property "Availability" "In Stock")
    (property "Check_prices" "https://www.snapeda.com/parts/1655/Adafruit+Industries+LLC/view-part/?ref=eda")
    (property "Description" "\nAddressable Lighting Neopixel 10 LED Discrete Serial (Shift Register) Red, Green, Blue (RGB) 5.00mm L x 5.00mm W\n")
    (property "MANUFACTURER" "Adafruit Industries")
    (property "MAXIMUM_PACKAGE_HEIGHT" "1.6 mm")
    (property "MF" "Adafruit")
    (property "MP" "1655")
    (property "PARTREV" "01")
    (property "Package" "Adafruit")
    (property "Price" "None")
    (property "STANDARD" "Manufacturer recommendations")
    (property "Sheetfile" "demokeyboard.kicad_sch")
    (property "Sheetname" "")
    (property "SnapEDA_Link" "https://www.snapeda.com/parts/1655/Adafruit+Industries+LLC/view-part/?ref=snap")
    (attr smd)
    (fp_text reference "D51" (at -0.325 3.635) (layer "B.SilkS"))
    (fp_text value "1655" (at 1.58 -3.635) (layer "B.Fab"))
    (pad "1" smd rect (at -2.45 1.6 90) (size 1 1.5) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 87 "VSS") (pinfunction "VSS") (pintype "power_in") (solder_mask_margin 0.102))
    (pad "2" smd rect (at -2.45 -1.6 90) (size 1 1.5) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 85 "Net-(D50-DOUT)") (pinfunction "DIN") (pintype "input") (solder_mask_margin 0.102))
    (pad "3" smd rect (at 2.45 -1.6 90) (size 1 1.5) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 82 "VDD") (pinfunction "VDD") (pintype "power_in") (solder_mask_margin 0.102))
    (pad "4" smd rect (at 2.45 1.6 90) (size 1 1.5) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 86 "Net-(D51-DOUT)") (pinfunction "DOUT") (pintype "output") (solder_mask_margin 0.102))
  )
  (footprint "Diode_SMD:D_SOD-123" (layer "B.Cu")
    (at 121.19125 88.6035 90)
    (descr "SOD-123")
    (tags "SOD-123")
    (property "LCSC" "C81598")
    (property "Sheetfile" "demokeyboard.kicad_sch")
    (property "Sheetname" "")
    (property "Sim.Device" "D")
    (property "Sim.Pins" "1=K 2=A")
    (property "ki_description" "Diode, small symbol")
    (property "ki_keywords" "diode")
    (attr smd)
    (fp_text reference "D29" (at 0 2 90) (layer "B.SilkS"))
    (fp_text value "D_Small" (at 0 -2.1 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1.65 0 90) (size 0.9 1.2) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 61 "ROW2") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 1.65 0 90) (size 0.9 1.2) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 29 "Net-(D29-A)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SOD-123.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_SOD-123" (layer "B.Cu")
    (at 164.05375 50.5035 90)
    (descr "SOD-123")
    (tags "SOD-123")
    (property "LCSC" "C81598")
    (property "Sheetfile" "demokeyboard.kicad_sch")
    (property "Sheetname" "")
    (property "Sim.Device" "D")
    (property "Sim.Pins" "1=K 2=A")
    (property "ki_description" "Diode, small symbol")
    (property "ki_keywords" "diode")
    (attr smd)
    (fp_text reference "D8" (at 0 2 90) (layer "B.SilkS"))
    (fp_text value "D_Small" (at 0 -2.1 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1.65 0 90) (size 0.9 1.2) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 59 "ROW0") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 1.65 0 90) (size 0.9 1.2) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 8 "Net-(D8-A)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SOD-123.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_SOD-123" (layer "B.Cu")
    (at 178.34125 88.6035 90)
    (descr "SOD-123")
    (tags "SOD-123")
    (property "LCSC" "C81598")
    (property "Sheetfile" "demokeyboard.kicad_sch")
    (property "Sheetname" "")
    (property "Sim.Device" "D")
    (property "Sim.Pins" "1=K 2=A")
    (property "ki_description" "Diode, small symbol")
    (property "ki_keywords" "diode")
    (attr smd)
    (fp_text reference "D32" (at 0 2 90) (layer "B.SilkS"))
    (fp_text value "D_Small" (at 0 -2.1 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1.65 0 90) (size 0.9 1.2) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 61 "ROW2") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 1.65 0 90) (size 0.9 1.2) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 32 "Net-(D32-A)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SOD-123.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_SOD-123" (layer "B.Cu")
    (at 78.32875 69.5535 90)
    (descr "SOD-123")
    (tags "SOD-123")
    (property "LCSC" "C81598")
    (property "Sheetfile" "demokeyboard.kicad_sch")
    (property "Sheetname" "")
    (property "Sim.Device" "D")
    (property "Sim.Pins" "1=K 2=A")
    (property "ki_description" "Diode, small symbol")
    (property "ki_keywords" "diode")
    (attr smd)
    (fp_text reference "D15" (at 0 2 90) (layer "B.SilkS"))
    (fp_text value "D_Small" (at 0 -2.1 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1.65 0 90) (size 0.9 1.2) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 60 "ROW1") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 1.65 0 90) (size 0.9 1.2) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 15 "Net-(D15-A)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SOD-123.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_SOD-123" (layer "B.Cu")
    (at 178.34125 107.6535 90)
    (descr "SOD-123")
    (tags "SOD-123")
    (property "LCSC" "C81598")
    (property "Sheetfile" "demokeyboard.kicad_sch")
    (property "Sheetname" "")
    (property "Sim.Device" "D")
    (property "Sim.Pins" "1=K 2=A")
    (property "ki_description" "Diode, small symbol")
    (property "ki_keywords" "diode")
    (attr smd)
    (fp_text reference "D42" (at 0 2 90) (layer "B.SilkS"))
    (fp_text value "D_Small" (at 0 -2.1 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1.65 0 90) (size 0.9 1.2) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 62 "ROW3") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 1.65 0 90) (size 0.9 1.2) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 42 "Net-(D42-A)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SOD-123.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "1655:LED_1655" (layer "B.Cu")
    (at 44.2225 65.14725)
    (property "Availability" "In Stock")
    (property "Check_prices" "https://www.snapeda.com/parts/1655/Adafruit+Industries+LLC/view-part/?ref=eda")
    (property "Description" "\nAddressable Lighting Neopixel 10 LED Discrete Serial (Shift Register) Red, Green, Blue (RGB) 5.00mm L x 5.00mm W\n")
    (property "MANUFACTURER" "Adafruit Industries")
    (property "MAXIMUM_PACKAGE_HEIGHT" "1.6 mm")
    (property "MF" "Adafruit")
    (property "MP" "1655")
    (property "PARTREV" "01")
    (property "Package" "Adafruit")
    (property "Price" "None")
    (property "STANDARD" "Manufacturer recommendations")
    (property "Sheetfile" "demokeyboard.kicad_sch")
    (property "Sheetname" "")
    (property "SnapEDA_Link" "https://www.snapeda.com/parts/1655/Adafruit+Industries+LLC/view-part/?ref=snap")
    (attr smd)
    (fp_text reference "D47" (at -0.325 3.635) (layer "B.SilkS"))
    (fp_text value "1655" (at 1.58 -3.635) (layer "B.Fab"))
    (pad "1" smd rect (at -2.45 1.6 270) (size 1 1.5) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 87 "VSS") (pinfunction "VSS") (pintype "power_in") (solder_mask_margin 0.102))
    (pad "2" smd rect (at -2.45 -1.6 270) (size 1 1.5) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 92 "Net-(D47-DIN)") (pinfunction "DIN") (pintype "input") (solder_mask_margin 0.102))
    (pad "3" smd rect (at 2.45 -1.6 270) (size 1 1.5) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 82 "VDD") (pinfunction "VDD") (pintype "power_in") (solder_mask_margin 0.102))
    (pad "4" smd rect (at 2.45 1.6 270) (size 1 1.5) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 81 "Net-(D47-DOUT)") (pinfunction "DOUT") (pintype "output") (solder_mask_margin 0.102))
  )
  (footprint "Diode_SMD:D_SOD-123" (layer "B.Cu")
    (at 235.49125 107.6535 90)
    (descr "SOD-123")
    (tags "SOD-123")
    (property "LCSC" "C81598")
    (property "Sheetfile" "demokeyboard.kicad_sch")
    (property "Sheetname" "")
    (property "Sim.Device" "D")
    (property "Sim.Pins" "1=K 2=A")
    (property "ki_description" "Diode, small symbol")
    (property "ki_keywords" "diode")
    (attr smd)
    (fp_text reference "D45" (at 0 2 90) (layer "B.SilkS"))
    (fp_text value "D_Small" (at 0 -2.1 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1.65 0 90) (size 0.9 1.2) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 62 "ROW3") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 1.65 0 90) (size 0.9 1.2) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 45 "Net-(D45-A)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SOD-123.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_SOD-123" (layer "B.Cu")
    (at 106.90375 50.5035 90)
    (descr "SOD-123")
    (tags "SOD-123")
    (property "LCSC" "C81598")
    (property "Sheetfile" "demokeyboard.kicad_sch")
    (property "Sheetname" "")
    (property "Sim.Device" "D")
    (property "Sim.Pins" "1=K 2=A")
    (property "ki_description" "Diode, small symbol")
    (property "ki_keywords" "diode")
    (attr smd)
    (fp_text reference "D5" (at 0 2 90) (layer "B.SilkS"))
    (fp_text value "D_Small" (at 0 -2.1 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1.65 0 90) (size 0.9 1.2) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 59 "ROW0") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 1.65 0 90) (size 0.9 1.2) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 5 "Net-(D5-A)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SOD-123.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_SOD-123" (layer "B.Cu")
    (at 230.72875 69.5535 90)
    (descr "SOD-123")
    (tags "SOD-123")
    (property "LCSC" "C81598")
    (property "Sheetfile" "demokeyboard.kicad_sch")
    (property "Sheetname" "")
    (property "Sim.Device" "D")
    (property "Sim.Pins" "1=K 2=A")
    (property "ki_description" "Diode, small symbol")
    (property "ki_keywords" "diode")
    (attr smd)
    (fp_text reference "D23" (at 0 2 90) (layer "B.SilkS"))
    (fp_text value "D_Small" (at 0 -2.1 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1.65 0 90) (size 0.9 1.2) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 60 "ROW1") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 1.65 0 90) (size 0.9 1.2) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 23 "Net-(D23-A)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SOD-123.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_SOD-123" (layer "B.Cu")
    (at 211.67875 69.5535 90)
    (descr "SOD-123")
    (tags "SOD-123")
    (property "LCSC" "C81598")
    (property "Sheetfile" "demokeyboard.kicad_sch")
    (property "Sheetname" "")
    (property "Sim.Device" "D")
    (property "Sim.Pins" "1=K 2=A")
    (property "ki_description" "Diode, small symbol")
    (property "ki_keywords" "diode")
    (attr smd)
    (fp_text reference "D22" (at 0 2 90) (layer "B.SilkS"))
    (fp_text value "D_Small" (at 0 -2.1 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1.65 0 90) (size 0.9 1.2) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 60 "ROW1") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 1.65 0 90) (size 0.9 1.2) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 22 "Net-(D22-A)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SOD-123.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "1655:LED_1655" (layer "B.Cu")
    (at 149.794 55.84675)
    (property "Availability" "In Stock")
    (property "Check_prices" "https://www.snapeda.com/parts/1655/Adafruit+Industries+LLC/view-part/?ref=eda")
    (property "Description" "\nAddressable Lighting Neopixel 10 LED Discrete Serial (Shift Register) Red, Green, Blue (RGB) 5.00mm L x 5.00mm W\n")
    (property "MANUFACTURER" "Adafruit Industries")
    (property "MAXIMUM_PACKAGE_HEIGHT" "1.6 mm")
    (property "MF" "Adafruit")
    (property "MP" "1655")
    (property "PARTREV" "01")
    (property "Package" "Adafruit")
    (property "Price" "None")
    (property "STANDARD" "Manufacturer recommendations")
    (property "Sheetfile" "demokeyboard.kicad_sch")
    (property "Sheetname" "")
    (property "SnapEDA_Link" "https://www.snapeda.com/parts/1655/Adafruit+Industries+LLC/view-part/?ref=snap")
    (attr smd)
    (fp_text reference "D48" (at -0.325 3.635) (layer "B.SilkS"))
    (fp_text value "1655" (at 1.58 -3.635) (layer "B.Fab"))
    (pad "1" smd rect (at -2.45 1.6 270) (size 1 1.5) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 87 "VSS") (pinfunction "VSS") (pintype "power_in") (solder_mask_margin 0.102))
    (pad "2" smd rect (at -2.45 -1.6 270) (size 1 1.5) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 81 "Net-(D47-DOUT)") (pinfunction "DIN") (pintype "input") (solder_mask_margin 0.102))
    (pad "3" smd rect (at 2.45 -1.6 270) (size 1 1.5) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 82 "VDD") (pinfunction "VDD") (pintype "power_in") (solder_mask_margin 0.102))
    (pad "4" smd rect (at 2.45 1.6 270) (size 1 1.5) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 83 "Net-(D48-DOUT)") (pinfunction "DOUT") (pintype "output") (solder_mask_margin 0.102))
  )
  (footprint "Diode_SMD:D_SOD-123" (layer "B.Cu")
    (at 83.09125 88.6035 90)
    (descr "SOD-123")
    (tags "SOD-123")
    (property "LCSC" "C81598")
    (property "Sheetfile" "demokeyboard.kicad_sch")
    (property "Sheetname" "")
    (property "Sim.Device" "D")
    (property "Sim.Pins" "1=K 2=A")
    (property "ki_description" "Diode, small symbol")
    (property "ki_keywords" "diode")
    (attr smd)
    (fp_text reference "D27" (at 0 2 90) (layer "B.SilkS"))
    (fp_text value "D_Small" (at 0 -2.1 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1.65 0 90) (size 0.9 1.2) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 61 "ROW2") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 1.65 0 90) (size 0.9 1.2) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 27 "Net-(D27-A)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SOD-123.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "1655:LED_1655" (layer "B.Cu")
    (at 48.6725 95.74725 180)
    (property "Availability" "In Stock")
    (property "Check_prices" "https://www.snapeda.com/parts/1655/Adafruit+Industries+LLC/view-part/?ref=eda")
    (property "Description" "\nAddressable Lighting Neopixel 10 LED Discrete Serial (Shift Register) Red, Green, Blue (RGB) 5.00mm L x 5.00mm W\n")
    (property "MANUFACTURER" "Adafruit Industries")
    (property "MAXIMUM_PACKAGE_HEIGHT" "1.6 mm")
    (property "MF" "Adafruit")
    (property "MP" "1655")
    (property "PARTREV" "01")
    (property "Package" "Adafruit")
    (property "Price" "None")
    (property "STANDARD" "Manufacturer recommendations")
    (property "Sheetfile" "demokeyboard.kicad_sch")
    (property "Sheetname" "")
    (property "SnapEDA_Link" "https://www.snapeda.com/parts/1655/Adafruit+Industries+LLC/view-part/?ref=snap")
    (attr smd)
    (fp_text reference "D52" (at -0.325 3.635) (layer "B.SilkS"))
    (fp_text value "1655" (at 1.58 -3.635) (layer "B.Fab"))
    (pad "1" smd rect (at -2.45 1.6 90) (size 1 1.5) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 87 "VSS") (pinfunction "VSS") (pintype "power_in") (solder_mask_margin 0.102))
    (pad "2" smd rect (at -2.45 -1.6 90) (size 1 1.5) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 86 "Net-(D51-DOUT)") (pinfunction "DIN") (pintype "input") (solder_mask_margin 0.102))
    (pad "3" smd rect (at 2.45 -1.6 90) (size 1 1.5) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 82 "VDD") (pinfunction "VDD") (pintype "power_in") (solder_mask_margin 0.102))
    (pad "4" smd rect (at 2.45 1.6 90) (size 1 1.5) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 80 "unconnected-(D52-DOUT-Pad4)") (pinfunction "DOUT") (pintype "output") (solder_mask_margin 0.102))
  )
  (footprint "Diode_SMD:D_SOD-123" (layer "B.Cu")
    (at 97.37875 69.5535 90)
    (descr "SOD-123")
    (tags "SOD-123")
    (property "LCSC" "C81598")
    (property "Sheetfile" "demokeyboard.kicad_sch")
    (property "Sheetname" "")
    (property "Sim.Device" "D")
    (property "Sim.Pins" "1=K 2=A")
    (property "ki_description" "Diode, small symbol")
    (property "ki_keywords" "diode")
    (attr smd)
    (fp_text reference "D16" (at 0 2 90) (layer "B.SilkS"))
    (fp_text value "D_Small" (at 0 -2.1 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1.65 0 90) (size 0.9 1.2) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 60 "ROW1") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 1.65 0 90) (size 0.9 1.2) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 16 "Net-(D16-A)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SOD-123.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_SOD-123" (layer "B.Cu")
    (at 247.3975 50.5035 90)
    (descr "SOD-123")
    (tags "SOD-123")
    (property "LCSC" "C81598")
    (property "Sheetfile" "demokeyboard.kicad_sch")
    (property "Sheetname" "")
    (property "Sim.Device" "D")
    (property "Sim.Pins" "1=K 2=A")
    (property "ki_description" "Diode, small symbol")
    (property "ki_keywords" "diode")
    (attr smd)
    (fp_text reference "D12" (at 0 2 90) (layer "B.SilkS"))
    (fp_text value "D_Small" (at 0 -2.1 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1.65 0 90) (size 0.9 1.2) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 59 "ROW0") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 1.65 0 90) (size 0.9 1.2) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 12 "Net-(D12-A)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SOD-123.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_SOD-123" (layer "B.Cu")
    (at 235.49125 88.6035 90)
    (descr "SOD-123")
    (tags "SOD-123")
    (property "LCSC" "C81598")
    (property "Sheetfile" "demokeyboard.kicad_sch")
    (property "Sheetname" "")
    (property "Sim.Device" "D")
    (property "Sim.Pins" "1=K 2=A")
    (property "ki_description" "Diode, small symbol")
    (property "ki_keywords" "diode")
    (attr smd)
    (fp_text reference "D35" (at 0 2 90) (layer "B.SilkS"))
    (fp_text value "D_Small" (at 0 -2.1 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1.65 0 90) (size 0.9 1.2) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 61 "ROW2") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 1.65 0 90) (size 0.9 1.2) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 35 "Net-(D35-A)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SOD-123.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_SOD-123" (layer "B.Cu")
    (at 159.29125 88.6035 90)
    (descr "SOD-123")
    (tags "SOD-123")
    (property "LCSC" "C81598")
    (property "Sheetfile" "demokeyboard.kicad_sch")
    (property "Sheetname" "")
    (property "Sim.Device" "D")
    (property "Sim.Pins" "1=K 2=A")
    (property "ki_description" "Diode, small symbol")
    (property "ki_keywords" "diode")
    (attr smd)
    (fp_text reference "D31" (at 0 2 90) (layer "B.SilkS"))
    (fp_text value "D_Small" (at 0 -2.1 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1.65 0 90) (size 0.9 1.2) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 61 "ROW2") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 1.65 0 90) (size 0.9 1.2) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 31 "Net-(D31-A)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SOD-123.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_SOD-123" (layer "B.Cu")
    (at 216.44125 107.6535 90)
    (descr "SOD-123")
    (tags "SOD-123")
    (property "LCSC" "C81598")
    (property "Sheetfile" "demokeyboard.kicad_sch")
    (property "Sheetname" "")
    (property "Sim.Device" "D")
    (property "Sim.Pins" "1=K 2=A")
    (property "ki_description" "Diode, small symbol")
    (property "ki_keywords" "diode")
    (attr smd)
    (fp_text reference "D44" (at 0 2 90) (layer "B.SilkS"))
    (fp_text value "D_Small" (at 0 -2.1 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1.65 0 90) (size 0.9 1.2) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 62 "ROW3") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 1.65 0 90) (size 0.9 1.2) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 44 "Net-(D44-A)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SOD-123.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_arc (start 18.7975 39.4535) (mid 19.029984 38.892234) (end 19.59125 38.65975)
    (layer "Edge.Cuts"))
  (gr_line (start 18.7975 39.4535) (end 18.7975 115.6535)
    (layer "Edge.Cuts"))
  (gr_arc (start 19.59125 116.44725) (mid 19.029999 116.214751) (end 18.7975 115.6535)
    (layer "Edge.Cuts"))
  (gr_line (start 260.0975 115.6535) (end 260.106202 39.452955)
    (layer "Edge.Cuts"))
  (gr_arc (start 259.312452 38.659205) (mid 259.873747 38.891672) (end 260.106202 39.452955)
    (layer "Edge.Cuts"))
  (gr_line (start 259.312452 38.659205) (end 73.169375 38.65975)
    (layer "Edge.Cuts"))
  (gr_line (start 19.59125 116.44725) (end 259.30375 116.44725)
    (layer "Edge.Cuts"))
  (gr_line (start 73.169375 38.65975) (end 19.59125 38.65975)
    (layer "Edge.Cuts"))
  (gr_arc (start 260.0975 115.6535) (mid 259.865001 116.214751) (end 259.30375 116.44725)
    (layer "Edge.Cuts"))
  (gr_text "JackAndStephsWork.shop" (at 221.563 113.10925) (layer "F.SilkS"))
  (zone (net 87) (net_name "VSS") (layers "F&B.Cu") (hatch edge 0.5)
    (connect_pads (clearance 0.5))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 265.5915 118.70825)
        (xy 264.5735 34.97775)
        (xy 14.1455 35.99575)
        (xy 14.6545 119.72625)
      )
    )
  )
)
