(kicad_pcb (version 20221018) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A3")
  (title_block
    (title "32 Channel expanble thermocouple multiplexer")
    (date "2022-08-24")
    (company "Pi Play")
  )
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0)
    (aux_axis_origin 50 260)
    (pcbplotparams
      (layerselection 0x00010f0_ffffffff)
      (plot_on_all_layers_selection 0x0000000_00000000)
      (disableapertmacros false)
      (usegerberextensions true)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (dashed_line_dash_ratio 12.000000)
      (dashed_line_gap_ratio 3.000000)
      (svgprecision 6)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "PiPlaydrill/")
    )
  )
  (net 0 "")
  (net 1 "Net-(A0-C)")
  (net 2 "+5V")
  (net 3 "/(SPI_CE0_N)GPIO08")
  (net 4 "/GPIO05")
  (net 5 "/GPIO06")
  (net 6 "/GPIO09(SPI_MISO)")
  (net 7 "/GPIO10(SPI_MOSI)")
  (net 8 "/GPIO11(SPI_CLK)")
  (net 9 "/GPIO12")
  (net 10 "/GPIO13")
  (net 11 "/GPIO19")
  (net 12 "/GPIO20")
  (net 13 "/GPIO21")
  (net 14 "GND")
  (net 15 "/T-")
  (net 16 "/T+")
  (net 17 "+3V3")
  (net 18 "Net-(A1-C)")
  (net 19 "Net-(A2-C)")
  (net 20 "Net-(D1-K)")
  (net 21 "Net-(J3-Pin_1)")
  (net 22 "Net-(J3-Pin_2)")
  (net 23 "Net-(J3-Pin_3)")
  (net 24 "Net-(J3-Pin_4)")
  (net 25 "Net-(J3-Pin_5)")
  (net 26 "Net-(J3-Pin_6)")
  (net 27 "Net-(J3-Pin_7)")
  (net 28 "Net-(J3-Pin_8)")
  (net 29 "Net-(J4-Pin_1)")
  (net 30 "Net-(J4-Pin_2)")
  (net 31 "Net-(J4-Pin_3)")
  (net 32 "Net-(J4-Pin_4)")
  (net 33 "Net-(J4-Pin_5)")
  (net 34 "Net-(J4-Pin_6)")
  (net 35 "Net-(J4-Pin_7)")
  (net 36 "Net-(J4-Pin_8)")
  (net 37 "Net-(J5-Pin_1)")
  (net 38 "Net-(J5-Pin_2)")
  (net 39 "Net-(J5-Pin_3)")
  (net 40 "Net-(J5-Pin_4)")
  (net 41 "Net-(J5-Pin_5)")
  (net 42 "Net-(J5-Pin_6)")
  (net 43 "Net-(J5-Pin_7)")
  (net 44 "Net-(J5-Pin_8)")
  (net 45 "Net-(J6-Pin_1)")
  (net 46 "Net-(J6-Pin_2)")
  (net 47 "Net-(J6-Pin_3)")
  (net 48 "Net-(J6-Pin_4)")
  (net 49 "/GPIO17(GPIO_GEN0)")
  (net 50 "/GPIO27(GPIO_GEN2)")
  (net 51 "/GPIO22(GPIO_GEN3)")
  (net 52 "/(TXD0)GPIO14")
  (net 53 "/(RXD0)GPIO15")
  (net 54 "/(GPIO_GEN1)GPIO18")
  (net 55 "/(GPIO_GEN4)GPIO23")
  (net 56 "/(GPIO_GEN5)GPIO24")
  (net 57 "/ID_SD(I2CID EEPROM)")
  (net 58 "/(GPIO_GEN6)GPIO25")
  (net 59 "/(SPI_CE1_N)GPIO07")
  (net 60 "/(I2CID EEPROM)ID_SC")
  (net 61 "/GPIO16")
  (net 62 "/GPIO26")
  (net 63 "/GPIO02(SDA1,I2C)")
  (net 64 "/GPIO03(SCL1,I2C)")
  (net 65 "/GPIO04(GPIO_GCLK)")
  (net 66 "Net-(J6-Pin_5)")
  (net 67 "Net-(J6-Pin_6)")
  (net 68 "Net-(J6-Pin_7)")
  (net 69 "Net-(J6-Pin_8)")
  (net 70 "Net-(J7-Pin_1)")
  (net 71 "Net-(J7-Pin_2)")
  (net 72 "Net-(J7-Pin_3)")
  (net 73 "Net-(J7-Pin_4)")
  (net 74 "Net-(J7-Pin_5)")
  (net 75 "Net-(J7-Pin_6)")
  (net 76 "Net-(J7-Pin_7)")
  (net 77 "Net-(J7-Pin_8)")
  (net 78 "Net-(J8-Pin_1)")
  (net 79 "Net-(J8-Pin_2)")
  (net 80 "Net-(J8-Pin_3)")
  (net 81 "Net-(J8-Pin_4)")
  (net 82 "Net-(J8-Pin_5)")
  (net 83 "Net-(J8-Pin_6)")
  (net 84 "Net-(J8-Pin_7)")
  (net 85 "Net-(J8-Pin_8)")
  (net 86 "Net-(J9-Pin_1)")
  (net 87 "Net-(J9-Pin_2)")
  (net 88 "Net-(J9-Pin_3)")
  (net 89 "Net-(J9-Pin_4)")
  (net 90 "Net-(J9-Pin_5)")
  (net 91 "Net-(J9-Pin_6)")
  (net 92 "Net-(J9-Pin_7)")
  (net 93 "Net-(J9-Pin_8)")
  (net 94 "Net-(J10-Pin_1)")
  (net 95 "Net-(J10-Pin_2)")
  (net 96 "Net-(J10-Pin_3)")
  (net 97 "Net-(J10-Pin_4)")
  (net 98 "Net-(J10-Pin_5)")
  (net 99 "Net-(J10-Pin_6)")
  (net 100 "Net-(J10-Pin_7)")
  (net 101 "Net-(J10-Pin_8)")
  (net 102 "Net-(JP1-A)")
  (net 103 "/A2")
  (net 104 "/A1")
  (net 105 "/A0")
  (net 106 "Net-(U7-P7)")
  (net 107 "unconnected-(U2-DNC-Pad6)")
  (net 108 "/CS0")
  (net 109 "/CS1")
  (net 110 "/CS2")
  (net 111 "/CS3")
  (net 112 "unconnected-(U7-~{INT}-Pad1)")
  (net 113 "unconnected-(U7-NC-Pad3)")
  (net 114 "unconnected-(U7-NC-Pad8)")
  (net 115 "unconnected-(U7-NC-Pad13)")
  (net 116 "unconnected-(U7-NC-Pad18)")
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical" (layer "F.Cu")
    (at 81.690586 225.737316)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (property "Sheetfile" "TCMux.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J1" (at 0 -2.33) (layer "F.SilkS"))
    (fp_text value "TC Expansion" (at 0 4.87) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 1.27 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 15 "/T-") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 16 "/T+") (pinfunction "Pin_2") (pintype "passive"))
    (model "${KIPRJMOD}/ESQ-102-14-G-S.stp"
      (offset (xyz 0 -1.3 2.5))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 -90))
    )
  )
  (footprint "Jumper:SolderJumper-3_P1.3mm_Bridged12_RoundedPad1.0x1.5mm" (layer "F.Cu")
    (at 131.38828 221.1782)
    (descr "SMD Solder 3-pad Jumper, 1x1.5mm rounded Pads, 0.3mm gap, pads 1-2 bridged with 1 copper strip")
    (tags "net tie solder jumper bridged")
    (property "Sheetfile" "TCMux.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "3-pole Solder Jumper, pins 1+2 closed/bridged")
    (property "ki_keywords" "Solder Jumper SPDT")
    (attr exclude_from_pos_files)
    (net_tie_pad_groups "1, 2, 3")
    (fp_text reference "A2" (at -3.65168 0.259) (layer "F.SilkS"))
    (fp_text value "A2" (at 0 1.9) (layer "F.Fab"))
    (pad "1" smd custom (at -1.3 0) (size 1 0.5) (layers "F.Cu" "F.Mask")
      (net 14 "GND") (pinfunction "A") (pintype "passive") (zone_connect 2) (thermal_bridge_angle 45)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0) (fill yes))
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0) (fill yes))
        (gr_poly
          (pts
            (xy 0.55 0.75)
            (xy 0 0.75)
            (xy 0 -0.75)
            (xy 0.55 -0.75)
          )
          (width 0) (fill yes))
      ))
    (pad "2" smd rect (at 0 0) (size 1 1.5) (layers "F.Cu" "F.Mask")
      (net 19 "Net-(A2-C)") (pinfunction "C") (pintype "passive"))
    (pad "3" smd custom (at 1.3 0) (size 1 0.5) (layers "F.Cu" "F.Mask")
      (net 17 "+3V3") (pinfunction "B") (pintype "passive") (zone_connect 2) (thermal_bridge_angle 45)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0) (fill yes))
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0) (fill yes))
        (gr_poly
          (pts
            (xy 0 0.75)
            (xy -0.55 0.75)
            (xy -0.55 -0.75)
            (xy 0 -0.75)
          )
          (width 0) (fill yes))
      ))
  )
  (footprint "Package_SO:SSOP-20_4.4x6.5mm_P0.65mm" (layer "F.Cu")
    (at 130.606586 226.2582 180)
    (descr "SSOP20: plastic shrink small outline package; 20 leads; body width 4.4 mm; (see NXP SSOP-TSSOP-VSO-REFLOW.pdf and sot266-1_po.pdf)")
    (tags "SSOP 0.65")
    (property "Sheetfile" "TCMux.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "8 Bit Port/Expander to I2C Bus, SSOP-20")
    (property "ki_keywords" "I2C Expander")
    (attr smd)
    (fp_text reference "U7" (at 0 -4.3) (layer "F.SilkS"))
    (fp_text value "PCF8574ATS" (at 0 4.3) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect (at -2.9 -2.925 180) (size 1 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 112 "unconnected-(U7-~{INT}-Pad1)") (pinfunction "~{INT}") (pintype "open_collector"))
    (pad "2" smd rect (at -2.9 -2.275 180) (size 1 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 64 "/GPIO03(SCL1,I2C)") (pinfunction "SCL") (pintype "input"))
    (pad "3" smd rect (at -2.9 -1.625 180) (size 1 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 113 "unconnected-(U7-NC-Pad3)") (pinfunction "NC") (pintype "no_connect"))
    (pad "4" smd rect (at -2.9 -0.975 180) (size 1 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 63 "/GPIO02(SDA1,I2C)") (pinfunction "SDA") (pintype "bidirectional"))
    (pad "5" smd rect (at -2.9 -0.325 180) (size 1 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 17 "+3V3") (pinfunction "VDD") (pintype "power_in"))
    (pad "6" smd rect (at -2.9 0.325 180) (size 1 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "Net-(A0-C)") (pinfunction "A0") (pintype "input"))
    (pad "7" smd rect (at -2.9 0.975 180) (size 1 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 18 "Net-(A1-C)") (pinfunction "A1") (pintype "input"))
    (pad "8" smd rect (at -2.9 1.625 180) (size 1 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 114 "unconnected-(U7-NC-Pad8)") (pinfunction "NC") (pintype "no_connect"))
    (pad "9" smd rect (at -2.9 2.275 180) (size 1 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 19 "Net-(A2-C)") (pinfunction "A2") (pintype "input"))
    (pad "10" smd rect (at -2.9 2.925 180) (size 1 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 105 "/A0") (pinfunction "P0") (pintype "bidirectional"))
    (pad "11" smd rect (at 2.9 2.925 180) (size 1 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 104 "/A1") (pinfunction "P1") (pintype "bidirectional"))
    (pad "12" smd rect (at 2.9 2.275 180) (size 1 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 103 "/A2") (pinfunction "P2") (pintype "bidirectional"))
    (pad "13" smd rect (at 2.9 1.625 180) (size 1 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 115 "unconnected-(U7-NC-Pad13)") (pinfunction "NC") (pintype "no_connect"))
    (pad "14" smd rect (at 2.9 0.975 180) (size 1 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 108 "/CS0") (pinfunction "P3") (pintype "bidirectional"))
    (pad "15" smd rect (at 2.9 0.325 180) (size 1 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 14 "GND") (pinfunction "VSS") (pintype "power_in"))
    (pad "16" smd rect (at 2.9 -0.325 180) (size 1 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 109 "/CS1") (pinfunction "P4") (pintype "bidirectional"))
    (pad "17" smd rect (at 2.9 -0.975 180) (size 1 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 110 "/CS2") (pinfunction "P5") (pintype "bidirectional"))
    (pad "18" smd rect (at 2.9 -1.625 180) (size 1 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 116 "unconnected-(U7-NC-Pad18)") (pinfunction "NC") (pintype "no_connect"))
    (pad "19" smd rect (at 2.9 -2.275 180) (size 1 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 111 "/CS3") (pinfunction "P6") (pintype "bidirectional"))
    (pad "20" smd rect (at 2.9 -2.925 180) (size 1 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 106 "Net-(U7-P7)") (pinfunction "P7") (pintype "bidirectional"))
    (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/SSOP-20_4.4x6.5mm_P0.65mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm" (layer "F.Cu")
    (at 140.72628 203.5729 -90)
    (descr "SOIC, 8 Pin (JEDEC MS-012AA, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_8.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (property "Sheetfile" "TCMux.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "128 kb CMOS Serial EEPROM, SOIC-8/TSSOP-8/DFN-8")
    (property "ki_keywords" "I2C EEPROM Serial 128kb")
    (attr smd)
    (fp_text reference "U1" (at 0 3.496) (layer "F.SilkS"))
    (fp_text value "CAT24C128" (at 0 3.4 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.475 -1.905 270) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 14 "GND") (pinfunction "A0") (pintype "input"))
    (pad "2" smd roundrect (at -2.475 -0.635 270) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 14 "GND") (pinfunction "A1") (pintype "input"))
    (pad "3" smd roundrect (at -2.475 0.635 270) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 14 "GND") (pinfunction "A2") (pintype "input"))
    (pad "4" smd roundrect (at -2.475 1.905 270) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 14 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "5" smd roundrect (at 2.475 1.905 270) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 57 "/ID_SD(I2CID EEPROM)") (pinfunction "SDA") (pintype "bidirectional"))
    (pad "6" smd roundrect (at 2.475 0.635 270) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 60 "/(I2CID EEPROM)ID_SC") (pinfunction "SCL") (pintype "input"))
    (pad "7" smd roundrect (at 2.475 -0.635 270) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 102 "Net-(JP1-A)") (pinfunction "WP") (pintype "input"))
    (pad "8" smd roundrect (at 2.475 -1.905 270) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 17 "+3V3") (pinfunction "VCC") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-8_3.9x4.9mm_P1.27mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (at 143.55428 209.4942 180)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "TCMux.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, small symbol")
    (property "ki_keywords" "R resistor")
    (attr smd)
    (fp_text reference "R1" (at -3.328 -0.0143) (layer "F.SilkS"))
    (fp_text value "2k2" (at 0 1.82) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0 180) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 17 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 180) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 102 "Net-(JP1-A)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_2x20_P2.54mm_Vertical" (layer "F.Cu")
    (at 149.9108 202.819)
    (descr "Through hole straight pin header, 2x20, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x20 2.54mm double row")
    (property "Sheetfile" "TCMux.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "P1" (at 5.03768 -2.6557) (layer "F.SilkS"))
    (fp_text value "CONN_20X2" (at 1.27 50.59) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.27 24.13 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 17 "+3V3") (pinfunction "P1") (pintype "passive"))
    (pad "2" thru_hole oval (at 2.54 0) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 2 "+5V") (pinfunction "P2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 63 "/GPIO02(SDA1,I2C)") (pinfunction "P3") (pintype "passive"))
    (pad "4" thru_hole oval (at 2.54 2.54) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 2 "+5V") (pinfunction "P4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 64 "/GPIO03(SCL1,I2C)") (pinfunction "P5") (pintype "passive"))
    (pad "6" thru_hole oval (at 2.54 5.08) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 14 "GND") (pinfunction "P6") (pintype "passive"))
    (pad "7" thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 65 "/GPIO04(GPIO_GCLK)") (pinfunction "P7") (pintype "passive"))
    (pad "8" thru_hole oval (at 2.54 7.62) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 52 "/(TXD0)GPIO14") (pinfunction "P8") (pintype "passive"))
    (pad "9" thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 14 "GND") (pinfunction "P9") (pintype "passive"))
    (pad "10" thru_hole oval (at 2.54 10.16) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 53 "/(RXD0)GPIO15") (pinfunction "P10") (pintype "passive"))
    (pad "11" thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 49 "/GPIO17(GPIO_GEN0)") (pinfunction "P11") (pintype "passive"))
    (pad "12" thru_hole oval (at 2.54 12.7) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 54 "/(GPIO_GEN1)GPIO18") (pinfunction "P12") (pintype "passive"))
    (pad "13" thru_hole oval (at 0 15.24) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 50 "/GPIO27(GPIO_GEN2)") (pinfunction "P13") (pintype "passive"))
    (pad "14" thru_hole oval (at 2.54 15.24) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 14 "GND") (pinfunction "P14") (pintype "passive"))
    (pad "15" thru_hole oval (at 0 17.78) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 51 "/GPIO22(GPIO_GEN3)") (pinfunction "P15") (pintype "passive"))
    (pad "16" thru_hole oval (at 2.54 17.78) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 55 "/(GPIO_GEN4)GPIO23") (pinfunction "P16") (pintype "passive"))
    (pad "17" thru_hole oval (at 0 20.32) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 17 "+3V3") (pinfunction "P17") (pintype "passive"))
    (pad "18" thru_hole oval (at 2.54 20.32) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 56 "/(GPIO_GEN5)GPIO24") (pinfunction "P18") (pintype "passive"))
    (pad "19" thru_hole oval (at 0 22.86) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 7 "/GPIO10(SPI_MOSI)") (pinfunction "P19") (pintype "passive"))
    (pad "20" thru_hole oval (at 2.54 22.86) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 14 "GND") (pinfunction "P20") (pintype "passive"))
    (pad "21" thru_hole oval (at 0 25.4) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 6 "/GPIO09(SPI_MISO)") (pinfunction "P21") (pintype "passive"))
    (pad "22" thru_hole oval (at 2.54 25.4) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 58 "/(GPIO_GEN6)GPIO25") (pinfunction "P22") (pintype "passive"))
    (pad "23" thru_hole oval (at 0 27.94) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 8 "/GPIO11(SPI_CLK)") (pinfunction "P23") (pintype "passive"))
    (pad "24" thru_hole oval (at 2.54 27.94) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 3 "/(SPI_CE0_N)GPIO08") (pinfunction "P24") (pintype "passive"))
    (pad "25" thru_hole oval (at 0 30.48) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 14 "GND") (pintype "passive"))
    (pad "26" thru_hole oval (at 2.54 30.48) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 59 "/(SPI_CE1_N)GPIO07") (pinfunction "P26") (pintype "passive"))
    (pad "27" thru_hole oval (at 0 33.02) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 57 "/ID_SD(I2CID EEPROM)") (pinfunction "P27") (pintype "passive"))
    (pad "28" thru_hole oval (at 2.54 33.02) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 60 "/(I2CID EEPROM)ID_SC") (pinfunction "P28") (pintype "passive"))
    (pad "29" thru_hole oval (at 0 35.56) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 4 "/GPIO05") (pinfunction "P29") (pintype "passive"))
    (pad "30" thru_hole oval (at 2.54 35.56) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 14 "GND") (pinfunction "P30") (pintype "passive"))
    (pad "31" thru_hole oval (at 0 38.1) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 5 "/GPIO06") (pinfunction "P31") (pintype "passive"))
    (pad "32" thru_hole oval (at 2.54 38.1) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 9 "/GPIO12") (pinfunction "P32") (pintype "passive"))
    (pad "33" thru_hole oval (at 0 40.64) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 10 "/GPIO13") (pinfunction "P33") (pintype "passive"))
    (pad "34" thru_hole oval (at 2.54 40.64) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 14 "GND") (pinfunction "P34") (pintype "passive"))
    (pad "35" thru_hole oval (at 0 43.18) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 11 "/GPIO19") (pinfunction "P35") (pintype "passive"))
    (pad "36" thru_hole oval (at 2.54 43.18) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 61 "/GPIO16") (pinfunction "P36") (pintype "passive"))
    (pad "37" thru_hole oval (at 0 45.72) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 62 "/GPIO26") (pinfunction "P37") (pintype "passive"))
    (pad "38" thru_hole oval (at 2.54 45.72) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 12 "/GPIO20") (pinfunction "P38") (pintype "passive"))
    (pad "39" thru_hole oval (at 0 48.26) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 14 "GND") (pinfunction "P39") (pintype "passive"))
    (pad "40" thru_hole oval (at 2.54 48.26) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 13 "/GPIO21") (pinfunction "P40") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x20_P2.54mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_1206_3216Metric_Pad1.42x1.75mm_HandSolder" (layer "F.Cu")
    (at 140.02428 255.6857 90)
    (descr "LED SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "LED handsolder")
    (property "Sheetfile" "TCMux.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Light emitting diode, filled shape")
    (property "ki_keywords" "LED diode")
    (attr smd)
    (fp_text reference "D1" (at -0.1109 -2.31732) (layer "F.SilkS"))
    (fp_text value "Status" (at 0 1.82 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.4875 0 90) (size 1.425 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.175439)
      (net 20 "Net-(D1-K)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 1.4875 0 90) (size 1.425 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.175439)
      (net 17 "+3V3") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:8 pin Screw Terminal P 2.54mm" (layer "F.Cu")
    (at 91.81508 248.0514 180)
    (property "Sheetfile" "TCMux.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic screw terminal, single row, 01x08, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "screw terminal")
    (attr through_hole)
    (fp_text reference "J9" (at -0.36152 4.3892 unlocked) (layer "F.SilkS"))
    (fp_text value "Screw_Terminal_01x08" (at 7.1 4.3 180 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole oval (at 0 0 180) (size 1.4 2.5) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 86 "Net-(J9-Pin_1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 2.526127 0 180) (size 1.4 2.5) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 87 "Net-(J9-Pin_2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 5.071884 0 180) (size 1.4 2.5) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 88 "Net-(J9-Pin_3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 7.617641 0 180) (size 1.4 2.5) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 89 "Net-(J9-Pin_4)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 10.139606 0 180) (size 1.4 2.5) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 90 "Net-(J9-Pin_5)") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 12.7 0 180) (size 1.4 2.5) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 91 "Net-(J9-Pin_6)") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole oval (at 15.23112 0 180) (size 1.4 2.5) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 92 "Net-(J9-Pin_7)") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" thru_hole oval (at 17.776876 0 180) (size 1.4 2.5) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 93 "Net-(J9-Pin_8)") (pinfunction "Pin_8") (pintype "passive"))
    (model "${KIPRJMOD}/1725711.stp"
      (offset (xyz 19.2 3.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (footprint "Package_SO:TSSOP-28_4.4x9.7mm_P0.65mm" (layer "F.Cu")
    (at 113.214053 237.77358 90)
    (descr "TSSOP, 28 Pin (JEDEC MO-153 Var AE https://www.jedec.org/document_search?search_api_views_fulltext=MO-153), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "TSSOP SO")
    (property "Sheetfile" "TCMux.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U5" (at 0.08038 6.115147) (layer "F.SilkS"))
    (fp_text value "ADG1607" (at 0 5.8 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.8625 -4.225 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 17 "+3V3") (pinfunction "Vdd") (pintype "power_in"))
    (pad "2" smd roundrect (at -2.8625 -3.575 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 16 "/T+") (pinfunction "DB") (pintype "bidirectional"))
    (pad "3" smd roundrect (at -2.8625 -2.925 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25))
    (pad "4" smd roundrect (at -2.8625 -2.275 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 85 "Net-(J8-Pin_8)") (pinfunction "S8B") (pintype "bidirectional"))
    (pad "5" smd roundrect (at -2.8625 -1.625 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 83 "Net-(J8-Pin_6)") (pinfunction "S7B") (pintype "bidirectional"))
    (pad "6" smd roundrect (at -2.8625 -0.975 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 81 "Net-(J8-Pin_4)") (pinfunction "S6B") (pintype "bidirectional"))
    (pad "7" smd roundrect (at -2.8625 -0.325 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 79 "Net-(J8-Pin_2)") (pinfunction "S5B") (pintype "bidirectional"))
    (pad "8" smd roundrect (at -2.8625 0.325 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 77 "Net-(J7-Pin_8)") (pinfunction "S4B") (pintype "bidirectional"))
    (pad "9" smd roundrect (at -2.8625 0.975 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 75 "Net-(J7-Pin_6)") (pinfunction "S3B") (pintype "bidirectional"))
    (pad "10" smd roundrect (at -2.8625 1.625 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 73 "Net-(J7-Pin_4)") (pinfunction "S2B") (pintype "bidirectional"))
    (pad "11" smd roundrect (at -2.8625 2.275 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 71 "Net-(J7-Pin_2)") (pinfunction "S1B") (pintype "bidirectional"))
    (pad "12" smd roundrect (at -2.8625 2.925 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 14 "GND") (pinfunction "Gnd") (pintype "power_in"))
    (pad "13" smd roundrect (at -2.8625 3.575 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25))
    (pad "14" smd roundrect (at -2.8625 4.225 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25))
    (pad "15" smd roundrect (at 2.8625 4.225 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 103 "/A2") (pinfunction "A2") (pintype "input"))
    (pad "16" smd roundrect (at 2.8625 3.575 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 104 "/A1") (pinfunction "A1") (pintype "input"))
    (pad "17" smd roundrect (at 2.8625 2.925 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 105 "/A0") (pinfunction "A0") (pintype "input"))
    (pad "18" smd roundrect (at 2.8625 2.275 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 110 "/CS2") (pinfunction "EN") (pintype "input"))
    (pad "19" smd roundrect (at 2.8625 1.625 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 70 "Net-(J7-Pin_1)") (pinfunction "S1A") (pintype "bidirectional"))
    (pad "20" smd roundrect (at 2.8625 0.975 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 72 "Net-(J7-Pin_3)") (pinfunction "S2A") (pintype "bidirectional"))
    (pad "21" smd roundrect (at 2.8625 0.325 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 74 "Net-(J7-Pin_5)") (pinfunction "S3A") (pintype "bidirectional"))
    (pad "22" smd roundrect (at 2.8625 -0.325 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 76 "Net-(J7-Pin_7)") (pinfunction "S4A") (pintype "input"))
    (pad "23" smd roundrect (at 2.8625 -0.975 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 78 "Net-(J8-Pin_1)") (pinfunction "S5A") (pintype "bidirectional"))
    (pad "24" smd roundrect (at 2.8625 -1.625 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 80 "Net-(J8-Pin_3)") (pinfunction "S6A") (pintype "bidirectional"))
    (pad "25" smd roundrect (at 2.8625 -2.275 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 82 "Net-(J8-Pin_5)") (pinfunction "S7A") (pintype "bidirectional"))
    (pad "26" smd roundrect (at 2.8625 -2.925 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 84 "Net-(J8-Pin_7)") (pinfunction "S8A") (pintype "bidirectional"))
    (pad "27" smd roundrect (at 2.8625 -3.575 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 14 "GND") (pinfunction "Vss") (pintype "power_in"))
    (pad "28" smd roundrect (at 2.8625 -4.225 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 15 "/T-") (pinfunction "DA") (pintype "bidirectional"))
    (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/TSSOP-28_4.4x9.7mm_P0.65mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder" (layer "F.Cu")
    (at 106.952059 237.743416 90)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "TCMux.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C8" (at 0 -1.85) (layer "F.SilkS"))
    (fp_text value "100nF" (at 0 1.85 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0 90) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 17 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0 90) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 14 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Symbol:KiCad-Logo2_8mm_SilkScreen" (layer "F.Cu")
    (at 60.5536 227.7364)
    (descr "KiCad Logo")
    (tags "Logo KiCad")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 -6.35) (layer "F.SilkS") hide)
    (fp_text value "KiCad-Logo2_8mm_SilkScreen" (at 0 7.62) (layer "F.Fab") hide)
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (at 127.6426 238.4762 90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "TCMux.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, small symbol")
    (property "ki_keywords" "R resistor")
    (attr smd)
    (fp_text reference "R4" (at 0 -1.82) (layer "F.SilkS"))
    (fp_text value "1k" (at 0 1.82 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0 90) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 20 "Net-(D1-K)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 90) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 106 "Net-(U7-P7)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:8 pin Screw Terminal P 2.54mm" (layer "F.Cu")
    (at 112.59228 248.0262 180)
    (property "Sheetfile" "TCMux.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic screw terminal, single row, 01x08, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "screw terminal")
    (attr through_hole)
    (fp_text reference "J8" (at -0.53932 4.364 unlocked) (layer "F.SilkS"))
    (fp_text value "Screw_Terminal_01x08" (at 7.1 4.3 180 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole oval (at 0 0 180) (size 1.4 2.5) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 78 "Net-(J8-Pin_1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 2.526127 0 180) (size 1.4 2.5) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 79 "Net-(J8-Pin_2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 5.071884 0 180) (size 1.4 2.5) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 80 "Net-(J8-Pin_3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 7.617641 0 180) (size 1.4 2.5) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 81 "Net-(J8-Pin_4)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 10.139606 0 180) (size 1.4 2.5) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 82 "Net-(J8-Pin_5)") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 12.7 0 180) (size 1.4 2.5) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 83 "Net-(J8-Pin_6)") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole oval (at 15.23112 0 180) (size 1.4 2.5) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 84 "Net-(J8-Pin_7)") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" thru_hole oval (at 17.776876 0 180) (size 1.4 2.5) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 85 "Net-(J8-Pin_8)") (pinfunction "Pin_8") (pintype "passive"))
    (model "${KIPRJMOD}/1725711.stp"
      (offset (xyz 19.2 3.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (footprint "footprints:8 pin Screw Terminal P 2.54mm" (layer "F.Cu")
    (at 133.367121 248.0006 180)
    (property "Sheetfile" "TCMux.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic screw terminal, single row, 01x08, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "screw terminal")
    (attr through_hole)
    (fp_text reference "J7" (at -0.719479 4.3384 unlocked) (layer "F.SilkS"))
    (fp_text value "Screw_Terminal_01x08" (at 7.1 4.3 180 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole oval (at 0 0 180) (size 1.4 2.5) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 70 "Net-(J7-Pin_1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 2.526127 0 180) (size 1.4 2.5) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 71 "Net-(J7-Pin_2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 5.071884 0 180) (size 1.4 2.5) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 72 "Net-(J7-Pin_3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 7.617641 0 180) (size 1.4 2.5) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 73 "Net-(J7-Pin_4)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 10.139606 0 180) (size 1.4 2.5) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 74 "Net-(J7-Pin_5)") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 12.7 0 180) (size 1.4 2.5) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 75 "Net-(J7-Pin_6)") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole oval (at 15.23112 0 180) (size 1.4 2.5) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 76 "Net-(J7-Pin_7)") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" thru_hole oval (at 17.776876 0 180) (size 1.4 2.5) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 77 "Net-(J7-Pin_8)") (pinfunction "Pin_8") (pintype "passive"))
    (model "${KIPRJMOD}/1725711.stp"
      (offset (xyz 19.2 3.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (footprint "Symbol:OSHW-Logo2_14.6x12mm_SilkScreen" (layer "F.Cu")
    (at 60.9092 218.3384)
    (descr "Open Source Hardware Symbol")
    (tags "Logo Symbol OSHW")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 0) (layer "F.SilkS") hide)
    (fp_text value "OSHW-Logo2_14.6x12mm_SilkScreen" (at 0.75 0) (layer "F.Fab") hide)
  )
  (footprint "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder" (layer "F.Cu")
    (at 119.727462 216.332016 -90)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "TCMux.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C6" (at 0 -1.85) (layer "F.SilkS"))
    (fp_text value "100nF" (at 0 1.85 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0 270) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 17 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0 270) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 14 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder" (layer "F.Cu")
    (at 136.21428 223.7567 90)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "TCMux.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C2" (at 3.5895 -0.13268) (layer "F.SilkS"))
    (fp_text value "100nF" (at 0 1.85 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0 90) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 17 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0 90) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 14 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:8 pin Screw Terminal P 2.54mm" (layer "F.Cu")
    (at 73.992639 205.8622)
    (property "Sheetfile" "TCMux.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic screw terminal, single row, 01x08, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "screw terminal")
    (attr through_hole)
    (fp_text reference "J4" (at -0.231039 4.145 unlocked) (layer "F.SilkS"))
    (fp_text value "Screw_Terminal_01x08" (at 7.1 4.3 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole oval (at 0 0) (size 1.4 2.5) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 29 "Net-(J4-Pin_1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 2.526127 0) (size 1.4 2.5) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 30 "Net-(J4-Pin_2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 5.071884 0) (size 1.4 2.5) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 31 "Net-(J4-Pin_3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 7.617641 0) (size 1.4 2.5) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 32 "Net-(J4-Pin_4)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 10.139606 0) (size 1.4 2.5) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 33 "Net-(J4-Pin_5)") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 12.7 0) (size 1.4 2.5) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 34 "Net-(J4-Pin_6)") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole oval (at 15.23112 0) (size 1.4 2.5) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 35 "Net-(J4-Pin_7)") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" thru_hole oval (at 17.776876 0) (size 1.4 2.5) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 36 "Net-(J4-Pin_8)") (pinfunction "Pin_8") (pintype "passive"))
    (model "${KIPRJMOD}/1725711.stp"
      (offset (xyz 19.2 3.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (footprint "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder" (layer "F.Cu")
    (at 142.75828 225.805736 -90)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "TCMux.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C9" (at -3.733536 -0.21832) (layer "F.SilkS"))
    (fp_text value "100nF" (at 0 1.85 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0 270) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 17 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0 270) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 14 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Jumper:SolderJumper-3_P1.3mm_Bridged12_RoundedPad1.0x1.5mm" (layer "F.Cu")
    (at 131.4226 216.0982)
    (descr "SMD Solder 3-pad Jumper, 1x1.5mm rounded Pads, 0.3mm gap, pads 1-2 bridged with 1 copper strip")
    (tags "net tie solder jumper bridged")
    (property "Sheetfile" "TCMux.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "3-pole Solder Jumper, pins 1+2 closed/bridged")
    (property "ki_keywords" "Solder Jumper SPDT")
    (attr exclude_from_pos_files)
    (net_tie_pad_groups "1, 2, 3")
    (fp_text reference "A0" (at -3.686 0.259) (layer "F.SilkS"))
    (fp_text value "A0" (at 0 1.9) (layer "F.Fab"))
    (pad "1" smd custom (at -1.3 0) (size 1 0.5) (layers "F.Cu" "F.Mask")
      (net 14 "GND") (pinfunction "A") (pintype "passive") (zone_connect 2) (thermal_bridge_angle 45)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0) (fill yes))
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0) (fill yes))
        (gr_poly
          (pts
            (xy 0.55 0.75)
            (xy 0 0.75)
            (xy 0 -0.75)
            (xy 0.55 -0.75)
          )
          (width 0) (fill yes))
      ))
    (pad "2" smd rect (at 0 0) (size 1 1.5) (layers "F.Cu" "F.Mask")
      (net 1 "Net-(A0-C)") (pinfunction "C") (pintype "passive"))
    (pad "3" smd custom (at 1.3 0) (size 1 0.5) (layers "F.Cu" "F.Mask")
      (net 17 "+3V3") (pinfunction "B") (pintype "passive") (zone_connect 2) (thermal_bridge_angle 45)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0) (fill yes))
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0) (fill yes))
        (gr_poly
          (pts
            (xy 0 0.75)
            (xy -0.55 0.75)
            (xy -0.55 -0.75)
            (xy 0 -0.75)
          )
          (width 0) (fill yes))
      ))
  )
  (footprint "footprints:8 pin Screw Terminal P 2.54mm" (layer "F.Cu")
    (at 94.81028 205.8622)
    (property "Sheetfile" "TCMux.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic screw terminal, single row, 01x08, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "screw terminal")
    (attr through_hole)
    (fp_text reference "J5" (at -0.09368 4.145 unlocked) (layer "F.SilkS"))
    (fp_text value "Screw_Terminal_01x08" (at 7.1 4.3 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole oval (at 0 0) (size 1.4 2.5) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 37 "Net-(J5-Pin_1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 2.526127 0) (size 1.4 2.5) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 38 "Net-(J5-Pin_2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 5.071884 0) (size 1.4 2.5) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 39 "Net-(J5-Pin_3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 7.617641 0) (size 1.4 2.5) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 40 "Net-(J5-Pin_4)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 10.139606 0) (size 1.4 2.5) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 41 "Net-(J5-Pin_5)") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 12.7 0) (size 1.4 2.5) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 42 "Net-(J5-Pin_6)") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole oval (at 15.23112 0) (size 1.4 2.5) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 43 "Net-(J5-Pin_7)") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" thru_hole oval (at 17.776876 0) (size 1.4 2.5) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 44 "Net-(J5-Pin_8)") (pinfunction "Pin_8") (pintype "passive"))
    (model "${KIPRJMOD}/1725711.stp"
      (offset (xyz 19.2 3.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (footprint "Jumper:SolderJumper-3_P1.3mm_Bridged12_RoundedPad1.0x1.5mm" (layer "F.Cu")
    (at 131.41828 218.6382)
    (descr "SMD Solder 3-pad Jumper, 1x1.5mm rounded Pads, 0.3mm gap, pads 1-2 bridged with 1 copper strip")
    (tags "net tie solder jumper bridged")
    (property "Sheetfile" "TCMux.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "3-pole Solder Jumper, pins 1+2 closed/bridged")
    (property "ki_keywords" "Solder Jumper SPDT")
    (attr exclude_from_pos_files)
    (net_tie_pad_groups "1, 2, 3")
    (fp_text reference "A1" (at -3.68168 0.259) (layer "F.SilkS"))
    (fp_text value "A1" (at 0 1.9) (layer "F.Fab"))
    (pad "1" smd custom (at -1.3 0) (size 1 0.5) (layers "F.Cu" "F.Mask")
      (net 14 "GND") (pinfunction "A") (pintype "passive") (zone_connect 2) (thermal_bridge_angle 45)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0) (fill yes))
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0) (fill yes))
        (gr_poly
          (pts
            (xy 0.55 0.75)
            (xy 0 0.75)
            (xy 0 -0.75)
            (xy 0.55 -0.75)
          )
          (width 0) (fill yes))
      ))
    (pad "2" smd rect (at 0 0) (size 1 1.5) (layers "F.Cu" "F.Mask")
      (net 18 "Net-(A1-C)") (pinfunction "C") (pintype "passive"))
    (pad "3" smd custom (at 1.3 0) (size 1 0.5) (layers "F.Cu" "F.Mask")
      (net 17 "+3V3") (pinfunction "B") (pintype "passive") (zone_connect 2) (thermal_bridge_angle 45)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0) (fill yes))
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0) (fill yes))
        (gr_poly
          (pts
            (xy 0 0.75)
            (xy -0.55 0.75)
            (xy -0.55 -0.75)
            (xy 0 -0.75)
          )
          (width 0) (fill yes))
      ))
  )
  (footprint "Package_SO:TSSOP-28_4.4x9.7mm_P0.65mm" (layer "F.Cu")
    (at 71.073986 215.9537 -90)
    (descr "TSSOP, 28 Pin (JEDEC MO-153 Var AE https://www.jedec.org/document_search?search_api_views_fulltext=MO-153), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "TSSOP SO")
    (property "Sheetfile" "TCMux.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U3" (at 0 5.892386) (layer "F.SilkS"))
    (fp_text value "ADG1607" (at 0 5.8 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.8625 -4.225 270) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 17 "+3V3") (pinfunction "Vdd") (pintype "power_in"))
    (pad "2" smd roundrect (at -2.8625 -3.575 270) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 16 "/T+") (pinfunction "DB") (pintype "bidirectional"))
    (pad "3" smd roundrect (at -2.8625 -2.925 270) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25))
    (pad "4" smd roundrect (at -2.8625 -2.275 270) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 36 "Net-(J4-Pin_8)") (pinfunction "S8B") (pintype "bidirectional"))
    (pad "5" smd roundrect (at -2.8625 -1.625 270) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 34 "Net-(J4-Pin_6)") (pinfunction "S7B") (pintype "bidirectional"))
    (pad "6" smd roundrect (at -2.8625 -0.975 270) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 32 "Net-(J4-Pin_4)") (pinfunction "S6B") (pintype "bidirectional"))
    (pad "7" smd roundrect (at -2.8625 -0.325 270) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 30 "Net-(J4-Pin_2)") (pinfunction "S5B") (pintype "bidirectional"))
    (pad "8" smd roundrect (at -2.8625 0.325 270) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 28 "Net-(J3-Pin_8)") (pinfunction "S4B") (pintype "bidirectional"))
    (pad "9" smd roundrect (at -2.8625 0.975 270) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 26 "Net-(J3-Pin_6)") (pinfunction "S3B") (pintype "bidirectional"))
    (pad "10" smd roundrect (at -2.8625 1.625 270) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 24 "Net-(J3-Pin_4)") (pinfunction "S2B") (pintype "bidirectional"))
    (pad "11" smd roundrect (at -2.8625 2.275 270) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "Net-(J3-Pin_2)") (pinfunction "S1B") (pintype "bidirectional"))
    (pad "12" smd roundrect (at -2.8625 2.925 270) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 14 "GND") (pinfunction "Gnd") (pintype "power_in"))
    (pad "13" smd roundrect (at -2.8625 3.575 270) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25))
    (pad "14" smd roundrect (at -2.8625 4.225 270) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25))
    (pad "15" smd roundrect (at 2.8625 4.225 270) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 103 "/A2") (pinfunction "A2") (pintype "input"))
    (pad "16" smd roundrect (at 2.8625 3.575 270) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 104 "/A1") (pinfunction "A1") (pintype "input"))
    (pad "17" smd roundrect (at 2.8625 2.925 270) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 105 "/A0") (pinfunction "A0") (pintype "input"))
    (pad "18" smd roundrect (at 2.8625 2.275 270) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 108 "/CS0") (pinfunction "EN") (pintype "input"))
    (pad "19" smd roundrect (at 2.8625 1.625 270) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 21 "Net-(J3-Pin_1)") (pinfunction "S1A") (pintype "bidirectional"))
    (pad "20" smd roundrect (at 2.8625 0.975 270) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 23 "Net-(J3-Pin_3)") (pinfunction "S2A") (pintype "bidirectional"))
    (pad "21" smd roundrect (at 2.8625 0.325 270) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 25 "Net-(J3-Pin_5)") (pinfunction "S3A") (pintype "bidirectional"))
    (pad "22" smd roundrect (at 2.8625 -0.325 270) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 27 "Net-(J3-Pin_7)") (pinfunction "S4A") (pintype "input"))
    (pad "23" smd roundrect (at 2.8625 -0.975 270) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 29 "Net-(J4-Pin_1)") (pinfunction "S5A") (pintype "bidirectional"))
    (pad "24" smd roundrect (at 2.8625 -1.625 270) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 31 "Net-(J4-Pin_3)") (pinfunction "S6A") (pintype "bidirectional"))
    (pad "25" smd roundrect (at 2.8625 -2.275 270) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 33 "Net-(J4-Pin_5)") (pinfunction "S7A") (pintype "bidirectional"))
    (pad "26" smd roundrect (at 2.8625 -2.925 270) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 35 "Net-(J4-Pin_7)") (pinfunction "S8A") (pintype "bidirectional"))
    (pad "27" smd roundrect (at 2.8625 -3.575 270) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 14 "GND") (pinfunction "Vss") (pintype "power_in"))
    (pad "28" smd roundrect (at 2.8625 -4.225 270) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 15 "/T-") (pinfunction "DA") (pintype "bidirectional"))
    (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/TSSOP-28_4.4x9.7mm_P0.65mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder" (layer "F.Cu")
    (at 96.34298 232.0627 -90)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "TCMux.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C3" (at 0 -1.85) (layer "F.SilkS"))
    (fp_text value "100nF" (at 0 1.85 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0 270) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 17 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0 270) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 14 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder" (layer "F.Cu")
    (at 85.67498 221.711 90)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "TCMux.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C13" (at -0.031 2.56462) (layer "F.SilkS"))
    (fp_text value "100nF" (at 0 1.85 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0 90) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 15 "/T-") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0 90) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 14 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder" (layer "F.Cu")
    (at 85.67498 231.7702 90)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "TCMux.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C11" (at -3.6878 0.07542) (layer "F.SilkS"))
    (fp_text value "100nF" (at 0 1.85 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0 90) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 14 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0 90) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 16 "/T+") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_SO:TSSOP-14_4.4x5mm_P0.65mm" (layer "F.Cu")
    (at 93.60748 226.9442)
    (descr "TSSOP, 14 Pin (JEDEC MO-153 Var AB-1 https://www.jedec.org/document_search?search_api_views_fulltext=MO-153), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "TSSOP SO")
    (property "Sheetfile" "TCMux.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Precision Thermocouple to Digital Converter with Linearization, TSSOP-14")
    (property "ki_keywords" "Thermocouple converter serial")
    (attr smd)
    (fp_text reference "U2" (at 0 -3.45) (layer "F.SilkS"))
    (fp_text value "MAX31856" (at 0 3.45) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.8625 -1.95) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 14 "GND") (pinfunction "AGND") (pintype "power_in"))
    (pad "2" smd roundrect (at -2.8625 -1.3) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 15 "/T-") (pinfunction "BIAS") (pintype "input"))
    (pad "3" smd roundrect (at -2.8625 -0.65) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 15 "/T-") (pinfunction "T-") (pintype "input"))
    (pad "4" smd roundrect (at -2.8625 0) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 16 "/T+") (pinfunction "T+") (pintype "input"))
    (pad "5" smd roundrect (at -2.8625 0.65) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 17 "+3V3") (pinfunction "AVDD") (pintype "power_in"))
    (pad "6" smd roundrect (at -2.8625 1.3) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 107 "unconnected-(U2-DNC-Pad6)") (pinfunction "DNC") (pintype "no_connect"))
    (pad "7" smd roundrect (at -2.8625 1.95) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "/GPIO05") (pinfunction "~{DRDY}") (pintype "output"))
    (pad "8" smd roundrect (at 2.8625 1.95) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 17 "+3V3") (pinfunction "DVDD") (pintype "power_in"))
    (pad "9" smd roundrect (at 2.8625 1.3) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "/(SPI_CE0_N)GPIO08") (pinfunction "~{CS}") (pintype "input"))
    (pad "10" smd roundrect (at 2.8625 0.65) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 8 "/GPIO11(SPI_CLK)") (pinfunction "SCK") (pintype "input"))
    (pad "11" smd roundrect (at 2.8625 0) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 6 "/GPIO09(SPI_MISO)") (pinfunction "SDO") (pintype "output"))
    (pad "12" smd roundrect (at 2.8625 -0.65) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 7 "/GPIO10(SPI_MOSI)") (pinfunction "SDI") (pintype "input"))
    (pad "13" smd roundrect (at 2.8625 -1.3) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 10 "/GPIO13") (pinfunction "~{FAULT}") (pintype "output"))
    (pad "14" smd roundrect (at 2.8625 -1.95) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 14 "GND") (pinfunction "DGND") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/TSSOP-14_4.4x5mm_P0.65mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder" (layer "F.Cu")
    (at 145.35828 203.9304 90)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "TCMux.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C1" (at 0.0242 2.032) (layer "F.SilkS"))
    (fp_text value "100nF" (at 0 1.85 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0 90) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 17 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0 90) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 14 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_2.7mm_M2.5" (layer "F.Cu")
    (at 151.04428 255.9479 -90)
    (descr "Mounting Hole 2.7mm, no annular, M2.5")
    (tags "mounting hole 2.7mm no annular m2.5")
    (property "Sheetfile" "TCMux.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "MK2" (at 0 -3.7 90) (layer "F.SilkS") hide)
    (fp_text value "M2.5" (at 0 3.7 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0 270) (size 2.7 2.7) (drill 2.7) (layers "*.Cu" "*.Mask"))
  )
  (footprint "footprints:8 pin Screw Terminal P 2.54mm" (layer "F.Cu")
    (at 71.03788 248.0514 180)
    (property "Sheetfile" "TCMux.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic screw terminal, single row, 01x08, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "screw terminal")
    (attr through_hole)
    (fp_text reference "J10" (at -0.18372 4.3892 unlocked) (layer "F.SilkS"))
    (fp_text value "Screw_Terminal_01x08" (at 7.1 4.3 180 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole oval (at 0 0 180) (size 1.4 2.5) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 94 "Net-(J10-Pin_1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 2.526127 0 180) (size 1.4 2.5) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 95 "Net-(J10-Pin_2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 5.071884 0 180) (size 1.4 2.5) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 96 "Net-(J10-Pin_3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 7.617641 0 180) (size 1.4 2.5) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 97 "Net-(J10-Pin_4)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 10.139606 0 180) (size 1.4 2.5) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 98 "Net-(J10-Pin_5)") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 12.7 0 180) (size 1.4 2.5) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 99 "Net-(J10-Pin_6)") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole oval (at 15.23112 0 180) (size 1.4 2.5) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 100 "Net-(J10-Pin_7)") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" thru_hole oval (at 17.776876 0 180) (size 1.4 2.5) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 101 "Net-(J10-Pin_8)") (pinfunction "Pin_8") (pintype "passive"))
    (model "${KIPRJMOD}/1725711.stp"
      (offset (xyz 19.2 3.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (at 143.55428 214.5742 180)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "TCMux.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, small symbol")
    (property "ki_keywords" "R resistor")
    (attr smd)
    (fp_text reference "R3" (at -3.328 -0.0143) (layer "F.SilkS"))
    (fp_text value "2k2" (at 0 1.82) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0 180) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 17 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 180) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 57 "/ID_SD(I2CID EEPROM)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_SO:TSSOP-28_4.4x9.7mm_P0.65mm" (layer "F.Cu")
    (at 113.317462 216.293516 -90)
    (descr "TSSOP, 28 Pin (JEDEC MO-153 Var AE https://www.jedec.org/document_search?search_api_views_fulltext=MO-153), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "TSSOP SO")
    (property "Sheetfile" "TCMux.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U4" (at -0.126316 5.935862) (layer "F.SilkS"))
    (fp_text value "ADG1607" (at 0 5.8 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.8625 -4.225 270) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 17 "+3V3") (pinfunction "Vdd") (pintype "power_in"))
    (pad "2" smd roundrect (at -2.8625 -3.575 270) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 16 "/T+") (pinfunction "DB") (pintype "bidirectional"))
    (pad "3" smd roundrect (at -2.8625 -2.925 270) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25))
    (pad "4" smd roundrect (at -2.8625 -2.275 270) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 69 "Net-(J6-Pin_8)") (pinfunction "S8B") (pintype "bidirectional"))
    (pad "5" smd roundrect (at -2.8625 -1.625 270) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 67 "Net-(J6-Pin_6)") (pinfunction "S7B") (pintype "bidirectional"))
    (pad "6" smd roundrect (at -2.8625 -0.975 270) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 48 "Net-(J6-Pin_4)") (pinfunction "S6B") (pintype "bidirectional"))
    (pad "7" smd roundrect (at -2.8625 -0.325 270) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 46 "Net-(J6-Pin_2)") (pinfunction "S5B") (pintype "bidirectional"))
    (pad "8" smd roundrect (at -2.8625 0.325 270) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 44 "Net-(J5-Pin_8)") (pinfunction "S4B") (pintype "bidirectional"))
    (pad "9" smd roundrect (at -2.8625 0.975 270) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 42 "Net-(J5-Pin_6)") (pinfunction "S3B") (pintype "bidirectional"))
    (pad "10" smd roundrect (at -2.8625 1.625 270) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 40 "Net-(J5-Pin_4)") (pinfunction "S2B") (pintype "bidirectional"))
    (pad "11" smd roundrect (at -2.8625 2.275 270) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 38 "Net-(J5-Pin_2)") (pinfunction "S1B") (pintype "bidirectional"))
    (pad "12" smd roundrect (at -2.8625 2.925 270) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 14 "GND") (pinfunction "Gnd") (pintype "power_in"))
    (pad "13" smd roundrect (at -2.8625 3.575 270) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25))
    (pad "14" smd roundrect (at -2.8625 4.225 270) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25))
    (pad "15" smd roundrect (at 2.8625 4.225 270) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 103 "/A2") (pinfunction "A2") (pintype "input"))
    (pad "16" smd roundrect (at 2.8625 3.575 270) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 104 "/A1") (pinfunction "A1") (pintype "input"))
    (pad "17" smd roundrect (at 2.8625 2.925 270) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 105 "/A0") (pinfunction "A0") (pintype "input"))
    (pad "18" smd roundrect (at 2.8625 2.275 270) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 109 "/CS1") (pinfunction "EN") (pintype "input"))
    (pad "19" smd roundrect (at 2.8625 1.625 270) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 37 "Net-(J5-Pin_1)") (pinfunction "S1A") (pintype "bidirectional"))
    (pad "20" smd roundrect (at 2.8625 0.975 270) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 39 "Net-(J5-Pin_3)") (pinfunction "S2A") (pintype "bidirectional"))
    (pad "21" smd roundrect (at 2.8625 0.325 270) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 41 "Net-(J5-Pin_5)") (pinfunction "S3A") (pintype "bidirectional"))
    (pad "22" smd roundrect (at 2.8625 -0.325 270) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 43 "Net-(J5-Pin_7)") (pinfunction "S4A") (pintype "input"))
    (pad "23" smd roundrect (at 2.8625 -0.975 270) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 45 "Net-(J6-Pin_1)") (pinfunction "S5A") (pintype "bidirectional"))
    (pad "24" smd roundrect (at 2.8625 -1.625 270) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 47 "Net-(J6-Pin_3)") (pinfunction "S6A") (pintype "bidirectional"))
    (pad "25" smd roundrect (at 2.8625 -2.275 270) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 66 "Net-(J6-Pin_5)") (pinfunction "S7A") (pintype "bidirectional"))
    (pad "26" smd roundrect (at 2.8625 -2.925 270) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 68 "Net-(J6-Pin_7)") (pinfunction "S8A") (pintype "bidirectional"))
    (pad "27" smd roundrect (at 2.8625 -3.575 270) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 14 "GND") (pinfunction "Vss") (pintype "power_in"))
    (pad "28" smd roundrect (at 2.8625 -4.225 270) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 15 "/T-") (pinfunction "DA") (pintype "bidirectional"))
    (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/TSSOP-28_4.4x9.7mm_P0.65mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (at 143.55428 212.0342 180)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "TCMux.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, small symbol")
    (property "ki_keywords" "R resistor")
    (attr smd)
    (fp_text reference "R2" (at -3.328 -0.0143) (layer "F.SilkS"))
    (fp_text value "2k2" (at 0 1.82) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0 180) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 17 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 180) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 60 "/(I2CID EEPROM)ID_SC") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder" (layer "F.Cu")
    (at 77.464986 215.836316 -90)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "TCMux.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C5" (at 0.063684 -2.138614) (layer "F.SilkS"))
    (fp_text value "100nF" (at 0 1.85 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0 270) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 17 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0 270) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 14 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder" (layer "F.Cu")
    (at 85.678386 226.741 -90)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "TCMux.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C12" (at 0.0302 -2.510414) (layer "F.SilkS"))
    (fp_text value "100nF" (at 0 1.85 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0 270) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 15 "/T-") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0 270) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 16 "/T+") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder" (layer "F.Cu")
    (at 64.418586 237.426316 90)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "TCMux.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C7" (at 0 -1.85) (layer "F.SilkS"))
    (fp_text value "100nF" (at 0 1.85 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0 90) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 17 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0 90) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 14 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Jumper:SolderJumper-2_P1.3mm_Open_Pad1.0x1.5mm" (layer "F.Cu")
    (at 139.40428 209.4942 180)
    (descr "SMD Solder Jumper, 1x1.5mm Pads, 0.3mm gap, open")
    (tags "solder jumper open")
    (property "Sheetfile" "TCMux.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Solder Jumper, 2-pole, open")
    (property "ki_keywords" "solder jumper SPST")
    (attr exclude_from_pos_files)
    (fp_text reference "JP1" (at 0 -1.8) (layer "F.SilkS"))
    (fp_text value "!WP" (at 0 1.9) (layer "F.Fab"))
    (pad "1" smd rect (at -0.65 0 180) (size 1 1.5) (layers "F.Cu" "F.Mask")
      (net 102 "Net-(JP1-A)") (pinfunction "A") (pintype "passive"))
    (pad "2" smd rect (at 0.65 0 180) (size 1 1.5) (layers "F.Cu" "F.Mask")
      (net 14 "GND") (pinfunction "B") (pintype "passive"))
  )
  (footprint "footprints:8 pin Screw Terminal P 2.54mm" (layer "F.Cu")
    (at 115.584153 205.8622)
    (property "Sheetfile" "TCMux.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic screw terminal, single row, 01x08, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "screw terminal")
    (attr through_hole)
    (fp_text reference "J6" (at 0.087447 4.145 unlocked) (layer "F.SilkS"))
    (fp_text value "Screw_Terminal_01x08" (at 7.1 4.3 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole oval (at 0 0) (size 1.4 2.5) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 45 "Net-(J6-Pin_1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 2.526127 0) (size 1.4 2.5) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 46 "Net-(J6-Pin_2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 5.071884 0) (size 1.4 2.5) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 47 "Net-(J6-Pin_3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 7.617641 0) (size 1.4 2.5) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 48 "Net-(J6-Pin_4)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 10.139606 0) (size 1.4 2.5) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 66 "Net-(J6-Pin_5)") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 12.7 0) (size 1.4 2.5) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 67 "Net-(J6-Pin_6)") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole oval (at 15.23112 0) (size 1.4 2.5) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 68 "Net-(J6-Pin_7)") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" thru_hole oval (at 17.776876 0) (size 1.4 2.5) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 69 "Net-(J6-Pin_8)") (pinfunction "Pin_8") (pintype "passive"))
    (model "${KIPRJMOD}/1725711.stp"
      (offset (xyz 19.2 3.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (footprint "Package_SO:TSSOP-28_4.4x9.7mm_P0.65mm" (layer "F.Cu")
    (at 70.78898 237.426316 90)
    (descr "TSSOP, 28 Pin (JEDEC MO-153 Var AE https://www.jedec.org/document_search?search_api_views_fulltext=MO-153), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "TSSOP SO")
    (property "Sheetfile" "TCMux.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U6" (at -0.140884 5.99262) (layer "F.SilkS"))
    (fp_text value "ADG1607" (at 0 5.8 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.8625 -4.225 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 17 "+3V3") (pinfunction "Vdd") (pintype "power_in"))
    (pad "2" smd roundrect (at -2.8625 -3.575 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 16 "/T+") (pinfunction "DB") (pintype "bidirectional"))
    (pad "3" smd roundrect (at -2.8625 -2.925 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25))
    (pad "4" smd roundrect (at -2.8625 -2.275 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 101 "Net-(J10-Pin_8)") (pinfunction "S8B") (pintype "bidirectional"))
    (pad "5" smd roundrect (at -2.8625 -1.625 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 99 "Net-(J10-Pin_6)") (pinfunction "S7B") (pintype "bidirectional"))
    (pad "6" smd roundrect (at -2.8625 -0.975 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 97 "Net-(J10-Pin_4)") (pinfunction "S6B") (pintype "bidirectional"))
    (pad "7" smd roundrect (at -2.8625 -0.325 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 95 "Net-(J10-Pin_2)") (pinfunction "S5B") (pintype "bidirectional"))
    (pad "8" smd roundrect (at -2.8625 0.325 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 93 "Net-(J9-Pin_8)") (pinfunction "S4B") (pintype "bidirectional"))
    (pad "9" smd roundrect (at -2.8625 0.975 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 91 "Net-(J9-Pin_6)") (pinfunction "S3B") (pintype "bidirectional"))
    (pad "10" smd roundrect (at -2.8625 1.625 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 89 "Net-(J9-Pin_4)") (pinfunction "S2B") (pintype "bidirectional"))
    (pad "11" smd roundrect (at -2.8625 2.275 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 87 "Net-(J9-Pin_2)") (pinfunction "S1B") (pintype "bidirectional"))
    (pad "12" smd roundrect (at -2.8625 2.925 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 14 "GND") (pinfunction "Gnd") (pintype "power_in"))
    (pad "13" smd roundrect (at -2.8625 3.575 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25))
    (pad "14" smd roundrect (at -2.8625 4.225 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25))
    (pad "15" smd roundrect (at 2.8625 4.225 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 103 "/A2") (pinfunction "A2") (pintype "input"))
    (pad "16" smd roundrect (at 2.8625 3.575 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 104 "/A1") (pinfunction "A1") (pintype "input"))
    (pad "17" smd roundrect (at 2.8625 2.925 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 105 "/A0") (pinfunction "A0") (pintype "input"))
    (pad "18" smd roundrect (at 2.8625 2.275 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 111 "/CS3") (pinfunction "EN") (pintype "input"))
    (pad "19" smd roundrect (at 2.8625 1.625 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 86 "Net-(J9-Pin_1)") (pinfunction "S1A") (pintype "bidirectional"))
    (pad "20" smd roundrect (at 2.8625 0.975 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 88 "Net-(J9-Pin_3)") (pinfunction "S2A") (pintype "bidirectional"))
    (pad "21" smd roundrect (at 2.8625 0.325 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 90 "Net-(J9-Pin_5)") (pinfunction "S3A") (pintype "bidirectional"))
    (pad "22" smd roundrect (at 2.8625 -0.325 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 92 "Net-(J9-Pin_7)") (pinfunction "S4A") (pintype "input"))
    (pad "23" smd roundrect (at 2.8625 -0.975 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 94 "Net-(J10-Pin_1)") (pinfunction "S5A") (pintype "bidirectional"))
    (pad "24" smd roundrect (at 2.8625 -1.625 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 96 "Net-(J10-Pin_3)") (pinfunction "S6A") (pintype "bidirectional"))
    (pad "25" smd roundrect (at 2.8625 -2.275 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 98 "Net-(J10-Pin_5)") (pinfunction "S7A") (pintype "bidirectional"))
    (pad "26" smd roundrect (at 2.8625 -2.925 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 100 "Net-(J10-Pin_7)") (pinfunction "S8A") (pintype "bidirectional"))
    (pad "27" smd roundrect (at 2.8625 -3.575 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 14 "GND") (pinfunction "Vss") (pintype "power_in"))
    (pad "28" smd roundrect (at 2.8625 -4.225 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 15 "/T-") (pinfunction "DA") (pintype "bidirectional"))
    (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/TSSOP-28_4.4x9.7mm_P0.65mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_2.7mm_M2.5" (layer "F.Cu")
    (at 54.0066 239.7122 -90)
    (descr "Mounting Hole 2.7mm, no annular, M2.5")
    (tags "mounting hole 2.7mm no annular m2.5")
    (property "Sheetfile" "TCMux.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "MK4" (at -3.6954 2.6478 90) (layer "F.SilkS") hide)
    (fp_text value "M2.5" (at 0 3.7 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0 270) (size 2.7 2.7) (drill 2.7) (layers "*.Cu" "*.Mask"))
  )
  (footprint "footprints:PiLogoSmall" (layer "F.Cu")
    (at 100.838 217.551)
    (attr through_hole)
    (fp_text reference "G***" (at 0 0) (layer "F.SilkS") hide)
    (fp_text value "LOGO" (at 0.75 0) (layer "F.SilkS") hide)
  )
  (footprint "MountingHole:MountingHole_2.7mm_M2.5" (layer "F.Cu")
    (at 54.0258 214.2122 -90)
    (descr "Mounting Hole 2.7mm, no annular, M2.5")
    (tags "mounting hole 2.7mm no annular m2.5")
    (property "Sheetfile" "TCMux.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "MK3" (at 3.3642 3.101 90) (layer "F.SilkS") hide)
    (fp_text value "M2.5" (at 0 3.7 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0 270) (size 2.7 2.7) (drill 2.7) (layers "*.Cu" "*.Mask"))
  )
  (footprint "footprints:Marvin" (layer "F.Cu")
    (at 141.530486 254.664686)
    (attr board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "G***" (at 0 0) (layer "F.SilkS") hide)
    (fp_text value "LOGO" (at 0.75 0) (layer "F.SilkS") hide)
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical" (layer "F.Cu")
    (at 139.45628 227.7679 180)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (property "Sheetfile" "TCMux.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x04, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J2" (at -0.04052 10.0899) (layer "F.SilkS"))
    (fp_text value "I2C Expansion" (at 0 9.95) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 3.81 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 14 "GND") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 17 "+3V3") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 64 "/GPIO03(SCL1,I2C)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 7.62 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 63 "/GPIO02(SDA1,I2C)") (pinfunction "Pin_4") (pintype "passive"))
    (model "${KIPRJMOD}/ESQ-104-14-G-S.stp"
      (offset (xyz 0 -3.6 2.5))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 90))
    )
  )
  (footprint "Capacitor_Tantalum_SMD:CP_EIA-3216-18_Kemet-A_Pad1.58x1.35mm_HandSolder" (layer "F.Cu")
    (at 145.29828 225.892236 -90)
    (descr "Tantalum Capacitor SMD Kemet-A (3216-18 Metric), IPC_7351 nominal, (Body size from: http://www.kemet.com/Lists/ProductCatalog/Attachments/253/KEM_TC101_STD.pdf), generated with kicad-footprint-generator")
    (tags "capacitor tantalum")
    (property "Sheetfile" "TCMux.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C10" (at 3.164964 -0.09132) (layer "F.SilkS"))
    (fp_text value "10uF" (at 0 1.75 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.4375 0 270) (size 1.575 1.35) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.185185)
      (net 17 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect (at 1.4375 0 270) (size 1.575 1.35) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.185185)
      (net 14 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_Tantalum_SMD.3dshapes/CP_EIA-3216-18_Kemet-A.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder" (layer "F.Cu")
    (at 88.46898 230.0307 -90)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "TCMux.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C4" (at 0.7365 -1.85) (layer "F.SilkS"))
    (fp_text value "100nF" (at 0 1.85 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0 270) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 17 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0 270) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 14 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_2.7mm_M2.5" (layer "F.Cu")
    (at 151.04428 197.9479 -90)
    (descr "Mounting Hole 2.7mm, no annular, M2.5")
    (tags "mounting hole 2.7mm no annular m2.5")
    (property "Sheetfile" "TCMux.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "MK1" (at 0 -3.7 90) (layer "F.SilkS") hide)
    (fp_text value "M2.5" (at 0 3.7 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0 270) (size 2.7 2.7) (drill 2.7) (layers "*.Cu" "*.Mask"))
  )
  (footprint "footprints:8 pin Screw Terminal P 2.54mm" (layer "F.Cu")
    (at 53.216904 205.8622)
    (property "Sheetfile" "TCMux.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic screw terminal, single row, 01x08, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "screw terminal")
    (attr through_hole)
    (fp_text reference "J3" (at -1.2516 4.0132 unlocked) (layer "F.SilkS"))
    (fp_text value "Screw_Terminal_01x08" (at 7.1 4.3 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole oval (at 0 0) (size 1.4 2.5) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 21 "Net-(J3-Pin_1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 2.526127 0) (size 1.4 2.5) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 22 "Net-(J3-Pin_2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 5.071884 0) (size 1.4 2.5) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 23 "Net-(J3-Pin_3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 7.617641 0) (size 1.4 2.5) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 24 "Net-(J3-Pin_4)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 10.139606 0) (size 1.4 2.5) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 25 "Net-(J3-Pin_5)") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 12.7 0) (size 1.4 2.5) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 26 "Net-(J3-Pin_6)") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole oval (at 15.23112 0) (size 1.4 2.5) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 27 "Net-(J3-Pin_7)") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" thru_hole oval (at 17.776876 0) (size 1.4 2.5) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 28 "Net-(J3-Pin_8)") (pinfunction "Pin_8") (pintype "passive"))
    (model "${KIPRJMOD}/1725711.stp"
      (offset (xyz 19.2 3.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (footprint "Library:Barcode" (layer "B.Cu")
    (at 93.98 215.265 180)
    (attr board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "G***" (at 0 0) (layer "B.SilkS") hide)
    (fp_text value "LOGO" (at 0.75 0) (layer "B.SilkS") hide)
  )
  (gr_line (start 50.002927 196.908533) (end 50.01792 256.930514)
    (layer "Edge.Cuts"))
  (gr_line (start 53.0716 259.976834) (end 152.04428 259.9479)
    (layer "Edge.Cuts"))
  (gr_arc (start 152.04428 193.9479) (mid 154.165613 194.826573) (end 155.04428 196.9479)
    (layer "Edge.Cuts"))
  (gr_line (start 155.04428 256.9479) (end 155.04428 196.9479)
    (layer "Edge.Cuts"))
  (gr_arc (start 53.0716 259.976834) (mid 50.912733 259.087209) (end 50.01792 256.930514)
    (layer "Edge.Cuts"))
  (gr_arc (start 155.04428 256.9479) (mid 154.165599 259.069213) (end 152.04428 259.9479)
    (layer "Edge.Cuts"))
  (gr_arc (start 50.002927 196.908533) (mid 50.881597 194.787201) (end 53.002927 193.908533)
    (layer "Edge.Cuts"))
  (gr_line (start 152.04428 193.9479) (end 53.002927 193.908533)
    (layer "Edge.Cuts"))
  (gr_text "MOSI" (at 146.812 225.806) (layer "B.SilkS"))
  (gr_text "SDA1" (at 146.7612 205.4098) (layer "B.SilkS"))
  (gr_text "SCLK" (at 146.7104 230.8352) (layer "B.SilkS"))
  (gr_text "SCL1" (at 146.812 208.1022) (layer "B.SilkS"))
  (gr_text "MISO" (at 146.812 228.2698) (layer "B.SilkS"))
  (gr_text "https://hackaday.io/project/192812-expandable-thermocouple-multiplexor-board" (at 129.54 198.12) (layer "B.SilkS"))
  (gr_text "/FAULT" (at 145.796 243.3066) (layer "B.SilkS"))
  (gr_text "/DRDY" (at 146.0754 238.4044) (layer "B.SilkS"))
  (gr_text "CE" (at 147.6248 232.3338) (layer "B.SilkS"))
  (gr_text "Ch.32" (at 53.6702 255.0668) (layer "F.SilkS"))
  (gr_text "Another Project By" (at 141.9098 239.5728) (layer "F.SilkS"))
  (gr_text "Ch.1" (at 54.0512 198.6534) (layer "F.SilkS"))
  (gr_text "- + - + - + - +" (at 82.6516 201.1172) (layer "F.SilkS"))
  (gr_text "- + - + - + - +" (at 61.6966 201.1172) (layer "F.SilkS"))
  (gr_text "- + - + - + - +" (at 124.5616 201.1172) (layer "F.SilkS"))
  (gr_text "- + - + - + - +" (at 103.6066 201.1172) (layer "F.SilkS"))
  (gr_text "Pi-Play" (at 139.7254 241.6048) (layer "F.SilkS"))
  (gr_text "- + - + - + - +" (at 103.6066 252.5522 -180) (layer "F.SilkS"))
  (gr_text "- + - + - + - +" (at 124.5616 252.5522 -180) (layer "F.SilkS"))
  (gr_text "- + - + - + - +" (at 61.6966 252.5522 -180) (layer "F.SilkS"))
  (gr_text "I2C \nExpansion" (at 136.7028 231.9274) (layer "F.SilkS"))
  (gr_text "Thermocouples supported:\nK J R S T E B" (at 93.345 256.6416) (layer "F.SilkS"))
  (gr_text "TC\nExpansion" (at 72.9996 229.9716) (layer "F.SilkS"))
  (gr_text "- + - + - + - +" (at 82.6516 252.5522 -180) (layer "F.SilkS"))
  (gr_text "Ch.17" (at 133.1976 254.9652) (layer "F.SilkS"))
  (gr_text "Board\nAddress" (at 130.81 212.7504) (layer "F.SilkS"))
  (gr_text "Ch.16" (at 132.9182 198.4502) (layer "F.SilkS"))
  (gr_text "32 Channel Expandable Thermocouple\nMultiplexer for Raspberry Pi" (at 93.6244 197.2564) (layer "F.SilkS"))
  (dimension (type aligned) (layer "Dwgs.User")
    (pts (xy 50.01792 256.930514) (xy 155.04428 256.9479))
    (height 6.33)
    (gr_text "105.0264 mm" (at 102.530242 262.119207 359.9905153) (layer "Dwgs.User"))
    (format (prefix "") (suffix "") (units 3) (units_format 1) (precision 4))
    (style (thickness 0.1) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (dimension (type aligned) (layer "Dwgs.User")
    (pts (xy 152.04428 259.9479) (xy 152.04428 193.9479))
    (height 7.01052)
    (gr_text "66.0000 mm" (at 157.9048 226.9479 90) (layer "Dwgs.User"))
    (format (prefix "") (suffix "") (units 3) (units_format 1) (precision 4))
    (style (thickness 0.1) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (zone (net 14) (net_name "GND") (layer "F.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.254) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 49.6316 260.1722)
        (xy 49.6316 193.4972)
        (xy 155.0416 193.4972)
        (xy 155.0416 260.1722)
      )
    )
  )
  (zone (net 14) (net_name "GND") (layers "F&B.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.254) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 49.6316 260.1722)
        (xy 49.6316 193.4972)
        (xy 155.0416 193.4972)
        (xy 155.0416 260.1722)
      )
    )
  )
)
