(kicad_pcb (version 20221018) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (plot_on_all_layers_selection 0x0000000_00000000)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (dashed_line_dash_ratio 12.000000)
      (dashed_line_gap_ratio 3.000000)
      (svgprecision 4)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "VIN")
  (net 2 "GND")
  (net 3 "VBat")
  (net 4 "VINA")
  (net 5 "VOut")
  (net 6 "unconnected-(CN1-Pad4)")
  (net 7 "unconnected-(CN1-Pad3)")
  (net 8 "+5V")
  (net 9 "Net-(D2-K)")
  (net 10 "Net-(D2-A)")
  (net 11 "Net-(D3-K)")
  (net 12 "Net-(L1-Pad2)")
  (net 13 "Net-(L1-Pad1)")
  (net 14 "VCCSolar")
  (net 15 "Net-(U1-ISET)")
  (net 16 "Net-(U3-FB)")
  (net 17 "PG")
  (net 18 "PS")
  (net 19 "unconnected-(U1-EP-Pad9)")
  (net 20 "unconnected-(USBC1-SBU2-PadB8)")
  (net 21 "unconnected-(USBC1-CC1-PadA5)")
  (net 22 "unconnected-(USBC1-DN2-PadB7)")
  (net 23 "unconnected-(USBC1-DP1-PadA6)")
  (net 24 "unconnected-(USBC1-DN1-PadA7)")
  (net 25 "unconnected-(USBC1-DP2-PadB6)")
  (net 26 "unconnected-(USBC1-SBU1-PadA8)")
  (net 27 "unconnected-(USBC1-CC2-PadB5)")
  (footprint "easyeda2kicad:IND-SMD_L4.0-W4.0" (layer "F.Cu")
    (at 138.684 73.406)
    (property "LCSC Part" "C436670")
    (property "Sheetfile" "Solar-Buck-Boost.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "L1" (at 0.127 -3.048) (layer "F.SilkS"))
    (fp_text value "PSPNAQ4030-1R5M" (at -8.875 40.7175 -90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect (at -1.6 0) (size 1.6 3.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 13 "Net-(L1-Pad1)") (pinfunction "1") (pintype "unspecified"))
    (pad "2" smd rect (at 1.6 0) (size 1.6 3.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "Net-(L1-Pad2)") (pinfunction "2") (pintype "unspecified"))
    (model "${EASYEDA2KICAD}/easyeda2kicad.3dshapes/IND-SMD_L4.0-W4.0-H1.9.wrl"
      (offset (xyz 0 -0 -0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )
  (footprint "Resistor_SMD:R_0402_1005Metric" (layer "F.Cu")
    (at 143.595 94.613 -90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "Solar-Buck-Boost.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R7" (at -2.03 -0.042 90) (layer "F.SilkS"))
    (fp_text value "0" (at 0 1.17 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.51 0 270) (size 0.54 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "VINA") (pintype "passive"))
    (pad "2" smd roundrect (at 0.51 0 270) (size 0.54 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 18 "PS") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "easyeda2kicad:SOT-23_L2.9-W1.3-P1.90-LS2.4-BR" (layer "F.Cu")
    (at 117.856 81.534 180)
    (property "LCSC Part" "C347476")
    (property "Sheetfile" "Solar-Buck-Boost.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "Q1" (at 0.508 2.413) (layer "F.SilkS"))
    (fp_text value "AO3401A_C347476" (at 0 4.95) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect (at 1.15 0.95) (size 1 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 8 "+5V") (pinfunction "G") (pintype "unspecified"))
    (pad "2" smd rect (at 1.15 -0.95) (size 1 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "VIN") (pinfunction "S") (pintype "unspecified"))
    (pad "3" smd rect (at -1.15 0) (size 1 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 14 "VCCSolar") (pinfunction "D") (pintype "unspecified"))
    (model "${EASYEDA2KICAD}/easyeda2kicad.3dshapes/SOT-23-3P_L2.9-W1.3-H1.0-LS2.4-P0.95.wrl"
      (offset (xyz 0 -0 -0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (at 133.35 78.552 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "Solar-Buck-Boost.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C4" (at 2.352 0 180) (layer "F.SilkS"))
    (fp_text value "10uF" (at 0 1.68 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.95 0 90) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "VBat") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 90) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0402_1005Metric" (layer "F.Cu")
    (at 141.605 94.613 -90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "Solar-Buck-Boost.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R8" (at -2.03 0 90) (layer "F.SilkS"))
    (fp_text value "0" (at 0 1.17 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.51 0 270) (size 0.54 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 18 "PS") (pintype "passive"))
    (pad "2" smd roundrect (at 0.51 0 270) (size 0.54 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (at 143.256 81.788 -90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "Solar-Buck-Boost.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C5" (at 0 -1.778 -180) (layer "F.SilkS"))
    (fp_text value "100nF" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.775 0 270) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "VINA") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0 270) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_2.5mm" (layer "F.Cu")
    (at 107.442 96.012)
    (descr "Mounting Hole 2.5mm, no annular")
    (tags "mounting hole 2.5mm no annular")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 -3.5) (layer "F.SilkS") hide)
    (fp_text value "MountingHole_2.5mm" (at 0 3.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 2.5 2.5) (drill 2.5) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (at 124.46 84.074 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "Solar-Buck-Boost.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R2" (at 2.54 0 180) (layer "F.SilkS"))
    (fp_text value "3.6K" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 15 "Net-(U1-ISET)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (at 141.478 87.2255 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "Solar-Buck-Boost.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R6" (at 2.8975 -0.058 90) (layer "F.SilkS"))
    (fp_text value "1M" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 5 "VOut") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 17 "PG") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "easyeda2kicad:CONN-SMD_2001SMT-2P-WT" (layer "F.Cu")
    (at 120.904 73.914 180)
    (property "LCSC Part" "C132500")
    (property "Sheetfile" "Solar-Buck-Boost.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "CN1" (at 7.112 1.016) (layer "F.SilkS"))
    (fp_text value "2001SMT-2P_C132500" (at 0 6.75) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect (at -1 -2.75 180) (size 0.8 3.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "VBat") (pinfunction "1") (pintype "unspecified"))
    (pad "2" smd rect (at 1 -2.72 180) (size 0.8 3.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "2") (pintype "unspecified"))
    (pad "3" smd rect (at 3.5 2.75 180) (size 1.5 3.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 7 "unconnected-(CN1-Pad3)") (pinfunction "3") (pintype "unspecified+no_connect"))
    (pad "4" smd rect (at -3.5 2.75 180) (size 1.5 3.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 6 "unconnected-(CN1-Pad4)") (pinfunction "4") (pintype "unspecified+no_connect"))
    (model "${EASYEDA2KICAD}/easyeda2kicad.3dshapes/CONN-SMD_2001SMT-2P-WT.wrl"
      (offset (xyz 1 -3.23 -0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (at 143.002 77.282 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "Solar-Buck-Boost.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C6" (at 2.352 0) (layer "F.SilkS"))
    (fp_text value "22uF" (at 0 1.68 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.95 0 90) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "VOut") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 90) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (at 128.27 78.552 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "Solar-Buck-Boost.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C2" (at 2.352 0 180) (layer "F.SilkS"))
    (fp_text value "4.7uF" (at 0 1.68 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.95 0 90) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "VBat") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 90) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "easyeda2kicad:CAP-SMD_L3.5-W2.8-R-RD" (layer "F.Cu")
    (at 116.332 86.868 180)
    (property "LCSC Part" "C140371")
    (property "Sheetfile" "Solar-Buck-Boost.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C1" (at 0 2.54) (layer "F.SilkS"))
    (fp_text value "CA45-B-16V-22UF-M" (at -13.54 -32.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect (at 1.9 0 180) (size 1.9 2.38) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "VIN") (pinfunction "1") (pintype "input"))
    (pad "2" smd rect (at -1.9 0 180) (size 1.9 2.38) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "2") (pintype "input"))
    (model "${EASYEDA2KICAD}/easyeda2kicad.3dshapes/CASE-B_L3.5-W2.8-H1.9.wrl"
      (offset (xyz 0 0 1))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (at 147.574 77.282 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "Solar-Buck-Boost.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C8" (at 2.352 -0.178 180) (layer "F.SilkS"))
    (fp_text value "22uF" (at 0 2.696 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.95 0 90) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "VOut") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 90) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_2.5mm" (layer "F.Cu")
    (at 150.876 96.012)
    (descr "Mounting Hole 2.5mm, no annular")
    (tags "mounting hole 2.5mm no annular")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 -3.5) (layer "F.SilkS") hide)
    (fp_text value "MountingHole_2.5mm" (at 0 3.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 2.5 2.5) (drill 2.5) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Connector_PinSocket_2.54mm:PinSocket_1x01_P2.54mm_Vertical" (layer "F.Cu")
    (at 152.654 90.17)
    (descr "Through hole straight socket strip, 1x01, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x01 2.54mm single row")
    (property "Sheetfile" "Solar-Buck-Boost.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x01, script generated")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J3" (at 0 -2.77) (layer "F.SilkS") hide)
    (fp_text value "Conn_01x01_Pin" (at -4.318 5.056) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "Pin_1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x01_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "easyeda2kicad:SOIC-8_L4.9-W3.9-P1.27-LS6.0-BL-EP3.3-1" (layer "F.Cu")
    (at 130.99 84.206 -90)
    (property "LCSC Part" "C28078")
    (property "Sheetfile" "Solar-Buck-Boost.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U1" (at 3.678 0.0784 -180) (layer "F.SilkS"))
    (fp_text value "CN3063" (at 0 6.72 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd oval (at -1.9 2.72 270) (size 0.6 1.94) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "TEMP") (pintype "unspecified"))
    (pad "2" smd oval (at -0.63 2.72 270) (size 0.6 1.94) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "Net-(U1-ISET)") (pinfunction "ISET") (pintype "unspecified"))
    (pad "3" smd oval (at 0.64 2.72 270) (size 0.6 1.94) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "unspecified"))
    (pad "4" smd oval (at 1.9 2.72 270) (size 0.6 1.94) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "VIN") (pinfunction "VIN") (pintype "unspecified"))
    (pad "5" smd oval (at 1.9 -2.72 270) (size 0.6 1.94) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "VBat") (pinfunction "BAT") (pintype "unspecified"))
    (pad "6" smd oval (at 0.64 -2.72 270) (size 0.6 1.94) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "Net-(D2-K)") (pinfunction "DONE") (pintype "unspecified"))
    (pad "7" smd oval (at -0.63 -2.72 270) (size 0.6 1.94) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 11 "Net-(D3-K)") (pinfunction "CHRG") (pintype "unspecified"))
    (pad "8" smd oval (at -1.9 -2.72 270) (size 0.6 1.94) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "VBat") (pinfunction "FB") (pintype "unspecified"))
    (pad "9" smd rect (at 0 0 270) (size 3.3 2.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 19 "unconnected-(U1-EP-Pad9)") (pinfunction "EP") (pintype "unspecified+no_connect"))
    (model "${EASYEDA2KICAD}/easyeda2kicad.3dshapes/SOIC-8_L4.9-W3.9-P1.27-LS6.0-BL-EP3.3-1.wrl"
      (offset (xyz 0 -0.08 1))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinSocket_2.54mm:PinSocket_1x01_P2.54mm_Vertical" (layer "F.Cu")
    (at 152.654 78.232)
    (descr "Through hole straight socket strip, 1x01, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x01 2.54mm single row")
    (property "Sheetfile" "Solar-Buck-Boost.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x01, script generated")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J2" (at 0 -2.77) (layer "F.SilkS") hide)
    (fp_text value "Conn_01x01_Pin" (at -3.81 2.503) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 5 "VOut") (pinfunction "Pin_1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x01_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_2.5mm" (layer "F.Cu")
    (at 107.442 72.644)
    (descr "Mounting Hole 2.5mm, no annular")
    (tags "mounting hole 2.5mm no annular")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 -3.5) (layer "F.SilkS") hide)
    (fp_text value "MountingHole_2.5mm" (at 0 3.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 2.5 2.5) (drill 2.5) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (at 113.284 80.772 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "Solar-Buck-Boost.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R1" (at 2.286 0) (layer "F.SilkS"))
    (fp_text value "1K" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 8 "+5V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_0805_2012Metric" (layer "F.Cu")
    (at 132.588 95.3285 -90)
    (descr "LED SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "LED")
    (property "Sheetfile" "Solar-Buck-Boost.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Light emitting diode")
    (property "ki_keywords" "LED diode")
    (attr smd)
    (fp_text reference "D2" (at 2.4615 0) (layer "F.SilkS"))
    (fp_text value "LED" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9375 0 270) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 9 "Net-(D2-K)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9375 0 270) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 10 "Net-(D2-A)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "easyeda2kicad:USB-C_SMD-TYPE-C-31-M-12" (layer "F.Cu")
    (at 107.4785 84.34 -90)
    (property "LCSC Part" "C165948")
    (property "Sheetfile" "Solar-Buck-Boost.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "USBC1" (at -6.362 0.0365) (layer "F.SilkS"))
    (fp_text value "TYPE-C-31-M-12" (at 0 6.47 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "" thru_hole circle (at -2.9 -1.21 270) (size 0.75 0.75) (drill 0.75) (layers "*.Cu" "*.Mask"))
    (pad "" thru_hole circle (at 2.9 -1.21 270) (size 0.75 0.75) (drill 0.75) (layers "*.Cu" "*.Mask"))
    (pad "0" thru_hole oval (at -4.33 -1.71 270) (size 1.2 2) (drill oval 0.799998 1.600022) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "SH") (pintype "unspecified"))
    (pad "1" thru_hole oval (at 4.33 -1.71 270) (size 1.2 2) (drill oval 0.799998 1.599971) (layers "*.Cu" "*.Mask"))
    (pad "2" thru_hole oval (at 4.33 2.47 270) (size 1.2 1.8) (drill oval 0.799998 1.399997) (layers "*.Cu" "*.Mask"))
    (pad "3" thru_hole oval (at -4.33 2.47 270) (size 1.2 1.8) (drill oval 0.799998 1.399997) (layers "*.Cu" "*.Mask"))
    (pad "A1" smd rect (at -3.35 -2.47 270) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "unspecified"))
    (pad "A4" smd rect (at -2.55 -2.47 270) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 8 "+5V") (pinfunction "VBUS") (pintype "unspecified"))
    (pad "A5" smd rect (at -1.25 -2.47 270) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 21 "unconnected-(USBC1-CC1-PadA5)") (pinfunction "CC1") (pintype "unspecified+no_connect"))
    (pad "A6" smd rect (at -0.25 -2.47 270) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 23 "unconnected-(USBC1-DP1-PadA6)") (pinfunction "DP1") (pintype "unspecified+no_connect"))
    (pad "A7" smd rect (at 0.25 -2.47 270) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 24 "unconnected-(USBC1-DN1-PadA7)") (pinfunction "DN1") (pintype "unspecified+no_connect"))
    (pad "A8" smd rect (at 1.25 -2.47 270) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 26 "unconnected-(USBC1-SBU1-PadA8)") (pinfunction "SBU1") (pintype "unspecified+no_connect"))
    (pad "A9" smd rect (at 2.55 -2.47 270) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 8 "+5V") (pinfunction "VBUS") (pintype "unspecified"))
    (pad "A12" smd rect (at 3.35 -2.47 270) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "unspecified"))
    (pad "B1" smd rect (at 3.05 -2.47 270) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "unspecified"))
    (pad "B4" smd rect (at 2.25 -2.47 270) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 8 "+5V") (pinfunction "VBUS") (pintype "unspecified"))
    (pad "B5" smd rect (at 1.75 -2.47 270) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 27 "unconnected-(USBC1-CC2-PadB5)") (pinfunction "CC2") (pintype "unspecified+no_connect"))
    (pad "B6" smd rect (at 0.75 -2.47 270) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 25 "unconnected-(USBC1-DP2-PadB6)") (pinfunction "DP2") (pintype "unspecified+no_connect"))
    (pad "B7" smd rect (at -0.75 -2.47 270) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 22 "unconnected-(USBC1-DN2-PadB7)") (pinfunction "DN2") (pintype "unspecified+no_connect"))
    (pad "B8" smd rect (at -1.75 -2.47 270) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 20 "unconnected-(USBC1-SBU2-PadB8)") (pinfunction "SBU2") (pintype "unspecified+no_connect"))
    (pad "B9" smd rect (at -2.25 -2.47 270) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 8 "+5V") (pinfunction "VBUS") (pintype "unspecified"))
    (pad "B12" smd rect (at -3.05 -2.47 270) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "unspecified"))
    (model "${EASYEDA2KICAD}/easyeda2kicad.3dshapes/USB-C_SMD-TYPE-C-31-M-12.wrl"
      (offset (xyz 0 -2.5 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (at 146.939 87.202 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "Solar-Buck-Boost.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R4" (at 2.8975 0 90) (layer "F.SilkS"))
    (fp_text value "1M" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 5 "VOut") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 16 "Net-(U3-FB)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical" (layer "F.Cu")
    (at 129.789 72.136 90)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (property "Sheetfile" "Solar-Buck-Boost.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x02, script generated")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J1" (at 0 -2.5858 180) (layer "F.SilkS"))
    (fp_text value "Conn_01x02_Pin" (at -0.762 0.298 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 1.27) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 3 "VBat") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "Pin_2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (at 130.81 78.552 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "Solar-Buck-Boost.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C3" (at 2.352 0) (layer "F.SilkS"))
    (fp_text value "10uF" (at 0 1.68 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.95 0 90) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "VBat") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 90) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (at 143.568 87.2255 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "Solar-Buck-Boost.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R5" (at 2.8975 -0.156 90) (layer "F.SilkS"))
    (fp_text value "180K" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 16 "Net-(U3-FB)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_0805_2012Metric" (layer "F.Cu")
    (at 130.302 95.3285 -90)
    (descr "LED SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "LED")
    (property "Sheetfile" "Solar-Buck-Boost.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Light emitting diode")
    (property "ki_keywords" "LED diode")
    (attr smd)
    (fp_text reference "D3" (at 2.4615 0 -180) (layer "F.SilkS"))
    (fp_text value "LED" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9375 0 270) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 11 "Net-(D3-K)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9375 0 270) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 10 "Net-(D2-A)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (at 145.288 77.282 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "Solar-Buck-Boost.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C7" (at 2.352 0.038 180) (layer "F.SilkS"))
    (fp_text value "22uF" (at 0 1.68 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.95 0 90) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "VOut") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 90) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (at 131.064 90.678)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "Solar-Buck-Boost.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R3" (at 3.048 0.254) (layer "F.SilkS"))
    (fp_text value "1K" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 1 "VIN") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 10 "Net-(D2-A)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "easyeda2kicad:SMA_L4.2-W2.6-LS5.3-RD" (layer "F.Cu")
    (at 121.92 84.328 90)
    (property "LCSC Part" "C2480")
    (property "Sheetfile" "Solar-Buck-Boost.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D1" (at 4.826 0 180) (layer "F.SilkS"))
    (fp_text value "SS14" (at 0 4 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd rect (at -2.57 0 90) (size 2.2 1.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "VIN") (pinfunction "K") (pintype "unspecified"))
    (pad "2" smd rect (at 2.57 0 90) (size 2.2 1.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 8 "+5V") (pinfunction "A") (pintype "unspecified"))
    (model "${EASYEDA2KICAD}/easyeda2kicad.3dshapes/SMA_L4.2-W2.6-LS5.3-RD.wrl"
      (offset (xyz -0 0 -0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "easyeda2kicad:VSON-14_L4.0-W3.0-P0.50-BL-EP_TI_DSJ" (layer "F.Cu")
    (at 138.758 79.526 90)
    (property "LCSC Part" "C15483")
    (property "Sheetfile" "Solar-Buck-Boost.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U3" (at -3.3288 0.0276 180) (layer "F.SilkS"))
    (fp_text value "TPS63020DSJR" (at -6.35 -0.522 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd rect (at -1.5 1.45 90) (size 0.25 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "VINA") (pinfunction "VINA") (pintype "unspecified"))
    (pad "2" smd rect (at -1 1.45 90) (size 0.25 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "unspecified"))
    (pad "3" smd rect (at -0.5 1.45 90) (size 0.25 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 16 "Net-(U3-FB)") (pinfunction "FB") (pintype "unspecified"))
    (pad "4" smd rect (at 0 1.45 90) (size 0.25 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "VOut") (pinfunction "VOUT") (pintype "unspecified"))
    (pad "5" smd rect (at 0.5 1.45 90) (size 0.25 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "VOut") (pinfunction "VOUT") (pintype "unspecified"))
    (pad "6" smd rect (at 1 1.45 90) (size 0.25 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "Net-(L1-Pad2)") (pinfunction "L2") (pintype "unspecified"))
    (pad "7" smd rect (at 1.5 1.45 90) (size 0.25 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "Net-(L1-Pad2)") (pinfunction "L2") (pintype "unspecified"))
    (pad "8" smd rect (at 1.5 -1.45 90) (size 0.25 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 13 "Net-(L1-Pad1)") (pinfunction "L1") (pintype "unspecified"))
    (pad "9" smd rect (at 1 -1.45 90) (size 0.25 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 13 "Net-(L1-Pad1)") (pinfunction "L1") (pintype "unspecified"))
    (pad "10" smd rect (at 0.5 -1.45 270) (size 0.25 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "VBat") (pinfunction "VIN") (pintype "unspecified"))
    (pad "11" smd rect (at 0 -1.45 270) (size 0.25 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "VBat") (pinfunction "VIN") (pintype "unspecified"))
    (pad "12" smd rect (at -0.5 -1.45 270) (size 0.25 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "VINA") (pinfunction "EN") (pintype "unspecified"))
    (pad "13" smd rect (at -1 -1.45 270) (size 0.25 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 18 "PS") (pinfunction "PS/SYNC") (pintype "unspecified"))
    (pad "14" smd rect (at -1.5 -1.45 270) (size 0.25 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 17 "PG") (pinfunction "PG") (pintype "unspecified"))
    (pad "15" smd custom (at 0 0 90) (size 1 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "PGND") (pintype "unspecified") (thermal_bridge_angle 90)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly
          (pts
            (xy -2.2 -0.79)
            (xy -2.2 -0.59)
            (xy -1.43 -0.59)
            (xy -1.43 -0.33)
            (xy -2.2 -0.33)
            (xy -2.2 -0.13)
            (xy -1.43 -0.13)
            (xy -1.43 0.13)
            (xy -2.2 0.13)
            (xy -2.2 0.33)
            (xy -1.43 0.33)
            (xy -1.43 0.59)
            (xy -2.2 0.59)
            (xy -2.2 0.79)
            (xy 2.2 0.79)
            (xy 2.2 0.59)
            (xy 1.43 0.59)
            (xy 1.43 0.33)
            (xy 2.2 0.33)
            (xy 2.2 0.13)
            (xy 1.43 0.13)
            (xy 1.43 -0.13)
            (xy 2.2 -0.13)
            (xy 2.2 -0.33)
            (xy 1.43 -0.33)
            (xy 1.43 -0.59)
            (xy 2.2 -0.59)
            (xy 2.2 -0.79)
            (xy -2.2 -0.79)
          )
          (width 0.1) (fill yes))
      ))
    (model "${EASYEDA2KICAD}/easyeda2kicad.3dshapes/VSON-14_L4.0-W3.0-H1.0-P0.50.wrl"
      (offset (xyz 0 -0 -0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )
  (footprint "easyeda2kicad:CONN-TH_2P-P5.00_L7.6-W10.0" (layer "F.Cu")
    (at 119.126 94.742)
    (property "LCSC Part" "C395882")
    (property "Sheetfile" "Solar-Buck-Boost.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "H1" (at 0.1524 -4.9784) (layer "F.SilkS"))
    (fp_text value "DB301V-5.0-2P" (at 0 4) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at -2.5 0) (size 2 2) (drill 1.300023) (layers "*.Cu" "*.Mask")
      (net 14 "VCCSolar") (pinfunction "1") (pintype "unspecified"))
    (pad "2" thru_hole circle (at 2.5 0) (size 2 2) (drill 1.300023) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "2") (pintype "unspecified"))
    (model "${EASYEDA2KICAD}/easyeda2kicad.3dshapes/CONN-TH_DB5.00-LI-2P-301.wrl"
      (offset (xyz 2.5 -2.32 4))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_2.5mm" (layer "F.Cu")
    (at 150.876 72.644)
    (descr "Mounting Hole 2.5mm, no annular")
    (tags "mounting hole 2.5mm no annular")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 -3.5) (layer "F.SilkS") hide)
    (fp_text value "MountingHole_2.5mm" (at -2.032 4.262) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 2.5 2.5) (drill 2.5) (layers "*.Cu" "*.Mask"))
  )
  (gr_line (start 103.632 72.644) (end 103.632 96.012)
    (layer "Edge.Cuts"))
  (gr_arc (start 103.632 72.644) (mid 104.747923 69.949923) (end 107.442 68.834)
    (layer "Edge.Cuts"))
  (gr_arc (start 150.876 68.834) (mid 153.570077 69.949923) (end 154.686 72.644)
    (layer "Edge.Cuts"))
  (gr_line (start 154.686 96.012) (end 154.686 72.644)
    (layer "Edge.Cuts"))
  (gr_line (start 107.442 99.822) (end 150.876 99.822)
    (layer "Edge.Cuts"))
  (gr_line (start 150.876 68.834) (end 107.442 68.834)
    (layer "Edge.Cuts"))
  (gr_arc (start 154.686 96.012) (mid 153.570077 98.706077) (end 150.876 99.822)
    (layer "Edge.Cuts"))
  (gr_arc (start 107.442 99.822) (mid 104.747923 98.706077) (end 103.632 96.012)
    (layer "Edge.Cuts"))
  (gr_text "- VOut +" (at 153.162 87.9348 90) (layer "F.SilkS"))
  (gr_text "SOLARIN+" (at 112.7252 97.9932 90) (layer "F.SilkS"))
  (gr_text "SOLARIN-" (at 126.238 98.0948 90) (layer "F.SilkS"))
  (zone (net 2) (net_name "GND") (layers "F&B.Cu") (hatch edge 0.5)
    (connect_pads (clearance 0.5))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 150.749 69.215)
        (xy 152.4 69.596)
        (xy 153.289 70.104)
        (xy 153.924 71.247)
        (xy 154.305 72.263)
        (xy 154.305 96.647)
        (xy 154.051 97.409)
        (xy 153.416 98.298)
        (xy 152.4 98.933)
        (xy 151.384 99.314)
        (xy 107.315 99.314)
        (xy 105.918 98.933)
        (xy 105.029 98.298)
        (xy 104.267 97.282)
        (xy 104.013 96.266)
        (xy 104.013 72.39)
        (xy 104.394 71.12)
        (xy 105.156 70.231)
        (xy 106.045 69.596)
        (xy 106.934 69.215)
      )
    )
  )
)
