(kicad_pcb (version 20221018) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00310ff_ffffffff)
      (plot_on_all_layers_selection 0x0000000_00000000)
      (disableapertmacros false)
      (usegerberextensions true)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (dashed_line_dash_ratio 12.000000)
      (dashed_line_gap_ratio 3.000000)
      (svgprecision 4)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin true)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "Net-(U1-VC)")
  (net 2 "Net-(D2-K)")
  (net 3 "GND")
  (net 4 "Vbatt_12")
  (net 5 "Net-(D1-K)")
  (net 6 "+12V")
  (net 7 "+BATT")
  (net 8 "Vbatt_low")
  (net 9 "Net-(D5-K)")
  (net 10 "Net-(R1-Pad1)")
  (net 11 "Net-(R3-Pad2)")
  (footprint "Capacitor_THT:CP_Radial_D8.0mm_P3.50mm" (layer "F.Cu")
    (at 114.3 86.05 90)
    (descr "CP, Radial series, Radial, pin pitch=3.50mm, , diameter=8mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 3.50mm  diameter 8mm Electrolytic Capacitor")
    (property "Sheetfile" "down_converter.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Polarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr through_hole)
    (fp_text reference "C3" (at 6.04 3.175 180) (layer "F.SilkS"))
    (fp_text value "330uF/25V" (at 1.75 5.25 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.75 0 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 4 "Vbatt_12") (pintype "passive"))
    (pad "2" thru_hole circle (at 3.5 0 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 3 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_D8.0mm_P3.50mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_AMASS:AMASS_XT30U-F_1x02_P5.0mm_Vertical" (layer "F.Cu")
    (at 105.41 80.09 -90)
    (descr "Connector XT30 Vertical Cable Female, https://www.tme.eu/en/Document/3cbfa5cfa544d79584972dd5234a409e/XT30U%20SPEC.pdf")
    (tags "RC Connector XT30")
    (property "Sheetfile" "down_converter.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x02, script generated")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J3" (at -2.59 3.41) (layer "F.SilkS"))
    (fp_text value "Output" (at 2.5 4 90) (layer "F.Fab"))
    (fp_text user "-" (at -4 0 90) (layer "F.SilkS"))
    (fp_text user "+" (at 9 0 90) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 2.5 0 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 3.8 3.8) (drill 2.7) (layers "*.Cu" "*.Mask")
      (net 3 "GND") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole circle (at 5 0 270) (size 4 4) (drill 2.7) (layers "*.Cu" "*.Mask")
      (net 4 "Vbatt_12") (pinfunction "Pin_2") (pintype "passive"))
    (model "${KICAD7_3DMODEL_DIR}/Connector_AMASS.3dshapes/Amass_XT30UPB-F.wrl"
      (offset (xyz 2 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:TO-263-5_TabPin3" (layer "F.Cu")
    (at 140.74 63.5)
    (descr "TO-263/D2PAK/DDPAK SMD package, http://www.infineon.com/cms/en/product/packages/PG-TO263/PG-TO263-5-1/")
    (tags "D2PAK DDPAK TO-263 D2PAK-5 TO-263-5 SOT-426")
    (property "Sheetfile" "down_converter.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "5A 180kHz 36V Buck DC to DC Converter")
    (property "ki_keywords" "Buck DC-DC")
    (attr smd)
    (fp_text reference "U1" (at 4.04 -6.35) (layer "F.SilkS"))
    (fp_text value "XL4015" (at 0 6.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -7.65 -3.4) (size 4.6 1.1) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2272727273)
      (net 3 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "2" smd roundrect (at -7.65 -1.7) (size 4.6 1.1) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2272727273)
      (net 5 "Net-(D1-K)") (pinfunction "FB") (pintype "input"))
    (pad "3" smd roundrect (at -7.65 0) (size 4.6 1.1) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2272727273)
      (net 9 "Net-(D5-K)") (pinfunction "SW") (pintype "power_out"))
    (pad "3" smd roundrect (at -0.925 -2.775) (size 4.55 5.25) (layers "F.Cu" "F.Paste") (roundrect_rratio 0.05494505495)
      (net 9 "Net-(D5-K)") (pinfunction "SW") (pintype "power_out"))
    (pad "3" smd roundrect (at -0.925 2.775) (size 4.55 5.25) (layers "F.Cu" "F.Paste") (roundrect_rratio 0.05494505495)
      (net 9 "Net-(D5-K)") (pinfunction "SW") (pintype "power_out"))
    (pad "3" smd roundrect (at 1.5 0) (size 9.4 10.8) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.02659595745)
      (net 9 "Net-(D5-K)") (pinfunction "SW") (pintype "power_out"))
    (pad "3" smd roundrect (at 3.925 -2.775) (size 4.55 5.25) (layers "F.Cu" "F.Paste") (roundrect_rratio 0.05494505495)
      (net 9 "Net-(D5-K)") (pinfunction "SW") (pintype "power_out"))
    (pad "3" smd roundrect (at 3.925 2.775) (size 4.55 5.25) (layers "F.Cu" "F.Paste") (roundrect_rratio 0.05494505495)
      (net 9 "Net-(D5-K)") (pinfunction "SW") (pintype "power_out"))
    (pad "4" smd roundrect (at -7.65 1.7) (size 4.6 1.1) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2272727273)
      (net 1 "Net-(U1-VC)") (pinfunction "VC") (pintype "input"))
    (pad "5" smd roundrect (at -7.65 3.4) (size 4.6 1.1) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2272727273)
      (net 2 "Net-(D2-K)") (pinfunction "VIN") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/TO-263-5_TabPin3.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:CP_Radial_D8.0mm_P3.50mm" (layer "F.Cu")
    (at 125.73 64.46 90)
    (descr "CP, Radial series, Radial, pin pitch=3.50mm, , diameter=8mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 3.50mm  diameter 8mm Electrolytic Capacitor")
    (property "Sheetfile" "down_converter.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Polarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr through_hole)
    (fp_text reference "C4" (at 1.75 -5.25 90) (layer "F.SilkS"))
    (fp_text value "470uF/50V" (at 1.75 5.25 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.75 0 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 2 "Net-(D2-K)") (pintype "passive"))
    (pad "2" thru_hole circle (at 3.5 0 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 3 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_D8.0mm_P3.50mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical" (layer "F.Cu")
    (at 142.24 52.07 -90)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (property "Sheetfile" "down_converter.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J2" (at 0 -3.175 -180) (layer "F.SilkS"))
    (fp_text value "Shunt" (at 0 4.87 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 1.27) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 6 "+12V") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 8 "Vbatt_low") (pinfunction "Pin_2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_THT:D_DO-201AD_P15.24mm_Horizontal" (layer "F.Cu")
    (at 120.65 69.85 180)
    (descr "Diode, DO-201AD series, Axial, Horizontal, pin pitch=15.24mm, , length*diameter=9.5*5.2mm^2, , http://www.diodes.com/_files/packages/DO-201AD.pdf")
    (tags "Diode DO-201AD series Axial Horizontal pin pitch 15.24mm  length 9.5mm diameter 5.2mm")
    (property "Sheetfile" "down_converter.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "40V 3A Schottky Barrier Rectifier Diode, DO-201AD")
    (property "ki_keywords" "diode Schottky")
    (attr through_hole)
    (fp_text reference "D5" (at 7.62 -3.72) (layer "F.SilkS"))
    (fp_text value "1N5825" (at 7.62 3.72) (layer "F.Fab"))
    (fp_text user "K" (at 0 -2.6) (layer "F.SilkS"))
    (fp_text user "K" (at 0 -2.6) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 8.3325 0) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 180) (size 3.2 3.2) (drill 1.6) (layers "*.Cu" "*.Mask")
      (net 9 "Net-(D5-K)") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole oval (at 15.24 0 180) (size 3.2 3.2) (drill 1.6) (layers "*.Cu" "*.Mask")
      (net 3 "GND") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-201AD_P15.24mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Inductor_SMD:L_Bourns_SRP1245A" (layer "F.Cu")
    (at 140.97 81.28 -90)
    (descr "Bourns SRP1245A series SMD inductor http://www.bourns.com/docs/Product-Datasheets/SRP1245A.pdf")
    (tags "Bourns SRP1245A SMD inductor")
    (property "Sheetfile" "down_converter.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Inductor with ferrite core, small symbol")
    (property "ki_keywords" "inductor choke coil reactor magnetic")
    (attr smd)
    (fp_text reference "L2" (at 3.175 -7.62) (layer "F.SilkS"))
    (fp_text value "47uH/3.5A" (at 0 7.4 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd rect (at -5.55 0 270) (size 3.1 5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "Net-(D5-K)") (pintype "passive"))
    (pad "2" smd rect (at 5.55 0 270) (size 3.1 5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "Vbatt_12") (pintype "passive"))
    (model "${KICAD7_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_Bourns_SRR1260.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_AMASS:AMASS_XT30U-M_1x02_P5.0mm_Vertical" (layer "F.Cu")
    (at 105.41 59.65 90)
    (descr "Connector XT30 Vertical Cable Male, https://www.tme.eu/en/Document/3cbfa5cfa544d79584972dd5234a409e/XT30U%20SPEC.pdf")
    (tags "RC Connector XT30")
    (property "Sheetfile" "down_converter.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x02, script generated")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J1" (at -5.35 -1.91 180) (layer "F.SilkS"))
    (fp_text value "BAT" (at 2.5 4 90) (layer "F.Fab"))
    (fp_text user "-" (at -4 0 90) (layer "F.SilkS"))
    (fp_text user "+" (at 9 0 90) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 2.5 0 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 3.8 3.8) (drill 2.7) (layers "*.Cu" "*.Mask")
      (net 3 "GND") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole circle (at 5 0 90) (size 3.8 3.8) (drill 2.7) (layers "*.Cu" "*.Mask")
      (net 7 "+BATT") (pinfunction "Pin_2") (pintype "passive"))
    (model "${KICAD7_3DMODEL_DIR}/Connector_AMASS.3dshapes/Amass_XT30UPB-M.wrl"
      (offset (xyz 2 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Inductor_SMD:L_Bourns_SRP1245A" (layer "F.Cu")
    (at 125.73 81.28 -90)
    (descr "Bourns SRP1245A series SMD inductor http://www.bourns.com/docs/Product-Datasheets/SRP1245A.pdf")
    (tags "Bourns SRP1245A SMD inductor")
    (property "Sheetfile" "down_converter.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Inductor with ferrite core, small symbol")
    (property "ki_keywords" "inductor choke coil reactor magnetic")
    (attr smd)
    (fp_text reference "L1" (at 3.175 -7.62) (layer "F.SilkS"))
    (fp_text value "47uH/3.5A" (at 0 7.4 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd rect (at -5.55 0 270) (size 3.1 5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "Net-(D5-K)") (pintype "passive"))
    (pad "2" smd rect (at 5.55 0 270) (size 3.1 5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "Vbatt_12") (pintype "passive"))
    (model "${KICAD7_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_Bourns_SRR1260.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder" (layer "B.Cu")
    (at 118.11 84.1125 -90)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "down_converter.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C2" (at 0 1.85 90) (layer "B.SilkS"))
    (fp_text value "1uF" (at 0 -1.85 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1.5625 0 270) (size 1.325 1.8) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.1886792453)
      (net 3 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0 270) (size 1.325 1.8) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.1886792453)
      (net 4 "Vbatt_12") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "B.Cu")
    (at 125.73 81.28 -90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "down_converter.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, small symbol")
    (property "ki_keywords" "R resistor")
    (attr smd)
    (fp_text reference "R1" (at 0 1.82 90) (layer "B.SilkS"))
    (fp_text value "19.1K" (at 0 -1.82 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1.55 0 270) (size 1.3 1.75) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.1923076923)
      (net 10 "Net-(R1-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 270) (size 1.3 1.75) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.1923076923)
      (net 4 "Vbatt_12") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "B.Cu")
    (at 139.7 67.03 90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "down_converter.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, small symbol")
    (property "ki_keywords" "R resistor")
    (attr smd)
    (fp_text reference "R4" (at 0 1.82 90) (layer "B.SilkS"))
    (fp_text value "2.2K" (at 0 -1.82 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1.55 0 90) (size 1.3 1.75) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.1923076923)
      (net 11 "Net-(R3-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 90) (size 1.3 1.75) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.1923076923)
      (net 3 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_SMC_Handsoldering" (layer "B.Cu")
    (at 116.84 62.23 180)
    (descr "Diode SMC (DO-214AB) Handsoldering")
    (tags "Diode SMC (DO-214AB) Handsoldering")
    (property "Sheetfile" "down_converter.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Schottky diode")
    (property "ki_keywords" "diode Schottky")
    (attr smd)
    (fp_text reference "D3" (at 8.255 -2.54) (layer "B.SilkS"))
    (fp_text value "MBRS340" (at 0 -4.2) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 1.5) (layer "B.Fab"))
    (pad "1" smd roundrect (at -4.4 0 90) (size 3.3 4.5) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.07575757576)
      (net 2 "Net-(D2-K)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 4.4 0 90) (size 3.3 4.5) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.07575757576)
      (net 7 "+BATT") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SMC.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder" (layer "B.Cu")
    (at 128.27 62.23 -90)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "down_converter.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C5" (at -3.81 0 90) (layer "B.SilkS"))
    (fp_text value "1uF" (at 0 -1.85 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1.5625 0 270) (size 1.325 1.8) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.1886792453)
      (net 3 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0 270) (size 1.325 1.8) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.1886792453)
      (net 2 "Net-(D2-K)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "B.Cu")
    (at 131.8 77.47 180)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "down_converter.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, small symbol")
    (property "ki_keywords" "R resistor")
    (attr smd)
    (fp_text reference "R2" (at 0 1.82) (layer "B.SilkS"))
    (fp_text value "10K" (at 0 -1.82) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1.55 0 180) (size 1.3 1.75) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.1923076923)
      (net 5 "Net-(D1-K)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 180) (size 1.3 1.75) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.1923076923)
      (net 10 "Net-(R1-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "B.Cu")
    (at 131.8 72.39)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "down_converter.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, small symbol")
    (property "ki_keywords" "R resistor")
    (attr smd)
    (fp_text reference "R3" (at 0 1.82) (layer "B.SilkS"))
    (fp_text value "0" (at 0 -1.82) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1.55 0) (size 1.3 1.75) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.1923076923)
      (net 10 "Net-(R1-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0) (size 1.3 1.75) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.1923076923)
      (net 11 "Net-(R3-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_SMF" (layer "B.Cu")
    (at 139.7 59.69 90)
    (descr "Diode SMF (DO-219AB), http://www.vishay.com/docs/95572/smf_do-219ab.pdf")
    (tags "Diode SMF (DO-214AB)")
    (property "Sheetfile" "down_converter.kicad_sch")
    (property "Sheetname" "")
    (property "Sim.Device" "D")
    (property "Sim.Pins" "1=K 2=A")
    (property "ki_description" "Diode")
    (property "ki_keywords" "diode")
    (attr smd)
    (fp_text reference "D4" (at 0 -1.905 90) (layer "B.SilkS"))
    (fp_text value "S1FLM-GS08" (at 0 -2 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1.45 0 90) (size 1.3 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.1923076923)
      (net 5 "Net-(D1-K)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 1.45 0 90) (size 1.3 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.1923076923)
      (net 8 "Vbatt_low") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SMF.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_SMF" (layer "B.Cu")
    (at 142.24 59.69 90)
    (descr "Diode SMF (DO-219AB), http://www.vishay.com/docs/95572/smf_do-219ab.pdf")
    (tags "Diode SMF (DO-214AB)")
    (property "Sheetfile" "down_converter.kicad_sch")
    (property "Sheetname" "")
    (property "Sim.Device" "D")
    (property "Sim.Pins" "1=K 2=A")
    (property "ki_description" "Diode")
    (property "ki_keywords" "diode")
    (attr smd)
    (fp_text reference "D1" (at 0 2 90) (layer "B.SilkS"))
    (fp_text value "S1FLM-GS08" (at 0 -2 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1.45 0 90) (size 1.3 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.1923076923)
      (net 5 "Net-(D1-K)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 1.45 0 90) (size 1.3 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.1923076923)
      (net 6 "+12V") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SMF.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_SMC_Handsoldering" (layer "B.Cu")
    (at 116.84 54.61 180)
    (descr "Diode SMC (DO-214AB) Handsoldering")
    (tags "Diode SMC (DO-214AB) Handsoldering")
    (property "Sheetfile" "down_converter.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Schottky diode")
    (property "ki_keywords" "diode Schottky")
    (attr smd)
    (fp_text reference "D2" (at -8.255 1.905) (layer "B.SilkS"))
    (fp_text value "MBRS340" (at 0 -4.2) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 1.5) (layer "B.Fab"))
    (pad "1" smd roundrect (at -4.4 0 90) (size 3.3 4.5) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.07575757576)
      (net 2 "Net-(D2-K)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 4.4 0 90) (size 3.3 4.5) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.07575757576)
      (net 7 "+BATT") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SMC.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder" (layer "B.Cu")
    (at 127 68.58 180)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "down_converter.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C1" (at 0 1.85) (layer "B.SilkS"))
    (fp_text value "1uF" (at 0 -1.85) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1.5625 0 180) (size 1.325 1.8) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.1886792453)
      (net 1 "Net-(U1-VC)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0 180) (size 1.325 1.8) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.1886792453)
      (net 2 "Net-(D2-K)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_circle (center 146.05 72) (end 147.56 72)
    (fill none) (layer "Edge.Cuts"))
  (gr_circle (center 113.5 77) (end 115.01 77)
    (fill none) (layer "Edge.Cuts"))
  (gr_circle (center 130 53) (end 131.51 53)
    (fill none) (layer "Edge.Cuts"))
  (gr_rect locked (start 100 50) (end 150 90)
    (fill none) (layer "Edge.Cuts"))
  (gr_text "12V converter v1 - 08/2023" (at 147.955 79.375 -90) (layer "B.SilkS"))
  (gr_text "12V converter v1 - 08/2023" (at 149.225 79.375 90) (layer "F.SilkS"))
  (gr_text "+12V" (at 142.24 54.61) (layer "F.SilkS"))
  (gr_text "BATT" (at 102.5 59.5 90) (layer "F.SilkS"))
  (gr_text "OUT" (at 102.5 86 90) (layer "F.SilkS"))
  (gr_text "Low Batt" (at 133.985 55.245) (layer "F.SilkS"))
  (zone (net 4) (net_name "Vbatt_12") (layer "F.Cu") (hatch edge 0.5)
    (priority 2)
    (connect_pads yes (clearance 0.5))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 106.68 83.82)
        (xy 106.68 89.535)
        (xy 143.51 89.535)
        (xy 143.51 85.09)
        (xy 107.95 85.09)
        (xy 107.95 83.82)
      )
    )
  )
  (zone (net 9) (net_name "Net-(D5-K)") (layer "F.Cu") (hatch edge 0.5)
    (priority 3)
    (connect_pads yes (clearance 0.5))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 119.38 71.12)
        (xy 119.38 77.47)
        (xy 143.51 77.47)
        (xy 143.51 68.58)
        (xy 137.16 68.58)
        (xy 137.16 71.12)
      )
    )
  )
  (zone (net 3) (net_name "GND") (layer "F.Cu") (hatch edge 0.5)
    (priority 1)
    (connect_pads (clearance 0.5))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 100.33 50.165)
        (xy 149.86 50.165)
        (xy 149.86 89.535)
        (xy 100.33 89.535)
      )
    )
  )
  (zone (net 0) (net_name "") (layers "F&B.Cu") (hatch edge 0.5)
    (connect_pads (clearance 0))
    (min_thickness 0.25) (filled_areas_thickness no)
    (keepout (tracks not_allowed) (vias not_allowed) (pads not_allowed) (copperpour not_allowed) (footprints allowed))
    (fill (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 144.018 69.85)
        (xy 144.018 73.914)
        (xy 147.955 73.914)
        (xy 147.955 69.85)
      )
    )
  )
  (zone (net 0) (net_name "") (layers "F&B.Cu") (hatch edge 0.5)
    (connect_pads (clearance 0))
    (min_thickness 0.25) (filled_areas_thickness no)
    (keepout (tracks not_allowed) (vias not_allowed) (pads not_allowed) (copperpour not_allowed) (footprints allowed))
    (fill (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 111.506 74.93)
        (xy 111.506 78.994)
        (xy 115.443 78.994)
        (xy 115.443 74.93)
      )
    )
  )
  (zone (net 0) (net_name "") (layers "F&B.Cu") (hatch edge 0.5)
    (connect_pads (clearance 0))
    (min_thickness 0.25) (filled_areas_thickness no)
    (keepout (tracks not_allowed) (vias not_allowed) (pads not_allowed) (copperpour not_allowed) (footprints allowed))
    (fill (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 128.016 50.927)
        (xy 128.016 54.991)
        (xy 131.953 54.991)
        (xy 131.953 50.927)
      )
    )
  )
  (zone (net 7) (net_name "+BATT") (layer "B.Cu") (hatch edge 0.5)
    (priority 5)
    (connect_pads (clearance 0.5))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 106.045 56.515)
        (xy 110.49 56.515)
        (xy 110.49 64.135)
        (xy 114.935 64.135)
        (xy 114.935 52.705)
        (xy 106.045 52.705)
      )
    )
  )
  (zone (net 3) (net_name "GND") (layer "B.Cu") (hatch edge 0.5)
    (priority 1)
    (connect_pads (clearance 0.5))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 100.33 50.165)
        (xy 149.86 50.165)
        (xy 149.86 90.17)
        (xy 100.33 90.17)
      )
    )
  )
  (zone (net 2) (net_name "Net-(D2-K)") (layer "B.Cu") (hatch edge 0.5)
    (priority 4)
    (connect_pads yes (clearance 0.5))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 118.745 52.705)
        (xy 118.745 65.405)
        (xy 126.365 65.405)
        (xy 126.365 64.135)
        (xy 123.825 64.135)
        (xy 123.825 52.705)
      )
    )
  )
)
