(kicad_pcb
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(title_block
		(title "FERROFLUID VU-METER")
		(date "2023-09-13")
		(rev "2")
	)
	(layers
		(0 "F.Cu" signal)
		(1 "In1.Cu" signal)
		(2 "In2.Cu" signal)
		(31 "B.Cu" signal)
		(32 "B.Adhes" user "B.Adhesive")
		(33 "F.Adhes" user "F.Adhesive")
		(34 "B.Paste" user)
		(35 "F.Paste" user)
		(36 "B.SilkS" user "B.Silkscreen")
		(37 "F.SilkS" user "F.Silkscreen")
		(38 "B.Mask" user)
		(39 "F.Mask" user)
		(40 "Dwgs.User" user "User.Drawings")
		(41 "Cmts.User" user "User.Comments")
		(42 "Eco1.User" user "User.Eco1")
		(43 "Eco2.User" user "User.Eco2")
		(44 "Edge.Cuts" user)
		(45 "Margin" user)
		(46 "B.CrtYd" user "B.Courtyard")
		(47 "F.CrtYd" user "F.Courtyard")
		(48 "B.Fab" user)
		(49 "F.Fab" user)
		(50 "User.1" user)
		(51 "User.2" user)
		(52 "User.3" user)
		(53 "User.4" user)
		(54 "User.5" user)
		(55 "User.6" user)
		(56 "User.7" user)
		(57 "User.8" user)
		(58 "User.9" user)
	)
	(setup
		(stackup
			(layer "F.SilkS"
				(type "Top Silk Screen")
			)
			(layer "F.Paste"
				(type "Top Solder Paste")
			)
			(layer "F.Mask"
				(type "Top Solder Mask")
				(thickness 0.01)
			)
			(layer "F.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 1"
				(type "prepreg")
				(thickness 0.1)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "In1.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 2"
				(type "core")
				(thickness 1.24)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "In2.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 3"
				(type "prepreg")
				(thickness 0.1)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "B.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "B.Mask"
				(type "Bottom Solder Mask")
				(thickness 0.01)
			)
			(layer "B.Paste"
				(type "Bottom Solder Paste")
			)
			(layer "B.SilkS"
				(type "Bottom Silk Screen")
			)
			(copper_finish "None")
			(dielectric_constraints no)
		)
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(pcbplotparams
			(layerselection 0x00010fc_ffffffff)
			(plot_on_all_layers_selection 0x0000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(viasonmask no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plotreference yes)
			(plotvalue yes)
			(plotfptext yes)
			(plotinvisibletext no)
			(sketchpadsonfab no)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 1)
			(scaleselection 1)
			(outputdirectory "")
		)
	)
	(net 0 "")
	(net 1 "GND")
	(net 2 "/BANDPASS")
	(net 3 "/HIGHPASS")
	(net 4 "/M_LINE")
	(net 5 "/R_LINE")
	(net 6 "/L_LINE")
	(net 7 "/SPK")
	(net 8 "/EQL")
	(net 9 "/LOWPASS")
	(net 10 "/PWR_SPK")
	(net 11 "/PWR_EM")
	(net 12 "+12V")
	(net 13 "-12V")
	(net 14 "Net-(U4A--)")
	(net 15 "Net-(U3A--)")
	(net 16 "Net-(J6-Pad4)")
	(net 17 "Net-(J4-Pin_1)")
	(net 18 "Net-(J4-Pin_2)")
	(net 19 "Net-(U5A--)")
	(net 20 "Net-(U2A-+)")
	(net 21 "Net-(Q3-B)")
	(net 22 "Net-(U2B--)")
	(net 23 "Net-(R22-Pad2)")
	(net 24 "Net-(U4B--)")
	(net 25 "Net-(J6-Pad2)")
	(net 26 "Net-(Q1-E)")
	(net 27 "Net-(Q1-C)")
	(net 28 "Net-(Q1-B)")
	(net 29 "Net-(J5-Pin_2)")
	(net 30 "Net-(D3-K)")
	(net 31 "Net-(D3-A)")
	(net 32 "Net-(D1-K)")
	(net 33 "Net-(D1-A)")
	(net 34 "/+12V_EM")
	(net 35 "/GND_SPK")
	(net 36 "/GND_EM")
	(net 37 "/+12V_SPK")
	(net 38 "/-12V_SPK")
	(net 39 "Net-(J2001-Pin_1)")
	(net 40 "Net-(PS1001-+VIN)")
	(net 41 "Net-(J1002-Pin_1)")
	(net 42 "Net-(PS1001-+VOUT)")
	(net 43 "Net-(J1002-Pin_2)")
	(net 44 "Net-(PS1001--VOUT)")
	(net 45 "Net-(J1002-Pin_3)")
	(net 46 "Net-(J2001-Pin_3)")
	(net 47 "Net-(J2001-Pin_2)")
	(net 48 "Net-(R1-Pad1)")
	(net 49 "Net-(J9-Pad4)")
	(net 50 "unconnected-(J10-Pin_4-Pad4)")
	(net 51 "/PWR_SPK2")
	(footprint "Diode_THT:D_DO-35_SOD27_P7.62mm_Horizontal"
		(layer "F.Cu")
		(at 210.82 43.18 -90)
		(descr "Diode, DO-35_SOD27 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
		(tags "Diode DO-35_SOD27 series Axial Horizontal pin pitch 7.62mm  length 4mm diameter 2mm")
		(property "Reference" "D4"
			(at 3.81 2.286 -90)
			(layer "F.SilkS")
		)
		(property "Value" "5.1V"
			(at 3.81 0 -90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Zener diode"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "project.kicad_sch")
		(attr through_hole)
		(fp_text user "K"
			(at 0 -1.8 -90)
			(layer "F.SilkS")
		)
		(fp_text user "${REFERENCE}"
			(at 3.81 2.286 -90)
			(layer "F.Fab")
		)
		(fp_text user "K"
			(at 0 -1.8 -90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 30 "Net-(D3-K)")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 7.62 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "A")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-35_SOD27_P7.62mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal"
		(layer "F.Cu")
		(at 91.44 71.12 90)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R11"
			(at 3.81 -2.54 90)
			(layer "F.SilkS")
		)
		(property "Value" "100k"
			(at 3.81 0 90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "project.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 3.81 -2.54 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 29 "Net-(J5-Pin_2)")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 7.62 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "/BANDPASS")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_Molex:Molex_KK-254_AE-6410-03A_1x03_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 121.92 43.18 90)
		(descr "Molex KK-254 Interconnect System, old/engineering part number: AE-6410-03A example for new part number: 22-27-2031, 3 Pins (http://www.molex.com/pdm_docs/sd/022272021_sd.pdf), generated with kicad-footprint-generator")
		(tags "connector Molex KK-254 vertical")
		(property "Reference" "J2001"
			(at 2.54 -4.12 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "INPUT"
			(at 2.54 4.08 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x03, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "project.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.54 -2.22 90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole roundrect
			(at 0 0 90)
			(size 1.74 2.19)
			(drill 1.19)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.143678)
			(net 39 "Net-(J2001-Pin_1)")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 2.54 0 90)
			(size 1.74 2.19)
			(drill 1.19)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 47 "Net-(J2001-Pin_2)")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 5.08 0 90)
			(size 1.74 2.19)
			(drill 1.19)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 46 "Net-(J2001-Pin_3)")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Connector_Molex.3dshapes/Molex_KK-254_AE-6410-03A_1x03_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal"
		(layer "F.Cu")
		(at 83.82 53.34 -90)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R19"
			(at 3.81 2.54 90)
			(layer "F.SilkS")
		)
		(property "Value" "100R"
			(at 3.81 0 90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "project.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 3.81 2.54 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "+12V")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 7.62 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 27 "Net-(Q1-C)")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_THT:C_Axial_L5.1mm_D3.1mm_P7.50mm_Horizontal"
		(layer "F.Cu")
		(at 104.14 91.44 90)
		(descr "C, Axial series, Axial, Horizontal, pin pitch=7.5mm, , length*diameter=5.1*3.1mm^2, http://www.vishay.com/docs/45231/arseries.pdf")
		(tags "C Axial series Axial Horizontal pin pitch 7.5mm  length 5.1mm diameter 3.1mm")
		(property "Reference" "C4"
			(at 3.75 -2.54 90)
			(layer "F.SilkS")
		)
		(property "Value" "0.22uF"
			(at 3.75 0 90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "project.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 3.75 -2.54 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "Net-(U3A--)")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 7.5 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "/HIGHPASS")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Axial_L5.1mm_D3.1mm_P7.50mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MountingHole:MountingHole_4.3mm_M4"
		(layer "F.Cu")
		(at 223.52 88.9 90)
		(descr "Mounting Hole 4.3mm, no annular, M4")
		(tags "mounting hole 4.3mm no annular m4")
		(property "Reference" "H2"
			(at 0 -5.3 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MountingHole_Pad"
			(at 0 5.3 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mounting Hole without connection"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "project.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at 0 0 90)
			(size 4.3 4.3)
			(drill 4.3)
			(layers "*.Cu" "*.Mask")
		)
	)
	(footprint "TestPoint:TestPoint_THTPad_D2.0mm_Drill1.0mm"
		(layer "F.Cu")
		(at 181.61 86.36 90)
		(descr "THT pad as test Point, diameter 2.0mm, hole diameter 1.0mm")
		(tags "test point THT pad")
		(property "Reference" "TP1"
			(at 0 -1.998 90)
			(layer "F.SilkS")
		)
		(property "Value" "TestPoint"
			(at 0 2.05 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "project.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 -2 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "+12V")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "Package_TO_SOT_THT:TO-220-3_Horizontal_TabDown"
		(layer "F.Cu")
		(at 198.12 58.42)
		(descr "TO-220-3, Horizontal, RM 2.54mm, see https://www.vishay.com/docs/66542/to-220-1.pdf")
		(tags "TO-220-3 Horizontal RM 2.54mm")
		(property "Reference" "Q4"
			(at -2.54 -1.27 90)
			(layer "F.SilkS")
		)
		(property "Value" "TIP32BG"
			(at 2.54 -8.255 90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "-6A Ic, -60V Vce, Power PNP Transistor, TO-220"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "project.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at -2.54 -1.27 90)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole oval
			(at 2.54 -16.66)
			(size 3.5 3.5)
			(drill 3.5)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.905 2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 21 "Net-(Q3-B)")
			(pinfunction "B")
			(pintype "input")
		)
		(pad "2" thru_hole oval
			(at 2.54 0)
			(size 1.905 2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 38 "/-12V_SPK")
			(pinfunction "C")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 5.08 0)
			(size 1.905 2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "/PWR_SPK")
			(pinfunction "E")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-220-3_Horizontal_TabDown.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_Molex:Molex_KK-254_AE-6410-04A_1x04_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 184.15 73.66)
		(descr "Molex KK-254 Interconnect System, old/engineering part number: AE-6410-04A example for new part number: 22-27-2041, 4 Pins (http://www.molex.com/pdm_docs/sd/022272021_sd.pdf), generated with kicad-footprint-generator")
		(tags "connector Molex KK-254 vertical")
		(property "Reference" "J1"
			(at -2.54 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "POWER INPUT (18-36 VDC)"
			(at 3.81 4.08 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x04, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "project.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at -2.54 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole roundrect
			(at 0 0)
			(size 1.74 2.19)
			(drill 1.19)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.143678)
			(net 12 "+12V")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 2.54 0)
			(size 1.74 2.19)
			(drill 1.19)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 5.08 0)
			(size 1.74 2.19)
			(drill 1.19)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 7.62 0)
			(size 1.74 2.19)
			(drill 1.19)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "-12V")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Connector_Molex.3dshapes/Molex_KK-254_AE-6410-04A_1x04_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_THT:C_Axial_L5.1mm_D3.1mm_P7.50mm_Horizontal"
		(layer "F.Cu")
		(at 88.9 43.3 -90)
		(descr "C, Axial series, Axial, Horizontal, pin pitch=7.5mm, , length*diameter=5.1*3.1mm^2, http://www.vishay.com/docs/45231/arseries.pdf")
		(tags "C Axial series Axial Horizontal pin pitch 7.5mm  length 5.1mm diameter 3.1mm")
		(property "Reference" "C6"
			(at 3.75 2.54 90)
			(layer "F.SilkS")
		)
		(property "Value" "10uF"
			(at 3.75 0 90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "project.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 3.75 2.54 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 7.5 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 28 "Net-(Q1-B)")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Axial_L5.1mm_D3.1mm_P7.50mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Fuse:Fuse_Littelfuse_372_D8.50mm"
		(layer "F.Cu")
		(at 135.89 50.8 -90)
		(descr "Fuse, Littelfuse, 372, 8.5x8mm, https://www.littelfuse.com/~/media/electronics/datasheets/fuses/littelfuse_fuse_372_datasheet.pdf.pdf")
		(tags "fuse tht radial")
		(property "Reference" "F1002"
			(at 2.54 -5 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "4A T"
			(at 2.54 1.27 90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Fuse"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "project.kicad_sch")
		(attr through_hole)
		(fp_text user "${VALUE} (+)"
			(at 2.54 5.08 90)
			(layer "F.SilkS")
		)
		(fp_text user "${REFERENCE}"
			(at 2.54 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 42 "Net-(PS1001-+VOUT)")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 5.08 0 270)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 41 "Net-(J1002-Pin_1)")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Fuse.3dshapes/Fuse_Littelfuse_372_D8.50mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_Molex:Molex_KK-254_AE-6410-02A_1x02_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 101.6 76.2)
		(descr "Molex KK-254 Interconnect System, old/engineering part number: AE-6410-02A example for new part number: 22-27-2021, 2 Pins (http://www.molex.com/pdm_docs/sd/022272021_sd.pdf), generated with kicad-footprint-generator")
		(tags "connector Molex KK-254 vertical")
		(property "Reference" "J4"
			(at -2.54 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x02"
			(at 1.27 4.08 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "project.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at -2.54 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole roundrect
			(at 0 0)
			(size 1.74 2.19)
			(drill 1.19)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.143678)
			(net 17 "Net-(J4-Pin_1)")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 2.54 0)
			(size 1.74 2.19)
			(drill 1.19)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 18 "Net-(J4-Pin_2)")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Connector_Molex.3dshapes/Molex_KK-254_AE-6410-02A_1x02_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_DIP:DIP-8_W7.62mm"
		(layer "F.Cu")
		(at 91.44 91.44 90)
		(descr "8-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
		(tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
		(property "Reference" "U3"
			(at 3.81 -2.54 90)
			(layer "F.SilkS")
		)
		(property "Value" "NE5532"
			(at 3.81 3.81 90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Dual Low-Noise Operational Amplifiers, DIP-8/SOIC-8"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "project.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 3.81 -2.54 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "/HIGHPASS")
			(pintype "output")
		)
		(pad "2" thru_hole oval
			(at 0 2.54 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "Net-(U3A--)")
			(pinfunction "-")
			(pintype "input")
		)
		(pad "3" thru_hole oval
			(at 0 5.08 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "+")
			(pintype "input")
		)
		(pad "4" thru_hole oval
			(at 0 7.62 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "-12V")
			(pinfunction "V-")
			(pintype "power_in")
		)
		(pad "5" thru_hole oval
			(at 7.62 7.62 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 29 "Net-(J5-Pin_2)")
			(pinfunction "+")
			(pintype "input")
		)
		(pad "6" thru_hole oval
			(at 7.62 5.08 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 17 "Net-(J4-Pin_1)")
			(pinfunction "-")
			(pintype "input")
		)
		(pad "7" thru_hole oval
			(at 7.62 2.54 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "/LOWPASS")
			(pintype "output")
		)
		(pad "8" thru_hole oval
			(at 7.62 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "+12V")
			(pinfunction "V+")
			(pintype "power_in")
		)
		(model "${KICAD6_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-8_W7.62mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MountingHole:MountingHole_4.3mm_M4"
		(layer "F.Cu")
		(at 172.72 58.42)
		(descr "Mounting Hole 4.3mm, no annular, M4")
		(tags "mounting hole 4.3mm no annular m4")
		(property "Reference" "H1002"
			(at 0 -5.3 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MountingHole_Pad"
			(at 0 5.3 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mounting Hole without connection"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "project.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 4.3 4.3)
			(drill 4.3)
			(layers "*.Cu" "*.Mask")
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal"
		(layer "F.Cu")
		(at 88.9 53.34 -90)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R20"
			(at 3.81 2.54 90)
			(layer "F.SilkS")
		)
		(property "Value" "100k"
			(at 3.81 0 90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "project.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 3.81 2.54 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 26 "Net-(Q1-E)")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 7.62 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_THTPad_D2.0mm_Drill1.0mm"
		(layer "F.Cu")
		(at 215.9 38.1 90)
		(descr "THT pad as test Point, diameter 2.0mm, hole diameter 1.0mm")
		(tags "test point THT pad")
		(property "Reference" "TP18"
			(at 0 -1.998 90)
			(layer "F.SilkS")
		)
		(property "Value" "TestPoint"
			(at 0 2.05 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "project.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 -2 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 21 "Net-(Q3-B)")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "Connector_Molex:Molex_KK-254_AE-6410-04A_1x04_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 185.42 63.5)
		(descr "Molex KK-254 Interconnect System, old/engineering part number: AE-6410-04A example for new part number: 22-27-2041, 4 Pins (http://www.molex.com/pdm_docs/sd/022272021_sd.pdf), generated with kicad-footprint-generator")
		(tags "connector Molex KK-254 vertical")
		(property "Reference" "J10"
			(at -2.54 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x04"
			(at 3.81 4.08 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x04, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "project.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at -2.54 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole roundrect
			(at 0 0)
			(size 1.74 2.19)
			(drill 1.19)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.143678)
			(net 37 "/+12V_SPK")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 2.54 0)
			(size 1.74 2.19)
			(drill 1.19)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 35 "/GND_SPK")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 5.08 0)
			(size 1.74 2.19)
			(drill 1.19)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 38 "/-12V_SPK")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 7.62 0)
			(size 1.74 2.19)
			(drill 1.19)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 50 "unconnected-(J10-Pin_4-Pad4)")
			(pinfunction "Pin_4")
			(pintype "passive+no_connect")
		)
		(model "${KICAD6_3DMODEL_DIR}/Connector_Molex.3dshapes/Molex_KK-254_AE-6410-04A_1x04_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_Molex:Molex_KK-254_AE-6410-04A_1x04_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 165.1 76.2)
		(descr "Molex KK-254 Interconnect System, old/engineering part number: AE-6410-04A example for new part number: 22-27-2041, 4 Pins (http://www.molex.com/pdm_docs/sd/022272021_sd.pdf), generated with kicad-footprint-generator")
		(tags "connector Molex KK-254 vertical")
		(property "Reference" "J2"
			(at -2.54 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x04"
			(at 3.81 6.62 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x04, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "project.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at -2.54 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole roundrect
			(at 0 0)
			(size 1.74 2.19)
			(drill 1.19)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.143678)
			(net 4 "/M_LINE")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 2.54 0)
			(size 1.74 2.19)
			(drill 1.19)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 5.08 0)
			(size 1.74 2.19)
			(drill 1.19)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "/R_LINE")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 7.62 0)
			(size 1.74 2.19)
			(drill 1.19)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "/L_LINE")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Connector_Molex.3dshapes/Molex_KK-254_AE-6410-04A_1x04_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_Molex:Molex_KK-254_AE-6410-04A_1x04_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 205.74 73.66)
		(descr "Molex KK-254 Interconnect System, old/engineering part number: AE-6410-04A example for new part number: 22-27-2041, 4 Pins (http://www.molex.com/pdm_docs/sd/022272021_sd.pdf), generated with kicad-footprint-generator")
		(tags "connector Molex KK-254 vertical")
		(property "Reference" "J9"
			(at -2.54 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x02"
			(at 3.81 4.08 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "project.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 3.81 -2.22 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole roundrect
			(at 0 0)
			(size 1.74 2.19)
			(drill 1.19)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.143678)
			(net 51 "/PWR_SPK2")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 2.54 0)
			(size 1.74 2.19)
			(drill 1.19)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "/PWR_SPK")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 5.08 0)
			(size 1.74 2.19)
			(drill 1.19)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 19 "Net-(U5A--)")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 7.62 0)
			(size 1.74 2.19)
			(drill 1.19)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 49 "Net-(J9-Pad4)")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Connector_Molex.3dshapes/Molex_KK-254_AE-6410-04A_1x04_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_THTPad_D2.0mm_Drill1.0mm"
		(layer "F.Cu")
		(at 226.06 63.5 90)
		(descr "THT pad as test Point, diameter 2.0mm, hole diameter 1.0mm")
		(tags "test point THT pad")
		(property "Reference" "TP16"
			(at 0 -1.998 90)
			(layer "F.SilkS")
		)
		(property "Value" "TestPoint"
			(at 0 2.05 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "project.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 -2 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 23 "Net-(R22-Pad2)")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "Fuse:Fuse_Littelfuse_372_D8.50mm"
		(layer "F.Cu")
		(at 123.19 50.8 -90)
		(descr "Fuse, Littelfuse, 372, 8.5x8mm, https://www.littelfuse.com/~/media/electronics/datasheets/fuses/littelfuse_fuse_372_datasheet.pdf.pdf")
		(tags "fuse tht radial")
		(property "Reference" "F1003"
			(at 2.54 -5 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "4A T"
			(at 2.54 1.27 90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Fuse"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "project.kicad_sch")
		(attr through_hole)
		(fp_text user "${VALUE} (-)"
			(at 2.54 5.08 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "${REFERENCE}"
			(at 2.54 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 44 "Net-(PS1001--VOUT)")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 5.08 0 270)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 43 "Net-(J1002-Pin_2)")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Fuse.3dshapes/Fuse_Littelfuse_372_D8.50mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_DIP:DIP-8_W7.62mm"
		(layer "F.Cu")
		(at 132.08 81.28 90)
		(descr "8-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
		(tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
		(property "Reference" "U2"
			(at 3.81 -2.54 90)
			(layer "F.SilkS")
		)
		(property "Value" "NE5532"
			(at 3.81 3.81 90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Dual Low-Noise Operational Amplifiers, DIP-8/SOIC-8"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "project.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 3.81 -2.54 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "/SPK")
			(pintype "output")
		)
		(pad "2" thru_hole oval
			(at 0 2.54 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "/SPK")
			(pinfunction "-")
			(pintype "input")
		)
		(pad "3" thru_hole oval
			(at 0 5.08 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 20 "Net-(U2A-+)")
			(pinfunction "+")
			(pintype "input")
		)
		(pad "4" thru_hole oval
			(at 0 7.62 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "-12V")
			(pinfunction "V-")
			(pintype "power_in")
		)
		(pad "5" thru_hole oval
			(at 7.62 7.62 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 20 "Net-(U2A-+)")
			(pinfunction "+")
			(pintype "input")
		)
		(pad "6" thru_hole oval
			(at 7.62 5.08 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 22 "Net-(U2B--)")
			(pinfunction "-")
			(pintype "input")
		)
		(pad "7" thru_hole oval
			(at 7.62 2.54 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "/EQL")
			(pintype "output")
		)
		(pad "8" thru_hole oval
			(at 7.62 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "+12V")
			(pinfunction "V+")
			(pintype "power_in")
		)
		(model "${KICAD6_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-8_W7.62mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_THT:CP_Radial_D6.3mm_P2.50mm"
		(layer "F.Cu")
		(at 191.81 81.28)
		(descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=6.3mm, Electrolytic Capacitor")
		(tags "CP Radial series Radial pin pitch 2.50mm  diameter 6.3mm Electrolytic Capacitor")
		(property "Reference" "C2"
			(at -3.215 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "1µF"
			(at 1.23 1.905 0)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Polarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "project.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at -3.215 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.5 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "-12V")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_D6.3mm_P2.50mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_Molex:Molex_KK-254_AE-6410-04A_1x04_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 73.66 76.2)
		(descr "Molex KK-254 Interconnect System, old/engineering part number: AE-6410-04A example for new part number: 22-27-2041, 4 Pins (http://www.molex.com/pdm_docs/sd/022272021_sd.pdf), generated with kicad-footprint-generator")
		(tags "connector Molex KK-254 vertical")
		(property "Reference" "J6"
			(at -2.54 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x04"
			(at 3.81 4.08 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "project.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at -2.54 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole roundrect
			(at 0 0)
			(size 1.74 2.19)
			(drill 1.19)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.143678)
			(net 14 "Net-(U4A--)")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 2.54 0)
			(size 1.74 2.19)
			(drill 1.19)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "Net-(J6-Pad2)")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 5.08 0)
			(size 1.74 2.19)
			(drill 1.19)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "Net-(U3A--)")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 7.62 0)
			(size 1.74 2.19)
			(drill 1.19)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 16 "Net-(J6-Pad4)")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Connector_Molex.3dshapes/Molex_KK-254_AE-6410-04A_1x04_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_THTPad_D2.0mm_Drill1.0mm"
		(layer "F.Cu")
		(at 132.08 86.36 90)
		(descr "THT pad as test Point, diameter 2.0mm, hole diameter 1.0mm")
		(tags "test point THT pad")
		(property "Reference" "TP8"
			(at 0 -1.998 90)
			(layer "F.SilkS")
		)
		(property "Value" "TestPoint"
			(at 0 2.05 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "project.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 -2 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "/SPK")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "TestPoint:TestPoint_THTPad_D2.0mm_Drill1.0mm"
		(layer "F.Cu")
		(at 91.44 38.1 90)
		(descr "THT pad as test Point, diameter 2.0mm, hole diameter 1.0mm")
		(tags "test point THT pad")
		(property "Reference" "TP15"
			(at 0 -1.998 90)
			(layer "F.SilkS")
		)
		(property "Value" "TestPoint"
			(at 0 2.05 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "project.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 -2 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "/PWR_EM")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal"
		(layer "F.Cu")
		(at 86.36 83.82 -90)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R12"
			(at 3.81 2.54 90)
			(layer "F.SilkS")
		)
		(property "Value" "2.2k"
			(at 3.81 0 90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "project.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 3.81 2.54 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "/LOWPASS")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 7.62 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 16 "Net-(J6-Pad4)")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal"
		(layer "F.Cu")
		(at 109.22 81.28 90)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R8"
			(at 3.81 -2.54 90)
			(layer "F.SilkS")
		)
		(property "Value" "4.7k"
			(at 3.81 0 90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "project.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 3.81 -2.54 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 17 "Net-(J4-Pin_1)")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 7.62 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 18 "Net-(J4-Pin_2)")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_THT:C_Axial_L5.1mm_D3.1mm_P7.50mm_Horizontal"
		(layer "F.Cu")
		(at 73.66 50.68 90)
		(descr "C, Axial series, Axial, Horizontal, pin pitch=7.5mm, , length*diameter=5.1*3.1mm^2, http://www.vishay.com/docs/45231/arseries.pdf")
		(tags "C Axial series Axial Horizontal pin pitch 7.5mm  length 5.1mm diameter 3.1mm")
		(property "Reference" "C5"
			(at 3.75 -2.54 90)
			(layer "F.SilkS")
		)
		(property "Value" "10uF"
			(at 3.75 0 90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "project.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 3.75 -2.54 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 7.5 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 32 "Net-(D1-K)")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Axial_L5.1mm_D3.1mm_P7.50mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_THT:D_DO-35_SOD27_P7.62mm_Horizontal"
		(layer "F.Cu")
		(at 215.9 43.18 -90)
		(descr "Diode, DO-35_SOD27 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
		(tags "Diode DO-35_SOD27 series Axial Horizontal pin pitch 7.62mm  length 4mm diameter 2mm")
		(property "Reference" "D3"
			(at 3.81 2.286 -90)
			(layer "F.SilkS")
		)
		(property "Value" "5.1V"
			(at 3.81 0 -90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Zener diode"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "project.kicad_sch")
		(attr through_hole)
		(fp_text user "K"
			(at 0 -1.8 -90)
			(layer "F.SilkS")
		)
		(fp_text user "${REFERENCE}"
			(at 3.81 2.286 -90)
			(layer "F.Fab")
		)
		(fp_text user "K"
			(at 0 -1.8 -90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 30 "Net-(D3-K)")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 7.62 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 31 "Net-(D3-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-35_SOD27_P7.62mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal"
		(layer "F.Cu")
		(at 205.74 60.96 -90)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R24"
			(at 3.81 2.54 90)
			(layer "F.SilkS")
		)
		(property "Value" "1M"
			(at 3.81 0 90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "project.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 3.81 2.54 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 51 "/PWR_SPK2")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 7.62 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 35 "/GND_SPK")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Symbol:OSHW-Logo2_9.8x8mm_Copper_Mask"
		(layer "F.Cu")
		(at 210.82 86.36)
		(descr "Open Source Hardware Symbol")
		(tags "Logo Symbol OSHW")
		(property "Reference" "SYM2"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Logo_Open_Hardware_Small"
			(at 0.75 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Open Hardware logo, small"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Enable" "0"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "project.kicad_sch")
		(attr exclude_from_pos_files)
	)
	(footprint "Fuse:Fuse_Littelfuse_372_D8.50mm"
		(layer "F.Cu")
		(at 138.43 40.64 180)
		(descr "Fuse, Littelfuse, 372, 8.5x8mm, https://www.littelfuse.com/~/media/electronics/datasheets/fuses/littelfuse_fuse_372_datasheet.pdf.pdf")
		(tags "fuse tht radial")
		(property "Reference" "F1001"
			(at 2.54 -5 180)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "6.3A T"
			(at 7.62 0 -90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Fuse"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "project.kicad_sch")
		(attr through_hole)
		(fp_text user "${VALUE}"
			(at 7.62 0 -90)
			(layer "F.SilkS")
		)
		(fp_text user "${REFERENCE}"
			(at 2.54 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at 0 0 180)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 40 "Net-(PS1001-+VIN)")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 5.08 0 180)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 39 "Net-(J2001-Pin_1)")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Fuse.3dshapes/Fuse_Littelfuse_372_D8.50mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_Molex:Molex_KK-254_AE-6410-03A_1x03_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 121.92 66.04 90)
		(descr "Molex KK-254 Interconnect System, old/engineering part number: AE-6410-03A example for new part number: 22-27-2031, 3 Pins (http://www.molex.com/pdm_docs/sd/022272021_sd.pdf), generated with kicad-footprint-generator")
		(tags "connector Molex KK-254 vertical")
		(property "Reference" "J1003"
			(at 2.54 -4.12 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "OUTPUT"
			(at 2.54 4.08 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x03, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "project.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.54 -2.22 90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole roundrect
			(at 0 0 90)
			(size 1.74 2.19)
			(drill 1.19)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.143678)
			(net 41 "Net-(J1002-Pin_1)")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 2.54 0 90)
			(size 1.74 2.19)
			(drill 1.19)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 43 "Net-(J1002-Pin_2)")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 5.08 0 90)
			(size 1.74 2.19)
			(drill 1.19)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 45 "Net-(J1002-Pin_3)")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Connector_Molex.3dshapes/Molex_KK-254_AE-6410-03A_1x03_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal"
		(layer "F.Cu")
		(at 83.82 43.18 -90)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R17"
			(at 3.81 2.54 90)
			(layer "F.SilkS")
		)
		(property "Value" "1k"
			(at 3.81 0 90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "project.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 3.81 2.54 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 32 "Net-(D1-K)")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 7.62 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 28 "Net-(Q1-B)")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "_custom_footprints:TEN602425N"
		(layer "F.Cu")
		(at 147.32 20.32 -90)
		(descr "TEN 60-2425N-1")
		(tags "Power Supply")
		(property "Reference" "PS1001"
			(at 22.86 -7.76 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "~"
			(at 22.86 -7.76 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "project.kicad_sch")
		(attr through_hole exclude_from_pos_files)
		(pad "1" thru_hole circle
			(at 20.32 0)
			(size 1.8 1.8)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 40 "Net-(PS1001-+VIN)")
			(pinfunction "+VIN")
			(pintype "input")
		)
		(pad "2" thru_hole circle
			(at 20.32 -5.08)
			(size 1.8 1.8)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 47 "Net-(J2001-Pin_2)")
			(pinfunction "-VIN")
			(pintype "input")
		)
		(pad "3" thru_hole circle
			(at 20.32 -15.24)
			(size 1.8 1.8)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 46 "Net-(J2001-Pin_3)")
			(pinfunction "ON/OFF")
			(pintype "input")
		)
		(pad "4" thru_hole circle
			(at 44.45 2.54)
			(size 1.8 1.8)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 42 "Net-(PS1001-+VOUT)")
			(pinfunction "+VOUT")
			(pintype "input")
		)
		(pad "5" thru_hole circle
			(at 44.45 -7.62)
			(size 1.8 1.8)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 45 "Net-(J1002-Pin_3)")
			(pinfunction "COM")
			(pintype "input")
		)
		(pad "6" thru_hole circle
			(at 44.45 -17.78)
			(size 1.8 1.8)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 44 "Net-(PS1001--VOUT)")
			(pinfunction "-VOUT")
			(pintype "input")
		)
		(model "${KIPRJMOD}/TEN_60-2422N.stp"
			(offset
				(xyz 23 8 0.2)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 90 -180 90)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal"
		(layer "F.Cu")
		(at 226.06 76.2 90)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R22"
			(at 3.81 -2.54 90)
			(layer "F.SilkS")
		)
		(property "Value" "47k"
			(at 3.81 0 90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "project.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 3.81 -2.54 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 19 "Net-(U5A--)")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 7.62 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 23 "Net-(R22-Pad2)")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_THT:TO-220-3_Horizontal_TabDown"
		(layer "F.Cu")
		(at 101.6 58.42)
		(descr "TO-220-3, Horizontal, RM 2.54mm, see https://www.vishay.com/docs/66542/to-220-1.pdf")
		(tags "TO-220-3 Horizontal RM 2.54mm")
		(property "Reference" "Q2"
			(at -2.54 -1.27 90)
			(layer "F.SilkS")
		)
		(property "Value" "TIP31CG"
			(at 2.54 -8.255 90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "6A Ic, 60V Vce, Power NPN Transistor, TO-220"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "project.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at -2.54 -1.27 90)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole oval
			(at 2.54 -16.66)
			(size 3.5 3.5)
			(drill 3.5)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.905 2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 26 "Net-(Q1-E)")
			(pinfunction "B")
			(pintype "input")
		)
		(pad "2" thru_hole oval
			(at 2.54 0)
			(size 1.905 2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "/PWR_EM")
			(pinfunction "C")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 5.08 0)
			(size 1.905 2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 36 "/GND_EM")
			(pinfunction "E")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-220-3_Horizontal_TabDown.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MountingHole:MountingHole_4.3mm_M4"
		(layer "F.Cu")
		(at 223.52 40.64 90)
		(descr "Mounting Hole 4.3mm, no annular, M4")
		(tags "mounting hole 4.3mm no annular m4")
		(property "Reference" "H1"
			(at 0 -5.3 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MountingHole_Pad"
			(at 0 5.3 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mounting Hole without connection"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "project.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at 0 0 90)
			(size 4.3 4.3)
			(drill 4.3)
			(layers "*.Cu" "*.Mask")
		)
	)
	(footprint "TestPoint:TestPoint_THTPad_D2.0mm_Drill1.0mm"
		(layer "F.Cu")
		(at 210.82 38.1 90)
		(descr "THT pad as test Point, diameter 2.0mm, hole diameter 1.0mm")
		(tags "test point THT pad")
		(property "Reference" "TP19"
			(at 0 -1.998 90)
			(layer "F.SilkS")
		)
		(property "Value" "TestPoint"
			(at 0 2.05 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "project.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 -2 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "/PWR_SPK")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "Connector_Molex:Molex_KK-254_AE-6410-04A_1x04_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 165.1 83.82)
		(descr "Molex KK-254 Interconnect System, old/engineering part number: AE-6410-04A example for new part number: 22-27-2041, 4 Pins (http://www.molex.com/pdm_docs/sd/022272021_sd.pdf), generated with kicad-footprint-generator")
		(tags "connector Molex KK-254 vertical")
		(property "Reference" "J3"
			(at -2.54 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x04"
			(at 3.81 4.08 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x04, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "project.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at -2.54 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole roundrect
			(at 0 0)
			(size 1.74 2.19)
			(drill 1.19)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.143678)
			(net 4 "/M_LINE")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 2.54 0)
			(size 1.74 2.19)
			(drill 1.19)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 5.08 0)
			(size 1.74 2.19)
			(drill 1.19)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "/R_LINE")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 7.62 0)
			(size 1.74 2.19)
			(drill 1.19)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "/L_LINE")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Connector_Molex.3dshapes/Molex_KK-254_AE-6410-04A_1x04_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_THTPad_D2.0mm_Drill1.0mm"
		(layer "F.Cu")
		(at 81.28 38.1 90)
		(descr "THT pad as test Point, diameter 2.0mm, hole diameter 1.0mm")
		(tags "test point THT pad")
		(property "Reference" "TP13"
			(at 0 -1.998 90)
			(layer "F.SilkS")
		)
		(property "Value" "TestPoint"
			(at 0 2.05 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "project.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 -2 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 32 "Net-(D1-K)")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "MountingHole:MountingHole_4.3mm_M4"
		(layer "F.Cu")
		(at 68.58 88.9 90)
		(descr "Mounting Hole 4.3mm, no annular, M4")
		(tags "mounting hole 4.3mm no annular m4")
		(property "Reference" "H3"
			(at 0 -5.3 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MountingHole_Pad"
			(at 0 5.3 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mounting Hole without connection"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "project.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at 0 0 90)
			(size 4.3 4.3)
			(drill 4.3)
			(layers "*.Cu" "*.Mask")
		)
	)
	(footprint "TestPoint:TestPoint_THTPad_D2.0mm_Drill1.0mm"
		(layer "F.Cu")
		(at 160.02 83.82 90)
		(descr "THT pad as test Point, diameter 2.0mm, hole diameter 1.0mm")
		(tags "test point THT pad")
		(property "Reference" "TP4"
			(at 0 -1.998 90)
			(layer "F.SilkS")
		)
		(property "Value" "TestPoint"
			(at 0 2.05 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "project.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 -2 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "/R_LINE")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "Connector_Molex:Molex_KK-254_AE-6410-03A_1x03_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 137.16 66.04 90)
		(descr "Molex KK-254 Interconnect System, old/engineering part number: AE-6410-03A example for new part number: 22-27-2031, 3 Pins (http://www.molex.com/pdm_docs/sd/022272021_sd.pdf), generated with kicad-footprint-generator")
		(tags "connector Molex KK-254 vertical")
		(property "Reference" "J1002"
			(at 2.54 -4.12 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "OUTPUT"
			(at 2.54 4.08 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x03, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "project.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.54 -2.22 90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole roundrect
			(at 0 0 90)
			(size 1.74 2.19)
			(drill 1.19)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.143678)
			(net 41 "Net-(J1002-Pin_1)")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 2.54 0 90)
			(size 1.74 2.19)
			(drill 1.19)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 43 "Net-(J1002-Pin_2)")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 5.08 0 90)
			(size 1.74 2.19)
			(drill 1.19)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 45 "Net-(J1002-Pin_3)")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Connector_Molex.3dshapes/Molex_KK-254_AE-6410-03A_1x03_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal"
		(layer "F.Cu")
		(at 68.58 48.26 -90)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R16"
			(at 3.81 2.54 90)
			(layer "F.SilkS")
		)
		(property "Value" "100k"
			(at 3.81 0 90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "project.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 3.81 2.54 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 32 "Net-(D1-K)")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 7.62 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal"
		(layer "F.Cu")
		(at 149.86 73.66 -90)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R1"
			(at 3.81 2.54 90)
			(layer "F.SilkS")
		)
		(property "Value" "4.7k"
			(at 3.81 0 90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "project.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 3.81 2.54 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 48 "Net-(R1-Pad1)")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 7.62 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal"
		(layer "F.Cu")
		(at 226.06 58.42 90)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R23"
			(at 3.81 -2.54 90)
			(layer "F.SilkS")
		)
		(property "Value" "1k"
			(at 3.81 0 90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "project.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 3.81 -2.54 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 23 "Net-(R22-Pad2)")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 7.62 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 31 "Net-(D3-A)")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal"
		(layer "F.Cu")
		(at 149.86 91.44 90)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R2"
			(at 3.81 -2.54 90)
			(layer "F.SilkS")
		)
		(property "Value" "1k"
			(at 3.81 0 90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "project.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 3.81 -2.54 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "/R_LINE")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 7.62 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 20 "Net-(U2A-+)")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_Molex:Molex_KK-254_AE-6410-02A_1x02_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 198.12 63.5)
		(descr "Molex KK-254 Interconnect System, old/engineering part number: AE-6410-02A example for new part number: 22-27-2021, 2 Pins (http://www.molex.com/pdm_docs/sd/022272021_sd.pdf), generated with kicad-footprint-generator")
		(tags "connector Molex KK-254 vertical")
		(property "Reference" "J11"
			(at -2.54 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x02"
			(at 1.27 4.08 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "project.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at -2.54 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole roundrect
			(at 0 0)
			(size 1.74 2.19)
			(drill 1.19)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.143678)
			(net 35 "/GND_SPK")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 2.54 0)
			(size 1.74 2.19)
			(drill 1.19)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 51 "/PWR_SPK2")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Connector_Molex.3dshapes/Molex_KK-254_AE-6410-02A_1x02_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MountingHole:MountingHole_4.3mm_M4"
		(layer "F.Cu")
		(at 68.58 40.64 90)
		(descr "Mounting Hole 4.3mm, no annular, M4")
		(tags "mounting hole 4.3mm no annular m4")
		(property "Reference" "H4"
			(at 0 -5.3 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MountingHole_Pad"
			(at 0 5.3 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mounting Hole without connection"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "project.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at 0 0 90)
			(size 4.3 4.3)
			(drill 4.3)
			(layers "*.Cu" "*.Mask")
		)
	)
	(footprint "Capacitor_THT:CP_Radial_D6.3mm_P2.50mm"
		(layer "F.Cu")
		(at 181.65 81.28)
		(descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=6.3mm, Electrolytic Capacitor")
		(tags "CP Radial series Radial pin pitch 2.50mm  diameter 6.3mm Electrolytic Capacitor")
		(property "Reference" "C1"
			(at -3.215 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "1µF"
			(at 1.23 1.905 0)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Polarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "project.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at -3.215 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "+12V")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.5 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_D6.3mm_P2.50mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal"
		(layer "F.Cu")
		(at 68.58 71.12 -90)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R13"
			(at 3.81 2.54 -90)
			(layer "F.SilkS")
		)
		(property "Value" "2.2k"
			(at 3.81 0 -90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "project.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 3.81 2.54 -90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "/BANDPASS")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 7.62 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "Net-(J6-Pad2)")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MountingHole:MountingHole_4.3mm_M4"
		(layer "F.Cu")
		(at 172.72 40.64)
		(descr "Mounting Hole 4.3mm, no annular, M4")
		(tags "mounting hole 4.3mm no annular m4")
		(property "Reference" "H1001"
			(at 0 -5.3 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MountingHole_Pad"
			(at 0 5.3 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mounting Hole without connection"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "project.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 4.3 4.3)
			(drill 4.3)
			(layers "*.Cu" "*.Mask")
		)
	)
	(footprint "TestPoint:TestPoint_THTPad_D2.0mm_Drill1.0mm"
		(layer "F.Cu")
		(at 160.02 91.44 90)
		(descr "THT pad as test Point, diameter 2.0mm, hole diameter 1.0mm")
		(tags "test point THT pad")
		(property "Reference" "TP5"
			(at 0 -1.998 90)
			(layer "F.SilkS")
		)
		(property "Value" "TestPoint"
			(at 0 2.05 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "project.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 -2 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "/L_LINE")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "TestPoint:TestPoint_THTPad_D2.0mm_Drill1.0mm"
		(layer "F.Cu")
		(at 194.31 86.36 90)
		(descr "THT pad as test Point, diameter 2.0mm, hole diameter 1.0mm")
		(tags "test point THT pad")
		(property "Reference" "TP2"
			(at 0 -1.998 90)
			(layer "F.SilkS")
		)
		(property "Value" "TestPoint"
			(at 0 2.05 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "project.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 -2 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "-12V")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal"
		(layer "F.Cu")
		(at 121.92 81.28 90)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R5"
			(at 3.81 -2.54 90)
			(layer "F.SilkS")
		)
		(property "Value" "1k"
			(at 3.81 0 90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "project.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 3.81 -2.54 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 7.62 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 22 "Net-(U2B--)")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_THTPad_D2.0mm_Drill1.0mm"
		(layer "F.Cu")
		(at 81.28 83.82 90)
		(descr "THT pad as test Point, diameter 2.0mm, hole diameter 1.0mm")
		(tags "test point THT pad")
		(property "Reference" "TP9"
			(at 0 -1.998 90)
			(layer "F.SilkS")
		)
		(property "Value" "TestPoint"
			(at 0 2.05 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "project.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 -2 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "/LOWPASS")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "Package_DIP:DIP-8_W7.62mm"
		(layer "F.Cu")
		(at 73.66 71.12 90)
		(descr "8-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
		(tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
		(property "Reference" "U4"
			(at 3.81 -2.54 90)
			(layer "F.SilkS")
		)
		(property "Value" "NE5532"
			(at 3.81 3.81 90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Dual Low-Noise Operational Amplifiers, DIP-8/SOIC-8"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "project.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 3.81 -2.54 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "/BANDPASS")
			(pintype "output")
		)
		(pad "2" thru_hole oval
			(at 0 2.54 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "Net-(U4A--)")
			(pinfunction "-")
			(pintype "input")
		)
		(pad "3" thru_hole oval
			(at 0 5.08 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "+")
			(pintype "input")
		)
		(pad "4" thru_hole oval
			(at 0 7.62 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "-12V")
			(pinfunction "V-")
			(pintype "power_in")
		)
		(pad "5" thru_hole oval
			(at 7.62 7.62 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "/BANDPASS")
			(pinfunction "+")
			(pintype "input")
		)
		(pad "6" thru_hole oval
			(at 7.62 5.08 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 24 "Net-(U4B--)")
			(pinfunction "-")
			(pintype "input")
		)
		(pad "7" thru_hole oval
			(at 7.62 2.54 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 33 "Net-(D1-A)")
			(pintype "output")
		)
		(pad "8" thru_hole oval
			(at 7.62 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "+12V")
			(pinfunction "V+")
			(pintype "power_in")
		)
		(model "${KICAD6_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-8_W7.62mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_THTPad_D2.0mm_Drill1.0mm"
		(layer "F.Cu")
		(at 138.43 86.36 90)
		(descr "THT pad as test Point, diameter 2.0mm, hole diameter 1.0mm")
		(tags "test point THT pad")
		(property "Reference" "TP6"
			(at 0 -1.998 90)
			(layer "F.SilkS")
		)
		(property "Value" "TestPoint"
			(at 2.54 2.05 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "project.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 -2 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 20 "Net-(U2A-+)")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "Connector_Molex:Molex_KK-254_AE-6410-02A_1x02_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 99.06 63.5)
		(descr "Molex KK-254 Interconnect System, old/engineering part number: AE-6410-02A example for new part number: 22-27-2021, 2 Pins (http://www.molex.com/pdm_docs/sd/022272021_sd.pdf), generated with kicad-footprint-generator")
		(tags "connector Molex KK-254 vertical")
		(property "Reference" "J8"
			(at -2.54 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x02"
			(at 3.81 4.08 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "project.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at -2.54 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole roundrect
			(at 0 0)
			(size 1.74 2.19)
			(drill 1.19)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.143678)
			(net 11 "/PWR_EM")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 2.54 0)
			(size 1.74 2.19)
			(drill 1.19)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 34 "/+12V_EM")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Connector_Molex.3dshapes/Molex_KK-254_AE-6410-02A_1x02_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal"
		(layer "F.Cu")
		(at 114.3 83.82 -90)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R9"
			(at 3.81 2.54 90)
			(layer "F.SilkS")
		)
		(property "Value" "470R"
			(at 3.81 0 90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "project.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 3.81 2.54 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 17 "Net-(J4-Pin_1)")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 7.62 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "/HIGHPASS")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_DIP:DIP-8_W7.62mm"
		(layer "F.Cu")
		(at 213.36 63.5 90)
		(descr "8-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
		(tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
		(property "Reference" "U5"
			(at 3.81 -2.54 90)
			(layer "F.SilkS")
		)
		(property "Value" "NE5532"
			(at 3.81 3.81 90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Dual Low-Noise Operational Amplifiers, DIP-8/SOIC-8"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "project.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 3.81 -2.54 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 23 "Net-(R22-Pad2)")
			(pintype "output")
		)
		(pad "2" thru_hole oval
			(at 0 2.54 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 19 "Net-(U5A--)")
			(pinfunction "-")
			(pintype "input")
		)
		(pad "3" thru_hole oval
			(at 0 5.08 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "+")
			(pintype "input")
		)
		(pad "4" thru_hole oval
			(at 0 7.62 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "-12V")
			(pinfunction "V-")
			(pintype "power_in")
		)
		(pad "5" thru_hole oval
			(at 7.62 7.62 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 31 "Net-(D3-A)")
			(pinfunction "+")
			(pintype "input")
		)
		(pad "6" thru_hole oval
			(at 7.62 5.08 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "/PWR_SPK")
			(pinfunction "-")
			(pintype "input")
		)
		(pad "7" thru_hole oval
			(at 7.62 2.54 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 21 "Net-(Q3-B)")
			(pintype "output")
		)
		(pad "8" thru_hole oval
			(at 7.62 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "+12V")
			(pinfunction "V+")
			(pintype "power_in")
		)
		(model "${KICAD6_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-8_W7.62mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_THTPad_D2.0mm_Drill1.0mm"
		(layer "F.Cu")
		(at 68.58 66.04 90)
		(descr "THT pad as test Point, diameter 2.0mm, hole diameter 1.0mm")
		(tags "test point THT pad")
		(property "Reference" "TP10"
			(at 0 -1.998 90)
			(layer "F.SilkS")
		)
		(property "Value" "TestPoint"
			(at 0 2.05 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "project.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 -2 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "/BANDPASS")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal"
		(layer "F.Cu")
		(at 144.78 83.82 -90)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R4"
			(at 3.81 2.54 90)
			(layer "F.SilkS")
		)
		(property "Value" "1M"
			(at 3.81 0 90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "project.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 3.81 2.54 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 20 "Net-(U2A-+)")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 7.62 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal"
		(layer "F.Cu")
		(at 109.22 91.44 90)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R10"
			(at 3.81 -2.54 90)
			(layer "F.SilkS")
		)
		(property "Value" "2.2k"
			(at 3.81 0 90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "project.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 3.81 -2.54 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 17 "Net-(J4-Pin_1)")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 7.62 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "/LOWPASS")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_THT:TO-92_Inline_Wide"
		(layer "F.Cu")
		(at 93.98 53.34 -90)
		(descr "TO-92 leads in-line, wide, drill 0.75mm (see NXP sot054_po.pdf)")
		(tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
		(property "Reference" "Q1"
			(at 2.54 2.54 90)
			(layer "F.SilkS")
		)
		(property "Value" "PN2222A"
			(at 2.54 -2.48 90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "1A Ic, 40V Vce, NPN Transistor, General Purpose Transistor, TO-92"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "project.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.54 2.54 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 270)
			(size 1.5 1.5)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 26 "Net-(Q1-E)")
			(pinfunction "E")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.54 0 270)
			(size 1.5 1.5)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 28 "Net-(Q1-B)")
			(pinfunction "B")
			(pintype "input")
		)
		(pad "3" thru_hole circle
			(at 5.08 0 270)
			(size 1.5 1.5)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 27 "Net-(Q1-C)")
			(pinfunction "C")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-92_Inline_Wide.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_THT:TO-220-3_Horizontal_TabDown"
		(layer "F.Cu")
		(at 185.42 58.42)
		(descr "TO-220-3, Horizontal, RM 2.54mm, see https://www.vishay.com/docs/66542/to-220-1.pdf")
		(tags "TO-220-3 Horizontal RM 2.54mm")
		(property "Reference" "Q3"
			(at -2.54 -1.27 90)
			(layer "F.SilkS")
		)
		(property "Value" "TIP31CG"
			(at 2.54 -8.255 90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "6A Ic, 60V Vce, Power NPN Transistor, TO-220"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "project.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at -2.54 -1.27 90)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole oval
			(at 2.54 -16.66)
			(size 3.5 3.5)
			(drill 3.5)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.905 2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 21 "Net-(Q3-B)")
			(pinfunction "B")
			(pintype "input")
		)
		(pad "2" thru_hole oval
			(at 2.54 0)
			(size 1.905 2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 37 "/+12V_SPK")
			(pinfunction "C")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 5.08 0)
			(size 1.905 2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "/PWR_SPK")
			(pinfunction "E")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-220-3_Horizontal_TabDown.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal"
		(layer "F.Cu")
		(at 73.66 60.96 90)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R15"
			(at 3.81 -2.54 90)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 3.81 0 90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "project.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 3.81 -2.54 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 24 "Net-(U4B--)")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 7.62 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 33 "Net-(D1-A)")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_THTPad_D2.0mm_Drill1.0mm"
		(layer "F.Cu")
		(at 68.58 60.96 90)
		(descr "THT pad as test Point, diameter 2.0mm, hole diameter 1.0mm")
		(tags "test point THT pad")
		(property "Reference" "TP12"
			(at 0 -1.998 90)
			(layer "F.SilkS")
		)
		(property "Value" "TestPoint"
			(at 0 2.05 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "project.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 -2 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 33 "Net-(D1-A)")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "TestPoint:TestPoint_THTPad_D2.0mm_Drill1.0mm"
		(layer "F.Cu")
		(at 220.98 50.8 90)
		(descr "THT pad as test Point, diameter 2.0mm, hole diameter 1.0mm")
		(tags "test point THT pad")
		(property "Reference" "TP17"
			(at 0 -1.998 90)
			(layer "F.SilkS")
		)
		(property "Value" "TestPoint"
			(at 0 2.05 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "project.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 -2 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 31 "Net-(D3-A)")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal"
		(layer "F.Cu")
		(at 114.3 81.28 90)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R7"
			(at 3.81 -2.54 90)
			(layer "F.SilkS")
		)
		(property "Value" "470R"
			(at 3.81 0 90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "project.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 3.81 -2.54 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "/EQL")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 7.62 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 18 "Net-(J4-Pin_2)")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_THT:C_Axial_L5.1mm_D3.1mm_P7.50mm_Horizontal"
		(layer "F.Cu")
		(at 86.36 71.12 90)
		(descr "C, Axial series, Axial, Horizontal, pin pitch=7.5mm, , length*diameter=5.1*3.1mm^2, http://www.vishay.com/docs/45231/arseries.pdf")
		(tags "C Axial series Axial Horizontal pin pitch 7.5mm  length 5.1mm diameter 3.1mm")
		(property "Reference" "C3"
			(at 3.75 -2.54 90)
			(layer "F.SilkS")
		)
		(property "Value" "0.22uF"
			(at 3.81 0 90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "project.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 3.81 -2.54 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "Net-(U4A--)")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 7.5 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "/BANDPASS")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Axial_L5.1mm_D3.1mm_P7.50mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal"
		(layer "F.Cu")
		(at 127 73.66 -90)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R6"
			(at 3.81 2.54 90)
			(layer "F.SilkS")
		)
		(property "Value" "1k"
			(at 3.81 0 90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "project.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 3.81 2.54 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 22 "Net-(U2B--)")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 7.62 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "/EQL")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal"
		(layer "F.Cu")
		(at 220.98 76.2 90)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R21"
			(at 3.81 -2.54 90)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 3.81 0 90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "project.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 3.81 -2.54 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "/SPK")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 7.62 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 49 "Net-(J9-Pad4)")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_THT:D_DO-41_SOD81_P7.62mm_Horizontal"
		(layer "F.Cu")
		(at 106.68 69.85 180)
		(descr "Diode, DO-41_SOD81 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=5.2*2.7mm^2, , http://www.diodes.com/_files/packages/DO-41%20(Plastic).pdf")
		(tags "Diode DO-41_SOD81 series Axial Horizontal pin pitch 7.62mm  length 5.2mm diameter 2.7mm")
		(property "Reference" "D2"
			(at 10.16 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "1N4007"
			(at 3.81 0 0)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Diode"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" "D"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "project.kicad_sch")
		(attr through_hole)
		(fp_text user "K"
			(at 0 -2.1 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(fp_text user "${REFERENCE}"
			(at 10.16 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 180)
			(size 2.2 2.2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 34 "/+12V_EM")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 7.62 0 180)
			(size 2.2 2.2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "/PWR_EM")
			(pinfunction "A")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-41_SOD81_P7.62mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal"
		(layer "F.Cu")
		(at 154.94 91.44 90)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R3"
			(at 3.81 -2.54 90)
			(layer "F.SilkS")
		)
		(property "Value" "1k"
			(at 3.81 0 90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "project.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 3.81 -2.54 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "/L_LINE")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 7.62 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 20 "Net-(U2A-+)")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_THTPad_D2.0mm_Drill1.0mm"
		(layer "F.Cu")
		(at 125.73 86.36 90)
		(descr "THT pad as test Point, diameter 2.0mm, hole diameter 1.0mm")
		(tags "test point THT pad")
		(property "Reference" "TP7"
			(at 0 -1.998 90)
			(layer "F.SilkS")
		)
		(property "Value" "TestPoint"
			(at 0 2.05 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "project.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 -2 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "/EQL")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "TestPoint:TestPoint_THTPad_D2.0mm_Drill1.0mm"
		(layer "F.Cu")
		(at 81.28 88.9 90)
		(descr "THT pad as test Point, diameter 2.0mm, hole diameter 1.0mm")
		(tags "test point THT pad")
		(property "Reference" "TP11"
			(at 0 -1.998 90)
			(layer "F.SilkS")
		)
		(property "Value" "TestPoint"
			(at 2.54 2.05 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "project.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 -2 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "/HIGHPASS")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal"
		(layer "F.Cu")
		(at 93.98 50.8 90)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R18"
			(at 3.81 -2.54 90)
			(layer "F.SilkS")
		)
		(property "Value" "4.7k"
			(at 3.81 0 90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "project.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 3.81 -2.54 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 28 "Net-(Q1-B)")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 7.62 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "-12V")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_THT:D_DO-35_SOD27_P7.62mm_Horizontal"
		(layer "F.Cu")
		(at 78.74 43.18 -90)
		(descr "Diode, DO-35_SOD27 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
		(tags "Diode DO-35_SOD27 series Axial Horizontal pin pitch 7.62mm  length 4mm diameter 2mm")
		(property "Reference" "D1"
			(at 3.81 2.286 -90)
			(layer "F.SilkS")
		)
		(property "Value" "1N4148"
			(at 3.81 0 -90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Diode"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" "D"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "project.kicad_sch")
		(attr through_hole)
		(fp_text user "K"
			(at 0 -1.8 -90)
			(layer "F.SilkS")
		)
		(fp_text user "${REFERENCE}"
			(at 3.81 2.286 -90)
			(layer "F.Fab")
		)
		(fp_text user "K"
			(at 0 -1.8 -90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 32 "Net-(D1-K)")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 7.62 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 33 "Net-(D1-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-35_SOD27_P7.62mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_Molex:Molex_KK-254_AE-6410-02A_1x02_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 88.9 76.2)
		(descr "Molex KK-254 Interconnect System, old/engineering part number: AE-6410-02A example for new part number: 22-27-2021, 2 Pins (http://www.molex.com/pdm_docs/sd/022272021_sd.pdf), generated with kicad-footprint-generator")
		(tags "connector Molex KK-254 vertical")
		(property "Reference" "J5"
			(at -2.54 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x02"
			(at 1.27 4.08 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "project.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at -2.54 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole roundrect
			(at 0 0)
			(size 1.74 2.19)
			(drill 1.19)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.143678)
			(net 1 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 2.54 0)
			(size 1.74 2.19)
			(drill 1.19)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 29 "Net-(J5-Pin_2)")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Connector_Molex.3dshapes/Molex_KK-254_AE-6410-02A_1x02_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_THTPad_D2.0mm_Drill1.0mm"
		(layer "F.Cu")
		(at 187.96 86.36 90)
		(descr "THT pad as test Point, diameter 2.0mm, hole diameter 1.0mm")
		(tags "test point THT pad")
		(property "Reference" "TP3"
			(at 0 -1.998 90)
			(layer "F.SilkS")
		)
		(property "Value" "TestPoint"
			(at 0 2.05 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "project.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 -2 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "Package_DIP:DIP-4_W7.62mm"
		(layer "F.Cu")
		(at 157.48 73.66 -90)
		(descr "4-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
		(tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
		(property "Reference" "U1"
			(at 3.81 5.08 -90)
			(layer "F.SilkS")
		)
		(property "Value" "CPC1333G"
			(at 3.81 1.27 -90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Form B, Solid State Relay (Photo MOSFET) 60V, 0.15A, 16Ohm, SO-4"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "project.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 3.81 5.08 -90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "+12V")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 2.54 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 48 "Net-(R1-Pad1)")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 7.62 2.54 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 7.62 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 20 "Net-(U2A-+)")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-4_W7.62mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_Molex:Molex_KK-254_AE-6410-03A_1x03_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 129.54 66.04 90)
		(descr "Molex KK-254 Interconnect System, old/engineering part number: AE-6410-03A example for new part number: 22-27-2031, 3 Pins (http://www.molex.com/pdm_docs/sd/022272021_sd.pdf), generated with kicad-footprint-generator")
		(tags "connector Molex KK-254 vertical")
		(property "Reference" "J1004"
			(at 2.54 -4.12 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "OUTPUT"
			(at 2.54 4.08 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x03, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "project.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.54 -2.22 90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole roundrect
			(at 0 0 90)
			(size 1.74 2.19)
			(drill 1.19)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.143678)
			(net 41 "Net-(J1002-Pin_1)")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 2.54 0 90)
			(size 1.74 2.19)
			(drill 1.19)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 43 "Net-(J1002-Pin_2)")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 5.08 0 90)
			(size 1.74 2.19)
			(drill 1.19)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 45 "Net-(J1002-Pin_3)")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Connector_Molex.3dshapes/Molex_KK-254_AE-6410-03A_1x03_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_THTPad_D2.0mm_Drill1.0mm"
		(layer "F.Cu")
		(at 86.36 38.1 90)
		(descr "THT pad as test Point, diameter 2.0mm, hole diameter 1.0mm")
		(tags "test point THT pad")
		(property "Reference" "TP14"
			(at 0 -1.998 90)
			(layer "F.SilkS")
		)
		(property "Value" "TestPoint"
			(at 0 2.05 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "project.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 -2 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 28 "Net-(Q1-B)")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal"
		(layer "F.Cu")
		(at 78.74 53.34 -90)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R14"
			(at 3.81 2.54 90)
			(layer "F.SilkS")
		)
		(property "Value" "100R"
			(at 3.81 0 90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "project.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 3.81 2.54 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 7.62 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 24 "Net-(U4B--)")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_Molex:Molex_KK-254_AE-6410-02A_1x02_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 106.68 63.5)
		(descr "Molex KK-254 Interconnect System, old/engineering part number: AE-6410-02A example for new part number: 22-27-2021, 2 Pins (http://www.molex.com/pdm_docs/sd/022272021_sd.pdf), generated with kicad-footprint-generator")
		(tags "connector Molex KK-254 vertical")
		(property "Reference" "J7"
			(at -2.54 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x02"
			(at 1.27 3.81 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "project.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at -2.54 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole roundrect
			(at 0 0)
			(size 1.74 2.19)
			(drill 1.19)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.143678)
			(net 34 "/+12V_EM")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 2.54 0)
			(size 1.74 2.19)
			(drill 1.19)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 36 "/GND_EM")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Connector_Molex.3dshapes/Molex_KK-254_AE-6410-02A_1x02_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(gr_line
		(start 177.8 39.37)
		(end 179.07 40.64)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 228.6 94.10282)
		(end 63.5 94.10282)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 177.8 57.15)
		(end 179.07 58.42)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 180.34 71.12)
		(end 180.34 60.96)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 116.84 48.26)
		(end 116.84 68.58)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 116.84 35.56)
		(end 116.84 45.72)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 180.34 57.15)
		(end 180.34 43.18)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 180.34 60.96)
		(end 179.07 59.69)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 177.8 45.72)
		(end 177.8 43.18)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 179.07 40.64)
		(end 180.34 39.37)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.76 35.49859)
		(end 111.76 71.18141)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 116.84 68.58)
		(end 177.8 68.58)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 63.5 94.10282)
		(end 63.5 35.56)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 63.5 35.56)
		(end 111.76 35.49859)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 177.8 68.58)
		(end 177.8 60.96)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 177.8 45.72)
		(end 116.84 45.72)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 177.8 48.26)
		(end 116.84 48.26)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 116.84 35.56)
		(end 177.8 35.56)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 228.6 35.56)
		(end 228.6 94.10282)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 177.8 39.37)
		(end 177.8 35.56)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 179.07 58.42)
		(end 180.34 57.15)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.76 71.18141)
		(end 180.34 71.12)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 179.07 41.91)
		(end 177.8 43.18)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 177.8 57.15)
		(end 177.8 48.26)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 180.34 35.56)
		(end 180.34 39.37)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 180.34 43.18)
		(end 179.07 41.91)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 179.07 59.69)
		(end 177.8 60.96)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 180.34 35.56)
		(end 228.6 35.56)
		(layer "Edge.Cuts")
	)
	(gr_text "P/N: TEN 60-2422N (TRACO Power)"
		(at 154.94 50.8 0)
		(layer "B.SilkS")
	)
	(gr_text "CTL SIGNAL:\nOn: 3.0 to 12VDC or open circuit\nOff: 0 to 1.2VDC or short circuit\nRefers to 'Remote' and '-VIN' Pin"
		(at 154.94 62.23 0)
		(layer "B.SilkS")
	)
	(gr_text "P/N: TEN 60-2422N (TRACO Power)"
		(at 154.94 38.1 0)
		(layer "B.SilkS")
	)
	(gr_text "DC/DC CONVERTER\nIN: 18-36VDC\nOUT: ±12VDC 2x2.5A (60W)"
		(at 154.94 55.88 0)
		(layer "B.SilkS" knockout)
	)
	(gr_text "NOT TO GROUND"
		(at 104.14 38.1 0)
		(layer "F.SilkS")
	)
	(gr_text "AUDIO INPUT"
		(at 118.11 92.71 0)
		(layer "F.SilkS" knockout)
	)
	(gr_text "+"
		(at 118.618 43.18 90)
		(layer "F.SilkS")
	)
	(gr_text "POWER INPUT"
		(at 176.53 92.71 0)
		(layer "F.SilkS" knockout)
	)
	(gr_text "-"
		(at 126.238 63.5 90)
		(layer "F.SilkS")
	)
	(gr_text "+"
		(at 118.618 66.04 90)
		(layer "F.SilkS")
	)
	(gr_text "-"
		(at 133.858 63.5 90)
		(layer "F.SilkS")
	)
	(gr_text "CTL"
		(at 126.365 38.1 90)
		(layer "F.SilkS")
	)
	(gr_text "0"
		(at 118.745 60.96 90)
		(layer "F.SilkS")
	)
	(gr_text "-"
		(at 118.618 40.64 90)
		(layer "F.SilkS")
	)
	(gr_text "CTL"
		(at 118.745 38.1 90)
		(layer "F.SilkS")
	)
	(gr_text "AUDIO OUTPUT"
		(at 201.93 92.71 0)
		(layer "F.SilkS" knockout)
	)
	(gr_text "HEATSINKS NOT TO GROUND"
		(at 194.31 38.1 0)
		(layer "F.SilkS")
	)
	(gr_text "OUTPUT"
		(at 129.54 58.42 0)
		(layer "F.SilkS")
	)
	(gr_text "|     |"
		(at 214.63 87.63 0)
		(layer "F.SilkS" knockout)
	)
	(gr_text "ANALYZER"
		(at 64.77 92.71 0)
		(layer "F.SilkS" knockout)
	)
	(gr_text "INPUT"
		(at 128.27 40.64 90)
		(layer "F.SilkS")
	)
	(gr_text "+"
		(at 126.238 43.18 90)
		(layer "F.SilkS")
	)
	(gr_text "-"
		(at 126.238 40.64 90)
		(layer "F.SilkS")
	)
	(gr_text "0"
		(at 126.365 60.96 90)
		(layer "F.SilkS")
	)
	(gr_text "0"
		(at 141.605 60.96 90)
		(layer "F.SilkS")
	)
	(gr_text "+"
		(at 126.238 66.04 90)
		(layer "F.SilkS")
	)
	(gr_text "+"
		(at 141.478 66.04 90)
		(layer "F.SilkS")
	)
	(gr_text "-"
		(at 141.478 63.5 90)
		(layer "F.SilkS")
	)
	(gr_text "FERROFLUID VU-METER\nREV 2\nREMI BERTHOZ"
		(at 226.06 85.09 0)
		(layer "F.SilkS")
	)
	(gr_text "+"
		(at 133.858 66.04 90)
		(layer "F.SilkS")
	)
	(gr_text "-"
		(at 118.618 63.5 90)
		(layer "F.SilkS")
	)
	(gr_text "0"
		(at 133.985 60.96 90)
		(layer "F.SilkS")
	)
	(gr_text "K"
		(at 106.68 71.755 0)
		(layer "F.Fab")
	)
	(dimension
		(type aligned)
		(layer "Dwgs.User")
		(pts
			(xy 111.76 33.02) (xy 63.5 33.02)
		)
		(height 0)
		(gr_text "48,2600 mm"
			(at 87.63 31.87 0)
			(layer "Dwgs.User")
		)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 1)
			(precision 4)
		)
		(style
			(thickness 0.15)
			(arrow_length 1.27)
			(text_position_mode 0)
			(extension_height 0.58642)
			(extension_offset 0.5) keep_text_aligned)
	)
	(dimension
		(type aligned)
		(layer "Dwgs.User")
		(pts
			(xy 228.6 33.02) (xy 180.34 33.02)
		)
		(height 0)
		(gr_text "48,2600 mm"
			(at 204.47 31.87 0)
			(layer "Dwgs.User")
		)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 1)
			(precision 4)
		)
		(style
			(thickness 0.15)
			(arrow_length 1.27)
			(text_position_mode 0)
			(extension_height 0.58642)
			(extension_offset 0.5) keep_text_aligned)
	)
	(dimension
		(type aligned)
		(layer "F.Fab")
		(pts
			(xy 63.5 94.10282) (xy 228.6 93.98)
		)
		(height 5.955761)
		(gr_text "165,1000 mm"
			(at 146.053576 98.847169 0.04262305476)
			(layer "F.Fab")
		)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 1)
			(precision 4)
		)
		(style
			(thickness 0.1)
			(arrow_length 1.27)
			(text_position_mode 0)
			(extension_height 0.58642)
			(extension_offset 0.5) keep_text_aligned)
	)
	(dimension
		(type aligned)
		(layer "F.Fab")
		(pts
			(xy 111.76 34.29) (xy 180.34 34.29)
		)
		(height -3.81)
		(gr_text "68,5800 mm"
			(at 146.05 29.33 0)
			(layer "F.Fab")
		)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 1)
			(precision 4)
		)
		(style
			(thickness 0.1)
			(arrow_length 1.27)
			(text_position_mode 0)
			(extension_height 0.58642)
			(extension_offset 0.5) keep_text_aligned)
	)
	(dimension
		(type aligned)
		(layer "F.Fab")
		(pts
			(xy 68.58 43.18) (xy 223.52 43.18)
		)
		(height -16.51)
		(gr_text "154,9400 mm"
			(at 146.05 25.52 0)
			(layer "F.Fab")
		)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 1)
			(precision 4)
		)
		(style
			(thickness 0.1)
			(arrow_length 1.27)
			(text_position_mode 0)
			(extension_height 0.58642)
			(extension_offset 0.5) keep_text_aligned)
	)
	(dimension
		(type aligned)
		(layer "F.Fab")
		(pts
			(xy 68.58 43.18) (xy 68.58 91.44)
		)
		(height 10.16)
		(gr_text "48,2600 mm"
			(at 57.27 67.31 90)
			(layer "F.Fab")
		)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 1)
			(precision 4)
		)
		(style
			(thickness 0.1)
			(arrow_length 1.27)
			(text_position_mode 0)
			(extension_height 0.58642)
			(extension_offset 0.5) keep_text_aligned)
	)
	(dimension
		(type aligned)
		(layer "F.Fab")
		(pts
			(xy 229.87 71.12) (xy 229.87 35.56)
		)
		(height 3.81)
		(gr_text "35,5600 mm"
			(at 232.53 53.34 90)
			(layer "F.Fab")
		)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 1)
			(precision 4)
		)
		(style
			(thickness 0.1)
			(arrow_length 1.27)
			(text_position_mode 0)
			(extension_height 0.58642)
			(extension_offset 0.5) keep_text_aligned)
	)
	(dimension
		(type aligned)
		(layer "F.Fab")
		(pts
			(xy 229.87 71.12) (xy 229.87 93.98)
		)
		(height -3.81)
		(gr_text "22,8600 mm"
			(at 232.53 82.55 90)
			(layer "F.Fab")
		)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 1)
			(precision 4)
		)
		(style
			(thickness 0.1)
			(arrow_length 1.27)
			(text_position_mode 0)
			(extension_height 0.58642)
			(extension_offset 0.5) keep_text_aligned)
	)
	(zone
		(net 42)
		(net_name "Net-(PS1001-+VOUT)")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 3)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 116.84 48.26) (xy 116.84 52.705) (xy 141.605 52.705) (xy 141.605 68.58) (xy 168.91 68.58) (xy 168.91 48.26)
			)
		)
	)
	(zone
		(net 41)
		(net_name "Net-(J1002-Pin_1)")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 4)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 116.84 53.975) (xy 140.335 53.975) (xy 140.335 68.58) (xy 116.84 68.58)
			)
		)
	)
	(zone
		(net 39)
		(net_name "Net-(J2001-Pin_1)")
		(layers "F&B.Cu")
		(hatch edge 0.5)
		(priority 5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 116.84 38.1) (xy 134.62 38.1) (xy 134.62 45.72) (xy 116.84 45.72)
			)
		)
	)
	(zone
		(net 40)
		(net_name "Net-(PS1001-+VIN)")
		(layers "F&B.Cu")
		(hatch edge 0.5)
		(priority 5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 157.48 38.1) (xy 137.16 38.1) (xy 137.16 45.72) (xy 157.48 45.72)
			)
		)
	)
	(zone
		(net 1)
		(net_name "GND")
		(layer "In1.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0.254)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
			(smoothing fillet)
			(radius 1.084)
		)
		(polygon
			(pts
				(xy 207.01 35.56) (xy 207.01 55.88) (xy 209.55 55.88) (xy 209.55 74.93) (xy 200.66 74.93) (xy 200.66 68.58)
				(xy 180.34 68.58) (xy 180.34 71.12) (xy 111.76 71.12) (xy 93.98 71.12) (xy 93.98 59.69) (xy 97.79 59.69)
				(xy 97.79 35.56) (xy 63.5 35.56) (xy 63.5 93.98) (xy 228.6 93.98) (xy 228.6 35.56)
			)
		)
	)
	(zone
		(net 45)
		(net_name "Net-(J1002-Pin_3)")
		(layers "In1.Cu" "In2.Cu")
		(hatch edge 0.5)
		(priority 3)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 116.84 48.26) (xy 116.84 68.58) (xy 168.91 68.58) (xy 168.91 48.26)
			)
		)
	)
	(zone
		(net 47)
		(net_name "Net-(J2001-Pin_2)")
		(layers "In1.Cu" "In2.Cu")
		(hatch edge 0.5)
		(priority 6)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 116.84 38.1) (xy 168.91 38.1) (xy 168.91 45.72) (xy 116.84 45.72)
			)
		)
	)
	(zone
		(net 1)
		(net_name "GND")
		(layer "In2.Cu")
		(hatch edge 0.5)
		(priority 1)
		(connect_pads
			(clearance 0.254)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 128.27 85.09) (xy 135.89 85.09) (xy 135.89 87.63) (xy 162.56 87.63) (xy 162.56 86.461438) (xy 167.64 86.36)
				(xy 167.64 91.44) (xy 162.56 91.44) (xy 162.56 90.17) (xy 128.27 90.17)
			)
		)
	)
	(zone
		(net 12)
		(net_name "+12V")
		(layer "In2.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0.254)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
			(smoothing fillet)
			(radius 1.084)
		)
		(polygon
			(pts
				(xy 207.01 35.56) (xy 207.01 55.88) (xy 209.55 55.88) (xy 209.55 74.93) (xy 200.66 74.93) (xy 200.66 68.58)
				(xy 180.34 68.58) (xy 180.34 71.12) (xy 111.76 71.12) (xy 93.98 71.12) (xy 93.98 59.69) (xy 97.79 59.69)
				(xy 97.79 35.56) (xy 63.5 35.56) (xy 63.5 93.98) (xy 228.6 93.98) (xy 228.6 35.56)
			)
		)
	)
	(zone
		(net 43)
		(net_name "Net-(J1002-Pin_2)")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 4)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 116.84 53.975) (xy 140.335 53.975) (xy 140.335 68.58) (xy 116.84 68.58)
			)
		)
	)
	(zone
		(net 44)
		(net_name "Net-(PS1001--VOUT)")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 3)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 116.84 48.26) (xy 116.84 52.705) (xy 141.605 52.705) (xy 141.605 68.58) (xy 168.91 68.58) (xy 168.91 48.26)
			)
		)
	)
	(zone
		(net 13)
		(net_name "-12V")
		(layer "B.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0.254)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
			(smoothing fillet)
			(radius 1.084)
		)
		(polygon
			(pts
				(xy 207.01 35.56) (xy 207.01 55.88) (xy 209.55 55.88) (xy 209.55 74.93) (xy 200.66 74.93) (xy 200.66 68.58)
				(xy 180.34 68.58) (xy 180.34 71.12) (xy 111.76 71.12) (xy 93.98 71.12) (xy 93.98 59.69) (xy 97.79 59.69)
				(xy 97.79 35.56) (xy 63.5 35.56) (xy 63.5 93.98) (xy 228.6 93.98) (xy 228.6 35.56)
			)
		)
	)
)