(kicad_sch
	(version 20231120)
	(generator "eeschema")
	(generator_version "8.0")
	(paper "A4")
	(lib_symbols
		(symbol "LED:SK6812MINI"
			(pin_names
				(offset 0.254)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "D"
				(at 5.08 5.715 0)
			)
			(property "Value" "SK6812MINI"
				(at 1.27 -5.715 0)
			)
			(property "Footprint" "LED_SMD:LED_SK6812MINI_PLCC4_3.5x3.5mm_P1.75mm"
				(at 1.27 -7.62 0)
			)
			(property "Datasheet" "https://cdn-shop.adafruit.com/product-files/2686/SK6812MINI_REV.01-1-2.pdf"
				(at 2.54 -9.525 0)
			)
			(property "Description" "RGB LED with integrated controller"
				(at 0 0 0)
			)
			(property "ki_keywords" "RGB LED NeoPixel Mini addressable"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "LED*SK6812MINI*PLCC*3.5x3.5mm*P1.75mm*"
				(at 0 0 0)
			)
			(symbol "SK6812MINI_0_0"
				(text "RGB"
					(at 2.286 -4.191 0)
				)
			)
			(symbol "SK6812MINI_0_1"
				(polyline
					(pts
						(xy 1.27 -3.556) (xy 1.778 -3.556)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.27 -2.54) (xy 1.778 -2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 4.699 -3.556) (xy 2.667 -3.556)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 2.286 -2.54) (xy 1.27 -3.556) (xy 1.27 -3.048)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 2.286 -1.524) (xy 1.27 -2.54) (xy 1.27 -2.032)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 3.683 -1.016) (xy 3.683 -3.556) (xy 3.683 -4.064)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 4.699 -1.524) (xy 2.667 -1.524) (xy 3.683 -3.556) (xy 4.699 -1.524)
					)
					(fill
						(type none)
					)
				)
				(rectangle
					(start 5.08 5.08)
					(end -5.08 -5.08)
					(fill
						(type background)
					)
				)
			)
			(symbol "SK6812MINI_1_1"
				(pin output line
					(at 7.62 0 180)
					(length 2.54)
					(name "DOUT")
					(number "1")
				)
				(pin power_in line
					(at 0 -7.62 90)
					(length 2.54)
					(name "VSS")
					(number "2")
				)
				(pin input line
					(at -7.62 0 0)
					(length 2.54)
					(name "DIN")
					(number "3")
				)
				(pin power_in line
					(at 0 7.62 270)
					(length 2.54)
					(name "VDD")
					(number "4")
				)
			)
		)
		(symbol "MCU_Module:Arduino_Nano_Every"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "A"
				(at -10.16 23.495 0)
			)
			(property "Value" "Arduino_Nano_Every"
				(at 5.08 -24.13 0)
			)
			(property "Footprint" "Module:Arduino_Nano"
				(at 0 0 0)
			)
			(property "Datasheet" "https://content.arduino.cc/assets/NANOEveryV3.0_sch.pdf"
				(at 0 0 0)
			)
			(property "Description" "Arduino Nano Every"
				(at 0 0 0)
			)
			(property "ki_keywords" "Arduino nano microcontroller module USB UPDI AATMega4809 AVR"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "Arduino*Nano*"
				(at 0 0 0)
			)
			(symbol "Arduino_Nano_Every_0_1"
				(rectangle
					(start -10.16 22.86)
					(end 10.16 -22.86)
					(fill
						(type background)
					)
				)
			)
			(symbol "Arduino_Nano_Every_1_1"
				(pin bidirectional line
					(at -12.7 20.32 0)
					(length 2.54)
					(name "TX1")
					(number "1")
				)
				(pin bidirectional line
					(at -12.7 0 0)
					(length 2.54)
					(name "D7")
					(number "10")
				)
				(pin bidirectional line
					(at -12.7 -2.54 0)
					(length 2.54)
					(name "D8")
					(number "11")
				)
				(pin bidirectional line
					(at -12.7 -5.08 0)
					(length 2.54)
					(name "D9")
					(number "12")
				)
				(pin bidirectional line
					(at -12.7 -7.62 0)
					(length 2.54)
					(name "D10")
					(number "13")
				)
				(pin bidirectional line
					(at -12.7 -12.7 0)
					(length 2.54)
					(name "MOSI")
					(number "14")
				)
				(pin bidirectional line
					(at -12.7 -15.24 0)
					(length 2.54)
					(name "MISO")
					(number "15")
				)
				(pin bidirectional line
					(at -12.7 -17.78 0)
					(length 2.54)
					(name "SCK")
					(number "16")
				)
				(pin power_out line
					(at 2.54 25.4 270)
					(length 2.54)
					(name "3V3")
					(number "17")
				)
				(pin input line
					(at 12.7 5.08 180)
					(length 2.54)
					(name "AREF")
					(number "18")
				)
				(pin bidirectional line
					(at 12.7 0 180)
					(length 2.54)
					(name "A0")
					(number "19")
				)
				(pin bidirectional line
					(at -12.7 17.78 0)
					(length 2.54)
					(name "RX1")
					(number "2")
				)
				(pin bidirectional line
					(at 12.7 -2.54 180)
					(length 2.54)
					(name "A1")
					(number "20")
				)
				(pin bidirectional line
					(at 12.7 -5.08 180)
					(length 2.54)
					(name "A2")
					(number "21")
				)
				(pin bidirectional line
					(at 12.7 -7.62 180)
					(length 2.54)
					(name "A3")
					(number "22")
				)
				(pin bidirectional line
					(at 12.7 -10.16 180)
					(length 2.54)
					(name "SDA/A4")
					(number "23")
				)
				(pin bidirectional line
					(at 12.7 -12.7 180)
					(length 2.54)
					(name "SCL/A5")
					(number "24")
				)
				(pin bidirectional line
					(at 12.7 -15.24 180)
					(length 2.54)
					(name "A6")
					(number "25")
				)
				(pin bidirectional line
					(at 12.7 -17.78 180)
					(length 2.54)
					(name "A7")
					(number "26")
				)
				(pin power_out line
					(at 5.08 25.4 270)
					(length 2.54)
					(name "+5V")
					(number "27")
				)
				(pin input line
					(at 12.7 12.7 180)
					(length 2.54)
					(name "~{RESET}")
					(number "28")
				)
				(pin passive line
					(at 0 -25.4 90)
					(length 2.54) hide
					(name "GND")
					(number "29")
				)
				(pin input line
					(at 12.7 15.24 180)
					(length 2.54)
					(name "~{RESET}")
					(number "3")
				)
				(pin power_in line
					(at -2.54 25.4 270)
					(length 2.54)
					(name "VIN")
					(number "30")
				)
				(pin power_in line
					(at 0 -25.4 90)
					(length 2.54)
					(name "GND")
					(number "4")
				)
				(pin bidirectional line
					(at -12.7 12.7 0)
					(length 2.54)
					(name "D2")
					(number "5")
				)
				(pin bidirectional line
					(at -12.7 10.16 0)
					(length 2.54)
					(name "D3")
					(number "6")
				)
				(pin bidirectional line
					(at -12.7 7.62 0)
					(length 2.54)
					(name "D4")
					(number "7")
				)
				(pin bidirectional line
					(at -12.7 5.08 0)
					(length 2.54)
					(name "D5")
					(number "8")
				)
				(pin bidirectional line
					(at -12.7 2.54 0)
					(length 2.54)
					(name "D6")
					(number "9")
				)
			)
		)
		(symbol "Switch:SW_Push_Dual"
			(pin_names
				(offset 1.016) hide)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "SW"
				(at 0 7.62 0)
			)
			(property "Value" "SW_Push_Dual"
				(at 0 -6.35 0)
			)
			(property "Footprint" ""
				(at 0 7.62 0)
			)
			(property "Datasheet" "~"
				(at 0 0 0)
			)
			(property "Description" "Push button switch, generic, symbol, four pins"
				(at 0 0 0)
			)
			(property "ki_keywords" "switch normally-open pushbutton push-button"
				(at 0 0 0)
			)
			(symbol "SW_Push_Dual_0_1"
				(circle
					(center -2.032 -2.54)
					(radius 0.508)
					(fill
						(type none)
					)
				)
				(circle
					(center -2.032 2.54)
					(radius 0.508)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -0.508) (xy 0 -1.016)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 0.508) (xy 0 0)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 1.016) (xy 0 1.524)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 2.032) (xy 0 2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 3.048) (xy 0 3.556)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 3.81) (xy 0 5.588)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 2.54 -1.27) (xy -2.54 -1.27)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 2.54 3.81) (xy -2.54 3.81)
					)
					(fill
						(type none)
					)
				)
				(circle
					(center 2.032 -2.54)
					(radius 0.508)
					(fill
						(type none)
					)
				)
				(circle
					(center 2.032 2.54)
					(radius 0.508)
					(fill
						(type none)
					)
				)
				(pin passive line
					(at -5.08 2.54 0)
					(length 2.54)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 5.08 2.54 180)
					(length 2.54)
					(name "2")
					(number "2")
				)
				(pin passive line
					(at -5.08 -2.54 0)
					(length 2.54)
					(name "3")
					(number "3")
				)
				(pin passive line
					(at 5.08 -2.54 180)
					(length 2.54)
					(name "4")
					(number "4")
				)
			)
			(symbol "SW_Push_Dual_1_1"
				(rectangle
					(start -3.175 5.715)
					(end 3.175 -4.445)
					(fill
						(type background)
					)
				)
			)
		)
	)
	(junction
		(at 199.39 88.9)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 153.67 88.9)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 168.91 104.14)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 102.87 125.73)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 123.19 88.9)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 184.15 88.9)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 114.3 125.73)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 138.43 88.9)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 123.19 104.14)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 199.39 104.14)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 153.67 104.14)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 184.15 104.14)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 138.43 104.14)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 168.91 88.9)
		(diameter 0)
		(color 0 0 0 0)
	)
	(wire
		(pts
			(xy 153.67 88.9) (xy 168.91 88.9)
		)
	)
	(wire
		(pts
			(xy 93.98 125.73) (xy 93.98 120.65)
		)
	)
	(wire
		(pts
			(xy 99.06 140.97) (xy 102.87 140.97)
		)
	)
	(wire
		(pts
			(xy 111.76 66.04) (xy 78.74 66.04)
		)
	)
	(wire
		(pts
			(xy 87.63 49.53) (xy 77.47 49.53)
		)
	)
	(wire
		(pts
			(xy 78.74 82.55) (xy 81.28 82.55)
		)
	)
	(wire
		(pts
			(xy 123.19 88.9) (xy 109.22 88.9)
		)
	)
	(wire
		(pts
			(xy 102.87 125.73) (xy 93.98 125.73)
		)
	)
	(wire
		(pts
			(xy 109.22 69.85) (xy 99.06 69.85)
		)
	)
	(wire
		(pts
			(xy 77.47 85.09) (xy 81.28 85.09)
		)
	)
	(wire
		(pts
			(xy 168.91 88.9) (xy 184.15 88.9)
		)
	)
	(wire
		(pts
			(xy 123.19 104.14) (xy 138.43 104.14)
		)
	)
	(wire
		(pts
			(xy 199.39 88.9) (xy 214.63 88.9)
		)
	)
	(wire
		(pts
			(xy 153.67 104.14) (xy 168.91 104.14)
		)
	)
	(wire
		(pts
			(xy 77.47 49.53) (xy 77.47 85.09)
		)
	)
	(wire
		(pts
			(xy 111.76 96.52) (xy 111.76 66.04)
		)
	)
	(wire
		(pts
			(xy 77.47 102.87) (xy 81.28 102.87)
		)
	)
	(wire
		(pts
			(xy 114.3 125.73) (xy 102.87 125.73)
		)
	)
	(wire
		(pts
			(xy 168.91 104.14) (xy 184.15 104.14)
		)
	)
	(wire
		(pts
			(xy 184.15 104.14) (xy 199.39 104.14)
		)
	)
	(wire
		(pts
			(xy 123.19 104.14) (xy 123.19 125.73)
		)
	)
	(wire
		(pts
			(xy 138.43 88.9) (xy 153.67 88.9)
		)
	)
	(wire
		(pts
			(xy 102.87 140.97) (xy 102.87 125.73)
		)
	)
	(wire
		(pts
			(xy 123.19 125.73) (xy 114.3 125.73)
		)
	)
	(wire
		(pts
			(xy 123.19 88.9) (xy 138.43 88.9)
		)
	)
	(wire
		(pts
			(xy 88.9 135.89) (xy 77.47 135.89)
		)
	)
	(wire
		(pts
			(xy 115.57 96.52) (xy 111.76 96.52)
		)
	)
	(wire
		(pts
			(xy 114.3 54.61) (xy 114.3 125.73)
		)
	)
	(wire
		(pts
			(xy 199.39 104.14) (xy 214.63 104.14)
		)
	)
	(wire
		(pts
			(xy 109.22 88.9) (xy 109.22 69.85)
		)
	)
	(wire
		(pts
			(xy 97.79 54.61) (xy 114.3 54.61)
		)
	)
	(wire
		(pts
			(xy 78.74 66.04) (xy 78.74 82.55)
		)
	)
	(wire
		(pts
			(xy 138.43 104.14) (xy 153.67 104.14)
		)
	)
	(wire
		(pts
			(xy 184.15 88.9) (xy 199.39 88.9)
		)
	)
	(wire
		(pts
			(xy 77.47 135.89) (xy 77.47 102.87)
		)
	)
	(label "ARCA1D"
		(at 186.69 191.77 0)
		(fields_autoplaced yes)
	)
	(label "Right Button"
		(at 87.63 146.05 0)
		(fields_autoplaced yes)
	)
	(label "NeoPixel Strip"
		(at 156.21 109.22 0)
		(fields_autoplaced yes)
	)
	(label "Left Button"
		(at 87.63 59.69 0)
		(fields_autoplaced yes)
	)
	(symbol
		(lib_id "LED:SK6812MINI")
		(at 199.39 96.52 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "D6"
			(at 212.09 90.2014 0)
		)
		(property "Value" "SK6812MINI"
			(at 212.09 92.7414 0)
		)
		(property "Footprint" "LED_SMD:LED_SK6812MINI_PLCC4_3.5x3.5mm_P1.75mm"
			(at 200.66 104.14 0)
		)
		(property "Datasheet" "https://cdn-shop.adafruit.com/product-files/2686/SK6812MINI_REV.01-1-2.pdf"
			(at 201.93 106.045 0)
		)
		(property "Description" "RGB LED with integrated controller"
			(at 199.39 96.52 0)
		)
		(pin "1")
		(pin "2")
		(pin "3")
		(pin "4")
		(instances
			(project "arca1d"
				(path
					(reference "D6")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "LED:SK6812MINI")
		(at 168.91 96.52 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "D4"
			(at 181.61 90.2014 0)
		)
		(property "Value" "SK6812MINI"
			(at 181.61 92.7414 0)
		)
		(property "Footprint" "LED_SMD:LED_SK6812MINI_PLCC4_3.5x3.5mm_P1.75mm"
			(at 170.18 104.14 0)
		)
		(property "Datasheet" "https://cdn-shop.adafruit.com/product-files/2686/SK6812MINI_REV.01-1-2.pdf"
			(at 171.45 106.045 0)
		)
		(property "Description" "RGB LED with integrated controller"
			(at 168.91 96.52 0)
		)
		(pin "1")
		(pin "2")
		(pin "3")
		(pin "4")
		(instances
			(project "arca1d"
				(path
					(reference "D4")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Switch:SW_Push_Dual")
		(at 93.98 138.43 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "SW1"
			(at 93.98 128.27 0)
		)
		(property "Value" "SW_Push_Dual"
			(at 93.98 130.81 0)
		)
		(property "Footprint" ""
			(at 93.98 130.81 0)
		)
		(property "Datasheet" "~"
			(at 93.98 138.43 0)
		)
		(property "Description" "Push button switch, generic, symbol, four pins"
			(at 93.98 138.43 0)
		)
		(pin "1")
		(pin "2")
		(pin "4")
		(pin "3")
		(instances
			(project ""
				(path
					(reference "SW1")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "MCU_Module:Arduino_Nano_Every")
		(at 93.98 95.25 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "A1"
			(at 96.1741 120.65 0)
		)
		(property "Value" "Arduino_Nano_Every"
			(at 96.1741 123.19 0)
		)
		(property "Footprint" "Module:Arduino_Nano"
			(at 93.98 95.25 0)
		)
		(property "Datasheet" "https://content.arduino.cc/assets/NANOEveryV3.0_sch.pdf"
			(at 93.98 95.25 0)
		)
		(property "Description" "Arduino Nano Every"
			(at 93.98 95.25 0)
		)
		(pin "19")
		(pin "21")
		(pin "22")
		(pin "9")
		(pin "16")
		(pin "1")
		(pin "11")
		(pin "8")
		(pin "23")
		(pin "5")
		(pin "27")
		(pin "13")
		(pin "30")
		(pin "2")
		(pin "4")
		(pin "14")
		(pin "25")
		(pin "29")
		(pin "12")
		(pin "6")
		(pin "7")
		(pin "10")
		(pin "15")
		(pin "17")
		(pin "24")
		(pin "26")
		(pin "28")
		(pin "18")
		(pin "3")
		(pin "20")
		(instances
			(project ""
				(path
					(reference "A1")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "LED:SK6812MINI")
		(at 138.43 96.52 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "D2"
			(at 151.13 90.2014 0)
		)
		(property "Value" "SK6812MINI"
			(at 151.13 92.7414 0)
		)
		(property "Footprint" "LED_SMD:LED_SK6812MINI_PLCC4_3.5x3.5mm_P1.75mm"
			(at 139.7 104.14 0)
		)
		(property "Datasheet" "https://cdn-shop.adafruit.com/product-files/2686/SK6812MINI_REV.01-1-2.pdf"
			(at 140.97 106.045 0)
		)
		(property "Description" "RGB LED with integrated controller"
			(at 138.43 96.52 0)
		)
		(pin "1")
		(pin "2")
		(pin "3")
		(pin "4")
		(instances
			(project ""
				(path
					(reference "D2")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "LED:SK6812MINI")
		(at 184.15 96.52 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "D5"
			(at 196.85 90.2014 0)
		)
		(property "Value" "SK6812MINI"
			(at 196.85 92.7414 0)
		)
		(property "Footprint" "LED_SMD:LED_SK6812MINI_PLCC4_3.5x3.5mm_P1.75mm"
			(at 185.42 104.14 0)
		)
		(property "Datasheet" "https://cdn-shop.adafruit.com/product-files/2686/SK6812MINI_REV.01-1-2.pdf"
			(at 186.69 106.045 0)
		)
		(property "Description" "RGB LED with integrated controller"
			(at 184.15 96.52 0)
		)
		(pin "1")
		(pin "2")
		(pin "3")
		(pin "4")
		(instances
			(project "arca1d"
				(path
					(reference "D5")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Switch:SW_Push_Dual")
		(at 92.71 52.07 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "SW2"
			(at 92.71 41.91 0)
		)
		(property "Value" "SW_Push_Dual"
			(at 92.71 44.45 0)
		)
		(property "Footprint" ""
			(at 92.71 44.45 0)
		)
		(property "Datasheet" "~"
			(at 92.71 52.07 0)
		)
		(property "Description" "Push button switch, generic, symbol, four pins"
			(at 92.71 52.07 0)
		)
		(pin "1")
		(pin "2")
		(pin "4")
		(pin "3")
		(instances
			(project ""
				(path
					(reference "SW2")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "LED:SK6812MINI")
		(at 153.67 96.52 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "D3"
			(at 166.37 90.2014 0)
		)
		(property "Value" "SK6812MINI"
			(at 166.37 92.7414 0)
		)
		(property "Footprint" "LED_SMD:LED_SK6812MINI_PLCC4_3.5x3.5mm_P1.75mm"
			(at 154.94 104.14 0)
		)
		(property "Datasheet" "https://cdn-shop.adafruit.com/product-files/2686/SK6812MINI_REV.01-1-2.pdf"
			(at 156.21 106.045 0)
		)
		(property "Description" "RGB LED with integrated controller"
			(at 153.67 96.52 0)
		)
		(pin "1")
		(pin "2")
		(pin "3")
		(pin "4")
		(instances
			(project "arca1d"
				(path
					(reference "D3")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "LED:SK6812MINI")
		(at 123.19 96.52 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "D1"
			(at 135.89 90.2014 0)
		)
		(property "Value" "SK6812MINI"
			(at 135.89 92.7414 0)
		)
		(property "Footprint" "LED_SMD:LED_SK6812MINI_PLCC4_3.5x3.5mm_P1.75mm"
			(at 124.46 104.14 0)
		)
		(property "Datasheet" "https://cdn-shop.adafruit.com/product-files/2686/SK6812MINI_REV.01-1-2.pdf"
			(at 125.73 106.045 0)
		)
		(property "Description" "RGB LED with integrated controller"
			(at 123.19 96.52 0)
		)
		(pin "1")
		(pin "2")
		(pin "3")
		(pin "4")
		(instances
			(project ""
				(path
					(reference "D1")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "LED:SK6812MINI")
		(at 214.63 96.52 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "D7"
			(at 227.33 90.2014 0)
		)
		(property "Value" "SK6812MINI"
			(at 227.33 92.7414 0)
		)
		(property "Footprint" "LED_SMD:LED_SK6812MINI_PLCC4_3.5x3.5mm_P1.75mm"
			(at 215.9 104.14 0)
		)
		(property "Datasheet" "https://cdn-shop.adafruit.com/product-files/2686/SK6812MINI_REV.01-1-2.pdf"
			(at 217.17 106.045 0)
		)
		(property "Description" "RGB LED with integrated controller"
			(at 214.63 96.52 0)
		)
		(pin "1")
		(pin "2")
		(pin "3")
		(pin "4")
		(instances
			(project "arca1d"
				(path
					(reference "D7")
					(unit 1)
				)
			)
		)
	)
	(sheet_instances
		(path
			(page "1")
		)
	)
)
