(footprint "squareSAOAO"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at -7.62 -10.16 0)
		(unlocked yes)
		(layer "F.SilkS")
		(hide yes)
	)
	(property "Value" "squareSAOAO"
		(at 4.5 -10.5 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(property "Footprint" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_line
		(start -9.5 -8.5)
		(end -9.5 8.5)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start -8.5 9.5)
		(end 8.5 9.5)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start 8.5 -9.5)
		(end -8.5 -9.5)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start 9.5 8.5)
		(end 9.5 -8.5)
		(layer "Edge.Cuts")
	)
	(fp_arc
		(start -9.5 -8.5)
		(mid -9.207107 -9.207107)
		(end -8.5 -9.5)
		(layer "Edge.Cuts")
	)
	(fp_arc
		(start -8.5 9.5)
		(mid -9.207107 9.207107)
		(end -9.5 8.5)
		(layer "Edge.Cuts")
	)
	(fp_arc
		(start 8.5 -9.5)
		(mid 9.207107 -9.207107)
		(end 9.5 -8.5)
		(layer "Edge.Cuts")
	)
	(fp_arc
		(start 9.5 8.5)
		(mid 9.207107 9.207107)
		(end 8.5 9.5)
		(layer "Edge.Cuts")
	)
	(fp_text user "GND VCC GND"
		(at 0 6 0)
		(unlocked yes)
		(layer "Dwgs.User")
	)
	(fp_text user "1.27mm header"
		(at 0 5.5 0)
		(unlocked yes)
		(layer "Dwgs.User")
	)
	(fp_text user "${REFERENCE}"
		(at 4.5 -12.5 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(dimension
		(type aligned)
		(layer "Dwgs.User")
		(pts
			(xy 9.5 -9.5) (xy 9.5 -8.5)
		)
		(height -6)
		(gr_text "1.0000 mm"
			(at 14.35 -9 90)
			(layer "Dwgs.User")
		)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 1)
			(precision 4)
		)
		(style
			(thickness 0.1)
			(arrow_length 1.27)
			(text_position_mode 0)
			(extension_height 0.58642)
			(extension_offset 0.5) keep_text_aligned)
	)
	(dimension
		(type aligned)
		(layer "Dwgs.User")
		(pts
			(xy -9.5 10) (xy 9.5 10)
		)
		(height 8.5)
		(gr_text "19.0000 mm"
			(at 0 17.35 0)
			(layer "Dwgs.User")
		)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 1)
			(precision 4)
		)
		(style
			(thickness 0.1)
			(arrow_length 1.27)
			(text_position_mode 0)
			(extension_height 0.58642)
			(extension_offset 0.5) keep_text_aligned)
	)
	(dimension
		(type aligned)
		(layer "Dwgs.User")
		(pts
			(xy -9.5 -9.5) (xy -9.5 9.5)
		)
		(height 3)
		(gr_text "19.0000 mm"
			(at -13.65 0 90)
			(layer "Dwgs.User")
		)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 1)
			(precision 4)
		)
		(style
			(thickness 0.1)
			(arrow_length 1.27)
			(text_position_mode 0)
			(extension_height 0.58642)
			(extension_offset 0.5) keep_text_aligned)
	)
	(dimension
		(type aligned)
		(layer "Dwgs.User")
		(pts
			(xy 0 8) (xy 0 9.5)
		)
		(height -15)
		(gr_text "1.5000 mm"
			(at 13.85 8.75 90)
			(layer "Dwgs.User")
		)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 1)
			(precision 4)
		)
		(style
			(thickness 0.1)
			(arrow_length 1.27)
			(text_position_mode 0)
			(extension_height 0.58642)
			(extension_offset 0.5) keep_text_aligned)
	)
	(pad "1" thru_hole roundrect
		(at -1.27 8)
		(size 1 1.5)
		(drill 0.6
			(offset 0 0.25)
		)
		(layers "*.Cu" "F.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.25)
	)
	(pad "2" thru_hole roundrect
		(at 0 8)
		(size 1 1.5)
		(drill 0.6
			(offset 0 0.25)
		)
		(layers "*.Cu" "F.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.5)
	)
	(pad "3" thru_hole roundrect
		(at 1.27 8)
		(size 1 1.5)
		(drill 0.6
			(offset 0 0.25)
		)
		(layers "*.Cu" "F.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.25)
	)
)
