(kicad_pcb (version 4) (host pcbnew 4.0.5-e0-6337~49~ubuntu16.04.1)
  (general
    (links 6)
    (no_connects 0)
    (area 141.709974 102.004999 191.475001 109.295001)
    (thickness 1.6)
    (drawings 12)
    (tracks 46)
    (zones 0)
    (modules 3)
    (nets 5)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.4)
    (trace_clearance 0.33)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.4)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.6)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00000_00000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative true)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 5)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 VCC)
  (net 2 GND)
  (net 3 DI)
  (net 4 DO)
  (net_class Default "This is the default net class."
    (clearance 0.33)
    (trace_width 0.4)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net DI)
    (add_net DO)
    (add_net GND)
    (add_net VCC)
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5415D6EA)
    (at 143.5227 104.394 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C1 (at 0 -2.1 270) (layer F.SilkS))
    (fp_text value C (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_WS2812B-PLCC4 (layer F.Cu) (tedit 56C9C7F7)
    (at 148.5011 105.0036)
    (descr http://www.world-semi.com/uploads/soft/150522/1-150522091P5.pdf)
    (tags "LED NeoPixel")
    (attr smd)
    (fp_text reference LED1 (at 0 -3.5) (layer F.SilkS))
    (fp_text value WS2812B (at 0 4) (layer F.Fab))
    (pad 3 smd rect (at 2.5 1.6) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 4 smd rect (at 2.5 -1.6) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 3 DI))
    (pad 2 smd rect (at -2.5 1.6) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 4 DO))
    (pad 1 smd rect (at -2.5 -1.6) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (model LEDs.3dshapes/LED_WS2812B-PLCC4.wrl
      (at (xyz 0 0 0.004))
      (scale (xyz 0.385 0.385 0.385))
      (rotate (xyz 0 0 180))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x04 (layer F.Cu) (tedit 0)
    (at 182.54 106.98 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P1 (at 0 -5.1 90) (layer F.SilkS))
    (fp_text value CONN_01X04 (at 0 -3.1 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 DO))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 DI))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 VCC))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x04.wrl
      (at (xyz 0 -0.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (gr_line (start 191.36 104.44) (end 156.67 104.43) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 154.33 102.08) (end 142.18 102.09) (layer Edge.Cuts) (width 0.15))
  (dimension 4.5001 (width 0.3) (layer Dwgs.User)
    (gr_text "4.500 mm" (at 198.080156 106.563464 89.6180338) (layer Dwgs.User))
    (feature1 (pts (xy 192.036394 108.773272) (xy 199.415126 108.822464)))
    (feature2 (pts (xy 192.066394 104.273272) (xy 199.445126 104.322464)))
    (crossbar (pts (xy 196.745186 104.304464) (xy 196.715186 108.804464)))
    (arrow1a (pts (xy 196.715186 108.804464) (xy 196.136288 107.674076)))
    (arrow1b (pts (xy 196.715186 108.804464) (xy 197.309104 107.681895)))
    (arrow2a (pts (xy 196.745186 104.304464) (xy 196.151268 105.427033)))
    (arrow2b (pts (xy 196.745186 104.304464) (xy 197.324084 105.434852)))
  )
  (dimension 7.300438 (width 0.3) (layer Dwgs.User)
    (gr_text "7.300 mm" (at 134.940344 105.601236 89.37212618) (layer Dwgs.User))
    (feature1 (pts (xy 139.35 109.3) (xy 133.550425 109.236443)))
    (feature2 (pts (xy 139.43 102) (xy 133.630425 101.936443)))
    (crossbar (pts (xy 136.330263 101.96603) (xy 136.250263 109.26603)))
    (arrow1a (pts (xy 136.250263 109.26603) (xy 135.676222 108.133168)))
    (arrow1b (pts (xy 136.250263 109.26603) (xy 136.848993 108.14602)))
    (arrow2a (pts (xy 136.330263 101.96603) (xy 135.731533 103.08604)))
    (arrow2b (pts (xy 136.330263 101.96603) (xy 136.904304 103.098892)))
  )
  (gr_line (start 191.4 105.66) (end 191.4 105.67) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 191.4 104.84) (end 191.4 105.66) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 156.67 104.43) (end 154.34 102.09) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 149.34 104.51) (end 143.06 108.71) (angle 52.35226663) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 191.4 109.22) (end 191.4 104.43) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 191.4 105.67) (end 191.4 106.15) (angle 90) (layer Edge.Cuts) (width 0.15))
  (dimension 49.768208 (width 0.3) (layer Dwgs.User)
    (gr_text "49.768 mm" (at 166.615896 91.106) (layer Dwgs.User))
    (feature1 (pts (xy 191.5 105.3) (xy 191.5 89.756)))
    (feature2 (pts (xy 141.731792 105.3) (xy 141.731792 89.756)))
    (crossbar (pts (xy 141.731792 92.456) (xy 191.5 92.456)))
    (arrow1a (pts (xy 191.5 92.456) (xy 190.373496 93.042421)))
    (arrow1b (pts (xy 191.5 92.456) (xy 190.373496 91.869579)))
    (arrow2a (pts (xy 141.731792 92.456) (xy 142.858296 93.042421)))
    (arrow2b (pts (xy 141.731792 92.456) (xy 142.858296 91.869579)))
  )
  (gr_line (start 191.4 108.76) (end 143.06 108.72) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 141.71 101.96) (xy 191.39 101.89) (xy 191.32 109.14) (xy 141.64 109.07) (xy 141.64 101.89)
      )
    )
  )
)
