(kicad_pcb (version 20160815) (host pcbnew "(2016-09-06 BZR 7133, Git df40159)-product")
  (general
    (links 24)
    (no_connects 0)
    (area 170.924999 58.424999 185.075001 100.575001)
    (thickness 1.6)
    (drawings 18)
    (tracks 124)
    (zones 0)
    (modules 15)
    (nets 14)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 1)
    (user_trace_width 0.21)
    (user_trace_width 0.23)
    (user_trace_width 0.35)
    (user_trace_width 0.4)
    (user_trace_width 0.5)
    (user_trace_width 0.8)
    (user_trace_width 1)
    (user_trace_width 1.5)
    (trace_clearance 0.19)
    (zone_clearance 0.2)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 1)
    (via_drill 0.6)
    (via_min_size 0.6)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.3)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.99898 1.99898)
    (pad_drill 1.00076)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010f0_ffffffff)
      (usegerberextensions true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask true)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk true)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "C:/drojf/Dropbox/PCB/PCBS to send out/wakeuplight_torch"))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 "Net-(D1-Pad1)")
  (net 3 "Net-(D2-Pad2)")
  (net 4 "Net-(D2-Pad1)")
  (net 5 "Net-(D3-Pad2)")
  (net 6 "Net-(D3-Pad1)")
  (net 7 "Net-(D4-Pad2)")
  (net 8 "Net-(D4-Pad1)")
  (net 9 /VIN)
  (net 10 /SW)
  (net 11 /FB)
  (net 12 /CTRL)
  (net 13 /VOUT)
  (net_class Default "This is the default net class."
    (clearance 0.19)
    (trace_width 0.25)
    (via_dia 1)
    (via_drill 0.6)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (diff_pair_gap 0.25)
    (diff_pair_width 0.2)
    (add_net /CTRL)
    (add_net /FB)
    (add_net /SW)
    (add_net /VIN)
    (add_net /VOUT)
    (add_net GND)
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D2-Pad1)")
    (add_net "Net-(D2-Pad2)")
    (add_net "Net-(D3-Pad1)")
    (add_net "Net-(D3-Pad2)")
    (add_net "Net-(D4-Pad1)")
    (add_net "Net-(D4-Pad2)")
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM15mm (layer F.Cu) (tedit 569FCEE8)
    (at 183.515 61.2 270)
    (descr "Resistor, Axial, RM 15mm,")
    (tags "Resistor Axial RM 15mm")
    (fp_text reference R1 (at 7.5 -3.74904 270) (layer F.SilkS))
    (fp_text value 10R (at 7.5 4.0005 270) (layer F.Fab))
    (pad 2 thru_hole circle (at 15 0 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 11 /FB))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 1 GND))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM15mm.wrl
      (at (xyz 0.295 0 0))
      (scale (xyz 0.395 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_1206 (layer F.Cu) (tedit 57ABE035)
    (at 175.895 79.52486 90)
    (descr "LED 1206 smd package")
    (tags "LED1206 SMD")
    (attr smd)
    (fp_text reference D1 (at 0 -2 90) (layer F.SilkS))
    (fp_text value LED (at 0 2 90) (layer F.Fab))
    (pad 2 smd rect (at 1.41986 0 270) (size 1.59766 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 13 /VOUT))
    (pad 1 smd rect (at -1.41986 0 270) (size 1.59766 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(D1-Pad1)"))
    (model LEDs.3dshapes/LED_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_1206 (layer F.Cu) (tedit 57ABE035)
    (at 175.895 90.95486 90)
    (descr "LED 1206 smd package")
    (tags "LED1206 SMD")
    (attr smd)
    (fp_text reference D2 (at 0 -2 90) (layer F.SilkS))
    (fp_text value LED (at 0 2 90) (layer F.Fab))
    (pad 2 smd rect (at 1.41986 0 270) (size 1.59766 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(D2-Pad2)"))
    (pad 1 smd rect (at -1.41986 0 270) (size 1.59766 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(D2-Pad1)"))
    (model LEDs.3dshapes/LED_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_1206 (layer F.Cu) (tedit 57ABE035)
    (at 180.975 96.66986 270)
    (descr "LED 1206 smd package")
    (tags "LED1206 SMD")
    (attr smd)
    (fp_text reference D3 (at 0 -2 270) (layer F.SilkS))
    (fp_text value LED (at 0 2 270) (layer F.Fab))
    (pad 2 smd rect (at 1.41986 0 90) (size 1.59766 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(D3-Pad2)"))
    (pad 1 smd rect (at -1.41986 0 90) (size 1.59766 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(D3-Pad1)"))
    (model LEDs.3dshapes/LED_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_1206 (layer F.Cu) (tedit 57ABE035)
    (at 180.975 85.23986 270)
    (descr "LED 1206 smd package")
    (tags "LED1206 SMD")
    (attr smd)
    (fp_text reference D4 (at 0 -2 270) (layer F.SilkS))
    (fp_text value LED (at 0 2 270) (layer F.Fab))
    (pad 2 smd rect (at 1.41986 0 90) (size 1.59766 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(D4-Pad2)"))
    (pad 1 smd rect (at -1.41986 0 90) (size 1.59766 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(D4-Pad1)"))
    (model LEDs.3dshapes/LED_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_1206 (layer F.Cu) (tedit 57ABE035)
    (at 175.895 85.23986 90)
    (descr "LED 1206 smd package")
    (tags "LED1206 SMD")
    (attr smd)
    (fp_text reference D5 (at 0 -2 90) (layer F.SilkS))
    (fp_text value LED (at 0 2 90) (layer F.Fab))
    (pad 2 smd rect (at 1.41986 0 270) (size 1.59766 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(D1-Pad1)"))
    (pad 1 smd rect (at -1.41986 0 270) (size 1.59766 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(D2-Pad2)"))
    (model LEDs.3dshapes/LED_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_1206 (layer F.Cu) (tedit 57ABE035)
    (at 175.895 96.66986 90)
    (descr "LED 1206 smd package")
    (tags "LED1206 SMD")
    (attr smd)
    (fp_text reference D6 (at 0 -2 90) (layer F.SilkS))
    (fp_text value LED (at 0 2 90) (layer F.Fab))
    (pad 2 smd rect (at 1.41986 0 270) (size 1.59766 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(D2-Pad1)"))
    (pad 1 smd rect (at -1.41986 0 270) (size 1.59766 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(D3-Pad2)"))
    (model LEDs.3dshapes/LED_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_1206 (layer F.Cu) (tedit 57ABE035)
    (at 180.975 90.95486 270)
    (descr "LED 1206 smd package")
    (tags "LED1206 SMD")
    (attr smd)
    (fp_text reference D7 (at 0 -2 270) (layer F.SilkS))
    (fp_text value LED (at 0 2 270) (layer F.Fab))
    (pad 2 smd rect (at 1.41986 0 90) (size 1.59766 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(D3-Pad1)"))
    (pad 1 smd rect (at -1.41986 0 90) (size 1.59766 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(D4-Pad2)"))
    (model LEDs.3dshapes/LED_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_1206 (layer F.Cu) (tedit 57ABE035)
    (at 180.975 79.52486 270)
    (descr "LED 1206 smd package")
    (tags "LED1206 SMD")
    (attr smd)
    (fp_text reference D8 (at 0 -2 270) (layer F.SilkS))
    (fp_text value LED (at 0 2 270) (layer F.Fab))
    (pad 2 smd rect (at 1.41986 0 90) (size 1.59766 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(D4-Pad1)"))
    (pad 1 smd rect (at -1.41986 0 90) (size 1.59766 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 11 /FB))
    (model LEDs.3dshapes/LED_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Capacitors_ThroughHole:C_Radial_D5_L11_P2.5 (layer F.Cu) (tedit 58425210)
    (at 173.736 67.223 90)
    (descr "Radial Electrolytic Capacitor Diameter 5mm x Length 11mm, Pitch 2.5mm")
    (tags "Electrolytic Capacitor")
    (fp_text reference C1 (at 4.358 -1.651 -180) (layer F.SilkS))
    (fp_text value CP (at 1.25 3.8 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 /VIN))
    (pad 2 thru_hole circle (at 2.5 0 90) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model Capacitors_ThroughHole.3dshapes/C_Radial_D5_L11_P2.5.wrl
      (at (xyz 0.049213 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module SMD_INDUCTOR_GENERAL:SMD_INDUCTOR (layer F.Cu) (tedit 584251DB)
    (at 185.166 67.183 180)
    (fp_text reference L1 (at 5.461 -1.397 180) (layer F.SilkS))
    (fp_text value 22uH (at 5.461 1.778 270) (layer F.SilkS))
    (pad 2 smd rect (at 8.001 0.508 180) (size 2.5 5.7) (layers F.Cu F.Paste F.Mask)
      (net 9 /VIN))
    (pad 1 smd rect (at 2.921 0.508 180) (size 2.5 5.7) (layers F.Cu F.Paste F.Mask)
      (net 10 /SW))
  )
  (module Capacitors_SMD:C_1206 (layer F.Cu) (tedit 58425158)
    (at 173.887 71.628 180)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C2 (at 0.026644 -1.706249 180) (layer F.SilkS))
    (fp_text value 2.2uF (at 0 2.3 180) (layer F.Fab))
    (pad 1 smd rect (at -1.5 0 180) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 9 /VIN))
    (pad 2 smd rect (at 1.5 0 180) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer F.Cu) (tedit 5842515C)
    (at 173.887 75.438 180)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C3 (at -3.151 0 180) (layer F.SilkS))
    (fp_text value 1uF (at 0 2.3 180) (layer F.Fab))
    (pad 1 smd rect (at -1.5 0 180) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 13 /VOUT))
    (pad 2 smd rect (at 1.5 0 180) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Angled_1x03 (layer F.Cu) (tedit 584250F6)
    (at 175.26 60.96 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P1 (at 1.27 -3.175 180) (layer F.Fab))
    (fp_text value CONN_01X03 (at 0 -3.1 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 9 /VIN))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 12 /CTRL))
    (model Pin_Headers.3dshapes/Pin_Header_Angled_1x03.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Housings_DFN_QFN:DFN-6-1EP_2x2mm_Pitch0.65mm (layer F.Cu) (tedit 54130A77)
    (at 179.705 72.517)
    (descr "6-Lead Plastic Dual Flat, No Lead Package (MA) - 2x2x0.9 mm Body [DFN] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "DFN 0.65")
    (attr smd)
    (fp_text reference U1 (at 0 -2.025) (layer F.SilkS))
    (fp_text value AL3050 (at 0 2.025) (layer F.Fab))
    (pad 1 smd rect (at -1.05 -0.65) (size 0.65 0.35) (layers F.Cu F.Paste F.Mask)
      (net 12 /CTRL))
    (pad 2 smd rect (at -1.05 0) (size 0.65 0.35) (layers F.Cu F.Paste F.Mask)
      (net 9 /VIN))
    (pad 3 smd rect (at -1.05 0.65) (size 0.65 0.35) (layers F.Cu F.Paste F.Mask)
      (net 13 /VOUT))
    (pad 4 smd rect (at 1.05 0.65) (size 0.65 0.35) (layers F.Cu F.Paste F.Mask)
      (net 11 /FB))
    (pad 5 smd rect (at 1.05 0) (size 0.65 0.35) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at 1.05 -0.65) (size 0.65 0.35) (layers F.Cu F.Paste F.Mask)
      (net 10 /SW))
    (pad 7 smd rect (at 0 0.4) (size 1 0.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_paste_margin_ratio -0.2))
    (pad 7 smd rect (at 0 -0.4) (size 1 0.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_paste_margin_ratio -0.2))
    (model Housings_DFN_QFN.3dshapes/DFN-6-1EP_2x2mm_Pitch0.65mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "VCC\nGND\nDIM" (at 177.8 64.77 90) (layer B.SilkS))
  (gr_text 1 (at 177.8 70.612) (layer F.SilkS))
  (gr_text FB (at 184.023 78.105) (layer F.SilkS))
  (gr_text VOUT (at 172.974 78.232) (layer F.SilkS))
  (gr_text > (at 174.879 64.77) (layer F.SilkS))
  (gr_text VCC (at 175.26 62.865) (layer F.SilkS))
  (gr_text GND (at 177.8 62.865) (layer F.SilkS))
  (gr_text DIM (at 180.34 62.865) (layer F.SilkS))
  (gr_text "MINI LED DRIVER\nAL3050" (at 177.927 87.757 270) (layer B.SilkS))
  (dimension 42 (width 0.3) (layer Dwgs.User)
    (gr_text "42.000 mm" (at 167.150001 79.5 270) (layer Dwgs.User))
    (feature1 (pts (xy 171 100.5) (xy 165.800001 100.5)))
    (feature2 (pts (xy 171 58.5) (xy 165.800001 58.5)))
    (crossbar (pts (xy 168.500001 58.5) (xy 168.500001 100.5)))
    (arrow1a (pts (xy 168.500001 100.5) (xy 167.91358 99.373496)))
    (arrow1b (pts (xy 168.500001 100.5) (xy 169.086422 99.373496)))
    (arrow2a (pts (xy 168.500001 58.5) (xy 167.91358 59.626504)))
    (arrow2b (pts (xy 168.500001 58.5) (xy 169.086422 59.626504)))
  )
  (dimension 14 (width 0.3) (layer Dwgs.User)
    (gr_text "14.000 mm" (at 178 45.65) (layer Dwgs.User))
    (feature1 (pts (xy 171 58.5) (xy 171 44.3)))
    (feature2 (pts (xy 185 58.5) (xy 185 44.3)))
    (crossbar (pts (xy 185 47) (xy 171 47)))
    (arrow1a (pts (xy 171 47) (xy 172.126504 46.413579)))
    (arrow1b (pts (xy 171 47) (xy 172.126504 47.586421)))
    (arrow2a (pts (xy 185 47) (xy 183.873496 46.413579)))
    (arrow2b (pts (xy 185 47) (xy 183.873496 47.586421)))
  )
  (gr_line (start 171 100.5) (end 171 58.5) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 185 100.5) (end 171 100.5) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 185 58.5) (end 185 100.5) (layer Edge.Cuts) (width 0.15))
  (dimension 1.905 (width 0.3) (layer Dwgs.User)
    (gr_text "1.905 mm" (at 256.968 62.0395 270) (layer Dwgs.User))
    (feature1 (pts (xy 261.62 62.992) (xy 255.618 62.992)))
    (feature2 (pts (xy 261.62 61.087) (xy 255.618 61.087)))
    (crossbar (pts (xy 258.318 61.087) (xy 258.318 62.992)))
    (arrow1a (pts (xy 258.318 62.992) (xy 257.731579 61.865496)))
    (arrow1b (pts (xy 258.318 62.992) (xy 258.904421 61.865496)))
    (arrow2a (pts (xy 258.318 61.087) (xy 257.731579 62.213504)))
    (arrow2b (pts (xy 258.318 61.087) (xy 258.904421 62.213504)))
  )
  (dimension 1.778 (width 0.3) (layer Dwgs.User)
    (gr_text "1.778 mm" (at 258.746 57.15 270) (layer Dwgs.User))
    (feature1 (pts (xy 261.62 58.039) (xy 257.396 58.039)))
    (feature2 (pts (xy 261.62 56.261) (xy 257.396 56.261)))
    (crossbar (pts (xy 260.096 56.261) (xy 260.096 58.039)))
    (arrow1a (pts (xy 260.096 58.039) (xy 259.509579 56.912496)))
    (arrow1b (pts (xy 260.096 58.039) (xy 260.682421 56.912496)))
    (arrow2a (pts (xy 260.096 56.261) (xy 259.509579 57.387504)))
    (arrow2b (pts (xy 260.096 56.261) (xy 260.682421 57.387504)))
  )
  (dimension 4.699 (width 0.3) (layer Dwgs.User)
    (gr_text "4.699 mm" (at 267.415 59.4995 270) (layer Dwgs.User))
    (feature1 (pts (xy 261.62 61.849) (xy 268.765 61.849)))
    (feature2 (pts (xy 261.62 57.15) (xy 268.765 57.15)))
    (crossbar (pts (xy 266.065 57.15) (xy 266.065 61.849)))
    (arrow1a (pts (xy 266.065 61.849) (xy 265.478579 60.722496)))
    (arrow1b (pts (xy 266.065 61.849) (xy 266.651421 60.722496)))
    (arrow2a (pts (xy 266.065 57.15) (xy 265.478579 58.276504)))
    (arrow2b (pts (xy 266.065 57.15) (xy 266.651421 58.276504)))
  )
  (gr_line (start 185 58.5) (end 171 58.5) (layer Edge.Cuts) (width 0.15))
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.5))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 184.912 100.457) (xy 171.069 100.457) (xy 171.069 58.547) (xy 184.912 58.547)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.5))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 171.069 58.547) (xy 184.912 58.547) (xy 184.912 100.457) (xy 171.069 100.457)
      )
    )
  )
  (zone (net 2) (net_name "Net-(D1-Pad1)") (layer F.Cu) (hatch edge 0.508)
    (priority 2)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 178.181 79.375) (xy 171.45 79.375) (xy 171.45 84.963) (xy 178.181 84.963)
      )
    )
  )
  (zone (net 2) (net_name "Net-(D1-Pad1)") (layer B.Cu) (hatch edge 0.508)
    (priority 2)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 178.181 79.375) (xy 171.45 79.375) (xy 171.45 84.963) (xy 178.181 84.963)
      )
    )
  )
  (zone (net 8) (net_name "Net-(D4-Pad1)") (layer F.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 185.039 79.502) (xy 178.435 79.502) (xy 178.435 84.963) (xy 185.039 84.963)
      )
    )
  )
  (zone (net 8) (net_name "Net-(D4-Pad1)") (layer B.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 185.039 79.502) (xy 178.435 79.502) (xy 178.435 84.963) (xy 185.039 84.963)
      )
    )
  )
  (zone (net 7) (net_name "Net-(D4-Pad2)") (layer F.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 185.039 85.471) (xy 178.435 85.471) (xy 178.435 90.678) (xy 185.039 90.678)
      )
    )
  )
  (zone (net 3) (net_name "Net-(D2-Pad2)") (layer F.Cu) (hatch edge 0.508)
    (priority 2)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 178.181 85.344) (xy 171.45 85.344) (xy 171.45 90.678) (xy 178.181 90.678)
      )
    )
  )
  (zone (net 3) (net_name "Net-(D2-Pad2)") (layer B.Cu) (hatch edge 0.508)
    (priority 2)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 178.181 85.344) (xy 171.45 85.344) (xy 171.45 90.678) (xy 178.181 90.678)
      )
    )
  )
  (zone (net 7) (net_name "Net-(D4-Pad2)") (layer B.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 185.039 85.471) (xy 178.435 85.471) (xy 178.435 90.678) (xy 185.039 90.678)
      )
    )
  )
  (zone (net 4) (net_name "Net-(D2-Pad1)") (layer F.Cu) (hatch edge 0.508)
    (priority 2)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 178.181 91.186) (xy 171.45 91.186) (xy 171.45 96.52) (xy 178.181 96.52)
      )
    )
  )
  (zone (net 6) (net_name "Net-(D3-Pad1)") (layer F.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 185.039 91.313) (xy 178.435 91.313) (xy 178.435 96.52) (xy 185.039 96.52)
      )
    )
  )
  (zone (net 6) (net_name "Net-(D3-Pad1)") (layer B.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 185.039 91.313) (xy 178.435 91.313) (xy 178.435 96.52) (xy 185.039 96.52)
      )
    )
  )
  (zone (net 4) (net_name "Net-(D2-Pad1)") (layer B.Cu) (hatch edge 0.508)
    (priority 2)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 178.181 91.186) (xy 171.45 91.186) (xy 171.45 96.52) (xy 178.181 96.52)
      )
    )
  )
  (zone (net 5) (net_name "Net-(D3-Pad2)") (layer F.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 171.45 97.155) (xy 184.912 97.155) (xy 184.912 100.3935) (xy 171.45 100.33)
      )
    )
  )
  (zone (net 5) (net_name "Net-(D3-Pad2)") (layer B.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 171.45 97.155) (xy 185.039 97.155) (xy 185.039 100.394155) (xy 171.45 100.330655)
      )
    )
  )
  (zone (net 13) (net_name /VOUT) (layer F.Cu) (hatch edge 0.508)
    (priority 2)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 171.45 79.121) (xy 178.181 79.0575) (xy 178.054 74.93) (xy 177.165 73.406) (xy 174.371 73.406)
        (xy 174.371 76.835) (xy 171.45 76.835)
      )
    )
  )
  (zone (net 11) (net_name /FB) (layer F.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 178.435 79.121) (xy 185.039 79.121) (xy 185.039 74.295) (xy 183.896 74.295) (xy 182.372 72.898)
        (xy 182.118 73.406) (xy 181.991 74.295)
      )
    )
  )
  (zone (net 11) (net_name /FB) (layer B.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 178.435 79.121) (xy 185.039 79.121) (xy 185.039 74.295) (xy 181.991 74.295)
      )
    )
  )
  (zone (net 9) (net_name /VIN) (layer F.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 176.276 69.088) (xy 178.308 69.088) (xy 178.308 69.596) (xy 176.276 71.12) (xy 176.276 72.644)
        (xy 174.498 73.025) (xy 174.498 70.485) (xy 175.895 69.85)
      )
    )
  )
)
