(kicad_pcb
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(31 "B.Cu" signal)
		(32 "B.Adhes" user "B.Adhesive")
		(33 "F.Adhes" user "F.Adhesive")
		(34 "B.Paste" user)
		(35 "F.Paste" user)
		(36 "B.SilkS" user "B.Silkscreen")
		(37 "F.SilkS" user "F.Silkscreen")
		(38 "B.Mask" user)
		(39 "F.Mask" user)
		(40 "Dwgs.User" user "User.Drawings")
		(41 "Cmts.User" user "User.Comments")
		(42 "Eco1.User" user "User.Eco1")
		(43 "Eco2.User" user "User.Eco2")
		(44 "Edge.Cuts" user)
		(45 "Margin" user)
		(46 "B.CrtYd" user "B.Courtyard")
		(47 "F.CrtYd" user "F.Courtyard")
		(48 "B.Fab" user)
		(49 "F.Fab" user)
		(50 "User.1" user)
		(51 "User.2" user)
		(52 "User.3" user)
		(53 "User.4" user)
		(54 "User.5" user)
		(55 "User.6" user)
		(56 "User.7" user)
		(57 "User.8" user)
		(58 "User.9" user)
	)
	(setup
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(pcbplotparams
			(layerselection 0x00010fc_ffffffff)
			(plot_on_all_layers_selection 0x0000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(viasonmask no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plotreference yes)
			(plotvalue yes)
			(plotfptext yes)
			(plotinvisibletext no)
			(sketchpadsonfab no)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 1)
			(scaleselection 1)
			(outputdirectory "")
		)
	)
	(net 0 "")
	(net 1 "GND")
	(net 2 "Net-(J3-Pin_1)")
	(net 3 "Net-(J4-In)")
	(net 4 "Net-(JP1-A)")
	(net 5 "Net-(JP1-B)")
	(net 6 "Net-(JP2-B)")
	(net 7 "Net-(Q1-B)")
	(net 8 "Net-(Q3-B)")
	(net 9 "Net-(Q4-B)")
	(net 10 "Net-(Q5-G)")
	(net 11 "Net-(D1-K)")
	(net 12 "Net-(D1-A)")
	(footprint "Capacitor_THT:CP_Radial_D6.3mm_P2.50mm"
		(layer "F.Cu")
		(at 187 85.5 90)
		(descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=6.3mm, Electrolytic Capacitor")
		(tags "CP Radial series Radial pin pitch 2.50mm  diameter 6.3mm Electrolytic Capacitor")
		(property "Reference" "C3"
			(at -3 0 180)
			(layer "F.SilkS")
		)
		(property "Value" "100µF"
			(at 1.25 4.4 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_THT:CP_Radial_D6.3mm_P2.50mm"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "ESK107M025AE3EA"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Polarized capacitor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "CP_*")
		(sheetname "Root")
		(sheetfile "DriverBoard.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.25 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "Net-(D1-K)")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.5 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_D6.3mm_P2.50mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
		(layer "F.Cu")
		(at 181 93.58 90)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R8"
			(at 5.08 2.5 180)
			(layer "F.SilkS")
		)
		(property "Value" "R"
			(at 5.08 2.37 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "DriverBoard.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 5.08 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 10.16 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "Net-(D1-K)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_THT:TO-92L_Inline_Wide"
		(layer "F.Cu")
		(at 154.5 96.92 -90)
		(descr "TO-92L leads in-line (large body variant of TO-92), also known as TO-226, wide, drill 0.75mm (see https://www.diodes.com/assets/Package-Files/TO92L.pdf and http://www.ti.com/lit/an/snoa059/snoa059.pdf)")
		(tags "TO-92L Inline Wide transistor")
		(property "Reference" "Q3"
			(at 2.58 2.5 -90)
			(layer "F.SilkS")
		)
		(property "Value" "BC547B"
			(at 2.54 2.79 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-92L_Inline_Wide"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "NPN transistor, collector/base/emitter"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "DriverBoard.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.54 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 270)
			(size 1.5 1.5)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "Net-(Q1-B)")
			(pinfunction "C")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.54 0 270)
			(size 1.5 1.5)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "Net-(Q3-B)")
			(pinfunction "B")
			(pintype "input")
		)
		(pad "3" thru_hole circle
			(at 5.08 0 270)
			(size 1.5 1.5)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "E")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-92L_Inline_Wide.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Library:Connector_banana"
		(layer "F.Cu")
		(at 201 75 180)
		(property "Reference" "J1"
			(at 0 -0.5 180)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Power +"
			(at 0 1 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" "Library:Connector_banana"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x01, script generated"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "Root")
		(sheetfile "DriverBoard.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 2.5 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at -7.5 0 180)
			(size 3 3)
			(drill 2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "Net-(D1-K)")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "1" thru_hole circle
			(at 10.5 0 180)
			(size 3 3)
			(drill 2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "Net-(D1-K)")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 168.96 102 90)
		(descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x02 2.54mm single row")
		(property "Reference" "JP1"
			(at 0 -2.33 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Jumper_2_Open"
			(at 0 4.87 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Jumper, 2-pole, open"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Jumper* TestPoint*2Pads* TestPoint*Bridge*")
		(sheetname "Root")
		(sheetfile "DriverBoard.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 1.27 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "Net-(JP1-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 2.54 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "Net-(JP1-B)")
			(pinfunction "B")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_THT:CP_Radial_D6.3mm_P2.50mm"
		(layer "F.Cu")
		(at 187 92 -90)
		(descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=6.3mm, Electrolytic Capacitor")
		(tags "CP Radial series Radial pin pitch 2.50mm  diameter 6.3mm Electrolytic Capacitor")
		(property "Reference" "C2"
			(at 5.5 0 180)
			(layer "F.SilkS")
		)
		(property "Value" "100µF"
			(at 1.25 4.4 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_THT:CP_Radial_D6.3mm_P2.50mm"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "ESK107M025AE3EA"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Polarized capacitor"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "CP_*")
		(sheetname "Root")
		(sheetfile "DriverBoard.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.25 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "Net-(D1-K)")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.5 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_D6.3mm_P2.50mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x01_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 169 121.5)
		(descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x01 2.54mm single row")
		(property "Reference" "TP1"
			(at 0 -2.33 0)
			(layer "F.SilkS")
		)
		(property "Value" "TestPoint"
			(at 0 2.33 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_PinHeader_2.54mm:PinHeader_1x01_P2.54mm_Vertical"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "Root")
		(sheetfile "DriverBoard.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "Net-(JP1-A)")
			(pinfunction "1")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_THT:TO-92L_Inline_Wide"
		(layer "F.Cu")
		(at 146.5 96.96 -90)
		(descr "TO-92L leads in-line (large body variant of TO-92), also known as TO-226, wide, drill 0.75mm (see https://www.diodes.com/assets/Package-Files/TO92L.pdf and http://www.ti.com/lit/an/snoa059/snoa059.pdf)")
		(tags "TO-92L Inline Wide transistor")
		(property "Reference" "Q4"
			(at 2.54 2.5 -90)
			(layer "F.SilkS")
		)
		(property "Value" "BC547B"
			(at 2.54 2.79 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-92L_Inline_Wide"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "NPN transistor, collector/base/emitter"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "DriverBoard.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.54 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 270)
			(size 1.5 1.5)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "Net-(Q3-B)")
			(pinfunction "C")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.54 0 270)
			(size 1.5 1.5)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "Net-(Q4-B)")
			(pinfunction "B")
			(pintype "input")
		)
		(pad "3" thru_hole circle
			(at 5.08 0 270)
			(size 1.5 1.5)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "E")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-92L_Inline_Wide.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 168.96 107 90)
		(descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x02 2.54mm single row")
		(property "Reference" "JP2"
			(at -3 1.04 180)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Jumper_2_Open"
			(at 0 4.87 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Jumper, 2-pole, open"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Jumper* TestPoint*2Pads* TestPoint*Bridge*")
		(sheetname "Root")
		(sheetfile "DriverBoard.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 1.27 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "Net-(JP1-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 2.54 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "Net-(JP2-B)")
			(pinfunction "B")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
		(layer "F.Cu")
		(at 176.84 102)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R5"
			(at 5.16 -2 0)
			(layer "F.SilkS")
		)
		(property "Value" "R"
			(at 5.08 2.37 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "DriverBoard.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 5.08 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "Net-(JP1-B)")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 10.16 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "Net-(Q5-G)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x01_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 209.5 97)
		(descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x01 2.54mm single row")
		(property "Reference" "TP4"
			(at -3 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "TestPoint"
			(at 0 2.33 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_PinHeader_2.54mm:PinHeader_1x01_P2.54mm_Vertical"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "Root")
		(sheetfile "DriverBoard.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "Net-(D1-A)")
			(pinfunction "1")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_Coaxial:BNC_TEConnectivity_1478204_Vertical"
		(layer "F.Cu")
		(at 135.5 115.5)
		(descr "BNC female PCB mount 4 pin straight chassis connector http://www.te.com/usa-en/product-1-1478204-0.html")
		(tags "BNC female PCB mount 4 pin straight chassis connector ")
		(property "Reference" "J4"
			(at -0.25 -6.25 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Conn_Coaxial"
			(at 0 6.5 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_Coaxial:BNC_TEConnectivity_1478204_Vertical"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "coaxial connector (BNC, SMA, SMB, SMC, Cinch/RCA, LEMO, ...)"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*BNC* *SMA* *SMB* *SMC* *Cinch* *LEMO* *UMRF* *MCX* *U.FL*")
		(sheetname "Root")
		(sheetfile "DriverBoard.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 3.556 3.556)
			(drill 1.27)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "Net-(J4-In)")
			(pinfunction "In")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at -3.175 -3.175)
			(size 3.81 3.81)
			(drill 1.524)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at -3.175 3.175)
			(size 3.81 3.81)
			(drill 1.524)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 3.175 -3.175)
			(size 3.81 3.81)
			(drill 1.524)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 3.175 3.175)
			(size 3.81 3.81)
			(drill 1.524)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_Coaxial.3dshapes/BNC_TEConnectivity_1478204_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_THT:CP_Radial_D6.3mm_P2.50mm"
		(layer "F.Cu")
		(at 162 87.5)
		(descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=6.3mm, Electrolytic Capacitor")
		(tags "CP Radial series Radial pin pitch 2.50mm  diameter 6.3mm Electrolytic Capacitor")
		(property "Reference" "C1"
			(at 1 4.5 180)
			(layer "F.SilkS")
		)
		(property "Value" "C"
			(at 1.25 4.4 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_THT:CP_Radial_D6.3mm_P2.50mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "DriverBoard.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.25 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "Net-(J3-Pin_1)")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.5 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_D6.3mm_P2.50mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Library:Connector_banana"
		(layer "F.Cu")
		(at 138.5 75)
		(property "Reference" "J3"
			(at 0 -0.5 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "V_Drive"
			(at 0 1 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" "Library:Connector_banana"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x01, script generated"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "Root")
		(sheetfile "DriverBoard.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 2.5 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at -7.5 0)
			(size 3 3)
			(drill 2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "Net-(J3-Pin_1)")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "1" thru_hole circle
			(at 10.5 0)
			(size 3 3)
			(drill 2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "Net-(J3-Pin_1)")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
	)
	(footprint "Package_TO_SOT_THT:TO-220-3_Horizontal_TabDown"
		(layer "F.Cu")
		(at 191 101.96 -90)
		(descr "TO-220-3, Horizontal, RM 2.54mm, see https://www.vishay.com/docs/66542/to-220-1.pdf")
		(tags "TO-220-3 Horizontal RM 2.54mm")
		(property "Reference" "Q5"
			(at 8.54 -9.23 180)
			(layer "F.SilkS")
		)
		(property "Value" "IRF610PBF"
			(at 2.54 2 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-3_Horizontal_TabDown"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "P-MOSFET transistor, gate/drain/source"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "DriverBoard.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.54 -20.58 90)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole oval
			(at 2.54 -16.66 270)
			(size 3.5 3.5)
			(drill 3.5)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" thru_hole rect
			(at 0 0 270)
			(size 1.905 2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "Net-(Q5-G)")
			(pinfunction "G")
			(pintype "input")
		)
		(pad "2" thru_hole oval
			(at 2.54 0 270)
			(size 1.905 2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "Net-(D1-A)")
			(pinfunction "D")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 5.08 0 270)
			(size 1.905 2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "S")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-220-3_Horizontal_TabDown.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_THT:TO-92L_Inline_Wide"
		(layer "F.Cu")
		(at 162 104.5 -90)
		(descr "TO-92L leads in-line (large body variant of TO-92), also known as TO-226, wide, drill 0.75mm (see https://www.diodes.com/assets/Package-Files/TO92L.pdf and http://www.ti.com/lit/an/snoa059/snoa059.pdf)")
		(tags "TO-92L Inline Wide transistor")
		(property "Reference" "Q1"
			(at 2.5 2.5 -90)
			(layer "F.SilkS")
		)
		(property "Value" "BC557B"
			(at 2.54 2.79 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-92L_Inline_Wide"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "PNP transistor, collector/base/emitter"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "DriverBoard.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.54 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 270)
			(size 1.5 1.5)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "C")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.54 0 270)
			(size 1.5 1.5)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "Net-(Q1-B)")
			(pinfunction "B")
			(pintype "input")
		)
		(pad "3" thru_hole circle
			(at 5.08 0 270)
			(size 1.5 1.5)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "Net-(JP1-A)")
			(pinfunction "E")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-92L_Inline_Wide.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TerminalBlock_Phoenix:TerminalBlock_Phoenix_MKDS-1,5-2-5.08_1x02_P5.08mm_Horizontal"
		(layer "F.Cu")
		(at 206.305 92.045 90)
		(descr "Terminal Block Phoenix MKDS-1,5-2-5.08, 2 pins, pitch 5.08mm, size 10.2x9.8mm^2, drill diamater 1.3mm, pad diameter 2.6mm, see http://www.farnell.com/datasheets/100425.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix")
		(tags "THT Terminal Block Phoenix MKDS-1,5-2-5.08 pitch 5.08mm size 10.2x9.8mm^2 drill 1.3mm pad 2.6mm")
		(property "Reference" "J5"
			(at 2.54 -6.26 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Terminals"
			(at 2.54 5.66 90)
			(layer "F.Fab")
		)
		(property "Footprint" "TerminalBlock_Phoenix:TerminalBlock_Phoenix_MKDS-1,5-2-5.08_1x02_P5.08mm_Horizontal"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x02, script generated"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "Root")
		(sheetfile "DriverBoard.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.54 3.2 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 2.6 2.6)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "Net-(D1-A)")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 5.08 0 90)
			(size 2.6 2.6)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "Net-(D1-K)")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/TerminalBlock_Phoenix.3dshapes/TerminalBlock_Phoenix_MKDS-1,5-2-5.08_1x02_P5.08mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
		(layer "F.Cu")
		(at 176.84 107)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R6"
			(at 5.16 -2 0)
			(layer "F.SilkS")
		)
		(property "Value" "R"
			(at 5.08 2.37 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "DriverBoard.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 5.08 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "Net-(JP2-B)")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 10.16 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "Net-(Q5-G)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x01_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 184.5 121.5)
		(descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x01 2.54mm single row")
		(property "Reference" "TP2"
			(at 0 -2.33 0)
			(layer "F.SilkS")
		)
		(property "Value" "TestPoint"
			(at 0 2.33 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_PinHeader_2.54mm:PinHeader_1x01_P2.54mm_Vertical"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "Root")
		(sheetfile "DriverBoard.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "Net-(Q5-G)")
			(pinfunction "1")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x01_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 146 121.5)
		(descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x01 2.54mm single row")
		(property "Reference" "TP3"
			(at 0 -2.33 0)
			(layer "F.SilkS")
		)
		(property "Value" "TestPoint"
			(at 0 2.33 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_PinHeader_2.54mm:PinHeader_1x01_P2.54mm_Vertical"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "Root")
		(sheetfile "DriverBoard.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "Net-(J4-In)")
			(pinfunction "1")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
		(layer "F.Cu")
		(at 146.5 92.5 90)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R2"
			(at 5 2.5 180)
			(layer "F.SilkS")
		)
		(property "Value" "4k7"
			(at 5.08 2.37 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "DriverBoard.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 5.08 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "Net-(Q3-B)")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 10.16 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "Net-(J3-Pin_1)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_THT:TO-92L_Inline_Wide"
		(layer "F.Cu")
		(at 162 96.92 -90)
		(descr "TO-92L leads in-line (large body variant of TO-92), also known as TO-226, wide, drill 0.75mm (see https://www.diodes.com/assets/Package-Files/TO92L.pdf and http://www.ti.com/lit/an/snoa059/snoa059.pdf)")
		(tags "TO-92L Inline Wide transistor")
		(property "Reference" "Q2"
			(at 2.58 2.5 -90)
			(layer "F.SilkS")
		)
		(property "Value" "BC547B"
			(at 2.54 2.79 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-92L_Inline_Wide"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "NPN transistor, collector/base/emitter"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "DriverBoard.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.54 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 270)
			(size 1.5 1.5)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "Net-(J3-Pin_1)")
			(pinfunction "C")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.54 0 270)
			(size 1.5 1.5)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "Net-(Q1-B)")
			(pinfunction "B")
			(pintype "input")
		)
		(pad "3" thru_hole circle
			(at 5.08 0 270)
			(size 1.5 1.5)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "Net-(JP1-A)")
			(pinfunction "E")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-92L_Inline_Wide.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
		(layer "F.Cu")
		(at 145.84 107)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R4"
			(at 5.16 -2 0)
			(layer "F.SilkS")
		)
		(property "Value" "4k7"
			(at 5.08 2.37 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "DriverBoard.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 5.08 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 10.16 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "Net-(JP1-A)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
		(layer "F.Cu")
		(at 154.5 92.5 90)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R3"
			(at 5 2.5 180)
			(layer "F.SilkS")
		)
		(property "Value" "4k7"
			(at 5.08 2.37 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "DriverBoard.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 5.08 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "Net-(Q1-B)")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 10.16 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "Net-(J3-Pin_1)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Library:Connector_banana"
		(layer "F.Cu")
		(at 201 118 180)
		(property "Reference" "J2"
			(at 0 -0.5 180)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Power -"
			(at 0 1 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" "Library:Connector_banana"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x01, script generated"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "Root")
		(sheetfile "DriverBoard.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 2.5 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at -7.5 0 180)
			(size 3 3)
			(drill 2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "1" thru_hole circle
			(at 10.5 0 180)
			(size 3 3)
			(drill 2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
	)
	(footprint "Diode_THT:D_5W_P12.70mm_Horizontal"
		(layer "F.Cu")
		(at 195.5 82.65 -90)
		(descr "Diode, 5W series, Axial, Horizontal, pin pitch=12.7mm, , length*diameter=8.9*3.7mm^2, , http://www.diodes.com/_files/packages/8686949.gif")
		(tags "Diode 5W series Axial Horizontal pin pitch 12.7mm  length 8.9mm diameter 3.7mm")
		(property "Reference" "D1"
			(at 6.35 -2.97 180)
			(layer "F.SilkS")
		)
		(property "Value" "D"
			(at 6.35 2.97 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Diode_THT:D_5W_P12.70mm_Horizontal"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Diode"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" "D"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TO-???* *_Diode_* *SingleDiode* D_*")
		(sheetname "Root")
		(sheetfile "DriverBoard.kicad_sch")
		(attr through_hole)
		(fp_text user "K"
			(at 0 -2.4 90)
			(layer "F.SilkS")
		)
		(fp_text user "${REFERENCE}"
			(at 7.0175 0 90)
			(layer "F.Fab")
		)
		(fp_text user "K"
			(at 0 -2.4 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 270)
			(size 2.8 2.8)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "Net-(D1-K)")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 12.7 0 270)
			(size 2.8 2.8)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "Net-(D1-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Diode_THT.3dshapes/D_5W_P12.70mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
		(layer "F.Cu")
		(at 135.5 96.5 -90)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R1"
			(at 5.08 -2.37 180)
			(layer "F.SilkS")
		)
		(property "Value" "4k7"
			(at 5.08 2.37 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "DriverBoard.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 5.08 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "Net-(Q4-B)")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 10.16 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "Net-(J4-In)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(gr_line
		(start 129 69)
		(end 210 69)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 129 124)
		(mid 127.585786 123.414214)
		(end 127 122)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 127 122)
		(end 127 71)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 210 69)
		(mid 211.414214 69.585786)
		(end 212 71)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 212 71)
		(end 212 122)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 127 71)
		(mid 127.585786 69.585786)
		(end 129 69)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 210 124)
		(end 129 124)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 212 122)
		(mid 211.414214 123.414214)
		(end 210 124)
		(layer "Edge.Cuts")
	)
	(gr_text "V_DRIVER\n0-18V"
		(at 151 77 0)
		(layer "F.SilkS")
	)
	(gr_text "Rg-LOW"
		(at 167 99.5 0)
		(layer "F.SilkS")
	)
	(gr_text "GND_PLANE"
		(at 157.5 117.5 0)
		(layer "F.SilkS")
	)
	(gr_text "MOSFET driver V1.2\nexperiment board\n-> Variable R_g\n-> Variable V_drv\n\n2024\nhackaday.io/voltweasel"
		(at 128 92 0)
		(layer "F.SilkS")
	)
	(gr_text "TRIGGER\n0-5V"
		(at 141 115 0)
		(layer "F.SilkS")
	)
	(gr_text "GND"
		(at 188.5 116 0)
		(layer "F.SilkS")
	)
	(gr_text "V_Load\n0-24V"
		(at 188 77 0)
		(layer "F.SilkS")
	)
	(gr_text "Rg-HIGH"
		(at 167 111 0)
		(layer "F.SilkS")
	)
	(zone
		(net 11)
		(net_name "Net-(D1-K)")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 5)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 1)
		)
		(polygon
			(pts
				(xy 188.5 69.5) (xy 187.5 70.5) (xy 187.5 78.5) (xy 186.5 79.5) (xy 180 79.5) (xy 179 80.5) (xy 179 87)
				(xy 185 93) (xy 189 93) (xy 192.5 89) (xy 210.5 89) (xy 211.5 88) (xy 211.5 70.5) (xy 210.5 69.5)
			)
		)
	)
	(zone
		(net 1)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.1)
		(priority 1)
		(connect_pads
			(clearance 1)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 210.5 69.5) (xy 211.5 70.5) (xy 211.5 122.5) (xy 210.5 123.5) (xy 128.5 123.5) (xy 127.5 122.5)
				(xy 127.5 70.5) (xy 128.5 69.5)
			)
		)
	)
	(zone
		(net 12)
		(net_name "Net-(D1-A)")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 3)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 1)
		)
		(polygon
			(pts
				(xy 210.5 90) (xy 211.5 91) (xy 211.5 104.5) (xy 210.5 105.5) (xy 193.5 105.5) (xy 193 105.5) (xy 192.5 105.5)
				(xy 190.5 105.5) (xy 189.5 104.5) (xy 189.5 94) (xy 193.5 90)
			)
		)
	)
	(zone
		(net 1)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.1)
		(priority 1)
		(connect_pads
			(clearance 1)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 210.5 69.5) (xy 211.5 70.5) (xy 211.5 122.5) (xy 210.5 123.5) (xy 128.5 123.5) (xy 127.5 122.5)
				(xy 127.5 70.5) (xy 128.5 69.5)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "B.Mask")
		(hatch edge 0.1)
		(priority 1)
		(connect_pads
			(clearance 1)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 150 123.5) (xy 165 123.5) (xy 165 122.5) (xy 165 119.5) (xy 164 118.5) (xy 151 118.5) (xy 150 119.5)
				(xy 150 122.5)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "F.Mask")
		(hatch edge 0.1)
		(priority 1)
		(connect_pads
			(clearance 1)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 150 123.5) (xy 165 123.5) (xy 165 122.5) (xy 165 119.5) (xy 164 118.5) (xy 151 118.5) (xy 150 119.5)
				(xy 150 122.5)
			)
		)
	)
)
