(kicad_pcb (version 20171130) (host pcbnew "(5.1.4)-1")
  (general
    (thickness 1.6)
    (drawings 10)
    (tracks 572)
    (zones 0)
    (modules 53)
    (nets 69)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (1 In1.Cu signal)
    (2 In2.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user hide)
    (33 F.Adhes user)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user hide)
    (39 F.Mask user hide)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user hide)
    (45 Margin user hide)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.3)
    (user_trace_width 0.4)
    (user_trace_width 0.6)
    (user_trace_width 0.8)
    (user_trace_width 1)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (user_via 0.6 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.2 1.2)
    (pad_drill 1.2)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 110.236 92.837)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x310fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "gerber-v4-1"))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 GNDA)
  (net 3 555)
  (net 4 +5V)
  (net 5 +5VA)
  (net 6 "Net-(U1-Pad1)")
  (net 7 "Net-(U1-Pad8)")
  (net 8 "Net-(U1-Pad20)")
  (net 9 TX0)
  (net 10 "Net-(U1-Pad22)")
  (net 11 "Net-(U1-Pad25)")
  (net 12 "Net-(U1-Pad26)")
  (net 13 "Net-(U1-Pad28)")
  (net 14 "Net-(U1-Pad36)")
  (net 15 "Net-(U1-Pad37)")
  (net 16 "Net-(U1-Pad38)")
  (net 17 "Net-(U1-Pad39)")
  (net 18 "Net-(U1-Pad40)")
  (net 19 "Net-(U1-Pad41)")
  (net 20 "Net-(U1-Pad42)")
  (net 21 "Net-(D1-Pad3)")
  (net 22 "Net-(D1-Pad2)")
  (net 23 "Net-(D2-Pad2)")
  (net 24 "Net-(D2-Pad3)")
  (net 25 ISO_OUT)
  (net 26 PC7)
  (net 27 PB6)
  (net 28 PC6)
  (net 29 PB5)
  (net 30 PD7)
  (net 31 PD0)
  (net 32 "Net-(F1-Pad2)")
  (net 33 "Net-(VR1-PadMP2)")
  (net 34 "Net-(VR1-PadMP1)")
  (net 35 "Net-(C5-Pad2)")
  (net 36 "Net-(C6-Pad1)")
  (net 37 "Net-(C7-Pad1)")
  (net 38 "Net-(C8-Pad1)")
  (net 39 "Net-(J1-PadB5)")
  (net 40 "Net-(J1-PadA6)")
  (net 41 "Net-(J1-PadA8)")
  (net 42 "Net-(J1-PadA5)")
  (net 43 "Net-(J1-PadB8)")
  (net 44 "Net-(J1-PadA7)")
  (net 45 "Net-(J1-PadS1)")
  (net 46 "Net-(J4-Pad2)")
  (net 47 "Net-(R6-Pad2)")
  (net 48 "Net-(U2-Pad5)")
  (net 49 "Net-(RN2-Pad6)")
  (net 50 "Net-(VR1-Pad3)")
  (net 51 "Net-(VR1-Pad5)")
  (net 52 RESET)
  (net 53 MOSI)
  (net 54 SCK)
  (net 55 MISO)
  (net 56 "Net-(D1-Pad4)")
  (net 57 "Net-(D2-Pad4)")
  (net 58 "Net-(J2-Pad3)")
  (net 59 "Net-(J3-Pad3)")
  (net 60 "Net-(J4-Pad3)")
  (net 61 "Net-(C9-Pad1)")
  (net 62 "Net-(C13-Pad2)")
  (net 63 "Net-(C13-Pad1)")
  (net 64 "Net-(R3-Pad1)")
  (net 65 "Net-(R4-Pad1)")
  (net 66 "Net-(R7-Pad2)")
  (net 67 "Net-(R8-Pad2)")
  (net 68 "Net-(RN2-Pad3)")
  (net_class Default "Dies ist die voreingestellte Netzklasse."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +5V)
    (add_net +5VA)
    (add_net 555)
    (add_net GND)
    (add_net GNDA)
    (add_net ISO_OUT)
    (add_net MISO)
    (add_net MOSI)
    (add_net "Net-(C13-Pad1)")
    (add_net "Net-(C13-Pad2)")
    (add_net "Net-(C5-Pad2)")
    (add_net "Net-(C6-Pad1)")
    (add_net "Net-(C7-Pad1)")
    (add_net "Net-(C8-Pad1)")
    (add_net "Net-(C9-Pad1)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D1-Pad3)")
    (add_net "Net-(D1-Pad4)")
    (add_net "Net-(D2-Pad2)")
    (add_net "Net-(D2-Pad3)")
    (add_net "Net-(D2-Pad4)")
    (add_net "Net-(F1-Pad2)")
    (add_net "Net-(J1-PadA5)")
    (add_net "Net-(J1-PadA6)")
    (add_net "Net-(J1-PadA7)")
    (add_net "Net-(J1-PadA8)")
    (add_net "Net-(J1-PadB5)")
    (add_net "Net-(J1-PadB8)")
    (add_net "Net-(J1-PadS1)")
    (add_net "Net-(J2-Pad3)")
    (add_net "Net-(J3-Pad3)")
    (add_net "Net-(J4-Pad2)")
    (add_net "Net-(J4-Pad3)")
    (add_net "Net-(R3-Pad1)")
    (add_net "Net-(R4-Pad1)")
    (add_net "Net-(R6-Pad2)")
    (add_net "Net-(R7-Pad2)")
    (add_net "Net-(R8-Pad2)")
    (add_net "Net-(RN2-Pad3)")
    (add_net "Net-(RN2-Pad6)")
    (add_net "Net-(U1-Pad1)")
    (add_net "Net-(U1-Pad20)")
    (add_net "Net-(U1-Pad22)")
    (add_net "Net-(U1-Pad25)")
    (add_net "Net-(U1-Pad26)")
    (add_net "Net-(U1-Pad28)")
    (add_net "Net-(U1-Pad36)")
    (add_net "Net-(U1-Pad37)")
    (add_net "Net-(U1-Pad38)")
    (add_net "Net-(U1-Pad39)")
    (add_net "Net-(U1-Pad40)")
    (add_net "Net-(U1-Pad41)")
    (add_net "Net-(U1-Pad42)")
    (add_net "Net-(U1-Pad8)")
    (add_net "Net-(U2-Pad5)")
    (add_net "Net-(VR1-Pad3)")
    (add_net "Net-(VR1-Pad5)")
    (add_net "Net-(VR1-PadMP1)")
    (add_net "Net-(VR1-PadMP2)")
    (add_net PB5)
    (add_net PB6)
    (add_net PC6)
    (add_net PC7)
    (add_net PD0)
    (add_net PD7)
    (add_net RESET)
    (add_net SCK)
    (add_net TX0)
  )
  (module ADUM5028-5BRIZ:SOIC127P1031X265-8N (layer F.Cu) (tedit 60D2FD49)
    (at 145.9738 112.5982)
    (attr smd)
    (fp_text reference U3 (at 0.2032 -4.1402) (layer F.SilkS))
    (fp_text value ADUM5028-5BRIZ-ADUM5028-5BRIZ-midi-biodata-esp32_rev4-iso-sensor-rescue (at -2.175 3.837) (layer F.SilkS) hide)
    (pad 8 smd rect (at 4.84 -1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 63 "Net-(C13-Pad1)"))
    (pad 7 smd rect (at 4.84 -0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 62 "Net-(C13-Pad2)"))
    (pad 6 smd rect (at 4.84 0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 63 "Net-(C13-Pad1)"))
    (pad 5 smd rect (at 4.84 1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 62 "Net-(C13-Pad2)"))
    (pad 4 smd rect (at -4.84 1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -4.84 0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 4 +5V))
    (pad 2 smd rect (at -4.84 -0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -4.84 -1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -4.825 -3.175) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 0 smd rect (at -4.825 -4.425) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask))
    (pad 5 smd rect (at 4.85 -3.15) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 62 "Net-(C13-Pad2)"))
    (pad 0 smd rect (at 4.85 -4.4) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask))
    (pad 0 smd rect (at 4.85 3.15) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask))
    (pad 5 smd rect (at 4.85 4.4) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 62 "Net-(C13-Pad2)"))
    (pad 1 smd rect (at -4.825 4.425) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 0 smd rect (at -4.825 3.175) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask))
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 157.59962 100.23348)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C15 (at -0.21106 1.63576) (layer F.SilkS))
    (fp_text value 4.7uF (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GNDA))
    (pad 1 smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 +5VA))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SamacSys_Parts:RK14J12R0A0C (layer B.Cu) (tedit 60BF38F7)
    (at 139.6238 118.3386)
    (descr RK14J12R0A0C-7)
    (tags "Variable Resistor")
    (attr smd)
    (fp_text reference VR1 (at -0.0254 -8.255) (layer B.SilkS))
    (fp_text value RK14J12R0A0C (at -0.375 -2.35) (layer B.SilkS) hide)
    (fp_text user %R (at 0 -0.35) (layer B.Fab))
    (pad MP2 smd rect (at 6.1 4.125 270) (size 1.4 3.2) (layers B.Cu B.Paste B.Mask)
      (net 33 "Net-(VR1-PadMP2)"))
    (pad MP1 smd rect (at -6.1 4.125 270) (size 1.4 3.2) (layers B.Cu B.Paste B.Mask)
      (net 34 "Net-(VR1-PadMP1)"))
    (pad 5 smd rect (at 3.975 -6.35) (size 1.2 1.7) (layers B.Cu B.Paste B.Mask)
      (net 51 "Net-(VR1-Pad5)"))
    (pad 4 smd rect (at 2 -6.35) (size 1.2 1.7) (layers B.Cu B.Paste B.Mask)
      (net 18 "Net-(U1-Pad40)"))
    (pad 3 smd rect (at -0.025 -6.35) (size 1.2 1.7) (layers B.Cu B.Paste B.Mask)
      (net 50 "Net-(VR1-Pad3)"))
    (pad 2 smd rect (at -2 -6.35) (size 1.2 1.7) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -4 -6.35) (size 1.2 1.7) (layers B.Cu B.Paste B.Mask)
      (net 4 +5V))
    (pad 6 thru_hole circle (at 4.85 1.625) (size 1.2 1.2) (drill 1.2) (layers *.Cu *.Mask))
    (pad 6 thru_hole circle (at -4.775 1.65) (size 1.2 1.2) (drill 1.2) (layers *.Cu *.Mask))
  )
  (module Symbol:WEEE-Logo_4.2x6mm_SilkScreen (layer F.Cu) (tedit 0)
    (at 141.61008 91.77528)
    (descr "Waste Electrical and Electronic Equipment Directive")
    (tags "Logo WEEE")
    (attr virtual)
    (fp_text reference REF** (at 0 0) (layer F.SilkS) hide)
    (fp_text value WEEE-Logo_4.2x6mm_SilkScreen (at 0.75 0) (layer F.Fab) hide)
  )
  (module Symbol:CE-Logo_8.5x6mm_SilkScreen (layer F.Cu) (tedit 0)
    (at 148.88972 91.97848)
    (descr "CE marking")
    (tags "Logo CE certification")
    (attr virtual)
    (fp_text reference REF** (at 0 0) (layer F.SilkS) hide)
    (fp_text value CE-Logo_8.5x6mm_SilkScreen (at 0.75 0) (layer F.Fab) hide)
  )
  (module leetronics_logo:drawing (layer F.Cu) (tedit 0)
    (at 163.60648 111.48568 90)
    (fp_text reference Ref** (at 0 0 90) (layer F.SilkS) hide)
    (fp_text value Val** (at 0 0 90) (layer F.SilkS) hide)
  )
  (module Connector_PinHeader_2.54mm:PinHeader_2x03_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 127.0762 116.1034)
    (descr "Through hole straight pin header, 2x03, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x03 2.54mm double row")
    (fp_text reference ISP1 (at -2.3622 2.4384 90) (layer F.SilkS))
    (fp_text value AVR-ISP-6 (at 1.27 7.41) (layer F.Fab))
    (fp_text user %R (at 1.27 2.54 90) (layer F.Fab))
    (pad 6 thru_hole oval (at 2.54 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 5 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 52 RESET))
    (pad 4 thru_hole oval (at 2.54 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 53 MOSI))
    (pad 3 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 54 SCK))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 +5V))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 55 MISO))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x03_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 157.6832 114.2007 270)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C14 (at -2.8448 0.0508 90) (layer F.SilkS))
    (fp_text value 4.7uF (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GNDA))
    (pad 1 smd roundrect (at -0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 +5VA))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 162.03676 98.5012 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C9 (at -0.0509 -1.3716 90) (layer F.SilkS))
    (fp_text value 4200pF (at 0 1.4478 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GNDA))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 61 "Net-(C9-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 155.3742 113.411 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference L1 (at -0.00268 1.10236) (layer F.SilkS))
    (fp_text value L (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 63 "Net-(C13-Pad1)"))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 +5VA))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 116.9669 99.314 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R2 (at -0.0254 1.4224) (layer F.SilkS))
    (fp_text value 5,1K (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 39 "Net-(J1-PadB5)"))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 116.9415 112.3442 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1 (at 0 -1.43) (layer F.SilkS))
    (fp_text value 5,1K (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 42 "Net-(J1-PadA5)"))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 125.3744 110.8456 225)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C7 (at 2.370788 -0.107763 45) (layer F.SilkS))
    (fp_text value 1uF (at 0 1.43 45) (layer F.Fab))
    (fp_text user %R (at 0 0 45) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 225) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0 225) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 37 "Net-(C7-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Fiducial:Fiducial_0.75mm_Mask1.5mm (layer B.Cu) (tedit 5C18CB26)
    (at 115.43792 90.40876)
    (descr "Circular Fiducial, 0.75mm bare copper, 1.5mm soldermask opening (Level B)")
    (tags fiducial)
    (attr smd)
    (fp_text reference FID6 (at 0.14732 -3.23088) (layer B.SilkS))
    (fp_text value Fiducial (at -0.06096 -4.61772) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad "" smd circle (at 0 0) (size 0.75 0.75) (layers B.Cu B.Mask)
      (solder_mask_margin 0.375) (clearance 0.375))
  )
  (module Fiducial:Fiducial_0.75mm_Mask1.5mm (layer F.Cu) (tedit 5C18CB26)
    (at 162.52952 121.19864)
    (descr "Circular Fiducial, 0.75mm bare copper, 1.5mm soldermask opening (Level B)")
    (tags fiducial)
    (attr smd)
    (fp_text reference FID5 (at -0.24892 3.78968) (layer F.SilkS))
    (fp_text value Fiducial (at -0.11684 6.69544) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad "" smd circle (at 0 0) (size 0.75 0.75) (layers F.Cu F.Mask)
      (solder_mask_margin 0.375) (clearance 0.375))
  )
  (module Fiducial:Fiducial_0.75mm_Mask1.5mm (layer B.Cu) (tedit 5C18CB26)
    (at 118.02364 117.58676)
    (descr "Circular Fiducial, 0.75mm bare copper, 1.5mm soldermask opening (Level B)")
    (tags fiducial)
    (attr smd)
    (fp_text reference FID4 (at 1.7526 6.72084) (layer B.SilkS))
    (fp_text value Fiducial (at -0.13208 -1.96596) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad "" smd circle (at 0 0) (size 0.75 0.75) (layers B.Cu B.Mask)
      (solder_mask_margin 0.375) (clearance 0.375))
  )
  (module Fiducial:Fiducial_0.75mm_Mask1.5mm (layer F.Cu) (tedit 5C18CB26)
    (at 115.443 90.42908)
    (descr "Circular Fiducial, 0.75mm bare copper, 1.5mm soldermask opening (Level B)")
    (tags fiducial)
    (attr smd)
    (fp_text reference FID3 (at 0.11176 -3.24612) (layer F.SilkS))
    (fp_text value Fiducial (at -0.06604 -4.64312) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad "" smd circle (at 0 0) (size 0.75 0.75) (layers F.Cu F.Mask)
      (solder_mask_margin 0.375) (clearance 0.375))
  )
  (module Fiducial:Fiducial_0.75mm_Mask1.5mm (layer B.Cu) (tedit 5C18CB26)
    (at 162.56 121.158)
    (descr "Circular Fiducial, 0.75mm bare copper, 1.5mm soldermask opening (Level B)")
    (tags fiducial)
    (attr smd)
    (fp_text reference FID2 (at -0.29972 3.81) (layer B.SilkS))
    (fp_text value Fiducial (at -0.16764 5.2832) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad "" smd circle (at 0 0) (size 0.75 0.75) (layers B.Cu B.Mask)
      (solder_mask_margin 0.375) (clearance 0.375))
  )
  (module Fiducial:Fiducial_0.75mm_Mask1.5mm (layer F.Cu) (tedit 5C18CB26)
    (at 118.01348 117.59184)
    (descr "Circular Fiducial, 0.75mm bare copper, 1.5mm soldermask opening (Level B)")
    (tags fiducial)
    (attr smd)
    (fp_text reference FID1 (at -1.84404 6.731) (layer F.SilkS))
    (fp_text value Fiducial (at 0 2) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad "" smd circle (at 0 0) (size 0.75 0.75) (layers F.Cu F.Mask)
      (solder_mask_margin 0.375) (clearance 0.375))
  )
  (module libs:PJ-226-4A (layer B.Cu) (tedit 604E59CC)
    (at 159.1244 105.8632 180)
    (attr smd)
    (fp_text reference J4 (at -2.064 -3.4584 180) (layer B.SilkS))
    (fp_text value SENSOR (at -4.7056 -7.9716 90) (layer B.SilkS))
    (pad "" np_thru_hole circle (at 2.575 0.05 180) (size 1.2 1.2) (drill 1.2) (layers *.Cu *.Mask B.SilkS))
    (pad "" np_thru_hole circle (at -4.475 0 180) (size 1.2 1.2) (drill 1.2) (layers *.Cu *.Mask B.SilkS))
    (pad 2 smd rect (at 4.85 0.025 180) (size 2.5 1.5) (layers B.Cu B.Paste B.Mask)
      (net 46 "Net-(J4-Pad2)"))
    (pad 4 smd rect (at -4.325 -2.85 90) (size 2.5 1.5) (layers B.Cu B.Paste B.Mask))
    (pad 1 smd rect (at -4.35 2.925 90) (size 2.5 1.5) (layers B.Cu B.Paste B.Mask)
      (net 61 "Net-(C9-Pad1)"))
    (pad 3 smd rect (at -1.625 2.9 90) (size 2.5 1.5) (layers B.Cu B.Paste B.Mask)
      (net 60 "Net-(J4-Pad3)"))
  )
  (module Crystal:Crystal_SMD_3225-4Pin_3.2x2.5mm (layer F.Cu) (tedit 5A0FD1B2)
    (at 134.7978 110.8202 225)
    (descr "SMD Crystal SERIES SMD3225/4 http://www.txccrystal.com/images/pdf/7m-accuracy.pdf, 3.2x2.5mm^2 package")
    (tags "SMD SMT crystal")
    (autoplace_cost90 10)
    (attr smd)
    (fp_text reference Y1 (at 0.017961 -2.280985 45) (layer F.SilkS))
    (fp_text value Crystal (at 0 2.45 45) (layer F.Fab))
    (fp_text user %R (at 0 0 45) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0.85 225) (size 1.4 1.2) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(C5-Pad2)"))
    (pad 2 smd rect (at 1.1 0.85 225) (size 1.4 1.2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at 1.1 -0.85 225) (size 1.4 1.2) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(C6-Pad1)"))
    (pad 4 smd rect (at -1.1 -0.85 225) (size 1.4 1.2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Crystal.3dshapes/Crystal_SMD_3225-4Pin_3.2x2.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_USB:USB_C_Receptacle_Palconn_UTC16-G (layer B.Cu) (tedit 60B5FBFC)
    (at 117.3988 105.8672 90)
    (descr http://www.palpilot.com/wp-content/uploads/2017/05/UTC027-GKN-OR-Rev-A.pdf)
    (tags "USB C Type-C Receptacle USB2.0")
    (attr smd)
    (fp_text reference J1 (at -0.0762 4.5212 90) (layer B.SilkS))
    (fp_text value USB_C_Receptacle_USB2.0 (at 0 -6.24 90) (layer B.Fab))
    (fp_text user %R (at 0 -1.18 90) (layer B.Fab))
    (fp_text user "PCB Edge" (at 0 -3.43 90) (layer Dwgs.User))
    (pad S1 thru_hole oval (at -4.32 1.93) (size 2.1 1) (drill oval 1.7 0.6) (layers *.Cu *.Mask)
      (net 45 "Net-(J1-PadS1)"))
    (pad S1 thru_hole oval (at 4.32 1.93) (size 2.1 1) (drill oval 1.7 0.6) (layers *.Cu *.Mask)
      (net 45 "Net-(J1-PadS1)"))
    (pad S1 thru_hole oval (at -4.32 -2.24) (size 1.8 1) (drill oval 1.4 0.6) (layers *.Cu *.Mask)
      (net 45 "Net-(J1-PadS1)"))
    (pad S1 thru_hole oval (at 4.32 -2.24) (size 1.8 1) (drill oval 1.4 0.6) (layers *.Cu *.Mask)
      (net 45 "Net-(J1-PadS1)"))
    (pad B7 smd rect (at -0.75 2.51 270) (size 0.3 1.16) (layers B.Cu B.Paste B.Mask)
      (net 44 "Net-(J1-PadA7)"))
    (pad A6 smd rect (at -0.25 2.51 270) (size 0.3 1.16) (layers B.Cu B.Paste B.Mask)
      (net 40 "Net-(J1-PadA6)"))
    (pad A7 smd rect (at 0.25 2.51 270) (size 0.3 1.16) (layers B.Cu B.Paste B.Mask)
      (net 44 "Net-(J1-PadA7)"))
    (pad B8 smd rect (at -1.75 2.51 270) (size 0.3 1.16) (layers B.Cu B.Paste B.Mask)
      (net 43 "Net-(J1-PadB8)"))
    (pad A5 smd rect (at -1.25 2.51 270) (size 0.3 1.16) (layers B.Cu B.Paste B.Mask)
      (net 42 "Net-(J1-PadA5)"))
    (pad A8 smd rect (at 1.25 2.51 270) (size 0.3 1.16) (layers B.Cu B.Paste B.Mask)
      (net 41 "Net-(J1-PadA8)"))
    (pad B6 smd rect (at 0.75 2.51 270) (size 0.3 1.16) (layers B.Cu B.Paste B.Mask)
      (net 40 "Net-(J1-PadA6)"))
    (pad B5 smd rect (at 1.75 2.51 270) (size 0.3 1.16) (layers B.Cu B.Paste B.Mask)
      (net 39 "Net-(J1-PadB5)"))
    (pad "" np_thru_hole circle (at 2.89 1.45 270) (size 0.6 0.6) (drill 0.6) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -2.89 1.45 270) (size 0.6 0.6) (drill 0.6) (layers *.Cu *.Mask))
    (pad A4 smd rect (at -2.4 2.51 90) (size 0.6 1.16) (layers B.Cu B.Paste B.Mask)
      (net 32 "Net-(F1-Pad2)"))
    (pad B9 smd rect (at -2.4 2.51 90) (size 0.6 1.16) (layers B.Cu B.Paste B.Mask)
      (net 32 "Net-(F1-Pad2)"))
    (pad A1 smd rect (at -3.2 2.51 90) (size 0.6 1.16) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad B12 smd rect (at -3.2 2.51 90) (size 0.6 1.16) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad B4 smd rect (at 2.4 2.51 90) (size 0.6 1.16) (layers B.Cu B.Paste B.Mask)
      (net 32 "Net-(F1-Pad2)"))
    (pad B1 smd rect (at 3.2 2.51 90) (size 0.6 1.16) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad A9 smd rect (at 2.4 2.51 90) (size 0.6 1.16) (layers B.Cu B.Paste B.Mask)
      (net 32 "Net-(F1-Pad2)"))
    (pad A12 smd rect (at 3.2 2.51 90) (size 0.6 1.16) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Connector_USB.3dshapes/USB_C_Receptacle_Palconn_UTC16-G.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 124.6124 109.2454 225)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R4 (at 2.083419 0.035921 45) (layer F.SilkS))
    (fp_text value 27R (at 0 1.43 45) (layer F.Fab))
    (fp_text user %R (at 0 0 45) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0 225) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 65 "Net-(R4-Pad1)"))
    (pad 2 smd roundrect (at 0.7875 0 225) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 40 "Net-(J1-PadA6)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 127.9144 97.8408 315)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R6 (at -2.047498 0.035921 225) (layer F.SilkS))
    (fp_text value 0R (at 0 1.43 135) (layer F.Fab))
    (fp_text user %R (at 0 0 135) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 315) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 47 "Net-(R6-Pad2)"))
    (pad 1 smd roundrect (at -0.7875 0 315) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Fuse:Fuse_0805_2012Metric (layer F.Cu) (tedit 5B36C52C)
    (at 122.8067 103.505 180)
    (descr "Fuse SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference F1 (at 2.7917 0) (layer F.SilkS))
    (fp_text value Fuse (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 32 "Net-(F1-Pad2)"))
    (pad 1 smd roundrect (at -0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 +5V))
    (model ${KISYS3DMOD}/Fuse.3dshapes/Fuse_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 124.686087 100.556087 135)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C1 (at 2.277431 -0.053882 225) (layer F.SilkS))
    (fp_text value 4.7uF (at 0 1.65 135) (layer F.Fab))
    (fp_text user %R (at 0 0 135) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 135) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.9375 0 135) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 +5V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_Array_Convex_4x0603 (layer F.Cu) (tedit 58E0A8B2)
    (at 135.644932 100.240124 45)
    (descr "Chip Resistor Network, ROHM MNR14 (see mnr_g.pdf)")
    (tags "resistor array")
    (attr smd)
    (fp_text reference RN2 (at 2.731972 0.344604 135) (layer F.SilkS))
    (fp_text value R_Pack04 (at 0 2.8 45) (layer F.Fab))
    (fp_text user %R (at 0 0 135) (layer F.Fab))
    (pad 1 smd rect (at -0.9 -1.2 45) (size 0.8 0.5) (layers F.Cu F.Paste F.Mask)
      (net 30 PD7))
    (pad 3 smd rect (at -0.9 0.4 45) (size 0.8 0.4) (layers F.Cu F.Paste F.Mask)
      (net 68 "Net-(RN2-Pad3)"))
    (pad 2 smd rect (at -0.9 -0.4 45) (size 0.8 0.4) (layers F.Cu F.Paste F.Mask)
      (net 31 PD0))
    (pad 4 smd rect (at -0.9 1.2 45) (size 0.8 0.5) (layers F.Cu F.Paste F.Mask)
      (net 4 +5V))
    (pad 7 smd rect (at 0.9 -0.4 45) (size 0.8 0.4) (layers F.Cu F.Paste F.Mask)
      (net 57 "Net-(D2-Pad4)"))
    (pad 8 smd rect (at 0.9 -1.2 45) (size 0.8 0.5) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(D2-Pad2)"))
    (pad 6 smd rect (at 0.9 0.4 45) (size 0.8 0.4) (layers F.Cu F.Paste F.Mask)
      (net 49 "Net-(RN2-Pad6)"))
    (pad 5 smd rect (at 0.9 1.2 45) (size 0.8 0.5) (layers F.Cu F.Paste F.Mask)
      (net 59 "Net-(J3-Pad3)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_Array_Convex_4x0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 133.9849 116.4336)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R7 (at -2.2605 0.127) (layer F.SilkS))
    (fp_text value 5,1K (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 -1.4224) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 66 "Net-(R7-Pad2)"))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 38 "Net-(C8-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 133.9849 118.11)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C8 (at -2.2351 0.0508) (layer F.SilkS))
    (fp_text value 1uF (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 1.3208) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 38 "Net-(C8-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 126.2888 99.1362 135)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C4 (at 2.137301 0.017961 225) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.43 135) (layer F.Fab))
    (fp_text user %R (at 0 0 135) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 135) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0 135) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 +5V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 126.540847 112.066753 225)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C3 (at 2.368026 0 225) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.43 45) (layer F.Fab))
    (fp_text user %R (at 0 0 45) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 225) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0 225) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 +5V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 137.793047 102.363953 45)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C2 (at 2.463352 0.161645 45) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.43 45) (layer F.Fab))
    (fp_text user %R (at 0 0 45) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 45) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0 45) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 +5V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module libs:LED_RGB_EASR3212RGBA0 (layer B.Cu) (tedit 604CD4DD)
    (at 143.3576 105.8164 90)
    (descr "RGB LED 3.2x2.7mm http://www.avagotech.com/docs/AV02-0610EN")
    (tags "LED 3227")
    (attr smd)
    (fp_text reference D2 (at -0.0254 1.6764 90) (layer B.SilkS))
    (fp_text value LED_RGBA (at 0 -2.45 90) (layer B.Fab))
    (fp_text user %R (at 0 2.3 90) (layer B.Fab))
    (pad 3 smd rect (at 1.45 0.375 270) (size 0.7 0.7) (layers B.Cu B.Paste B.Mask)
      (net 24 "Net-(D2-Pad3)"))
    (pad 4 smd rect (at -1.4 0.375 270) (size 0.7 0.7) (layers B.Cu B.Paste B.Mask)
      (net 57 "Net-(D2-Pad4)"))
    (pad 2 smd rect (at 1.45 -0.6 270) (size 0.7 0.7) (layers B.Cu B.Paste B.Mask)
      (net 23 "Net-(D2-Pad2)"))
    (pad 1 smd rect (at -1.4 -0.6 270) (size 0.7 0.7) (layers B.Cu B.Paste B.Mask)
      (net 4 +5V))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_RGB_1210.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module libs:LED_RGB_EASR3212RGBA0 (layer B.Cu) (tedit 604CD4DD)
    (at 130.7084 105.8164 90)
    (descr "RGB LED 3.2x2.7mm http://www.avagotech.com/docs/AV02-0610EN")
    (tags "LED 3227")
    (attr smd)
    (fp_text reference D1 (at -0.0508 1.778 90) (layer B.SilkS))
    (fp_text value LED_RGBA (at -8.763 -8.382 90) (layer B.Fab))
    (fp_text user %R (at 0 2.3 90) (layer B.Fab))
    (pad 3 smd rect (at 1.45 0.375 270) (size 0.7 0.7) (layers B.Cu B.Paste B.Mask)
      (net 21 "Net-(D1-Pad3)"))
    (pad 4 smd rect (at -1.4 0.375 270) (size 0.7 0.7) (layers B.Cu B.Paste B.Mask)
      (net 56 "Net-(D1-Pad4)"))
    (pad 2 smd rect (at 1.45 -0.6 270) (size 0.7 0.7) (layers B.Cu B.Paste B.Mask)
      (net 22 "Net-(D1-Pad2)"))
    (pad 1 smd rect (at -1.4 -0.6 270) (size 0.7 0.7) (layers B.Cu B.Paste B.Mask)
      (net 4 +5V))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_RGB_1210.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 139.1158 114.0715 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C11 (at -2.6669 0 90) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 +5V))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 153.1366 113.9698 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C13 (at -2.8194 0 90) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 62 "Net-(C13-Pad2)"))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 63 "Net-(C13-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 158.85658 94.54896 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C12 (at 0.02022 1.36652) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 +5VA))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GNDA))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 136.8298 108.5596 135)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C5 (at -0.377171 1.095591 135) (layer F.SilkS))
    (fp_text value 22pF (at 0 1.43 135) (layer F.Fab))
    (fp_text user %R (at 0 0 135) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0 135) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.7875 0 135) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 35 "Net-(C5-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 132.335953 113.184353 135)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C6 (at 0 -1.43 135) (layer F.SilkS))
    (fp_text value 22pF (at 0 1.43 135) (layer F.Fab))
    (fp_text user %R (at 0 0 135) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 135) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0 135) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 36 "Net-(C6-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 152.23734 99.88804 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R8 (at 0.02022 -1.36652) (layer F.SilkS))
    (fp_text value 1K (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 +5VA))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 67 "Net-(R8-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 154.87904 100.74148 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R9 (at 2.52476 0.0254 90) (layer F.SilkS))
    (fp_text value 100K (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 +5VA))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 46 "Net-(J4-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 123.444 108.1278 225)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R3 (at 2.011577 0 225) (layer F.SilkS))
    (fp_text value 27R (at 0 1.43 45) (layer F.Fab))
    (fp_text user %R (at 0 0 45) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 225) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 44 "Net-(J1-PadA7)"))
    (pad 1 smd roundrect (at -0.7875 0 225) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 64 "Net-(R3-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 140.83284 105.24236 225)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R5 (at -2.2099 -0.0508 45) (layer F.SilkS))
    (fp_text value 10K (at 0 1.43 45) (layer F.Fab))
    (fp_text user %R (at 0 0 45) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 225) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 +5V))
    (pad 1 smd roundrect (at -0.7875 0 225) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 52 RESET))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_DFN_QFN:QFN-44-1EP_7x7mm_P0.5mm_EP5.2x5.2mm (layer F.Cu) (tedit 5C26A111)
    (at 129.9718 105.7148 45)
    (descr "QFN, 44 Pin (http://ww1.microchip.com/downloads/en/DeviceDoc/2512S.pdf#page=17), generated with kicad-footprint-generator ipc_dfn_qfn_generator.py")
    (tags "QFN DFN_QFN")
    (attr smd)
    (fp_text reference U1 (at -1.688288 -4.885259 45) (layer F.SilkS))
    (fp_text value ATmega32U4-MU (at 0 4.82 45) (layer F.Fab))
    (fp_text user %R (at 0 0 45) (layer F.Fab))
    (pad 44 smd roundrect (at -2.5 -3.3375 45) (size 0.25 1.075) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 +5V))
    (pad 43 smd roundrect (at -2 -3.3375 45) (size 0.25 1.075) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 42 smd roundrect (at -1.5 -3.3375 45) (size 0.25 1.075) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 20 "Net-(U1-Pad42)"))
    (pad 41 smd roundrect (at -1 -3.3375 45) (size 0.25 1.075) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 "Net-(U1-Pad41)"))
    (pad 40 smd roundrect (at -0.5 -3.3375 45) (size 0.25 1.075) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 "Net-(U1-Pad40)"))
    (pad 39 smd roundrect (at 0 -3.3375 45) (size 0.25 1.075) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 17 "Net-(U1-Pad39)"))
    (pad 38 smd roundrect (at 0.5 -3.3375 45) (size 0.25 1.075) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 16 "Net-(U1-Pad38)"))
    (pad 37 smd roundrect (at 1 -3.3375 45) (size 0.25 1.075) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 15 "Net-(U1-Pad37)"))
    (pad 36 smd roundrect (at 1.5 -3.3375 45) (size 0.25 1.075) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 14 "Net-(U1-Pad36)"))
    (pad 35 smd roundrect (at 2 -3.3375 45) (size 0.25 1.075) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 34 smd roundrect (at 2.5 -3.3375 45) (size 0.25 1.075) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 +5V))
    (pad 33 smd roundrect (at 3.3375 -2.5 45) (size 1.075 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 47 "Net-(R6-Pad2)"))
    (pad 32 smd roundrect (at 3.3375 -2 45) (size 1.075 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 26 PC7))
    (pad 31 smd roundrect (at 3.3375 -1.5 45) (size 1.075 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 28 PC6))
    (pad 30 smd roundrect (at 3.3375 -1 45) (size 1.075 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 27 PB6))
    (pad 29 smd roundrect (at 3.3375 -0.5 45) (size 1.075 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 29 PB5))
    (pad 28 smd roundrect (at 3.3375 0 45) (size 1.075 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 13 "Net-(U1-Pad28)"))
    (pad 27 smd roundrect (at 3.3375 0.5 45) (size 1.075 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 30 PD7))
    (pad 26 smd roundrect (at 3.3375 1 45) (size 1.075 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 12 "Net-(U1-Pad26)"))
    (pad 25 smd roundrect (at 3.3375 1.5 45) (size 1.075 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 11 "Net-(U1-Pad25)"))
    (pad 24 smd roundrect (at 3.3375 2 45) (size 1.075 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 +5V))
    (pad 23 smd roundrect (at 3.3375 2.5 45) (size 1.075 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 22 smd roundrect (at 2.5 3.3375 45) (size 0.25 1.075) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 10 "Net-(U1-Pad22)"))
    (pad 21 smd roundrect (at 2 3.3375 45) (size 0.25 1.075) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 9 TX0))
    (pad 20 smd roundrect (at 1.5 3.3375 45) (size 0.25 1.075) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 "Net-(U1-Pad20)"))
    (pad 19 smd roundrect (at 1 3.3375 45) (size 0.25 1.075) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 25 ISO_OUT))
    (pad 18 smd roundrect (at 0.5 3.3375 45) (size 0.25 1.075) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 31 PD0))
    (pad 17 smd roundrect (at 0 3.3375 45) (size 0.25 1.075) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 35 "Net-(C5-Pad2)"))
    (pad 16 smd roundrect (at -0.5 3.3375 45) (size 0.25 1.075) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 36 "Net-(C6-Pad1)"))
    (pad 15 smd roundrect (at -1 3.3375 45) (size 0.25 1.075) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 14 smd roundrect (at -1.5 3.3375 45) (size 0.25 1.075) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 +5V))
    (pad 13 smd roundrect (at -2 3.3375 45) (size 0.25 1.075) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 52 RESET))
    (pad 12 smd roundrect (at -2.5 3.3375 45) (size 0.25 1.075) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 66 "Net-(R7-Pad2)"))
    (pad 11 smd roundrect (at -3.3375 2.5 45) (size 1.075 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 55 MISO))
    (pad 10 smd roundrect (at -3.3375 2 45) (size 1.075 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 53 MOSI))
    (pad 9 smd roundrect (at -3.3375 1.5 45) (size 1.075 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 54 SCK))
    (pad 8 smd roundrect (at -3.3375 1 45) (size 1.075 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 "Net-(U1-Pad8)"))
    (pad 7 smd roundrect (at -3.3375 0.5 45) (size 1.075 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 +5V))
    (pad 6 smd roundrect (at -3.3375 0 45) (size 1.075 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 37 "Net-(C7-Pad1)"))
    (pad 5 smd roundrect (at -3.3375 -0.5 45) (size 1.075 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 4 smd roundrect (at -3.3375 -1 45) (size 1.075 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 65 "Net-(R4-Pad1)"))
    (pad 3 smd roundrect (at -3.3375 -1.5 45) (size 1.075 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 64 "Net-(R3-Pad1)"))
    (pad 2 smd roundrect (at -3.3375 -2 45) (size 1.075 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 +5V))
    (pad 1 smd roundrect (at -3.3375 -2.5 45) (size 1.075 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 "Net-(U1-Pad1)"))
    (pad "" smd roundrect (at 1.95 1.95 45) (size 1.05 1.05) (layers F.Paste) (roundrect_rratio 0.238095))
    (pad "" smd roundrect (at 1.95 0.65 45) (size 1.05 1.05) (layers F.Paste) (roundrect_rratio 0.238095))
    (pad "" smd roundrect (at 1.95 -0.65 45) (size 1.05 1.05) (layers F.Paste) (roundrect_rratio 0.238095))
    (pad "" smd roundrect (at 1.95 -1.95 45) (size 1.05 1.05) (layers F.Paste) (roundrect_rratio 0.238095))
    (pad "" smd roundrect (at 0.65 1.95 45) (size 1.05 1.05) (layers F.Paste) (roundrect_rratio 0.238095))
    (pad "" smd roundrect (at 0.65 0.65 45) (size 1.05 1.05) (layers F.Paste) (roundrect_rratio 0.238095))
    (pad "" smd roundrect (at 0.65 -0.65 45) (size 1.05 1.05) (layers F.Paste) (roundrect_rratio 0.238095))
    (pad "" smd roundrect (at 0.65 -1.95 45) (size 1.05 1.05) (layers F.Paste) (roundrect_rratio 0.238095))
    (pad "" smd roundrect (at -0.65 1.95 45) (size 1.05 1.05) (layers F.Paste) (roundrect_rratio 0.238095))
    (pad "" smd roundrect (at -0.65 0.65 45) (size 1.05 1.05) (layers F.Paste) (roundrect_rratio 0.238095))
    (pad "" smd roundrect (at -0.65 -0.65 45) (size 1.05 1.05) (layers F.Paste) (roundrect_rratio 0.238095))
    (pad "" smd roundrect (at -0.65 -1.95 45) (size 1.05 1.05) (layers F.Paste) (roundrect_rratio 0.238095))
    (pad "" smd roundrect (at -1.95 1.95 45) (size 1.05 1.05) (layers F.Paste) (roundrect_rratio 0.238095))
    (pad "" smd roundrect (at -1.95 0.65 45) (size 1.05 1.05) (layers F.Paste) (roundrect_rratio 0.238095))
    (pad "" smd roundrect (at -1.95 -0.65 45) (size 1.05 1.05) (layers F.Paste) (roundrect_rratio 0.238095))
    (pad "" smd roundrect (at -1.95 -1.95 45) (size 1.05 1.05) (layers F.Paste) (roundrect_rratio 0.238095))
    (pad 45 smd roundrect (at 0 0 45) (size 5.2 5.2) (layers F.Cu F.Mask) (roundrect_rratio 0.048077)
      (net 1 GND))
    (model ${KISYS3DMOD}/Package_DFN_QFN.3dshapes/QFN-44-1EP_7x7mm_P0.5mm_EP5.2x5.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_SO:VSSOP-8_3.0x3.0mm_P0.65mm (layer F.Cu) (tedit 5A02F25C)
    (at 157.5406 97.196)
    (descr "VSSOP-8 3.0 x 3.0, http://www.ti.com/lit/ds/symlink/lm75b.pdf")
    (tags "VSSOP-8 3.0 x 3.0")
    (attr smd)
    (fp_text reference U2 (at -1.44744 -2.31176 180) (layer F.SilkS))
    (fp_text value LM555 (at 0.02 2.73) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -2.2 -0.975 270) (size 0.45 1.45) (layers F.Cu F.Paste F.Mask)
      (net 2 GNDA))
    (pad 2 smd rect (at -2.2 -0.325 270) (size 0.45 1.45) (layers F.Cu F.Paste F.Mask)
      (net 61 "Net-(C9-Pad1)"))
    (pad 3 smd rect (at -2.2 0.325 270) (size 0.45 1.45) (layers F.Cu F.Paste F.Mask)
      (net 3 555))
    (pad 4 smd rect (at -2.2 0.975 270) (size 0.45 1.45) (layers F.Cu F.Paste F.Mask)
      (net 5 +5VA))
    (pad 5 smd rect (at 2.2 0.975 270) (size 0.45 1.45) (layers F.Cu F.Paste F.Mask)
      (net 48 "Net-(U2-Pad5)"))
    (pad 6 smd rect (at 2.2 0.325 270) (size 0.45 1.45) (layers F.Cu F.Paste F.Mask)
      (net 61 "Net-(C9-Pad1)"))
    (pad 7 smd rect (at 2.2 -0.325 270) (size 0.45 1.45) (layers F.Cu F.Paste F.Mask)
      (net 46 "Net-(J4-Pad2)"))
    (pad 8 smd rect (at 2.2 -0.975 270) (size 0.45 1.45) (layers F.Cu F.Paste F.Mask)
      (net 5 +5VA))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/VSSOP-8_3.0x3.0mm_P0.65mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_Array_Convex_4x0603 (layer F.Cu) (tedit 58E0A8B2)
    (at 132.419132 97.141324 45)
    (descr "Chip Resistor Network, ROHM MNR14 (see mnr_g.pdf)")
    (tags "resistor array")
    (attr smd)
    (fp_text reference RN1 (at 2.767893 0.021315 135) (layer F.SilkS))
    (fp_text value R_Pack04 (at 0 2.8 45) (layer F.Fab))
    (fp_text user %R (at 0 0 135) (layer F.Fab))
    (pad 5 smd rect (at 0.9 1.2 45) (size 0.8 0.5) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(D2-Pad3)"))
    (pad 6 smd rect (at 0.9 0.4 45) (size 0.8 0.4) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(D1-Pad2)"))
    (pad 8 smd rect (at 0.9 -1.2 45) (size 0.8 0.5) (layers F.Cu F.Paste F.Mask)
      (net 56 "Net-(D1-Pad4)"))
    (pad 7 smd rect (at 0.9 -0.4 45) (size 0.8 0.4) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(D1-Pad3)"))
    (pad 4 smd rect (at -0.9 1.2 45) (size 0.8 0.5) (layers F.Cu F.Paste F.Mask)
      (net 29 PB5))
    (pad 2 smd rect (at -0.9 -0.4 45) (size 0.8 0.4) (layers F.Cu F.Paste F.Mask)
      (net 28 PC6))
    (pad 3 smd rect (at -0.9 0.4 45) (size 0.8 0.4) (layers F.Cu F.Paste F.Mask)
      (net 27 PB6))
    (pad 1 smd rect (at -0.9 -1.2 45) (size 0.8 0.5) (layers F.Cu F.Paste F.Mask)
      (net 26 PC7))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_Array_Convex_4x0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Button_Switch_SMD:SW_SPST_TL3342 (layer F.Cu) (tedit 5A02FC95)
    (at 133.6802 91.2622)
    (descr "Low-profile SMD Tactile Switch, https://www.e-switch.com/system/asset/product_line/data_sheet/165/TL3342.pdf")
    (tags "SPST Tactile Switch")
    (attr smd)
    (fp_text reference SW1 (at 4.9022 0 90) (layer F.SilkS))
    (fp_text value SW_Push (at -0.0508 -0.0508) (layer F.Fab))
    (fp_text user %R (at 5.18668 -0.0508) (layer F.Fab))
    (pad 1 smd rect (at -3.15 -1.9) (size 1.7 1) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at 3.15 -1.9) (size 1.7 1) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -3.15 1.9) (size 1.7 1) (layers F.Cu F.Paste F.Mask)
      (net 52 RESET))
    (pad 2 smd rect (at 3.15 1.9) (size 1.7 1) (layers F.Cu F.Paste F.Mask)
      (net 52 RESET))
    (model ${KISYS3DMOD}/Button_Switch_SMD.3dshapes/SW_SPST_TL3342.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 137.2362 114.2977 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C10 (at -3.1011 0.1016 90) (layer F.SilkS))
    (fp_text value 4,7uF (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 +5V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 155.2956 114.935)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference L2 (at -0.01016 1.16332) (layer F.SilkS))
    (fp_text value L (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 62 "Net-(C13-Pad2)"))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GNDA))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_SO:SO-4_4.4x2.3mm_P1.27mm (layer F.Cu) (tedit 5B1E4D3A)
    (at 146.0242 98.8822 180)
    (descr "4-Lead Plastic Small Outline (SO), see http://datasheet.octopart.com/OPIA403BTRE-Optek-datasheet-5328560.pdf")
    (tags "SO SOIC 1.27")
    (attr smd)
    (fp_text reference U4 (at 0 -2.1) (layer F.SilkS))
    (fp_text value LTV-355T (at 0 2.3) (layer F.Fab))
    (fp_text user %R (at 0 -0.065) (layer F.Fab))
    (pad 4 smd rect (at 3.15 -0.635 180) (size 2 0.64) (layers F.Cu F.Paste F.Mask)
      (net 25 ISO_OUT))
    (pad 3 smd rect (at 3.15 0.635 180) (size 2 0.64) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -3.15 0.635 180) (size 2 0.64) (layers F.Cu F.Paste F.Mask)
      (net 3 555))
    (pad 1 smd rect (at -3.15 -0.635 180) (size 2 0.64) (layers F.Cu F.Paste F.Mask)
      (net 67 "Net-(R8-Pad2)"))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/SO-4_4.4x2.3mm_P1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 139.447953 103.899287 45)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R10 (at 2.640195 0.089803 45) (layer F.SilkS))
    (fp_text value 10K (at 0 1.43 45) (layer F.Fab))
    (fp_text user %R (at -0.0254 0.0762 45) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0 45) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 +5V))
    (pad 2 smd roundrect (at 0.7875 0 45) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 25 ISO_OUT))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module libs:PJ-320-4A (layer B.Cu) (tedit 604CD116)
    (at 120.2436 93.7006 180)
    (attr smd)
    (fp_text reference J3 (at 0.9652 4.0386 180) (layer B.SilkS))
    (fp_text value MIDI (at 5.8166 -4.699 90) (layer B.SilkS))
    (pad 1 smd rect (at -4.05 3.325 90) (size 2.5 1.2) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -2.825 -3.225 90) (size 2.5 1.2) (layers B.Cu B.Paste B.Mask)
      (net 9 TX0))
    (pad 4 smd rect (at 3.875 -3.25 90) (size 2.5 1.2) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad "" np_thru_hole circle (at 5.55 0.025 180) (size 1.1 1.1) (drill 1.1) (layers *.Cu *.Mask B.SilkS))
    (pad "" np_thru_hole circle (at -1.425 0 180) (size 1.1 1.1) (drill 1.1) (layers *.Cu *.Mask B.SilkS))
    (pad 3 smd rect (at 1 -3.225 90) (size 2.5 1.2) (layers B.Cu B.Paste B.Mask)
      (net 59 "Net-(J3-Pad3)"))
  )
  (module libs:PJ-320-4A (layer B.Cu) (tedit 604CD116)
    (at 120.269 117.602 180)
    (attr smd)
    (fp_text reference J2 (at 0.9398 4.0386 180) (layer B.SilkS))
    (fp_text value CV (at 5.6896 4.6736 90) (layer B.SilkS))
    (pad 3 smd rect (at 1 -3.225 90) (size 2.5 1.2) (layers B.Cu B.Paste B.Mask)
      (net 58 "Net-(J2-Pad3)"))
    (pad "" np_thru_hole circle (at -1.425 0 180) (size 1.1 1.1) (drill 1.1) (layers *.Cu *.Mask B.SilkS))
    (pad "" np_thru_hole circle (at 5.55 0.025 180) (size 1.1 1.1) (drill 1.1) (layers *.Cu *.Mask B.SilkS))
    (pad 4 smd rect (at 3.875 -3.25 90) (size 2.5 1.2) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -2.825 -3.225 90) (size 2.5 1.2) (layers B.Cu B.Paste B.Mask)
      (net 38 "Net-(C8-Pad1)"))
    (pad 1 smd rect (at -4.05 3.325 90) (size 2.5 1.2) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
  )
  (gr_text RESET (at 128.6002 91.44 90) (layer F.SilkS))
  (gr_text "MIDI Biodata \nSonification Device \nv4" (at 153.67508 120.65) (layer F.SilkS))
  (gr_line (start 113.0046 88.138) (end 113.0046 123.4948) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 165.0238 88.138) (end 113.0046 88.138) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 164.9984 123.4948) (end 165.0238 88.138) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 113.0046 123.4948) (end 164.9984 123.4948) (layer Edge.Cuts) (width 0.1))
  (zone (net 2) (net_name GNDA) (layer In1.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 148.219617 117.591836) (xy 156.468624 117.591845) (xy 156.348977 107.551194) (xy 148.237663 107.525847) (xy 148.197634 88.646)
        (xy 164.809234 88.646) (xy 164.809234 123.2408) (xy 153.252234 123.2408) (xy 150.20925 123.2408) (xy 150.19655 119.69115)
        (xy 148.20265 119.67845)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 113.157 88.0618) (xy 144.4498 88.099899) (xy 144.4498 123.329702) (xy 113.284 123.2916) (xy 113.284 88.265)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer In1.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 113.1316 88.019519) (xy 144.4244 88.057618) (xy 144.4244 123.287421) (xy 113.2586 123.249319) (xy 113.2586 88.222719)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 113.157 88.052923) (xy 144.4498 88.091022) (xy 144.4498 123.320825) (xy 113.284 123.282723) (xy 113.284 88.256123)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer In2.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 113.1316 87.989731) (xy 144.4244 88.02783) (xy 144.4244 123.257633) (xy 113.2586 123.219531) (xy 113.2586 88.192931)
      )
    )
  )
  (zone (net 2) (net_name GNDA) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 148.219244 117.584452) (xy 156.468251 117.584461) (xy 156.348604 107.54381) (xy 148.23729 107.518463) (xy 148.197261 88.638616)
        (xy 164.808861 88.638616) (xy 164.808861 123.233416) (xy 153.251861 123.233416) (xy 150.208877 123.233416) (xy 150.196177 119.683766)
        (xy 148.202277 119.671066)
      )
    )
  )
  (zone (net 2) (net_name GNDA) (layer In2.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 148.201811 117.580953) (xy 156.450818 117.580962) (xy 156.331171 107.540311) (xy 148.219857 107.514964) (xy 148.179828 88.635117)
        (xy 164.791428 88.635117) (xy 164.791428 123.229917) (xy 153.234428 123.229917) (xy 150.191444 123.229917) (xy 150.178744 119.680267)
        (xy 148.184844 119.667567)
      )
    )
  )
  (zone (net 2) (net_name GNDA) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 148.201811 117.561824) (xy 156.450818 117.561833) (xy 156.331171 107.521182) (xy 148.219857 107.495835) (xy 148.179828 88.615988)
        (xy 164.791428 88.615988) (xy 164.791428 123.210788) (xy 153.234428 123.210788) (xy 150.191444 123.210788) (xy 150.178744 119.661138)
        (xy 148.184844 119.648438)
      )
    )
  )
)
