(kicad_pcb
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(31 "B.Cu" signal)
		(32 "B.Adhes" user "B.Adhesive")
		(33 "F.Adhes" user "F.Adhesive")
		(34 "B.Paste" user)
		(35 "F.Paste" user)
		(36 "B.SilkS" user "B.Silkscreen")
		(37 "F.SilkS" user "F.Silkscreen")
		(38 "B.Mask" user)
		(39 "F.Mask" user)
		(40 "Dwgs.User" user "User.Drawings")
		(41 "Cmts.User" user "User.Comments")
		(42 "Eco1.User" user "User.Eco1")
		(43 "Eco2.User" user "User.Eco2")
		(44 "Edge.Cuts" user)
		(45 "Margin" user)
		(46 "B.CrtYd" user "B.Courtyard")
		(47 "F.CrtYd" user "F.Courtyard")
		(48 "B.Fab" user)
		(49 "F.Fab" user)
		(50 "User.1" user)
		(51 "User.2" user)
		(52 "User.3" user)
		(53 "User.4" user)
		(54 "User.5" user)
		(55 "User.6" user)
		(56 "User.7" user)
		(57 "User.8" user)
		(58 "User.9" user)
	)
	(setup
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(pcbplotparams
			(layerselection 0x00010fc_ffffffff)
			(plot_on_all_layers_selection 0x0000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(viasonmask no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plotreference yes)
			(plotvalue yes)
			(plotfptext yes)
			(plotinvisibletext no)
			(sketchpadsonfab no)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 1)
			(scaleselection 1)
			(outputdirectory "")
		)
	)
	(net 0 "")
	(net 1 "GND")
	(net 2 "+5V")
	(net 3 "Net-(D1-K)")
	(net 4 "VDD")
	(net 5 "Net-(J1-Pin_1)")
	(net 6 "E")
	(net 7 "D")
	(net 8 "UART_RX")
	(net 9 "UART_TX")
	(net 10 "SCL")
	(net 11 "SDA")
	(net 12 "A0")
	(net 13 "B")
	(net 14 "B1")
	(net 15 "G2")
	(net 16 "LAT")
	(net 17 "R1")
	(net 18 "R2")
	(net 19 "CLK")
	(net 20 "A")
	(net 21 "G1")
	(net 22 "OE")
	(net 23 "B2")
	(net 24 "C")
	(net 25 "A1")
	(net 26 "A2")
	(net 27 "A3")
	(net 28 "UPDI")
	(net 29 "Net-(U4-SW)")
	(net 30 "unconnected-(U2-VREFA{slash}PD7-Pad17)")
	(net 31 "unconnected-(U2-PD6-Pad16)")
	(net 32 "Net-(U4-BOOT)")
	(net 33 "Net-(U4-EN)")
	(net 34 "Net-(R7-Pad2)")
	(net 35 "Net-(U4-FB)")
	(net 36 "Net-(R10-Pad2)")
	(net 37 "Temp")
	(net 38 "Net-(U2-~{RESET}{slash}PF6)")
	(net 39 "Net-(JP7-A)")
	(net 40 "unconnected-(U2-PF5-Pad25)")
	(net 41 "Net-(JP8-A)")
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(at 149.75 58.75)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C9"
			(at -2.75 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "22u"
			(at 0 1.68 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "MatrixDriver.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.212766)
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.212766)
			(net 2 "+5V")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(at 128.5 79.5)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R13"
			(at 3.25 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 0 1.65 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "MatrixDriver.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.208333)
			(net 41 "Net-(JP8-A)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.208333)
			(net 10 "SCL")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Kicad_Libs:ECS_Coil"
		(layer "F.Cu")
		(at 151.75 65 90)
		(property "Reference" "L1"
			(at 0 -0.5 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "10u, ECS-MPIL0630-100MC"
			(at 0 1 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" "Kicad_Libs:ECS_Coil"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Inductor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Choke_* *Coil* Inductor_* L_*")
		(sheetname "Root")
		(sheetfile "MatrixDriver.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 2.5 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -3.1 0 90)
			(size 1.8 4.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 29 "Net-(U4-SW)")
			(pinfunction "1")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "2" smd roundrect
			(at 3.1 0 90)
			(size 1.8 4.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "+5V")
			(pinfunction "2")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
	)
	(footprint "Connector_JST:JST_PH_S3B-PH-SM4-TB_1x03-1MP_P2.00mm_Horizontal"
		(layer "F.Cu")
		(at 141.5 88.5)
		(descr "JST PH series connector, S3B-PH-SM4-TB (http://www.jst-mfg.com/product/pdf/eng/ePH.pdf), generated with kicad-footprint-generator")
		(tags "connector JST PH horizontal")
		(property "Reference" "J7"
			(at -6.5 -4 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "UART"
			(at 0 5.8 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_JST:JST_PH_S3B-PH-SM4-TB_1x03-1MP_P2.00mm_Horizontal"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x03, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "Root")
		(sheetfile "MatrixDriver.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 1.5 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2 -2.85)
			(size 1 3.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 9 "UART_TX")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0 -2.85)
			(size 1 3.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 8 "UART_RX")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at 2 -2.85)
			(size 1 3.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "MP" smd roundrect
			(at -4.35 2.9)
			(size 1.5 3.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.166667)
		)
		(pad "MP" smd roundrect
			(at 4.35 2.9)
			(size 1.5 3.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.166667)
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_JST.3dshapes/JST_PH_S3B-PH-SM4-TB_1x03-1MP_P2.00mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(at 157.75 76.25)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R6"
			(at 2.75 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "100k"
			(at 0 1.65 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "MatrixDriver.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.208333)
			(net 33 "Net-(U4-EN)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.208333)
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_JST:JST_XA_S02B-XASK-1_1x02_P2.50mm_Horizontal"
		(layer "F.Cu")
		(at 152.5 84)
		(descr "JST XA series connector, S02B-XASK-1 (http://www.jst-mfg.com/product/pdf/eng/eXA1.pdf), generated with kicad-footprint-generator")
		(tags "connector JST XA horizontal hook")
		(property "Reference" "J1"
			(at 1.25 -4.6 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "PWR IN"
			(at 1.25 10.4 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_JST:JST_XA_S02B-XASK-1_1x02_P2.50mm_Horizontal"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "Root")
		(sheetfile "MatrixDriver.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.25 2.5 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole oval
			(at 1.25 6.5)
			(size 2.8 2)
			(drill oval 2.8 2)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" thru_hole roundrect
			(at 0 0)
			(size 1.7 1.95)
			(drill 0.95)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.147059)
			(net 5 "Net-(J1-Pin_1)")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 2.5 0)
			(size 1.7 1.95)
			(drill 0.95)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_JST.3dshapes/JST_XA_S02B-XASK-1_1x02_P2.50mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(at 110 66.25)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C5"
			(at -2.75 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "0.1u"
			(at 0 1.68 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "MatrixDriver.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.212766)
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.212766)
			(net 3 "Net-(D1-K)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(at 138.5 58.75)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R3"
			(at 2.75 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 0 1.65 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "MatrixDriver.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.208333)
			(net 26 "A2")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.208333)
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(at 157.75 63.75 180)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R8"
			(at -2.75 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 0 1.65 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "MatrixDriver.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1 0 180)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.208333)
			(net 34 "Net-(R7-Pad2)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1 0 180)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.208333)
			(net 35 "Net-(U4-FB)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Jumper:SolderJumper-2_P1.3mm_Open_RoundedPad1.0x1.5mm"
		(layer "F.Cu")
		(at 123.25 82 180)
		(descr "SMD Solder Jumper, 1x1.5mm, rounded Pads, 0.3mm gap, open")
		(tags "solder jumper open")
		(property "Reference" "JP7"
			(at 3 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "Pullup_en"
			(at 0 1.9 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Jumper:SolderJumper-2_P1.3mm_Open_RoundedPad1.0x1.5mm"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Solder Jumper, 2-pole, open"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SolderJumper*Open*")
		(sheetname "Root")
		(sheetfile "MatrixDriver.kicad_sch")
		(zone_connect 1)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "1" smd custom
			(at -0.65 0 180)
			(size 1 0.5)
			(layers "F.Cu" "F.Mask")
			(net 39 "Net-(JP7-A)")
			(pinfunction "A")
			(pintype "passive")
			(zone_connect 2)
			(thermal_bridge_angle 45)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_circle
					(center 0 0.25)
					(end 0.5 0.25)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0 -0.25)
					(end 0.5 -0.25)
					(width 0)
					(fill yes)
				)
				(gr_poly
					(pts
						(xy 0.5 0.75) (xy 0 0.75) (xy 0 -0.75) (xy 0.5 -0.75)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "2" smd custom
			(at 0.65 0 180)
			(size 1 0.5)
			(layers "F.Cu" "F.Mask")
			(net 3 "Net-(D1-K)")
			(pinfunction "B")
			(pintype "passive")
			(zone_connect 2)
			(thermal_bridge_angle 45)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_circle
					(center 0 0.25)
					(end 0.5 0.25)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0 -0.25)
					(end 0.5 -0.25)
					(width 0)
					(fill yes)
				)
				(gr_poly
					(pts
						(xy 0 0.75) (xy -0.5 0.75) (xy -0.5 -0.75) (xy 0 -0.75)
					)
					(width 0)
					(fill yes)
				)
			)
		)
	)
	(footprint "Jumper:SolderJumper-2_P1.3mm_Open_RoundedPad1.0x1.5mm"
		(layer "F.Cu")
		(at 113.5 73.5)
		(descr "SMD Solder Jumper, 1x1.5mm, rounded Pads, 0.3mm gap, open")
		(tags "solder jumper open")
		(property "Reference" "JP2"
			(at 0 2 0)
			(layer "F.SilkS")
		)
		(property "Value" "PWR_DCDC"
			(at 0 1.9 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Jumper:SolderJumper-2_P1.3mm_Open_RoundedPad1.0x1.5mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Solder Jumper, 2-pole, open"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SolderJumper*Open*")
		(sheetname "Root")
		(sheetfile "MatrixDriver.kicad_sch")
		(zone_connect 1)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "1" smd custom
			(at -0.65 0)
			(size 1 0.5)
			(layers "F.Cu" "F.Mask")
			(net 3 "Net-(D1-K)")
			(pinfunction "A")
			(pintype "passive")
			(zone_connect 2)
			(thermal_bridge_angle 45)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_circle
					(center 0 0.25)
					(end 0.5 0.25)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0 -0.25)
					(end 0.5 -0.25)
					(width 0)
					(fill yes)
				)
				(gr_poly
					(pts
						(xy 0.5 0.75) (xy 0 0.75) (xy 0 -0.75) (xy 0.5 -0.75)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "2" smd custom
			(at 0.65 0)
			(size 1 0.5)
			(layers "F.Cu" "F.Mask")
			(net 2 "+5V")
			(pinfunction "B")
			(pintype "passive")
			(zone_connect 2)
			(thermal_bridge_angle 45)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_circle
					(center 0 0.25)
					(end 0.5 0.25)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0 -0.25)
					(end 0.5 -0.25)
					(width 0)
					(fill yes)
				)
				(gr_poly
					(pts
						(xy 0 0.75) (xy -0.5 0.75) (xy -0.5 -0.75) (xy 0 -0.75)
					)
					(width 0)
					(fill yes)
				)
			)
		)
	)
	(footprint "Package_QFP:TQFP-32_7x7mm_P0.8mm"
		(layer "F.Cu")
		(at 120 61.25 135)
		(descr "32-Lead Plastic Thin Quad Flatpack (PT) - 7x7x1.0 mm Body, 2.00 mm [TQFP] (see Microchip Packaging Specification 00000049BS.pdf)")
		(tags "QFP 0.8")
		(property "Reference" "U2"
			(at 0 -6.05 135)
			(layer "F.SilkS")
		)
		(property "Value" "AVR128DA32x-xPT"
			(at 0 6.05 135)
			(layer "F.Fab")
		)
		(property "Footprint" "Package_QFP:TQFP-32_7x7mm_P0.8mm"
			(at 0 0 135)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/AVR128DA28-32-48-64-DataSheet-DS40002183B.pdf"
			(at 0 0 135)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "24MHz, 128kB Flash, 16kB SRAM, EEPROM with Touch Sensing, TQFP-32"
			(at 0 0 135)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TQFP*7x7mm*P0.8mm*")
		(sheetname "Root")
		(sheetfile "MatrixDriver.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 135)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -4.25 -2.8 135)
			(size 1.6 0.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 10 "SCL")
			(pinfunction "PA3")
			(pintype "bidirectional")
		)
		(pad "2" smd rect
			(at -4.25 -2 135)
			(size 1.6 0.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 37 "Temp")
			(pinfunction "PA4")
			(pintype "bidirectional")
		)
		(pad "3" smd rect
			(at -4.25 -1.2 135)
			(size 1.6 0.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 12 "A0")
			(pinfunction "PA5")
			(pintype "bidirectional")
		)
		(pad "4" smd rect
			(at -4.25 -0.4 135)
			(size 1.6 0.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 25 "A1")
			(pinfunction "PA6")
			(pintype "bidirectional")
		)
		(pad "5" smd rect
			(at -4.25 0.4 135)
			(size 1.6 0.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 26 "A2")
			(pinfunction "PA7")
			(pintype "bidirectional")
		)
		(pad "6" smd rect
			(at -4.25 1.2 135)
			(size 1.6 0.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 22 "OE")
			(pinfunction "PC0")
			(pintype "bidirectional")
		)
		(pad "7" smd rect
			(at -4.25 2 135)
			(size 1.6 0.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 16 "LAT")
			(pinfunction "PC1")
			(pintype "bidirectional")
		)
		(pad "8" smd rect
			(at -4.25 2.8 135)
			(size 1.6 0.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 19 "CLK")
			(pinfunction "PC2")
			(pintype "bidirectional")
		)
		(pad "9" smd rect
			(at -2.8 4.25 225)
			(size 1.6 0.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 27 "A3")
			(pinfunction "PC3")
			(pintype "bidirectional")
		)
		(pad "10" smd rect
			(at -2 4.25 225)
			(size 1.6 0.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 17 "R1")
			(pinfunction "PD0")
			(pintype "bidirectional")
		)
		(pad "11" smd rect
			(at -1.2 4.25 225)
			(size 1.6 0.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 21 "G1")
			(pinfunction "PD1")
			(pintype "bidirectional")
		)
		(pad "12" smd rect
			(at -0.4 4.25 225)
			(size 1.6 0.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 14 "B1")
			(pinfunction "PD2")
			(pintype "bidirectional")
		)
		(pad "13" smd rect
			(at 0.4 4.25 225)
			(size 1.6 0.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 18 "R2")
			(pinfunction "PD3")
			(pintype "bidirectional")
		)
		(pad "14" smd rect
			(at 1.2 4.25 225)
			(size 1.6 0.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 15 "G2")
			(pinfunction "PD4")
			(pintype "bidirectional")
		)
		(pad "15" smd rect
			(at 2 4.25 225)
			(size 1.6 0.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 23 "B2")
			(pinfunction "PD5")
			(pintype "bidirectional")
		)
		(pad "16" smd rect
			(at 2.8 4.25 225)
			(size 1.6 0.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 31 "unconnected-(U2-PD6-Pad16)")
			(pinfunction "PD6")
			(pintype "bidirectional")
		)
		(pad "17" smd rect
			(at 4.25 2.8 135)
			(size 1.6 0.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 30 "unconnected-(U2-VREFA{slash}PD7-Pad17)")
			(pinfunction "VREFA/PD7")
			(pintype "bidirectional")
		)
		(pad "18" smd rect
			(at 4.25 2 135)
			(size 1.6 0.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 3 "Net-(D1-K)")
			(pinfunction "AVDD")
			(pintype "power_in")
		)
		(pad "19" smd rect
			(at 4.25 1.2 135)
			(size 1.6 0.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "20" smd rect
			(at 4.25 0.4 135)
			(size 1.6 0.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 20 "A")
			(pinfunction "XTAL32K1/PF0")
			(pintype "bidirectional")
		)
		(pad "21" smd rect
			(at 4.25 -0.4 135)
			(size 1.6 0.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 13 "B")
			(pinfunction "XTAL32K2/PF1")
			(pintype "bidirectional")
		)
		(pad "22" smd rect
			(at 4.25 -1.2 135)
			(size 1.6 0.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 24 "C")
			(pinfunction "PF2")
			(pintype "bidirectional")
		)
		(pad "23" smd rect
			(at 4.25 -2 135)
			(size 1.6 0.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 7 "D")
			(pinfunction "PF3")
			(pintype "bidirectional")
		)
		(pad "24" smd rect
			(at 4.25 -2.8 135)
			(size 1.6 0.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 6 "E")
			(pinfunction "PF4")
			(pintype "bidirectional")
		)
		(pad "25" smd rect
			(at 2.8 -4.25 225)
			(size 1.6 0.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 40 "unconnected-(U2-PF5-Pad25)")
			(pinfunction "PF5")
			(pintype "bidirectional")
		)
		(pad "26" smd rect
			(at 2 -4.25 225)
			(size 1.6 0.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 38 "Net-(U2-~{RESET}{slash}PF6)")
			(pinfunction "~{RESET}/PF6")
			(pintype "bidirectional")
		)
		(pad "27" smd rect
			(at 1.2 -4.25 225)
			(size 1.6 0.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 28 "UPDI")
			(pinfunction "UPDI")
			(pintype "input")
		)
		(pad "28" smd rect
			(at 0.4 -4.25 225)
			(size 1.6 0.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 3 "Net-(D1-K)")
			(pinfunction "VDD")
			(pintype "power_in")
		)
		(pad "29" smd rect
			(at -0.4 -4.25 225)
			(size 1.6 0.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "30" smd rect
			(at -1.2 -4.25 225)
			(size 1.6 0.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 9 "UART_TX")
			(pinfunction "PA0")
			(pintype "bidirectional")
		)
		(pad "31" smd rect
			(at -2 -4.25 225)
			(size 1.6 0.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 8 "UART_RX")
			(pinfunction "PA1")
			(pintype "bidirectional")
		)
		(pad "32" smd rect
			(at -2.8 -4.25 225)
			(size 1.6 0.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 11 "SDA")
			(pinfunction "PA2")
			(pintype "bidirectional")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_QFP.3dshapes/TQFP-32_7x7mm_P0.8mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Jumper:SolderJumper-2_P1.3mm_Open_RoundedPad1.0x1.5mm"
		(layer "F.Cu")
		(at 123.25 79.5 180)
		(descr "SMD Solder Jumper, 1x1.5mm, rounded Pads, 0.3mm gap, open")
		(tags "solder jumper open")
		(property "Reference" "JP8"
			(at 3 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "Pullup_en"
			(at 0 1.9 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Jumper:SolderJumper-2_P1.3mm_Open_RoundedPad1.0x1.5mm"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Solder Jumper, 2-pole, open"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SolderJumper*Open*")
		(sheetname "Root")
		(sheetfile "MatrixDriver.kicad_sch")
		(zone_connect 1)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "1" smd custom
			(at -0.65 0 180)
			(size 1 0.5)
			(layers "F.Cu" "F.Mask")
			(net 41 "Net-(JP8-A)")
			(pinfunction "A")
			(pintype "passive")
			(zone_connect 2)
			(thermal_bridge_angle 45)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_circle
					(center 0 0.25)
					(end 0.5 0.25)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0 -0.25)
					(end 0.5 -0.25)
					(width 0)
					(fill yes)
				)
				(gr_poly
					(pts
						(xy 0.5 0.75) (xy 0 0.75) (xy 0 -0.75) (xy 0.5 -0.75)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "2" smd custom
			(at 0.65 0 180)
			(size 1 0.5)
			(layers "F.Cu" "F.Mask")
			(net 3 "Net-(D1-K)")
			(pinfunction "B")
			(pintype "passive")
			(zone_connect 2)
			(thermal_bridge_angle 45)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_circle
					(center 0 0.25)
					(end 0.5 0.25)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0 -0.25)
					(end 0.5 -0.25)
					(width 0)
					(fill yes)
				)
				(gr_poly
					(pts
						(xy 0 0.75) (xy -0.5 0.75) (xy -0.5 -0.75) (xy 0 -0.75)
					)
					(width 0)
					(fill yes)
				)
			)
		)
	)
	(footprint "Jumper:SolderJumper-2_P1.3mm_Open_RoundedPad1.0x1.5mm"
		(layer "F.Cu")
		(at 133.5 61.25)
		(descr "SMD Solder Jumper, 1x1.5mm, rounded Pads, 0.3mm gap, open")
		(tags "solder jumper open")
		(property "Reference" "JP4"
			(at -3 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "Add0010"
			(at 0 1.9 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Jumper:SolderJumper-2_P1.3mm_Open_RoundedPad1.0x1.5mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Solder Jumper, 2-pole, open"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SolderJumper*Open*")
		(sheetname "Root")
		(sheetfile "MatrixDriver.kicad_sch")
		(zone_connect 1)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "1" smd custom
			(at -0.65 0)
			(size 1 0.5)
			(layers "F.Cu" "F.Mask")
			(net 25 "A1")
			(pinfunction "A")
			(pintype "passive")
			(zone_connect 2)
			(thermal_bridge_angle 45)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_circle
					(center 0 0.25)
					(end 0.5 0.25)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0 -0.25)
					(end 0.5 -0.25)
					(width 0)
					(fill yes)
				)
				(gr_poly
					(pts
						(xy 0.5 0.75) (xy 0 0.75) (xy 0 -0.75) (xy 0.5 -0.75)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "2" smd custom
			(at 0.65 0)
			(size 1 0.5)
			(layers "F.Cu" "F.Mask")
			(net 3 "Net-(D1-K)")
			(pinfunction "B")
			(pintype "passive")
			(zone_connect 2)
			(thermal_bridge_angle 45)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_circle
					(center 0 0.25)
					(end 0.5 0.25)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0 -0.25)
					(end 0.5 -0.25)
					(width 0)
					(fill yes)
				)
				(gr_poly
					(pts
						(xy 0 0.75) (xy -0.5 0.75) (xy -0.5 -0.75) (xy 0 -0.75)
					)
					(width 0)
					(fill yes)
				)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(at 149.75 73.75)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C2"
			(at -2.75 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "4.7u"
			(at 0 1.68 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "MatrixDriver.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.212766)
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.212766)
			(net 5 "Net-(J1-Pin_1)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(at 138.5 61.25)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R2"
			(at 2.75 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 0 1.65 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "MatrixDriver.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.208333)
			(net 25 "A1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.208333)
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_JST:JST_PH_S4B-PH-SM4-TB_1x04-1MP_P2.00mm_Horizontal"
		(layer "F.Cu")
		(at 112.5 88.6)
		(descr "JST PH series connector, S4B-PH-SM4-TB (http://www.jst-mfg.com/product/pdf/eng/ePH.pdf), generated with kicad-footprint-generator")
		(tags "connector JST PH horizontal")
		(property "Reference" "J4"
			(at -7.5 -4 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TWI 01"
			(at 0 5.8 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_JST:JST_PH_S4B-PH-SM4-TB_1x04-1MP_P2.00mm_Horizontal"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x04, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "Root")
		(sheetfile "MatrixDriver.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 1.5 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -3 -2.85)
			(size 1 3.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "VDD")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at -1 -2.85)
			(size 1 3.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at 1 -2.85)
			(size 1 3.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 11 "SDA")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" smd roundrect
			(at 3 -2.85)
			(size 1 3.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 10 "SCL")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "MP" smd roundrect
			(at -5.35 2.9)
			(size 1.5 3.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.166667)
		)
		(pad "MP" smd roundrect
			(at 5.35 2.9)
			(size 1.5 3.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.166667)
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_JST.3dshapes/JST_PH_S4B-PH-SM4-TB_1x04-1MP_P2.00mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(at 157.75 71.25)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R11"
			(at 3.25 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 0 1.65 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "MatrixDriver.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.208333)
			(net 36 "Net-(R10-Pad2)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.208333)
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23-6"
		(layer "F.Cu")
		(at 153.75 72.25 -90)
		(descr "SOT, 6 Pin (https://www.jedec.org/sites/default/files/docs/Mo-178c.PDF variant AB), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "U4"
			(at -2.5 -1 180)
			(layer "F.SilkS")
		)
		(property "Value" "TPS54202 / TPS54302"
			(at 0 2.4 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps54202.pdf"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "2A, 4.5 to 28V Input, EMI Friendly integrated switch synchronous step-down regulator, pulse-skipping, SOT-23-6"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SOT?23*")
		(sheetname "Root")
		(sheetfile "MatrixDriver.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.1375 -0.95 270)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "2" smd roundrect
			(at -1.1375 0 270)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 29 "Net-(U4-SW)")
			(pinfunction "SW")
			(pintype "power_out")
		)
		(pad "3" smd roundrect
			(at -1.1375 0.95 270)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 5 "Net-(J1-Pin_1)")
			(pinfunction "VIN")
			(pintype "power_in")
		)
		(pad "4" smd roundrect
			(at 1.1375 0.95 270)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 35 "Net-(U4-FB)")
			(pinfunction "FB")
			(pintype "input")
		)
		(pad "5" smd roundrect
			(at 1.1375 0 270)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 33 "Net-(U4-EN)")
			(pinfunction "EN")
			(pintype "input")
		)
		(pad "6" smd roundrect
			(at 1.1375 -0.95 270)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 32 "Net-(U4-BOOT)")
			(pinfunction "BOOT")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-6.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(at 110 63.75)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C4"
			(at -2.75 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "4.7u"
			(at 0 1.68 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "MatrixDriver.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.212766)
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.212766)
			(net 3 "Net-(D1-K)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(at 110 61.25)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R12"
			(at -3.25 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 0 1.65 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "MatrixDriver.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.208333)
			(net 3 "Net-(D1-K)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.208333)
			(net 38 "Net-(U2-~{RESET}{slash}PF6)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_SMD:D_SMA"
		(layer "F.Cu")
		(at 111.5 69.5 180)
		(descr "Diode SMA (DO-214AC)")
		(tags "Diode SMA (DO-214AC)")
		(property "Reference" "D1"
			(at 4.5 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "3SMAJ5919B-TP"
			(at 0 2.6 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Diode_SMD:D_SMA"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Zener diode"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TO-???* *_Diode_* *SingleDiode* D_*")
		(sheetname "Root")
		(sheetfile "MatrixDriver.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -2.5 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2 0 180)
			(size 2.5 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.1388888889)
			(net 3 "Net-(D1-K)")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 2 0 180)
			(size 2.5 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.1388888889)
			(net 1 "GND")
			(pinfunction "A")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SMA.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(at 138.5 63.75)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R1"
			(at 2.75 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 0 1.65 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "MatrixDriver.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.208333)
			(net 12 "A0")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.208333)
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Jumper:SolderJumper-2_P1.3mm_Open_RoundedPad1.0x1.5mm"
		(layer "F.Cu")
		(at 109.5 73.5 180)
		(descr "SMD Solder Jumper, 1x1.5mm, rounded Pads, 0.3mm gap, open")
		(tags "solder jumper open")
		(property "Reference" "JP1"
			(at 0 -2 0)
			(layer "F.SilkS")
		)
		(property "Value" "PWR_TWI"
			(at 0 1.9 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Jumper:SolderJumper-2_P1.3mm_Open_RoundedPad1.0x1.5mm"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Solder Jumper, 2-pole, open"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SolderJumper*Open*")
		(sheetname "Root")
		(sheetfile "MatrixDriver.kicad_sch")
		(zone_connect 1)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "1" smd custom
			(at -0.65 0 180)
			(size 1 0.5)
			(layers "F.Cu" "F.Mask")
			(net 3 "Net-(D1-K)")
			(pinfunction "A")
			(pintype "passive")
			(zone_connect 2)
			(thermal_bridge_angle 45)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_circle
					(center 0 0.25)
					(end 0.5 0.25)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0 -0.25)
					(end 0.5 -0.25)
					(width 0)
					(fill yes)
				)
				(gr_poly
					(pts
						(xy 0.5 0.75) (xy 0 0.75) (xy 0 -0.75) (xy 0.5 -0.75)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "2" smd custom
			(at 0.65 0 180)
			(size 1 0.5)
			(layers "F.Cu" "F.Mask")
			(net 4 "VDD")
			(pinfunction "B")
			(pintype "passive")
			(zone_connect 2)
			(thermal_bridge_angle 45)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_circle
					(center 0 0.25)
					(end 0.5 0.25)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0 -0.25)
					(end 0.5 -0.25)
					(width 0)
					(fill yes)
				)
				(gr_poly
					(pts
						(xy 0 0.75) (xy -0.5 0.75) (xy -0.5 -0.75) (xy 0 -0.75)
					)
					(width 0)
					(fill yes)
				)
			)
		)
	)
	(footprint "Connector_JST:JST_PH_S4B-PH-SM4-TB_1x04-1MP_P2.00mm_Horizontal"
		(layer "F.Cu")
		(at 127.5 88.5)
		(descr "JST PH series connector, S4B-PH-SM4-TB (http://www.jst-mfg.com/product/pdf/eng/ePH.pdf), generated with kicad-footprint-generator")
		(tags "connector JST PH horizontal")
		(property "Reference" "J6"
			(at -7.5 -4 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TWI 02"
			(at 0 5.8 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_JST:JST_PH_S4B-PH-SM4-TB_1x04-1MP_P2.00mm_Horizontal"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x04, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "Root")
		(sheetfile "MatrixDriver.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 1.5 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -3 -2.85)
			(size 1 3.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "VDD")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at -1 -2.85)
			(size 1 3.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at 1 -2.85)
			(size 1 3.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 11 "SDA")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" smd roundrect
			(at 3 -2.85)
			(size 1 3.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 10 "SCL")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "MP" smd roundrect
			(at -5.35 2.9)
			(size 1.5 3.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.166667)
		)
		(pad "MP" smd roundrect
			(at 5.35 2.9)
			(size 1.5 3.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.166667)
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_JST.3dshapes/JST_PH_S4B-PH-SM4-TB_1x04-1MP_P2.00mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Jumper:SolderJumper-2_P1.3mm_Open_RoundedPad1.0x1.5mm"
		(layer "F.Cu")
		(at 133.5 63.75)
		(descr "SMD Solder Jumper, 1x1.5mm, rounded Pads, 0.3mm gap, open")
		(tags "solder jumper open")
		(property "Reference" "JP3"
			(at -3 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "Add0001"
			(at 0 1.9 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Jumper:SolderJumper-2_P1.3mm_Open_RoundedPad1.0x1.5mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Solder Jumper, 2-pole, open"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SolderJumper*Open*")
		(sheetname "Root")
		(sheetfile "MatrixDriver.kicad_sch")
		(zone_connect 1)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "1" smd custom
			(at -0.65 0)
			(size 1 0.5)
			(layers "F.Cu" "F.Mask")
			(net 12 "A0")
			(pinfunction "A")
			(pintype "passive")
			(zone_connect 2)
			(thermal_bridge_angle 45)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_circle
					(center 0 0.25)
					(end 0.5 0.25)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0 -0.25)
					(end 0.5 -0.25)
					(width 0)
					(fill yes)
				)
				(gr_poly
					(pts
						(xy 0.5 0.75) (xy 0 0.75) (xy 0 -0.75) (xy 0.5 -0.75)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "2" smd custom
			(at 0.65 0)
			(size 1 0.5)
			(layers "F.Cu" "F.Mask")
			(net 3 "Net-(D1-K)")
			(pinfunction "B")
			(pintype "passive")
			(zone_connect 2)
			(thermal_bridge_angle 45)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_circle
					(center 0 0.25)
					(end 0.5 0.25)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0 -0.25)
					(end 0.5 -0.25)
					(width 0)
					(fill yes)
				)
				(gr_poly
					(pts
						(xy 0 0.75) (xy -0.5 0.75) (xy -0.5 -0.75) (xy 0 -0.75)
					)
					(width 0)
					(fill yes)
				)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(at 157.75 73.75 180)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C6"
			(at -2.75 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "0.1u"
			(at 0 1.68 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "MatrixDriver.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.0375 0 180)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.212766)
			(net 29 "Net-(U4-SW)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.0375 0 180)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.212766)
			(net 32 "Net-(U4-BOOT)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_JST:JST_XA_S02B-XASK-1_1x02_P2.50mm_Horizontal"
		(layer "F.Cu")
		(at 144.5 50 180)
		(descr "JST XA series connector, S02B-XASK-1 (http://www.jst-mfg.com/product/pdf/eng/eXA1.pdf), generated with kicad-footprint-generator")
		(tags "connector JST XA horizontal hook")
		(property "Reference" "J3"
			(at 1.25 -4.6 180)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "5V OUT"
			(at 1.25 10.4 180)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_JST:JST_XA_S02B-XASK-1_1x02_P2.50mm_Horizontal"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "Root")
		(sheetfile "MatrixDriver.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.25 2.5 180)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole oval
			(at 1.25 6.5 180)
			(size 2.8 2)
			(drill oval 2.8 2)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" thru_hole roundrect
			(at 0 0 180)
			(size 1.7 1.95)
			(drill 0.95)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.147059)
			(net 2 "+5V")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 2.5 0 180)
			(size 1.7 1.95)
			(drill 0.95)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_JST.3dshapes/JST_XA_S02B-XASK-1_1x02_P2.50mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(at 127.5 82)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R14"
			(at 3.25 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 0 1.65 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "MatrixDriver.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.208333)
			(net 39 "Net-(JP7-A)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.208333)
			(net 11 "SDA")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(at 138.5 56.25)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R4"
			(at 2.75 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 0 1.65 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "MatrixDriver.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.208333)
			(net 27 "A3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.208333)
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Kicad_Libs:Formfactor"
		(locked yes)
		(layer "F.Cu")
		(at 135 44)
		(property "Reference" "J8"
			(at -38.75 -0.75 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Housing"
			(at -30.5 -2.5 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" "Kicad_Libs:Formfactor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x01, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "Root")
		(sheetfile "MatrixDriver.kicad_sch")
		(fp_line
			(start -45 48)
			(end -45 -2)
			(layer "Edge.Cuts")
		)
		(fp_line
			(start -43 -4)
			(end 38 -4)
			(layer "Edge.Cuts")
		)
		(fp_line
			(start 38 50)
			(end -43 50)
			(layer "Edge.Cuts")
		)
		(fp_line
			(start 40 -2)
			(end 40 48)
			(layer "Edge.Cuts")
		)
		(fp_arc
			(start -45 -2)
			(mid -44.414214 -3.414214)
			(end -43 -4)
			(layer "Edge.Cuts")
		)
		(fp_arc
			(start -43 50)
			(mid -44.414214 49.414214)
			(end -45 48)
			(layer "Edge.Cuts")
		)
		(fp_arc
			(start 38 -4)
			(mid 39.414214 -3.414214)
			(end 40 -2)
			(layer "Edge.Cuts")
		)
		(fp_arc
			(start 40 48)
			(mid 39.414214 49.414214)
			(end 38 50)
			(layer "Edge.Cuts")
		)
		(fp_text user "${REFERENCE}"
			(at -30.5 -1 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(dimension
			(type aligned)
			(layer "F.Fab")
			(pts
				(xy 90 42) (xy 175 42)
			)
			(height -7)
			(gr_text "85,0000 mm"
				(at 132.5 33.85 0)
				(layer "F.Fab")
			)
			(format
				(prefix "")
				(suffix "")
				(units 3)
				(units_format 1)
				(precision 4)
			)
			(style
				(thickness 0.1)
				(arrow_length 1.27)
				(text_position_mode 0)
				(extension_height 0.58642)
				(extension_offset 0.5) keep_text_aligned)
		)
		(dimension
			(type aligned)
			(layer "F.Fab")
			(pts
				(xy 92 40) (xy 92 94)
			)
			(height 5)
			(gr_text "54,0000 mm"
				(at 85.85 67 90)
				(layer "F.Fab")
			)
			(format
				(prefix "")
				(suffix "")
				(units 3)
				(units_format 1)
				(precision 4)
			)
			(style
				(thickness 0.1)
				(arrow_length 1.27)
				(text_position_mode 0)
				(extension_height 0.58642)
				(extension_offset 0.5) keep_text_aligned)
		)
		(pad "1" thru_hole circle
			(at -42.75 2 180)
			(size 0.6 0.6)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "1" thru_hole circle
			(at -42.75 44 180)
			(size 0.6 0.6)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "1" thru_hole circle
			(at -41.651651 -0.651651 180)
			(size 0.6 0.6)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "1" thru_hole circle
			(at -41.651651 41.348349 180)
			(size 0.6 0.6)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "1" thru_hole circle
			(at -41.65165 4.65165 180)
			(size 0.6 0.6)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "1" thru_hole circle
			(at -41.65165 46.65165 180)
			(size 0.6 0.6)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "1" thru_hole circle
			(at -39 -1.75 180)
			(size 0.6 0.6)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "1" thru_hole circle
			(at -39 2 180)
			(size 10 10)
			(drill 5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "1" thru_hole circle
			(at -39 5.75 180)
			(size 0.6 0.6)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "1" thru_hole circle
			(at -39 40.25 180)
			(size 0.6 0.6)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "1" thru_hole circle
			(at -39 44 270)
			(size 10 10)
			(drill 5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "1" thru_hole circle
			(at -39 47.75 180)
			(size 0.6 0.6)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "1" thru_hole circle
			(at -36.34835 4.65165 180)
			(size 0.6 0.6)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "1" thru_hole circle
			(at -36.34835 46.65165 180)
			(size 0.6 0.6)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "1" thru_hole circle
			(at -36.348349 -0.651651 180)
			(size 0.6 0.6)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "1" thru_hole circle
			(at -36.348349 41.348349 180)
			(size 0.6 0.6)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "1" thru_hole circle
			(at -35.25 2 180)
			(size 0.6 0.6)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "1" thru_hole circle
			(at -35.25 44 180)
			(size 0.6 0.6)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "1" thru_hole circle
			(at 30.25 2 180)
			(size 0.6 0.6)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "1" thru_hole circle
			(at 30.25 44 180)
			(size 0.6 0.6)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "1" thru_hole circle
			(at 31.348349 -0.651651 180)
			(size 0.6 0.6)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "1" thru_hole circle
			(at 31.348349 41.348349 180)
			(size 0.6 0.6)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "1" thru_hole circle
			(at 31.34835 4.65165 180)
			(size 0.6 0.6)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "1" thru_hole circle
			(at 31.34835 46.65165 180)
			(size 0.6 0.6)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "1" thru_hole circle
			(at 34 -1.75 180)
			(size 0.6 0.6)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "1" thru_hole circle
			(at 34 2 90)
			(size 10 10)
			(drill 5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "1" thru_hole circle
			(at 34 5.75 180)
			(size 0.6 0.6)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "1" thru_hole circle
			(at 34 40.25 180)
			(size 0.6 0.6)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "1" thru_hole circle
			(at 34 44)
			(size 10 10)
			(drill 5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "1" thru_hole circle
			(at 34 47.75 180)
			(size 0.6 0.6)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "1" thru_hole circle
			(at 36.65165 4.65165 180)
			(size 0.6 0.6)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "1" thru_hole circle
			(at 36.65165 46.65165 180)
			(size 0.6 0.6)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "1" thru_hole circle
			(at 36.651651 -0.651651 180)
			(size 0.6 0.6)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "1" thru_hole circle
			(at 36.651651 41.348349 180)
			(size 0.6 0.6)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "1" thru_hole circle
			(at 37.75 2 180)
			(size 0.6 0.6)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "1" thru_hole circle
			(at 37.75 44 180)
			(size 0.6 0.6)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
	)
	(footprint "Connector_IDC:IDC-Header_2x08_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 128.89 45.9975 -90)
		(descr "Through hole IDC box header, 2x08, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0")
		(tags "Through hole vertical IDC box header THT 2x08 2.54mm double row")
		(property "Reference" "J5"
			(at 1.27 -6.1 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "HUB75 OUT"
			(at 1.27 23.88 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_IDC:IDC-Header_2x08_P2.54mm_Vertical"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, double row, 02x08, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_2x??_*")
		(sheetname "Root")
		(sheetfile "MatrixDriver.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole roundrect
			(at 0 0 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.147059)
			(net 17 "R1")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.54 0 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 21 "G1")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at 0 2.54 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "B1")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole circle
			(at 2.54 2.54 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "5" thru_hole circle
			(at 0 5.08 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 18 "R2")
			(pinfunction "Pin_5")
			(pintype "passive")
		)
		(pad "6" thru_hole circle
			(at 2.54 5.08 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "G2")
			(pinfunction "Pin_6")
			(pintype "passive")
		)
		(pad "7" thru_hole circle
			(at 0 7.62 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 23 "B2")
			(pinfunction "Pin_7")
			(pintype "passive")
		)
		(pad "8" thru_hole circle
			(at 2.54 7.62 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "E")
			(pinfunction "Pin_8")
			(pintype "passive")
		)
		(pad "9" thru_hole circle
			(at 0 10.16 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 20 "A")
			(pinfunction "Pin_9")
			(pintype "passive")
		)
		(pad "10" thru_hole circle
			(at 2.54 10.16 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "B")
			(pinfunction "Pin_10")
			(pintype "passive")
		)
		(pad "11" thru_hole circle
			(at 0 12.7 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 24 "C")
			(pinfunction "Pin_11")
			(pintype "passive")
		)
		(pad "12" thru_hole circle
			(at 2.54 12.7 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "D")
			(pinfunction "Pin_12")
			(pintype "passive")
		)
		(pad "13" thru_hole circle
			(at 0 15.24 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 19 "CLK")
			(pinfunction "Pin_13")
			(pintype "passive")
		)
		(pad "14" thru_hole circle
			(at 2.54 15.24 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 16 "LAT")
			(pinfunction "Pin_14")
			(pintype "passive")
		)
		(pad "15" thru_hole circle
			(at 0 17.78 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 22 "OE")
			(pinfunction "Pin_15")
			(pintype "passive")
		)
		(pad "16" thru_hole circle
			(at 2.54 17.78 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_16")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_IDC.3dshapes/IDC-Header_2x08_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23"
		(layer "F.Cu")
		(at 146 65)
		(descr "SOT, 3 Pin (https://www.jedec.org/system/files/docs/to-236h.pdf variant AB), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "U3"
			(at 0 -2.4 0)
			(layer "F.SilkS")
		)
		(property "Value" "MCP9700Ax-ETT"
			(at 0 2.4 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/devicedoc/20001942g.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Low power, analog thermistor temperature sensor, ±2C accuracy, -40C to +125C, in SOT-23-3"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SOT?23*")
		(sheetname "Root")
		(sheetfile "MatrixDriver.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 -0.95)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 3 "Net-(D1-K)")
			(pinfunction "V_{DD}")
			(pintype "power_in")
		)
		(pad "2" smd roundrect
			(at -0.9375 0.95)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 37 "Temp")
			(pinfunction "V_{OUT}")
			(pintype "output")
		)
		(pad "3" smd roundrect
			(at 0.9375 0)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(at 157.75 68.75)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R10"
			(at 3.25 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 0 1.65 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "MatrixDriver.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.208333)
			(net 35 "Net-(U4-FB)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.208333)
			(net 36 "Net-(R10-Pad2)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(at 149.75 76.25)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C3"
			(at -2.75 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "0.1u"
			(at 0 1.68 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "MatrixDriver.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.212766)
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.212766)
			(net 5 "Net-(J1-Pin_1)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Jumper:SolderJumper-2_P1.3mm_Open_RoundedPad1.0x1.5mm"
		(layer "F.Cu")
		(at 133.5 56.25)
		(descr "SMD Solder Jumper, 1x1.5mm, rounded Pads, 0.3mm gap, open")
		(tags "solder jumper open")
		(property "Reference" "JP6"
			(at -3 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "Add1000"
			(at 0 1.9 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Jumper:SolderJumper-2_P1.3mm_Open_RoundedPad1.0x1.5mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Solder Jumper, 2-pole, open"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SolderJumper*Open*")
		(sheetname "Root")
		(sheetfile "MatrixDriver.kicad_sch")
		(zone_connect 1)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "1" smd custom
			(at -0.65 0)
			(size 1 0.5)
			(layers "F.Cu" "F.Mask")
			(net 27 "A3")
			(pinfunction "A")
			(pintype "passive")
			(zone_connect 2)
			(thermal_bridge_angle 45)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_circle
					(center 0 0.25)
					(end 0.5 0.25)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0 -0.25)
					(end 0.5 -0.25)
					(width 0)
					(fill yes)
				)
				(gr_poly
					(pts
						(xy 0.5 0.75) (xy 0 0.75) (xy 0 -0.75) (xy 0.5 -0.75)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "2" smd custom
			(at 0.65 0)
			(size 1 0.5)
			(layers "F.Cu" "F.Mask")
			(net 3 "Net-(D1-K)")
			(pinfunction "B")
			(pintype "passive")
			(zone_connect 2)
			(thermal_bridge_angle 45)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_circle
					(center 0 0.25)
					(end 0.5 0.25)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0 -0.25)
					(end 0.5 -0.25)
					(width 0)
					(fill yes)
				)
				(gr_poly
					(pts
						(xy 0 0.75) (xy -0.5 0.75) (xy -0.5 -0.75) (xy 0 -0.75)
					)
					(width 0)
					(fill yes)
				)
			)
		)
	)
	(footprint "Jumper:SolderJumper-2_P1.3mm_Open_RoundedPad1.0x1.5mm"
		(layer "F.Cu")
		(at 133.5 58.75)
		(descr "SMD Solder Jumper, 1x1.5mm, rounded Pads, 0.3mm gap, open")
		(tags "solder jumper open")
		(property "Reference" "JP5"
			(at -3 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "Add0100"
			(at 0 1.9 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Jumper:SolderJumper-2_P1.3mm_Open_RoundedPad1.0x1.5mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Solder Jumper, 2-pole, open"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SolderJumper*Open*")
		(sheetname "Root")
		(sheetfile "MatrixDriver.kicad_sch")
		(zone_connect 1)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "1" smd custom
			(at -0.65 0)
			(size 1 0.5)
			(layers "F.Cu" "F.Mask")
			(net 26 "A2")
			(pinfunction "A")
			(pintype "passive")
			(zone_connect 2)
			(thermal_bridge_angle 45)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_circle
					(center 0 0.25)
					(end 0.5 0.25)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0 -0.25)
					(end 0.5 -0.25)
					(width 0)
					(fill yes)
				)
				(gr_poly
					(pts
						(xy 0.5 0.75) (xy 0 0.75) (xy 0 -0.75) (xy 0.5 -0.75)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "2" smd custom
			(at 0.65 0)
			(size 1 0.5)
			(layers "F.Cu" "F.Mask")
			(net 3 "Net-(D1-K)")
			(pinfunction "B")
			(pintype "passive")
			(zone_connect 2)
			(thermal_bridge_angle 45)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_circle
					(center 0 0.25)
					(end 0.5 0.25)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0 -0.25)
					(end 0.5 -0.25)
					(width 0)
					(fill yes)
				)
				(gr_poly
					(pts
						(xy 0 0.75) (xy -0.5 0.75) (xy -0.5 -0.75) (xy 0 -0.75)
					)
					(width 0)
					(fill yes)
				)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(at 153.75 76.25)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R5"
			(at 0 1.75 0)
			(layer "F.SilkS")
		)
		(property "Value" "500k"
			(at 0 1.65 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "MatrixDriver.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.208333)
			(net 5 "Net-(J1-Pin_1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.208333)
			(net 33 "Net-(U4-EN)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(at 149.75 71.25)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C1"
			(at -2.75 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "4.7u"
			(at 0 1.68 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "MatrixDriver.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.212766)
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.212766)
			(net 5 "Net-(J1-Pin_1)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(at 157.75 66.25)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R9"
			(at 2.75 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 0 1.65 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "MatrixDriver.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.208333)
			(net 35 "Net-(U4-FB)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.208333)
			(net 36 "Net-(R10-Pad2)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(at 157.75 61.25)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R7"
			(at 2.75 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "100k"
			(at 0 1.65 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "MatrixDriver.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.208333)
			(net 2 "+5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.208333)
			(net 34 "Net-(R7-Pad2)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(at 157.75 56.25 180)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C8"
			(at -2.75 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "22u"
			(at 0 1.68 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "MatrixDriver.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.0375 0 180)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.212766)
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.0375 0 180)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.212766)
			(net 2 "+5V")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(at 157.75 58.75 180)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C7"
			(at -2.75 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "22u"
			(at 0 1.68 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "MatrixDriver.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.0375 0 180)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.212766)
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.0375 0 180)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.212766)
			(net 2 "+5V")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(at 149.75 56.25)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C10"
			(at -3.25 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "22u"
			(at 0 1.68 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "MatrixDriver.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.212766)
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.212766)
			(net 2 "+5V")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_JST:JST_XA_S02B-XASK-1_1x02_P2.50mm_Horizontal"
		(layer "F.Cu")
		(at 155 50 180)
		(descr "JST XA series connector, S02B-XASK-1 (http://www.jst-mfg.com/product/pdf/eng/eXA1.pdf), generated with kicad-footprint-generator")
		(tags "connector JST XA horizontal hook")
		(property "Reference" "J2"
			(at 1.25 -4.6 180)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "5V OUT"
			(at 1.25 10.4 180)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_JST:JST_XA_S02B-XASK-1_1x02_P2.50mm_Horizontal"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "Root")
		(sheetfile "MatrixDriver.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.25 2.5 180)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole oval
			(at 1.25 6.5 180)
			(size 2.8 2)
			(drill oval 2.8 2)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" thru_hole roundrect
			(at 0 0 180)
			(size 1.7 1.95)
			(drill 0.95)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.147059)
			(net 2 "+5V")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 2.5 0 180)
			(size 1.7 1.95)
			(drill 0.95)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_JST.3dshapes/JST_XA_S02B-XASK-1_1x02_P2.50mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Kicad_Libs:UPDI_Pads"
		(layer "B.Cu")
		(at 95.25 65.5 180)
		(property "Reference" "Prog1"
			(at -1 4.75 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "ProgPads"
			(at -3.81 0 -90)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Footprint" "Kicad_Libs:UPDI_Pads"
			(at 0 6.08 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 6.08 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x03, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 6.08 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "Root")
		(sheetfile "MatrixDriver.kicad_sch")
		(attr smd)
		(fp_text user "V+"
			(at 1.778 -0.762 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(fp_text user "Gnd"
			(at 1.524 -3.302 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(fp_text user "UPDI"
			(at -1.778 0 -90)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(fp_text user "Prog"
			(at 1.524 1.778 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(fp_text user "${REFERENCE}"
			(at 0.508 -4.826 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at 0 2.54 180)
			(size 3 2)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 28 "UPDI")
			(pinfunction "Pin_1")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "2" smd roundrect
			(at 0 0 180)
			(size 3 2)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 3 "Net-(D1-K)")
			(pinfunction "Pin_2")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "3" smd roundrect
			(at 0 -2.54 180)
			(size 3 2)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "Pin_3")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
	)
	(gr_text "TWI/UART to HUB75 module \nKoakuma V2\nhackaday.io/voltweasel"
		(at 174 59 0)
		(layer "B.SilkS")
	)
	(gr_text "2x 5V Output\n1A/Connector"
		(at 148.5 46.5 0)
		(layer "B.SilkS")
	)
	(gr_text "VIN\nGND"
		(at 153.75 85.75 90)
		(layer "B.SilkS")
	)
	(gr_text "G1\n\nGND\n\nG2\n\nE\n\nB\n\nD\n\nLAT\n\nGND"
		(at 129.5 50 -90)
		(layer "B.SilkS")
	)
	(gr_text "R1\n\nB1\n\nR2\n\nB2\n\nA\n\nC\n\nCLK\n\nOE"
		(at 129.5 44.5 -90)
		(layer "B.SilkS")
	)
	(gr_text "PWR in to\n5V regulator\n24V max."
		(at 153.75 80.5 0)
		(layer "B.SilkS")
	)
	(gr_text "UART\n(opt)"
		(at 141.5 89.25 0)
		(layer "B.SilkS")
	)
	(gr_text "2x TWI paralleled\nfor chaining\n3,3V and 5V compatible"
		(at 120 89.25 0)
		(layer "B.SilkS")
	)
	(gr_text "UART"
		(at 135 85.5 90)
		(layer "F.SilkS")
	)
	(gr_text "V+\nGND\nSDA\nSCL"
		(at 112.5 83.5 90)
		(layer "F.SilkS")
	)
	(gr_text "GND\n5V"
		(at 153.75 52 90)
		(layer "F.SilkS")
	)
	(gr_text "PWR OUT MATRIX"
		(at 148.5 40.75 90)
		(layer "F.SilkS")
	)
	(gr_text "TWI/CHAIN"
		(at 120 85.5 90)
		(layer "F.SilkS")
	)
	(gr_text "TX\nRX\nGND"
		(at 141.5 83.25 90)
		(layer "F.SilkS")
	)
	(gr_text "PWR OUT MATRIX"
		(at 138.25 40.75 90)
		(layer "F.SilkS")
	)
	(gr_text "TWI/CHAIN"
		(at 105 85 90)
		(layer "F.SilkS")
	)
	(gr_text "PWR IN MATRIX"
		(at 149 82.5 90)
		(layer "F.SilkS")
	)
	(gr_text "GND\n5V"
		(at 143.25 52 90)
		(layer "F.SilkS")
	)
	(gr_text "VIN\nGND"
		(at 153.75 82.25 90)
		(layer "F.SilkS")
	)
	(zone
		(net 2)
		(net_name "+5V")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 2)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 154.5 48.75) (xy 154 49.25) (xy 154 54.5) (xy 153.5 55) (xy 150 55) (xy 149.75 55.25) (xy 149.75 60)
				(xy 149.25 60.5) (xy 149.25 63) (xy 149.5 63.25) (xy 153.75 63.25) (xy 154.75 62.25) (xy 157.25 62.25)
				(xy 157.5 62) (xy 157.5 49.25) (xy 157 48.75)
			)
		)
	)
	(zone
		(net 29)
		(net_name "Net-(U4-SW)")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 1)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 153.5 71.75) (xy 153.5 70.25) (xy 152.75 69.5) (xy 149.5 69.5) (xy 149.25 69.25) (xy 149.25 67)
				(xy 149.5 66.75) (xy 154 66.75) (xy 154.25 67) (xy 154.25 69.25) (xy 154 70.25) (xy 154 71.75)
			)
		)
	)
	(zone
		(net 2)
		(net_name "+5V")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 2)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 147 51.5) (xy 147.5 52) (xy 153.5 52) (xy 154 51.5) (xy 154 55.25) (xy 149.75 55.25) (xy 149.75 55)
				(xy 149.25 54.5) (xy 144 54.5) (xy 143.5 54) (xy 143.5 49.25) (xy 144 48.75) (xy 146.5 48.75) (xy 147 49.25)
			)
		)
	)
	(zone
		(net 5)
		(net_name "Net-(J1-Pin_1)")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 1)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 153 71.75) (xy 153 70.25) (xy 152.5 69.75) (xy 150.25 69.75) (xy 150 70) (xy 150 85.825) (xy 150.25 86.075)
				(xy 153.25 86.075) (xy 153.5 85.825) (xy 153.5 75.575) (xy 153.25 75.325) (xy 152.25 75.325) (xy 152 75.075)
				(xy 152 72.25) (xy 152.25 72) (xy 152.75 72)
			)
		)
	)
	(zone
		(net 1)
		(net_name "GND")
		(layers "F&B.Cu")
		(hatch edge 0.5)
		(priority 5)
		(connect_pads yes
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 1)
		)
		(polygon
			(pts
				(xy 102 40) (xy 102 52) (xy 90 52) (xy 90 40)
			)
		)
	)
	(zone
		(net 1)
		(net_name "GND")
		(layers "F&B.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0.25)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 175 40) (xy 90 40) (xy 90 94) (xy 175 94)
			)
		)
	)
	(zone
		(net 1)
		(net_name "GND")
		(layers "F&B.Cu")
		(hatch edge 0.5)
		(priority 5)
		(connect_pads yes
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 1)
		)
		(polygon
			(pts
				(xy 175 40) (xy 175 52) (xy 163 52) (xy 163 40)
			)
		)
	)
	(zone
		(net 1)
		(net_name "GND")
		(layers "F&B.Cu")
		(hatch edge 0.5)
		(priority 5)
		(connect_pads yes
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 1)
		)
		(polygon
			(pts
				(xy 102 82) (xy 102 94) (xy 90 94) (xy 90 82)
			)
		)
	)
	(zone
		(net 1)
		(net_name "GND")
		(layers "F&B.Cu")
		(hatch edge 0.5)
		(priority 5)
		(connect_pads yes
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 1)
		)
		(polygon
			(pts
				(xy 175 82) (xy 175 94) (xy 163 94) (xy 163 82)
			)
		)
	)
)
