(kicad_sch
	(version 20231120)
	(generator "eeschema")
	(generator_version "8.0")
	(paper "A4")
	(lib_symbols
		(symbol "Connector:TestPoint"
			(pin_numbers hide)
			(pin_names
				(offset 0.762) hide)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "TP"
				(at 0 6.858 0)
			)
			(property "Value" "TestPoint"
				(at 0 5.08 0)
			)
			(property "Footprint" ""
				(at 5.08 0 0)
			)
			(property "Datasheet" "~"
				(at 5.08 0 0)
			)
			(property "Description" "test point"
				(at 0 0 0)
			)
			(property "ki_keywords" "test point tp"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "Pin* Test*"
				(at 0 0 0)
			)
			(symbol "TestPoint_0_1"
				(circle
					(center 0 3.302)
					(radius 0.762)
					(fill
						(type none)
					)
				)
			)
			(symbol "TestPoint_1_1"
				(pin passive line
					(at 0 0 90)
					(length 2.54)
					(name "1")
					(number "1")
				)
			)
		)
		(symbol "Connector:USB_B_Micro"
			(pin_names
				(offset 1.016)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "J"
				(at -5.08 11.43 0)
			)
			(property "Value" "USB_B_Micro"
				(at -5.08 8.89 0)
			)
			(property "Footprint" ""
				(at 3.81 -1.27 0)
			)
			(property "Datasheet" "~"
				(at 3.81 -1.27 0)
			)
			(property "Description" "USB Micro Type B connector"
				(at 0 0 0)
			)
			(property "ki_keywords" "connector USB micro"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "USB*"
				(at 0 0 0)
			)
			(symbol "USB_B_Micro_0_1"
				(rectangle
					(start -5.08 -7.62)
					(end 5.08 7.62)
					(fill
						(type background)
					)
				)
				(circle
					(center -3.81 2.159)
					(radius 0.635)
					(fill
						(type outline)
					)
				)
				(circle
					(center -0.635 3.429)
					(radius 0.381)
					(fill
						(type outline)
					)
				)
				(rectangle
					(start -0.127 -7.62)
					(end 0.127 -6.858)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -1.905 2.159) (xy 0.635 2.159)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -3.175 2.159) (xy -2.54 2.159) (xy -1.27 3.429) (xy -0.635 3.429)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -2.54 2.159) (xy -1.905 2.159) (xy -1.27 0.889) (xy 0 0.889)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0.635 2.794) (xy 0.635 1.524) (xy 1.905 2.159) (xy 0.635 2.794)
					)
					(fill
						(type outline)
					)
				)
				(polyline
					(pts
						(xy -4.318 5.588) (xy -1.778 5.588) (xy -2.032 4.826) (xy -4.064 4.826) (xy -4.318 5.588)
					)
					(fill
						(type outline)
					)
				)
				(polyline
					(pts
						(xy -4.699 5.842) (xy -4.699 5.588) (xy -4.445 4.826) (xy -4.445 4.572) (xy -1.651 4.572) (xy -1.651 4.826)
						(xy -1.397 5.588) (xy -1.397 5.842) (xy -4.699 5.842)
					)
					(fill
						(type none)
					)
				)
				(rectangle
					(start 0.254 1.27)
					(end -0.508 0.508)
					(fill
						(type outline)
					)
				)
				(rectangle
					(start 5.08 -5.207)
					(end 4.318 -4.953)
					(fill
						(type none)
					)
				)
				(rectangle
					(start 5.08 -2.667)
					(end 4.318 -2.413)
					(fill
						(type none)
					)
				)
				(rectangle
					(start 5.08 -0.127)
					(end 4.318 0.127)
					(fill
						(type none)
					)
				)
				(rectangle
					(start 5.08 4.953)
					(end 4.318 5.207)
					(fill
						(type none)
					)
				)
			)
			(symbol "USB_B_Micro_1_1"
				(pin power_out line
					(at 7.62 5.08 180)
					(length 2.54)
					(name "VBUS")
					(number "1")
				)
				(pin bidirectional line
					(at 7.62 -2.54 180)
					(length 2.54)
					(name "D-")
					(number "2")
				)
				(pin bidirectional line
					(at 7.62 0 180)
					(length 2.54)
					(name "D+")
					(number "3")
				)
				(pin passive line
					(at 7.62 -5.08 180)
					(length 2.54)
					(name "ID")
					(number "4")
				)
				(pin power_out line
					(at 0 -10.16 90)
					(length 2.54)
					(name "GND")
					(number "5")
				)
				(pin passive line
					(at -2.54 -10.16 90)
					(length 2.54)
					(name "Shield")
					(number "6")
				)
			)
		)
		(symbol "Device:C_Small"
			(pin_numbers hide)
			(pin_names
				(offset 0.254) hide)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "C"
				(at 0.254 1.778 0)
			)
			(property "Value" "C_Small"
				(at 0.254 -2.032 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" "~"
				(at 0 0 0)
			)
			(property "Description" "Unpolarized capacitor, small symbol"
				(at 0 0 0)
			)
			(property "ki_keywords" "capacitor cap"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "C_*"
				(at 0 0 0)
			)
			(symbol "C_Small_0_1"
				(polyline
					(pts
						(xy -1.524 -0.508) (xy 1.524 -0.508)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -1.524 0.508) (xy 1.524 0.508)
					)
					(fill
						(type none)
					)
				)
			)
			(symbol "C_Small_1_1"
				(pin passive line
					(at 0 2.54 270)
					(length 2.032)
					(name "~")
					(number "1")
				)
				(pin passive line
					(at 0 -2.54 90)
					(length 2.032)
					(name "~")
					(number "2")
				)
			)
		)
		(symbol "Device:Crystal_GND24_Small"
			(pin_names
				(offset 1.016) hide)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "Y"
				(at 1.27 4.445 0)
			)
			(property "Value" "Crystal_GND24_Small"
				(at 1.27 2.54 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" "~"
				(at 0 0 0)
			)
			(property "Description" "Four pin crystal, GND on pins 2 and 4, small symbol"
				(at 0 0 0)
			)
			(property "ki_keywords" "quartz ceramic resonator oscillator"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "Crystal*"
				(at 0 0 0)
			)
			(symbol "Crystal_GND24_Small_0_1"
				(rectangle
					(start -0.762 -1.524)
					(end 0.762 1.524)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -1.27 -0.762) (xy -1.27 0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.27 -0.762) (xy 1.27 0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -1.27 -1.27) (xy -1.27 -1.905) (xy 1.27 -1.905) (xy 1.27 -1.27)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -1.27 1.27) (xy -1.27 1.905) (xy 1.27 1.905) (xy 1.27 1.27)
					)
					(fill
						(type none)
					)
				)
			)
			(symbol "Crystal_GND24_Small_1_1"
				(pin passive line
					(at -2.54 0 0)
					(length 1.27)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 0 -2.54 90)
					(length 0.635)
					(name "2")
					(number "2")
				)
				(pin passive line
					(at 2.54 0 180)
					(length 1.27)
					(name "3")
					(number "3")
				)
				(pin passive line
					(at 0 2.54 270)
					(length 0.635)
					(name "4")
					(number "4")
				)
			)
		)
		(symbol "Device:L_Small"
			(pin_numbers hide)
			(pin_names
				(offset 0.254) hide)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "L"
				(at 0.762 1.016 0)
			)
			(property "Value" "L_Small"
				(at 0.762 -1.016 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" "~"
				(at 0 0 0)
			)
			(property "Description" "Inductor, small symbol"
				(at 0 0 0)
			)
			(property "ki_keywords" "inductor choke coil reactor magnetic"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "Choke_* *Coil* Inductor_* L_*"
				(at 0 0 0)
			)
			(symbol "L_Small_0_1"
				(arc
					(start 0 -2.032)
					(mid 0.5058 -1.524)
					(end 0 -1.016)
					(fill
						(type none)
					)
				)
				(arc
					(start 0 -1.016)
					(mid 0.5058 -0.508)
					(end 0 0)
					(fill
						(type none)
					)
				)
				(arc
					(start 0 0)
					(mid 0.5058 0.508)
					(end 0 1.016)
					(fill
						(type none)
					)
				)
				(arc
					(start 0 1.016)
					(mid 0.5058 1.524)
					(end 0 2.032)
					(fill
						(type none)
					)
				)
			)
			(symbol "L_Small_1_1"
				(pin passive line
					(at 0 2.54 270)
					(length 0.508)
					(name "~")
					(number "1")
				)
				(pin passive line
					(at 0 -2.54 90)
					(length 0.508)
					(name "~")
					(number "2")
				)
			)
		)
		(symbol "Device:R_Small"
			(pin_numbers hide)
			(pin_names
				(offset 0.254) hide)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "R"
				(at 0.762 0.508 0)
			)
			(property "Value" "R_Small"
				(at 0.762 -1.016 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" "~"
				(at 0 0 0)
			)
			(property "Description" "Resistor, small symbol"
				(at 0 0 0)
			)
			(property "ki_keywords" "R resistor"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "R_*"
				(at 0 0 0)
			)
			(symbol "R_Small_0_1"
				(rectangle
					(start -0.762 1.778)
					(end 0.762 -1.778)
					(fill
						(type none)
					)
				)
			)
			(symbol "R_Small_1_1"
				(pin passive line
					(at 0 2.54 270)
					(length 0.762)
					(name "~")
					(number "1")
				)
				(pin passive line
					(at 0 -2.54 90)
					(length 0.762)
					(name "~")
					(number "2")
				)
			)
		)
		(symbol "MCU_Microchip_ATmega:ATmega32U4-M"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "U1"
				(at -14.732 -46.736 0)
			)
			(property "Value" "ATmega32U4-M"
				(at -8.636 -57.15 0)
			)
			(property "Footprint" "Package_DFN_QFN:QFN-44-1EP_7x7mm_P0.5mm_EP5.2x5.2mm"
				(at -70.104 56.388 0)
			)
			(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-7766-8-bit-AVR-ATmega16U4-32U4_Datasheet.pdf"
				(at -45.72 61.468 0)
			)
			(property "Description" "16MHz, 32kB Flash, 2.5kB SRAM, 1kB EEPROM, USB 2.0, QFN-44"
				(at -68.834 51.308 0)
			)
			(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR USB"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
				(at 0 0 0)
			)
			(symbol "ATmega32U4-M_0_1"
				(rectangle
					(start -12.7 43.18)
					(end 12.7 -43.18)
					(fill
						(type background)
					)
				)
			)
			(symbol "ATmega32U4-M_1_1"
				(pin bidirectional line
					(at 15.24 -17.78 180)
					(length 2.54)
					(name "PE6")
					(number "1")
				)
				(pin bidirectional line
					(at 15.24 33.02 180)
					(length 2.54)
					(name "PB2")
					(number "10")
				)
				(pin bidirectional line
					(at 15.24 30.48 180)
					(length 2.54)
					(name "PB3")
					(number "11")
				)
				(pin bidirectional line
					(at 15.24 20.32 180)
					(length 2.54)
					(name "PB7")
					(number "12")
				)
				(pin input line
					(at -15.24 38.1 0)
					(length 2.54)
					(name "~{RESET}")
					(number "13")
				)
				(pin power_in line
					(at -1.27 45.72 270)
					(length 2.54)
					(name "VCC")
					(number "14")
				)
				(pin power_in line
					(at -3.81 -45.72 90)
					(length 2.54)
					(name "GND")
					(number "15")
				)
				(pin output line
					(at -15.24 27.94 0)
					(length 2.54)
					(name "XTAL2")
					(number "16")
				)
				(pin input line
					(at -15.24 33.02 0)
					(length 2.54)
					(name "XTAL1")
					(number "17")
				)
				(pin bidirectional line
					(at 15.24 7.62 180)
					(length 2.54)
					(name "PD0")
					(number "18")
				)
				(pin bidirectional line
					(at 15.24 5.08 180)
					(length 2.54)
					(name "PD1")
					(number "19")
				)
				(pin power_in line
					(at -3.81 45.72 270)
					(length 2.54)
					(name "UVCC")
					(number "2")
				)
				(pin bidirectional line
					(at 15.24 2.54 180)
					(length 2.54)
					(name "PD2")
					(number "20")
				)
				(pin bidirectional line
					(at 15.24 0 180)
					(length 2.54)
					(name "PD3")
					(number "21")
				)
				(pin bidirectional line
					(at 15.24 -5.08 180)
					(length 2.54)
					(name "PD5")
					(number "22")
				)
				(pin passive line
					(at -1.27 -45.72 90)
					(length 2.54)
					(name "GND")
					(number "23")
				)
				(pin power_in line
					(at 1.27 45.72 270)
					(length 2.54)
					(name "AVCC")
					(number "24")
				)
				(pin bidirectional line
					(at 15.24 -2.54 180)
					(length 2.54)
					(name "PD4")
					(number "25")
				)
				(pin bidirectional line
					(at 15.24 -7.62 180)
					(length 2.54)
					(name "PD6")
					(number "26")
				)
				(pin bidirectional line
					(at 15.24 -10.16 180)
					(length 2.54)
					(name "PD7")
					(number "27")
				)
				(pin bidirectional line
					(at 15.24 27.94 180)
					(length 2.54)
					(name "PB4")
					(number "28")
				)
				(pin bidirectional line
					(at 15.24 25.4 180)
					(length 2.54)
					(name "PB5")
					(number "29")
				)
				(pin bidirectional line
					(at -15.24 10.16 0)
					(length 2.54)
					(name "D-")
					(number "3")
				)
				(pin bidirectional line
					(at 15.24 22.86 180)
					(length 2.54)
					(name "PB6")
					(number "30")
				)
				(pin bidirectional line
					(at 15.24 15.24 180)
					(length 2.54)
					(name "PC6")
					(number "31")
				)
				(pin bidirectional line
					(at 15.24 12.7 180)
					(length 2.54)
					(name "PC7")
					(number "32")
				)
				(pin bidirectional line
					(at 15.24 -15.24 180)
					(length 2.54)
					(name "~{HWB}/PE2")
					(number "33")
				)
				(pin power_in line
					(at 3.81 45.72 270)
					(length 2.54)
					(name "VCC")
					(number "34")
				)
				(pin passive line
					(at 1.27 -45.72 90)
					(length 2.54)
					(name "GND")
					(number "35")
				)
				(pin bidirectional line
					(at 15.24 -35.56 180)
					(length 2.54)
					(name "PF7")
					(number "36")
				)
				(pin bidirectional line
					(at 15.24 -33.02 180)
					(length 2.54)
					(name "PF6")
					(number "37")
				)
				(pin bidirectional line
					(at 15.24 -30.48 180)
					(length 2.54)
					(name "PF5")
					(number "38")
				)
				(pin bidirectional line
					(at 15.24 -27.94 180)
					(length 2.54)
					(name "PF4")
					(number "39")
				)
				(pin bidirectional line
					(at -15.24 12.7 0)
					(length 2.54)
					(name "D+")
					(number "4")
				)
				(pin bidirectional line
					(at 15.24 -25.4 180)
					(length 2.54)
					(name "PF1")
					(number "40")
				)
				(pin bidirectional line
					(at 15.24 -22.86 180)
					(length 2.54)
					(name "PF0")
					(number "41")
				)
				(pin passive line
					(at -15.24 22.86 0)
					(length 2.54)
					(name "AREF")
					(number "42")
				)
				(pin passive line
					(at 3.81 -45.72 90)
					(length 2.54)
					(name "GND")
					(number "43")
				)
				(pin power_in line
					(at 6.35 45.72 270)
					(length 2.54)
					(name "AVCC")
					(number "44")
				)
				(pin passive line
					(at 6.35 -45.72 90)
					(length 2.54)
					(name "GND")
					(number "45")
				)
				(pin passive line
					(at -6.35 -45.72 90)
					(length 2.54)
					(name "UGND")
					(number "5")
				)
				(pin passive line
					(at -15.24 5.08 0)
					(length 2.54)
					(name "UCAP")
					(number "6")
				)
				(pin input line
					(at -15.24 17.78 0)
					(length 2.54)
					(name "VBUS")
					(number "7")
				)
				(pin bidirectional line
					(at 15.24 38.1 180)
					(length 2.54)
					(name "PB0")
					(number "8")
				)
				(pin bidirectional line
					(at 15.24 35.56 180)
					(length 2.54)
					(name "PB1")
					(number "9")
				)
			)
		)
		(symbol "power:+5V"
			(power)
			(pin_numbers hide)
			(pin_names
				(offset 0) hide)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "#PWR"
				(at 0 -3.81 0)
			)
			(property "Value" "+5V"
				(at 0 3.556 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" "Power symbol creates a global label with name \"+5V\""
				(at 0 0 0)
			)
			(property "ki_keywords" "global power"
				(at 0 0 0)
			)
			(symbol "+5V_0_1"
				(polyline
					(pts
						(xy -0.762 1.27) (xy 0 2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 0) (xy 0 2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 2.54) (xy 0.762 1.27)
					)
					(fill
						(type none)
					)
				)
			)
			(symbol "+5V_1_1"
				(pin power_in line
					(at 0 0 90)
					(length 0)
					(name "~")
					(number "1")
				)
			)
		)
		(symbol "power:GND"
			(power)
			(pin_numbers hide)
			(pin_names
				(offset 0) hide)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "#PWR"
				(at 0 -6.35 0)
			)
			(property "Value" "GND"
				(at 0 -3.81 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
				(at 0 0 0)
			)
			(property "ki_keywords" "global power"
				(at 0 0 0)
			)
			(symbol "GND_0_1"
				(polyline
					(pts
						(xy 0 0) (xy 0 -1.27) (xy 1.27 -1.27) (xy 0 -2.54) (xy -1.27 -1.27) (xy 0 -1.27)
					)
					(fill
						(type none)
					)
				)
			)
			(symbol "GND_1_1"
				(pin power_in line
					(at 0 0 270)
					(length 0)
					(name "~")
					(number "1")
				)
			)
		)
	)
	(junction
		(at 27.94 49.53)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 77.47 116.84)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 26.67 99.06)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 74.93 116.84)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 31.75 101.6)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 31.75 99.06)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 43.18 43.18)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 67.31 116.84)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 31.75 91.44)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 67.31 22.86)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 72.39 116.84)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 36.83 99.06)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 33.02 165.1)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 31.75 93.98)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 43.18 38.1)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 26.67 93.98)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 69.85 22.86)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 77.47 20.32)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 27.94 45.72)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 69.85 116.84)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 36.83 93.98)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 40.64 49.53)
		(diameter 0)
		(color 0 0 0 0)
	)
	(no_connect
		(at 55.88 48.26)
	)
	(wire
		(pts
			(xy 31.75 90.17) (xy 31.75 91.44)
		)
	)
	(wire
		(pts
			(xy 43.18 43.18) (xy 55.88 43.18)
		)
	)
	(wire
		(pts
			(xy 35.56 60.96) (xy 40.64 60.96)
		)
	)
	(wire
		(pts
			(xy 36.83 93.98) (xy 46.99 93.98)
		)
	)
	(wire
		(pts
			(xy 54.61 25.4) (xy 54.61 33.02)
		)
	)
	(wire
		(pts
			(xy 67.31 19.05) (xy 67.31 22.86)
		)
	)
	(wire
		(pts
			(xy 30.48 165.1) (xy 33.02 165.1)
		)
	)
	(wire
		(pts
			(xy 31.75 101.6) (xy 31.75 99.06)
		)
	)
	(wire
		(pts
			(xy 67.31 22.86) (xy 67.31 25.4)
		)
	)
	(wire
		(pts
			(xy 43.18 38.1) (xy 55.88 38.1)
		)
	)
	(wire
		(pts
			(xy 27.94 50.8) (xy 27.94 49.53)
		)
	)
	(wire
		(pts
			(xy 33.02 38.1) (xy 43.18 38.1)
		)
	)
	(wire
		(pts
			(xy 77.47 25.4) (xy 77.47 20.32)
		)
	)
	(wire
		(pts
			(xy 54.61 33.02) (xy 55.88 33.02)
		)
	)
	(wire
		(pts
			(xy 40.64 49.53) (xy 27.94 49.53)
		)
	)
	(wire
		(pts
			(xy 36.83 99.06) (xy 46.99 99.06)
		)
	)
	(wire
		(pts
			(xy 35.56 165.1) (xy 35.56 177.8)
		)
	)
	(wire
		(pts
			(xy 67.31 22.86) (xy 69.85 22.86)
		)
	)
	(wire
		(pts
			(xy 33.02 43.18) (xy 33.02 45.72)
		)
	)
	(wire
		(pts
			(xy 69.85 22.86) (xy 69.85 25.4)
		)
	)
	(wire
		(pts
			(xy 72.39 22.86) (xy 72.39 25.4)
		)
	)
	(wire
		(pts
			(xy 96.52 86.36) (xy 86.36 86.36)
		)
	)
	(wire
		(pts
			(xy 69.85 116.84) (xy 72.39 116.84)
		)
	)
	(wire
		(pts
			(xy 31.75 99.06) (xy 36.83 99.06)
		)
	)
	(wire
		(pts
			(xy 74.93 116.84) (xy 77.47 116.84)
		)
	)
	(wire
		(pts
			(xy 31.75 102.87) (xy 31.75 101.6)
		)
	)
	(wire
		(pts
			(xy 35.56 58.42) (xy 46.99 58.42)
		)
	)
	(wire
		(pts
			(xy 77.47 116.84) (xy 82.55 116.84)
		)
	)
	(wire
		(pts
			(xy 64.77 116.84) (xy 67.31 116.84)
		)
	)
	(wire
		(pts
			(xy 40.64 49.53) (xy 45.72 49.53)
		)
	)
	(wire
		(pts
			(xy 77.47 20.32) (xy 74.93 20.32)
		)
	)
	(wire
		(pts
			(xy 27.94 45.72) (xy 27.94 49.53)
		)
	)
	(wire
		(pts
			(xy 52.07 138.43) (xy 52.07 149.86)
		)
	)
	(wire
		(pts
			(xy 50.8 74.93) (xy 50.8 71.12)
		)
	)
	(wire
		(pts
			(xy 55.88 66.04) (xy 50.8 66.04)
		)
	)
	(wire
		(pts
			(xy 67.31 116.84) (xy 69.85 116.84)
		)
	)
	(wire
		(pts
			(xy 31.75 93.98) (xy 36.83 93.98)
		)
	)
	(wire
		(pts
			(xy 101.6 86.36) (xy 105.41 86.36)
		)
	)
	(wire
		(pts
			(xy 16.51 93.98) (xy 26.67 93.98)
		)
	)
	(wire
		(pts
			(xy 52.07 53.34) (xy 55.88 53.34)
		)
	)
	(wire
		(pts
			(xy 33.02 165.1) (xy 35.56 165.1)
		)
	)
	(wire
		(pts
			(xy 77.47 15.24) (xy 96.52 15.24)
		)
	)
	(wire
		(pts
			(xy 26.67 99.06) (xy 31.75 99.06)
		)
	)
	(wire
		(pts
			(xy 27.94 35.56) (xy 27.94 45.72)
		)
	)
	(wire
		(pts
			(xy 33.02 35.56) (xy 33.02 38.1)
		)
	)
	(wire
		(pts
			(xy 54.61 17.78) (xy 54.61 20.32)
		)
	)
	(wire
		(pts
			(xy 72.39 116.84) (xy 74.93 116.84)
		)
	)
	(wire
		(pts
			(xy 31.75 91.44) (xy 31.75 93.98)
		)
	)
	(wire
		(pts
			(xy 16.51 99.06) (xy 26.67 99.06)
		)
	)
	(wire
		(pts
			(xy 40.64 149.86) (xy 52.07 149.86)
		)
	)
	(wire
		(pts
			(xy 69.85 22.86) (xy 72.39 22.86)
		)
	)
	(wire
		(pts
			(xy 33.02 43.18) (xy 43.18 43.18)
		)
	)
	(wire
		(pts
			(xy 55.88 60.96) (xy 45.72 60.96)
		)
	)
	(wire
		(pts
			(xy 40.64 40.64) (xy 40.64 49.53)
		)
	)
	(wire
		(pts
			(xy 45.72 49.53) (xy 45.72 40.64)
		)
	)
	(wire
		(pts
			(xy 26.67 93.98) (xy 31.75 93.98)
		)
	)
	(wire
		(pts
			(xy 52.07 58.42) (xy 55.88 58.42)
		)
	)
	(label "D+"
		(at 55.88 58.42 180)
	)
	(label "D-"
		(at 55.88 60.96 180)
	)
	(global_label "COL 3"
		(shape input)
		(at 86.36 63.5 0)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 86.36 63.5 0)
		)
	)
	(global_label "ROW 4"
		(shape input)
		(at 86.36 58.42 0)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 86.36 58.42 0)
		)
	)
	(global_label "COL 1"
		(shape input)
		(at 86.36 68.58 0)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 86.36 68.58 0)
		)
	)
	(global_label "COL 11"
		(shape input)
		(at 86.36 78.74 0)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 86.36 78.74 0)
		)
	)
	(global_label "D-"
		(shape input)
		(at 35.56 60.96 180)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 35.56 60.96 0)
		)
	)
	(global_label "COL 5"
		(shape input)
		(at 86.36 38.1 0)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 86.36 38.1 0)
		)
	)
	(global_label "COL 8"
		(shape input)
		(at 86.36 71.12 0)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 86.36 71.12 0)
		)
	)
	(global_label "COL 7"
		(shape input)
		(at 86.36 33.02 0)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 86.36 33.02 0)
		)
	)
	(global_label "COL 4"
		(shape input)
		(at 86.36 40.64 0)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 86.36 40.64 0)
		)
	)
	(global_label "COL 6"
		(shape input)
		(at 86.36 35.56 0)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 86.36 35.56 0)
		)
	)
	(global_label "COL 2"
		(shape input)
		(at 86.36 66.04 0)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 86.36 66.04 0)
		)
	)
	(global_label "COL 0"
		(shape input)
		(at 86.36 81.28 0)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 86.36 81.28 0)
		)
	)
	(global_label "ROW 2"
		(shape input)
		(at 86.36 45.72 0)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 86.36 45.72 0)
		)
	)
	(global_label "COL 10"
		(shape input)
		(at 86.36 73.66 0)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 86.36 73.66 0)
		)
	)
	(global_label "ROW 3"
		(shape input)
		(at 86.36 55.88 0)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 86.36 55.88 0)
		)
	)
	(global_label "D-"
		(shape input)
		(at 40.64 157.48 0)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 40.64 157.48 0)
		)
	)
	(global_label "COL 9"
		(shape input)
		(at 86.36 76.2 0)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 86.36 76.2 0)
		)
	)
	(global_label "ROW 1"
		(shape input)
		(at 86.36 48.26 0)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 86.36 48.26 0)
		)
	)
	(global_label "ROW 0"
		(shape input)
		(at 86.36 43.18 0)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 86.36 43.18 0)
		)
	)
	(global_label "ROW 5"
		(shape input)
		(at 86.36 106.68 0)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 86.36 106.68 0)
		)
	)
	(global_label "D+"
		(shape input)
		(at 40.64 154.94 0)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 40.64 154.94 0)
		)
	)
	(global_label "D+"
		(shape input)
		(at 35.56 58.42 180)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 35.56 58.42 0)
		)
	)
	(symbol
		(lib_id "Device:R_Small")
		(at 43.18 60.96 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "RC1"
			(at 43.18 55.9816 90)
		)
		(property "Value" "22"
			(at 43.18 58.293 90)
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric"
			(at 43.18 60.96 0)
		)
		(property "Datasheet" "https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf"
			(at 43.18 60.96 0)
		)
		(property "Description" "Resistor"
			(at 43.18 60.96 0)
		)
		(property "Manufacturer" "Panasonic"
			(at 43.18 60.96 0)
		)
		(property "Manufacturer P/N" "  ERJ-6GEYJ220V"
			(at 43.18 60.96 0)
		)
		(property "Package" "0805_2012Metric"
			(at 43.18 60.96 0)
		)
		(property "Type" "SMD"
			(at 43.18 60.96 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "Keyboard V1"
				(path
					(reference "RC1")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Connector:TestPoint")
		(at 86.36 101.6 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "F5"
			(at 91.44 101.5999 90)
		)
		(property "Value" "TestPoint"
			(at 91.44 102.8699 90)
		)
		(property "Footprint" "Connector_Wire:SolderWire-0.1sqmm_1x01_D0.4mm_OD1mm"
			(at 86.36 106.68 0)
		)
		(property "Datasheet" "~"
			(at 86.36 106.68 0)
		)
		(property "Description" "test point"
			(at 86.36 101.6 0)
		)
		(property "Manufacturer" ""
			(at 86.36 101.6 0)
		)
		(property "Manufacturer P/N" ""
			(at 86.36 101.6 0)
		)
		(property "Package" ""
			(at 86.36 101.6 0)
		)
		(property "Type" ""
			(at 86.36 101.6 0)
		)
		(pin "1")
		(instances
			(project "Keyboard V1"
				(path
					(reference "F5")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Connector:TestPoint")
		(at 86.36 104.14 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "F6"
			(at 91.44 104.1399 90)
		)
		(property "Value" "TestPoint"
			(at 91.44 105.4099 90)
		)
		(property "Footprint" "Connector_Wire:SolderWire-0.1sqmm_1x01_D0.4mm_OD1mm"
			(at 86.36 109.22 0)
		)
		(property "Datasheet" "~"
			(at 86.36 109.22 0)
		)
		(property "Description" "test point"
			(at 86.36 104.14 0)
		)
		(property "Manufacturer" ""
			(at 86.36 104.14 0)
		)
		(property "Manufacturer P/N" ""
			(at 86.36 104.14 0)
		)
		(property "Package" ""
			(at 86.36 104.14 0)
		)
		(property "Type" ""
			(at 86.36 104.14 0)
		)
		(pin "1")
		(instances
			(project "Keyboard V1"
				(path
					(reference "F6")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Connector:USB_B_Micro")
		(at 33.02 154.94 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "J2"
			(at 33.02 142.24 0)
		)
		(property "Value" "USB Micro Type B connector"
			(at 33.02 144.78 0)
		)
		(property "Footprint" "Library:AMPHENOL_10118192-0002LF"
			(at 36.83 156.21 0)
		)
		(property "Datasheet" "https://cdn.amphenol-https://cdn.amphenol-cs.com/media/wysiwyg/files/documentation/datasheet/inputoutput/io_usb_micro.pdf"
			(at 36.83 156.21 0)
		)
		(property "Description" "USB Micro Type B connector"
			(at 33.02 154.94 0)
		)
		(property "Manufacturer" "Amphenol"
			(at 33.02 154.94 0)
		)
		(property "Manufacturer P/N" "10118192-0002LF"
			(at 33.02 154.94 0)
		)
		(property "Package" ""
			(at 33.02 154.94 0)
		)
		(property "Type" "SMD"
			(at 33.02 154.94 0)
		)
		(pin "1")
		(pin "2")
		(pin "3")
		(pin "4")
		(pin "6")
		(pin "5")
		(instances
			(project ""
				(path
					(reference "J2")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:C_Small")
		(at 36.83 96.52 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C5"
			(at 39.1668 95.3516 0)
		)
		(property "Value" "0.1uF"
			(at 39.1668 97.663 0)
		)
		(property "Footprint" "Capacitor_SMD:C_0805_2012Metric"
			(at 36.83 96.52 0)
		)
		(property "Datasheet" "https://mm.digikey.com/Volume0/opasdata/d220001/medias/docus/609/CL21B104KBCNNN_Spec.pdf"
			(at 36.83 96.52 0)
		)
		(property "Description" "Capacitor"
			(at 36.83 96.52 0)
		)
		(property "Manufacturer" "Samsung Electro-Mechanics"
			(at 36.83 96.52 0)
		)
		(property "Manufacturer P/N" "CL21B104KBCNNNC"
			(at 36.83 96.52 0)
		)
		(property "Package" "0805_2012Metric"
			(at 36.83 96.52 0)
		)
		(property "Type" "SMD"
			(at 36.83 96.52 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "Keyboard V1"
				(path
					(reference "C5")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:R_Small")
		(at 99.06 86.36 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "RC4"
			(at 99.06 81.3816 90)
		)
		(property "Value" "10k"
			(at 99.06 83.693 90)
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric"
			(at 99.06 86.36 0)
		)
		(property "Datasheet" "https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf"
			(at 99.06 86.36 0)
		)
		(property "Description" "Resistor"
			(at 99.06 86.36 0)
		)
		(property "Manufacturer" "Panasonic"
			(at 99.06 86.36 0)
		)
		(property "Manufacturer P/N" "  ERJ-6GEYJ103V"
			(at 99.06 86.36 0)
		)
		(property "Package" "0805_2012Metric"
			(at 99.06 86.36 0)
		)
		(property "Type" "SMD"
			(at 99.06 86.36 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "Keyboard V1"
				(path
					(reference "RC4")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:C_Small")
		(at 16.51 96.52 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C1"
			(at 18.8468 95.3516 0)
		)
		(property "Value" "0.1uF"
			(at 18.8468 97.663 0)
		)
		(property "Footprint" "Capacitor_SMD:C_0805_2012Metric"
			(at 16.51 96.52 0)
		)
		(property "Datasheet" "https://mm.digikey.com/Volume0/opasdata/d220001/medias/docus/609/CL21B104KBCNNN_Spec.pdf"
			(at 16.51 96.52 0)
		)
		(property "Description" "Capacitor"
			(at 16.51 96.52 0)
		)
		(property "Manufacturer" "Samsung Electro-Mechanics"
			(at 16.51 96.52 0)
		)
		(property "Manufacturer P/N" "CL21B104KBCNNNC"
			(at 16.51 96.52 0)
		)
		(property "Package" "0805_2012Metric"
			(at 16.51 96.52 0)
		)
		(property "Type" "SMD"
			(at 16.51 96.52 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "Keyboard V1"
				(path
					(reference "C1")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:R_Small")
		(at 54.61 22.86 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "RC3"
			(at 56.1086 21.6916 0)
		)
		(property "Value" "10k"
			(at 56.1086 24.003 0)
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric"
			(at 54.61 22.86 0)
		)
		(property "Datasheet" "https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf"
			(at 54.61 22.86 0)
		)
		(property "Description" "Resistor"
			(at 54.61 22.86 0)
		)
		(property "Manufacturer" "Panasonic"
			(at 54.61 22.86 0)
		)
		(property "Manufacturer P/N" "  ERJ-6GEYJ103V"
			(at 54.61 22.86 0)
		)
		(property "Package" "0805_2012Metric"
			(at 54.61 22.86 0)
		)
		(property "Type" "SMD"
			(at 54.61 22.86 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "Keyboard V1"
				(path
					(reference "RC3")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Connector:TestPoint")
		(at 31.75 101.6 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "GND1"
			(at 36.83 101.5999 90)
		)
		(property "Value" "TestPoint"
			(at 36.83 102.8699 90)
		)
		(property "Footprint" "Connector_Wire:SolderWire-0.1sqmm_1x01_D0.4mm_OD1mm"
			(at 31.75 106.68 0)
		)
		(property "Datasheet" "~"
			(at 31.75 106.68 0)
		)
		(property "Description" "test point"
			(at 31.75 101.6 0)
		)
		(property "Manufacturer" ""
			(at 31.75 101.6 0)
		)
		(property "Manufacturer P/N" ""
			(at 31.75 101.6 0)
		)
		(property "Package" ""
			(at 31.75 101.6 0)
		)
		(property "Type" ""
			(at 31.75 101.6 0)
		)
		(pin "1")
		(instances
			(project "Keyboard V1"
				(path
					(reference "GND1")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 96.52 15.24 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR04"
			(at 96.52 21.59 0)
		)
		(property "Value" "GND"
			(at 96.647 19.6342 0)
		)
		(property "Footprint" ""
			(at 96.52 15.24 0)
		)
		(property "Datasheet" ""
			(at 96.52 15.24 0)
		)
		(property "Description" ""
			(at 96.52 15.24 0)
		)
		(pin "1")
		(instances
			(project "Keyboard V1"
				(path
					(reference "#PWR04")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:+5V")
		(at 67.31 19.05 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR08"
			(at 67.31 22.86 0)
		)
		(property "Value" "+5V"
			(at 67.691 14.6558 0)
		)
		(property "Footprint" ""
			(at 67.31 19.05 0)
		)
		(property "Datasheet" ""
			(at 67.31 19.05 0)
		)
		(property "Description" ""
			(at 67.31 19.05 0)
		)
		(pin "1")
		(instances
			(project "Keyboard V1"
				(path
					(reference "#PWR08")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 27.94 50.8 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR01"
			(at 27.94 57.15 0)
		)
		(property "Value" "GND"
			(at 28.067 55.1942 0)
		)
		(property "Footprint" ""
			(at 27.94 50.8 0)
		)
		(property "Datasheet" ""
			(at 27.94 50.8 0)
		)
		(property "Description" ""
			(at 27.94 50.8 0)
		)
		(pin "1")
		(instances
			(project "Keyboard V1"
				(path
					(reference "#PWR01")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Connector:TestPoint")
		(at 31.75 91.44 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "+5V1"
			(at 36.83 91.4399 90)
		)
		(property "Value" "TestPoint"
			(at 36.83 92.7099 90)
		)
		(property "Footprint" "Connector_Wire:SolderWire-0.1sqmm_1x01_D0.4mm_OD1mm"
			(at 31.75 96.52 0)
		)
		(property "Datasheet" "~"
			(at 31.75 96.52 0)
		)
		(property "Description" "test point"
			(at 31.75 91.44 0)
		)
		(property "Manufacturer" ""
			(at 31.75 91.44 0)
		)
		(property "Manufacturer P/N" ""
			(at 31.75 91.44 0)
		)
		(property "Package" ""
			(at 31.75 91.44 0)
		)
		(property "Type" ""
			(at 31.75 91.44 0)
		)
		(pin "1")
		(instances
			(project "Keyboard V1"
				(path
					(reference "+5V1")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Connector:TestPoint")
		(at 86.36 93.98 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "F0"
			(at 91.44 93.9799 90)
		)
		(property "Value" "TestPoint"
			(at 91.44 95.2499 90)
		)
		(property "Footprint" "Connector_Wire:SolderWire-0.1sqmm_1x01_D0.4mm_OD1mm"
			(at 86.36 99.06 0)
		)
		(property "Datasheet" "~"
			(at 86.36 99.06 0)
		)
		(property "Description" "test point"
			(at 86.36 93.98 0)
		)
		(property "Manufacturer" ""
			(at 86.36 93.98 0)
		)
		(property "Manufacturer P/N" ""
			(at 86.36 93.98 0)
		)
		(property "Package" ""
			(at 86.36 93.98 0)
		)
		(property "Type" ""
			(at 86.36 93.98 0)
		)
		(pin "1")
		(instances
			(project ""
				(path
					(reference "F0")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:C_Small")
		(at 26.67 96.52 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C2"
			(at 29.0068 95.3516 0)
		)
		(property "Value" "0.1uF"
			(at 29.0068 97.663 0)
		)
		(property "Footprint" "Capacitor_SMD:C_0805_2012Metric"
			(at 26.67 96.52 0)
		)
		(property "Datasheet" "https://mm.digikey.com/Volume0/opasdata/d220001/medias/docus/609/CL21B104KBCNNN_Spec.pdf"
			(at 26.67 96.52 0)
		)
		(property "Description" "Capacitor"
			(at 26.67 96.52 0)
		)
		(property "Manufacturer" "Samsung Electro-Mechanics"
			(at 26.67 96.52 0)
		)
		(property "Manufacturer P/N" "CL21B104KBCNNNC"
			(at 26.67 96.52 0)
		)
		(property "Package" "0805_2012Metric"
			(at 26.67 96.52 0)
		)
		(property "Type" "SMD"
			(at 26.67 96.52 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "Keyboard V1"
				(path
					(reference "C2")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:L_Small")
		(at 74.93 22.86 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "L1"
			(at 76.454 24.13 90)
		)
		(property "Value" "10uH"
			(at 73.66 22.098 90)
		)
		(property "Footprint" "Inductor_SMD:L_0805_2012Metric"
			(at 74.93 22.86 0)
		)
		(property "Datasheet" "https://product.tdk.com/en/system/files/dam/doc/product/inductor/inductor/smd/catalog/inductor_automotive_standard_mlf2012_en.pdf"
			(at 74.93 22.86 0)
		)
		(property "Description" "Inductor"
			(at 74.93 22.86 0)
		)
		(property "Manufacturer" "TDK"
			(at 74.93 22.86 0)
		)
		(property "Manufacturer P/N" "  MLF2012E100JTD25"
			(at 74.93 22.86 0)
		)
		(property "Package" "0805_2012Metric"
			(at 74.93 22.86 0)
		)
		(property "Type" "SMD"
			(at 74.93 22.86 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project ""
				(path
					(reference "L1")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 82.55 116.84 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR09"
			(at 82.55 123.19 0)
		)
		(property "Value" "GND"
			(at 82.677 121.2342 0)
		)
		(property "Footprint" ""
			(at 82.55 116.84 0)
		)
		(property "Datasheet" ""
			(at 82.55 116.84 0)
		)
		(property "Description" ""
			(at 82.55 116.84 0)
		)
		(pin "1")
		(instances
			(project "Keyboard V1"
				(path
					(reference "#PWR09")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 50.8 74.93 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR05"
			(at 50.8 81.28 0)
		)
		(property "Value" "GND"
			(at 50.927 79.3242 0)
		)
		(property "Footprint" ""
			(at 50.8 74.93 0)
		)
		(property "Datasheet" ""
			(at 50.8 74.93 0)
		)
		(property "Description" ""
			(at 50.8 74.93 0)
		)
		(pin "1")
		(instances
			(project "Keyboard V1"
				(path
					(reference "#PWR05")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:+5V")
		(at 54.61 17.78 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR07"
			(at 54.61 21.59 0)
		)
		(property "Value" "+5V"
			(at 54.991 13.3858 0)
		)
		(property "Footprint" ""
			(at 54.61 17.78 0)
		)
		(property "Datasheet" ""
			(at 54.61 17.78 0)
		)
		(property "Description" ""
			(at 54.61 17.78 0)
		)
		(pin "1")
		(instances
			(project "Keyboard V1"
				(path
					(reference "#PWR07")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:+5V")
		(at 52.07 138.43 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR011"
			(at 52.07 142.24 0)
		)
		(property "Value" "+5V"
			(at 52.451 134.0358 0)
		)
		(property "Footprint" ""
			(at 52.07 138.43 0)
		)
		(property "Datasheet" ""
			(at 52.07 138.43 0)
		)
		(property "Description" ""
			(at 52.07 138.43 0)
		)
		(pin "1")
		(instances
			(project "Keyboard V1"
				(path
					(reference "#PWR011")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:C_Small")
		(at 46.99 96.52 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C6"
			(at 49.3268 95.3516 0)
		)
		(property "Value" "10uF"
			(at 49.3268 97.663 0)
		)
		(property "Footprint" "Capacitor_SMD:C_0805_2012Metric"
			(at 46.99 96.52 0)
		)
		(property "Datasheet" "https://mm.digikey.com/Volume0/opasdata/d220001/medias/docus/609/CL21A106KOQNNNE_Spec.pdf"
			(at 46.99 96.52 0)
		)
		(property "Description" "Capacitor"
			(at 46.99 96.52 0)
		)
		(property "Manufacturer" "Samsung Electro-Mechanics"
			(at 46.99 96.52 0)
		)
		(property "Manufacturer P/N" "CL21A106KOQNNNE"
			(at 46.99 96.52 0)
		)
		(property "Package" "0805_2012Metric"
			(at 46.99 96.52 0)
		)
		(property "Type" "SMD"
			(at 46.99 96.52 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "Keyboard V1"
				(path
					(reference "C6")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:+5V")
		(at 31.75 90.17 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR02"
			(at 31.75 93.98 0)
		)
		(property "Value" "+5V"
			(at 32.131 85.7758 0)
		)
		(property "Footprint" ""
			(at 31.75 90.17 0)
		)
		(property "Datasheet" ""
			(at 31.75 90.17 0)
		)
		(property "Description" ""
			(at 31.75 90.17 0)
		)
		(pin "1")
		(instances
			(project "Keyboard V1"
				(path
					(reference "#PWR02")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:+5V")
		(at 52.07 53.34 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR06"
			(at 52.07 57.15 0)
		)
		(property "Value" "+5V"
			(at 52.451 48.9458 0)
		)
		(property "Footprint" ""
			(at 52.07 53.34 0)
		)
		(property "Datasheet" ""
			(at 52.07 53.34 0)
		)
		(property "Description" ""
			(at 52.07 53.34 0)
		)
		(pin "1")
		(instances
			(project "Keyboard V1"
				(path
					(reference "#PWR06")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Connector:TestPoint")
		(at 86.36 99.06 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "F4"
			(at 91.44 99.0599 90)
		)
		(property "Value" "TestPoint"
			(at 91.44 100.3299 90)
		)
		(property "Footprint" "Connector_Wire:SolderWire-0.1sqmm_1x01_D0.4mm_OD1mm"
			(at 86.36 104.14 0)
		)
		(property "Datasheet" "~"
			(at 86.36 104.14 0)
		)
		(property "Description" "test point"
			(at 86.36 99.06 0)
		)
		(property "Manufacturer" ""
			(at 86.36 99.06 0)
		)
		(property "Manufacturer P/N" ""
			(at 86.36 99.06 0)
		)
		(property "Package" ""
			(at 86.36 99.06 0)
		)
		(property "Type" ""
			(at 86.36 99.06 0)
		)
		(pin "1")
		(instances
			(project "Keyboard V1"
				(path
					(reference "F4")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:R_Small")
		(at 49.53 58.42 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "RC2"
			(at 49.53 53.4416 90)
		)
		(property "Value" "22"
			(at 49.53 55.753 90)
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric"
			(at 49.53 58.42 0)
		)
		(property "Datasheet" "https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C301.pdf"
			(at 49.53 58.42 0)
		)
		(property "Description" "Resistor"
			(at 49.53 58.42 0)
		)
		(property "Manufacturer" "Panasonic"
			(at 49.53 58.42 0)
		)
		(property "Manufacturer P/N" "  ERJ-6GEYJ220V"
			(at 49.53 58.42 0)
		)
		(property "Package" "0805_2012Metric"
			(at 49.53 58.42 0)
		)
		(property "Type" "SMD"
			(at 49.53 58.42 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "Keyboard V1"
				(path
					(reference "RC2")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:C_Small")
		(at 30.48 35.56 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C3"
			(at 30.48 29.7434 90)
		)
		(property "Value" "22pF"
			(at 30.48 32.0548 90)
		)
		(property "Footprint" "Capacitor_SMD:C_0805_2012Metric"
			(at 30.48 35.56 0)
		)
		(property "Datasheet" "https://mm.digikey.com/Volume0/opasdata/d220001/medias/docus/5534/CL21C220JB61PNC%20Spec.pdf"
			(at 30.48 35.56 0)
		)
		(property "Description" "Capacitor"
			(at 30.48 35.56 0)
		)
		(property "Manufacturer" "Samsung Electro-Mechanics"
			(at 30.48 35.56 0)
		)
		(property "Manufacturer P/N" "CL21C220JB61PNC"
			(at 30.48 35.56 0)
		)
		(property "Package" "0805_2012Metric"
			(at 30.48 35.56 0)
		)
		(property "Type" "SMD"
			(at 30.48 35.56 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "Keyboard V1"
				(path
					(reference "C3")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:C_Small")
		(at 50.8 68.58 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C7"
			(at 53.1368 67.4116 0)
		)
		(property "Value" "1uF"
			(at 53.1368 69.723 0)
		)
		(property "Footprint" "Capacitor_SMD:C_0805_2012Metric"
			(at 50.8 68.58 0)
		)
		(property "Datasheet" "https://mm.digikey.com/Volume0/opasdata/d220001/medias/docus/1105/CL21B105KAFNNNE_Spec.pdf"
			(at 50.8 68.58 0)
		)
		(property "Description" "Capacitor"
			(at 50.8 68.58 0)
		)
		(property "Manufacturer" "Samsung Electro-Mechanics"
			(at 50.8 68.58 0)
		)
		(property "Manufacturer P/N" "CL21B105KAFNNNE"
			(at 50.8 68.58 0)
		)
		(property "Package" "0805_2012Metric"
			(at 50.8 68.58 0)
		)
		(property "Type" "SMD"
			(at 50.8 68.58 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "Keyboard V1"
				(path
					(reference "C7")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "MCU_Microchip_ATmega:ATmega32U4-M")
		(at 71.12 71.12 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "U1"
			(at 56.388 117.856 0)
		)
		(property "Value" "16MHz, 32kB Flash, 2.5kB SRAM, 1kB EEPROM, USB 2.0"
			(at 62.484 128.27 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-44-1EP_7x7mm_P0.5mm_EP5.2x5.2mm"
			(at 1.016 14.732 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-7766-8-bit-AVR-ATmega16U4-32U4_Datasheet.pdf"
			(at 25.4 9.652 0)
		)
		(property "Description" "Microcontroller"
			(at 2.286 19.812 0)
		)
		(property "Manufacturer" "Atmel"
			(at 71.12 71.12 0)
		)
		(property "Manufacturer P/N" "ATmega32U4-M"
			(at 71.12 71.12 0)
		)
		(property "Package" "QFN-44-1EP_7x7mm_P0.5mm_EP5.2x5.2mm"
			(at 71.12 71.12 0)
		)
		(property "Type" "SMD"
			(at 71.12 71.12 0)
		)
		(pin "15")
		(pin "32")
		(pin "17")
		(pin "14")
		(pin "38")
		(pin "24")
		(pin "40")
		(pin "5")
		(pin "27")
		(pin "35")
		(pin "33")
		(pin "22")
		(pin "7")
		(pin "9")
		(pin "21")
		(pin "13")
		(pin "25")
		(pin "19")
		(pin "12")
		(pin "4")
		(pin "11")
		(pin "28")
		(pin "16")
		(pin "29")
		(pin "31")
		(pin "42")
		(pin "6")
		(pin "8")
		(pin "10")
		(pin "36")
		(pin "39")
		(pin "18")
		(pin "30")
		(pin "41")
		(pin "1")
		(pin "2")
		(pin "45")
		(pin "23")
		(pin "3")
		(pin "26")
		(pin "43")
		(pin "34")
		(pin "37")
		(pin "44")
		(pin "20")
		(instances
			(project ""
				(path
					(reference "U1")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Connector:TestPoint")
		(at 86.36 96.52 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "F1"
			(at 91.44 96.5199 90)
		)
		(property "Value" "TestPoint"
			(at 91.44 97.7899 90)
		)
		(property "Footprint" "Connector_Wire:SolderWire-0.1sqmm_1x01_D0.4mm_OD1mm"
			(at 86.36 101.6 0)
		)
		(property "Datasheet" "~"
			(at 86.36 101.6 0)
		)
		(property "Description" "test point"
			(at 86.36 96.52 0)
		)
		(property "Manufacturer" ""
			(at 86.36 96.52 0)
		)
		(property "Manufacturer P/N" ""
			(at 86.36 96.52 0)
		)
		(property "Package" ""
			(at 86.36 96.52 0)
		)
		(property "Type" ""
			(at 86.36 96.52 0)
		)
		(pin "1")
		(instances
			(project "Keyboard V1"
				(path
					(reference "F1")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:C_Small")
		(at 30.48 45.72 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C4"
			(at 30.48 39.9034 90)
		)
		(property "Value" "22pF"
			(at 30.48 42.2148 90)
		)
		(property "Footprint" "Capacitor_SMD:C_0805_2012Metric"
			(at 30.48 45.72 0)
		)
		(property "Datasheet" "https://mm.digikey.com/Volume0/opasdata/d220001/medias/docus/5534/CL21C220JB61PNC%20Spec.pdf"
			(at 30.48 45.72 0)
		)
		(property "Description" "Capacitor"
			(at 30.48 45.72 0)
		)
		(property "Manufacturer" "Samsung Electro-Mechanics"
			(at 30.48 45.72 0)
		)
		(property "Manufacturer P/N" "CL21C220JB61PNC"
			(at 30.48 45.72 0)
		)
		(property "Package" "0805_2012Metric"
			(at 30.48 45.72 0)
		)
		(property "Type" "SMD"
			(at 30.48 45.72 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "Keyboard V1"
				(path
					(reference "C4")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:Crystal_GND24_Small")
		(at 43.18 40.64 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "Y1"
			(at 46.8376 39.4716 90)
		)
		(property "Value" "16MHz"
			(at 46.8376 41.783 90)
		)
		(property "Footprint" "Crystal:Crystal_SMD_3225-4Pin_3.2x2.5mm"
			(at 43.18 40.64 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/FL.pdf"
			(at 43.18 40.64 0)
		)
		(property "Description" "Crystal"
			(at 43.18 40.64 0)
		)
		(property "Manufacturer" "Diodes Incorporated"
			(at 43.18 40.64 0)
		)
		(property "Manufacturer P/N" "FL1600087"
			(at 43.18 40.64 0)
		)
		(property "Package" "4-SMD, No Lead (3.2x2.5mm)"
			(at 43.18 40.64 0)
		)
		(property "Type" "SMD"
			(at 43.18 40.64 0)
		)
		(pin "2")
		(pin "4")
		(pin "3")
		(pin "1")
		(instances
			(project "Keyboard V1"
				(path
					(reference "Y1")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 105.41 86.36 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR010"
			(at 105.41 92.71 0)
		)
		(property "Value" "GND"
			(at 105.537 90.7542 0)
		)
		(property "Footprint" ""
			(at 105.41 86.36 0)
		)
		(property "Datasheet" ""
			(at 105.41 86.36 0)
		)
		(property "Description" ""
			(at 105.41 86.36 0)
		)
		(pin "1")
		(instances
			(project "Keyboard V1"
				(path
					(reference "#PWR010")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 35.56 177.8 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR012"
			(at 35.56 184.15 0)
		)
		(property "Value" "GND"
			(at 35.687 182.1942 0)
		)
		(property "Footprint" ""
			(at 35.56 177.8 0)
		)
		(property "Datasheet" ""
			(at 35.56 177.8 0)
		)
		(property "Description" ""
			(at 35.56 177.8 0)
		)
		(pin "1")
		(instances
			(project "Keyboard V1"
				(path
					(reference "#PWR012")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:C_Small")
		(at 77.47 17.78 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C8"
			(at 79.8068 16.6116 0)
		)
		(property "Value" "0.1uF"
			(at 79.8068 18.923 0)
		)
		(property "Footprint" "Capacitor_SMD:C_0805_2012Metric"
			(at 77.47 17.78 0)
		)
		(property "Datasheet" "https://mm.digikey.com/Volume0/opasdata/d220001/medias/docus/609/CL21B104KBCNNN_Spec.pdf"
			(at 77.47 17.78 0)
		)
		(property "Description" "Capacitor"
			(at 77.47 17.78 0)
		)
		(property "Manufacturer" "Samsung Electro-Mechanics"
			(at 77.47 17.78 0)
		)
		(property "Manufacturer P/N" "CL21B104KBCNNNC"
			(at 77.47 17.78 0)
		)
		(property "Package" "0805_2012Metric"
			(at 77.47 17.78 0)
		)
		(property "Type" "SMD"
			(at 77.47 17.78 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "Keyboard V1"
				(path
					(reference "C8")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 31.75 102.87 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR03"
			(at 31.75 109.22 0)
		)
		(property "Value" "GND"
			(at 31.877 107.2642 0)
		)
		(property "Footprint" ""
			(at 31.75 102.87 0)
		)
		(property "Datasheet" ""
			(at 31.75 102.87 0)
		)
		(property "Description" ""
			(at 31.75 102.87 0)
		)
		(pin "1")
		(instances
			(project "Keyboard V1"
				(path
					(reference "#PWR03")
					(unit 1)
				)
			)
		)
	)
	(sheet
		(at 166.37 67.31)
		(size 39.37 24.13)
		(fields_autoplaced yes)
		(fill
			(color 0 0 0 0.0000)
		)
		(property "Sheetname" "Key Matrix"
			(at 166.37 66.5984 0)
		)
		(property "Sheetfile" "Sheet2.kicad_sch"
			(at 166.37 92.0246 0)
		)
		(instances
			(project "Keyboard V1"
				(path
					(page "2")
				)
			)
		)
	)
	(sheet_instances
		(path
			(page "1")
		)
	)
)
