(kicad_pcb
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A3")
	(layers
		(0 "F.Cu" signal)
		(31 "B.Cu" signal)
		(32 "B.Adhes" user "B.Adhesive")
		(33 "F.Adhes" user "F.Adhesive")
		(34 "B.Paste" user)
		(35 "F.Paste" user)
		(36 "B.SilkS" user "B.Silkscreen")
		(37 "F.SilkS" user "F.Silkscreen")
		(38 "B.Mask" user)
		(39 "F.Mask" user)
		(40 "Dwgs.User" user "User.Drawings")
		(41 "Cmts.User" user "User.Comments")
		(42 "Eco1.User" user "User.Eco1")
		(43 "Eco2.User" user "User.Eco2")
		(44 "Edge.Cuts" user)
		(45 "Margin" user)
		(46 "B.CrtYd" user "B.Courtyard")
		(47 "F.CrtYd" user "F.Courtyard")
		(48 "B.Fab" user)
		(49 "F.Fab" user)
		(50 "User.1" user)
		(51 "User.2" user)
		(52 "User.3" user)
		(53 "User.4" user)
		(54 "User.5" user)
		(55 "User.6" user)
		(56 "User.7" user)
		(57 "User.8" user)
		(58 "User.9" user)
	)
	(setup
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(pcbplotparams
			(layerselection 0x00010fc_ffffffff)
			(plot_on_all_layers_selection 0x0000000_00000000)
			(disableapertmacros no)
			(usegerberextensions yes)
			(usegerberattributes no)
			(usegerberadvancedattributes no)
			(creategerberjobfile no)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(viasonmask no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plotreference yes)
			(plotvalue yes)
			(plotfptext yes)
			(plotinvisibletext no)
			(sketchpadsonfab no)
			(subtractmaskfromsilk yes)
			(outputformat 1)
			(mirror no)
			(drillshape 0)
			(scaleselection 1)
			(outputdirectory "PDP1_IO_panel_gerbers/")
		)
	)
	(net 0 "")
	(footprint "case-solder-footprints:side-pad-fCu"
		(layer "F.Cu")
		(at 230.53 27.02 -90)
		(property "Reference" "REF**"
			(at 4.1 -5 -90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "side-pad-fCu"
			(at 4.1 -3.5 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "case-solder-footprints:side-pad-fCu"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
	)
	(footprint "case-solder-footprints:side-pad-fCu"
		(layer "F.Cu")
		(at 230.53 184.52 -90)
		(property "Reference" "REF**"
			(at 4.1 -5 -90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "side-pad-fCu"
			(at 4.1 -3.5 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "case-solder-footprints:side-pad-fCu"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
	)
	(footprint "case-solder-footprints:side-pad-fCu"
		(layer "F.Cu")
		(at 153.73 236.49 90)
		(property "Reference" "REF**"
			(at 4.1 -5 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "side-pad-fCu"
			(at 4.1 -3.5 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "case-solder-footprints:side-pad-fCu"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
	)
	(footprint "case-solder-footprints:side-pad-fCu"
		(layer "F.Cu")
		(at 230.53 132.02 -90)
		(property "Reference" "REF**"
			(at 4.1 -5 -90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "side-pad-fCu"
			(at 4.1 -3.5 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "case-solder-footprints:side-pad-fCu"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
	)
	(footprint "case-solder-footprints:side-pad-fCu"
		(layer "F.Cu")
		(at 153.73 152.49 90)
		(property "Reference" "REF**"
			(at 4.1 -5 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "side-pad-fCu"
			(at 4.1 -3.5 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "case-solder-footprints:side-pad-fCu"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
	)
	(footprint "case-solder-footprints:side-pad-fCu"
		(layer "F.Cu")
		(at 170.76 274.83 180)
		(property "Reference" "REF**"
			(at 4.1 -5 180)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "side-pad-fCu"
			(at 4.099999 -3.499998 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "case-solder-footprints:side-pad-fCu"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
	)
	(footprint "case-solder-footprints:side-pad-fCu"
		(layer "F.Cu")
		(at 170.76 22.85 180)
		(property "Reference" "REF**"
			(at 4.1 -5 180)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "side-pad-fCu"
			(at 4.099999 -3.499998 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "case-solder-footprints:side-pad-fCu"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
	)
	(footprint "case-solder-footprints:side-pad-fCu"
		(layer "F.Cu")
		(at 160.26 22.86 180)
		(property "Reference" "REF**"
			(at 4.1 -5 180)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "side-pad-fCu"
			(at 4.099999 -3.499998 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "case-solder-footprints:side-pad-fCu"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
	)
	(footprint "case-solder-footprints:side-pad-fCu"
		(layer "F.Cu")
		(at 241.96 22.86 180)
		(property "Reference" "REF**"
			(at 4.1 -5 180)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "side-pad-fCu"
			(at 4.099999 -3.499998 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "case-solder-footprints:side-pad-fCu"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
	)
	(footprint "case-solder-footprints:side-pad-fCu"
		(layer "F.Cu")
		(at 153.73 194.49 90)
		(property "Reference" "REF**"
			(at 4.1 -5 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "side-pad-fCu"
			(at 4.1 -3.5 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "case-solder-footprints:side-pad-fCu"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
	)
	(footprint "case-solder-footprints:side-pad-fCu"
		(layer "F.Cu")
		(at 230.53 247.52 -90)
		(property "Reference" "REF**"
			(at 4.1 -5 -90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "side-pad-fCu"
			(at 4.1 -3.5 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "case-solder-footprints:side-pad-fCu"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
	)
	(footprint "case-solder-footprints:side-pad-fCu"
		(layer "F.Cu")
		(at 230.53 111.02 -90)
		(property "Reference" "REF**"
			(at 4.1 -5 -90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "side-pad-fCu"
			(at 4.1 -3.5 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "case-solder-footprints:side-pad-fCu"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
	)
	(footprint "case-solder-footprints:side-pad-fCu"
		(layer "F.Cu")
		(at 153.73 141.99 90)
		(property "Reference" "REF**"
			(at 4.1 -5 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "side-pad-fCu"
			(at 4.1 -3.5 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "case-solder-footprints:side-pad-fCu"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
	)
	(footprint "case-solder-footprints:side-pad-fCu"
		(layer "F.Cu")
		(at 153.73 173.49 90)
		(property "Reference" "REF**"
			(at 4.1 -5 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "side-pad-fCu"
			(at 4.1 -3.5 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "case-solder-footprints:side-pad-fCu"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
	)
	(footprint "case-solder-footprints:side-pad-fCu"
		(layer "F.Cu")
		(at 153.73 68.49 90)
		(property "Reference" "REF**"
			(at 4.1 -5 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "side-pad-fCu"
			(at 4.1 -3.5 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "case-solder-footprints:side-pad-fCu"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
	)
	(footprint "case-solder-footprints:side-pad-fCu"
		(layer "F.Cu")
		(at 311.44 60.95)
		(property "Reference" "REF**"
			(at 4.1 -5 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "side-pad-fCu"
			(at 4.099999 -3.499998 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "case-solder-footprints:side-pad-fCu"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
	)
	(footprint "case-solder-footprints:side-pad-fCu"
		(layer "F.Cu")
		(at 230.53 226.52 -90)
		(property "Reference" "REF**"
			(at 4.1 -5 -90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "side-pad-fCu"
			(at 4.1 -3.5 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "case-solder-footprints:side-pad-fCu"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
	)
	(footprint "case-solder-footprints:side-pad-fCu"
		(layer "F.Cu")
		(at 230.53 79.52 -90)
		(property "Reference" "REF**"
			(at 4.1 -5 -90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "side-pad-fCu"
			(at 4.1 -3.5 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "case-solder-footprints:side-pad-fCu"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
	)
	(footprint "case-solder-footprints:side-pad-fCu"
		(layer "F.Cu")
		(at 249.43 20.17)
		(property "Reference" "REF**"
			(at 4.1 -5 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "side-pad-fCu"
			(at 4.099999 -3.499998 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "case-solder-footprints:side-pad-fCu"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
	)
	(footprint "case-solder-footprints:side-pad-fCu"
		(layer "F.Cu")
		(at 202.25 22.85 180)
		(property "Reference" "REF**"
			(at 4.1 -5 180)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "side-pad-fCu"
			(at 4.099999 -3.499998 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "case-solder-footprints:side-pad-fCu"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
	)
	(footprint "case-solder-footprints:side-pad-fCu"
		(layer "F.Cu")
		(at 230.53 100.52 -90)
		(property "Reference" "REF**"
			(at 4.1 -5 -90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "side-pad-fCu"
			(at 4.1 -3.5 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "case-solder-footprints:side-pad-fCu"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
	)
	(footprint "case-solder-footprints:side-pad-fCu"
		(layer "F.Cu")
		(at 311.39 224.1)
		(property "Reference" "REF**"
			(at 4.1 -5 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "side-pad-fCu"
			(at 4.099999 -3.499998 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "case-solder-footprints:side-pad-fCu"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
	)
	(footprint "case-solder-footprints:side-pad-fCu"
		(layer "F.Cu")
		(at 328.94 60.96)
		(property "Reference" "REF**"
			(at 4.1 -5 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "side-pad-fCu"
			(at 4.099999 -3.499998 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "case-solder-footprints:side-pad-fCu"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
	)
	(footprint "case-solder-footprints:side-pad-fCu"
		(layer "F.Cu")
		(at 238.93 272.16)
		(property "Reference" "REF**"
			(at 4.1 -5 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "side-pad-fCu"
			(at 4.099999 -3.499998 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "case-solder-footprints:side-pad-fCu"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
	)
	(footprint "case-solder-footprints:side-pad-fCu"
		(layer "F.Cu")
		(at 153.73 131.49 90)
		(property "Reference" "REF**"
			(at 4.1 -5 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "side-pad-fCu"
			(at 4.1 -3.5 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "case-solder-footprints:side-pad-fCu"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
	)
	(footprint "case-solder-footprints:side-pad-fCu"
		(layer "F.Cu")
		(at 153.73 120.99 90)
		(property "Reference" "REF**"
			(at 4.1 -5 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "side-pad-fCu"
			(at 4.1 -3.5 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "case-solder-footprints:side-pad-fCu"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
	)
	(footprint "case-solder-footprints:side-pad-fCu"
		(layer "F.Cu")
		(at 353.38 224.1)
		(property "Reference" "REF**"
			(at 4.1 -5 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "side-pad-fCu"
			(at 4.099999 -3.499998 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "case-solder-footprints:side-pad-fCu"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
	)
	(footprint "case-solder-footprints:side-pad-fCu"
		(layer "F.Cu")
		(at 153.73 99.99 90)
		(property "Reference" "REF**"
			(at 4.1 -5 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "side-pad-fCu"
			(at 4.1 -3.5 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "case-solder-footprints:side-pad-fCu"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
	)
	(footprint "case-solder-footprints:side-pad-fCu"
		(layer "F.Cu")
		(at 241.96 274.86 180)
		(property "Reference" "REF**"
			(at 4.1 -5 180)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "side-pad-fCu"
			(at 4.099999 -3.499998 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "case-solder-footprints:side-pad-fCu"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
	)
	(footprint "case-solder-footprints:side-pad-fCu"
		(layer "F.Cu")
		(at 191.76 22.86 180)
		(property "Reference" "REF**"
			(at 4.1 -5 180)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "side-pad-fCu"
			(at 4.099999 -3.499998 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "case-solder-footprints:side-pad-fCu"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
	)
	(footprint "case-solder-footprints:side-pad-fCu"
		(layer "F.Cu")
		(at 153.73 246.99 90)
		(property "Reference" "REF**"
			(at 4.1 -5 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "side-pad-fCu"
			(at 4.1 -3.5 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "case-solder-footprints:side-pad-fCu"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
	)
	(footprint "case-solder-footprints:side-pad-fCu"
		(layer "F.Cu")
		(at 363.88 224.09)
		(property "Reference" "REF**"
			(at 4.1 -5 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "side-pad-fCu"
			(at 4.099999 -3.499998 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "case-solder-footprints:side-pad-fCu"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
	)
	(footprint "case-solder-footprints:side-pad-fCu"
		(layer "F.Cu")
		(at 230.53 90.02 -90)
		(property "Reference" "REF**"
			(at 4.1 -5 -90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "side-pad-fCu"
			(at 4.1 -3.5 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "case-solder-footprints:side-pad-fCu"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
	)
	(footprint "case-solder-footprints:side-pad-fCu"
		(layer "F.Cu")
		(at 153.73 36.99 90)
		(property "Reference" "REF**"
			(at 4.1 -5 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "side-pad-fCu"
			(at 4.1 -3.5 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "case-solder-footprints:side-pad-fCu"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
	)
	(footprint "case-solder-footprints:side-pad-fCu"
		(layer "F.Cu")
		(at 191.76 274.84 180)
		(property "Reference" "REF**"
			(at 4.1 -5 180)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "side-pad-fCu"
			(at 4.099999 -3.499998 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "case-solder-footprints:side-pad-fCu"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
	)
	(footprint "case-solder-footprints:side-pad-fCu"
		(layer "F.Cu")
		(at 153.73 47.49 90)
		(property "Reference" "REF**"
			(at 4.1 -5 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "side-pad-fCu"
			(at 4.1 -3.5 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "case-solder-footprints:side-pad-fCu"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
	)
	(footprint "case-solder-footprints:side-pad-fCu"
		(layer "F.Cu")
		(at 230.53 237.02 -90)
		(property "Reference" "REF**"
			(at 4.1 -5 -90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "side-pad-fCu"
			(at 4.1 -3.5 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "case-solder-footprints:side-pad-fCu"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
	)
	(footprint "case-solder-footprints:side-pad-fCu"
		(layer "F.Cu")
		(at 153.73 215.49 90)
		(property "Reference" "REF**"
			(at 4.1 -5 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "side-pad-fCu"
			(at 4.1 -3.5 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "case-solder-footprints:side-pad-fCu"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
	)
	(footprint "case-solder-footprints:side-pad-fCu"
		(layer "F.Cu")
		(at 153.73 267.99 90)
		(property "Reference" "REF**"
			(at 4.1 -5 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "side-pad-fCu"
			(at 4.1 -3.5 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "case-solder-footprints:side-pad-fCu"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
	)
	(footprint "case-solder-footprints:side-pad-fCu"
		(layer "F.Cu")
		(at 153.73 183.99 90)
		(property "Reference" "REF**"
			(at 4.1 -5 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "side-pad-fCu"
			(at 4.1 -3.5 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "case-solder-footprints:side-pad-fCu"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
	)
	(footprint "case-solder-footprints:side-pad-fCu"
		(layer "F.Cu")
		(at 181.26 22.85 180)
		(property "Reference" "REF**"
			(at 4.1 -5 180)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "side-pad-fCu"
			(at 4.099999 -3.499998 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "case-solder-footprints:side-pad-fCu"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
	)
	(footprint "case-solder-footprints:side-pad-fCu"
		(layer "F.Cu")
		(at 230.53 163.52 -90)
		(property "Reference" "REF**"
			(at 4.1 -5 -90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "side-pad-fCu"
			(at 4.1 -3.5 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "case-solder-footprints:side-pad-fCu"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
	)
	(footprint "case-solder-footprints:side-pad-fCu"
		(layer "F.Cu")
		(at 153.73 110.49 90)
		(property "Reference" "REF**"
			(at 4.1 -5 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "side-pad-fCu"
			(at 4.1 -3.5 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "case-solder-footprints:side-pad-fCu"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
	)
	(footprint "case-solder-footprints:side-pad-fCu"
		(layer "F.Cu")
		(at 230.53 69.02 -90)
		(property "Reference" "REF**"
			(at 4.1 -5 -90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "side-pad-fCu"
			(at 4.1 -3.5 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "case-solder-footprints:side-pad-fCu"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
	)
	(footprint "case-solder-footprints:side-pad-fCu"
		(layer "F.Cu")
		(at 153.73 257.49 90)
		(property "Reference" "REF**"
			(at 4.1 -5 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "side-pad-fCu"
			(at 4.1 -3.5 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "case-solder-footprints:side-pad-fCu"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
	)
	(footprint "case-solder-footprints:side-pad-fCu"
		(layer "F.Cu")
		(at 153.73 78.99 90)
		(property "Reference" "REF**"
			(at 4.1 -5 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "side-pad-fCu"
			(at 4.1 -3.5 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "case-solder-footprints:side-pad-fCu"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
	)
	(footprint "case-solder-footprints:side-pad-fCu"
		(layer "F.Cu")
		(at 321.89 224.1)
		(property "Reference" "REF**"
			(at 4.1 -5 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "side-pad-fCu"
			(at 4.099999 -3.499998 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "case-solder-footprints:side-pad-fCu"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
	)
	(footprint "case-solder-footprints:side-pad-fCu"
		(layer "F.Cu")
		(at 153.73 204.99 90)
		(property "Reference" "REF**"
			(at 4.1 -5 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "side-pad-fCu"
			(at 4.1 -3.5 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "case-solder-footprints:side-pad-fCu"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
	)
	(footprint "case-solder-footprints:side-pad-fCu"
		(layer "F.Cu")
		(at 153.73 162.99 90)
		(property "Reference" "REF**"
			(at 4.1 -5 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "side-pad-fCu"
			(at 4.1 -3.5 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "case-solder-footprints:side-pad-fCu"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
	)
	(footprint "case-solder-footprints:side-pad-fCu"
		(layer "F.Cu")
		(at 230.53 174.02 -90)
		(property "Reference" "REF**"
			(at 4.1 -5 -90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "side-pad-fCu"
			(at 4.1 -3.5 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "case-solder-footprints:side-pad-fCu"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
	)
	(footprint "case-solder-footprints:side-pad-fCu"
		(layer "F.Cu")
		(at 230.53 121.52 -90)
		(property "Reference" "REF**"
			(at 4.1 -5 -90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "side-pad-fCu"
			(at 4.1 -3.5 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "case-solder-footprints:side-pad-fCu"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
	)
	(footprint "case-solder-footprints:side-pad-fCu"
		(layer "F.Cu")
		(at 342.88 224.1)
		(property "Reference" "REF**"
			(at 4.1 -5 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "side-pad-fCu"
			(at 4.099999 -3.499998 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "case-solder-footprints:side-pad-fCu"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
	)
	(footprint "case-solder-footprints:slot-solder-pad"
		(layer "F.Cu")
		(at 309.13 73.879999 90)
		(property "Reference" "REF**"
			(at 4.1 -5 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "slot-solder-pad"
			(at 4.1 -3.5 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "case-solder-footprints:slot-solder-pad"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
	)
	(footprint "case-solder-footprints:side-pad-fCu"
		(layer "F.Cu")
		(at 230.53 195.02 -90)
		(property "Reference" "REF**"
			(at 4.1 -5 -90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "side-pad-fCu"
			(at 4.1 -3.5 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "case-solder-footprints:side-pad-fCu"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
	)
	(footprint "case-solder-footprints:side-pad-fCu"
		(layer "F.Cu")
		(at 238.93 20.16)
		(property "Reference" "REF**"
			(at 4.1 -5 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "side-pad-fCu"
			(at 4.099999 -3.499998 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "case-solder-footprints:side-pad-fCu"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
	)
	(footprint "case-solder-footprints:side-pad-fCu"
		(layer "F.Cu")
		(at 153.73 89.49 90)
		(property "Reference" "REF**"
			(at 4.1 -5 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "side-pad-fCu"
			(at 4.1 -3.5 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "case-solder-footprints:side-pad-fCu"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
	)
	(footprint "case-solder-footprints:slot-solder-pad"
		(layer "F.Cu")
		(at 310.13 213.890001 -90)
		(property "Reference" "REF**"
			(at 4.1 -5 -90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "slot-solder-pad"
			(at 4.1 -3.5 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "case-solder-footprints:slot-solder-pad"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
	)
	(footprint "case-solder-footprints:side-pad-fCu"
		(layer "F.Cu")
		(at 230.53 205.52 -90)
		(property "Reference" "REF**"
			(at 4.1 -5 -90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "side-pad-fCu"
			(at 4.1 -3.5 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "case-solder-footprints:side-pad-fCu"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
	)
	(footprint "case-solder-footprints:side-pad-fCu"
		(layer "F.Cu")
		(at 230.53 153.02 -90)
		(property "Reference" "REF**"
			(at 4.1 -5 -90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "side-pad-fCu"
			(at 4.1 -3.5 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "case-solder-footprints:side-pad-fCu"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
	)
	(footprint "case-solder-footprints:side-pad-fCu"
		(layer "F.Cu")
		(at 181.26 274.83 180)
		(property "Reference" "REF**"
			(at 4.1 -5 180)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "side-pad-fCu"
			(at 4.099999 -3.499998 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "case-solder-footprints:side-pad-fCu"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
	)
	(footprint "case-solder-footprints:side-pad-fCu"
		(layer "F.Cu")
		(at 153.73 225.99 90)
		(property "Reference" "REF**"
			(at 4.1 -5 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "side-pad-fCu"
			(at 4.1 -3.5 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "case-solder-footprints:side-pad-fCu"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
	)
	(footprint "case-solder-footprints:side-pad-fCu"
		(layer "F.Cu")
		(at 153.73 57.99 90)
		(property "Reference" "REF**"
			(at 4.1 -5 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "side-pad-fCu"
			(at 4.1 -3.5 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "case-solder-footprints:side-pad-fCu"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
	)
	(footprint "case-solder-footprints:side-pad-fCu"
		(layer "F.Cu")
		(at 230.53 142.52 -90)
		(property "Reference" "REF**"
			(at 4.1 -5 -90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "side-pad-fCu"
			(at 4.1 -3.5 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "case-solder-footprints:side-pad-fCu"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
	)
	(footprint "case-solder-footprints:side-pad-fCu"
		(layer "F.Cu")
		(at 230.53 37.52 -90)
		(property "Reference" "REF**"
			(at 4.1 -5 -90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "side-pad-fCu"
			(at 4.1 -3.5 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "case-solder-footprints:side-pad-fCu"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
	)
	(footprint "case-solder-footprints:side-pad-fCu"
		(layer "F.Cu")
		(at 230.53 216.02 -90)
		(property "Reference" "REF**"
			(at 4.1 -5 -90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "side-pad-fCu"
			(at 4.1 -3.5 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "case-solder-footprints:side-pad-fCu"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
	)
	(footprint "case-solder-footprints:side-pad-fCu"
		(layer "F.Cu")
		(at 249.43 272.16)
		(property "Reference" "REF**"
			(at 4.1 -5 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "side-pad-fCu"
			(at 4.099999 -3.499998 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "case-solder-footprints:side-pad-fCu"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
	)
	(footprint "case-solder-footprints:side-pad-fCu"
		(layer "F.Cu")
		(at 212.75 22.85 180)
		(property "Reference" "REF**"
			(at 4.1 -5 180)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "side-pad-fCu"
			(at 4.099999 -3.499998 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "case-solder-footprints:side-pad-fCu"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
	)
	(footprint "case-solder-footprints:side-pad-fCu"
		(layer "F.Cu")
		(at 332.38 224.09)
		(property "Reference" "REF**"
			(at 4.1 -5 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "side-pad-fCu"
			(at 4.099999 -3.499998 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "case-solder-footprints:side-pad-fCu"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
	)
	(footprint "case-solder-footprints:side-pad-fCu"
		(layer "F.Cu")
		(at 230.53 258.02 -90)
		(property "Reference" "REF**"
			(at 4.1 -5 -90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "side-pad-fCu"
			(at 4.1 -3.5 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "case-solder-footprints:side-pad-fCu"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
	)
	(footprint "case-solder-footprints:side-pad-fCu"
		(layer "F.Cu")
		(at 318.44 60.95)
		(property "Reference" "REF**"
			(at 4.1 -5 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "side-pad-fCu"
			(at 4.099999 -3.499998 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "case-solder-footprints:side-pad-fCu"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
	)
	(footprint "case-solder-footprints:side-pad-fCu"
		(layer "F.Cu")
		(at 230.53 58.52 -90)
		(property "Reference" "REF**"
			(at 4.1 -5 -90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "side-pad-fCu"
			(at 4.1 -3.5 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "case-solder-footprints:side-pad-fCu"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
	)
	(footprint "case-solder-footprints:side-pad-fCu"
		(layer "F.Cu")
		(at 202.25 274.83 180)
		(property "Reference" "REF**"
			(at 4.1 -5 180)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "side-pad-fCu"
			(at 4.099999 -3.499998 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "case-solder-footprints:side-pad-fCu"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
	)
	(footprint "case-solder-footprints:side-pad-fCu"
		(layer "F.Cu")
		(at 230.53 48.02 -90)
		(property "Reference" "REF**"
			(at 4.1 -5 -90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "side-pad-fCu"
			(at 4.1 -3.5 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "case-solder-footprints:side-pad-fCu"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
	)
	(footprint "case-solder-footprints:side-pad-fCu"
		(layer "F.Cu")
		(at 160.26 274.84 180)
		(property "Reference" "REF**"
			(at 4.1 -5 180)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "side-pad-fCu"
			(at 4.099999 -3.499998 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "case-solder-footprints:side-pad-fCu"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
	)
	(footprint "case-solder-footprints:side-pad-fCu"
		(layer "F.Cu")
		(at 212.75 274.83 180)
		(property "Reference" "REF**"
			(at 4.1 -5 180)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "side-pad-fCu"
			(at 4.099999 -3.499998 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "case-solder-footprints:side-pad-fCu"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
	)
	(footprint "case-solder-footprints:side-pad-fCu"
		(layer "B.Cu")
		(at 88.02 60.96 180)
		(property "Reference" "REF**"
			(at 4.1 5 0)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "side-pad-fCu"
			(at 4.099999 3.499998 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "case-solder-footprints:side-pad-fCu"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(attr smd)
	)
	(footprint "case-solder-footprints:side-pad-fCu"
		(layer "B.Cu")
		(at 103.350001 310.53 -90)
		(property "Reference" "REF**"
			(at 4.1 5 90)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "side-pad-fCu"
			(at 4.1 3.5 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "case-solder-footprints:side-pad-fCu"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(attr smd)
	)
	(footprint "case-solder-footprints:side-pad-fCu"
		(layer "B.Cu")
		(at 246.190001 309.16 180)
		(property "Reference" "REF**"
			(at 4.1 5 0)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "side-pad-fCu"
			(at 4.1 3.5 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "case-solder-footprints:side-pad-fCu"
			(at 0 0 360)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 360)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 360)
			(layer "B.Fab")
			(hide yes)
		)
		(attr smd)
	)
	(footprint "case-solder-footprints:side-pad-fCu"
		(layer "B.Cu")
		(at 131.210001 379.6)
		(property "Reference" "REF**"
			(at 4.1 5 180)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "side-pad-fCu"
			(at 4.1 3.5 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "case-solder-footprints:side-pad-fCu"
			(at 0 0 360)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 360)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 360)
			(layer "B.Fab")
			(hide yes)
		)
		(attr smd)
	)
	(footprint "case-solder-footprints:side-pad-fCu"
		(layer "B.Cu")
		(at 299.210001 379.3)
		(property "Reference" "REF**"
			(at 4.1 5 180)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "side-pad-fCu"
			(at 4.1 3.5 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "case-solder-footprints:side-pad-fCu"
			(at 0 0 360)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 360)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 360)
			(layer "B.Fab")
			(hide yes)
		)
		(attr smd)
	)
	(footprint "case-solder-footprints:side-pad-fCu"
		(layer "B.Cu")
		(at 103.350001 346.99 -90)
		(property "Reference" "REF**"
			(at 4.1 5 90)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "side-pad-fCu"
			(at 4.1 3.5 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "case-solder-footprints:side-pad-fCu"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(attr smd)
	)
	(footprint "case-solder-footprints:slot-solder-pad-back"
		(layer "B.Cu")
		(at 261.83 222.71 90)
		(property "Reference" "REF**"
			(at 4.1 5 -90)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "slot-solder-pad-back"
			(at 4.1 3.5 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "case-solder-footprints:slot-solder-pad-back"
			(at 0 0 -90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "B.Fab")
			(hide yes)
		)
		(attr smd)
	)
	(footprint "case-solder-footprints:slot-solder-pad-back"
		(layer "B.Cu")
		(at 261.83 72.31 90)
		(property "Reference" "REF**"
			(at 4.1 5 -90)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "slot-solder-pad-back"
			(at 4.1 3.5 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "case-solder-footprints:slot-solder-pad-back"
			(at 0 0 -90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "B.Fab")
			(hide yes)
		)
		(attr smd)
	)
	(footprint "case-solder-footprints:side-pad-fCu"
		(layer "B.Cu")
		(at 103.350001 321.03 -90)
		(property "Reference" "REF**"
			(at 4.1 5 90)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "side-pad-fCu"
			(at 4.1 3.5 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "case-solder-footprints:side-pad-fCu"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(attr smd)
	)
	(footprint "case-solder-footprints:side-pad-fCu"
		(layer "B.Cu")
		(at 351.190001 309.16 180)
		(property "Reference" "REF**"
			(at 4.1 5 0)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "side-pad-fCu"
			(at 4.1 3.5 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "case-solder-footprints:side-pad-fCu"
			(at 0 0 360)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 360)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 360)
			(layer "B.Fab")
			(hide yes)
		)
		(attr smd)
	)
	(footprint "case-solder-footprints:slot-solder-pad-back"
		(layer "B.Cu")
		(at 261.83 147.51 90)
		(property "Reference" "REF**"
			(at 4.1 5 -90)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "slot-solder-pad-back"
			(at 4.1 3.5 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "case-solder-footprints:slot-solder-pad-back"
			(at 0 0 -90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "B.Fab")
			(hide yes)
		)
		(attr smd)
	)
	(footprint "case-solder-footprints:side-pad-fCu"
		(layer "B.Cu")
		(at 330.710001 379.6)
		(property "Reference" "REF**"
			(at 4.1 5 180)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "side-pad-fCu"
			(at 4.1 3.5 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "case-solder-footprints:side-pad-fCu"
			(at 0 0 360)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 360)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 360)
			(layer "B.Fab")
			(hide yes)
		)
		(attr smd)
	)
	(footprint "case-solder-footprints:side-pad-fCu"
		(layer "B.Cu")
		(at 277.690001 309.16 180)
		(property "Reference" "REF**"
			(at 4.1 5 0)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "side-pad-fCu"
			(at 4.1 3.5 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "case-solder-footprints:side-pad-fCu"
			(at 0 0 360)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 360)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 360)
			(layer "B.Fab")
			(hide yes)
		)
		(attr smd)
	)
	(footprint "case-solder-footprints:side-pad-fCu"
		(layer "B.Cu")
		(at 298.690001 309.16 180)
		(property "Reference" "REF**"
			(at 4.1 5 0)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "side-pad-fCu"
			(at 4.1 3.5 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "case-solder-footprints:side-pad-fCu"
			(at 0 0 360)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 360)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 360)
			(layer "B.Fab")
			(hide yes)
		)
		(attr smd)
	)
	(footprint "case-solder-footprints:side-pad-fCu"
		(layer "B.Cu")
		(at 173.210001 379.6)
		(property "Reference" "REF**"
			(at 4.1 5 180)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "side-pad-fCu"
			(at 4.1 3.5 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "case-solder-footprints:side-pad-fCu"
			(at 0 0 360)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 360)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 360)
			(layer "B.Fab")
			(hide yes)
		)
		(attr smd)
	)
	(footprint "case-solder-footprints:side-pad-fCu"
		(layer "B.Cu")
		(at 95.07 224.1 180)
		(property "Reference" "REF**"
			(at 4.1 5 0)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "side-pad-fCu"
			(at 4.099999 3.499998 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "case-solder-footprints:side-pad-fCu"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(attr smd)
	)
	(footprint "case-solder-footprints:side-pad-fCu"
		(layer "B.Cu")
		(at 84.58 224.09 180)
		(property "Reference" "REF**"
			(at 4.1 5 0)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "side-pad-fCu"
			(at 4.099999 3.499998 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "case-solder-footprints:side-pad-fCu"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(attr smd)
	)
	(footprint "case-solder-footprints:side-pad-fCu"
		(layer "B.Cu")
		(at 278.210001 379.6)
		(property "Reference" "REF**"
			(at 4.1 5 180)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "side-pad-fCu"
			(at 4.1 3.5 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "case-solder-footprints:side-pad-fCu"
			(at 0 0 360)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 360)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 360)
			(layer "B.Fab")
			(hide yes)
		)
		(attr smd)
	)
	(footprint "case-solder-footprints:side-pad-fCu"
		(layer "B.Cu")
		(at 63.58 224.1 180)
		(property "Reference" "REF**"
			(at 4.1 5 0)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "side-pad-fCu"
			(at 4.099999 3.499998 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "case-solder-footprints:side-pad-fCu"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(attr smd)
	)
	(footprint "case-solder-footprints:side-pad-fCu"
		(layer "B.Cu")
		(at 98.52 60.95 180)
		(property "Reference" "REF**"
			(at 4.1 5 0)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "side-pad-fCu"
			(at 4.099999 3.499998 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "case-solder-footprints:side-pad-fCu"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(attr smd)
	)
	(footprint "case-solder-footprints:side-pad-fCu"
		(layer "B.Cu")
		(at 105.57 224.1 180)
		(property "Reference" "REF**"
			(at 4.1 5 0)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "side-pad-fCu"
			(at 4.099999 3.499998 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "case-solder-footprints:side-pad-fCu"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(attr smd)
	)
	(footprint "case-solder-footprints:side-pad-fCu"
		(layer "B.Cu")
		(at 267.710001 379.6)
		(property "Reference" "REF**"
			(at 4.1 5 180)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "side-pad-fCu"
			(at 4.1 3.5 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "case-solder-footprints:side-pad-fCu"
			(at 0 0 360)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 360)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 360)
			(layer "B.Fab")
			(hide yes)
		)
		(attr smd)
	)
	(footprint "case-solder-footprints:side-pad-fCu"
		(layer "B.Cu")
		(at 141.710001 379.6)
		(property "Reference" "REF**"
			(at 4.1 5 180)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "side-pad-fCu"
			(at 4.1 3.5 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "case-solder-footprints:side-pad-fCu"
			(at 0 0 360)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 360)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 360)
			(layer "B.Fab")
			(hide yes)
		)
		(attr smd)
	)
	(footprint "case-solder-footprints:side-pad-fCu"
		(layer "B.Cu")
		(at 74.08 224.1 180)
		(property "Reference" "REF**"
			(at 4.1 5 0)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "side-pad-fCu"
			(at 4.099999 3.499998 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "case-solder-footprints:side-pad-fCu"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(attr smd)
	)
	(footprint "case-solder-footprints:side-pad-fCu"
		(layer "B.Cu")
		(at 235.690001 309.46 180)
		(property "Reference" "REF**"
			(at 4.1 5 0)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "side-pad-fCu"
			(at 4.1 3.5 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "case-solder-footprints:side-pad-fCu"
			(at 0 0 360)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 360)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 360)
			(layer "B.Fab")
			(hide yes)
		)
		(attr smd)
	)
	(footprint "case-solder-footprints:side-pad-fCu"
		(layer "B.Cu")
		(at 320.210001 379.6)
		(property "Reference" "REF**"
			(at 4.1 5 180)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "side-pad-fCu"
			(at 4.1 3.5 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "case-solder-footprints:side-pad-fCu"
			(at 0 0 360)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 360)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 360)
			(layer "B.Fab")
			(hide yes)
		)
		(attr smd)
	)
	(footprint "case-solder-footprints:side-pad-fCu"
		(layer "B.Cu")
		(at 214.690001 309.16 180)
		(property "Reference" "REF**"
			(at 4.1 5 0)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "side-pad-fCu"
			(at 4.1 3.5 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "case-solder-footprints:side-pad-fCu"
			(at 0 0 360)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 360)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 360)
			(layer "B.Fab")
			(hide yes)
		)
		(attr smd)
	)
	(footprint "case-solder-footprints:side-pad-fCu"
		(layer "B.Cu")
		(at 193.690001 309.16 180)
		(property "Reference" "REF**"
			(at 4.1 5 0)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "side-pad-fCu"
			(at 4.1 3.5 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "case-solder-footprints:side-pad-fCu"
			(at 0 0 360)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 360)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 360)
			(layer "B.Fab")
			(hide yes)
		)
		(attr smd)
	)
	(footprint "case-solder-footprints:side-pad-fCu"
		(layer "B.Cu")
		(at 120.190001 309.16 180)
		(property "Reference" "REF**"
			(at 4.1 5 0)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "side-pad-fCu"
			(at 4.1 3.5 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "case-solder-footprints:side-pad-fCu"
			(at 0 0 360)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 360)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 360)
			(layer "B.Fab")
			(hide yes)
		)
		(attr smd)
	)
	(footprint "case-solder-footprints:side-pad-fCu"
		(layer "B.Cu")
		(at 358.050001 378.23 90)
		(property "Reference" "REF**"
			(at 4.1 5 -90)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "side-pad-fCu"
			(at 4.1 3.5 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "case-solder-footprints:side-pad-fCu"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(attr smd)
	)
	(footprint "case-solder-footprints:side-pad-fCu"
		(layer "B.Cu")
		(at 53.08 224.09 180)
		(property "Reference" "REF**"
			(at 4.1 5 0)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "side-pad-fCu"
			(at 4.099999 3.499998 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "case-solder-footprints:side-pad-fCu"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(attr smd)
	)
	(footprint "case-solder-footprints:side-pad-fCu"
		(layer "B.Cu")
		(at 309.710001 379.6)
		(property "Reference" "REF**"
			(at 4.1 5 180)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "side-pad-fCu"
			(at 4.1 3.5 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "case-solder-footprints:side-pad-fCu"
			(at 0 0 360)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 360)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 360)
			(layer "B.Fab")
			(hide yes)
		)
		(attr smd)
	)
	(footprint "case-solder-footprints:side-pad-fCu"
		(layer "B.Cu")
		(at 225.710001 379.3)
		(property "Reference" "REF**"
			(at 4.1 5 180)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "side-pad-fCu"
			(at 4.1 3.5 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "case-solder-footprints:side-pad-fCu"
			(at 0 0 360)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 360)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 360)
			(layer "B.Fab")
			(hide yes)
		)
		(attr smd)
	)
	(footprint "case-solder-footprints:side-pad-fCu"
		(layer "B.Cu")
		(at 358.050001 357.23 90)
		(property "Reference" "REF**"
			(at 4.1 5 -90)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "side-pad-fCu"
			(at 4.1 3.5 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "case-solder-footprints:side-pad-fCu"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(attr smd)
	)
	(footprint "case-solder-footprints:side-pad-fCu"
		(layer "B.Cu")
		(at 110.210001 379.6)
		(property "Reference" "REF**"
			(at 4.1 5 180)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "side-pad-fCu"
			(at 4.1 3.5 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "case-solder-footprints:side-pad-fCu"
			(at 0 0 360)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 360)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 360)
			(layer "B.Fab")
			(hide yes)
		)
		(attr smd)
	)
	(footprint "case-solder-footprints:side-pad-fCu"
		(layer "B.Cu")
		(at 172.690001 309.16 180)
		(property "Reference" "REF**"
			(at 4.1 5 0)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "side-pad-fCu"
			(at 4.1 3.5 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "case-solder-footprints:side-pad-fCu"
			(at 0 0 360)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 360)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 360)
			(layer "B.Fab")
			(hide yes)
		)
		(attr smd)
	)
	(footprint "case-solder-footprints:side-pad-fCu"
		(layer "B.Cu")
		(at 358.050001 320.77 90)
		(property "Reference" "REF**"
			(at 4.1 5 -90)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "side-pad-fCu"
			(at 4.1 3.5 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "case-solder-footprints:side-pad-fCu"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(attr smd)
	)
	(footprint "case-solder-footprints:side-pad-fCu"
		(layer "B.Cu")
		(at 130.690001 309.16 180)
		(property "Reference" "REF**"
			(at 4.1 5 0)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "side-pad-fCu"
			(at 4.1 3.5 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "case-solder-footprints:side-pad-fCu"
			(at 0 0 360)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 360)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 360)
			(layer "B.Fab")
			(hide yes)
		)
		(attr smd)
	)
	(footprint "case-solder-footprints:side-pad-fCu"
		(layer "B.Cu")
		(at 204.710001 379.6)
		(property "Reference" "REF**"
			(at 4.1 5 180)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "side-pad-fCu"
			(at 4.1 3.5 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "case-solder-footprints:side-pad-fCu"
			(at 0 0 360)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 360)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 360)
			(layer "B.Fab")
			(hide yes)
		)
		(attr smd)
	)
	(footprint "case-solder-footprints:side-pad-fCu"
		(layer "B.Cu")
		(at 288.710001 379.6)
		(property "Reference" "REF**"
			(at 4.1 5 180)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "side-pad-fCu"
			(at 4.1 3.5 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "case-solder-footprints:side-pad-fCu"
			(at 0 0 360)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 360)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 360)
			(layer "B.Fab")
			(hide yes)
		)
		(attr smd)
	)
	(footprint "case-solder-footprints:slot-solder-pad"
		(layer "B.Cu")
		(at 107.83 73.879999 90)
		(property "Reference" "REF**"
			(at 4.1 5 -90)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "slot-solder-pad"
			(at 4.1 3.5 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "case-solder-footprints:slot-solder-pad"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(attr smd)
	)
	(footprint "case-solder-footprints:slot-solder-pad"
		(layer "B.Cu")
		(at 106.83 213.890001 -90)
		(property "Reference" "REF**"
			(at 4.1 5 90)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "slot-solder-pad"
			(at 4.1 3.5 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "case-solder-footprints:slot-solder-pad"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(attr smd)
	)
	(footprint "case-solder-footprints:side-pad-fCu"
		(layer "B.Cu")
		(at 340.690001 309.16 180)
		(property "Reference" "REF**"
			(at 4.1 5 0)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "side-pad-fCu"
			(at 4.1 3.5 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "case-solder-footprints:side-pad-fCu"
			(at 0 0 360)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 360)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 360)
			(layer "B.Fab")
			(hide yes)
		)
		(attr smd)
	)
	(footprint "case-solder-footprints:side-pad-fCu"
		(layer "B.Cu")
		(at 257.210001 379.6)
		(property "Reference" "REF**"
			(at 4.1 5 180)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "side-pad-fCu"
			(at 4.1 3.5 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "case-solder-footprints:side-pad-fCu"
			(at 0 0 360)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 360)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 360)
			(layer "B.Fab")
			(hide yes)
		)
		(attr smd)
	)
	(footprint "case-solder-footprints:side-pad-fCu"
		(layer "B.Cu")
		(at 236.210001 379.6)
		(property "Reference" "REF**"
			(at 4.1 5 180)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "side-pad-fCu"
			(at 4.1 3.5 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "case-solder-footprints:side-pad-fCu"
			(at 0 0 360)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 360)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 360)
			(layer "B.Fab")
			(hide yes)
		)
		(attr smd)
	)
	(footprint "case-solder-footprints:side-pad-fCu"
		(layer "B.Cu")
		(at 267.190001 309.16 180)
		(property "Reference" "REF**"
			(at 4.1 5 0)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "side-pad-fCu"
			(at 4.1 3.5 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "case-solder-footprints:side-pad-fCu"
			(at 0 0 360)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 360)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 360)
			(layer "B.Fab")
			(hide yes)
		)
		(attr smd)
	)
	(footprint "case-solder-footprints:side-pad-fCu"
		(layer "B.Cu")
		(at 151.690001 309.16 180)
		(property "Reference" "REF**"
			(at 4.1 5 0)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "side-pad-fCu"
			(at 4.1 3.5 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "case-solder-footprints:side-pad-fCu"
			(at 0 0 360)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 360)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 360)
			(layer "B.Fab")
			(hide yes)
		)
		(attr smd)
	)
	(footprint "case-solder-footprints:side-pad-fCu"
		(layer "B.Cu")
		(at 162.190001 309.46 180)
		(property "Reference" "REF**"
			(at 4.1 5 0)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "side-pad-fCu"
			(at 4.1 3.5 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "case-solder-footprints:side-pad-fCu"
			(at 0 0 360)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 360)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 360)
			(layer "B.Fab")
			(hide yes)
		)
		(attr smd)
	)
	(footprint "case-solder-footprints:side-pad-fCu"
		(layer "B.Cu")
		(at 120.710001 379.6)
		(property "Reference" "REF**"
			(at 4.1 5 180)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "side-pad-fCu"
			(at 4.1 3.5 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "case-solder-footprints:side-pad-fCu"
			(at 0 0 360)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 360)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 360)
			(layer "B.Fab")
			(hide yes)
		)
		(attr smd)
	)
	(footprint "case-solder-footprints:side-pad-fCu"
		(layer "B.Cu")
		(at 358.050001 367.73 90)
		(property "Reference" "REF**"
			(at 4.1 5 -90)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "side-pad-fCu"
			(at 4.1 3.5 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "case-solder-footprints:side-pad-fCu"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(attr smd)
	)
	(footprint "case-solder-footprints:side-pad-fCu"
		(layer "B.Cu")
		(at 288.190001 309.16 180)
		(property "Reference" "REF**"
			(at 4.1 5 0)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "side-pad-fCu"
			(at 4.1 3.5 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "case-solder-footprints:side-pad-fCu"
			(at 0 0 360)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 360)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 360)
			(layer "B.Fab")
			(hide yes)
		)
		(attr smd)
	)
	(footprint "case-solder-footprints:side-pad-fCu"
		(layer "B.Cu")
		(at 256.690001 309.16 180)
		(property "Reference" "REF**"
			(at 4.1 5 0)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "side-pad-fCu"
			(at 4.1 3.5 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "case-solder-footprints:side-pad-fCu"
			(at 0 0 360)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 360)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 360)
			(layer "B.Fab")
			(hide yes)
		)
		(attr smd)
	)
	(footprint "case-solder-footprints:side-pad-fCu"
		(layer "B.Cu")
		(at 246.710001 379.6)
		(property "Reference" "REF**"
			(at 4.1 5 180)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "side-pad-fCu"
			(at 4.1 3.5 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "case-solder-footprints:side-pad-fCu"
			(at 0 0 360)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 360)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 360)
			(layer "B.Fab")
			(hide yes)
		)
		(attr smd)
	)
	(footprint "case-solder-footprints:side-pad-fCu"
		(layer "B.Cu")
		(at 103.350001 357.49 -90)
		(property "Reference" "REF**"
			(at 4.1 5 90)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "side-pad-fCu"
			(at 4.1 3.5 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "case-solder-footprints:side-pad-fCu"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(attr smd)
	)
	(footprint "case-solder-footprints:side-pad-fCu"
		(layer "B.Cu")
		(at 183.190001 309.16 180)
		(property "Reference" "REF**"
			(at 4.1 5 0)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "side-pad-fCu"
			(at 4.1 3.5 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "case-solder-footprints:side-pad-fCu"
			(at 0 0 360)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 360)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 360)
			(layer "B.Fab")
			(hide yes)
		)
		(attr smd)
	)
	(footprint "case-solder-footprints:side-pad-fCu"
		(layer "B.Cu")
		(at 103.350001 367.99 -90)
		(property "Reference" "REF**"
			(at 4.1 5 90)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "side-pad-fCu"
			(at 4.1 3.5 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "case-solder-footprints:side-pad-fCu"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(attr smd)
	)
	(footprint "case-solder-footprints:side-pad-fCu"
		(layer "B.Cu")
		(at 358.050001 341.77 90)
		(property "Reference" "REF**"
			(at 4.1 5 -90)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "side-pad-fCu"
			(at 4.1 3.5 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "case-solder-footprints:side-pad-fCu"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(attr smd)
	)
	(footprint "case-solder-footprints:slot-solder-pad-back"
		(layer "B.Cu")
		(at 215.096665 147.490001 90)
		(property "Reference" "REF**"
			(at 4.1 5 -90)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "slot-solder-pad-back"
			(at 4.1 3.5 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "case-solder-footprints:slot-solder-pad-back"
			(at 0 0 -90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "B.Fab")
			(hide yes)
		)
		(attr smd)
	)
	(footprint "case-solder-footprints:side-pad-fCu"
		(layer "B.Cu")
		(at 162.710001 379.6)
		(property "Reference" "REF**"
			(at 4.1 5 180)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "side-pad-fCu"
			(at 4.1 3.5 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "case-solder-footprints:side-pad-fCu"
			(at 0 0 360)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 360)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 360)
			(layer "B.Fab")
			(hide yes)
		)
		(attr smd)
	)
	(footprint "case-solder-footprints:side-pad-fCu"
		(layer "B.Cu")
		(at 194.210001 379.6)
		(property "Reference" "REF**"
			(at 4.1 5 180)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "side-pad-fCu"
			(at 4.1 3.5 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "case-solder-footprints:side-pad-fCu"
			(at 0 0 360)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 360)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 360)
			(layer "B.Fab")
			(hide yes)
		)
		(attr smd)
	)
	(footprint "case-solder-footprints:side-pad-fCu"
		(layer "B.Cu")
		(at 330.190001 309.16 180)
		(property "Reference" "REF**"
			(at 4.1 5 0)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "side-pad-fCu"
			(at 4.1 3.5 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "case-solder-footprints:side-pad-fCu"
			(at 0 0 360)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 360)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 360)
			(layer "B.Fab")
			(hide yes)
		)
		(attr smd)
	)
	(footprint "case-solder-footprints:side-pad-fCu"
		(layer "B.Cu")
		(at 141.190001 309.16 180)
		(property "Reference" "REF**"
			(at 4.1 5 0)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "side-pad-fCu"
			(at 4.1 3.5 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "case-solder-footprints:side-pad-fCu"
			(at 0 0 360)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 360)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 360)
			(layer "B.Fab")
			(hide yes)
		)
		(attr smd)
	)
	(footprint "case-solder-footprints:side-pad-fCu"
		(layer "B.Cu")
		(at 215.210001 379.6)
		(property "Reference" "REF**"
			(at 4.1 5 180)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "side-pad-fCu"
			(at 4.1 3.5 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "case-solder-footprints:side-pad-fCu"
			(at 0 0 360)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 360)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 360)
			(layer "B.Fab")
			(hide yes)
		)
		(attr smd)
	)
	(footprint "case-solder-footprints:slot-solder-pad-back"
		(layer "B.Cu")
		(at 215.096665 72.290001 90)
		(property "Reference" "REF**"
			(at 4.1 5 -90)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "slot-solder-pad-back"
			(at 4.1 3.5 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "case-solder-footprints:slot-solder-pad-back"
			(at 0 0 -90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "B.Fab")
			(hide yes)
		)
		(attr smd)
	)
	(footprint "case-solder-footprints:side-pad-fCu"
		(layer "B.Cu")
		(at 183.710001 379.6)
		(property "Reference" "REF**"
			(at 4.1 5 180)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "side-pad-fCu"
			(at 4.1 3.5 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "case-solder-footprints:side-pad-fCu"
			(at 0 0 360)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 360)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 360)
			(layer "B.Fab")
			(hide yes)
		)
		(attr smd)
	)
	(footprint "case-solder-footprints:side-pad-fCu"
		(layer "B.Cu")
		(at 152.210001 379.3)
		(property "Reference" "REF**"
			(at 4.1 5 180)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "side-pad-fCu"
			(at 4.1 3.5 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "case-solder-footprints:side-pad-fCu"
			(at 0 0 360)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 360)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 360)
			(layer "B.Fab")
			(hide yes)
		)
		(attr smd)
	)
	(footprint "case-solder-footprints:side-pad-fCu"
		(layer "B.Cu")
		(at 225.190001 309.16 180)
		(property "Reference" "REF**"
			(at 4.1 5 0)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "side-pad-fCu"
			(at 4.1 3.5 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "case-solder-footprints:side-pad-fCu"
			(at 0 0 360)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 360)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 360)
			(layer "B.Fab")
			(hide yes)
		)
		(attr smd)
	)
	(footprint "case-solder-footprints:side-pad-fCu"
		(layer "B.Cu")
		(at 204.190001 309.16 180)
		(property "Reference" "REF**"
			(at 4.1 5 0)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "side-pad-fCu"
			(at 4.1 3.5 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "case-solder-footprints:side-pad-fCu"
			(at 0 0 360)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 360)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 360)
			(layer "B.Fab")
			(hide yes)
		)
		(attr smd)
	)
	(footprint "case-solder-footprints:side-pad-fCu"
		(layer "B.Cu")
		(at 105.52 60.95 180)
		(property "Reference" "REF**"
			(at 4.1 5 0)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "side-pad-fCu"
			(at 4.099999 3.499998 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "case-solder-footprints:side-pad-fCu"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(attr smd)
	)
	(footprint "case-solder-footprints:side-pad-fCu"
		(layer "B.Cu")
		(at 319.690001 309.16 180)
		(property "Reference" "REF**"
			(at 4.1 5 0)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "side-pad-fCu"
			(at 4.1 3.5 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "case-solder-footprints:side-pad-fCu"
			(at 0 0 360)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 360)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 360)
			(layer "B.Fab")
			(hide yes)
		)
		(attr smd)
	)
	(footprint "case-solder-footprints:side-pad-fCu"
		(layer "B.Cu")
		(at 358.050001 331.27 90)
		(property "Reference" "REF**"
			(at 4.1 5 -90)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "side-pad-fCu"
			(at 4.1 3.5 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "case-solder-footprints:side-pad-fCu"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(attr smd)
	)
	(footprint "case-solder-footprints:side-pad-fCu"
		(layer "B.Cu")
		(at 341.210001 379.6)
		(property "Reference" "REF**"
			(at 4.1 5 180)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "side-pad-fCu"
			(at 4.1 3.5 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "case-solder-footprints:side-pad-fCu"
			(at 0 0 360)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 360)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 360)
			(layer "B.Fab")
			(hide yes)
		)
		(attr smd)
	)
	(footprint "case-solder-footprints:slot-solder-pad-back"
		(layer "B.Cu")
		(at 215.096665 222.690001 90)
		(property "Reference" "REF**"
			(at 4.1 5 -90)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "slot-solder-pad-back"
			(at 4.1 3.5 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "case-solder-footprints:slot-solder-pad-back"
			(at 0 0 -90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "B.Fab")
			(hide yes)
		)
		(attr smd)
	)
	(footprint "case-solder-footprints:side-pad-fCu"
		(layer "B.Cu")
		(at 309.190001 309.46 180)
		(property "Reference" "REF**"
			(at 4.1 5 0)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "side-pad-fCu"
			(at 4.1 3.5 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "case-solder-footprints:side-pad-fCu"
			(at 0 0 360)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 360)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 360)
			(layer "B.Fab")
			(hide yes)
		)
		(attr smd)
	)
	(footprint "case-solder-footprints:side-pad-fCu"
		(layer "B.Cu")
		(at 103.350001 331.53 -90)
		(property "Reference" "REF**"
			(at 4.1 5 90)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "side-pad-fCu"
			(at 4.1 3.5 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "case-solder-footprints:side-pad-fCu"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(attr smd)
	)
	(gr_line
		(start 106.48 212.860001)
		(end 106.48 214.860001)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 311.430001 72.15)
		(mid 311.960272 72.369728)
		(end 312.18 72.899999)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 307.4 379.95)
		(end 307.4 381.45)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 230.48 276.81)
		(end 232.48 276.81)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 101.400001 323.11)
		(end 101.400001 321.11)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 294.550001 343.63)
		(end 294.550001 345.13)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 308.400001 308.81)
		(end 308.400001 309.11)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 360.000002 323.11)
		(end 360.000002 321.11)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 51.27 228.76)
		(end 51.27 227.16)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 228.200001 379.95)
		(end 228.200001 379.65)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 227.48 273.2)
		(end 227.48 275.21)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.38 19.79)
		(end 153.38 21.79)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 158.38 276.79)
		(end 156.38 276.79)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 167.840001 345.13)
		(end 167.840001 343.63)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 308.4 379.65)
		(end 307.4 379.65)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 323.19 228.76)
		(end 313.58 228.76)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 259.483335 19.809999)
		(end 259.483335 18.209999)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 233.200001 308.81)
		(end 233.200001 309.11)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 227.48 21.81)
		(end 227.48 83.66)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 105.58 59)
		(end 105.58 60.6)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 358.400002 323.11)
		(end 360.000002 323.11)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 228.200001 379.95)
		(end 159.070001 379.95)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.000001 379.95)
		(end 103 379.95)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 78.576665 59)
		(end 103.38 59)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.000002 308.81)
		(end 103.000001 308.81)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 303.4 379.65)
		(end 303.4 379.95)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 323.19 228.76)
		(end 361.36 228.76)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 303.400001 308.81)
		(end 302.330001 308.81)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 343.483335 59)
		(end 340.583335 59)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 311.429999 215.61)
		(end 311.229999 215.61)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 308.400001 308.81)
		(end 358.400002 308.81)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 105.58 59)
		(end 108.48 59)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 311.38 228.76)
		(end 308.48 228.76)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 158.000001 379.65)
		(end 158.000001 379.95)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 232.200001 381.45)
		(end 232.200001 379.95)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 232.200001 308.81)
		(end 232.200001 307.31)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 229.200001 307.31)
		(end 229.200001 308.81)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 312.18 214.86)
		(mid 311.960359 215.39036)
		(end 311.429999 215.61)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 358.400002 343.63)
		(end 358.400002 323.11)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 304.400001 307.31)
		(end 304.400001 308.81)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 104.78 72.899999)
		(mid 104.999728 72.369728)
		(end 105.529999 72.15)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 210.69 19.79)
		(end 158.38 19.79)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 46.17 228.76)
		(end 49.07 228.76)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 229.200001 309.11)
		(end 228.200001 309.11)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 232.48 19.809999)
		(end 232.48 18.209999)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 103 367.65)
		(end 103 379.95)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 312.18 74.899999)
		(mid 311.960301 75.4303)
		(end 311.43 75.65)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 310.48 212.860001)
		(end 310.48 214.860001)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 359.250001 367.65)
		(end 360.000001 367.65)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 232.200001 379.95)
		(end 232.200001 379.65)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 311.38 59)
		(end 308.48 59)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 213.74 149.14)
		(end 213.74 145.84)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 340.583335 59)
		(end 340.583335 60.6)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 304.4 381.45)
		(end 304.4 379.95)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.000002 307.31)
		(end 157.000002 308.81)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 212.69 275.19)
		(end 212.69 276.79)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 303.400001 309.11)
		(end 303.400001 308.81)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 103.000001 343.63)
		(end 103.000001 345.13)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 365.69 228.76)
		(end 365.69 227.16)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 313.58 60.6)
		(end 311.38 60.6)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 307.4 379.65)
		(end 307.4 379.95)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 103.38 228.76)
		(end 103.38 227.16)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 308.4 379.95)
		(end 358.400001 379.95)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 259.483335 275.21)
		(end 262.483335 275.21)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 229.200001 379.65)
		(end 229.200001 379.95)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.000001 379.95)
		(end 157.000001 379.65)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.000001 379.65)
		(end 158.000001 379.65)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 156.38 276.79)
		(end 156.38 275.19)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.000002 308.81)
		(end 157.000002 309.11)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 230.48 18.209999)
		(end 232.48 18.209999)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 259.483335 19.809999)
		(end 262.483335 19.809999)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 231.700001 345.13)
		(end 231.700001 343.63)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 165.840001 343.63)
		(end 105.010001 343.63)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 356.400001 343.63)
		(end 294.550001 343.63)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 211.94 145.84)
		(end 211.94 149.14)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 358.400001 365.65)
		(end 358.400001 345.13)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.000002 308.81)
		(end 153.000002 309.11)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 165.840001 345.13)
		(end 105.010001 345.13)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.000001 381.45)
		(end 157.000001 379.95)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 154.000002 307.31)
		(end 157.000002 307.31)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.38 21.79)
		(end 153.38 83.64)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 213.74 70.64)
		(end 211.94 70.64)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 105.010001 345.13)
		(end 105.010001 343.63)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 340.583335 60.6)
		(end 338.383335 60.6)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 211.94 73.94)
		(end 213.74 73.94)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 103 365.65)
		(end 101.4 365.65)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 356.400001 345.13)
		(end 294.550001 345.13)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 311.38 59)
		(end 311.38 60.6)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 212.69 275.19)
		(end 215.69 275.19)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 213.74 73.94)
		(end 213.74 70.64)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 233.200001 379.95)
		(end 303.4 379.95)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 213.74 224.34)
		(end 213.74 221.04)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.000002 309.11)
		(end 154.000002 309.11)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 311.38 228.76)
		(end 311.38 227.16)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 105.73 75.649999)
		(end 105.53 75.65)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 360.000001 365.65)
		(end 358.400001 365.65)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 154.000001 381.45)
		(end 157.000001 381.45)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 212.69 19.79)
		(end 212.69 18.19)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 105.53 75.65)
		(mid 104.999699 75.4303)
		(end 104.78 74.899999)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 227.48 85.66)
		(end 227.48 83.66)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 211.94 224.34)
		(end 213.74 224.34)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 308.48 59)
		(end 308.48 228.76)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 311.230001 72.15)
		(end 311.430001 72.15)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 311.23 75.649999)
		(end 311.43 75.65)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 370.79 228.76)
		(end 367.89 228.76)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 154.000001 379.95)
		(end 154.000001 381.45)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 359.250001 367.65)
		(end 358.400001 367.65)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 105.73 212.11)
		(mid 106.260301 212.3297)
		(end 106.48 212.860001)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 361.36 228.76)
		(end 365.69 228.76)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 104.78 214.86)
		(end 104.78 212.86)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 313.58 227.16)
		(end 311.38 227.16)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 101.400001 321.11)
		(end 103.000001 321.11)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.000002 309.11)
		(end 158.000002 309.11)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 105.530001 215.61)
		(end 105.730001 215.61)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 232.48 275.21)
		(end 232.48 276.81)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 307.400001 308.81)
		(end 307.400001 307.31)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 211.94 70.64)
		(end 211.94 73.94)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.38 210.35)
		(end 153.38 212.35)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 211.94 221.04)
		(end 211.94 224.34)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 307.4 381.45)
		(end 304.4 381.45)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 262.483335 275.21)
		(end 262.483335 19.809999)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 105.729999 72.15)
		(mid 106.260359 72.36964)
		(end 106.48 72.9)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 229.700001 345.13)
		(end 167.840001 345.13)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 154.000001 379.65)
		(end 154.000001 379.95)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 93.77 228.76)
		(end 103.38 228.76)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 228.200001 379.65)
		(end 229.200001 379.65)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 105.729999 72.15)
		(end 105.529999 72.15)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 233.200001 379.65)
		(end 233.200001 379.95)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 307.400001 309.11)
		(end 307.400001 308.81)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 156.38 18.19)
		(end 156.38 19.79)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 360.000002 321.11)
		(end 358.400002 321.11)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 76.376665 60.6)
		(end 78.576665 60.6)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 103.000001 323.11)
		(end 101.400001 323.11)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 210.69 19.79)
		(end 210.69 18.19)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 307.400001 307.31)
		(end 304.400001 307.31)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.000001 379.95)
		(end 153.000001 379.65)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 105.53 212.110001)
		(end 105.73 212.11)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 227.48 21.81)
		(end 227.48 19.809999)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 156.38 19.79)
		(end 153.38 19.79)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 158.38 18.19)
		(end 156.38 18.19)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 103.000001 308.81)
		(end 103.000001 321.11)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 103.38 227.16)
		(end 105.58 227.16)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 312.18 74.899999)
		(end 312.18 72.899999)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 233.200001 309.11)
		(end 232.200001 309.11)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 106.48 74.9)
		(mid 106.260301 75.430301)
		(end 105.73 75.65)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 310.48 212.860001)
		(mid 310.699699 212.3297)
		(end 311.23 212.11)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 105.58 228.76)
		(end 108.48 228.76)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 158.38 275.19)
		(end 158.38 276.79)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.38 212.35)
		(end 153.38 273.18)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 311.23 75.65)
		(mid 310.699699 75.430301)
		(end 310.48 74.9)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 103.000001 323.11)
		(end 103.000001 343.63)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 310.48 72.9)
		(end 310.48 74.9)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 212.69 19.79)
		(end 215.69 19.79)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 310.48 72.9)
		(mid 310.699641 72.36964)
		(end 311.230001 72.15)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 313.58 228.76)
		(end 313.58 227.16)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 227.48 85.66)
		(end 227.48 146.51)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 304.400001 309.11)
		(end 303.400001 309.11)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 158.000001 379.95)
		(end 159.070001 379.95)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 311.229999 215.61)
		(mid 310.699728 215.390272)
		(end 310.48 214.860001)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 105.530001 215.61)
		(mid 104.999641 215.39036)
		(end 104.78 214.86)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.38 85.64)
		(end 153.38 146.49)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 356.400001 345.13)
		(end 356.400001 343.63)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 232.200001 307.31)
		(end 229.200001 307.31)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 210.69 275.19)
		(end 210.69 276.79)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 78.576665 59)
		(end 78.576665 60.6)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 360.000001 365.65)
		(end 360.000001 367.65)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 108.48 59)
		(end 108.48 228.76)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 229.700001 345.13)
		(end 229.700001 343.63)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 257.483335 276.81)
		(end 259.483335 276.81)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 230.48 19.809999)
		(end 230.48 18.209999)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 210.69 18.19)
		(end 212.69 18.19)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 227.48 148.51)
		(end 227.48 210.37)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 213.74 145.84)
		(end 211.94 145.84)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 311.43 212.11)
		(mid 311.960301 212.329699)
		(end 312.18 212.86)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 358.400002 343.63)
		(end 358.400002 345.13)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 232.200001 309.11)
		(end 232.200001 308.81)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.000001 379.65)
		(end 154.000001 379.65)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 104.78 212.86)
		(mid 104.999699 212.329699)
		(end 105.53 212.11)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 257.483335 19.809999)
		(end 257.483335 18.209999)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 156.38 275.19)
		(end 153.38 275.19)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 228.200001 308.81)
		(end 158.000002 308.81)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.38 146.49)
		(end 153.38 148.49)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 338.383335 59)
		(end 313.58 59)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 104.78 74.899999)
		(end 104.78 72.899999)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 228.200001 309.11)
		(end 228.200001 308.81)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 227.48 19.809999)
		(end 230.48 19.809999)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 229.200001 308.81)
		(end 229.200001 309.11)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 213.74 221.04)
		(end 211.94 221.04)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 158.38 19.79)
		(end 158.38 18.19)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.38 273.18)
		(end 153.38 275.19)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 227.48 275.21)
		(end 230.48 275.21)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 304.4 379.65)
		(end 303.4 379.65)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 232.200001 379.65)
		(end 233.200001 379.65)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 227.48 212.37)
		(end 227.48 273.2)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 76.376665 59)
		(end 76.376665 60.6)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 304.400001 308.81)
		(end 304.400001 309.11)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 106.48 214.860001)
		(mid 106.260272 215.390272)
		(end 105.730001 215.61)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 101.4 365.65)
		(end 101.4 367.65)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 229.200001 381.45)
		(end 232.200001 381.45)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 233.200001 308.81)
		(end 302.330001 308.81)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 292.550001 345.13)
		(end 292.550001 343.63)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 232.48 19.809999)
		(end 257.483335 19.809999)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 365.69 227.16)
		(end 367.89 227.16)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 358.400001 379.95)
		(end 358.400001 367.65)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 259.483335 275.21)
		(end 259.483335 276.81)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 103.38 60.6)
		(end 105.58 60.6)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 215.69 275.190001)
		(end 215.69 19.79)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 49.07 227.16)
		(end 49.07 228.76)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 308.4 379.95)
		(end 308.4 379.65)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 304.4 379.95)
		(end 304.4 379.65)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.38 148.49)
		(end 153.38 210.35)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 55.6 228.76)
		(end 51.27 228.76)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 103 345.13)
		(end 103 365.65)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 73.476665 59)
		(end 76.376665 59)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 103.38 59)
		(end 103.38 60.6)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 257.483335 18.209999)
		(end 259.483335 18.209999)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 358.400002 321.11)
		(end 358.400002 308.81)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 338.383335 59)
		(end 338.383335 60.6)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 292.550001 345.13)
		(end 231.700001 345.13)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 313.58 59)
		(end 313.58 60.6)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 101.4 367.65)
		(end 103 367.65)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 211.94 149.14)
		(end 213.74 149.14)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 308.400001 309.11)
		(end 307.400001 309.11)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 232.48 275.21)
		(end 257.483335 275.21)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 105.58 228.76)
		(end 105.58 227.16)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 229.200001 379.95)
		(end 229.200001 381.45)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 154.000002 308.81)
		(end 154.000002 307.31)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 93.77 228.76)
		(end 55.6 228.76)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 73.476665 59)
		(end 46.17 228.76)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 311.43 212.110001)
		(end 311.23 212.11)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 154.000002 309.11)
		(end 154.000002 308.81)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 229.700001 343.63)
		(end 167.840001 343.63)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 210.69 275.19)
		(end 158.38 275.19)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 227.48 148.51)
		(end 227.48 146.51)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 165.840001 345.13)
		(end 165.840001 343.63)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 106.48 72.9)
		(end 106.48 74.9)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.38 83.64)
		(end 153.38 85.64)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 158.000002 309.11)
		(end 158.000002 308.81)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 312.18 214.86)
		(end 312.18 212.86)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 210.69 276.79)
		(end 212.69 276.79)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 257.483335 275.21)
		(end 257.483335 276.81)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 230.48 275.21)
		(end 230.48 276.81)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 343.483335 59)
		(end 370.79 228.76)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 367.89 227.16)
		(end 367.89 228.76)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 292.550001 343.63)
		(end 231.700001 343.63)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 227.48 212.37)
		(end 227.48 210.37)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 51.27 227.16)
		(end 49.07 227.16)
		(layer "Edge.Cuts")
	)
	(gr_text "CLICK-IN REMOVABLE BACK PANEL \nBOTTOM STRIP\nINNER SIDE"
		(at 320.380001 369.38 180)
		(layer "B.SilkS")
	)
	(gr_text "CLICK-IN REMOVABLE BACK PANEL \nTOP STRIP\nINNER SIDE"
		(at 321.030001 319.4 180)
		(layer "B.SilkS")
	)
	(gr_text "BOTTOM PANEL\nINSIDE\nFRONT"
		(at 163.51 37.77 90)
		(layer "F.SilkS")
	)
	(gr_text "TOP PANEL\nINSIDE\nFRONT"
		(at 237.49 33.55 90)
		(layer "F.SilkS")
	)
	(gr_text "1.34mm"
		(at 73.568332 57.680457 0)
		(layer "Cmts.User")
	)
	(gr_text "1.34mm"
		(at 343.391668 57.680457 0)
		(layer "Cmts.User")
	)
)
