(kicad_pcb
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(31 "B.Cu" signal)
		(32 "B.Adhes" user "B.Adhesive")
		(33 "F.Adhes" user "F.Adhesive")
		(34 "B.Paste" user)
		(35 "F.Paste" user)
		(36 "B.SilkS" user "B.Silkscreen")
		(37 "F.SilkS" user "F.Silkscreen")
		(38 "B.Mask" user)
		(39 "F.Mask" user)
		(40 "Dwgs.User" user "User.Drawings")
		(41 "Cmts.User" user "User.Comments")
		(42 "Eco1.User" user "User.Eco1")
		(43 "Eco2.User" user "User.Eco2")
		(44 "Edge.Cuts" user)
		(45 "Margin" user)
		(46 "B.CrtYd" user "B.Courtyard")
		(47 "F.CrtYd" user "F.Courtyard")
		(48 "B.Fab" user)
		(49 "F.Fab" user)
		(50 "User.1" user)
		(51 "User.2" user)
		(52 "User.3" user)
		(53 "User.4" user)
		(54 "User.5" user)
		(55 "User.6" user)
		(56 "User.7" user)
		(57 "User.8" user)
		(58 "User.9" user)
	)
	(setup
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(pcbplotparams
			(layerselection 0x00010fc_ffffffff)
			(plot_on_all_layers_selection 0x0000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(viasonmask no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plotreference yes)
			(plotvalue yes)
			(plotfptext yes)
			(plotinvisibletext no)
			(sketchpadsonfab no)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 1)
			(scaleselection 1)
			(outputdirectory "")
		)
	)
	(net 0 "")
	(net 1 "GND")
	(net 2 "SCL")
	(net 3 "VDD")
	(net 4 "SDA")
	(net 5 "Net-(J6-Pin_2)")
	(net 6 "Net-(JP3-A)")
	(net 7 "UPDI")
	(net 8 "Net-(J7-Pin_2)")
	(net 9 "Net-(Q1-B)")
	(net 10 "Net-(Q1-C)")
	(net 11 "unconnected-(U1-PA4-Pad2)")
	(net 12 "Net-(Q2-C)")
	(net 13 "unconnected-(U1-PA1-Pad31)")
	(net 14 "unconnected-(U1-VREFA{slash}PD7-Pad17)")
	(net 15 "unconnected-(U1-PA0-Pad30)")
	(net 16 "Net-(Q2-B)")
	(net 17 "Net-(Q3-B)")
	(net 18 "Net-(Q3-C)")
	(net 19 "Net-(Q4-B)")
	(net 20 "Net-(Q4-C)")
	(net 21 "Net-(U2-B2)")
	(net 22 "Net-(U2-B1)")
	(net 23 "Net-(U3-B2)")
	(net 24 "Net-(U3-B1)")
	(net 25 "Net-(U4-B2)")
	(net 26 "Net-(U4-B1)")
	(net 27 "Net-(U5-B2)")
	(net 28 "Net-(U5-B1)")
	(net 29 "Net-(U1-~{RESET}{slash}PF6)")
	(net 30 "unconnected-(U1-XTAL32K1{slash}PF0-Pad20)")
	(net 31 "unconnected-(U1-XTAL32K2{slash}PF1-Pad21)")
	(net 32 "/Power_out_1/Power")
	(net 33 "/Power_out_1/Shunt")
	(net 34 "/S1")
	(net 35 "/S2")
	(net 36 "/S3")
	(net 37 "/S4")
	(net 38 "Net-(JP6-A)")
	(net 39 "Net-(JP5-A)")
	(net 40 "Net-(J2-Pin_2)")
	(net 41 "/H1")
	(net 42 "Net-(J1-Pin_2)")
	(net 43 "/L1")
	(net 44 "/H2")
	(net 45 "/L2")
	(net 46 "/H3")
	(net 47 "/L3")
	(net 48 "/H4")
	(net 49 "/L4")
	(net 50 "unconnected-(U1-PF5-Pad25)")
	(net 51 "Net-(JP4-A)")
	(net 52 "unconnected-(U6B-+-Pad5)")
	(net 53 "unconnected-(U6B---Pad6)")
	(net 54 "unconnected-(U6-Pad7)")
	(net 55 "/OPAMP")
	(net 56 "Net-(U6A--)")
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(at 213.75 119.75)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R13"
			(at 3.25 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "4k7"
			(at 0 1.65 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Power_out_3")
		(sheetfile "PWR.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.208333)
			(net 47 "/L3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.208333)
			(net 26 "Net-(U4-B1)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_QFP:TQFP-32_7x7mm_P0.8mm"
		(layer "F.Cu")
		(at 201 126.5 135)
		(descr "32-Lead Plastic Thin Quad Flatpack (PT) - 7x7x1.0 mm Body, 2.00 mm [TQFP] (see Microchip Packaging Specification 00000049BS.pdf)")
		(tags "QFP 0.8")
		(property "Reference" "U1"
			(at -4.419417 -4.772971 135)
			(layer "F.SilkS")
		)
		(property "Value" "AVR16EA32T-I/PT"
			(at 0 6.05 135)
			(layer "F.Fab")
		)
		(property "Footprint" "Package_QFP:TQFP-32_7x7mm_P0.8mm"
			(at 0 0 135)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/AVR128DA28-32-48-64-DataSheet-DS40002183B.pdf"
			(at 0 0 135)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "24MHz, 128kB Flash, 16kB SRAM, EEPROM with Touch Sensing, TQFP-32"
			(at 0 0 135)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TQFP*7x7mm*P0.8mm*")
		(sheetname "Root")
		(sheetfile "PWM_Module.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 135)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -4.25 -2.8 135)
			(size 1.6 0.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "SCL")
			(pinfunction "PA3")
			(pintype "bidirectional")
		)
		(pad "2" smd rect
			(at -4.25 -2 135)
			(size 1.6 0.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 11 "unconnected-(U1-PA4-Pad2)")
			(pinfunction "PA4")
			(pintype "bidirectional")
		)
		(pad "3" smd rect
			(at -4.25 -1.2 135)
			(size 1.6 0.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 6 "Net-(JP3-A)")
			(pinfunction "PA5")
			(pintype "bidirectional")
		)
		(pad "4" smd rect
			(at -4.25 -0.4 135)
			(size 1.6 0.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 51 "Net-(JP4-A)")
			(pinfunction "PA6")
			(pintype "bidirectional")
		)
		(pad "5" smd rect
			(at -4.25 0.4 135)
			(size 1.6 0.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 39 "Net-(JP5-A)")
			(pinfunction "PA7")
			(pintype "bidirectional")
		)
		(pad "6" smd rect
			(at -4.25 1.2 135)
			(size 1.6 0.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 38 "Net-(JP6-A)")
			(pinfunction "PC0")
			(pintype "bidirectional")
		)
		(pad "7" smd rect
			(at -4.25 2 135)
			(size 1.6 0.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 55 "/OPAMP")
			(pinfunction "PC1")
			(pintype "bidirectional")
		)
		(pad "8" smd rect
			(at -4.25 2.8 135)
			(size 1.6 0.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 41 "/H1")
			(pinfunction "PC2")
			(pintype "bidirectional")
		)
		(pad "9" smd rect
			(at -2.8 4.25 225)
			(size 1.6 0.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 43 "/L1")
			(pinfunction "PC3")
			(pintype "bidirectional")
		)
		(pad "10" smd rect
			(at -2 4.25 225)
			(size 1.6 0.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 34 "/S1")
			(pinfunction "PD0")
			(pintype "bidirectional")
		)
		(pad "11" smd rect
			(at -1.2 4.25 225)
			(size 1.6 0.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 44 "/H2")
			(pinfunction "PD1")
			(pintype "bidirectional")
		)
		(pad "12" smd rect
			(at -0.4 4.25 225)
			(size 1.6 0.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 45 "/L2")
			(pinfunction "PD2")
			(pintype "bidirectional")
		)
		(pad "13" smd rect
			(at 0.4 4.25 225)
			(size 1.6 0.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 35 "/S2")
			(pinfunction "PD3")
			(pintype "bidirectional")
		)
		(pad "14" smd rect
			(at 1.2 4.25 225)
			(size 1.6 0.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 46 "/H3")
			(pinfunction "PD4")
			(pintype "bidirectional")
		)
		(pad "15" smd rect
			(at 2 4.25 225)
			(size 1.6 0.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 47 "/L3")
			(pinfunction "PD5")
			(pintype "bidirectional")
		)
		(pad "16" smd rect
			(at 2.8 4.25 225)
			(size 1.6 0.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 36 "/S3")
			(pinfunction "PD6")
			(pintype "bidirectional")
		)
		(pad "17" smd rect
			(at 4.25 2.8 135)
			(size 1.6 0.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 14 "unconnected-(U1-VREFA{slash}PD7-Pad17)")
			(pinfunction "VREFA/PD7")
			(pintype "bidirectional")
		)
		(pad "18" smd rect
			(at 4.25 2 135)
			(size 1.6 0.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 3 "VDD")
			(pinfunction "AVDD")
			(pintype "power_in")
		)
		(pad "19" smd rect
			(at 4.25 1.2 135)
			(size 1.6 0.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "20" smd rect
			(at 4.25 0.4 135)
			(size 1.6 0.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 30 "unconnected-(U1-XTAL32K1{slash}PF0-Pad20)")
			(pinfunction "XTAL32K1/PF0")
			(pintype "bidirectional")
		)
		(pad "21" smd rect
			(at 4.25 -0.4 135)
			(size 1.6 0.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 31 "unconnected-(U1-XTAL32K2{slash}PF1-Pad21)")
			(pinfunction "XTAL32K2/PF1")
			(pintype "bidirectional")
		)
		(pad "22" smd rect
			(at 4.25 -1.2 135)
			(size 1.6 0.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 49 "/L4")
			(pinfunction "PF2")
			(pintype "bidirectional")
		)
		(pad "23" smd rect
			(at 4.25 -2 135)
			(size 1.6 0.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 48 "/H4")
			(pinfunction "PF3")
			(pintype "bidirectional")
		)
		(pad "24" smd rect
			(at 4.25 -2.8 135)
			(size 1.6 0.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 37 "/S4")
			(pinfunction "PF4")
			(pintype "bidirectional")
		)
		(pad "25" smd rect
			(at 2.8 -4.25 225)
			(size 1.6 0.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 50 "unconnected-(U1-PF5-Pad25)")
			(pinfunction "PF5")
			(pintype "bidirectional")
		)
		(pad "26" smd rect
			(at 2 -4.25 225)
			(size 1.6 0.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 29 "Net-(U1-~{RESET}{slash}PF6)")
			(pinfunction "~{RESET}/PF6")
			(pintype "bidirectional")
		)
		(pad "27" smd rect
			(at 1.2 -4.25 225)
			(size 1.6 0.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 7 "UPDI")
			(pinfunction "UPDI")
			(pintype "input")
		)
		(pad "28" smd rect
			(at 0.4 -4.25 225)
			(size 1.6 0.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 3 "VDD")
			(pinfunction "VDD")
			(pintype "power_in")
		)
		(pad "29" smd rect
			(at -0.4 -4.25 225)
			(size 1.6 0.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "30" smd rect
			(at -1.2 -4.25 225)
			(size 1.6 0.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 15 "unconnected-(U1-PA0-Pad30)")
			(pinfunction "PA0")
			(pintype "bidirectional")
		)
		(pad "31" smd rect
			(at -2 -4.25 225)
			(size 1.6 0.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 13 "unconnected-(U1-PA1-Pad31)")
			(pinfunction "PA1")
			(pintype "bidirectional")
		)
		(pad "32" smd rect
			(at -2.8 -4.25 225)
			(size 1.6 0.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 4 "SDA")
			(pinfunction "PA2")
			(pintype "bidirectional")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_QFP.3dshapes/TQFP-32_7x7mm_P0.8mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_JST:JST_XA_S03B-XASK-1_1x03_P2.50mm_Horizontal"
		(layer "F.Cu")
		(at 238.5 103.9 180)
		(descr "JST XA series connector, S03B-XASK-1 (http://www.jst-mfg.com/product/pdf/eng/eXA1.pdf), generated with kicad-footprint-generator")
		(tags "connector JST XA horizontal hook")
		(property "Reference" "J1"
			(at -0.25 -2.35 0)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x03"
			(at 2.5 10.4 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_JST:JST_XA_S03B-XASK-1_1x03_P2.50mm_Horizontal"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x03, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "Power_out_1")
		(sheetfile "PWR.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.5 2.5 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole oval
			(at 2.5 6.5 180)
			(size 2.8 2)
			(drill oval 2.8 2)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" thru_hole roundrect
			(at 0 0 180)
			(size 1.7 1.95)
			(drill 0.95)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.147059)
			(net 33 "/Power_out_1/Shunt")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 2.5 0 180)
			(size 1.7 1.95)
			(drill 0.95)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 42 "Net-(J1-Pin_2)")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 5 0 180)
			(size 1.7 1.95)
			(drill 0.95)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 34 "/S1")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_JST.3dshapes/JST_XA_S03B-XASK-1_1x03_P2.50mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(at 211.25 114 180)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R11"
			(at 0 -1.65 180)
			(layer "F.SilkS")
		)
		(property "Value" "4k7"
			(at 0 1.65 180)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Power_out_3")
		(sheetfile "PWR.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1 0 180)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.208333)
			(net 18 "Net-(Q3-C)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1 0 180)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.208333)
			(net 25 "Net-(U4-B2)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Library:PowerDI5060"
		(layer "F.Cu")
		(at 236 111)
		(property "Reference" "U2"
			(at -1.75 -3.75 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "DXTC3C100PDQ-13"
			(at -4.675 0 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" "Library:PowerDI5060"
			(at -1.905 3.175 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at -1.905 3.175 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at -1.905 3.175 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Power_out_1")
		(sheetfile "PWR.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at -3.175 0 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.905 3.175)
			(size 0.61 1.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 33 "/Power_out_1/Shunt")
			(pinfunction "E1")
			(pintype "unspecified")
			(thermal_bridge_angle 45)
		)
		(pad "2" smd roundrect
			(at -0.635 3.175)
			(size 0.61 1.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 22 "Net-(U2-B1)")
			(pinfunction "B1")
			(pintype "unspecified")
			(thermal_bridge_angle 45)
		)
		(pad "3" smd roundrect
			(at 0.635 3.175)
			(size 0.61 1.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 32 "/Power_out_1/Power")
			(pinfunction "E2")
			(pintype "unspecified")
			(thermal_bridge_angle 45)
		)
		(pad "4" smd roundrect
			(at 1.905 3.175)
			(size 0.61 1.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 21 "Net-(U2-B2)")
			(pinfunction "B2")
			(pintype "unspecified")
			(thermal_bridge_angle 45)
		)
		(pad "5" smd roundrect
			(at 1.905 -2.29)
			(size 0.61 1.02)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 42 "Net-(J1-Pin_2)")
			(pinfunction "C2")
			(pintype "unspecified")
			(thermal_bridge_angle 45)
		)
		(pad "6" smd roundrect
			(at 0.635 -2.29)
			(size 0.61 1.02)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 42 "Net-(J1-Pin_2)")
			(pinfunction "C2")
			(pintype "unspecified")
			(thermal_bridge_angle 45)
		)
		(pad "6" smd roundrect
			(at 1.27 -0.1524 90)
			(size 3.783 1.82)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.1)
			(net 42 "Net-(J1-Pin_2)")
			(pinfunction "C2")
			(pintype "unspecified")
			(thermal_bridge_angle 45)
		)
		(pad "7" smd roundrect
			(at -1.27 -0.1524 90)
			(size 3.783 1.82)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.1)
			(net 42 "Net-(J1-Pin_2)")
			(pinfunction "C1")
			(pintype "unspecified")
			(thermal_bridge_angle 45)
		)
		(pad "7" smd roundrect
			(at -0.635 -2.29)
			(size 0.61 1.02)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 42 "Net-(J1-Pin_2)")
			(pinfunction "C1")
			(pintype "unspecified")
			(thermal_bridge_angle 45)
		)
		(pad "8" smd roundrect
			(at -1.905 -2.29)
			(size 0.61 1.02)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 42 "Net-(J1-Pin_2)")
			(pinfunction "C1")
			(pintype "unspecified")
			(thermal_bridge_angle 45)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(at 223 127.25 -90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R20"
			(at 0 -1.65 90)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 0 1.65 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "PWM_Module.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1 0 270)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.208333)
			(net 56 "Net-(U6A--)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1 0 270)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.208333)
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_JST:JST_PH_S4B-PH-SM4-TB_1x04-1MP_P2.00mm_Horizontal"
		(layer "F.Cu")
		(at 192.25 142.6)
		(descr "JST PH series connector, S4B-PH-SM4-TB (http://www.jst-mfg.com/product/pdf/eng/ePH.pdf), generated with kicad-footprint-generator")
		(tags "connector JST PH horizontal")
		(property "Reference" "J3"
			(at 1.75 0.25 0)
			(layer "F.SilkS")
		)
		(property "Value" "TWI 01"
			(at 0 5.8 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_JST:JST_PH_S4B-PH-SM4-TB_1x04-1MP_P2.00mm_Horizontal"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x04, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "Root")
		(sheetfile "PWM_Module.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 1.5 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -3 -2.85)
			(size 1 3.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 3 "VDD")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at -1 -2.85)
			(size 1 3.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at 1 -2.85)
			(size 1 3.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "SDA")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" smd roundrect
			(at 3 -2.85)
			(size 1 3.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "SCL")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "MP" smd roundrect
			(at -5.35 2.9)
			(size 1.5 3.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.166667)
		)
		(pad "MP" smd roundrect
			(at 5.35 2.9)
			(size 1.5 3.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.166667)
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_JST.3dshapes/JST_PH_S4B-PH-SM4-TB_1x04-1MP_P2.00mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_JST:JST_XA_S02B-XASK-1_1x02_P2.50mm_Horizontal"
		(layer "F.Cu")
		(at 234.75 138.1)
		(descr "JST XA series connector, S02B-XASK-1 (http://www.jst-mfg.com/product/pdf/eng/eXA1.pdf), generated with kicad-footprint-generator")
		(tags "connector JST XA horizontal hook")
		(property "Reference" "J8"
			(at 1.25 -4.6 0)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x02"
			(at 1.25 10.4 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_JST:JST_XA_S02B-XASK-1_1x02_P2.50mm_Horizontal"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "Root")
		(sheetfile "PWM_Module.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.25 2.5 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole oval
			(at 1.25 6.5)
			(size 2.8 2)
			(drill oval 2.8 2)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" thru_hole roundrect
			(at 0 0)
			(size 1.7 1.95)
			(drill 0.95)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.147059)
			(net 32 "/Power_out_1/Power")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 2.5 0)
			(size 1.7 1.95)
			(drill 0.95)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_JST.3dshapes/JST_XA_S02B-XASK-1_1x02_P2.50mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_JST:JST_PH_S4B-PH-SM4-TB_1x04-1MP_P2.00mm_Horizontal"
		(layer "F.Cu")
		(at 209.75 142.6)
		(descr "JST PH series connector, S4B-PH-SM4-TB (http://www.jst-mfg.com/product/pdf/eng/ePH.pdf), generated with kicad-footprint-generator")
		(tags "connector JST PH horizontal")
		(property "Reference" "J4"
			(at 1.25 0.25 0)
			(layer "F.SilkS")
		)
		(property "Value" "TWI 02"
			(at 0 5.8 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_JST:JST_PH_S4B-PH-SM4-TB_1x04-1MP_P2.00mm_Horizontal"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x04, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "Root")
		(sheetfile "PWM_Module.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 1.5 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -3 -2.85)
			(size 1 3.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 3 "VDD")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at -1 -2.85)
			(size 1 3.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at 1 -2.85)
			(size 1 3.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "SDA")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" smd roundrect
			(at 3 -2.85)
			(size 1 3.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "SCL")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "MP" smd roundrect
			(at -5.35 2.9)
			(size 1.5 3.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.166667)
		)
		(pad "MP" smd roundrect
			(at 5.35 2.9)
			(size 1.5 3.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.166667)
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_JST.3dshapes/JST_PH_S4B-PH-SM4-TB_1x04-1MP_P2.00mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Library:PowerDI5060"
		(layer "F.Cu")
		(at 206 111)
		(property "Reference" "U4"
			(at -1.75 -3.75 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "DXTC3C100PDQ-13"
			(at -4.675 0 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" "Library:PowerDI5060"
			(at -1.905 3.175 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at -1.905 3.175 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at -1.905 3.175 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Power_out_3")
		(sheetfile "PWR.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at -3.175 0 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.905 3.175)
			(size 0.61 1.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 33 "/Power_out_1/Shunt")
			(pinfunction "E1")
			(pintype "unspecified")
			(thermal_bridge_angle 45)
		)
		(pad "2" smd roundrect
			(at -0.635 3.175)
			(size 0.61 1.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 26 "Net-(U4-B1)")
			(pinfunction "B1")
			(pintype "unspecified")
			(thermal_bridge_angle 45)
		)
		(pad "3" smd roundrect
			(at 0.635 3.175)
			(size 0.61 1.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 32 "/Power_out_1/Power")
			(pinfunction "E2")
			(pintype "unspecified")
			(thermal_bridge_angle 45)
		)
		(pad "4" smd roundrect
			(at 1.905 3.175)
			(size 0.61 1.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 25 "Net-(U4-B2)")
			(pinfunction "B2")
			(pintype "unspecified")
			(thermal_bridge_angle 45)
		)
		(pad "5" smd roundrect
			(at 1.905 -2.29)
			(size 0.61 1.02)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 5 "Net-(J6-Pin_2)")
			(pinfunction "C2")
			(pintype "unspecified")
			(thermal_bridge_angle 45)
		)
		(pad "6" smd roundrect
			(at 0.635 -2.29)
			(size 0.61 1.02)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 5 "Net-(J6-Pin_2)")
			(pinfunction "C2")
			(pintype "unspecified")
			(thermal_bridge_angle 45)
		)
		(pad "6" smd roundrect
			(at 1.27 -0.1524 90)
			(size 3.783 1.82)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.1)
			(net 5 "Net-(J6-Pin_2)")
			(pinfunction "C2")
			(pintype "unspecified")
			(thermal_bridge_angle 45)
		)
		(pad "7" smd roundrect
			(at -1.27 -0.1524 90)
			(size 3.783 1.82)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.1)
			(net 5 "Net-(J6-Pin_2)")
			(pinfunction "C1")
			(pintype "unspecified")
			(thermal_bridge_angle 45)
		)
		(pad "7" smd roundrect
			(at -0.635 -2.29)
			(size 0.61 1.02)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 5 "Net-(J6-Pin_2)")
			(pinfunction "C1")
			(pintype "unspecified")
			(thermal_bridge_angle 45)
		)
		(pad "8" smd roundrect
			(at -1.905 -2.29)
			(size 0.61 1.02)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 5 "Net-(J6-Pin_2)")
			(pinfunction "C1")
			(pintype "unspecified")
			(thermal_bridge_angle 45)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(at 191.5 132)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C4"
			(at -3 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "4.7u"
			(at 0 1.68 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "PWM_Module.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.212766)
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.212766)
			(net 3 "VDD")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(at 189.5 117.75 90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R16"
			(at 0 1.75 90)
			(layer "F.SilkS")
		)
		(property "Value" "4k7"
			(at 0 1.65 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Power_out_4")
		(sheetfile "PWR.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1 0 90)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.208333)
			(net 49 "/L4")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1 0 90)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.208333)
			(net 28 "Net-(U5-B1)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
		(layer "F.Cu")
		(at 229.25 124)
		(descr "SOIC, 8 Pin (JEDEC MS-012AA, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_8.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOIC SO")
		(property "Reference" "U6"
			(at -2.75 -3.4 0)
			(layer "F.SilkS")
		)
		(property "Value" "LM358"
			(at 0 3.4 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm2904-n.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Low-Power, Dual Operational Amplifiers, DIP-8/SOIC-8/TO-99-8"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm* TO*99* OnSemi*Micro8* TSSOP*3x3mm*P0.65mm* TSSOP*4.4x3mm*P0.65mm* MSOP*3x3mm*P0.65mm* SSOP*3.9x4.9mm*P0.635mm* LFCSP*2x2mm*P0.5mm* *SIP* SOIC*5.3x6.2mm*P1.27mm*")
		(sheetname "Root")
		(sheetfile "PWM_Module.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.475 -1.905)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 55 "/OPAMP")
			(pintype "output")
		)
		(pad "2" smd roundrect
			(at -2.475 -0.635)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 56 "Net-(U6A--)")
			(pinfunction "-")
			(pintype "input")
		)
		(pad "3" smd roundrect
			(at -2.475 0.635)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 33 "/Power_out_1/Shunt")
			(pinfunction "+")
			(pintype "input")
		)
		(pad "4" smd roundrect
			(at -2.475 1.905)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "V-")
			(pintype "power_in")
		)
		(pad "5" smd roundrect
			(at 2.475 1.905)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 52 "unconnected-(U6B-+-Pad5)")
			(pinfunction "+")
			(pintype "input")
		)
		(pad "6" smd roundrect
			(at 2.475 0.635)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 53 "unconnected-(U6B---Pad6)")
			(pinfunction "-")
			(pintype "input")
		)
		(pad "7" smd roundrect
			(at 2.475 -0.635)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 54 "unconnected-(U6-Pad7)")
			(pintype "output")
		)
		(pad "8" smd roundrect
			(at 2.475 -1.905)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 32 "/Power_out_1/Power")
			(pinfunction "V+")
			(pintype "power_in")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-8_3.9x4.9mm_P1.27mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Jumper:SolderJumper-2_P1.3mm_Open_RoundedPad1.0x1.5mm"
		(layer "F.Cu")
		(at 228.75 144.5 -90)
		(descr "SMD Solder Jumper, 1x1.5mm, rounded Pads, 0.3mm gap, open")
		(tags "solder jumper open")
		(property "Reference" "JP6"
			(at 2.5 0 180)
			(layer "F.SilkS")
		)
		(property "Value" "Add1000"
			(at 0 1.9 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Jumper:SolderJumper-2_P1.3mm_Open_RoundedPad1.0x1.5mm"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Solder Jumper, 2-pole, open"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SolderJumper*Open*")
		(sheetname "Root")
		(sheetfile "PWM_Module.kicad_sch")
		(zone_connect 1)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "1" smd custom
			(at -0.65 0 270)
			(size 1 0.5)
			(layers "F.Cu" "F.Mask")
			(net 38 "Net-(JP6-A)")
			(pinfunction "A")
			(pintype "passive")
			(zone_connect 2)
			(thermal_bridge_angle 45)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_circle
					(center 0 0.25)
					(end 0.5 0.25)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0 -0.25)
					(end 0.5 -0.25)
					(width 0)
					(fill yes)
				)
				(gr_poly
					(pts
						(xy 0.5 0.75) (xy 0 0.75) (xy 0 -0.75) (xy 0.5 -0.75)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "2" smd custom
			(at 0.65 0 270)
			(size 1 0.5)
			(layers "F.Cu" "F.Mask")
			(net 3 "VDD")
			(pinfunction "B")
			(pintype "passive")
			(zone_connect 2)
			(thermal_bridge_angle 45)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_circle
					(center 0 0.25)
					(end 0.5 0.25)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0 -0.25)
					(end 0.5 -0.25)
					(width 0)
					(fill yes)
				)
				(gr_poly
					(pts
						(xy 0 0.75) (xy -0.5 0.75) (xy -0.5 -0.75) (xy 0 -0.75)
					)
					(width 0)
					(fill yes)
				)
			)
		)
	)
	(footprint "Connector_JST:JST_XA_S03B-XASK-1_1x03_P2.50mm_Horizontal"
		(layer "F.Cu")
		(at 223.5 103.9 180)
		(descr "JST XA series connector, S03B-XASK-1 (http://www.jst-mfg.com/product/pdf/eng/eXA1.pdf), generated with kicad-footprint-generator")
		(tags "connector JST XA horizontal hook")
		(property "Reference" "J2"
			(at 0 -2.35 0)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x03"
			(at 2.5 10.4 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_JST:JST_XA_S03B-XASK-1_1x03_P2.50mm_Horizontal"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x03, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "Power_out_2")
		(sheetfile "PWR.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.5 2.5 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole oval
			(at 2.5 6.5 180)
			(size 2.8 2)
			(drill oval 2.8 2)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" thru_hole roundrect
			(at 0 0 180)
			(size 1.7 1.95)
			(drill 0.95)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.147059)
			(net 33 "/Power_out_1/Shunt")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 2.5 0 180)
			(size 1.7 1.95)
			(drill 0.95)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 40 "Net-(J2-Pin_2)")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 5 0 180)
			(size 1.7 1.95)
			(drill 0.95)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 35 "/S2")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_JST.3dshapes/JST_XA_S03B-XASK-1_1x03_P2.50mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Jumper:SolderJumper-2_P1.3mm_Open_RoundedPad1.0x1.5mm"
		(layer "F.Cu")
		(at 225.75 144.5 -90)
		(descr "SMD Solder Jumper, 1x1.5mm, rounded Pads, 0.3mm gap, open")
		(tags "solder jumper open")
		(property "Reference" "JP5"
			(at 2.5 0.25 180)
			(layer "F.SilkS")
		)
		(property "Value" "Add0100"
			(at 0 1.9 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Jumper:SolderJumper-2_P1.3mm_Open_RoundedPad1.0x1.5mm"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Solder Jumper, 2-pole, open"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SolderJumper*Open*")
		(sheetname "Root")
		(sheetfile "PWM_Module.kicad_sch")
		(zone_connect 1)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "1" smd custom
			(at -0.65 0 270)
			(size 1 0.5)
			(layers "F.Cu" "F.Mask")
			(net 39 "Net-(JP5-A)")
			(pinfunction "A")
			(pintype "passive")
			(zone_connect 2)
			(thermal_bridge_angle 45)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_circle
					(center 0 0.25)
					(end 0.5 0.25)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0 -0.25)
					(end 0.5 -0.25)
					(width 0)
					(fill yes)
				)
				(gr_poly
					(pts
						(xy 0.5 0.75) (xy 0 0.75) (xy 0 -0.75) (xy 0.5 -0.75)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "2" smd custom
			(at 0.65 0 270)
			(size 1 0.5)
			(layers "F.Cu" "F.Mask")
			(net 3 "VDD")
			(pinfunction "B")
			(pintype "passive")
			(zone_connect 2)
			(thermal_bridge_angle 45)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_circle
					(center 0 0.25)
					(end 0.5 0.25)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0 -0.25)
					(end 0.5 -0.25)
					(width 0)
					(fill yes)
				)
				(gr_poly
					(pts
						(xy 0 0.75) (xy -0.5 0.75) (xy -0.5 -0.75) (xy 0 -0.75)
					)
					(width 0)
					(fill yes)
				)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(at 226.25 114 180)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R8"
			(at 0 -1.65 180)
			(layer "F.SilkS")
		)
		(property "Value" "4k7"
			(at 0 1.65 180)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Power_out_2")
		(sheetfile "PWR.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1 0 180)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.208333)
			(net 12 "Net-(Q2-C)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1 0 180)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.208333)
			(net 23 "Net-(U3-B2)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Jumper:SolderJumper-2_P1.3mm_Open_RoundedPad1.0x1.5mm"
		(layer "F.Cu")
		(at 219.75 144.5 -90)
		(descr "SMD Solder Jumper, 1x1.5mm, rounded Pads, 0.3mm gap, open")
		(tags "solder jumper open")
		(property "Reference" "JP3"
			(at 2.5 0 180)
			(layer "F.SilkS")
		)
		(property "Value" "Add0001"
			(at 0 1.9 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Jumper:SolderJumper-2_P1.3mm_Open_RoundedPad1.0x1.5mm"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Solder Jumper, 2-pole, open"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SolderJumper*Open*")
		(sheetname "Root")
		(sheetfile "PWM_Module.kicad_sch")
		(zone_connect 1)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "1" smd custom
			(at -0.65 0 270)
			(size 1 0.5)
			(layers "F.Cu" "F.Mask")
			(net 6 "Net-(JP3-A)")
			(pinfunction "A")
			(pintype "passive")
			(zone_connect 2)
			(thermal_bridge_angle 45)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_circle
					(center 0 0.25)
					(end 0.5 0.25)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0 -0.25)
					(end 0.5 -0.25)
					(width 0)
					(fill yes)
				)
				(gr_poly
					(pts
						(xy 0.5 0.75) (xy 0 0.75) (xy 0 -0.75) (xy 0.5 -0.75)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "2" smd custom
			(at 0.65 0 270)
			(size 1 0.5)
			(layers "F.Cu" "F.Mask")
			(net 3 "VDD")
			(pinfunction "B")
			(pintype "passive")
			(zone_connect 2)
			(thermal_bridge_angle 45)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_circle
					(center 0 0.25)
					(end 0.5 0.25)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0 -0.25)
					(end 0.5 -0.25)
					(width 0)
					(fill yes)
				)
				(gr_poly
					(pts
						(xy 0 0.75) (xy -0.5 0.75) (xy -0.5 -0.75) (xy 0 -0.75)
					)
					(width 0)
					(fill yes)
				)
			)
		)
	)
	(footprint "Kicad_Libs:Formfactor"
		(locked yes)
		(layer "F.Cu")
		(at 216 98)
		(property "Reference" "J5"
			(at -38.75 -0.75 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Conn_01x01"
			(at -30.5 -2.5 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" "Kicad_Libs:Formfactor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x01, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "Root")
		(sheetfile "PWM_Module.kicad_sch")
		(fp_line
			(start -45 48)
			(end -45 -2)
			(layer "Edge.Cuts")
		)
		(fp_line
			(start -43 -4)
			(end 38 -4)
			(layer "Edge.Cuts")
		)
		(fp_line
			(start 38 50)
			(end -43 50)
			(layer "Edge.Cuts")
		)
		(fp_line
			(start 40 -2)
			(end 40 48)
			(layer "Edge.Cuts")
		)
		(fp_arc
			(start -45 -2)
			(mid -44.414214 -3.414214)
			(end -43 -4)
			(layer "Edge.Cuts")
		)
		(fp_arc
			(start -43 50)
			(mid -44.414214 49.414214)
			(end -45 48)
			(layer "Edge.Cuts")
		)
		(fp_arc
			(start 38 -4)
			(mid 39.414214 -3.414214)
			(end 40 -2)
			(layer "Edge.Cuts")
		)
		(fp_arc
			(start 40 48)
			(mid 39.414214 49.414214)
			(end 38 50)
			(layer "Edge.Cuts")
		)
		(fp_text user "${REFERENCE}"
			(at -30.5 -1 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(dimension
			(type aligned)
			(layer "F.Fab")
			(pts
				(xy 173 94) (xy 173 148)
			)
			(height 5)
			(gr_text "54,0000 mm"
				(at 166.85 121 90)
				(layer "F.Fab")
			)
			(format
				(prefix "")
				(suffix "")
				(units 3)
				(units_format 1)
				(precision 4)
			)
			(style
				(thickness 0.1)
				(arrow_length 1.27)
				(text_position_mode 0)
				(extension_height 0.58642)
				(extension_offset 0.5) keep_text_aligned)
		)
		(dimension
			(type aligned)
			(layer "F.Fab")
			(pts
				(xy 171 96) (xy 256 96)
			)
			(height -7)
			(gr_text "85,0000 mm"
				(at 213.5 87.85 0)
				(layer "F.Fab")
			)
			(format
				(prefix "")
				(suffix "")
				(units 3)
				(units_format 1)
				(precision 4)
			)
			(style
				(thickness 0.1)
				(arrow_length 1.27)
				(text_position_mode 0)
				(extension_height 0.58642)
				(extension_offset 0.5) keep_text_aligned)
		)
		(pad "1" thru_hole circle
			(at -42.75 2 180)
			(size 0.6 0.6)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "1" thru_hole circle
			(at -42.75 44 180)
			(size 0.6 0.6)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "1" thru_hole circle
			(at -41.651651 -0.651651 180)
			(size 0.6 0.6)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "1" thru_hole circle
			(at -41.651651 41.348349 180)
			(size 0.6 0.6)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "1" thru_hole circle
			(at -41.65165 4.65165 180)
			(size 0.6 0.6)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "1" thru_hole circle
			(at -41.65165 46.65165 180)
			(size 0.6 0.6)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "1" thru_hole circle
			(at -39 -1.75 180)
			(size 0.6 0.6)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "1" thru_hole circle
			(at -39 2 180)
			(size 10 10)
			(drill 5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "1" thru_hole circle
			(at -39 5.75 180)
			(size 0.6 0.6)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "1" thru_hole circle
			(at -39 40.25 180)
			(size 0.6 0.6)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "1" thru_hole circle
			(at -39 44 270)
			(size 10 10)
			(drill 5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "1" thru_hole circle
			(at -39 47.75 180)
			(size 0.6 0.6)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "1" thru_hole circle
			(at -36.34835 4.65165 180)
			(size 0.6 0.6)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "1" thru_hole circle
			(at -36.34835 46.65165 180)
			(size 0.6 0.6)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "1" thru_hole circle
			(at -36.348349 -0.651651 180)
			(size 0.6 0.6)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "1" thru_hole circle
			(at -36.348349 41.348349 180)
			(size 0.6 0.6)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "1" thru_hole circle
			(at -35.25 2 180)
			(size 0.6 0.6)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "1" thru_hole circle
			(at -35.25 44 180)
			(size 0.6 0.6)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "1" thru_hole circle
			(at 30.25 2 180)
			(size 0.6 0.6)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "1" thru_hole circle
			(at 30.25 44 180)
			(size 0.6 0.6)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "1" thru_hole circle
			(at 31.348349 -0.651651 180)
			(size 0.6 0.6)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "1" thru_hole circle
			(at 31.348349 41.348349 180)
			(size 0.6 0.6)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "1" thru_hole circle
			(at 31.34835 4.65165 180)
			(size 0.6 0.6)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "1" thru_hole circle
			(at 31.34835 46.65165 180)
			(size 0.6 0.6)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "1" thru_hole circle
			(at 34 -1.75 180)
			(size 0.6 0.6)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "1" thru_hole circle
			(at 34 2 90)
			(size 10 10)
			(drill 5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "1" thru_hole circle
			(at 34 5.75 180)
			(size 0.6 0.6)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "1" thru_hole circle
			(at 34 40.25 180)
			(size 0.6 0.6)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "1" thru_hole circle
			(at 34 44)
			(size 10 10)
			(drill 5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "1" thru_hole circle
			(at 34 47.75 180)
			(size 0.6 0.6)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "1" thru_hole circle
			(at 36.65165 4.65165 180)
			(size 0.6 0.6)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "1" thru_hole circle
			(at 36.65165 46.65165 180)
			(size 0.6 0.6)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "1" thru_hole circle
			(at 36.651651 -0.651651 180)
			(size 0.6 0.6)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "1" thru_hole circle
			(at 36.651651 41.348349 180)
			(size 0.6 0.6)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "1" thru_hole circle
			(at 37.75 2 180)
			(size 0.6 0.6)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "1" thru_hole circle
			(at 37.75 44 180)
			(size 0.6 0.6)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
	)
	(footprint "Shunt:R3637"
		(layer "F.Cu")
		(at 243.75 124 -90)
		(property "Reference" "R18"
			(at 0.254 -6.096 -90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "Shnt"
			(at 0 5.612 -90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" "Shunt:R3637"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "PWM_Module.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 7.112 -90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -3.63 0 270)
			(size 3.2 9.91)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 33 "/Power_out_1/Shunt")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "2" smd roundrect
			(at 3.63 0 270)
			(size 3.2 9.91)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(at 213.75 127.25)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R9"
			(at 2.75 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "4k7"
			(at 0 1.65 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Power_out_2")
		(sheetfile "PWR.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.208333)
			(net 44 "/H2")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.208333)
			(net 16 "Net-(Q2-B)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(at 213.75 122.25)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R12"
			(at 3.25 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "4k7"
			(at 0 1.65 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Power_out_3")
		(sheetfile "PWR.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.208333)
			(net 46 "/H3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.208333)
			(net 17 "Net-(Q3-B)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Jumper:SolderJumper-2_P1.3mm_Open_RoundedPad1.0x1.5mm"
		(layer "F.Cu")
		(at 231.25 131.5 180)
		(descr "SMD Solder Jumper, 1x1.5mm, rounded Pads, 0.3mm gap, open")
		(tags "solder jumper open")
		(property "Reference" "JP1"
			(at 0 -1.8 0)
			(layer "F.SilkS")
		)
		(property "Value" "Vdd-Vpp"
			(at 0 1.9 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Jumper:SolderJumper-2_P1.3mm_Open_RoundedPad1.0x1.5mm"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Solder Jumper, 2-pole, open"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SolderJumper*Open*")
		(sheetname "Root")
		(sheetfile "PWM_Module.kicad_sch")
		(zone_connect 1)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "1" smd custom
			(at -0.65 0 180)
			(size 1 0.5)
			(layers "F.Cu" "F.Mask")
			(net 32 "/Power_out_1/Power")
			(pinfunction "A")
			(pintype "passive")
			(zone_connect 2)
			(thermal_bridge_angle 45)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_circle
					(center 0 0.25)
					(end 0.5 0.25)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0 -0.25)
					(end 0.5 -0.25)
					(width 0)
					(fill yes)
				)
				(gr_poly
					(pts
						(xy 0.5 0.75) (xy 0 0.75) (xy 0 -0.75) (xy 0.5 -0.75)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "2" smd custom
			(at 0.65 0 180)
			(size 1 0.5)
			(layers "F.Cu" "F.Mask")
			(net 3 "VDD")
			(pinfunction "B")
			(pintype "passive")
			(zone_connect 2)
			(thermal_bridge_angle 45)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_circle
					(center 0 0.25)
					(end 0.5 0.25)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0 -0.25)
					(end 0.5 -0.25)
					(width 0)
					(fill yes)
				)
				(gr_poly
					(pts
						(xy 0 0.75) (xy -0.5 0.75) (xy -0.5 -0.75) (xy 0 -0.75)
					)
					(width 0)
					(fill yes)
				)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(at 222.75 140.5 90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R2"
			(at 2.75 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 0 1.65 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "PWM_Module.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1 0 90)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.208333)
			(net 51 "Net-(JP4-A)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1 0 90)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.208333)
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(at 191.5 126 180)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R17"
			(at 3.25 -0.25 180)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 0 1.65 180)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "PWM_Module.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1 0 180)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.208333)
			(net 29 "Net-(U1-~{RESET}{slash}PF6)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1 0 180)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.208333)
			(net 3 "VDD")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_SMD:D_SMA"
		(layer "F.Cu")
		(at 191.5 135.5)
		(descr "Diode SMA (DO-214AC)")
		(tags "Diode SMA (DO-214AC)")
		(property "Reference" "D1"
			(at -4.75 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "3SMAJ5919B-TP"
			(at 0 2.6 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Diode_SMD:D_SMA"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Zener diode"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TO-???* *_Diode_* *SingleDiode* D_*")
		(sheetname "Root")
		(sheetfile "PWM_Module.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -2.5 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2 0)
			(size 2.5 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.1388888889)
			(net 3 "VDD")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 2 0)
			(size 2.5 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.1388888889)
			(net 1 "GND")
			(pinfunction "A")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SMA.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(at 225.75 140.5 90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R3"
			(at 2.75 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 0 1.65 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "PWM_Module.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1 0 90)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.208333)
			(net 39 "Net-(JP5-A)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1 0 90)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.208333)
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23_Handsoldering"
		(layer "F.Cu")
		(at 227 110.5 180)
		(descr "SOT-23, Handsoldering")
		(tags "SOT-23")
		(property "Reference" "Q2"
			(at -1.25 2.5 0)
			(layer "F.SilkS")
		)
		(property "Value" "MMBT3904-7-F"
			(at 0 2.5 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23_Handsoldering"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "NPN transistor, base/emitter/collector"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Power_out_2")
		(sheetfile "PWR.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.5 -0.95 180)
			(size 1.9 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 16 "Net-(Q2-B)")
			(pinfunction "B")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -1.5 0.95 180)
			(size 1.9 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "E")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at 1.5 0 180)
			(size 1.9 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 12 "Net-(Q2-C)")
			(pinfunction "C")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23_Handsoldering"
		(layer "F.Cu")
		(at 197 110.5 180)
		(descr "SOT-23, Handsoldering")
		(tags "SOT-23")
		(property "Reference" "Q4"
			(at -1.5 2.5 0)
			(layer "F.SilkS")
		)
		(property "Value" "MMBT3904-7-F"
			(at 0 2.5 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23_Handsoldering"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "NPN transistor, base/emitter/collector"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Power_out_4")
		(sheetfile "PWR.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.5 -0.95 180)
			(size 1.9 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 19 "Net-(Q4-B)")
			(pinfunction "B")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -1.5 0.95 180)
			(size 1.9 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "E")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at 1.5 0 180)
			(size 1.9 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 20 "Net-(Q4-C)")
			(pinfunction "C")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(at 223 123.25 -90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R19"
			(at 0 -1.65 90)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 0 1.65 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "PWM_Module.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1 0 270)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.208333)
			(net 55 "/OPAMP")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1 0 270)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.208333)
			(net 56 "Net-(U6A--)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(at 187 117.75 90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R15"
			(at 0 -1.65 90)
			(layer "F.SilkS")
		)
		(property "Value" "4k7"
			(at 0 1.65 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Power_out_4")
		(sheetfile "PWR.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1 0 90)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.208333)
			(net 48 "/H4")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1 0 90)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.208333)
			(net 19 "Net-(Q4-B)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(at 219.75 140.5 90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R1"
			(at 2.75 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 0 1.65 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "PWM_Module.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1 0 90)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.208333)
			(net 6 "Net-(JP3-A)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1 0 90)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.208333)
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Jumper:SolderJumper-2_P1.3mm_Open_RoundedPad1.0x1.5mm"
		(layer "F.Cu")
		(at 222.75 144.5 -90)
		(descr "SMD Solder Jumper, 1x1.5mm, rounded Pads, 0.3mm gap, open")
		(tags "solder jumper open")
		(property "Reference" "JP4"
			(at 2.5 0.25 180)
			(layer "F.SilkS")
		)
		(property "Value" "Add0010"
			(at 0 1.9 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Jumper:SolderJumper-2_P1.3mm_Open_RoundedPad1.0x1.5mm"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Solder Jumper, 2-pole, open"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SolderJumper*Open*")
		(sheetname "Root")
		(sheetfile "PWM_Module.kicad_sch")
		(zone_connect 1)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "1" smd custom
			(at -0.65 0 270)
			(size 1 0.5)
			(layers "F.Cu" "F.Mask")
			(net 51 "Net-(JP4-A)")
			(pinfunction "A")
			(pintype "passive")
			(zone_connect 2)
			(thermal_bridge_angle 45)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_circle
					(center 0 0.25)
					(end 0.5 0.25)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0 -0.25)
					(end 0.5 -0.25)
					(width 0)
					(fill yes)
				)
				(gr_poly
					(pts
						(xy 0.5 0.75) (xy 0 0.75) (xy 0 -0.75) (xy 0.5 -0.75)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "2" smd custom
			(at 0.65 0 270)
			(size 1 0.5)
			(layers "F.Cu" "F.Mask")
			(net 3 "VDD")
			(pinfunction "B")
			(pintype "passive")
			(zone_connect 2)
			(thermal_bridge_angle 45)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_circle
					(center 0 0.25)
					(end 0.5 0.25)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0 -0.25)
					(end 0.5 -0.25)
					(width 0)
					(fill yes)
				)
				(gr_poly
					(pts
						(xy 0 0.75) (xy -0.5 0.75) (xy -0.5 -0.75) (xy 0 -0.75)
					)
					(width 0)
					(fill yes)
				)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(at 213.75 132.25)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R6"
			(at 2.75 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "4k7"
			(at 0 1.65 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Power_out_1")
		(sheetfile "PWR.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.208333)
			(net 41 "/H1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.208333)
			(net 9 "Net-(Q1-B)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(at 196.25 114 180)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R14"
			(at 0 -1.65 180)
			(layer "F.SilkS")
		)
		(property "Value" "4k7"
			(at 0 1.65 180)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Power_out_4")
		(sheetfile "PWR.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1 0 180)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.208333)
			(net 20 "Net-(Q4-C)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1 0 180)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.208333)
			(net 27 "Net-(U5-B2)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_JST:JST_XA_S03B-XASK-1_1x03_P2.50mm_Horizontal"
		(layer "F.Cu")
		(at 193.5 103.9 180)
		(descr "JST XA series connector, S03B-XASK-1 (http://www.jst-mfg.com/product/pdf/eng/eXA1.pdf), generated with kicad-footprint-generator")
		(tags "connector JST XA horizontal hook")
		(property "Reference" "J7"
			(at 0 -2.6 0)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x03"
			(at 2.5 10.4 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_JST:JST_XA_S03B-XASK-1_1x03_P2.50mm_Horizontal"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x03, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "Power_out_4")
		(sheetfile "PWR.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.5 2.5 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole oval
			(at 2.5 6.5 180)
			(size 2.8 2)
			(drill oval 2.8 2)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" thru_hole roundrect
			(at 0 0 180)
			(size 1.7 1.95)
			(drill 0.95)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.147059)
			(net 33 "/Power_out_1/Shunt")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 2.5 0 180)
			(size 1.7 1.95)
			(drill 0.95)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "Net-(J7-Pin_2)")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 5 0 180)
			(size 1.7 1.95)
			(drill 0.95)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 37 "/S4")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_JST.3dshapes/JST_XA_S03B-XASK-1_1x03_P2.50mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(at 228.75 140.5 90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R4"
			(at 2.75 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 0 1.65 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "PWM_Module.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1 0 90)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.208333)
			(net 38 "Net-(JP6-A)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1 0 90)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.208333)
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Library:PowerDI5060"
		(layer "F.Cu")
		(at 191 111)
		(property "Reference" "U5"
			(at -1.75 -3.75 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "DXTC3C100PDQ-13"
			(at -4.675 0 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" "Library:PowerDI5060"
			(at -1.905 3.175 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at -1.905 3.175 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at -1.905 3.175 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Power_out_4")
		(sheetfile "PWR.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at -3.175 0 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.905 3.175)
			(size 0.61 1.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 33 "/Power_out_1/Shunt")
			(pinfunction "E1")
			(pintype "unspecified")
			(thermal_bridge_angle 45)
		)
		(pad "2" smd roundrect
			(at -0.635 3.175)
			(size 0.61 1.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 28 "Net-(U5-B1)")
			(pinfunction "B1")
			(pintype "unspecified")
			(thermal_bridge_angle 45)
		)
		(pad "3" smd roundrect
			(at 0.635 3.175)
			(size 0.61 1.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 32 "/Power_out_1/Power")
			(pinfunction "E2")
			(pintype "unspecified")
			(thermal_bridge_angle 45)
		)
		(pad "4" smd roundrect
			(at 1.905 3.175)
			(size 0.61 1.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 27 "Net-(U5-B2)")
			(pinfunction "B2")
			(pintype "unspecified")
			(thermal_bridge_angle 45)
		)
		(pad "5" smd roundrect
			(at 1.905 -2.29)
			(size 0.61 1.02)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 8 "Net-(J7-Pin_2)")
			(pinfunction "C2")
			(pintype "unspecified")
			(thermal_bridge_angle 45)
		)
		(pad "6" smd roundrect
			(at 0.635 -2.29)
			(size 0.61 1.02)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 8 "Net-(J7-Pin_2)")
			(pinfunction "C2")
			(pintype "unspecified")
			(thermal_bridge_angle 45)
		)
		(pad "6" smd roundrect
			(at 1.27 -0.1524 90)
			(size 3.783 1.82)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.1)
			(net 8 "Net-(J7-Pin_2)")
			(pinfunction "C2")
			(pintype "unspecified")
			(thermal_bridge_angle 45)
		)
		(pad "7" smd roundrect
			(at -1.27 -0.1524 90)
			(size 3.783 1.82)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.1)
			(net 8 "Net-(J7-Pin_2)")
			(pinfunction "C1")
			(pintype "unspecified")
			(thermal_bridge_angle 45)
		)
		(pad "7" smd roundrect
			(at -0.635 -2.29)
			(size 0.61 1.02)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 8 "Net-(J7-Pin_2)")
			(pinfunction "C1")
			(pintype "unspecified")
			(thermal_bridge_angle 45)
		)
		(pad "8" smd roundrect
			(at -1.905 -2.29)
			(size 0.61 1.02)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 8 "Net-(J7-Pin_2)")
			(pinfunction "C1")
			(pintype "unspecified")
			(thermal_bridge_angle 45)
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23_Handsoldering"
		(layer "F.Cu")
		(at 212 110.5 180)
		(descr "SOT-23, Handsoldering")
		(tags "SOT-23")
		(property "Reference" "Q3"
			(at -1.5 2.5 0)
			(layer "F.SilkS")
		)
		(property "Value" "MMBT3904-7-F"
			(at 0 2.5 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23_Handsoldering"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "NPN transistor, base/emitter/collector"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Power_out_3")
		(sheetfile "PWR.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.5 -0.95 180)
			(size 1.9 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 17 "Net-(Q3-B)")
			(pinfunction "B")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -1.5 0.95 180)
			(size 1.9 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "E")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at 1.5 0 180)
			(size 1.9 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 18 "Net-(Q3-C)")
			(pinfunction "C")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23_Handsoldering"
		(layer "F.Cu")
		(at 242 110.5 180)
		(descr "SOT-23, Handsoldering")
		(tags "SOT-23")
		(property "Reference" "Q1"
			(at -2 -2.75 0)
			(layer "F.SilkS")
		)
		(property "Value" "MMBT3904-7-F"
			(at 0 2.5 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23_Handsoldering"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "NPN transistor, base/emitter/collector"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Power_out_1")
		(sheetfile "PWR.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.5 -0.95 180)
			(size 1.9 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 9 "Net-(Q1-B)")
			(pinfunction "B")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -1.5 0.95 180)
			(size 1.9 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "E")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at 1.5 0 180)
			(size 1.9 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 10 "Net-(Q1-C)")
			(pinfunction "C")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(at 241.25 114 180)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R5"
			(at 0 -1.65 180)
			(layer "F.SilkS")
		)
		(property "Value" "4k7"
			(at 0 1.65 180)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Power_out_1")
		(sheetfile "PWR.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1 0 180)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.208333)
			(net 10 "Net-(Q1-C)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1 0 180)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.208333)
			(net 21 "Net-(U2-B2)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_JST:JST_XA_S03B-XASK-1_1x03_P2.50mm_Horizontal"
		(layer "F.Cu")
		(at 208.5 103.9 180)
		(descr "JST XA series connector, S03B-XASK-1 (http://www.jst-mfg.com/product/pdf/eng/eXA1.pdf), generated with kicad-footprint-generator")
		(tags "connector JST XA horizontal hook")
		(property "Reference" "J6"
			(at 0 -2.35 0)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x03"
			(at 2.5 10.4 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_JST:JST_XA_S03B-XASK-1_1x03_P2.50mm_Horizontal"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x03, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "Power_out_3")
		(sheetfile "PWR.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.5 2.5 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole oval
			(at 2.5 6.5 180)
			(size 2.8 2)
			(drill oval 2.8 2)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" thru_hole roundrect
			(at 0 0 180)
			(size 1.7 1.95)
			(drill 0.95)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.147059)
			(net 33 "/Power_out_1/Shunt")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 2.5 0 180)
			(size 1.7 1.95)
			(drill 0.95)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "Net-(J6-Pin_2)")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 5 0 180)
			(size 1.7 1.95)
			(drill 0.95)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 36 "/S3")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_JST.3dshapes/JST_XA_S03B-XASK-1_1x03_P2.50mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(at 213.75 124.75)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R10"
			(at 3.25 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "4k7"
			(at 0 1.65 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Power_out_2")
		(sheetfile "PWR.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.208333)
			(net 45 "/L2")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.208333)
			(net 24 "Net-(U3-B1)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(at 191.5 129)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C3"
			(at -3 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "4.7u"
			(at 0 1.68 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "PWM_Module.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.212766)
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.212766)
			(net 3 "VDD")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Library:PowerDI5060"
		(layer "F.Cu")
		(at 221 111)
		(property "Reference" "U3"
			(at -1.75 -3.75 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "DXTC3C100PDQ-13"
			(at -4.675 0 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" "Library:PowerDI5060"
			(at -1.905 3.175 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at -1.905 3.175 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at -1.905 3.175 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Power_out_2")
		(sheetfile "PWR.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at -3.175 0 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.905 3.175)
			(size 0.61 1.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 33 "/Power_out_1/Shunt")
			(pinfunction "E1")
			(pintype "unspecified")
			(thermal_bridge_angle 45)
		)
		(pad "2" smd roundrect
			(at -0.635 3.175)
			(size 0.61 1.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 24 "Net-(U3-B1)")
			(pinfunction "B1")
			(pintype "unspecified")
			(thermal_bridge_angle 45)
		)
		(pad "3" smd roundrect
			(at 0.635 3.175)
			(size 0.61 1.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 32 "/Power_out_1/Power")
			(pinfunction "E2")
			(pintype "unspecified")
			(thermal_bridge_angle 45)
		)
		(pad "4" smd roundrect
			(at 1.905 3.175)
			(size 0.61 1.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 23 "Net-(U3-B2)")
			(pinfunction "B2")
			(pintype "unspecified")
			(thermal_bridge_angle 45)
		)
		(pad "5" smd roundrect
			(at 1.905 -2.29)
			(size 0.61 1.02)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 40 "Net-(J2-Pin_2)")
			(pinfunction "C2")
			(pintype "unspecified")
			(thermal_bridge_angle 45)
		)
		(pad "6" smd roundrect
			(at 0.635 -2.29)
			(size 0.61 1.02)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 40 "Net-(J2-Pin_2)")
			(pinfunction "C2")
			(pintype "unspecified")
			(thermal_bridge_angle 45)
		)
		(pad "6" smd roundrect
			(at 1.27 -0.1524 90)
			(size 3.783 1.82)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.1)
			(net 40 "Net-(J2-Pin_2)")
			(pinfunction "C2")
			(pintype "unspecified")
			(thermal_bridge_angle 45)
		)
		(pad "7" smd roundrect
			(at -1.27 -0.1524 90)
			(size 3.783 1.82)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.1)
			(net 40 "Net-(J2-Pin_2)")
			(pinfunction "C1")
			(pintype "unspecified")
			(thermal_bridge_angle 45)
		)
		(pad "7" smd roundrect
			(at -0.635 -2.29)
			(size 0.61 1.02)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 40 "Net-(J2-Pin_2)")
			(pinfunction "C1")
			(pintype "unspecified")
			(thermal_bridge_angle 45)
		)
		(pad "8" smd roundrect
			(at -1.905 -2.29)
			(size 0.61 1.02)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 40 "Net-(J2-Pin_2)")
			(pinfunction "C1")
			(pintype "unspecified")
			(thermal_bridge_angle 45)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(at 213.75 129.75)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R7"
			(at 2.75 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "4k7"
			(at 0 1.65 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Power_out_1")
		(sheetfile "PWR.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.208333)
			(net 43 "/L1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.208333)
			(net 22 "Net-(U2-B1)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Kicad_Libs:UPDI_Pads"
		(layer "B.Cu")
		(at 176.25 125.75 180)
		(property "Reference" "Prog1"
			(at -1.27 4.75 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "ProgPads"
			(at -3.81 0 -90)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Footprint" "Kicad_Libs:UPDI_Pads"
			(at 0 6.08 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 6.08 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x03, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 6.08 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "Root")
		(sheetfile "PWM_Module.kicad_sch")
		(attr smd)
		(fp_text user "Gnd"
			(at 1.524 -3.302 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(fp_text user "V+"
			(at 1.778 -0.762 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(fp_text user "Prog"
			(at 1.524 1.778 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(fp_text user "UPDI"
			(at -1.778 0 -90)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(fp_text user "${REFERENCE}"
			(at 0.508 -4.826 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at 0 2.54 180)
			(size 3 2)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 7 "UPDI")
			(pinfunction "Pin_1")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "2" smd roundrect
			(at 0 0 180)
			(size 3 2)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 3 "VDD")
			(pinfunction "Pin_2")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "3" smd roundrect
			(at 0 -2.54 180)
			(size 3 2)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "Pin_3")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
	)
	(gr_text "TWI to PWM/Servo module\nALICE V2\nhackaday.io/voltweasel"
		(at 255 114 0)
		(layer "B.SilkS")
	)
	(gr_text "VDD\nGND\nSDA\nSCL"
		(at 212.75 137.5 90)
		(layer "F.SilkS")
	)
	(zone
		(net 5)
		(net_name "Net-(J6-Pin_2)")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 1)
		(connect_pads yes
			(clearance 0.25)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 205 103) (xy 205.5 102.5) (xy 206.5 102.5) (xy 207 103) (xy 207 105) (xy 208.25 106.25) (xy 208.25 112.75)
				(xy 208 113) (xy 204 113) (xy 203.75 112.75) (xy 203.75 106.25) (xy 205 105)
			)
		)
	)
	(zone
		(net 33)
		(net_name "/Power_out_1/Shunt")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 4)
		(connect_pads yes
			(clearance 0.25)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 189.5 115) (xy 189.25 115.25) (xy 186 115.25) (xy 185.25 114.5) (xy 185.25 108.5) (xy 185.75 108)
				(xy 186.75 108) (xy 187.25 108.5) (xy 187.25 112.5) (xy 188 113.25) (xy 189.25 113.25) (xy 189.5 113.5)
			)
		)
	)
	(zone
		(net 33)
		(net_name "/Power_out_1/Shunt")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 4)
		(connect_pads yes
			(clearance 0.25)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 204.5 115) (xy 204.25 115.25) (xy 201 115.25) (xy 200.25 114.5) (xy 200.25 108.5) (xy 200.75 108)
				(xy 201.75 108) (xy 202.25 108.5) (xy 202.25 112.5) (xy 203 113.25) (xy 204.25 113.25) (xy 204.5 113.5)
			)
		)
	)
	(zone
		(net 40)
		(net_name "Net-(J2-Pin_2)")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 1)
		(connect_pads yes
			(clearance 0.25)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 220 103) (xy 220.5 102.5) (xy 221.5 102.5) (xy 222 103) (xy 222 105) (xy 223.25 106.25) (xy 223.25 112.75)
				(xy 223 113) (xy 219 113) (xy 218.75 112.75) (xy 218.75 106.25) (xy 220 105)
			)
		)
	)
	(zone
		(net 32)
		(net_name "/Power_out_1/Power")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 1)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 191 113.5) (xy 191.25 113.25) (xy 192 113.25) (xy 192.25 113.5) (xy 192.25 115.25) (xy 192.5 115.5)
				(xy 205.75 115.5) (xy 206 115.25) (xy 206 113.5) (xy 206.25 113.25) (xy 207 113.25) (xy 207.25 113.5)
				(xy 207.25 115.25) (xy 207.5 115.5) (xy 220.75 115.5) (xy 221 115.25) (xy 221 113.5) (xy 221.25 113.25)
				(xy 222 113.25) (xy 222.25 113.5) (xy 222.25 115.25) (xy 222.5 115.5) (xy 235.75 115.5) (xy 236 115.25)
				(xy 236 113.5) (xy 236.25 113.25) (xy 237 113.25) (xy 237.25 113.5) (xy 237.25 118.5) (xy 237.25 134.5)
				(xy 236 135.75) (xy 236 138.75) (xy 235.5 139.25) (xy 234 139.25) (xy 233.5 138.75) (xy 233.5 119)
				(xy 233 118.5) (xy 191.25 118.5) (xy 191 118.25)
			)
		)
	)
	(zone
		(net 33)
		(net_name "/Power_out_1/Shunt")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 4)
		(connect_pads yes
			(clearance 0.25)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 219.5 115) (xy 219.25 115.25) (xy 216 115.25) (xy 215.25 114.5) (xy 215.25 108.5) (xy 215.75 108)
				(xy 216.75 108) (xy 217.25 108.5) (xy 217.25 112.5) (xy 218 113.25) (xy 219.25 113.25) (xy 219.5 113.5)
			)
		)
	)
	(zone
		(net 8)
		(net_name "Net-(J7-Pin_2)")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 1)
		(connect_pads yes
			(clearance 0.25)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 190 103) (xy 190.5 102.5) (xy 191.5 102.5) (xy 192 103) (xy 192 105) (xy 193.25 106.25) (xy 193.25 112.75)
				(xy 193 113) (xy 189 113) (xy 188.75 112.75) (xy 188.75 106.25) (xy 190 105)
			)
		)
	)
	(zone
		(net 33)
		(net_name "/Power_out_1/Shunt")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 4)
		(connect_pads yes
			(clearance 0.25)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 234.5 115) (xy 234.25 115.25) (xy 231 115.25) (xy 230.25 114.5) (xy 230.25 108.5) (xy 230.75 108)
				(xy 231.75 108) (xy 232.25 108.5) (xy 232.25 112.5) (xy 233 113.25) (xy 234.25 113.25) (xy 234.5 113.5)
			)
		)
	)
	(zone
		(net 42)
		(net_name "Net-(J1-Pin_2)")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 1)
		(connect_pads yes
			(clearance 0.25)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 235 103) (xy 235.5 102.5) (xy 236.5 102.5) (xy 237 103) (xy 237 105) (xy 238.25 106.25) (xy 238.25 112.75)
				(xy 238 113) (xy 234 113) (xy 233.75 112.75) (xy 233.75 106.25) (xy 235 105)
			)
		)
	)
	(zone
		(net 33)
		(net_name "/Power_out_1/Shunt")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 2)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 248.5 122.25) (xy 249.25 121.5) (xy 249.25 117.25) (xy 248.5 116.5) (xy 239 116.5) (xy 238.25 117.25)
				(xy 238.25 121.5) (xy 239 122.25)
			)
		)
	)
	(zone
		(net 1)
		(net_name "GND")
		(layers "F&B.Cu")
		(hatch edge 0.5)
		(connect_pads yes
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 244 106) (xy 256 106) (xy 256 94) (xy 244 94)
			)
		)
	)
	(zone
		(net 1)
		(net_name "GND")
		(layers "F&B.Cu")
		(hatch edge 0.5)
		(priority 5)
		(connect_pads yes
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 244 148) (xy 256 148) (xy 256 136) (xy 244 136)
			)
		)
	)
	(zone
		(net 1)
		(net_name "GND")
		(layers "F&B.Cu")
		(hatch edge 0.5)
		(priority 5)
		(connect_pads yes
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 171 148) (xy 183 148) (xy 183 136) (xy 171 136)
			)
		)
	)
	(zone
		(net 1)
		(net_name "GND")
		(layers "F&B.Cu")
		(hatch edge 0.5)
		(priority 5)
		(connect_pads yes
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 171 106) (xy 183 106) (xy 183 94) (xy 171 94)
			)
		)
	)
	(zone
		(net 1)
		(net_name "GND")
		(layers "F&B.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 1)
		)
		(polygon
			(pts
				(xy 256 94) (xy 171 94) (xy 171 148) (xy 256 148)
			)
		)
	)
	(zone
		(net 33)
		(net_name "/Power_out_1/Shunt")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 3)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 249.25 118.25) (xy 248.5 119) (xy 239 119) (xy 238.25 118.25) (xy 238.25 112.25) (xy 237.75 111.5)
				(xy 185.75 111.5) (xy 185.25 111) (xy 185.25 105.75) (xy 185.75 105.25) (xy 192 105.25) (xy 192.5 104.75)
				(xy 192.5 103) (xy 193 102.5) (xy 194 102.5) (xy 194.5 103) (xy 194.5 104.75) (xy 195 105.25) (xy 207 105.25)
				(xy 207.5 104.75) (xy 207.5 103) (xy 208 102.5) (xy 209 102.5) (xy 209.5 103) (xy 209.5 104.75)
				(xy 210 105.25) (xy 222 105.25) (xy 222.5 104.75) (xy 222.5 103) (xy 223 102.5) (xy 224 102.5) (xy 224.5 103)
				(xy 224.5 104.75) (xy 224.994048 105.25) (xy 237 105.25) (xy 237.524017 104.75) (xy 237.5 103) (xy 238 102.5)
				(xy 239 102.5) (xy 239.5 103) (xy 239.5 104.75) (xy 240 105.25) (xy 245 105.25) (xy 249.25 109.5)
			)
		)
	)
)
